osmo-gmr 0.2.104-2b98 Osmocom GMR-1

Data Fields
ambe_synth Struct Reference
AMBE vocoder » AMBE vocoder - internal API

AMBE synthesizer state. More...

`#include <private.h>`

## Data Fields
int16_t | u_prev
| Last 'u' of previous subframe.
float | uw_prev [121]
| Unvoiced data from previous subframe.
float | psi1
| Current PSI angle for fundamental.
float | phi [56]
| Current phase for each harmonic.
float | SE
| Current energy parameter.

## Detailed Description

AMBE synthesizer state.

The documentation for this struct was generated from the following file:

- src/codec/private.h