09:30:23.645390 13825 C5G_Tests.ttcn:324 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating'.
09:30:24.655996 13825 C5G_Tests.ttcn:324 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating' was executed successfully (exit status: 0).
09:30:24.656126 13825 C5G_Tests.ttcn:324 Test case TC_periodic_registration_updating started.
09:30:24.656388 13825 C5G_Tests.ttcn:324 Initializing variables, timers and ports of component type C5G_Tests.MTC_CT inside testcase TC_periodic_registration_updating.
09:30:24.656482 13825 C5G_Tests.ttcn:324 Port NGAP_UNIT[0] was started.
09:30:24.656523 13825 C5G_Tests.ttcn:324 Port NGAP_PROC[0] was started.
09:30:24.656546 13825 C5G_Tests.ttcn:324 Port TEID0 was started.
09:30:24.656569 13825 C5G_Tests.ttcn:324 Component type C5G_Tests.MTC_CT was initialized.
09:30:24.656595 13825 C5G_Tests.ttcn:191 Start timer g_Tguard: 30 s
09:30:24.656629 13825 C5G_Tests.ttcn:192 Altstep as_Tguard was activated as default, id 1
09:30:24.656659 13825 C5G_Tests.ttcn:183 Creating new PTC with component type GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:30:24.660186 14059 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:30:24.660230 14059 - TTCN-3 Parallel Test Component started on e15dac43427e. Component reference: GTP1U_EM(12), component type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM. Version: 11.1.0.
09:30:24.660249 14059 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:30:24.660306 14059 - Connected to MC.
09:30:24.660325 14059 - Initializing variables, timers and ports of component type GTPv1U_Emulation.GTPv1U_Emulation_CT inside testcase TC_periodic_registration_updating.
09:30:24.660375 13825 C5G_Tests.ttcn:183 PTC was created. Component reference: 12, alive: no, type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:30:24.660419 13825 C5G_Tests.ttcn:184 Mapping port GTP1U_EM(12):GTP1U to system:GTP1U.
09:30:24.661408 14059 - Port GTP1U was started.
09:30:24.661441 14059 - Port TEID0 was started.
09:30:24.661453 14059 - Port CLIENT was started.
09:30:24.661464 14059 - Port CLIENT_PROC was started.
09:30:24.661476 14059 - Port UECUPS was started.
09:30:24.661488 14059 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was initialized.
09:30:24.661530 14059 - Port GTP1U was mapped to system:GTP1U.
09:30:24.661571 13825 C5G_Tests.ttcn:184 Map operation of GTP1U_EM(12):GTP1U to system:GTP1U finished.
09:30:24.661590 13825 C5G_Tests.ttcn:185 Connecting ports GTP1U_EM(12):TEID0 and mtc:TEID0.
09:30:24.661776 13825 C5G_Tests.ttcn:185 Port TEID0 is waiting for connection from GTP1U_EM(12):TEID0 on UNIX pathname /tmp/ttcn3-portconn-876fa674.
09:30:24.661836 14059 - Port TEID0 has established the connection with mtc:TEID0 using transport type UNIX.
09:30:24.661898 13825 C5G_Tests.ttcn:185 Port TEID0 has accepted the connection from GTP1U_EM(12):TEID0.
09:30:24.661958 13825 C5G_Tests.ttcn:185 Connect operation on GTP1U_EM(12):TEID0 and mtc:TEID0 finished.
09:30:24.661990 13825 C5G_Tests.ttcn:186 Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}) on component GTP1U_EM(12).
09:30:24.662043 13825 C5G_Tests.ttcn:186 Function was started.
09:30:24.662174 13825 C5G_Tests.ttcn:161 Creating new PTC with component type NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:30:24.662213 14059 - Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}).
09:30:24.662595 14059 Osmocom_Types.ttcn:65 Random number generator was initialized with seed 13.662591: srand48(1001838446).
09:30:24.662634 14059 Osmocom_Types.ttcn:65 Function rnd() returned 0.857574.
09:30:24.662734 14059 Osmocom_Types.ttcn:65 Function rnd() returned 0.514194.
09:30:24.662861 14059 GTPv1U_Emulation.ttcnpp:214 Mapping port GTP1U_EM(12):UECUPS to system:UECUPS.
09:30:24.662918 14059 GTPv1U_Emulation.ttcnpp:214 Port UECUPS was mapped to system:UECUPS.
09:30:24.662965 14059 GTPv1U_Emulation.ttcnpp:214 Map operation of GTP1U_EM(12):UECUPS to system:UECUPS finished.
09:30:24.663347 14059 GTPv1U_Emulation.ttcnpp:215 entering f__IPL4__PROVIDER__connect: :-1 -> 127.0.0.20:4268 / SCTP
09:30:24.663635 14059 GTPv1U_Emulation.ttcnpp:215 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:30:24.664460 14060 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:30:24.664496 14060 - TTCN-3 Parallel Test Component started on e15dac43427e. Component reference: TC_periodic_registration_updating-NGAP0(13), component type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0. Version: 11.1.0.
09:30:24.664513 14060 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:30:24.664562 14060 - Connected to MC.
09:30:24.664578 14060 - Initializing variables, timers and ports of component type NGAP_Emulation.NGAP_Emulation_CT inside testcase TC_periodic_registration_updating.
09:30:24.664606 13825 C5G_Tests.ttcn:161 PTC was created. Component reference: 13, alive: no, type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:30:24.664663 13825 C5G_Tests.ttcn:162 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:30:24.665104 14059 GTPv1U_Emulation.ttcnpp:190 Sent on UECUPS to system @UECUPS_CodecPort.UECUPS_Send : {
    connId := 1,
    msg := {
        reset_all_state := { }
    }
}
09:30:24.665262 14059 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Encoding @UECUPS_Types.PDU_UECUPS: {
    reset_all_state := { }
}
09:30:24.665404 14059 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Stream after encoding: '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
09:30:24.665558 14059 GTPv1U_Emulation.ttcnpp:190 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := <unbound>,
    msg := '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
}
09:30:24.665671 14060 - Port NGAP was started.
09:30:24.665697 14060 - Port NGAP_CLIENT was started.
09:30:24.665709 14060 - Port NGAP_PROC was started.
09:30:24.665720 14060 - Port NGAP_UNIT was started.
09:30:24.665732 14060 - Component type NGAP_Emulation.NGAP_Emulation_CT was initialized.
09:30:24.665766 14060 - Port NGAP was mapped to system:NGAP_CODEC_PT.
09:30:24.665812 13825 C5G_Tests.ttcn:162 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:30:24.665849 13825 C5G_Tests.ttcn:163 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0].
09:30:24.665910 14059 GTPv1U_Emulation.ttcnpp:191 Start timer T: 30 s
09:30:24.666023 13825 C5G_Tests.ttcn:163 Port NGAP_PROC[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-b657f519.
09:30:24.666057 14060 - Port NGAP_PROC has established the connection with mtc:NGAP_PROC[0] using transport type UNIX.
09:30:24.666099 13825 C5G_Tests.ttcn:163 Port NGAP_PROC[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:24.666131 13825 C5G_Tests.ttcn:163 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0] finished.
09:30:24.666156 13825 C5G_Tests.ttcn:164 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0].
09:30:24.666294 13825 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT on UNIX pathname /tmp/ttcn3-portconn-a74eec08.
09:30:24.666321 14060 - Port NGAP_UNIT has established the connection with mtc:NGAP_UNIT[0] using transport type UNIX.
09:30:24.666361 13825 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:30:24.666396 13825 C5G_Tests.ttcn:164 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0] finished.
09:30:24.666450 13825 C5G_Tests.ttcn:165 Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0") on component TC_periodic_registration_updating-NGAP0(13).
09:30:24.666485 14059 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:24.666568 13825 C5G_Tests.ttcn:165 Function was started.
09:30:24.666646 14060 - Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0").
09:30:24.666648 14059 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS failed: Type of the first message in the queue is not @UECUPS_CodecPort.UECUPS_RecvFrom.
09:30:24.666754 14059 GTPv1U_Emulation.ttcnpp:194 Matching on port UECUPS succeeded:  matched
09:30:24.666809 14059 GTPv1U_Emulation.ttcnpp:194 Receive operation on port UECUPS succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:24.666842 14059 GTPv1U_Emulation.ttcnpp:194 Message with id 1 was extracted from the queue of UECUPS.
09:30:24.666986 14059 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 0,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
} id 2
09:30:24.667061 14059 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Stream before decoding: '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
09:30:24.667196 14060 NGAP_Emulation.ttcn:452 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:30:24.667208 14059 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Decoded @UECUPS_Types.PDU_UECUPS: {
    reset_all_state_res := {
        result := OK (1)
    }
}
09:30:24.667236 14060 NGAP_Emulation.ttcn:452 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:30:24.667284 14059 GTPv1U_Emulation.ttcnpp:192 Incoming message was mapped to @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:30:24.667380 14059 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS succeeded:  matched
09:30:24.667414 14059 GTPv1U_Emulation.ttcnpp:193 Receive operation on port UECUPS succeeded, message from system(): @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:30:24.667438 14060 NGAP_Emulation.ttcn:457 entering f__IPL4__PROVIDER__connect: 127.0.0.202:50000 -> 127.0.0.5:38412 / SCTP
09:30:24.667444 14059 GTPv1U_Emulation.ttcnpp:193 Message with id 2 was extracted from the queue of UECUPS.
09:30:24.667517 14059 GTPv1U_Emulation.ttcnpp:225 Altstep as_uecups_ind was activated as default, id 1
09:30:24.667586 14060 NGAP_Emulation.ttcn:457 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:30:24.668171 14060 NGAP_Emulation.ttcn:469 Sent on NGAP_UNIT to mtc @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
}
09:30:24.668338 13825 C5G_Tests.ttcn:166 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:30:24.668391 13825 C5G_Tests.ttcn:166 Matching on port NGAP_UNIT[0] succeeded:  matched
09:30:24.668426 13825 C5G_Tests.ttcn:166 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:30:24.668457 13825 C5G_Tests.ttcn:166 Message with id 1 was extracted from the queue of NGAP_UNIT[0].
09:30:24.668801 13825 C5G_Tests.ttcn:268 Sent on NGAP_UNIT[0] to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
}
09:30:24.669122 13825 C5G_Tests.ttcn:269 Start timer T: 5 s
09:30:24.670633 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:24.672823 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_UNIT from mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:24.673198 14060 NGAP_Emulation.ttcn:542 Matching on port NGAP_UNIT succeeded:  matched
09:30:24.673274 14060 NGAP_Emulation.ttcn:542 Receive operation on port NGAP_UNIT succeeded, message from mtc: @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:24.673311 14060 NGAP_Emulation.ttcn:542 Message with id 1 was extracted from the queue of NGAP_UNIT.
09:30:24.676517 14060 NGAP_Emulation.ttcn:544 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupRequest := {
                    protocolIEs := {
                        {
                            id := 27,
                            criticality := reject (0),
                            value_ := {
                                globalRANNodeID := {
                                    globalGNB_ID := {
                                        pLMNIdentity := '99F907'O,
                                        gNB_ID := {
                                            gNB_ID := '0000000000000000000000'B
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 102,
                            criticality := reject (0),
                            value_ := {
                                supportedTAList := {
                                    {
                                        tAC := '000001'O,
                                        broadcastPLMNList := {
                                            {
                                                pLMNIdentity := '99F907'O,
                                                tAISliceSupportList := {
                                                    {
                                                        s_NSSAI := {
                                                            sST := '01'O,
                                                            sD := omit,
                                                            iE_Extensions := omit
                                                        },
                                                        iE_Extensions := omit
                                                    }
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 21,
                            criticality := ignore (1),
                            value_ := {
                                pagingDRX := v32 (0)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.677685 14060 NGAP_Emulation.ttcn:544 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '00150025000003001B00080099F907000000000066000D00000000010099F907000000080015400100'O
}
09:30:24.678602 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP failed: Type of the first message in the queue is not @NGAP_CodecPort.NGAP_RecvFrom.
09:30:24.678750 14060 NGAP_Emulation.ttcn:600 Matching on port NGAP succeeded:  matched
09:30:24.678811 14060 NGAP_Emulation.ttcn:600 Receive operation on port NGAP succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:30:24.678851 14060 NGAP_Emulation.ttcn:600 Message with id 1 was extracted from the queue of NGAP.
09:30:24.679018 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '201500320000040001000E05806F70656E3567732D616D663000600008000099F90702004000564001FF005000080099F90700000008'O
} id 2
09:30:24.681074 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:24.681327 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:24.681412 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:24.681469 14060 NGAP_Emulation.ttcn:548 Message with id 2 was extracted from the queue of NGAP.
09:30:24.681663 14060 C5G_Tests.ttcn:128 Sent on NGAP_UNIT to mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.682335 13825 C5G_Tests.ttcn:270 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:24.682438 13825 C5G_Tests.ttcn:271 Matching on port NGAP_UNIT[0] succeeded:  matched
09:30:24.682488 13825 C5G_Tests.ttcn:271 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:30:24.682529 13825 C5G_Tests.ttcn:271 Message with id 2 was extracted from the queue of NGAP_UNIT[0].
09:30:24.682560 13825 C5G_Tests.ttcn:272 setverdict(pass): none -> pass
09:30:24.682678 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.706328.
09:30:24.682720 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.839337.
09:30:24.682749 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.526475.
09:30:24.682775 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.517190.
09:30:24.682801 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.312708.
09:30:24.682827 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.117660.
09:30:24.682852 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.691212.
09:30:24.682878 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.391685.
09:30:24.682903 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.352683.
09:30:24.682928 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.075679.
09:30:24.682953 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.501699.
09:30:24.682978 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.622094.
09:30:24.683003 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.966870.
09:30:24.683028 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.126460.
09:30:24.683053 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.250899.
09:30:24.683078 13825 Osmocom_Types.ttcn:65 Function rnd() returned 0.392491.
09:30:24.683146 13825 C5G_Tests.ttcn:216 Creating new PTC with component type ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:30:24.685987 14061 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:30:24.686073 14061 - TTCN-3 Parallel Test Component started on e15dac43427e. Component reference: TC_periodic_registration_updating0(14), component type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0. Version: 11.1.0.
09:30:24.686107 14061 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:30:24.686207 14061 - Connected to MC.
09:30:24.686244 14061 - Initializing variables, timers and ports of component type ConnHdlr.ConnHdlr inside testcase TC_periodic_registration_updating.
09:30:24.686278 13825 C5G_Tests.ttcn:216 PTC was created. Component reference: 14, alive: no, type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:30:24.686328 13825 C5G_Tests.ttcn:218 Connecting ports TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:30:24.686563 14060 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT is waiting for connection from TC_periodic_registration_updating0(14):NGAP on UNIX pathname /tmp/ttcn3-portconn-1f7da15c.
09:30:24.687957 14061 - Port NGAP was started.
09:30:24.688015 14061 - Port NGAP_PROC was started.
09:30:24.688038 14061 - Port GTP1U[0] was started.
09:30:24.688060 14061 - Port GTP1U[1] was started.
09:30:24.688081 14061 - Port GTP1U[2] was started.
09:30:24.688103 14061 - Port GTP1U[3] was started.
09:30:24.688125 14061 - Port GTP1U_PROC[0] was started.
09:30:24.688147 14061 - Port GTP1U_PROC[1] was started.
09:30:24.688167 14061 - Port GTP1U_PROC[2] was started.
09:30:24.688187 14061 - Port GTP1U_PROC[3] was started.
09:30:24.688208 14061 - Component type ConnHdlr.ConnHdlr was initialized.
09:30:24.688283 14061 - Port NGAP has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT using transport type UNIX.
09:30:24.688351 14060 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT has accepted the connection from TC_periodic_registration_updating0(14):NGAP.
09:30:24.688378 13825 C5G_Tests.ttcn:218 Connect operation on TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT finished.
09:30:24.688412 13825 C5G_Tests.ttcn:219 Connecting ports TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:24.688583 14060 NGAP_Emulation.ttcn:485 Port NGAP_PROC is waiting for connection from TC_periodic_registration_updating0(14):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-567ae15.
09:30:24.688659 14061 - Port NGAP_PROC has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_PROC using transport type UNIX.
09:30:24.688721 14060 NGAP_Emulation.ttcn:485 Port NGAP_PROC has accepted the connection from TC_periodic_registration_updating0(14):NGAP_PROC.
09:30:24.688743 13825 C5G_Tests.ttcn:219 Connect operation on TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC finished.
09:30:24.688781 13825 C5G_Tests.ttcn:222 Connecting ports TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT.
09:30:24.688994 14059 GTPv1U_Emulation.ttcnpp:265 Port CLIENT is waiting for connection from TC_periodic_registration_updating0(14):GTP1U[0] on UNIX pathname /tmp/ttcn3-portconn-1825d238.
09:30:24.689041 14061 - Port GTP1U[0] has established the connection with GTP1U_EM(12):CLIENT using transport type UNIX.
09:30:24.689103 14059 GTPv1U_Emulation.ttcnpp:265 Port CLIENT has accepted the connection from TC_periodic_registration_updating0(14):GTP1U[0].
09:30:24.689120 13825 C5G_Tests.ttcn:222 Connect operation on TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT finished.
09:30:24.689152 13825 C5G_Tests.ttcn:223 Connecting ports TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:30:24.689378 14059 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC is waiting for connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-5a7ea655.
09:30:24.689435 14061 - Port GTP1U_PROC[0] has established the connection with GTP1U_EM(12):CLIENT_PROC using transport type UNIX.
09:30:24.689514 14059 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC has accepted the connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:30:24.689530 13825 C5G_Tests.ttcn:223 Connect operation on TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC finished.
09:30:24.689560 13825 C5G_Tests.ttcn:227 Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '7855316330569123'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}) on component TC_periodic_registration_updating0(14).
09:30:24.689685 13825 C5G_Tests.ttcn:227 Function was started.
09:30:24.690938 14061 - Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '7855316330569123'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}).
09:30:24.694690 14061 ConnHdlr.ttcn:538 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '111'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:24.695293 14061 ConnHdlr.ttcn:538 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004179000D0199F9072143000100000000002E028040'O
09:30:24.698219 14061 ConnHdlr.ttcn:543 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
}
09:30:24.699279 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:24.699388 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.699422 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.699450 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.699475 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.699761 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.699814 14060 NGAP_Emulation.ttcn:513 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:30:24.699846 14060 NGAP_Emulation.ttcn:513 Message with id 1 was extracted from the queue of NGAP_CLIENT.
09:30:24.701360 14060 NGAP_Emulation.ttcn:519 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 15,
            criticality := ignore (1),
            value_ := {
                initialUEMessage := {
                    protocolIEs := {
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := reject (0),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 90,
                            criticality := ignore (1),
                            value_ := {
                                rRCEstablishmentCause := mo_Signalling (3)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.701625 14060 NGAP_Emulation.ttcn:519 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '000F403D00000400550002000000260018177E004179000D0199F9072143000100000000002E0280400079000F4099F907000000000099F907000001005A400118'O
}
09:30:24.704587 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004403E000003000A000200020055000200000026002B2A7E0056020200002186F37F8B0C5B6D7F11462DF182742B182010BA25AD640AAC8000D8C279C47F31FA7B'O
} id 3
09:30:24.705104 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0056020200002186F37F8B0C5B6D7F11462DF182742B182010BA25AD640AAC8000D8C279C47F31FA7B'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:30:24.705172 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:24.705198 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0056020200002186F37F8B0C5B6D7F11462DF182742B182010BA25AD640AAC8000D8C279C47F31FA7B'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:30:24.705224 14060 NGAP_Emulation.ttcn:548 Message with id 3 was extracted from the queue of NGAP.
09:30:24.705398 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0056020200002186F37F8B0C5B6D7F11462DF182742B182010BA25AD640AAC8000D8C279C47F31FA7B'O
09:30:24.705958 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10000110111100110111111110001011000011000101101101101101011111110001000101000110001011011111000110000010011101000010101100011000'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10111010001001011010110101100100000010101010110010000000000000001101100011000010011110011100010001111111001100011111101001111011'B
        },
        eapMessage := omit
    }
}
09:30:24.706224 14060 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10000110111100110111111110001011000011000101101101101101011111110001000101000110001011011111000110000010011101000010101100011000'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10111010001001011010110101100100000010101010110010000000000000001101100011000010011110011100010001111111001100011111101001111011'B
        },
        eapMessage := omit
    }
}
09:30:24.706520 14061 ConnHdlr.ttcn:555 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10000110111100110111111110001011000011000101101101101101011111110001000101000110001011011111000110000010011101000010101100011000'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10111010001001011010110101100100000010101010110010000000000000001101100011000010011110011100010001111111001100011111101001111011'B
        },
        eapMessage := omit
    }
} id 1
09:30:24.706757 14061 ConnHdlr.ttcn:189 Matching on port NGAP succeeded:  matched
09:30:24.706801 14061 ConnHdlr.ttcn:189 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10000110111100110111111110001011000011000101101101101101011111110001000101000110001011011111000110000010011101000010101100011000'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '10111010001001011010110101100100000010101010110010000000000000001101100011000010011110011100010001111111001100011111101001111011'B
        },
        eapMessage := omit
    }
} id 1
09:30:24.706831 14061 ConnHdlr.ttcn:189 Message with id 1 was extracted from the queue of NGAP.
09:30:24.708506 14061 ConnHdlr.ttcn:234 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'CDB3D8192A5650345A717DC91D5747FB6579B458ACCCD3364E87D8E29C3D5C0E'O,
        k_nas_enc := 'F5871F941C9D49FAE70813B5BC6E79EE34D042CA4EA2589FF495B6557FE2DCD1'O
    }
}
09:30:24.708652 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'CDB3D8192A5650345A717DC91D5747FB6579B458ACCCD3364E87D8E29C3D5C0E'O,
        k_nas_enc := 'F5871F941C9D49FAE70813B5BC6E79EE34D042CA4EA2589FF495B6557FE2DCD1'O
    }
} id 2
09:30:24.708711 14061 ConnHdlr.ttcn:238 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01010100100010010000101001110110000010111100011011001001110100010001100101010111101101000001000001100100111001111101110010010111'B
        },
        eapMessage := omit
    }
}
09:30:24.708718 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.708740 14060 NGAP_Emulation.ttcn:487 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'CDB3D8192A5650345A717DC91D5747FB6579B458ACCCD3364E87D8E29C3D5C0E'O,
        k_nas_enc := 'F5871F941C9D49FAE70813B5BC6E79EE34D042CA4EA2589FF495B6557FE2DCD1'O
    }
} id 2
09:30:24.708757 14060 NGAP_Emulation.ttcn:487 Message with id 2 was extracted from the queue of NGAP_CLIENT.
09:30:24.708902 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01010100100010010000101001110110000010111100011011001001110100010001100101010111101101000001000001100100111001111101110010010111'B
        },
        eapMessage := omit
    }
} id 3
09:30:24.708983 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.709000 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.709015 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.709030 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.709052 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.709087 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.709107 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01010100100010010000101001110110000010111100011011001001110100010001100101010111101101000001000001100100111001111101110010010111'B
        },
        eapMessage := omit
    }
} id 3
09:30:24.709124 14060 NGAP_Emulation.ttcn:522 Message with id 3 was extracted from the queue of NGAP_CLIENT.
09:30:24.709180 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '01010100100010010000101001110110000010111100011011001001110100010001100101010111101101000001000001100100111001111101110010010111'B
        },
        eapMessage := omit
    }
}
09:30:24.709330 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00572D1054890A760BC6C9D11957B41064E7DC97'O
09:30:24.710145 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00572D1054890A760BC6C9D11957B41064E7DC97'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.710296 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403C000004000A0002000200550002000000260016157E00572D1054890A760BC6C9D11957B41064E7DC970079400F4099F907000000000099F907000001'O
}
09:30:24.714233 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044027000003000A0002000200550002000000260014137E03F1A8C4D0007E005D0102028040E1360102'O
} id 4
09:30:24.714579 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03F1A8C4D0007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:30:24.714792 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:24.714925 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E03F1A8C4D0007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:30:24.714994 14060 NGAP_Emulation.ttcn:548 Message with id 4 was extracted from the queue of NGAP.
09:30:24.715062 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E03F1A8C4D0007E005D0102028040E1360102'O
09:30:24.715164 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0011'B,
        messageAuthenticationCode := 'F1A8C4D0'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005D0102028040E1360102'O
    }
}
09:30:24.716305 14060 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E005D0102028040E1360102'O
09:30:24.717142 14060 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:30:24.717799 14060 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:30:24.718444 14061 ConnHdlr.ttcn:556 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:30:24.718993 14061 ConnHdlr.ttcn:250 Matching on port NGAP succeeded:  matched
09:30:24.719116 14061 ConnHdlr.ttcn:250 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:30:24.719164 14061 ConnHdlr.ttcn:250 Message with id 2 was extracted from the queue of NGAP.
09:30:24.719274 14061 ConnHdlr.ttcn:255 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
}
09:30:24.719388 14061 ConnHdlr.ttcn:260 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
}
09:30:24.719479 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:30:24.719711 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:30:24.719815 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:30:24.719877 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.719910 14060 NGAP_Emulation.ttcn:499 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:30:24.719923 14061 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:24.719943 14060 NGAP_Emulation.ttcn:499 Message with id 4 was extracted from the queue of NGAP_CLIENT.
09:30:24.720077 14061 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004129000D0199F9072143000100000000002E028040'O
09:30:24.720203 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:30:24.720256 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:30:24.720288 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:30:24.720358 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_alg_int := ?
} unmatched: First message in the queue does not match the template: 
09:30:24.720385 14061 ConnHdlr.ttcn:271 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7855316330569123'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:30:24.720399 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.720426 14060 NGAP_Emulation.ttcn:506 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:30:24.720454 14060 NGAP_Emulation.ttcn:506 Message with id 5 was extracted from the queue of NGAP_CLIENT.
09:30:24.720639 14061 NGAP_Emulation.ttcn:717 Called on NGAP_PROC to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { }
09:30:24.720857 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7855316330569123'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:30:24.720986 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.721010 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.721039 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.721055 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.721088 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.721112 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.721133 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7855316330569123'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:30:24.721153 14060 NGAP_Emulation.ttcn:522 Message with id 6 was extracted from the queue of NGAP_CLIENT.
09:30:24.721217 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7855316330569123'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:30:24.721337 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E005E7700090578553163305691237100177E004129000D0199F9072143000100000000002E028040'O
09:30:24.721922 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0100'B,
        messageAuthenticationCode := '6F6EB694'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005E7700090578553163305691237100177E004129000D0199F9072143000100000000002E028040'O
    }
}
09:30:24.722004 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E046F6EB694007E005E7700090578553163305691237100177E004129000D0199F9072143000100000000002E028040'O
09:30:24.722164 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E046F6EB694007E005E7700090578553163305691237100177E004129000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.722248 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4057000004000A0002000200550002000000260031307E046F6EB694007E005E7700090578553163305691237100177E004129000D0199F9072143000100000000002E0280400079400F4099F907000000000099F907000001'O
}
09:30:24.722439 14060 NGAP_Emulation.ttcn:485 Call enqueued on NGAP_PROC from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:30:24.722485 14060 NGAP_Emulation.ttcn:602 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register.
09:30:24.722506 14060 NGAP_Emulation.ttcn:606 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register_proc.
09:30:24.722536 14060 NGAP_Emulation.ttcn:610 Matching on port NGAP_PROC succeeded: { } with { } matched
09:30:24.722604 14060 NGAP_Emulation.ttcn:610 Getcall operation on port NGAP_PROC succeeded, call from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:30:24.722626 14060 NGAP_Emulation.ttcn:610 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:30:24.722658 14060 NGAP_Emulation.ttcn:613 Replied on NGAP_PROC to TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2
09:30:24.722775 14061 NGAP_Emulation.ttcn:717 Reply enqueued on NGAP_PROC from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:30:24.722867 14061 NGAP_Emulation.ttcn:718 Matching on port NGAP_PROC succeeded: { } with { } matched value 2 with ? matched
09:30:24.722947 14061 NGAP_Emulation.ttcn:718 Getreply operation on port NGAP_PROC succeeded, reply from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:30:24.722977 14061 NGAP_Emulation.ttcn:718 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:30:24.735106 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044056000005000A000200020055000200000026002F2E7E02D4AA6AA0017E0042010177000BF299F907020040C000041A54074099F90700000115020101210201005E0192006E400A0C3B9ACA00303B9ACA00000000020001'O
} id 5
09:30:24.736147 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02D4AA6AA0017E0042010177000BF299F907020040C000041A54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:30:24.736319 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:24.736380 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02D4AA6AA0017E0042010177000BF299F907020040C000041A54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:30:24.736415 14060 NGAP_Emulation.ttcn:548 Message with id 5 was extracted from the queue of NGAP.
09:30:24.736463 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02D4AA6AA0017E0042010177000BF299F907020040C000041A54074099F90700000115020101210201005E0192'O
09:30:24.736522 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'D4AA6AA0'O,
        sequenceNumber := '01'O,
        plainNASMessage := '7E0042010177000BF299F907020040C000041A54074099F90700000115020101210201005E0192'O
    }
}
09:30:24.736976 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C000041A54074099F90700000115020101210201005E0192'O
09:30:24.738334 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:24.739246 14060 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:24.740155 14061 ConnHdlr.ttcn:561 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:30:24.741336 14061 ConnHdlr.ttcn:561 Matching on port NGAP succeeded:  matched
09:30:24.741468 14061 ConnHdlr.ttcn:561 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:30:24.741536 14061 ConnHdlr.ttcn:561 Message with id 3 was extracted from the queue of NGAP.
09:30:24.741775 14061 ConnHdlr.ttcn:563 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:24.741974 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:30:24.742094 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.742131 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.742162 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.742217 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.742355 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.742431 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.742467 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:30:24.742502 14060 NGAP_Emulation.ttcn:522 Message with id 7 was extracted from the queue of NGAP_CLIENT.
09:30:24.742588 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:24.742654 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:30:24.743081 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '6BABA7B7'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:30:24.743193 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E026BABA7B7007E0043'O
09:30:24.743406 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E026BABA7B7007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.743515 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E026BABA7B7007E00430079400F4099F907000000000099F907000001'O
}
09:30:24.744229 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E0215B627DC027E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
} id 6
09:30:24.744410 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0215B627DC027E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:30:24.744528 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:24.744583 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0215B627DC027E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:30:24.744617 14060 NGAP_Emulation.ttcn:548 Message with id 6 was extracted from the queue of NGAP.
09:30:24.744672 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0215B627DC027E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
09:30:24.744724 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '15B627DC'O,
        sequenceNumber := '02'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
    }
}
09:30:24.745170 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
09:30:24.745777 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:24.746353 14060 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:24.746739 14061 ConnHdlr.ttcn:565 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:30:24.747240 14061 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:30:24.747316 14061 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:30:24.747369 14061 ConnHdlr.ttcn:279 Message with id 4 was extracted from the queue of NGAP.
09:30:24.747465 14061 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:24.747582 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:30:24.747666 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.747694 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.747720 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.747744 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.747822 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.747863 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.747897 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:30:24.747926 14060 NGAP_Emulation.ttcn:522 Message with id 8 was extracted from the queue of NGAP_CLIENT.
09:30:24.748007 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:24.748072 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:30:24.748107 14061 ConnHdlr.ttcn:577 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:24.748454 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '37EEB1D3'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:30:24.748522 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0237EEB1D3007E0055'O
09:30:24.748818 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0237EEB1D3007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.748990 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0237EEB1D3007E00550079400F4099F907000000000099F907000001'O
}
09:30:24.749713 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:30:24.750074 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.750122 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.750156 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.750181 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.750234 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.750289 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.750343 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:30:24.750383 14060 NGAP_Emulation.ttcn:522 Message with id 9 was extracted from the queue of NGAP_CLIENT.
09:30:24.750439 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C000041A'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:30:24.750590 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00412B000BF299F907020040C000041A2E028040'O
09:30:24.750969 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '89AC7CF0'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E00412B000BF299F907020040C000041A2E028040'O
    }
}
09:30:24.751014 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0289AC7CF0007E00412B000BF299F907020040C000041A2E028040'O
09:30:24.751185 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0289AC7CF0007E00412B000BF299F907020040C000041A2E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.751292 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4043000004000A000200020055000200000026001D1C7E0289AC7CF0007E00412B000BF299F907020040C000041A2E0280400079400F4099F907000000000099F907000001'O
}
09:30:24.953159 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044048000004000A000200020055000200000026002F2E7E02280ED712037E0042010177000BF299F907020040C00002CB54074099F90700000115020101210201005E0192000000020001'O
} id 7
09:30:24.953348 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02280ED712037E0042010177000BF299F907020040C00002CB54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:30:24.953439 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:24.953478 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02280ED712037E0042010177000BF299F907020040C00002CB54074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:30:24.953505 14060 NGAP_Emulation.ttcn:548 Message with id 7 was extracted from the queue of NGAP.
09:30:24.953539 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02280ED712037E0042010177000BF299F907020040C00002CB54074099F90700000115020101210201005E0192'O
09:30:24.953587 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '280ED712'O,
        sequenceNumber := '03'O,
        plainNASMessage := '7E0042010177000BF299F907020040C00002CB54074099F90700000115020101210201005E0192'O
    }
}
09:30:24.953950 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C00002CB54074099F90700000115020101210201005E0192'O
09:30:24.954123 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:24.954283 14060 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:30:24.954460 14061 ConnHdlr.ttcn:589 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:30:24.954671 14061 ConnHdlr.ttcn:589 Matching on port NGAP succeeded:  matched
09:30:24.954726 14061 ConnHdlr.ttcn:589 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:30:24.954763 14061 ConnHdlr.ttcn:589 Message with id 5 was extracted from the queue of NGAP.
09:30:24.954818 14061 ConnHdlr.ttcn:591 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:24.954872 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:30:24.954914 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.954938 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.954958 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.954978 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.955007 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.955036 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.955063 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:30:24.955086 14060 NGAP_Emulation.ttcn:522 Message with id 10 was extracted from the queue of NGAP_CLIENT.
09:30:24.955124 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:30:24.955158 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:30:24.955478 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '6BABA7B7'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:30:24.955531 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E026BABA7B7007E0043'O
09:30:24.955672 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E026BABA7B7007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.955753 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E026BABA7B7007E00430079400F4099F907000000000099F907000001'O
}
09:30:24.956148 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E0236B4A979047E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
} id 8
09:30:24.956235 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0236B4A979047E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:24.956287 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:24.956320 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0236B4A979047E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:24.956344 14060 NGAP_Emulation.ttcn:548 Message with id 8 was extracted from the queue of NGAP.
09:30:24.956376 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0236B4A979047E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
09:30:24.956411 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '36B4A979'O,
        sequenceNumber := '04'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
    }
}
09:30:24.956719 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752017190034200490100'O
09:30:24.956824 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:24.956897 14060 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:30:24.956983 14061 ConnHdlr.ttcn:593 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:30:24.957102 14061 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:30:24.957141 14061 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '01'O,
            day := '71'O ("q"),
            hour := '90'O,
            minute := '03'O,
            second := '42'O ("B"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:30:24.957169 14061 ConnHdlr.ttcn:279 Message with id 6 was extracted from the queue of NGAP.
09:30:24.957203 14061 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:24.957255 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:30:24.957301 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.957332 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.957354 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.957374 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.957407 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.957434 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.957457 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:30:24.957480 14060 NGAP_Emulation.ttcn:522 Message with id 11 was extracted from the queue of NGAP_CLIENT.
09:30:24.957510 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:30:24.957525 14061 ConnHdlr.ttcn:607 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        }
    }
}
09:30:24.957542 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:30:24.957873 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '37EEB1D3'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:30:24.957906 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0237EEB1D3007E0055'O
09:30:24.957999 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0237EEB1D3007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.958063 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E0237EEB1D3007E00550079400F4099F907000000000099F907000001'O
}
09:30:24.958209 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        }
    }
} id 12
09:30:24.958272 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.958300 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.958321 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.958340 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:24.958369 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:30:24.958397 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:30:24.958423 14060 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        }
    }
} id 12
09:30:24.958448 14060 NGAP_Emulation.ttcn:522 Message with id 12 was extracted from the queue of NGAP_CLIENT.
09:30:24.958476 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C00002CB'O
        }
    }
}
09:30:24.958529 14060 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004531000BF299F907020040C00002CB'O
09:30:24.958863 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '736811B1'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E004531000BF299F907020040C00002CB'O
    }
}
09:30:24.958894 14060 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02736811B1007E004531000BF299F907020040C00002CB'O
09:30:24.958977 14060 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02736811B1007E004531000BF299F907020040C00002CB'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:24.959054 14060 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403F000004000A0002000200550002000000260019187E02736811B1007E004531000BF299F907020040C00002CB0079400F4099F907000000000099F907000001'O
}
09:30:25.165148 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004401E000003000A000200020055000200000026000B0A7E02B01A5096057E0046'O
} id 9
09:30:25.165498 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02B01A5096057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:30:25.165601 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:25.165637 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02B01A5096057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:30:25.165664 14060 NGAP_Emulation.ttcn:548 Message with id 9 was extracted from the queue of NGAP.
09:30:25.165699 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02B01A5096057E0046'O
09:30:25.165737 14060 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'B01A5096'O,
        sequenceNumber := '05'O,
        plainNASMessage := '7E0046'O
    }
}
09:30:25.166052 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0046'O
09:30:25.166099 14060 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:30:25.166150 14060 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:30:25.166243 14061 ConnHdlr.ttcn:609 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:30:25.166269 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '002900100000020072000400020000000F400148'O
} id 10
09:30:25.166338 14061 ConnHdlr.ttcn:609 Matching on port NGAP succeeded:  matched
09:30:25.166367 14061 ConnHdlr.ttcn:609 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:30:25.166390 14061 ConnHdlr.ttcn:609 Message with id 7 was extracted from the queue of NGAP.
09:30:25.166822 14060 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:30:25.166885 14060 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:30:25.166915 14060 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:30:25.166943 14060 NGAP_Emulation.ttcn:548 Message with id 10 was extracted from the queue of NGAP.
09:30:25.167032 14060 NGAP_Emulation.ttcn:587 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:25.167713 14061 ConnHdlr.ttcn:610 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:25.168135 14061 ConnHdlr.ttcn:623 Matching on port NGAP succeeded:  matched
09:30:25.168170 14061 ConnHdlr.ttcn:623 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:30:25.168193 14061 ConnHdlr.ttcn:623 Message with id 8 was extracted from the queue of NGAP.
09:30:25.169244 14061 ConnHdlr.ttcn:624 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:25.169453 14061 - Function f_init_handler finished. PTC terminates.
09:30:25.169481 14061 - Terminating component type ConnHdlr.ConnHdlr.
09:30:25.169500 14061 - Removing unterminated connection between port NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:30:25.169538 14061 - Port NGAP was stopped.
09:30:25.169539 14060 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:30:25.169560 14061 - Removing unterminated connection between port NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:25.169588 14061 - Port NGAP_PROC was stopped.
09:30:25.169608 14061 - Removing unterminated connection between port GTP1U[0] and GTP1U_EM(12):CLIENT.
09:30:25.169620 14060 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:25.169634 14061 - Port GTP1U[0] was stopped.
09:30:25.169646 14060 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:25.169653 14061 - Port GTP1U[1] was stopped.
09:30:25.169657 14059 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT to TC_periodic_registration_updating0(14):GTP1U[0] was closed unexpectedly by the peer.
09:30:25.169666 14060 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:25.169671 14061 - Port GTP1U[2] was stopped.
09:30:25.169687 14060 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:30:25.169689 14061 - Port GTP1U[3] was stopped.
09:30:25.169704 14059 GTPv1U_Emulation.ttcnpp:265 Port CLIENT was disconnected from TC_periodic_registration_updating0(14):GTP1U[0].
09:30:25.169707 14061 - Removing unterminated connection between port GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:30:25.169739 14061 - Port GTP1U_PROC[0] was stopped.
09:30:25.169781 14059 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT_PROC to TC_periodic_registration_updating0(14):GTP1U_PROC[0] was closed unexpectedly by the peer.
09:30:25.169784 14061 - Port GTP1U_PROC[1] was stopped.
09:30:25.169802 14061 - Port GTP1U_PROC[2] was stopped.
09:30:25.169812 14059 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC was disconnected from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:30:25.169819 14061 - Port GTP1U_PROC[3] was stopped.
09:30:25.169837 14061 - Component type ConnHdlr.ConnHdlr was shut down inside testcase TC_periodic_registration_updating.
09:30:25.169867 14061 - Final verdict of PTC: none
09:30:25.169902 13825 C5G_Tests.ttcn:331 PTC with component reference 14 is done.
09:30:25.169933 14061 - Disconnected from MC.
09:30:25.169955 14061 - TTCN-3 Parallel Test Component finished.
09:30:25.169960 13825 C5G_Tests.ttcn:331 Terminating component type C5G_Tests.MTC_CT.
09:30:25.169967 14060 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := ?
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:30:25.169986 13825 C5G_Tests.ttcn:331 Default with id 1 (altstep as_Tguard) was deactivated.
09:30:25.170008 14060 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type.
09:30:25.170009 13825 C5G_Tests.ttcn:331 Stop timer g_Tguard: 30 s
09:30:25.170033 14060 NGAP_Emulation.ttcn:535 Matching on port NGAP_CLIENT succeeded:  matched
09:30:25.170035 13825 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_UNIT[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:30:25.170062 14060 NGAP_Emulation.ttcn:535 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:30:25.170079 13825 C5G_Tests.ttcn:331 Port NGAP_UNIT[0] was stopped.
09:30:25.170091 14060 NGAP_Emulation.ttcn:535 Message with id 13 was extracted from the queue of NGAP_CLIENT.
09:30:25.170103 13825 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_PROC[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:30:25.170138 13825 C5G_Tests.ttcn:331 Port NGAP_PROC[0] was stopped.
09:30:25.170163 13825 C5G_Tests.ttcn:331 Removing unterminated connection between port TEID0 and GTP1U_EM(12):TEID0.
09:30:25.170198 13825 C5G_Tests.ttcn:331 Port TEID0 was stopped.
09:30:25.170210 14059 GTPv1U_Emulation.ttcnpp:265 Connection of port TEID0 to mtc:TEID0 was closed unexpectedly by the peer.
09:30:25.170221 13825 C5G_Tests.ttcn:331 Component type C5G_Tests.MTC_CT was shut down inside testcase TC_periodic_registration_updating.
09:30:25.170241 14059 GTPv1U_Emulation.ttcnpp:265 Port TEID0 was disconnected from mtc:TEID0.
09:30:25.170245 13825 C5G_Tests.ttcn:331 Waiting for PTCs to finish.
09:30:25.170292 14059 GTPv1U_Emulation.ttcnpp:265 Kill was requested from MC.
09:30:25.170317 14059 GTPv1U_Emulation.ttcnpp:265 Terminating test component execution.
09:30:25.170674 14060 NGAP_Emulation.ttcn:538 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        successfulOutcome := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseComplete := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := ignore (1),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := ignore (1),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:30:25.170745 14059 - Function main was stopped. PTC terminates.
09:30:25.170795 14059 - Terminating component type GTPv1U_Emulation.GTPv1U_Emulation_CT.
09:30:25.170812 14060 NGAP_Emulation.ttcn:538 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '20290022000003000A400200020055400200000079400F4099F907000000000099F907000001'O
}
09:30:25.170838 14059 - Default with id 1 (altstep as_uecups_ind) was deactivated.
09:30:25.170871 14059 - Removing unterminated mapping between port GTP1U and system:GTP1U.
09:30:25.170917 14059 - Port GTP1U was unmapped from system:GTP1U.
09:30:25.170958 14059 - Port GTP1U was stopped.
09:30:25.170979 14059 - Port TEID0 was stopped.
09:30:25.170995 14059 - Port CLIENT was stopped.
09:30:25.171011 14060 NGAP_Emulation.ttcn:485 Connection of port NGAP_CLIENT to TC_periodic_registration_updating0(14):NGAP was closed unexpectedly by the peer.
09:30:25.171012 14059 - Port CLIENT_PROC was stopped.
09:30:25.171029 14059 - Removing unterminated mapping between port UECUPS and system:UECUPS.
09:30:25.171040 14060 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT was disconnected from TC_periodic_registration_updating0(14):NGAP.
09:30:25.171082 14060 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to TC_periodic_registration_updating0(14):NGAP_PROC was closed unexpectedly by the peer.
09:30:25.171104 14060 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from TC_periodic_registration_updating0(14):NGAP_PROC.
09:30:25.171138 14060 NGAP_Emulation.ttcn:485 Connection of port NGAP_UNIT to mtc:NGAP_UNIT[0] was closed unexpectedly by the peer.
09:30:25.171164 14060 NGAP_Emulation.ttcn:485 Port NGAP_UNIT was disconnected from mtc:NGAP_UNIT[0].
09:30:25.171245 14060 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to mtc:NGAP_PROC[0] was closed unexpectedly by the peer.
09:30:25.171271 14060 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from mtc:NGAP_PROC[0].
09:30:25.171298 14059 - Port UECUPS was unmapped from system:UECUPS.
09:30:25.171303 14060 NGAP_Emulation.ttcn:485 Kill was requested from MC.
09:30:25.171324 14060 NGAP_Emulation.ttcn:485 Terminating test component execution.
09:30:25.171327 14059 - Port UECUPS was stopped.
09:30:25.171344 14059 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:30:25.171368 14059 - Final verdict of PTC: none
09:30:25.171425 14059 - Disconnected from MC.
09:30:25.171448 14059 - TTCN-3 Parallel Test Component finished.
09:30:25.171647 14060 - Function main was stopped. PTC terminates.
09:30:25.171704 14060 - Terminating component type NGAP_Emulation.NGAP_Emulation_CT.
09:30:25.171727 14060 - Removing unterminated mapping between port NGAP and system:NGAP_CODEC_PT.
09:30:25.171964 14060 - Port NGAP was unmapped from system:NGAP_CODEC_PT.
09:30:25.172003 14060 - Port NGAP was stopped.
09:30:25.172024 14060 - Port NGAP_CLIENT was stopped.
09:30:25.172044 14060 - Port NGAP_PROC was stopped.
09:30:25.172063 14060 - Port NGAP_UNIT was stopped.
09:30:25.172082 14060 - Component type NGAP_Emulation.NGAP_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:30:25.172109 14060 - Final verdict of PTC: none
09:30:25.172165 14060 - Disconnected from MC.
09:30:25.172173 13825 C5G_Tests.ttcn:331 Setting final verdict of the test case.
09:30:25.172190 14060 - TTCN-3 Parallel Test Component finished.
09:30:25.172212 13825 C5G_Tests.ttcn:331 Local verdict of MTC: pass
09:30:25.172242 13825 C5G_Tests.ttcn:331 Local verdict of PTC GTP1U_EM(12): none (pass -> pass)
09:30:25.172331 13825 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating-NGAP0(13): none (pass -> pass)
09:30:25.172367 13825 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating0(14): none (pass -> pass)
09:30:25.172400 13825 C5G_Tests.ttcn:331 Test case TC_periodic_registration_updating finished. Verdict: pass
09:30:25.172436 13825 C5G_Tests.ttcn:331 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass'.
09:30:27.196131 13825 C5G_Tests.ttcn:331 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass' was executed successfully (exit status: 0).
09:30:27.196233 13825 C5G_Tests.ttcn:339 Switching to log file `C5G_Tests-TC_ue_context_release_no_pdu_session-e15dac43427e-mtc-13825.log'
