09:29:55.870671 13795 C5G_Tests.ttcn:324 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating'.
09:29:56.903115 13795 C5G_Tests.ttcn:324 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-start.sh C5G_Tests.TC_periodic_registration_updating' was executed successfully (exit status: 0).
09:29:56.903382 13795 C5G_Tests.ttcn:324 Test case TC_periodic_registration_updating started.
09:29:56.903550 13795 C5G_Tests.ttcn:324 Initializing variables, timers and ports of component type C5G_Tests.MTC_CT inside testcase TC_periodic_registration_updating.
09:29:56.903743 13795 C5G_Tests.ttcn:324 Port NGAP_UNIT[0] was started.
09:29:56.903911 13795 C5G_Tests.ttcn:324 Port NGAP_PROC[0] was started.
09:29:56.903978 13795 C5G_Tests.ttcn:324 Port TEID0 was started.
09:29:56.904169 13795 C5G_Tests.ttcn:324 Component type C5G_Tests.MTC_CT was initialized.
09:29:56.904234 13795 C5G_Tests.ttcn:191 Start timer g_Tguard: 30 s
09:29:56.904298 13795 C5G_Tests.ttcn:192 Altstep as_Tguard was activated as default, id 1
09:29:56.904363 13795 C5G_Tests.ttcn:183 Creating new PTC with component type GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:29:56.913055 14030 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:29:56.913256 14030 - TTCN-3 Parallel Test Component started on 3c561e6ea320. Component reference: GTP1U_EM(12), component type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM. Version: 11.1.0.
09:29:56.913370 14030 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:29:56.913563 14030 - Connected to MC.
09:29:56.913878 14030 - Initializing variables, timers and ports of component type GTPv1U_Emulation.GTPv1U_Emulation_CT inside testcase TC_periodic_registration_updating.
09:29:56.913928 13795 C5G_Tests.ttcn:183 PTC was created. Component reference: 12, alive: no, type: GTPv1U_Emulation.GTPv1U_Emulation_CT, component name: GTP1U_EM.
09:29:56.914091 13795 C5G_Tests.ttcn:184 Mapping port GTP1U_EM(12):GTP1U to system:GTP1U.
09:29:56.917633 14030 - Port GTP1U was started.
09:29:56.917964 14030 - Port TEID0 was started.
09:29:56.918270 14030 - Port CLIENT was started.
09:29:56.918571 14030 - Port CLIENT_PROC was started.
09:29:56.918875 14030 - Port UECUPS was started.
09:29:56.919177 14030 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was initialized.
09:29:56.919490 14030 - Port GTP1U was mapped to system:GTP1U.
09:29:56.919626 13795 C5G_Tests.ttcn:184 Map operation of GTP1U_EM(12):GTP1U to system:GTP1U finished.
09:29:56.919687 13795 C5G_Tests.ttcn:185 Connecting ports GTP1U_EM(12):TEID0 and mtc:TEID0.
09:29:56.920340 13795 C5G_Tests.ttcn:185 Port TEID0 is waiting for connection from GTP1U_EM(12):TEID0 on UNIX pathname /tmp/ttcn3-portconn-656ca674.
09:29:56.920475 14030 - Port TEID0 has established the connection with mtc:TEID0 using transport type UNIX.
09:29:56.920571 13795 C5G_Tests.ttcn:185 Port TEID0 has accepted the connection from GTP1U_EM(12):TEID0.
09:29:56.920651 13795 C5G_Tests.ttcn:185 Connect operation on GTP1U_EM(12):TEID0 and mtc:TEID0 finished.
09:29:56.920709 13795 C5G_Tests.ttcn:186 Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}) on component GTP1U_EM(12).
09:29:56.920821 13795 C5G_Tests.ttcn:186 Function was started.
09:29:56.921070 13795 C5G_Tests.ttcn:161 Creating new PTC with component type NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:29:56.921146 14030 - Starting function main({
    gtpu_bind_ip := omit,
    gtpu_bind_port := omit,
    use_gtpu_daemon := true
}).
09:29:56.921905 14030 Osmocom_Types.ttcn:65 Random number generator was initialized with seed 13.921897: srand48(1167383225).
09:29:56.921993 14030 Osmocom_Types.ttcn:65 Function rnd() returned 0.598308.
09:29:56.922196 14030 Osmocom_Types.ttcn:65 Function rnd() returned 0.202919.
09:29:56.922457 14030 GTPv1U_Emulation.ttcnpp:214 Mapping port GTP1U_EM(12):UECUPS to system:UECUPS.
09:29:56.922567 14030 GTPv1U_Emulation.ttcnpp:214 Port UECUPS was mapped to system:UECUPS.
09:29:56.922670 14030 GTPv1U_Emulation.ttcnpp:214 Map operation of GTP1U_EM(12):UECUPS to system:UECUPS finished.
09:29:56.923483 14030 GTPv1U_Emulation.ttcnpp:215 entering f__IPL4__PROVIDER__connect: :-1 -> 127.0.0.20:4268 / SCTP
09:29:56.924089 14030 GTPv1U_Emulation.ttcnpp:215 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:29:56.926987 14030 GTPv1U_Emulation.ttcnpp:190 Sent on UECUPS to system @UECUPS_CodecPort.UECUPS_Send : {
    connId := 1,
    msg := {
        reset_all_state := { }
    }
}
09:29:56.927301 14030 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Encoding @UECUPS_Types.PDU_UECUPS: {
    reset_all_state := { }
}
09:29:56.927578 14030 UECUPS_CodecPort.ttcn:56 f_enc_PDU_UECUPS(): Stream after encoding: '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
09:29:56.927883 14030 GTPv1U_Emulation.ttcnpp:190 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := <unbound>,
    msg := '7B2272657365745F616C6C5F7374617465223A7B7D7D'O ("{\"reset_all_state\":{}}")
}
09:29:56.928382 14030 GTPv1U_Emulation.ttcnpp:191 Start timer T: 30 s
09:29:56.928950 14031 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:29:56.929097 14031 - TTCN-3 Parallel Test Component started on 3c561e6ea320. Component reference: TC_periodic_registration_updating-NGAP0(13), component type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0. Version: 11.1.0.
09:29:56.929170 14031 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:29:56.929328 14031 - Connected to MC.
09:29:56.929385 14031 - Initializing variables, timers and ports of component type NGAP_Emulation.NGAP_Emulation_CT inside testcase TC_periodic_registration_updating.
09:29:56.929447 14030 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:56.929452 13795 C5G_Tests.ttcn:161 PTC was created. Component reference: 13, alive: no, type: NGAP_Emulation.NGAP_Emulation_CT, component name: TC_periodic_registration_updating-NGAP0.
09:29:56.929581 13795 C5G_Tests.ttcn:162 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:29:56.929774 14030 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS failed: Type of the first message in the queue is not @UECUPS_CodecPort.UECUPS_RecvFrom.
09:29:56.929968 14030 GTPv1U_Emulation.ttcnpp:194 Matching on port UECUPS succeeded:  matched
09:29:56.930065 14030 GTPv1U_Emulation.ttcnpp:194 Receive operation on port UECUPS succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:56.930130 14030 GTPv1U_Emulation.ttcnpp:194 Message with id 1 was extracted from the queue of UECUPS.
09:29:56.930384 14030 GTPv1U_Emulation.ttcnpp:192 Message enqueued on UECUPS from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 0,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
} id 2
09:29:56.930509 14030 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Stream before decoding: '7B2272657365745F616C6C5F73746174655F726573223A207B22726573756C74223A20224F4B227D7D'O ("{\"reset_all_state_res\": {\"result\": \"OK\"}}")
09:29:56.930769 14030 UECUPS_CodecPort.ttcn:50 f_dec_PDU_UECUPS(): Decoded @UECUPS_Types.PDU_UECUPS: {
    reset_all_state_res := {
        result := OK (1)
    }
}
09:29:56.930899 14030 GTPv1U_Emulation.ttcnpp:192 Incoming message was mapped to @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:29:56.931067 14030 GTPv1U_Emulation.ttcnpp:193 Matching on port UECUPS succeeded:  matched
09:29:56.931127 14030 GTPv1U_Emulation.ttcnpp:193 Receive operation on port UECUPS succeeded, message from system(): @UECUPS_CodecPort.UECUPS_RecvFrom : {
    connId := 1,
    remName := "127.0.0.20",
    remPort := 4268,
    locName := "127.0.0.1",
    locPort := 9999,
    msg := {
        reset_all_state_res := {
            result := OK (1)
        }
    }
} id 2
09:29:56.931177 14030 GTPv1U_Emulation.ttcnpp:193 Message with id 2 was extracted from the queue of UECUPS.
09:29:56.931298 14030 GTPv1U_Emulation.ttcnpp:225 Altstep as_uecups_ind was activated as default, id 1
09:29:56.932472 14031 - Port NGAP was started.
09:29:56.932539 14031 - Port NGAP_CLIENT was started.
09:29:56.932576 14031 - Port NGAP_PROC was started.
09:29:56.932611 14031 - Port NGAP_UNIT was started.
09:29:56.932652 14031 - Component type NGAP_Emulation.NGAP_Emulation_CT was initialized.
09:29:56.932748 14031 - Port NGAP was mapped to system:NGAP_CODEC_PT.
09:29:56.932841 13795 C5G_Tests.ttcn:162 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:29:56.932888 13795 C5G_Tests.ttcn:163 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0].
09:29:56.933219 13795 C5G_Tests.ttcn:163 Port NGAP_PROC[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-5454f519.
09:29:56.933461 14031 - Port NGAP_PROC has established the connection with mtc:NGAP_PROC[0] using transport type UNIX.
09:29:56.933560 13795 C5G_Tests.ttcn:163 Port NGAP_PROC[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:56.933615 13795 C5G_Tests.ttcn:163 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_PROC and mtc:NGAP_PROC[0] finished.
09:29:56.933661 13795 C5G_Tests.ttcn:164 Connecting ports TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0].
09:29:56.934046 13795 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] is waiting for connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT on UNIX pathname /tmp/ttcn3-portconn-454dec08.
09:29:56.934256 14031 - Port NGAP_UNIT has established the connection with mtc:NGAP_UNIT[0] using transport type UNIX.
09:29:56.934317 13795 C5G_Tests.ttcn:164 Port NGAP_UNIT[0] has accepted the connection from TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:29:56.934373 13795 C5G_Tests.ttcn:164 Connect operation on TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT and mtc:NGAP_UNIT[0] finished.
09:29:56.934421 13795 C5G_Tests.ttcn:165 Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0") on component TC_periodic_registration_updating-NGAP0(13).
09:29:56.934584 13795 C5G_Tests.ttcn:165 Function was started.
09:29:56.934858 14031 - Starting function main({
    create_cb := refers(NGAP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(C5G_Tests.NGapForwardUnitdataCallback)
}, {
    remote_ip := "127.0.0.5",
    remote_sctp_port := 38412,
    local_ip := "127.0.0.202",
    local_sctp_port := 50000,
    role := NG_NAS_ROLE_UE (0)
}, "TC_periodic_registration_updating-NGAP0").
09:29:56.936990 14031 NGAP_Emulation.ttcn:452 Mapping port TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT.
09:29:56.937141 14031 NGAP_Emulation.ttcn:452 Map operation of TC_periodic_registration_updating-NGAP0(13):NGAP to system:NGAP_CODEC_PT finished.
09:29:56.937968 14031 NGAP_Emulation.ttcn:457 entering f__IPL4__PROVIDER__connect: 127.0.0.202:50000 -> 127.0.0.5:38412 / SCTP
09:29:56.938536 14031 NGAP_Emulation.ttcn:457 Warning: sizes of 'struct sctp_event_subscribe': compile-time 14, kernel: 14
09:29:56.940765 14031 NGAP_Emulation.ttcn:469 Sent on NGAP_UNIT to mtc @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
}
09:29:56.940978 13795 C5G_Tests.ttcn:166 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:29:56.941065 13795 C5G_Tests.ttcn:166 Matching on port NGAP_UNIT[0] succeeded:  matched
09:29:56.941122 13795 C5G_Tests.ttcn:166 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_Event : {
    up_down := NGAPEM_EVENT_UP (1)
} id 1
09:29:56.941179 13795 C5G_Tests.ttcn:166 Message with id 1 was extracted from the queue of NGAP_UNIT[0].
09:29:56.941655 13795 C5G_Tests.ttcn:268 Sent on NGAP_UNIT[0] to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
}
09:29:56.941763 13795 C5G_Tests.ttcn:269 Start timer T: 5 s
09:29:56.943784 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:56.946034 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_UNIT from mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:56.946334 14031 NGAP_Emulation.ttcn:542 Matching on port NGAP_UNIT succeeded:  matched
09:29:56.946396 14031 NGAP_Emulation.ttcn:542 Receive operation on port NGAP_UNIT succeeded, message from mtc: @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupRequest := {
                protocolIEs := {
                    {
                        id := 27,
                        criticality := reject (0),
                        value_ := {
                            globalRANNodeID := {
                                globalGNB_ID := {
                                    pLMNIdentity := '99F907'O,
                                    gNB_ID := {
                                        gNB_ID := '0000000000000000000000'B
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 102,
                        criticality := reject (0),
                        value_ := {
                            supportedTAList := {
                                {
                                    tAC := '000001'O,
                                    broadcastPLMNList := {
                                        {
                                            pLMNIdentity := '99F907'O,
                                            tAISliceSupportList := {
                                                {
                                                    s_NSSAI := {
                                                        sST := '01'O,
                                                        sD := omit,
                                                        iE_Extensions := omit
                                                    },
                                                    iE_Extensions := omit
                                                }
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 21,
                        criticality := ignore (1),
                        value_ := {
                            pagingDRX := v32 (0)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:56.946429 14031 NGAP_Emulation.ttcn:542 Message with id 1 was extracted from the queue of NGAP_UNIT.
09:29:56.948724 14031 NGAP_Emulation.ttcn:544 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupRequest := {
                    protocolIEs := {
                        {
                            id := 27,
                            criticality := reject (0),
                            value_ := {
                                globalRANNodeID := {
                                    globalGNB_ID := {
                                        pLMNIdentity := '99F907'O,
                                        gNB_ID := {
                                            gNB_ID := '0000000000000000000000'B
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 102,
                            criticality := reject (0),
                            value_ := {
                                supportedTAList := {
                                    {
                                        tAC := '000001'O,
                                        broadcastPLMNList := {
                                            {
                                                pLMNIdentity := '99F907'O,
                                                tAISliceSupportList := {
                                                    {
                                                        s_NSSAI := {
                                                            sST := '01'O,
                                                            sD := omit,
                                                            iE_Extensions := omit
                                                        },
                                                        iE_Extensions := omit
                                                    }
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 21,
                            criticality := ignore (1),
                            value_ := {
                                pagingDRX := v32 (0)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:56.949354 14031 NGAP_Emulation.ttcn:544 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '00150025000003001B00080099F907000000000066000D00000000010099F907000000080015400100'O
}
09:29:56.949742 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP failed: Type of the first message in the queue is not @NGAP_CodecPort.NGAP_RecvFrom.
09:29:56.949797 14031 NGAP_Emulation.ttcn:600 Matching on port NGAP succeeded:  matched
09:29:56.949817 14031 NGAP_Emulation.ttcn:600 Receive operation on port NGAP succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    sctpEvent := {
        sctpAssocChange := {
            clientId := 1,
            proto := {
                sctp := {
                    sinfo_stream := omit,
                    sinfo_ppid := omit,
                    remSocks := omit,
                    assocId := omit
                }
            },
            sac_state := SCTP_COMM_UP (0)
        }
    }
} id 1
09:29:56.949831 14031 NGAP_Emulation.ttcn:600 Message with id 1 was extracted from the queue of NGAP.
09:29:56.949892 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 0,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '201500320000040001000E05806F70656E3567732D616D663000600008000099F90702004000564001FF005000080099F90700000008'O
} id 2
09:29:56.950778 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:56.950830 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:56.950848 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        successfulOutcome := {
            procedureCode := 21,
            criticality := reject (0),
            value_ := {
                nGSetupResponse := {
                    protocolIEs := {
                        {
                            id := 1,
                            criticality := reject (0),
                            value_ := {
                                aMFName := "open5gs-amf0"
                            }
                        },
                        {
                            id := 96,
                            criticality := reject (0),
                            value_ := {
                                servedGUAMIList := {
                                    {
                                        gUAMI := {
                                            pLMNIdentity := '99F907'O,
                                            aMFRegionID := '00000010'B,
                                            aMFSetID := '0000000001'B,
                                            aMFPointer := '000000'B,
                                            iE_Extensions := omit
                                        },
                                        backupAMFName := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 86,
                            criticality := ignore (1),
                            value_ := {
                                relativeAMFCapacity := 255
                            }
                        },
                        {
                            id := 80,
                            criticality := reject (0),
                            value_ := {
                                pLMNSupportList := {
                                    {
                                        pLMNIdentity := '99F907'O,
                                        sliceSupportList := {
                                            {
                                                s_NSSAI := {
                                                    sST := '01'O,
                                                    sD := omit,
                                                    iE_Extensions := omit
                                                },
                                                iE_Extensions := omit
                                            }
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:56.950862 14031 NGAP_Emulation.ttcn:548 Message with id 2 was extracted from the queue of NGAP.
09:29:56.950926 14031 C5G_Tests.ttcn:128 Sent on NGAP_UNIT to mtc @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:56.951127 13795 C5G_Tests.ttcn:270 Message enqueued on NGAP_UNIT[0] from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:56.951157 13795 C5G_Tests.ttcn:271 Matching on port NGAP_UNIT[0] succeeded:  matched
09:29:56.951172 13795 C5G_Tests.ttcn:271 Receive operation on port NGAP_UNIT[0] succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 21,
        criticality := reject (0),
        value_ := {
            nGSetupResponse := {
                protocolIEs := {
                    {
                        id := 1,
                        criticality := reject (0),
                        value_ := {
                            aMFName := "open5gs-amf0"
                        }
                    },
                    {
                        id := 96,
                        criticality := reject (0),
                        value_ := {
                            servedGUAMIList := {
                                {
                                    gUAMI := {
                                        pLMNIdentity := '99F907'O,
                                        aMFRegionID := '00000010'B,
                                        aMFSetID := '0000000001'B,
                                        aMFPointer := '000000'B,
                                        iE_Extensions := omit
                                    },
                                    backupAMFName := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 86,
                        criticality := ignore (1),
                        value_ := {
                            relativeAMFCapacity := 255
                        }
                    },
                    {
                        id := 80,
                        criticality := reject (0),
                        value_ := {
                            pLMNSupportList := {
                                {
                                    pLMNIdentity := '99F907'O,
                                    sliceSupportList := {
                                        {
                                            s_NSSAI := {
                                                sST := '01'O,
                                                sD := omit,
                                                iE_Extensions := omit
                                            },
                                            iE_Extensions := omit
                                        }
                                    },
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 2
09:29:56.951187 13795 C5G_Tests.ttcn:271 Message with id 2 was extracted from the queue of NGAP_UNIT[0].
09:29:56.951197 13795 C5G_Tests.ttcn:272 setverdict(pass): none -> pass
09:29:56.951235 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.739359.
09:29:56.951261 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.510015.
09:29:56.951272 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.010588.
09:29:56.951284 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.282724.
09:29:56.951309 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.559766.
09:29:56.951320 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.222176.
09:29:56.951329 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.218997.
09:29:56.951338 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.715736.
09:29:56.951347 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.709858.
09:29:56.951356 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.824716.
09:29:56.951365 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.780469.
09:29:56.951374 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.103797.
09:29:56.951384 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.052122.
09:29:56.951393 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.338791.
09:29:56.951402 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.770103.
09:29:56.951411 13795 Osmocom_Types.ttcn:65 Function rnd() returned 0.186815.
09:29:56.951443 13795 C5G_Tests.ttcn:216 Creating new PTC with component type ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:29:56.953118 14032 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:29:56.953145 14032 - TTCN-3 Parallel Test Component started on 3c561e6ea320. Component reference: TC_periodic_registration_updating0(14), component type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0. Version: 11.1.0.
09:29:56.953157 14032 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:29:56.953192 14032 - Connected to MC.
09:29:56.953203 14032 - Initializing variables, timers and ports of component type ConnHdlr.ConnHdlr inside testcase TC_periodic_registration_updating.
09:29:56.953217 13795 C5G_Tests.ttcn:216 PTC was created. Component reference: 14, alive: no, type: ConnHdlr.ConnHdlr, component name: TC_periodic_registration_updating0.
09:29:56.953230 13795 C5G_Tests.ttcn:218 Connecting ports TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:29:56.953325 14031 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT is waiting for connection from TC_periodic_registration_updating0(14):NGAP on UNIX pathname /tmp/ttcn3-portconn-3c7da15c.
09:29:56.953986 14032 - Port NGAP was started.
09:29:56.954077 14032 - Port NGAP_PROC was started.
09:29:56.954094 14032 - Port GTP1U[0] was started.
09:29:56.954108 14032 - Port GTP1U[1] was started.
09:29:56.954119 14032 - Port GTP1U[2] was started.
09:29:56.954187 14032 - Port GTP1U[3] was started.
09:29:56.954201 14032 - Port GTP1U_PROC[0] was started.
09:29:56.954269 14032 - Port GTP1U_PROC[1] was started.
09:29:56.954280 14032 - Port GTP1U_PROC[2] was started.
09:29:56.954290 14032 - Port GTP1U_PROC[3] was started.
09:29:56.954301 14032 - Component type ConnHdlr.ConnHdlr was initialized.
09:29:56.954336 14032 - Port NGAP has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT using transport type UNIX.
09:29:56.954381 14031 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT has accepted the connection from TC_periodic_registration_updating0(14):NGAP.
09:29:56.954388 13795 C5G_Tests.ttcn:218 Connect operation on TC_periodic_registration_updating0(14):NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT finished.
09:29:56.954399 13795 C5G_Tests.ttcn:219 Connecting ports TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:56.954543 14031 NGAP_Emulation.ttcn:485 Port NGAP_PROC is waiting for connection from TC_periodic_registration_updating0(14):NGAP_PROC on UNIX pathname /tmp/ttcn3-portconn-2667ae15.
09:29:56.954563 14032 - Port NGAP_PROC has established the connection with TC_periodic_registration_updating-NGAP0(13):NGAP_PROC using transport type UNIX.
09:29:56.954590 14031 NGAP_Emulation.ttcn:485 Port NGAP_PROC has accepted the connection from TC_periodic_registration_updating0(14):NGAP_PROC.
09:29:56.954596 13795 C5G_Tests.ttcn:219 Connect operation on TC_periodic_registration_updating0(14):NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC finished.
09:29:56.954605 13795 C5G_Tests.ttcn:222 Connecting ports TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT.
09:29:56.954908 14030 GTPv1U_Emulation.ttcnpp:265 Port CLIENT is waiting for connection from TC_periodic_registration_updating0(14):GTP1U[0] on UNIX pathname /tmp/ttcn3-portconn-3d25d238.
09:29:56.954929 14032 - Port GTP1U[0] has established the connection with GTP1U_EM(12):CLIENT using transport type UNIX.
09:29:56.955049 14030 GTPv1U_Emulation.ttcnpp:265 Port CLIENT has accepted the connection from TC_periodic_registration_updating0(14):GTP1U[0].
09:29:56.955054 13795 C5G_Tests.ttcn:222 Connect operation on TC_periodic_registration_updating0(14):GTP1U[0] and GTP1U_EM(12):CLIENT finished.
09:29:56.955070 13795 C5G_Tests.ttcn:223 Connecting ports TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:29:56.955203 14030 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC is waiting for connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-7f7ea655.
09:29:56.955222 14032 - Port GTP1U_PROC[0] has established the connection with GTP1U_EM(12):CLIENT_PROC using transport type UNIX.
09:29:56.955246 14030 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC has accepted the connection from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:29:56.955252 13795 C5G_Tests.ttcn:223 Connect operation on TC_periodic_registration_updating0(14):GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC finished.
09:29:56.955262 13795 C5G_Tests.ttcn:227 Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '7502522778710371'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}) on component TC_periodic_registration_updating0(14).
09:29:56.955309 13795 C5G_Tests.ttcn:227 Function was started.
09:29:56.955818 14032 - Starting function f_init_handler(refers(C5G_Tests.f_TC_periodic_registration_updating), {
    ngran_pars := {
        {
            global_ngran_id := {
                globalGNB_ID := {
                    pLMNIdentity := '99F907'O,
                    gNB_ID := {
                        gNB_ID := '0000000000000000000000'B
                    },
                    iE_Extensions := omit
                }
            },
            cell_identity := {
                nR_CGI := {
                    pLMNIdentity := '99F907'O,
                    nRCellIdentity := '000000000000000000000000000000000000'B,
                    iE_Extensions := omit
                }
            },
            supported_ta_list := {
                {
                    tAC := '000001'O,
                    broadcastPLMNList := {
                        {
                            pLMNIdentity := '99F907'O,
                            tAISliceSupportList := {
                                {
                                    s_NSSAI := {
                                        sST := '01'O,
                                        sD := omit,
                                        iE_Extensions := omit
                                    },
                                    iE_Extensions := omit
                                }
                            },
                            iE_Extensions := omit
                        }
                    },
                    iE_Extensions := omit
                }
            }
        }
    },
    ue_pars := {
        idx := 0,
        imsi := '999700000000000'H,
        imeisv := '7502522778710371'H,
        usim_key := '762A2206FE0B4151ACE403C86A11E479'O,
        usim_opc := '3C6E0B8A9C15224A8228B9A98CA1531D'O,
        apn := "internet",
        ran_id := 0,
        amf_id := omit,
        guti := omit,
        pti := '00'O,
        sess_pars := {
            id := 1,
            run_prog_pars := {
                run_as_user := "root",
                log_path_prefix := "./run_prog",
                tun_netns_name := "tun0",
                tun_dev_name := "tun0",
                ping_hostname := "10.45.0.1"
            },
            ran_gtpu_ip := "127.0.0.20",
            ran_gtpu_teid := '00000001'O,
            cn_gtpu_ip := omit,
            cn_gtpu_teid := omit,
            qos_rules := omit,
            ue_ip := omit
        }
    },
    c5g_idx := 0,
    kset_id := {
        iei := omit,
        tsc := '0'B,
        nasKeySetId := '111'B
    }
}).
09:29:56.957580 14032 ConnHdlr.ttcn:538 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '111'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:56.957878 14032 ConnHdlr.ttcn:538 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004179000D0199F9072143000100000000002E028040'O
09:29:56.959957 14032 ConnHdlr.ttcn:543 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
}
09:29:56.960682 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:56.960747 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.960770 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.960790 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.960808 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.961003 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT succeeded:  matched
09:29:56.961039 14031 NGAP_Emulation.ttcn:513 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := mo_Signalling (3)
                        }
                    }
                }
            }
        }
    }
} id 1
09:29:56.961061 14031 NGAP_Emulation.ttcn:513 Message with id 1 was extracted from the queue of NGAP_CLIENT.
09:29:56.962113 14031 NGAP_Emulation.ttcn:519 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 15,
            criticality := ignore (1),
            value_ := {
                initialUEMessage := {
                    protocolIEs := {
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E004179000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := reject (0),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 90,
                            criticality := ignore (1),
                            value_ := {
                                rRCEstablishmentCause := mo_Signalling (3)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:56.962371 14031 NGAP_Emulation.ttcn:519 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '000F403D00000400550002000000260018177E004179000D0199F9072143000100000000002E0280400079000F4099F907000000000099F907000001005A400118'O
}
09:29:56.964449 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004403E000003000A000200020055000200000026002B2A7E0056020200002199E8B036682C6B4D5831596E3FB9F345201051FFA1CA9D348000713DFA5B5821F539'O
} id 3
09:29:56.964834 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0056020200002199E8B036682C6B4D5831596E3FB9F345201051FFA1CA9D348000713DFA5B5821F539'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:29:56.964889 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:56.964917 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0056020200002199E8B036682C6B4D5831596E3FB9F345201051FFA1CA9D348000713DFA5B5821F539'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 3
09:29:56.964938 14031 NGAP_Emulation.ttcn:548 Message with id 3 was extracted from the queue of NGAP.
09:29:56.965104 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0056020200002199E8B036682C6B4D5831596E3FB9F345201051FFA1CA9D348000713DFA5B5821F539'O
09:29:56.965634 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10011001111010001011000000110110011010000010110001101011010011010101100000110001010110010110111000111111101110011111001101000101'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01010001111111111010000111001010100111010011010010000000000000000111000100111101111110100101101101011000001000011111010100111001'B
        },
        eapMessage := omit
    }
}
09:29:56.965886 14031 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10011001111010001011000000110110011010000010110001101011010011010101100000110001010110010110111000111111101110011111001101000101'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01010001111111111010000111001010100111010011010010000000000000000111000100111101111110100101101101011000001000011111010100111001'B
        },
        eapMessage := omit
    }
}
09:29:56.966127 14032 ConnHdlr.ttcn:555 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10011001111010001011000000110110011010000010110001101011010011010101100000110001010110010110111000111111101110011111001101000101'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01010001111111111010000111001010100111010011010010000000000000000111000100111101111110100101101101011000001000011111010100111001'B
        },
        eapMessage := omit
    }
} id 1
09:29:56.966315 14032 ConnHdlr.ttcn:189 Matching on port NGAP succeeded:  matched
09:29:56.966359 14032 ConnHdlr.ttcn:189 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    authentication_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010110'B,
        spareHalfOctet2 := '0'H,
        ngNasKeySetId := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        abba := {
            iei := omit,
            iel := '02'O,
            abbaValue := '0000'O
        },
        rand := {
            iei := '21'O ("!"),
            randValue := '10011001111010001011000000110110011010000010110001101011010011010101100000110001010110010110111000111111101110011111001101000101'B
        },
        autn := {
            iei := '20'O (" "),
            iel := '10'O,
            aUTN := '01010001111111111010000111001010100111010011010010000000000000000111000100111101111110100101101101011000001000011111010100111001'B
        },
        eapMessage := omit
    }
} id 1
09:29:56.966390 14032 ConnHdlr.ttcn:189 Message with id 1 was extracted from the queue of NGAP.
09:29:56.968322 14032 ConnHdlr.ttcn:234 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'EB2AC747EC0C7BD95DD472DB4D88182C83605108E17994D9E254FED71038F02E'O,
        k_nas_enc := 'CAC9603E29F869D7177538E80A7BEEA738581A61D1113CAC6F1174F8C0AE6EE0'O
    }
}
09:29:56.968438 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'EB2AC747EC0C7BD95DD472DB4D88182C83605108E17994D9E254FED71038F02E'O,
        k_nas_enc := 'CAC9603E29F869D7177538E80A7BEEA738581A61D1113CAC6F1174F8C0AE6EE0'O
    }
} id 2
09:29:56.968502 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT succeeded:  matched
09:29:56.968510 14032 ConnHdlr.ttcn:238 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00110011110101110001101010100010111110101101100110010101101111101110011100001110001000011010111110011001101001111110100110101011'B
        },
        eapMessage := omit
    }
}
09:29:56.968530 14031 NGAP_Emulation.ttcn:487 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_keys := {
        k_nas_int := 'EB2AC747EC0C7BD95DD472DB4D88182C83605108E17994D9E254FED71038F02E'O,
        k_nas_enc := 'CAC9603E29F869D7177538E80A7BEEA738581A61D1113CAC6F1174F8C0AE6EE0'O
    }
} id 2
09:29:56.968553 14031 NGAP_Emulation.ttcn:487 Message with id 2 was extracted from the queue of NGAP_CLIENT.
09:29:56.968730 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00110011110101110001101010100010111110101101100110010101101111101110011100001110001000011010111110011001101001111110100110101011'B
        },
        eapMessage := omit
    }
} id 3
09:29:56.968840 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.968867 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.968889 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.968910 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.968941 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:56.968993 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:56.969023 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00110011110101110001101010100010111110101101100110010101101111101110011100001110001000011010111110011001101001111110100110101011'B
        },
        eapMessage := omit
    }
} id 3
09:29:56.969048 14031 NGAP_Emulation.ttcn:522 Message with id 3 was extracted from the queue of NGAP_CLIENT.
09:29:56.969117 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    authentication_Response := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010111'B,
        authResponseParam := {
            iei := '2D'O ("-"),
            iel := '00'O,
            res := '00110011110101110001101010100010111110101101100110010101101111101110011100001110001000011010111110011001101001111110100110101011'B
        },
        eapMessage := omit
    }
}
09:29:56.969329 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00572D1033D71AA2FAD995BEE70E21AF99A7E9AB'O
09:29:56.970226 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E00572D1033D71AA2FAD995BEE70E21AF99A7E9AB'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:56.970370 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403C000004000A0002000200550002000000260016157E00572D1033D71AA2FAD995BEE70E21AF99A7E9AB0079400F4099F907000000000099F907000001'O
}
09:29:56.973655 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044027000003000A0002000200550002000000260014137E038F9DC734007E005D0102028040E1360102'O
} id 4
09:29:56.973788 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E038F9DC734007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:29:56.973862 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:56.973906 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E038F9DC734007E005D0102028040E1360102'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 4
09:29:56.973946 14031 NGAP_Emulation.ttcn:548 Message with id 4 was extracted from the queue of NGAP.
09:29:56.973988 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E038F9DC734007E005D0102028040E1360102'O
09:29:56.974042 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0011'B,
        messageAuthenticationCode := '8F9DC734'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005D0102028040E1360102'O
    }
}
09:29:56.975153 14031 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E005D0102028040E1360102'O
09:29:56.975460 14031 NG_CryptoFunctions.ttcn:242 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:29:56.975778 14031 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
}
09:29:56.976099 14032 ConnHdlr.ttcn:556 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:29:56.976407 14032 ConnHdlr.ttcn:250 Matching on port NGAP succeeded:  matched
09:29:56.976469 14032 ConnHdlr.ttcn:250 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    security_Mode_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011101'B,
        nasSecurityAlgorithms := {
            iei := omit,
            cipheringType := '0000'B,
            integrityType := '0001'B
        },
        spareHalfOctet2 := '0'H,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        ueSecurityCapability := {
            iei := omit,
            iel := '02'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        imeisvRequest := {
            iei := 'E'H,
            spare := '0'B,
            requestValue := '001'B
        },
        epsSecurityAlgorithms := omit,
        add5GSecurityInfo := {
            iei := '36'O ("6"),
            iel := '01'O,
            spareBits := '000000'B,
            rinmr := '1'B,
            hdp := '0'B
        },
        eapMessage := omit,
        abba := omit,
        replayedUESecurityCap := omit
    }
} id 2
09:29:56.976514 14032 ConnHdlr.ttcn:250 Message with id 2 was extracted from the queue of NGAP.
09:29:56.976591 14032 ConnHdlr.ttcn:255 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
}
09:29:56.976699 14032 ConnHdlr.ttcn:260 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
}
09:29:56.976722 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:29:56.976828 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:29:56.976893 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:29:56.976940 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT succeeded:  matched
09:29:56.976982 14031 NGAP_Emulation.ttcn:499 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_int := NG_NAS_ALG_IP_NIA1 (1)
} id 4
09:29:56.976986 14032 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '001'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000D'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '001'B,
            otherDigits := '99F907214300010000000000'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:56.977033 14031 NGAP_Emulation.ttcn:499 Message with id 4 was extracted from the queue of NGAP_CLIENT.
09:29:56.977132 14032 ConnHdlr.ttcn:270 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004129000D0199F9072143000100000000002E028040'O
09:29:56.977175 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:29:56.977227 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_keys := ?
} unmatched: First message in the queue does not match the template: 
09:29:56.977268 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    reset_nas_counts := ?
} unmatched: First message in the queue does not match the template: 
09:29:56.977345 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} with {
    set_nas_alg_int := ?
} unmatched: First message in the queue does not match the template: 
09:29:56.977391 14032 ConnHdlr.ttcn:271 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7502522778710371'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:29:56.977395 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT succeeded:  matched
09:29:56.977435 14031 NGAP_Emulation.ttcn:506 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_Config : {
    set_nas_alg_enc := NG_NAS_ALG_ENC_NEA0 (0)
} id 5
09:29:56.977477 14031 NGAP_Emulation.ttcn:506 Message with id 5 was extracted from the queue of NGAP_CLIENT.
09:29:56.977609 14032 NGAP_Emulation.ttcn:717 Called on NGAP_PROC to TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { }
09:29:56.977735 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7502522778710371'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:29:56.977884 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.977927 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.977966 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.978002 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:56.978049 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:56.978097 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:56.978144 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7502522778710371'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
} id 6
09:29:56.978188 14031 NGAP_Emulation.ttcn:522 Message with id 6 was extracted from the queue of NGAP_CLIENT.
09:29:56.978272 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Mode_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01011110'B,
        imeisv := {
            iei := '77'O ("w"),
            iel := '0000'O,
            idDigit1 := '0000'B,
            oddEvenInd := '0'B,
            typeOfId := '101'B,
            otherDigits := '7502522778710371'O
        },
        nasMsg := {
            iei := '71'O ("q"),
            iel := '0000'O,
            replayedNASMsgContainerValue := '7E004129000D0199F9072143000100000000002E028040'O
        },
        nonIMEISV_PEI := omit
    }
}
09:29:56.978433 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E005E7700090575025227787103717100177E004129000D0199F9072143000100000000002E028040'O
09:29:56.979533 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0100'B,
        messageAuthenticationCode := '752E4483'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E005E7700090575025227787103717100177E004129000D0199F9072143000100000000002E028040'O
    }
}
09:29:56.979609 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E04752E4483007E005E7700090575025227787103717100177E004129000D0199F9072143000100000000002E028040'O
09:29:56.979787 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E04752E4483007E005E7700090575025227787103717100177E004129000D0199F9072143000100000000002E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:56.979899 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4057000004000A0002000200550002000000260031307E04752E4483007E005E7700090575025227787103717100177E004129000D0199F9072143000100000000002E0280400079400F4099F907000000000099F907000001'O
}
09:29:56.980105 14031 NGAP_Emulation.ttcn:485 Call enqueued on NGAP_PROC from TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:29:56.980187 14031 NGAP_Emulation.ttcn:602 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register.
09:29:56.980229 14031 NGAP_Emulation.ttcn:606 Matching on port NGAP_PROC failed: The first entity in the queue is not a call for signature @NGAP_Emulation.NGAPEM_register_proc.
09:29:56.980272 14031 NGAP_Emulation.ttcn:610 Matching on port NGAP_PROC succeeded: { } with { } matched
09:29:56.980351 14031 NGAP_Emulation.ttcn:610 Getcall operation on port NGAP_PROC succeeded, call from TC_periodic_registration_updating0(14): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } id 1
09:29:56.980398 14031 NGAP_Emulation.ttcn:610 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:29:56.980464 14031 NGAP_Emulation.ttcn:613 Replied on NGAP_PROC to TC_periodic_registration_updating0(14) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2
09:29:56.980619 14032 NGAP_Emulation.ttcn:717 Reply enqueued on NGAP_PROC from TC_periodic_registration_updating-NGAP0(13) @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:29:56.980740 14032 NGAP_Emulation.ttcn:718 Matching on port NGAP_PROC succeeded: { } with { } matched value 2 with ? matched
09:29:56.980842 14032 NGAP_Emulation.ttcn:718 Getreply operation on port NGAP_PROC succeeded, reply from TC_periodic_registration_updating-NGAP0(13): @NGAP_Emulation.NGAPEM_obtain_amf_id : { } value 2 id 1
09:29:56.980887 14032 NGAP_Emulation.ttcn:718 Operation with id 1 was extracted from the queue of NGAP_PROC.
09:29:56.993897 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044056000005000A000200020055000200000026002F2E7E0235346F7C017E0042010177000BF299F907020040C000027054074099F90700000115020101210201005E0192006E400A0C3B9ACA00303B9ACA00000000020001'O
} id 5
09:29:56.994969 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0235346F7C017E0042010177000BF299F907020040C000027054074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:29:56.995134 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:56.995209 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0235346F7C017E0042010177000BF299F907020040C000027054074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 110,
                            criticality := ignore (1),
                            value_ := {
                                uEAggregateMaximumBitRate := {
                                    uEAggregateMaximumBitRateDL := 1000000000,
                                    uEAggregateMaximumBitRateUL := 1000000000,
                                    iE_Extensions := omit
                                }
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 5
09:29:56.995255 14031 NGAP_Emulation.ttcn:548 Message with id 5 was extracted from the queue of NGAP.
09:29:56.995315 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0235346F7C017E0042010177000BF299F907020040C000027054074099F90700000115020101210201005E0192'O
09:29:56.995386 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '35346F7C'O ("54o|"),
        sequenceNumber := '01'O,
        plainNASMessage := '7E0042010177000BF299F907020040C000027054074099F90700000115020101210201005E0192'O
    }
}
09:29:56.996555 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C000027054074099F90700000115020101210201005E0192'O
09:29:56.997893 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:56.999024 14031 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:57.000150 14032 ConnHdlr.ttcn:561 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:29:57.001164 14032 ConnHdlr.ttcn:561 Matching on port NGAP succeeded:  matched
09:29:57.001312 14032 ConnHdlr.ttcn:561 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 3
09:29:57.001402 14032 ConnHdlr.ttcn:561 Message with id 3 was extracted from the queue of NGAP.
09:29:57.001596 14032 ConnHdlr.ttcn:563 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:57.001761 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:29:57.001875 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.001930 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.001982 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.002041 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.002104 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:57.002164 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:57.002224 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 7
09:29:57.002281 14031 NGAP_Emulation.ttcn:522 Message with id 7 was extracted from the queue of NGAP_CLIENT.
09:29:57.002364 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:57.002451 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:29:57.003588 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '4EC4F0A5'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:29:57.003655 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E024EC4F0A5007E0043'O
09:29:57.003863 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E024EC4F0A5007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.004005 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E024EC4F0A5007E00430079400F4099F907000000000099F907000001'O
}
09:29:57.006069 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E0212CAF4FD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
} id 6
09:29:57.006273 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0212CAF4FD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:29:57.006356 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:57.006413 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0212CAF4FD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 6
09:29:57.006458 14031 NGAP_Emulation.ttcn:548 Message with id 6 was extracted from the queue of NGAP.
09:29:57.006515 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0212CAF4FD027E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
09:29:57.006577 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '12CAF4FD'O,
        sequenceNumber := '02'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
    }
}
09:29:57.007712 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
09:29:57.008173 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:57.008615 14031 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:57.008970 14032 ConnHdlr.ttcn:565 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:29:57.009374 14032 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:29:57.009448 14032 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 4
09:29:57.009496 14032 ConnHdlr.ttcn:279 Message with id 4 was extracted from the queue of NGAP.
09:29:57.009587 14032 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:57.009688 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:29:57.009758 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.009795 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.009829 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.009863 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.009905 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:57.009945 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:57.009986 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 8
09:29:57.010025 14031 NGAP_Emulation.ttcn:522 Message with id 8 was extracted from the queue of NGAP_CLIENT.
09:29:57.010065 14032 ConnHdlr.ttcn:577 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:57.010083 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:57.010144 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:29:57.011037 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'F5CF53E2'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:29:57.011093 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02F5CF53E2007E0055'O
09:29:57.011247 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02F5CF53E2007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.011350 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E02F5CF53E2007E00550079400F4099F907000000000099F907000001'O
}
09:29:57.011848 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:29:57.012161 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.012208 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.012246 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.012282 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.012332 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:57.012383 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:57.012446 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
} id 9
09:29:57.012491 14031 NGAP_Emulation.ttcn:522 Message with id 9 was extracted from the queue of NGAP_CLIENT.
09:29:57.012538 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Request := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000001'B,
        ngNasKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '010'B
        },
        registrationType := {
            fOR := '1'B,
            registrationType := '011'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000270'O
        },
        nonCurrentNativeKSI := omit,
        gmmCapability := omit,
        ueSecurityCapability := {
            iei := '2E'O ("."),
            iel := '00'O,
            ngeaCap := '80'O,
            ngiaCap := '40'O ("@"),
            eeaCap := omit,
            eiaCap := omit,
            spare := omit
        },
        requestedNSSAI := omit,
        lastVisitedRegisteredTai := omit,
        s1_UE_Capability := omit,
        ulDataStatus := omit,
        pduSessionStatus := omit,
        micoInd := omit,
        ueStatus := omit,
        additionalGUTI := omit,
        allowedPDUSessionStatus := omit,
        ueUsageSetting := omit,
        reqDRXParams := omit,
        epsMessage := omit,
        ladnInd := omit,
        payloadContainerType := omit,
        payload := omit,
        networkSlicingInd := omit,
        updateType := omit,
        msClassmark2 := omit,
        supportedCodecs := omit,
        nasMsg := omit,
        epsBearerContextStatus := omit,
        requestedExtdDRXParams := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        requestedMappedNSSAI := omit,
        additionalInfoReq := omit,
        requestedWUSAssistanceInfo := omit,
        n5GCInd := omit,
        requestedNB_N1DRXParams := omit,
        ueRequestType := omit,
        pagingRestrict := omit,
        serviceLvlAA := omit,
        nId := omit,
        msPLMNwDisasterCondition := omit,
        requestedPEIPS_AssistInfo := omit,
        t3512Value := omit
    }
}
09:29:57.012743 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E00412B000BF299F907020040C00002702E028040'O
09:29:57.013529 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '89B169EF'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E00412B000BF299F907020040C00002702E028040'O
    }
}
09:29:57.013589 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0289B169EF007E00412B000BF299F907020040C00002702E028040'O
09:29:57.013712 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0289B169EF007E00412B000BF299F907020040C00002702E028040'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.013796 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4043000004000A000200020055000200000026001D1C7E0289B169EF007E00412B000BF299F907020040C00002702E0280400079400F4099F907000000000099F907000001'O
}
09:29:57.215864 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044048000004000A000200020055000200000026002F2E7E027E2DFEC1037E0042010177000BF299F907020040C000078854074099F90700000115020101210201005E0192000000020001'O
} id 7
09:29:57.216485 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E027E2DFEC1037E0042010177000BF299F907020040C000078854074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:29:57.217013 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:57.217406 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E027E2DFEC1037E0042010177000BF299F907020040C000078854074099F90700000115020101210201005E0192'O
                            }
                        },
                        {
                            id := 0,
                            criticality := reject (0),
                            value_ := {
                                allowedNSSAI := {
                                    {
                                        s_NSSAI := {
                                            sST := '01'O,
                                            sD := omit,
                                            iE_Extensions := omit
                                        },
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 7
09:29:57.217741 14031 NGAP_Emulation.ttcn:548 Message with id 7 was extracted from the queue of NGAP.
09:29:57.218127 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E027E2DFEC1037E0042010177000BF299F907020040C000078854074099F90700000115020101210201005E0192'O
09:29:57.218505 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '7E2DFEC1'O,
        sequenceNumber := '03'O,
        plainNASMessage := '7E0042010177000BF299F907020040C000078854074099F90700000115020101210201005E0192'O
    }
}
09:29:57.220259 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0042010177000BF299F907020040C000078854074099F90700000115020101210201005E0192'O
09:29:57.220744 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:57.221208 14031 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
}
09:29:57.221811 14032 ConnHdlr.ttcn:589 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:29:57.222548 14032 ConnHdlr.ttcn:589 Matching on port NGAP succeeded:  matched
09:29:57.222953 14032 ConnHdlr.ttcn:589 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    registration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000010'B,
        registrationResult := {
            iel := '01'O,
            spare := '0'B,
            disasterRoamingResult := '0'B,
            emergencyRegistered := '0'B,
            nssaaPerformed := '0'B,
            smsAllowed := '0'B,
            resultValue := '001'B
        },
        guti := {
            iei := '77'O ("w"),
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        },
        equivalentPlmns := omit,
        taiList := {
            iei := '54'O ("T"),
            lvPart := {
                iel := '07'O ("\a"),
                listOfPartialTais := {
                    {
                        allowedType := '0'B,
                        typeOfList := '10'B,
                        numberOfElements := '00000'B,
                        partialTaiList := {
                            type0List := {
                                {
                                    plmnId := '99F907'O,
                                    tacList := {
                                        '000001'O
                                    }
                                }
                            }
                        }
                    }
                }
            }
        },
        allowedNSSAI := {
            iei := '15'O,
            lvPart := {
                iel := '02'O,
                s_nssai := {
                    {
                        iel := '01'O,
                        vPart := {
                            sst := '01'O,
                            sd := omit,
                            mappedSST := omit,
                            mappedSD := omit
                        }
                    }
                }
            }
        },
        rejectedNSSAI := omit,
        configuredNSSAI := omit,
        ngs_NetworkFeatureSupport := {
            iei := '21'O ("!"),
            iel := '02'O,
            mpsi := '0'B,
            iwk_N26 := '0'B,
            emf := '00'B,
            emc := '00'B,
            imsVoPS_n3GPP := '0'B,
            imsVoPS_3GPP := '1'B,
            ng_UP_CIoT := '0'B,
            ngIPHC_CP_CIoT := '0'B,
            n3Data := '0'B,
            ng_CP_CIoT := '0'B,
            restrictEC := '00'B,
            mcsi := '0'B,
            emcn3 := '0'B,
            spareBit := omit,
            pr := omit,
            rpr := omit,
            piv := omit,
            ncr := omit,
            ngEHC_CP_CIoT := omit,
            atsInd := omit,
            ngLCS := omit
        },
        pduSessionStatus := omit,
        pduSessionReactivationResult := omit,
        pduSessionReactResultError := omit,
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        saiList := omit,
        t3512Value := {
            iei := '5E'O ("^"),
            iel := '01'O,
            unit := '100'B,
            gprsTimerValue := '10010'B
        },
        non3GPPDeregisterValue := omit,
        t3502Value := omit,
        emergencyNumberList := omit,
        xtdEmergencyNumberList := omit,
        sorTransparentContainer := omit,
        eapMessage := omit,
        inclusionModeNSSAI := omit,
        operatorAccessCatDefs := omit,
        negotiatedDRXParams := omit,
        non3GPP_NW_ProvidedPolicies := omit,
        epsBearerContextStatus := omit,
        negotiatedExtdDRXParams := omit,
        t3447Value := omit,
        t3448Value := omit,
        t3324Value := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        pendingNSSAI := omit,
        cipheringKeyData := omit,
        cagInfoList := omit,
        truncatedS_TMSIConfig := omit,
        negotiatedWUSAssistanceInfo := omit,
        negotiatedNB_N1DRXParams := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        negotiatedPEIPS_AssistInfo := omit,
        ngAddRequestResult := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        forbidTAIList_Roaming := omit,
        forbidTAIList_RegProvService := omit,
        extdCAGInfoList := omit,
        nsagInfo := omit
    }
} id 5
09:29:57.223321 14032 ConnHdlr.ttcn:589 Message with id 5 was extracted from the queue of NGAP.
09:29:57.223735 14032 ConnHdlr.ttcn:591 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:57.223996 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:29:57.224175 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.224232 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.224281 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.224331 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.224394 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:57.224455 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:57.224515 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
} id 10
09:29:57.224576 14031 NGAP_Emulation.ttcn:522 Message with id 10 was extracted from the queue of NGAP_CLIENT.
09:29:57.224683 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    registration_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000011'B,
        sorTransparentContainer := omit
    }
}
09:29:57.224767 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0043'O
09:29:57.226152 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '4EC4F0A5'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0043'O
    }
}
09:29:57.226240 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E024EC4F0A5007E0043'O
09:29:57.226509 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E024EC4F0A5007E0043'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.226685 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E024EC4F0A5007E00430079400F4099F907000000000099F907000001'O
}
09:29:57.229504 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '00044047000003000A0002000200550002000000260034337E0283BC1F59047E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
} id 8
09:29:57.229689 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0283BC1F59047E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:57.229790 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:57.229865 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E0283BC1F59047E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:57.229927 14031 NGAP_Emulation.ttcn:548 Message with id 8 was extracted from the queue of NGAP.
09:29:57.230003 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0283BC1F59047E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
09:29:57.230083 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '83BC1F59'O,
        sequenceNumber := '04'O,
        plainNASMessage := '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
    }
}
09:29:57.231791 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0054430F90004F00700065006E003500470053450990004E00650078007446004752115190927500490100'O
09:29:57.232050 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:57.232280 14031 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
}
09:29:57.232615 14032 ConnHdlr.ttcn:593 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:29:57.233010 14032 ConnHdlr.ttcn:279 Matching on port NGAP succeeded:  matched
09:29:57.233161 14032 ConnHdlr.ttcn:279 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    configuration_Update_Command := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010100'B,
        configUpdateInd := omit,
        guti := omit,
        taiList := omit,
        allowedNSSAI := omit,
        saiList := omit,
        fullNetworkName := {
            iei := '43'O ("C"),
            iel := '0F'O,
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '5300470035006E00650070004F00'O
        },
        shortNetworkName := {
            iei := '45'O ("E"),
            iel := '09'O ("	"),
            ext := '1'B,
            codingScheme := '001'B,
            addCI := '0'B,
            spareBitCnt := '000'B,
            text := '7400780065004E00'O
        },
        localTimeZone := {
            iei := '46'O ("F"),
            timeZone := '00'O
        },
        localTimeZoneAndTime := {
            iei := '47'O ("G"),
            year := '52'O ("R"),
            month := '11'O,
            day := '51'O ("Q"),
            hour := '90'O,
            minute := '92'O,
            second := '75'O ("u"),
            timeZone := '00'O
        },
        daylightSavingTime := {
            iei := '49'O ("I"),
            iel := '01'O,
            spare := '000000'B,
            val := '00'B
        },
        ladnInfo := omit,
        micoInd := omit,
        networkSlicingInd := omit,
        configuredNSSAI := omit,
        rejectedNSSAI := omit,
        operatorAccessCatDefs := omit,
        smsInd := omit,
        t3447Value := omit,
        cagInfoList := omit,
        ueRadioCapabilityId := omit,
        ueRadioCapIdDeletionInd := omit,
        registrationResult := omit,
        truncatedS_TMSIConfig := omit,
        addConfigInfo := omit,
        extdRejectedNSSAI := omit,
        serviceLvlAA := omit,
        nssrgInfo := omit,
        disasterRoamingWaitRange := omit,
        disasterReturnWaitRange := omit,
        disasterPLMNList := omit,
        extdCAGInfoList := omit,
        updatedPEIPS_AssistInfo := omit,
        nsagInfo := omit,
        priorityInd := omit
    }
} id 6
09:29:57.233274 14032 ConnHdlr.ttcn:279 Message with id 6 was extracted from the queue of NGAP.
09:29:57.233413 14032 ConnHdlr.ttcn:280 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:57.233573 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:29:57.233668 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.233726 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.233781 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.233832 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.233898 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:57.233957 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:57.234016 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
} id 11
09:29:57.234073 14031 NGAP_Emulation.ttcn:522 Message with id 11 was extracted from the queue of NGAP_CLIENT.
09:29:57.234099 14032 ConnHdlr.ttcn:607 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        }
    }
}
09:29:57.234151 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    configuration_Update_Complete := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01010101'B
    }
}
09:29:57.234228 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E0055'O
09:29:57.235613 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'F5CF53E2'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E0055'O
    }
}
09:29:57.235685 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02F5CF53E2007E0055'O
09:29:57.235896 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02F5CF53E2007E0055'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.236050 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E4031000004000A000200020055000200000026000B0A7E02F5CF53E2007E00550079400F4099F907000000000099F907000001'O
}
09:29:57.236373 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        }
    }
} id 12
09:29:57.236504 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.236569 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.236619 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.236691 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.236755 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP-PDU-Descriptions.NGAP-PDU.
09:29:57.236820 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT succeeded:  matched
09:29:57.236886 14031 NGAP_Emulation.ttcn:522 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type : {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        }
    }
} id 12
09:29:57.236947 14031 NGAP_Emulation.ttcn:522 Message with id 12 was extracted from the queue of NGAP_CLIENT.
09:29:57.237013 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    deregistration_RequestMO := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000101'B,
        ngKSI := {
            iei := omit,
            tsc := '0'B,
            nasKeySetId := '011'B
        },
        deregistrationType := {
            switchOff := '0'B,
            reRegistration := '0'B,
            accessType := '01'B
        },
        ngMobileId := {
            iei := omit,
            iel := '000B'O,
            idDigit1 := '1111'B,
            oddEvenInd := '0'B,
            typeOfId := '010'B,
            otherDigits := '99F907020040C0000788'O
        }
    }
}
09:29:57.237142 14031 NG_CryptoFunctions.ttcn:319 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E004531000BF299F907020040C0000788'O
09:29:57.238589 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Encoding @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := '459EF008'O,
        sequenceNumber := '00'O,
        plainNASMessage := '7E004531000BF299F907020040C0000788'O
    }
}
09:29:57.238663 14031 NGAP_Emulation.ttcn:526 enc_NG_NAS_UL_Message_Type(): Stream after encoding: '7E02459EF008007E004531000BF299F907020040C0000788'O
09:29:57.238842 14031 NGAP_Emulation.ttcn:527 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        initiatingMessage := {
            procedureCode := 46,
            criticality := ignore (1),
            value_ := {
                uplinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02459EF008007E004531000BF299F907020040C0000788'O
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.238982 14031 NGAP_Emulation.ttcn:527 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '002E403F000004000A0002000200550002000000260019187E02459EF008007E004531000BF299F907020040C00007880079400F4099F907000000000099F907000001'O
}
09:29:57.454959 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '0004401E000003000A000200020055000200000026000B0A7E02F5002F75057E0046'O
} id 9
09:29:57.455487 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02F5002F75057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:29:57.455721 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:57.455863 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 4,
            criticality := ignore (1),
            value_ := {
                downlinkNASTransport := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := reject (0),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := reject (0),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 38,
                            criticality := reject (0),
                            value_ := {
                                nAS_PDU := '7E02F5002F75057E0046'O
                            }
                        }
                    }
                }
            }
        }
    }
} id 9
09:29:57.455931 14031 NGAP_Emulation.ttcn:548 Message with id 9 was extracted from the queue of NGAP.
09:29:57.456022 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E02F5002F75057E0046'O
09:29:57.456111 14031 NGAP_Emulation.ttcn:570 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    security_Protected_Nas_Message := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0010'B,
        messageAuthenticationCode := 'F5002F75'O,
        sequenceNumber := '05'O,
        plainNASMessage := '7E0046'O
    }
}
09:29:57.457581 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Stream before decoding: '7E0046'O
09:29:57.457677 14031 NG_CryptoFunctions.ttcn:261 dec_NG_NAS_DL_Message_Type(): Decoded @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type: {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:29:57.457793 14031 NGAP_Emulation.ttcn:580 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
}
09:29:57.458005 14032 ConnHdlr.ttcn:609 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:29:57.458064 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    proto := {
        sctp := {
            sinfo_stream := 1,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    userData := 0,
    msg := '002900100000020072000400020000000F400148'O
} id 10
09:29:57.458221 14032 ConnHdlr.ttcn:609 Matching on port NGAP succeeded:  matched
09:29:57.458293 14032 ConnHdlr.ttcn:609 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NG_NAS_MsgContainers.NG_NAS_DL_Message_Type : {
    deregistration_Accept := {
        protocolDiscriminator := '01111110'B,
        spareHalfOctet := '0'H,
        securityHeaderType := '0000'B,
        messageType := '01000110'B
    }
} id 7
09:29:57.458356 14032 ConnHdlr.ttcn:609 Message with id 7 was extracted from the queue of NGAP.
09:29:57.459291 14031 NGAP_Emulation.ttcn:485 Incoming message was mapped to @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:29:57.459404 14031 NGAP_Emulation.ttcn:548 Matching on port NGAP succeeded:  matched
09:29:57.459478 14031 NGAP_Emulation.ttcn:548 Receive operation on port NGAP succeeded, message from system(): @NGAP_CodecPort.NGAP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.5",
    remPort := 38412,
    locName := "127.0.0.202",
    locPort := 50000,
    msg := {
        initiatingMessage := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseCommand := {
                    protocolIEs := {
                        {
                            id := 114,
                            criticality := reject (0),
                            value_ := {
                                uE_NGAP_IDs := {
                                    uE_NGAP_ID_pair := {
                                        aMF_UE_NGAP_ID := 2,
                                        rAN_UE_NGAP_ID := 0,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        },
                        {
                            id := 15,
                            criticality := ignore (1),
                            value_ := {
                                cause := {
                                    nas := deregister (2)
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 10
09:29:57.459547 14031 NGAP_Emulation.ttcn:548 Message with id 10 was extracted from the queue of NGAP.
09:29:57.459750 14031 NGAP_Emulation.ttcn:587 Sent on NGAP_CLIENT to TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.460865 14032 ConnHdlr.ttcn:610 Message enqueued on NGAP from TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:57.461071 14032 ConnHdlr.ttcn:623 Matching on port NGAP succeeded:  matched
09:29:57.461088 14032 ConnHdlr.ttcn:623 Receive operation on port NGAP succeeded, message from TC_periodic_registration_updating-NGAP0(13): @NGAP-PDU-Descriptions.NGAP-PDU : {
    initiatingMessage := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseCommand := {
                protocolIEs := {
                    {
                        id := 114,
                        criticality := reject (0),
                        value_ := {
                            uE_NGAP_IDs := {
                                uE_NGAP_ID_pair := {
                                    aMF_UE_NGAP_ID := 2,
                                    rAN_UE_NGAP_ID := 0,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    },
                    {
                        id := 15,
                        criticality := ignore (1),
                        value_ := {
                            cause := {
                                nas := deregister (2)
                            }
                        }
                    }
                }
            }
        }
    }
} id 8
09:29:57.461099 14032 ConnHdlr.ttcn:623 Message with id 8 was extracted from the queue of NGAP.
09:29:57.461649 14032 ConnHdlr.ttcn:624 Sent on NGAP to TC_periodic_registration_updating-NGAP0(13) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.461765 14032 - Function f_init_handler finished. PTC terminates.
09:29:57.461826 14032 - Terminating component type ConnHdlr.ConnHdlr.
09:29:57.461877 14032 - Removing unterminated connection between port NGAP and TC_periodic_registration_updating-NGAP0(13):NGAP_CLIENT.
09:29:57.461963 14031 NGAP_Emulation.ttcn:485 Message enqueued on NGAP_CLIENT from TC_periodic_registration_updating0(14) @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:29:57.461963 14032 - Port NGAP was stopped.
09:29:57.462030 14032 - Removing unterminated connection between port NGAP_PROC and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:57.462104 14032 - Port NGAP_PROC was stopped.
09:29:57.462154 14032 - Removing unterminated connection between port GTP1U[0] and GTP1U_EM(12):CLIENT.
09:29:57.462157 14031 NGAP_Emulation.ttcn:487 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.462222 14031 NGAP_Emulation.ttcn:493 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.462223 14032 - Port GTP1U[0] was stopped.
09:29:57.462277 14031 NGAP_Emulation.ttcn:499 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.462285 14030 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT to TC_periodic_registration_updating0(14):GTP1U[0] was closed unexpectedly by the peer.
09:29:57.462287 14032 - Port GTP1U[1] was stopped.
09:29:57.462328 14031 NGAP_Emulation.ttcn:506 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NGAP_Emulation.NGAPEM_Config.
09:29:57.462339 14032 - Port GTP1U[2] was stopped.
09:29:57.462391 14032 - Port GTP1U[3] was stopped.
09:29:57.462441 14032 - Removing unterminated connection between port GTP1U_PROC[0] and GTP1U_EM(12):CLIENT_PROC.
09:29:57.462499 14030 GTPv1U_Emulation.ttcnpp:265 Port CLIENT was disconnected from TC_periodic_registration_updating0(14):GTP1U[0].
09:29:57.462513 14032 - Port GTP1U_PROC[0] was stopped.
09:29:57.462561 14032 - Port GTP1U_PROC[1] was stopped.
09:29:57.462610 14032 - Port GTP1U_PROC[2] was stopped.
09:29:57.462658 14032 - Port GTP1U_PROC[3] was stopped.
09:29:57.462710 14030 GTPv1U_Emulation.ttcnpp:265 Connection of port CLIENT_PROC to TC_periodic_registration_updating0(14):GTP1U_PROC[0] was closed unexpectedly by the peer.
09:29:57.462757 14032 - Component type ConnHdlr.ConnHdlr was shut down inside testcase TC_periodic_registration_updating.
09:29:57.462790 14030 GTPv1U_Emulation.ttcnpp:265 Port CLIENT_PROC was disconnected from TC_periodic_registration_updating0(14):GTP1U_PROC[0].
09:29:57.462819 14032 - Final verdict of PTC: none
09:29:57.462843 14031 NGAP_Emulation.ttcn:513 Matching on port NGAP_CLIENT {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} with {
    initiatingMessage := {
        procedureCode := 15,
        criticality := ignore (1),
        value_ := {
            initialUEMessage := {
                protocolIEs := {
                    {
                        id := 85,
                        criticality := reject (0),
                        value_ := {
                            rAN_UE_NGAP_ID := ?
                        }
                    },
                    {
                        id := 38,
                        criticality := reject (0),
                        value_ := {
                            nAS_PDU := ?
                        }
                    },
                    {
                        id := 121,
                        criticality := reject (0),
                        value_ := {
                            userLocationInformation := ?
                        }
                    },
                    {
                        id := 90,
                        criticality := ignore (1),
                        value_ := {
                            rRCEstablishmentCause := ?
                        }
                    }
                }
            }
        }
    }
} unmatched: First message in the queue does not match the template: 
09:29:57.462856 13795 C5G_Tests.ttcn:331 PTC with component reference 14 is done.
09:29:57.462920 14031 NGAP_Emulation.ttcn:522 Matching on port NGAP_CLIENT failed: Type of the first message in the queue is not @NG_NAS_MsgContainers.NG_NAS_UL_Message_Type.
09:29:57.462969 14032 - Disconnected from MC.
09:29:57.462978 14031 NGAP_Emulation.ttcn:535 Matching on port NGAP_CLIENT succeeded:  matched
09:29:57.463032 13795 C5G_Tests.ttcn:331 Terminating component type C5G_Tests.MTC_CT.
09:29:57.463036 14032 - TTCN-3 Parallel Test Component finished.
09:29:57.463065 14031 NGAP_Emulation.ttcn:535 Receive operation on port NGAP_CLIENT succeeded, message from TC_periodic_registration_updating0(14): @NGAP-PDU-Descriptions.NGAP-PDU : {
    successfulOutcome := {
        procedureCode := 41,
        criticality := reject (0),
        value_ := {
            uEContextReleaseComplete := {
                protocolIEs := {
                    {
                        id := 10,
                        criticality := ignore (1),
                        value_ := {
                            aMF_UE_NGAP_ID := 2
                        }
                    },
                    {
                        id := 85,
                        criticality := ignore (1),
                        value_ := {
                            rAN_UE_NGAP_ID := 0
                        }
                    },
                    {
                        id := 121,
                        criticality := ignore (1),
                        value_ := {
                            userLocationInformation := {
                                userLocationInformationNR := {
                                    nR_CGI := {
                                        pLMNIdentity := '99F907'O,
                                        nRCellIdentity := '000000000000000000000000000000000000'B,
                                        iE_Extensions := omit
                                    },
                                    tAI := {
                                        pLMNIdentity := '99F907'O,
                                        tAC := '000001'O,
                                        iE_Extensions := omit
                                    },
                                    timeStamp := omit,
                                    iE_Extensions := omit
                                }
                            }
                        }
                    }
                }
            }
        }
    }
} id 13
09:29:57.463106 13795 C5G_Tests.ttcn:331 Default with id 1 (altstep as_Tguard) was deactivated.
09:29:57.463148 14031 NGAP_Emulation.ttcn:535 Message with id 13 was extracted from the queue of NGAP_CLIENT.
09:29:57.463174 13795 C5G_Tests.ttcn:331 Stop timer g_Tguard: 30 s
09:29:57.463236 13795 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_UNIT[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_UNIT.
09:29:57.463349 13795 C5G_Tests.ttcn:331 Port NGAP_UNIT[0] was stopped.
09:29:57.463441 13795 C5G_Tests.ttcn:331 Removing unterminated connection between port NGAP_PROC[0] and TC_periodic_registration_updating-NGAP0(13):NGAP_PROC.
09:29:57.463526 13795 C5G_Tests.ttcn:331 Port NGAP_PROC[0] was stopped.
09:29:57.463617 13795 C5G_Tests.ttcn:331 Removing unterminated connection between port TEID0 and GTP1U_EM(12):TEID0.
09:29:57.463699 13795 C5G_Tests.ttcn:331 Port TEID0 was stopped.
09:29:57.463791 13795 C5G_Tests.ttcn:331 Component type C5G_Tests.MTC_CT was shut down inside testcase TC_periodic_registration_updating.
09:29:57.463811 14030 GTPv1U_Emulation.ttcnpp:265 Connection of port TEID0 to mtc:TEID0 was closed unexpectedly by the peer.
09:29:57.463856 13795 C5G_Tests.ttcn:331 Waiting for PTCs to finish.
09:29:57.463966 14030 GTPv1U_Emulation.ttcnpp:265 Port TEID0 was disconnected from mtc:TEID0.
09:29:57.464291 14030 GTPv1U_Emulation.ttcnpp:265 Kill was requested from MC.
09:29:57.464373 14030 GTPv1U_Emulation.ttcnpp:265 Terminating test component execution.
09:29:57.464510 14031 NGAP_Emulation.ttcn:538 Sent on NGAP to system @NGAP_CodecPort.NGAP_Send : {
    connId := 1,
    msg := {
        successfulOutcome := {
            procedureCode := 41,
            criticality := reject (0),
            value_ := {
                uEContextReleaseComplete := {
                    protocolIEs := {
                        {
                            id := 10,
                            criticality := ignore (1),
                            value_ := {
                                aMF_UE_NGAP_ID := 2
                            }
                        },
                        {
                            id := 85,
                            criticality := ignore (1),
                            value_ := {
                                rAN_UE_NGAP_ID := 0
                            }
                        },
                        {
                            id := 121,
                            criticality := ignore (1),
                            value_ := {
                                userLocationInformation := {
                                    userLocationInformationNR := {
                                        nR_CGI := {
                                            pLMNIdentity := '99F907'O,
                                            nRCellIdentity := '000000000000000000000000000000000000'B,
                                            iE_Extensions := omit
                                        },
                                        tAI := {
                                            pLMNIdentity := '99F907'O,
                                            tAC := '000001'O,
                                            iE_Extensions := omit
                                        },
                                        timeStamp := omit,
                                        iE_Extensions := omit
                                    }
                                }
                            }
                        }
                    }
                }
            }
        }
    }
}
09:29:57.464831 14031 NGAP_Emulation.ttcn:538 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        sctp := {
            sinfo_stream := omit,
            sinfo_ppid := 60,
            remSocks := omit,
            assocId := omit
        }
    },
    msg := '20290022000003000A400200020055400200000079400F4099F907000000000099F907000001'O
}
09:29:57.465283 14031 NGAP_Emulation.ttcn:485 Connection of port NGAP_CLIENT to TC_periodic_registration_updating0(14):NGAP was closed unexpectedly by the peer.
09:29:57.465317 14030 - Function main was stopped. PTC terminates.
09:29:57.465418 14031 NGAP_Emulation.ttcn:485 Port NGAP_CLIENT was disconnected from TC_periodic_registration_updating0(14):NGAP.
09:29:57.465454 14030 - Terminating component type GTPv1U_Emulation.GTPv1U_Emulation_CT.
09:29:57.465582 14031 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to TC_periodic_registration_updating0(14):NGAP_PROC was closed unexpectedly by the peer.
09:29:57.465706 14031 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from TC_periodic_registration_updating0(14):NGAP_PROC.
09:29:57.465806 14030 - Default with id 1 (altstep as_uecups_ind) was deactivated.
09:29:57.465920 14031 NGAP_Emulation.ttcn:485 Connection of port NGAP_UNIT to mtc:NGAP_UNIT[0] was closed unexpectedly by the peer.
09:29:57.465990 14030 - Removing unterminated mapping between port GTP1U and system:GTP1U.
09:29:57.466077 14031 NGAP_Emulation.ttcn:485 Port NGAP_UNIT was disconnected from mtc:NGAP_UNIT[0].
09:29:57.466134 14030 - Port GTP1U was unmapped from system:GTP1U.
09:29:57.466196 14031 NGAP_Emulation.ttcn:485 Connection of port NGAP_PROC to mtc:NGAP_PROC[0] was closed unexpectedly by the peer.
09:29:57.466270 14031 NGAP_Emulation.ttcn:485 Port NGAP_PROC was disconnected from mtc:NGAP_PROC[0].
09:29:57.466346 14031 NGAP_Emulation.ttcn:485 Kill was requested from MC.
09:29:57.466376 14030 - Port GTP1U was stopped.
09:29:57.466414 14031 NGAP_Emulation.ttcn:485 Terminating test component execution.
09:29:57.466501 14030 - Port TEID0 was stopped.
09:29:57.466562 14030 - Port CLIENT was stopped.
09:29:57.466655 14030 - Port CLIENT_PROC was stopped.
09:29:57.466750 14030 - Removing unterminated mapping between port UECUPS and system:UECUPS.
09:29:57.467244 14031 - Function main was stopped. PTC terminates.
09:29:57.467399 14030 - Port UECUPS was unmapped from system:UECUPS.
09:29:57.467416 14031 - Terminating component type NGAP_Emulation.NGAP_Emulation_CT.
09:29:57.467477 14031 - Removing unterminated mapping between port NGAP and system:NGAP_CODEC_PT.
09:29:57.467483 14030 - Port UECUPS was stopped.
09:29:57.467541 14030 - Component type GTPv1U_Emulation.GTPv1U_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:29:57.467708 14030 - Final verdict of PTC: none
09:29:57.468001 14030 - Disconnected from MC.
09:29:57.468064 14031 - Port NGAP was unmapped from system:NGAP_CODEC_PT.
09:29:57.468219 14031 - Port NGAP was stopped.
09:29:57.468258 14030 - TTCN-3 Parallel Test Component finished.
09:29:57.468274 14031 - Port NGAP_CLIENT was stopped.
09:29:57.468380 14031 - Port NGAP_PROC was stopped.
09:29:57.468444 14031 - Port NGAP_UNIT was stopped.
09:29:57.468778 14031 - Component type NGAP_Emulation.NGAP_Emulation_CT was shut down inside testcase TC_periodic_registration_updating.
09:29:57.468964 14031 - Final verdict of PTC: none
09:29:57.469436 14031 - Disconnected from MC.
09:29:57.469528 13795 C5G_Tests.ttcn:331 Setting final verdict of the test case.
09:29:57.469658 14031 - TTCN-3 Parallel Test Component finished.
09:29:57.469719 13795 C5G_Tests.ttcn:331 Local verdict of MTC: pass
09:29:57.469976 13795 C5G_Tests.ttcn:331 Local verdict of PTC GTP1U_EM(12): none (pass -> pass)
09:29:57.470154 13795 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating-NGAP0(13): none (pass -> pass)
09:29:57.470327 13795 C5G_Tests.ttcn:331 Local verdict of PTC TC_periodic_registration_updating0(14): none (pass -> pass)
09:29:57.470602 13795 C5G_Tests.ttcn:331 Test case TC_periodic_registration_updating finished. Verdict: pass
09:29:57.470830 13795 C5G_Tests.ttcn:331 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass'.
09:29:59.542754 13795 C5G_Tests.ttcn:331 External command `/home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/ttcn3-tcpdump-stop.sh C5G_Tests.TC_periodic_registration_updating pass' was executed successfully (exit status: 0).
09:29:59.542973 13795 C5G_Tests.ttcn:339 Switching to log file `C5G_Tests-TC_ue_context_release_no_pdu_session-3c561e6ea320-mtc-13795.log'
