+ CONFIG=sccplite
+ SITE_ID=1236
+ TRX_NUM=4
+ BTS_FEATURES=-fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX
+ respawn.sh osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
respawn: 0: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;31mDLINP[0;m[38;5;23m stream_cli.c:424 CLICONN(ts-0-1-oml,){CONNECTING} connect failed (-111)[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5601dda35090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5601dda388b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5601dda3bfd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5601dda3f6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40535){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5601dda34790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5601dda34790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5601dda34790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 0: stopped pid 9718 with status 0
respawn: 1: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f79d960090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55f79d9638b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55f79d966fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55f79d96a6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Unlocked -> Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Unlocked -> Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Unlocked -> Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Unlocked -> Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41399){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f79d95f790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f79d95f790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f79d95f790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 1: stopped pid 10072 with status 0
respawn: 2: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5654a7379090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5654a737c8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5654a737ffd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5654a73836f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33089){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5654a7378790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5654a7378790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5654a7378790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 2: stopped pid 16327 with status 0
respawn: 3: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5607728ed090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5607728f08b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5607728f3fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5607728f76f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41275){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5607728ec790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5607728ec790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5607728ec790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 3: stopped pid 16414 with status 0
respawn: 4: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562b889cd090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x562b889d08b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x562b889d3fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x562b889d76f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45237){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562b889cc790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562b889cc790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562b889cc790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 4: stopped pid 16492 with status 0
respawn: 5: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55bde2b3f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55bde2b428b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55bde2b45fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55bde2b496f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37643){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55bde2b3e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55bde2b3e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55bde2b3e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 5: stopped pid 16579 with status 0
respawn: 6: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556c724cd090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x556c724d08b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x556c724d3fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x556c724d76f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39969){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556c724cc790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556c724cc790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556c724cc790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 6: stopped pid 16655 with status 0
respawn: 7: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a3c1b3b090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55a3c1b3e8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55a3c1b41fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55a3c1b456f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37827){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a3c1b3a790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a3c1b3a790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a3c1b3a790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 7: stopped pid 16742 with status 0
respawn: 8: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5581fd49d090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5581fd4a08b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5581fd4a3fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5581fd4a76f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38817){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5581fd49c790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5581fd49c790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5581fd49c790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 8: stopped pid 16824 with status 0
respawn: 9: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a65aa03090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55a65aa068b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55a65aa09fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55a65aa0d6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43229){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a65aa02790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a65aa02790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a65aa02790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 9: stopped pid 16907 with status 0
respawn: 10: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556dcaea5090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x556dcaea88b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x556dcaeabfd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x556dcaeaf6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34447){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556dcaea4790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556dcaea4790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556dcaea4790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 10: stopped pid 16991 with status 0
respawn: 11: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5587ec002090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5587ec0058b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5587ec008fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5587ec00c6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33113){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5587ec001790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5587ec001790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5587ec001790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 11: stopped pid 17070 with status 0
respawn: 12: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a706a88090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55a706a8b8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55a706a8efd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55a706a926f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40603){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a706a87790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a706a87790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a706a87790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 12: stopped pid 17150 with status 0
respawn: 13: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561f7c442090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x561f7c4458b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x561f7c448fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x561f7c44c6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35917){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561f7c441790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561f7c441790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561f7c441790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 13: stopped pid 17235 with status 0
respawn: 14: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c90964c090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55c90964f8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55c909652fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55c9096566f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39727){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c90964b790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c90964b790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c90964b790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 14: stopped pid 17308 with status 0
respawn: 15: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d122400090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55d1224038b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55d122406fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55d12240a6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42251){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d1223ff790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d1223ff790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d1223ff790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 15: stopped pid 17389 with status 0
respawn: 16: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563eb1aa3090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x563eb1aa68b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x563eb1aa9fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x563eb1aad6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42773){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563eb1aa2790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563eb1aa2790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563eb1aa2790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 16: stopped pid 17463 with status 0
respawn: 17: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5634e746d090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5634e74708b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5634e7473fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5634e74776f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34257){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5634e746c790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5634e746c790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5634e746c790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 17: stopped pid 17545 with status 0
respawn: 18: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x563ca45f2090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x563ca45f58b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x563ca45f8fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x563ca45fc6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40563){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x563ca45f1790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x563ca45f1790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x563ca45f1790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 18: stopped pid 17627 with status 0
respawn: 19: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d09f53f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55d09f5428b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55d09f545fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55d09f5496f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35309){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d09f53e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d09f53e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d09f53e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 19: stopped pid 17704 with status 0
respawn: 20: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5654ba2cb090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5654ba2ce8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5654ba2d1fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5654ba2d56f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41305){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5654ba2ca790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5654ba2ca790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5654ba2ca790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 20: stopped pid 17782 with status 0
respawn: 21: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55dae2e58090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55dae2e5b8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55dae2e5efd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55dae2e626f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33247){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55dae2e57790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55dae2e57790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55dae2e57790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 21: stopped pid 17861 with status 0
respawn: 22: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c2c051a090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55c2c051d8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55c2c0520fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55c2c05246f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43387){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c2c0519790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c2c0519790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c2c0519790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 22: stopped pid 17946 with status 0
respawn: 23: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c2fd5ea090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55c2fd5ed8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55c2fd5f0fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55c2fd5f46f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45789){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c2fd5e9790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c2fd5e9790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c2fd5e9790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 23: stopped pid 18252 with status 0
respawn: 24: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559182b32090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x559182b358b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x559182b38fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x559182b3c6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39041){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559182b31790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559182b31790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559182b31790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 24: stopped pid 21165 with status 0
respawn: 25: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559c11063090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x559c110668b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x559c11069fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x559c1106d6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43915){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559c11062790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559c11062790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559c11062790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 25: stopped pid 21256 with status 0
respawn: 26: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561c865ad090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x561c865b08b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x561c865b3fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x561c865b76f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36961){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561c865ac790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561c865ac790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561c865ac790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 26: stopped pid 21351 with status 0
respawn: 27: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c1f6d8c090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55c1f6d8f8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55c1f6d92fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55c1f6d966f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46225){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c1f6d8b790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c1f6d8b790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c1f6d8b790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 27: stopped pid 21438 with status 0
respawn: 28: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fffdaeb090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55fffdaee8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55fffdaf1fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55fffdaf56f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35199){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fffdaea790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fffdaea790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fffdaea790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 28: stopped pid 21530 with status 0
respawn: 29: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5650118ba090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5650118bd8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5650118c0fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5650118c46f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33391){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5650118b9790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5650118b9790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5650118b9790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 29: stopped pid 21617 with status 0
respawn: 30: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5572607d3090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x5572607d68b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x5572607d9fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x5572607dd6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42281){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5572607d2790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5572607d2790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5572607d2790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 30: stopped pid 21708 with status 0
respawn: 31: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55dcd240f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55dcd24128b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55dcd2415fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55dcd24196f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38739){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55dcd240e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55dcd240e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55dcd240e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 31: stopped pid 21784 with status 0
respawn: 32: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56206fb64090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x56206fb678b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x56206fb6afd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x56206fb6e6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41883){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56206fb63790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56206fb63790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56206fb63790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 32: stopped pid 21876 with status 0
respawn: 33: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55623b6e9090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55623b6ec8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55623b6effd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55623b6f36f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35795){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55623b6e8790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55623b6e8790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55623b6e8790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 33: stopped pid 21965 with status 0
respawn: 34: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f021c32090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x55f021c358b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x55f021c38fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x55f021c3c6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39123){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f021c31790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f021c31790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f021c31790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 34: stopped pid 24963 with status 0
respawn: 35: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562f629c3090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x562f629c68b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x562f629c9fd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x562f629cd6f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39417){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562f629c2790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562f629c2790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562f629c2790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 35: stopped pid 25047 with status 0
respawn: 36: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1236 4
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1236/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,01,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,01,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,01,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,02,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,02,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,02,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,03,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,03,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,03,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,01,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,02,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,03,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x557cc1919090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx1)[0x557cc191c8b0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx2)[0x557cc191ffd0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx3)[0x557cc19236f0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
