+ CONFIG=vamos
+ SITE_ID=1234
+ TRX_NUM=1
+ BTS_FEATURES=-fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX
+ respawn.sh osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
respawn: 0: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;31mDLINP[0;m[38;5;23m stream_cli.c:444 CLICONN(ts-0-1-oml,){CONNECTING} connect failed (-111)[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38395){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;31mDABIS[0;m abis.c:105 OML link was closed early within 4 seconds. If this situation persists, please check your BTS and BSC configuration files for errors. A common error is a mismatch between unit_id configuration parameters of BTS and BSC.
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5120000006a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5120000006a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5120000006a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 0: stopped pid 9849 with status 0
respawn: 1: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:32937){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5120000006a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5120000006a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5120000006a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 1: stopped pid 9929 with status 0
respawn: 2: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37175){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5120000006a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5120000006a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5120000006a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 2: stopped pid 10001 with status 0
respawn: 3: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43459){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5120000006a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5120000006a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5120000006a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 3: stopped pid 10076 with status 0
respawn: 4: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33555){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5120000006a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5120000006a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5120000006a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 4: stopped pid 10149 with status 0
respawn: 5: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46635){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5120000006a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5120000006a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5120000006a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 5: stopped pid 10224 with status 0
respawn: 6: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:567 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39135){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5120000006a0]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:934 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5120000006a0]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5120000006a0]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 6: stopped pid 10304 with status 0
respawn: 7: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,VAMOS,OSMUX 127.0.0.1 1234 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1079 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:901 received ID_GET for unit ID 1234/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x512000000ca0]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
