\doxysection{gmr1\+\_\+pi4cxpsk\+\_\+burst Struct Reference}
\label{structgmr1__pi4cxpsk__burst}\index{gmr1\_pi4cxpsk\_burst@{gmr1\_pi4cxpsk\_burst}}


pi4-\/\+Cx\+PSK Burst format description  




{\ttfamily \#include $<$pi4cxpsk.\+h$>$}

\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
\mbox{\label{structgmr1__pi4cxpsk__burst_a835af391ae1715b41cbdd52efd1b378a}} 
struct \textbf{ gmr1\+\_\+pi4cxpsk\+\_\+modulation} $\ast$ {\bfseries mod}
\begin{DoxyCompactList}\small\item\em Modulation scheme ~\newline
 \end{DoxyCompactList}\item 
\mbox{\label{structgmr1__pi4cxpsk__burst_a30a0e6c90559f9b66def7814fe8f9af2}} 
int {\bfseries guard\+\_\+pre}
\begin{DoxyCompactList}\small\item\em Beginning guard period. \end{DoxyCompactList}\item 
\mbox{\label{structgmr1__pi4cxpsk__burst_a5985baf01b937f381470bb0d5810ea00}} 
int {\bfseries guard\+\_\+post}
\begin{DoxyCompactList}\small\item\em End guard period ~\newline
 \end{DoxyCompactList}\item 
\mbox{\label{structgmr1__pi4cxpsk__burst_ad164674725c949673b0a2ec24e0f0000}} 
int {\bfseries len}
\begin{DoxyCompactList}\small\item\em Total len with guard. \end{DoxyCompactList}\item 
\mbox{\label{structgmr1__pi4cxpsk__burst_a8205aeb2d88053361619f1baa0593a89}} 
int {\bfseries ebits}
\begin{DoxyCompactList}\small\item\em Number of encoded bits. \end{DoxyCompactList}\item 
\mbox{\label{structgmr1__pi4cxpsk__burst_a68e57bf2eeee31d4a9f5efb2dfb7a145}} 
struct \textbf{ gmr1\+\_\+pi4cxpsk\+\_\+sync} $\ast$ {\bfseries sync} [\textbf{ GMR1\+\_\+\+MAX\+\_\+\+SYNC}]
\begin{DoxyCompactList}\small\item\em Sync sequences. \end{DoxyCompactList}\item 
\mbox{\label{structgmr1__pi4cxpsk__burst_a743e2058421775d2033d5e455e7be163}} 
struct \textbf{ gmr1\+\_\+pi4cxpsk\+\_\+data} $\ast$ {\bfseries data}
\begin{DoxyCompactList}\small\item\em Data chunks. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
pi4-\/\+Cx\+PSK Burst format description 

The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
include/osmocom/gmr1/sdr/\textbf{ pi4cxpsk.\+h}\end{DoxyCompactItemize}
