08:48:41.540989 9718 BSC_Tests.ttcn:3187 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc0_connection_status'.
08:48:42.551736 9718 BSC_Tests.ttcn:3187 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc0_connection_status' was executed successfully (exit status: 0).
08:48:42.551953 9718 BSC_Tests.ttcn:3187 Test case TC_ctrl_msc0_connection_status started.
08:48:42.552039 9718 BSC_Tests.ttcn:3187 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:42.552752 9718 BSC_Tests.ttcn:3187 Port IPA_CTRL was started.
08:48:42.552848 9718 BSC_Tests.ttcn:3187 Port RSL_CCHAN[0] was started.
08:48:42.552923 9718 BSC_Tests.ttcn:3187 Port RSL_CCHAN[1] was started.
08:48:42.552990 9718 BSC_Tests.ttcn:3187 Port RSL_CCHAN[2] was started.
08:48:42.553054 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[0][0] was started.
08:48:42.553121 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[0][1] was started.
08:48:42.553186 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[0][2] was started.
08:48:42.553248 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[0][3] was started.
08:48:42.553310 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[1][0] was started.
08:48:42.553372 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[1][1] was started.
08:48:42.553434 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[1][2] was started.
08:48:42.553497 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[1][3] was started.
08:48:42.553559 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[2][0] was started.
08:48:42.553620 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[2][1] was started.
08:48:42.553681 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[2][2] was started.
08:48:42.553742 9718 BSC_Tests.ttcn:3187 Port IPA_RSL[2][3] was started.
08:48:42.553804 9718 BSC_Tests.ttcn:3187 Port IPA was started.
08:48:42.553867 9718 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CTRL was started.
08:48:42.553931 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][0] was started.
08:48:42.553993 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][1] was started.
08:48:42.554096 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][2] was started.
08:48:42.554160 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][3] was started.
08:48:42.554222 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][0] was started.
08:48:42.554284 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][1] was started.
08:48:42.554351 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][2] was started.
08:48:42.554571 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][3] was started.
08:48:42.554634 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][0] was started.
08:48:42.554707 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][1] was started.
08:48:42.554891 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][2] was started.
08:48:42.554972 9718 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][3] was started.
08:48:42.555032 9718 BSC_Tests.ttcn:3187 Port BSCVTY was started.
08:48:42.555090 9718 BSC_Tests.ttcn:3187 Port STPVTY was started.
08:48:42.555137 9718 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CFG_PORT[0] was started.
08:48:42.555189 9718 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CFG_PORT[1] was started.
08:48:42.555247 9718 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CFG_PORT[2] was started.
08:48:42.555294 9718 BSC_Tests.ttcn:3187 Port BSSAP was started.
08:48:42.555345 9718 BSC_Tests.ttcn:3187 Port BSSAP_LE was started.
08:48:42.555402 9718 BSC_Tests.ttcn:3187 Component type BSC_Tests.test_CT was initialized.
08:48:42.555463 9718 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
08:48:42.555526 9718 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
08:48:42.555603 9718 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
08:48:42.556263 9718 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
08:48:42.556381 9718 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
08:48:42.556528 9718 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
08:48:42.556668 9718 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:42.557009 9718 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:42.557279 9718 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:42.557511 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
08:48:42.557638 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.557738 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:42.557848 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:42.557922 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:42.557989 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:42.558055 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:42.558127 9718 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
08:48:42.558201 9718 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
08:48:42.558280 9718 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
08:48:42.558483 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
08:48:42.558639 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.558769 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.558842 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:42.558920 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
08:48:42.558996 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.559082 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:42.559183 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.559462 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
08:48:42.559592 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.559711 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.559867 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.560006 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
08:48:42.560083 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
08:48:42.560164 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.560313 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
08:48:42.560404 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.560889 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
08:48:42.561172 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.561534 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.561786 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.561893 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
08:48:42.561976 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
08:48:42.562236 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.562444 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
08:48:42.562588 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.562805 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
08:48:42.562945 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.563061 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.563199 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.563309 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
08:48:42.563405 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
08:48:42.563492 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.563699 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
08:48:42.563842 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.564063 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
08:48:42.564225 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.564353 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.564501 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.564679 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
08:48:42.564755 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
08:48:42.564875 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.565024 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:42.565168 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.565474 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
08:48:42.565815 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.566319 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.566468 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
08:48:42.566560 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
08:48:42.566819 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.566996 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:42.567176 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.567478 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
08:48:42.567740 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.567979 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.568169 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.568257 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
08:48:42.568455 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
08:48:42.568585 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.568742 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:42.568860 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.569070 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
08:48:42.569204 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.569318 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.569452 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.569526 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
08:48:42.569602 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
08:48:42.569683 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.569859 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:42.570105 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.570376 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
08:48:42.570580 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.570852 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.571070 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.571261 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
08:48:42.571402 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
08:48:42.571536 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.571663 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:42.571852 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.572219 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
08:48:42.572393 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.572522 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.572689 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.572775 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
08:48:42.572858 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
08:48:42.572959 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.573051 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:42.573182 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.573298 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
08:48:42.573432 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.573542 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.573615 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
08:48:42.573692 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
08:48:42.573767 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.573854 9718 StatsD_Checker.ttcnpp:404 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:42.581893 9812 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:42.582042 9812 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-STATS(10), component type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS. Version: 11.1.0.
08:48:42.582082 9812 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:42.582148 9812 - Connected to MC.
08:48:42.582176 9812 - Initializing variables, timers and ports of component type StatsD_Checker.StatsD_Checker_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:42.582202 9718 StatsD_Checker.ttcnpp:404 PTC was created. Component reference: 10, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:42.582257 9718 StatsD_Checker.ttcnpp:405 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(10).
08:48:42.582350 9718 StatsD_Checker.ttcnpp:405 Function was started.
08:48:42.582395 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
08:48:42.582450 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.582665 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
08:48:42.582744 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.582843 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.582979 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
08:48:42.583079 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
08:48:42.583168 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.583257 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
08:48:42.583373 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.583563 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 1" id 14
08:48:42.583763 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
08:48:42.583928 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.584114 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.584251 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:42.584493 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:42.584660 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 1" with ? matched
08:48:42.584777 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 1" id 14
08:48:42.584888 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 14 was extracted from the queue of BSCVTY.
08:48:42.585160 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.585353 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.585476 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
08:48:42.585585 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
08:48:42.585628 9812 - Port STATSVTY was started.
08:48:42.585745 9812 - Port STATSD_PROC was started.
08:48:42.585747 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.585821 9812 - Port STATS was started.
08:48:42.585893 9812 - Component type StatsD_Checker.StatsD_Checker_CT was initialized.
08:48:42.586026 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
08:48:42.586133 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.586153 9812 - Starting function main("127.0.0.1", 8125, 5.000000).
08:48:42.586294 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 2" id 16
08:48:42.586354 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
08:48:42.586477 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.586586 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.586694 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:42.586769 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:42.586783 9812 StatsD_Checker.ttcnpp:120 Mapping port VirtMSC-STATS(10):STATS to system:STATS.
08:48:42.586851 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 2" with ? matched
08:48:42.586917 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 2" id 16
08:48:42.586982 9812 StatsD_Checker.ttcnpp:120 Port STATS was mapped to system:STATS.
08:48:42.586986 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
08:48:42.587099 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.587114 9812 StatsD_Checker.ttcnpp:120 Map operation of VirtMSC-STATS(10):STATS to system:STATS finished.
08:48:42.587228 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.587297 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
08:48:42.587364 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
08:48:42.587435 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.587617 9718 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:42.587649 9812 StatsD_Checker.ttcnpp:121 entering f__IPL4__PROVIDER__listen: 127.0.0.1:8125 / UDP
08:48:42.589701 9812 StatsD_Checker.ttcnpp:129 Mapping port VirtMSC-STATS(10):STATSVTY to system:STATSVTY.
08:48:42.590306 9812 StatsD_Checker.ttcnpp:129 Message enqueued on STATSVTY from system integer : 2 id 1
08:48:42.590435 9812 StatsD_Checker.ttcnpp:129 Port STATSVTY was mapped to system:STATSVTY.
08:48:42.590483 9812 StatsD_Checker.ttcnpp:129 Map operation of VirtMSC-STATS(10):STATSVTY to system:STATSVTY finished.
08:48:42.590731 9812 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:42.590846 9812 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:42.590887 9812 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:42.591087 9812 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "enable"
08:48:42.591188 9812 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.591265 9812 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:42.591288 9812 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:42.591329 9812 Osmocom_VTY_Functions.ttcn:74 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:42.591356 9812 Osmocom_VTY_Functions.ttcn:75 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:42.591394 9812 Osmocom_VTY_Functions.ttcn:85 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:42.591487 9812 Osmocom_VTY_Functions.ttcn:86 Matching on port STATSVTY succeeded: 2 with ? matched
08:48:42.591535 9812 Osmocom_VTY_Functions.ttcn:86 Receive operation on port STATSVTY succeeded, message from system(): integer : 2 id 1
08:48:42.591568 9812 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of STATSVTY.
08:48:42.591691 9812 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 2
08:48:42.591790 9812 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.591834 9812 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.591857 9812 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:42.591886 9812 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of STATSVTY.
08:48:42.591928 9812 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.591971 9812 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "stats reset"
08:48:42.592005 9812 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.592051 9812 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 3
08:48:42.592062 9813 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:42.592085 9812 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.592118 9812 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.592140 9812 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 3
08:48:42.592159 9812 Osmocom_VTY_Functions.ttcn:73 Message with id 3 was extracted from the queue of STATSVTY.
08:48:42.592170 9813 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-SCCP(11), component type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP. Version: 11.1.0.
08:48:42.592182 9812 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.592200 9813 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:42.592249 9813 - Connected to MC.
08:48:42.592272 9813 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:42.592287 9718 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 11, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:42.592325 9718 SCCP_Adapter.ttcnpp:131 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:42.594023 9813 - Port SCCP_SP_PORT was started.
08:48:42.594068 9813 - Port MTP3_SCCP_PORT was started.
08:48:42.594086 9813 - Component type SCCP_Emulation.SCCP_CT was initialized.
08:48:42.595332 9814 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:42.595402 9814 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-IPA(12), component type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA. Version: 11.1.0.
08:48:42.595422 9814 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:42.595457 9814 - Connected to MC.
08:48:42.595474 9814 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:42.595486 9718 SCCP_Adapter.ttcnpp:131 PTC was created. Component reference: 12, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:42.595516 9718 SCCP_Adapter.ttcnpp:132 Mapping port VirtMSC-IPA(12):IPA_PORT to system:IPA_CODEC_PT.
08:48:42.596338 9814 - Port IPA_PORT was started.
08:48:42.596361 9814 - Port CFG_PORT was started.
08:48:42.596375 9814 - Port MTP3_SP_PORT was started.
08:48:42.596388 9814 - Port IPA_MGCP_PORT was started.
08:48:42.596402 9814 - Port IPA_RSL_PORT was started.
08:48:42.596415 9814 - Port IPA_OML_PORT was started.
08:48:42.596429 9814 - Port IPA_CTRL_PORT was started.
08:48:42.596443 9814 - Port IPA_SP_PORT was started.
08:48:42.596456 9814 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:42.596489 9814 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:42.596517 9718 SCCP_Adapter.ttcnpp:132 Map operation of VirtMSC-IPA(12):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:42.596538 9718 SCCP_Adapter.ttcnpp:134 Connecting ports VirtMSC-IPA(12):MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT.
08:48:42.596758 9813 - Port MTP3_SCCP_PORT is waiting for connection from VirtMSC-IPA(12):MTP3_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-8e78f476.
08:48:42.596784 9814 - Port MTP3_SP_PORT has established the connection with VirtMSC-SCCP(11):MTP3_SCCP_PORT using transport type UNIX.
08:48:42.596825 9813 - Port MTP3_SCCP_PORT has accepted the connection from VirtMSC-IPA(12):MTP3_SP_PORT.
08:48:42.596832 9718 SCCP_Adapter.ttcnpp:134 Connect operation on VirtMSC-IPA(12):MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT finished.
08:48:42.596848 9718 SCCP_Adapter.ttcnpp:136 Creating new alive PTC with component type IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:42.598860 9815 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:42.598930 9815 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-IPA-WAIT(13), component type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT. Version: 11.1.0.
08:48:42.598948 9815 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:42.598987 9815 - Connected to MC.
08:48:42.599012 9815 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_EventWaiter_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:42.599028 9718 SCCP_Adapter.ttcnpp:136 PTC was created. Component reference: 13, alive: yes, type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:42.599053 9718 SCCP_Adapter.ttcnpp:137 Connecting ports VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:42.599229 9814 - Port IPA_SP_PORT is waiting for connection from VirtMSC-IPA-WAIT(13):IPA_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-ab6bb203.
08:48:42.599798 9815 - Port IPA_SP_PORT was started.
08:48:42.599823 9815 - Component type IPA_Emulation.IPA_EventWaiter_CT was initialized.
08:48:42.599859 9815 - Port IPA_SP_PORT has established the connection with VirtMSC-IPA(12):IPA_SP_PORT using transport type UNIX.
08:48:42.599892 9814 - Port IPA_SP_PORT has accepted the connection from VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:42.599904 9718 SCCP_Adapter.ttcnpp:137 Connect operation on VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT finished.
08:48:42.599922 9718 SCCP_Adapter.ttcnpp:138 Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}) on component VirtMSC-IPA-WAIT(13).
08:48:42.599960 9718 SCCP_Adapter.ttcnpp:138 Function was started.
08:48:42.599981 9718 SCCP_Adapter.ttcnpp:140 Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true) on component VirtMSC-IPA(12).
08:48:42.600019 9718 SCCP_Adapter.ttcnpp:140 Function was started.
08:48:42.600087 9815 - Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}).
08:48:42.600094 9814 - Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true).
08:48:42.600279 9814 IPA_Emulation.ttcnpp:332 entering f__IPL4__PROVIDER__listen: 127.0.0.1:5000 / TCP
08:48:46.427357 9814 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:46.428209 9814 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:46.428396 9814 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:46.428623 9814 IPA_Emulation.ttcnpp:830 Matching on port IPA_PORT succeeded:  matched
08:48:46.428931 9814 IPA_Emulation.ttcnpp:830 Receive operation on port IPA_PORT succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:46.429121 9814 IPA_Emulation.ttcnpp:830 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:46.429276 9814 IPA_Emulation.ttcnpp:832 Established a new IPA connection (conn_id=2)
08:48:46.429871 9814 IPA_Emulation.ttcnpp:381 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(13) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
}
08:48:46.430213 9815 IPA_Emulation.ttcnpp:965 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(12) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:46.430275 9814 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:46.430415 9814 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:46.430443 9815 IPA_Emulation.ttcnpp:966 Matching on port IPA_SP_PORT ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:46.430495 9815 IPA_Emulation.ttcnpp:969 Matching on port IPA_SP_PORT succeeded.
08:48:46.430518 9815 IPA_Emulation.ttcnpp:969 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(12): @IPA_Emulation.ASP_IPA_Event: {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:46.430543 9815 IPA_Emulation.ttcnpp:969 Message with id 1 was extracted from the queue of IPA_SP_PORT.
08:48:46.430573 9814 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:46.430842 9814 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:46.430963 9814 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:46.431018 9814 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:46.431094 9814 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:46.431354 9814 IPA_Emulation.ttcnpp:745 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:46.431614 9814 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:46.431787 9814 IPA_Emulation.ttcnpp:381 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(13) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
}
08:48:46.431950 9815 IPA_Emulation.ttcnpp:965 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(12) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:46.432033 9814 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE00'O
} id 3
08:48:46.432135 9815 IPA_Emulation.ttcnpp:966 Matching on port IPA_SP_PORT succeeded:  matched
08:48:46.432219 9814 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:46.432235 9815 IPA_Emulation.ttcnpp:966 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(12): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:46.432327 9815 IPA_Emulation.ttcnpp:966 Message with id 2 was extracted from the queue of IPA_SP_PORT.
08:48:46.432360 9814 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:46.432445 9815 IPA_Emulation.ttcnpp:967 setverdict(pass): none -> pass
08:48:46.432482 9814 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:46.432599 9815 - Function waiter_main finished. PTC remains alive and is waiting for next start.
08:48:46.432600 9814 IPA_Emulation.ttcnpp:745 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:46.432776 9814 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_PING (0),
    u := omit
}
08:48:46.432830 9718 SCCP_Adapter.ttcnpp:151 PTC with component reference 13 is done.
08:48:46.432930 9814 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_PONG (1),
    u := omit
}
08:48:46.432951 9718 SCCP_Adapter.ttcnpp:152 Disconnecting ports VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:46.433116 9814 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '01'O
}
08:48:46.433447 9814 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE01'O
}
08:48:46.433628 9815 - Terminating the connection of port IPA_SP_PORT to VirtMSC-IPA(12):IPA_SP_PORT. No more messages can be sent through this connection.
08:48:46.433777 9814 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0016FD090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:46.433920 9814 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:46.434242 9814 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_SCCP (253) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:46.434335 9814 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:46.434411 9814 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:46.434570 9814 IPA_Emulation.ttcnpp:761 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:46.435774 9814 IPA_Emulation.ttcnpp:767 Sent on MTP3_SP_PORT to VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
}
08:48:46.436171 9814 IPA_Emulation.ttcnpp:743 Connection termination request was received on port IPA_SP_PORT from VirtMSC-IPA-WAIT(13):IPA_SP_PORT. No more data can be sent or received through this connection.
08:48:46.436295 9815 - Port IPA_SP_PORT was disconnected from VirtMSC-IPA(12):IPA_SP_PORT.
08:48:46.436422 9814 IPA_Emulation.ttcnpp:743 Port IPA_SP_PORT was disconnected from VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:46.436508 9718 SCCP_Adapter.ttcnpp:152 Disconnect operation on VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT finished.
08:48:46.436800 9718 BSC_Tests.ttcn:1221 Connecting ports mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT.
08:48:46.436807 9813 - Message enqueued on MTP3_SCCP_PORT from VirtMSC-IPA(12) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 1
08:48:46.437728 9718 BSC_Tests.ttcn:1221 Port SCCPLITE_IPA_CFG_PORT[0] is waiting for connection from VirtMSC-IPA(12):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-5f07b44b.
08:48:46.437878 9814 IPA_Emulation.ttcnpp:743 Port CFG_PORT has established the connection with mtc:SCCPLITE_IPA_CFG_PORT[0] using transport type UNIX.
08:48:46.438063 9718 BSC_Tests.ttcn:1221 Port SCCPLITE_IPA_CFG_PORT[0] has accepted the connection from VirtMSC-IPA(12):CFG_PORT.
08:48:46.438207 9718 BSC_Tests.ttcn:1221 Connect operation on mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT finished.
08:48:46.438328 9718 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:46.439071 9718 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(11):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-4a7cb81d.
08:48:46.439320 9813 - Incoming message was mapped to @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:46.439643 9813 - Port SCCP_SP_PORT has established the connection with mtc:BSSAP using transport type UNIX.
08:48:46.439799 9718 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:46.439937 9718 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT finished.
08:48:46.440056 9718 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}) on component VirtMSC-SCCP(11).
08:48:46.440284 9718 SCCP_Adapter.ttcnpp:165 Function was started.
08:48:46.440619 9813 - Starting function SCCPStart({
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}).
08:48:46.440753 9718 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(11) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 0,
                        causeValue := '0000000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:48:46.440874 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 0,
                    causeValue := '0000000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:46.441004 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
08:48:46.441087 9718 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
}
08:48:46.441227 9718 BSC_Tests.ttcn:899 Start timer T: 5 s
08:48:46.441329 9813 SCCP_Emulation.ttcn:1453 v_sccp_pdu_maxlen:268
08:48:46.442350 9813 SCCP_Emulation.ttcn:5443 Matching on port MTP3_SCCP_PORT succeeded:  matched
08:48:46.442510 9813 SCCP_Emulation.ttcn:5443 Receive operation on port MTP3_SCCP_PORT succeeded, message from VirtMSC-IPA(12): @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:46.442671 9813 SCCP_Emulation.ttcn:5443 Message with id 1 was extracted from the queue of MTP3_SCCP_PORT.
08:48:46.444494 9813 SCCP_Emulation.ttcn:3464 Sent on SCCP_SP_PORT to mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
}
08:48:46.445032 9718 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(11) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
} id 1
08:48:46.445187 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000430040120'O
08:48:46.445680 9813 SCCP_Emulation.ttcn:5439 Message enqueued on SCCP_SP_PORT from mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:46.445830 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 4,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 1,
                    causeValue := '0100000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:46.445970 9718 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:46.445987 9813 SCCP_Emulation.ttcn:5577 Matching on port SCCP_SP_PORT succeeded.
08:48:46.446134 9718 BSC_Tests.ttcn:901 Matching on port BSSAP .userData.pdu.bssmap{
    reset := {
        messageType := '30'O ("0"),
        cause := {
            elementIdentifier := '04'O,
            lengthIndicator := 1,
            causeValue := '0100000'B,
            extensionCauseValue := '0'B,
            spare1 := omit
        },
        a_InterfaceSelectorForReset := omit,
        osmuxSupport := omit
    }
} with {
    resetAck := {
        messageType := '31'O ("1"),
        a_InterfaceSelectorForReset := *,
        osmuxSupport := omit
    }
} unmatched: First message in the queue does not match the template: 
08:48:46.446296 9718 BSC_Tests.ttcn:905 Matching on port BSSAP succeeded:  matched
08:48:46.446322 9813 SCCP_Emulation.ttcn:5577 Check-receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req: {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:46.446400 9718 BSC_Tests.ttcn:905 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(11): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:46.446423 9813 SCCP_Emulation.ttcn:5585 Matching on port SCCP_SP_PORT failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_DATA_req.
08:48:46.446485 9718 BSC_Tests.ttcn:905 Message with id 1 was extracted from the queue of BSSAP.
08:48:46.446608 9718 BSC_Tests.ttcn:906 BSSMAP: Respoding to inbound RESET with RESET-ACK
08:48:46.446726 9813 SCCP_Emulation.ttcn:5591 Matching on port SCCP_SP_PORT succeeded:  matched
08:48:46.446858 9813 SCCP_Emulation.ttcn:5591 Receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:46.447118 9813 SCCP_Emulation.ttcn:5591 Message with id 1 was extracted from the queue of SCCP_SP_PORT.
08:48:46.447226 9718 BSC_Tests.ttcn:907 Sent on BSSAP to VirtMSC-SCCP(11) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:48:46.447527 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:46.447680 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000131'O
08:48:46.447764 9718 BSC_Tests.ttcn:907 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
}
08:48:46.449751 9813 SCCP_Emulation.ttcn:5223 Sent on MTP3_SCCP_PORT to VirtMSC-IPA(12) @SCCP_Types.ASP_MTP3_TRANSFERreq_sccp : {
    sio := '83'O,
    opc := 185,
    dpc := 187,
    sls := 0,
    data := {
        unitdata := {
            messageType := 9,
            protClass := {
                class := '0000'B,
                messageHandling := '0000'B
            },
            pointer1 := 0,
            pointer2 := 0,
            pointer3 := 0,
            calledPAddress := {
                paramLength := 4,
                addr := '43BB00FE'O
            },
            callingPAddress := {
                paramLength := 4,
                addr := '43B900FE'O
            },
            data := {
                paramLength := 6,
                data := '000430040100'O
            }
        }
    }
}
08:48:46.450623 9813 SCCP_Emulation.ttcn:5223 Outgoing message was mapped to @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:46.451190 9814 IPA_Emulation.ttcnpp:743 Message enqueued on MTP3_SP_PORT from VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
} id 1
08:48:46.451364 9813 SCCP_Emulation.ttcn:5439 Message enqueued on SCCP_SP_PORT from mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:46.451474 9813 SCCP_Emulation.ttcn:5577 Matching on port SCCP_SP_PORT succeeded.
08:48:46.451563 9813 SCCP_Emulation.ttcn:5577 Check-receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req: {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:46.451569 9814 IPA_Emulation.ttcnpp:865 Matching on port MTP3_SP_PORT succeeded:  matched
08:48:46.451655 9813 SCCP_Emulation.ttcn:5585 Matching on port SCCP_SP_PORT failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_DATA_req.
08:48:46.451694 9814 IPA_Emulation.ttcnpp:865 Receive operation on port MTP3_SP_PORT succeeded, message from VirtMSC-SCCP(11): @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
} id 1
08:48:46.451825 9814 IPA_Emulation.ttcnpp:865 Message with id 1 was extracted from the queue of MTP3_SP_PORT.
08:48:46.451860 9813 SCCP_Emulation.ttcn:5591 Matching on port SCCP_SP_PORT succeeded:  matched
08:48:46.451965 9814 IPA_Emulation.ttcnpp:868 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:46.451977 9813 SCCP_Emulation.ttcn:5591 Receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:46.452076 9814 IPA_Emulation.ttcnpp:868 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0016FD090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:46.452084 9813 SCCP_Emulation.ttcn:5591 Message with id 2 was extracted from the queue of SCCP_SP_PORT.
08:48:46.452362 9813 SCCP_Emulation.ttcn:5223 Sent on MTP3_SCCP_PORT to VirtMSC-IPA(12) @SCCP_Types.ASP_MTP3_TRANSFERreq_sccp : {
    sio := '83'O,
    opc := 185,
    dpc := 187,
    sls := 0,
    data := {
        unitdata := {
            messageType := 9,
            protClass := {
                class := '0000'B,
                messageHandling := '0000'B
            },
            pointer1 := 0,
            pointer2 := 0,
            pointer3 := 0,
            calledPAddress := {
                paramLength := 4,
                addr := '43BB00FE'O
            },
            callingPAddress := {
                paramLength := 4,
                addr := '43B900FE'O
            },
            data := {
                paramLength := 3,
                data := '000131'O
            }
        }
    }
}
08:48:46.452492 9813 SCCP_Emulation.ttcn:5223 Outgoing message was mapped to @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:46.452660 9814 IPA_Emulation.ttcnpp:743 Message enqueued on MTP3_SP_PORT from VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 2
08:48:46.453022 9814 IPA_Emulation.ttcnpp:865 Matching on port MTP3_SP_PORT succeeded:  matched
08:48:46.453363 9814 IPA_Emulation.ttcnpp:865 Receive operation on port MTP3_SP_PORT succeeded, message from VirtMSC-SCCP(11): @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 2
08:48:46.453545 9814 IPA_Emulation.ttcnpp:865 Message with id 2 was extracted from the queue of MTP3_SP_PORT.
08:48:46.453696 9814 IPA_Emulation.ttcnpp:868 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:46.453850 9814 IPA_Emulation.ttcnpp:868 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0013FD090003070B0443BB00FE0443B900FE03000131'O
}
08:48:46.477206 9814 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0013FD090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:46.477387 9814 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:46.477489 9814 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_SCCP (253) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:46.477572 9814 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:46.477647 9814 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:46.477806 9814 IPA_Emulation.ttcnpp:761 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:46.477914 9814 IPA_Emulation.ttcnpp:767 Sent on MTP3_SP_PORT to VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE03000131'O
}
08:48:46.478010 9813 SCCP_Emulation.ttcn:5439 Message enqueued on MTP3_SCCP_PORT from VirtMSC-IPA(12) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE03000131'O
} id 2
08:48:46.478148 9813 SCCP_Emulation.ttcn:5439 Incoming message was mapped to @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 3,
            data := '000131'O
        }
    }
} id 2
08:48:46.478204 9813 SCCP_Emulation.ttcn:5443 Matching on port MTP3_SCCP_PORT succeeded:  matched
08:48:46.478370 9813 SCCP_Emulation.ttcn:5443 Receive operation on port MTP3_SCCP_PORT succeeded, message from VirtMSC-IPA(12): @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 3,
            data := '000131'O
        }
    }
} id 2
08:48:46.478483 9813 SCCP_Emulation.ttcn:5443 Message with id 2 was extracted from the queue of MTP3_SCCP_PORT.
08:48:46.478607 9813 SCCP_Emulation.ttcn:3464 Sent on SCCP_SP_PORT to mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
}
08:48:46.478725 9718 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(11) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
} id 2
08:48:46.478842 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
08:48:46.479360 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 1,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:46.479515 9718 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 2
08:48:46.479641 9718 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
08:48:46.479804 9718 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(11): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 2
08:48:46.479894 9718 BSC_Tests.ttcn:901 Message with id 2 was extracted from the queue of BSSAP.
08:48:46.479967 9718 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
08:48:46.480028 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
08:48:46.480104 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:46.483330 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:46.483430 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 19
08:48:46.485551 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:46.487106 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:46.488455 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:46.489625 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:46.490575 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with ? matched
08:48:46.491646 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:46.491674 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 18 was extracted from the queue of BSCVTY.
08:48:46.491703 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:46.491728 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:46.491753 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 19
08:48:46.491767 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 19 was extracted from the queue of BSCVTY.
08:48:46.491780 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:46.491800 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:46.491826 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:46.491912 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 20
08:48:46.491935 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:46.491964 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:46.491991 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:46.492006 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 20
08:48:46.492060 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
08:48:46.492079 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:46.492095 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:46.492117 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:46.492166 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 21
08:48:46.492194 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:46.492215 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:46.492239 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:46.492252 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 21
08:48:46.492265 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
08:48:46.492278 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:46.492291 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
08:48:46.492307 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:46.492345 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 22
08:48:46.492365 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:46.492383 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:46.492409 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:46.492421 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 22
08:48:46.492435 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 22 was extracted from the queue of BSCVTY.
08:48:46.492447 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:46.492459 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:46.492474 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:46.492499 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
08:48:46.492517 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:46.492534 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:46.492555 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:46.492567 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
08:48:46.492579 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
08:48:46.492590 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:46.492601 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:46.492616 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:46.492661 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 24
08:48:46.492679 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:46.492697 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:46.492709 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 24
08:48:46.492721 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 24 was extracted from the queue of BSCVTY.
08:48:46.492732 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:46.492746 9718 BSC_Tests.ttcn:1191 msc 1 is not configured, skipping
08:48:46.492760 9718 BSC_Tests.ttcn:1191 msc 2 is not configured, skipping
08:48:46.492785 9718 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:46.495521 9816 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:46.495582 9816 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: IPA-CTRL-CLI-IPA(14), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA. Version: 11.1.0.
08:48:46.495599 9816 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:46.495643 9816 - Connected to MC.
08:48:46.495655 9816 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:46.495684 9718 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 14, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:46.495703 9718 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(14):IPA_PORT to system:IPA_CODEC_PT.
08:48:46.496917 9816 - Port IPA_PORT was started.
08:48:46.496949 9816 - Port CFG_PORT was started.
08:48:46.496960 9816 - Port MTP3_SP_PORT was started.
08:48:46.496969 9816 - Port IPA_MGCP_PORT was started.
08:48:46.496979 9816 - Port IPA_RSL_PORT was started.
08:48:46.496988 9816 - Port IPA_OML_PORT was started.
08:48:46.496998 9816 - Port IPA_CTRL_PORT was started.
08:48:46.497007 9816 - Port IPA_SP_PORT was started.
08:48:46.497016 9816 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:46.497054 9816 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:46.497111 9718 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(14):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:46.497144 9718 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:46.497341 9718 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-4037f21f.
08:48:46.497372 9816 - Port IPA_CTRL_PORT has established the connection with mtc:IPA_CTRL using transport type UNIX.
08:48:46.497402 9718 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT.
08:48:46.497419 9718 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
08:48:46.497444 9718 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false) on component IPA-CTRL-CLI-IPA(14).
08:48:46.497570 9718 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
08:48:46.497612 9718 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
08:48:46.497693 9816 - Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false).
08:48:46.497902 9816 IPA_Emulation.ttcnpp:316 entering f__IPL4__PROVIDER__connect: :0 -> 127.0.0.1:4249 / TCP
08:48:46.499046 9816 IPA_Emulation.ttcnpp:395 Sent on IPA_CTRL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:46.499179 9718 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:46.499235 9718 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
08:48:46.499276 9718 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:46.499384 9718 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
08:48:46.499436 9718 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:46.504844 9817 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:46.504964 9817 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMGW-MGCP-0(15), component type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0. Version: 11.1.0.
08:48:46.504998 9817 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:46.505085 9817 - Connected to MC.
08:48:46.505123 9817 - Initializing variables, timers and ports of component type MGCP_Emulation.MGCP_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:46.505199 9718 BSC_Tests.ttcn:1073 PTC was created. Component reference: 15, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:46.505293 9718 BSC_Tests.ttcn:1074 Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(15).
08:48:46.505444 9718 BSC_Tests.ttcn:1074 Function was started.
08:48:46.505500 9718 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:46.505769 9718 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.029994.
08:48:46.505848 9718 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "29994168",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:46.505911 9718 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:46.506105 9816 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "29994168",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:46.506284 9816 IPA_Emulation.ttcnpp:887 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:46.506341 9816 IPA_Emulation.ttcnpp:887 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "29994168",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:46.506381 9816 IPA_Emulation.ttcnpp:887 Message with id 1 was extracted from the queue of IPA_CTRL_PORT.
08:48:46.506778 9817 - Port MGCP was started.
08:48:46.506817 9817 - Port MGCP_CLIENT was started.
08:48:46.506838 9817 - Port MGCP_CLIENT_MULTI was started.
08:48:46.506859 9817 - Port MGCP_PROC was started.
08:48:46.506880 9817 - Component type MGCP_Emulation.MGCP_Emulation_CT was initialized.
08:48:46.506977 9817 - Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0").
08:48:46.507101 9816 IPA_Emulation.ttcnpp:890 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '474554203239393934313638206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 29994168 bts.0.oml-connection-state")
}
08:48:46.507289 9817 MGCP_Emulation.ttcn:279 Mapping port VirtMGW-MGCP-0(15):MGCP to system:MGCP_CODEC_PT.
08:48:46.507371 9817 MGCP_Emulation.ttcn:279 Port MGCP was mapped to system:MGCP_CODEC_PT.
08:48:46.507397 9816 IPA_Emulation.ttcnpp:890 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0028EE00474554203239393934313638206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:46.507437 9817 MGCP_Emulation.ttcn:279 Map operation of VirtMGW-MGCP-0(15):MGCP to system:MGCP_CODEC_PT finished.
08:48:46.507586 9817 MGCP_Emulation.ttcn:281 entering f__IPL4__PROVIDER__listen: 127.0.0.1:2427 / UDP
08:48:46.507839 9816 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 38679,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0037EE004745545F5245504C59203239393934313638206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
} id 1
08:48:46.508002 9816 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C59203239393934313638206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 29994168 bts.0.oml-connection-state degraded")
} id 1
08:48:46.508079 9816 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:46.508126 9816 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C59203239393934313638206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 29994168 bts.0.oml-connection-state degraded")
} id 1
08:48:46.508156 9816 IPA_Emulation.ttcnpp:761 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:46.508384 9816 IPA_Emulation.ttcnpp:634 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "29994168",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
08:48:46.508455 9718 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "29994168",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:48:46.508525 9718 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:46.508568 9718 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "29994168",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:48:46.508613 9718 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
08:48:46.508664 9718 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:46.508702 9718 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:47.508741 9718 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:47.508816 9718 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:47.511908 9819 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:47.511987 9819 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: IPA-BTS0-TRX0-RSL-IPA(16), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA. Version: 11.1.0.
08:48:47.512006 9819 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:47.512054 9819 - Connected to MC.
08:48:47.512077 9819 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:47.512142 9718 BSC_Tests.ttcn:951 PTC was created. Component reference: 16, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:47.512164 9718 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: {
    site_id := 1234,
    bts_id := 0,
    trx_id := 0
}
08:48:47.512181 9718 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
08:48:47.512195 9718 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(16):IPA_PORT to system:IPA_CODEC_PT.
08:48:47.513316 9819 - Port IPA_PORT was started.
08:48:47.513355 9819 - Port CFG_PORT was started.
08:48:47.513378 9819 - Port MTP3_SP_PORT was started.
08:48:47.513396 9819 - Port IPA_MGCP_PORT was started.
08:48:47.513415 9819 - Port IPA_RSL_PORT was started.
08:48:47.513433 9819 - Port IPA_OML_PORT was started.
08:48:47.513443 9819 - Port IPA_CTRL_PORT was started.
08:48:47.513453 9819 - Port IPA_SP_PORT was started.
08:48:47.513464 9819 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:47.513504 9819 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:47.513659 9718 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(16):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:47.513710 9718 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
08:48:47.513866 9718 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-50708b6e.
08:48:47.513926 9819 - Port CFG_PORT has established the connection with mtc:IPA_CFG_PORT[0][0] using transport type UNIX.
08:48:47.513949 9718 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT.
08:48:47.514010 9718 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
08:48:47.514080 9718 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
08:48:47.514309 9718 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-336aab76.
08:48:47.514333 9819 - Port IPA_RSL_PORT has established the connection with mtc:IPA_RSL[0][0] using transport type UNIX.
08:48:47.514361 9718 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT.
08:48:47.514378 9718 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
08:48:47.514393 9718 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true) on component IPA-BTS0-TRX0-RSL-IPA(16).
08:48:47.514429 9718 BSC_Tests.ttcn:969 Function was started.
08:48:47.514444 9718 BSC_Tests.ttcn:976 Start timer T: 10 s
08:48:47.514535 9819 - Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true).
08:48:47.514722 9819 IPA_Emulation.ttcnpp:316 entering f__IPL4__PROVIDER__connect: :10000 -> 127.0.0.1:3003 / TCP
08:48:47.515860 9819 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:47.516033 9819 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:47.516221 9819 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:47.516567 9819 IPA_Emulation.ttcnpp:385 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:47.516659 9718 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:47.516686 9718 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:47.516703 9718 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:47.516718 9718 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(16): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:47.516734 9718 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
08:48:47.517287 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0011FE0401080107010201030104010501010100'O
} id 1
08:48:47.517407 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:47.517436 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:47.517455 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:47.517527 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:47.517560 9819 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:47.517580 9819 IPA_Emulation.ttcnpp:745 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:47.517614 9819 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
08:48:47.517819 9819 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
08:48:47.517888 9819 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:47.517910 9819 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:47.517949 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:47.517966 9819 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:47.517981 9819 IPA_Emulation.ttcnpp:745 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:47.517997 9819 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:47.518031 9819 IPA_Emulation.ttcnpp:385 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
}
08:48:47.518064 9718 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:47.518126 9718 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:47.518156 9718 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(16): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:47.518206 9718 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
08:48:47.518214 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:47.518231 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:47.518237 9718 BSC_Tests.ttcn:979 Stop timer T: 10 s
08:48:47.518265 9718 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:47.518288 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.518291 9718 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.368969.
08:48:47.518303 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.518316 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:47.518326 9718 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "368968629",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:47.518327 9819 IPA_Emulation.ttcnpp:761 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:47.518358 9718 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:47.518370 9816 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "368968629",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:47.518402 9816 IPA_Emulation.ttcnpp:887 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:47.518416 9816 IPA_Emulation.ttcnpp:887 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "368968629",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:47.518428 9816 IPA_Emulation.ttcnpp:887 Message with id 2 was extracted from the queue of IPA_CTRL_PORT.
08:48:47.518493 9816 IPA_Emulation.ttcnpp:890 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420333638393638363239206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 368968629 bts.0.oml-connection-state")
}
08:48:47.518517 9816 IPA_Emulation.ttcnpp:890 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420333638393638363239206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:47.518587 9816 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 38679,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0039EE004745545F5245504C5920333638393638363239206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
} id 2
08:48:47.518608 9816 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920333638393638363239206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 368968629 bts.0.oml-connection-state connected")
} id 2
08:48:47.518650 9816 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.518681 9816 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920333638393638363239206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 368968629 bts.0.oml-connection-state connected")
} id 2
08:48:47.518705 9816 IPA_Emulation.ttcnpp:761 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:47.518750 9816 IPA_Emulation.ttcnpp:634 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "368968629",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
08:48:47.518817 9718 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "368968629",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:48:47.518849 9718 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:47.518877 9718 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "368968629",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:48:47.518894 9718 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
08:48:47.518942 9718 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:47.518974 9718 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:47.519477 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
}
08:48:47.519623 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:47.519624 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
08:48:47.519645 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:47.519661 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0006000C1101801E0A'O
} id 5
08:48:47.519676 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:47.519694 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:47.519711 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:47.519730 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:47.519746 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:47.519761 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:47.519775 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:47.519790 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:47.519804 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:47.519818 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:47.519832 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:47.519848 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:47.519862 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:47.519877 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '000400101A1E0D'O
} id 12
08:48:47.519891 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:47.519907 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.519921 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.519935 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:47.519950 9819 IPA_Emulation.ttcnpp:761 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:47.520007 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
}
08:48:47.520030 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520037 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
} id 4
08:48:47.520044 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520058 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:47.520073 9819 IPA_Emulation.ttcnpp:761 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:47.520097 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
}
08:48:47.520115 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520129 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520138 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
} id 5
08:48:47.520143 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:47.520157 9819 IPA_Emulation.ttcnpp:761 Message with id 6 was extracted from the queue of IPA_PORT.
08:48:47.520182 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:47.520199 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520212 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520216 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
} id 6
08:48:47.520226 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:47.520239 9819 IPA_Emulation.ttcnpp:761 Message with id 7 was extracted from the queue of IPA_PORT.
08:48:47.520261 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:47.520278 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520293 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520293 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 7
08:48:47.520307 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:47.520321 9819 IPA_Emulation.ttcnpp:761 Message with id 8 was extracted from the queue of IPA_PORT.
08:48:47.520343 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
}
08:48:47.520359 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520373 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520375 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
} id 8
08:48:47.520387 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:47.520401 9819 IPA_Emulation.ttcnpp:761 Message with id 9 was extracted from the queue of IPA_PORT.
08:48:47.520422 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:47.520440 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520453 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520455 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 9
08:48:47.520467 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:47.520481 9819 IPA_Emulation.ttcnpp:761 Message with id 10 was extracted from the queue of IPA_PORT.
08:48:47.520503 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:47.520520 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520534 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520536 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 10
08:48:47.520548 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:47.520562 9819 IPA_Emulation.ttcnpp:761 Message with id 11 was extracted from the queue of IPA_PORT.
08:48:47.520622 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:47.520652 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520666 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520667 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 11
08:48:47.520680 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:47.520694 9819 IPA_Emulation.ttcnpp:761 Message with id 12 was extracted from the queue of IPA_PORT.
08:48:47.520713 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
}
08:48:47.520744 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:47.520748 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
} id 12
08:48:47.520784 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:47.520801 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001400101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:47.520816 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:47.520832 9819 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:47.520848 9819 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:47.520863 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520877 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520891 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:47.520905 9819 IPA_Emulation.ttcnpp:761 Message with id 13 was extracted from the queue of IPA_PORT.
08:48:47.520926 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:47.520942 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.520951 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 13
08:48:47.520956 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.520970 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:47.520984 9819 IPA_Emulation.ttcnpp:761 Message with id 14 was extracted from the queue of IPA_PORT.
08:48:47.521004 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
}
08:48:47.521019 9819 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:47.521024 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
} id 14
08:48:47.521034 9819 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:47.521049 9819 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:47.521063 9819 IPA_Emulation.ttcnpp:761 Message with id 15 was extracted from the queue of IPA_PORT.
08:48:47.521211 9819 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:47.521244 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 15
08:48:48.519320 9718 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:48.519493 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:48.519641 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:48.519859 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 25
08:48:48.520021 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.520184 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:48.520328 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:48.520438 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 25
08:48:48.520494 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
08:48:48.520515 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:48.520532 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:48:48.520583 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:48.520681 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 26
08:48:48.520748 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.520775 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:48.520810 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:48:48.520827 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 26
08:48:48.520844 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
08:48:48.520861 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:48.520914 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:48:48.520965 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:48.521040 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:48.521097 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.521144 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:48.521194 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:48.521222 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:48.521249 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 27 was extracted from the queue of BSCVTY.
08:48:48.521281 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:48.521311 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:48.521349 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:48.521406 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:48.521450 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.521490 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:48.521535 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:48.521562 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:48.521588 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
08:48:48.521615 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:48.521643 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:48.521686 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:48.521733 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 29
08:48:48.521776 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.521817 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:48.521878 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 29
08:48:48.521906 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 29 was extracted from the queue of BSCVTY.
08:48:48.521937 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:48.521966 9718 Osmocom_VTY_Functions.ttcn:333 "TC_ctrl_msc0_connection_status() start"
08:48:48.522000 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_ctrl_msc0_connection_status() start"
08:48:48.522040 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:48.522183 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 30
08:48:48.522244 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.522293 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:48.522322 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 30
08:48:48.522350 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 30 was extracted from the queue of BSCVTY.
08:48:48.522378 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:48.522409 9718 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.356698.
08:48:48.522447 9718 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "356698192",
        variable := "msc.0.connection_status",
        val := omit
    }
}
08:48:48.522481 9718 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:48.522503 9816 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "356698192",
        variable := "msc.0.connection_status",
        val := omit
    }
} id 3
08:48:48.522553 9816 IPA_Emulation.ttcnpp:887 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:48.522570 9816 IPA_Emulation.ttcnpp:887 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "356698192",
        variable := "msc.0.connection_status",
        val := omit
    }
} id 3
08:48:48.522586 9816 IPA_Emulation.ttcnpp:887 Message with id 3 was extracted from the queue of IPA_CTRL_PORT.
08:48:48.522622 9816 IPA_Emulation.ttcnpp:890 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420333536363938313932206D73632E302E636F6E6E656374696F6E5F737461747573'O ("GET 356698192 msc.0.connection_status")
}
08:48:48.522647 9816 IPA_Emulation.ttcnpp:890 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0026EE0047455420333536363938313932206D73632E302E636F6E6E656374696F6E5F737461747573'O
}
08:48:48.522768 9816 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 38679,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0036EE004745545F5245504C5920333536363938313932206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O
} id 3
08:48:48.522792 9816 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920333536363938313932206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 356698192 msc.0.connection_status connected")
} id 3
08:48:48.522808 9816 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:48.522824 9816 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920333536363938313932206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 356698192 msc.0.connection_status connected")
} id 3
08:48:48.522839 9816 IPA_Emulation.ttcnpp:761 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:48.522867 9816 IPA_Emulation.ttcnpp:634 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "356698192",
        variable := "msc.0.connection_status",
        val := "connected"
    }
}
08:48:48.522900 9718 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "356698192",
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 4
08:48:48.522940 9718 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:48.522969 9718 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "356698192",
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 4
08:48:48.522997 9718 Osmocom_CTRL_Functions.ttcn:41 Message with id 4 was extracted from the queue of IPA_CTRL.
08:48:48.523039 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
08:48:48.523080 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:48.523444 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" id 31
08:48:48.523478 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
08:48:48.523524 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.523566 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:48.523620 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:48.523929 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:48.523959 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with ? matched
08:48:48.523978 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" id 31
08:48:48.523995 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 31 was extracted from the queue of BSCVTY.
08:48:48.524035 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:48.524059 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:48.524073 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
08:48:48.524093 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
08:48:48.524262 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:48.524297 9718 Osmocom_VTY_Functions.ttcn:260 talloc reports "struct bsc_subscr" x 0, expecting 0
08:48:48.524318 9718 Osmocom_VTY_Functions.ttcn:260 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
08:48:48.524335 9718 BSC_Tests.ttcn:888 Stopping all components.
08:48:48.524368 9812 StatsD_Checker.ttcnpp:138 Kill was requested from MC.
08:48:48.524371 9813 SCCP_Emulation.ttcn:5439 Stop was requested from MC.
08:48:48.524371 9816 IPA_Emulation.ttcnpp:743 Kill was requested from MC.
08:48:48.524374 9814 IPA_Emulation.ttcnpp:743 Stop was requested from MC.
08:48:48.524376 9817 MGCP_Emulation.ttcn:301 Stop was requested from MC.
08:48:48.524386 9819 IPA_Emulation.ttcnpp:743 Stop was requested from MC.
08:48:48.524400 9816 IPA_Emulation.ttcnpp:743 Terminating test component execution.
08:48:48.524403 9812 StatsD_Checker.ttcnpp:138 Terminating test component execution.
08:48:48.524415 9813 SCCP_Emulation.ttcn:5439 Stopping test component execution.
08:48:48.524420 9817 MGCP_Emulation.ttcn:301 Stopping test component execution.
08:48:48.524425 9814 IPA_Emulation.ttcnpp:743 Stopping test component execution.
08:48:48.524441 9819 IPA_Emulation.ttcnpp:743 Stopping test component execution.
08:48:48.524757 9813 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
08:48:48.524768 9817 - Function main was stopped. PTC remains alive and is waiting for next start.
08:48:48.524795 9814 - Function main_server was stopped. PTC remains alive and is waiting for next start.
08:48:48.524825 9812 - Function main was stopped. PTC terminates.
08:48:48.524928 9812 - Terminating component type StatsD_Checker.StatsD_Checker_CT.
08:48:48.525050 9812 - Removing unterminated mapping between port STATSVTY and system:STATSVTY.
08:48:48.525281 9812 - Port STATSVTY was unmapped from system:STATSVTY.
08:48:48.525305 9816 - Function main_client was stopped. PTC terminates.
08:48:48.525342 9819 - Function main_client was stopped. PTC remains alive and is waiting for next start.
08:48:48.525374 9812 - Port STATSVTY was stopped.
08:48:48.525449 9812 - Port STATSD_PROC was stopped.
08:48:48.525477 9812 - Removing unterminated mapping between port STATS and system:STATS.
08:48:48.525491 9816 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:48.525531 9816 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:48.525869 9812 - Port STATS was unmapped from system:STATS.
08:48:48.525920 9812 - Port STATS was stopped.
08:48:48.525926 9816 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:48.525951 9812 - Component type StatsD_Checker.StatsD_Checker_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.525973 9816 - Port IPA_PORT was stopped.
08:48:48.525992 9812 - Final verdict of PTC: none
08:48:48.526004 9816 - Port CFG_PORT was stopped.
08:48:48.526038 9816 - Port MTP3_SP_PORT was stopped.
08:48:48.526060 9812 - Disconnected from MC.
08:48:48.526064 9816 - Port IPA_MGCP_PORT was stopped.
08:48:48.526082 9812 - TTCN-3 Parallel Test Component finished.
08:48:48.526088 9816 - Port IPA_RSL_PORT was stopped.
08:48:48.526234 9816 - Port IPA_OML_PORT was stopped.
08:48:48.526295 9816 - Removing unterminated connection between port IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:48.526377 9816 - Port IPA_CTRL_PORT was stopped.
08:48:48.526381 9718 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT was closed unexpectedly by the peer.
08:48:48.526435 9718 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT.
08:48:48.526449 9816 - Port IPA_SP_PORT was stopped.
08:48:48.526512 9816 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.526544 9816 - Final verdict of PTC: none
08:48:48.526552 9718 BSC_Tests.ttcn:888 All components were stopped.
08:48:48.526569 9718 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
08:48:48.526586 9718 BSC_Tests.ttcn:890 Stopping test component execution.
08:48:48.526608 9718 BSC_Tests.ttcn:3193 Test case TC_ctrl_msc0_connection_status was stopped.
08:48:48.526616 9816 - Disconnected from MC.
08:48:48.526622 9718 BSC_Tests.ttcn:3193 Terminating component type BSC_Tests.test_CT.
08:48:48.526639 9718 BSC_Tests.ttcn:3193 Default with id 1 (altstep as_Tguard) was deactivated.
08:48:48.526641 9816 - TTCN-3 Parallel Test Component finished.
08:48:48.526654 9718 BSC_Tests.ttcn:3193 Stop timer T_guard: 30 s
08:48:48.526690 9718 BSC_Tests.ttcn:3193 Port IPA_CTRL was stopped.
08:48:48.526719 9718 BSC_Tests.ttcn:3193 Port RSL_CCHAN[0] was stopped.
08:48:48.526747 9718 BSC_Tests.ttcn:3193 Port RSL_CCHAN[1] was stopped.
08:48:48.526774 9718 BSC_Tests.ttcn:3193 Port RSL_CCHAN[2] was stopped.
08:48:48.526801 9718 BSC_Tests.ttcn:3193 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT.
08:48:48.526850 9718 BSC_Tests.ttcn:3193 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
08:48:48.526904 9718 BSC_Tests.ttcn:3193 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
08:48:48.526905 9819 - Connection of port IPA_RSL_PORT to mtc:IPA_RSL[0][0] was closed unexpectedly by the peer.
08:48:48.526936 9718 BSC_Tests.ttcn:3193 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
08:48:48.526973 9718 BSC_Tests.ttcn:3193 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527005 9718 BSC_Tests.ttcn:3193 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527023 9819 - Port IPA_RSL_PORT was disconnected from mtc:IPA_RSL[0][0].
08:48:48.527039 9718 BSC_Tests.ttcn:3193 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527071 9718 BSC_Tests.ttcn:3193 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527101 9718 BSC_Tests.ttcn:3193 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527132 9718 BSC_Tests.ttcn:3193 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527162 9718 BSC_Tests.ttcn:3193 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527192 9718 BSC_Tests.ttcn:3193 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527222 9718 BSC_Tests.ttcn:3193 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527257 9718 BSC_Tests.ttcn:3193 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
08:48:48.527284 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[0][0] was stopped.
08:48:48.527313 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[0][1] was stopped.
08:48:48.527342 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[0][2] was stopped.
08:48:48.527385 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[0][3] was stopped.
08:48:48.527413 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[1][0] was stopped.
08:48:48.527441 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[1][1] was stopped.
08:48:48.527475 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[1][2] was stopped.
08:48:48.527512 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[1][3] was stopped.
08:48:48.527609 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[2][0] was stopped.
08:48:48.527678 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[2][1] was stopped.
08:48:48.527736 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[2][2] was stopped.
08:48:48.527792 9718 BSC_Tests.ttcn:3193 Port IPA_RSL[2][3] was stopped.
08:48:48.527848 9718 BSC_Tests.ttcn:3193 Port IPA was stopped.
08:48:48.527907 9718 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CTRL was stopped.
08:48:48.527968 9718 BSC_Tests.ttcn:3193 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT.
08:48:48.528062 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][0] was stopped.
08:48:48.528089 9819 - Connection of port CFG_PORT to mtc:IPA_CFG_PORT[0][0] was closed unexpectedly by the peer.
08:48:48.528127 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][1] was stopped.
08:48:48.528159 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][2] was stopped.
08:48:48.528169 9819 - Port CFG_PORT was disconnected from mtc:IPA_CFG_PORT[0][0].
08:48:48.528189 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][3] was stopped.
08:48:48.528219 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][0] was stopped.
08:48:48.528251 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][1] was stopped.
08:48:48.528280 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][2] was stopped.
08:48:48.528309 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][3] was stopped.
08:48:48.528337 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][0] was stopped.
08:48:48.528365 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][1] was stopped.
08:48:48.528394 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][2] was stopped.
08:48:48.528422 9718 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][3] was stopped.
08:48:48.528449 9718 BSC_Tests.ttcn:3193 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
08:48:48.528508 9718 BSC_Tests.ttcn:3193 Port BSCVTY was unmapped from system:BSCVTY.
08:48:48.528539 9718 BSC_Tests.ttcn:3193 Port BSCVTY was stopped.
08:48:48.528568 9718 BSC_Tests.ttcn:3193 Port STPVTY was stopped.
08:48:48.528608 9718 BSC_Tests.ttcn:3193 Removing unterminated connection between port SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT.
08:48:48.528674 9718 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
08:48:48.528747 9814 - Connection of port CFG_PORT to mtc:SCCPLITE_IPA_CFG_PORT[0] was closed unexpectedly by the peer.
08:48:48.528761 9718 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
08:48:48.528798 9718 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
08:48:48.528829 9718 BSC_Tests.ttcn:3193 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:48.528850 9814 - Port CFG_PORT was disconnected from mtc:SCCPLITE_IPA_CFG_PORT[0].
08:48:48.528952 9718 BSC_Tests.ttcn:3193 Port BSSAP was stopped.
08:48:48.528956 9813 - Connection of port SCCP_SP_PORT to mtc:BSSAP was closed unexpectedly by the peer.
08:48:48.529019 9813 - Port SCCP_SP_PORT was disconnected from mtc:BSSAP.
08:48:48.529045 9718 BSC_Tests.ttcn:3193 Port BSSAP_LE was stopped.
08:48:48.529117 9718 BSC_Tests.ttcn:3193 Component type BSC_Tests.test_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.529190 9718 BSC_Tests.ttcn:3193 Waiting for PTCs to finish.
08:48:48.529265 9813 - Kill was requested from MC. Terminating idle PTC.
08:48:48.529282 9814 - Kill was requested from MC. Terminating idle PTC.
08:48:48.529288 9815 - Kill was requested from MC. Terminating idle PTC.
08:48:48.529343 9813 - Terminating component type SCCP_Emulation.SCCP_CT.
08:48:48.529348 9819 - Kill was requested from MC. Terminating idle PTC.
08:48:48.529382 9813 - Port SCCP_SP_PORT was stopped.
08:48:48.529391 9815 - Terminating component type IPA_Emulation.IPA_EventWaiter_CT.
08:48:48.529421 9819 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:48.529437 9813 - Removing unterminated connection between port MTP3_SCCP_PORT and VirtMSC-IPA(12):MTP3_SP_PORT.
08:48:48.529437 9814 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:48.529453 9815 - Port IPA_SP_PORT was stopped.
08:48:48.529469 9817 - Kill was requested from MC. Terminating idle PTC.
08:48:48.529472 9813 - Port MTP3_SCCP_PORT was stopped.
08:48:48.529479 9819 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:48.529561 9815 - Component type IPA_Emulation.IPA_EventWaiter_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.529567 9813 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.529594 9814 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:48.529624 9813 - Final verdict of PTC: none
08:48:48.529636 9817 - Terminating component type MGCP_Emulation.MGCP_Emulation_CT.
08:48:48.529649 9815 - Final verdict of PTC: pass
08:48:48.529712 9817 - Removing unterminated mapping between port MGCP and system:MGCP_CODEC_PT.
08:48:48.529736 9813 - Disconnected from MC.
08:48:48.529789 9813 - TTCN-3 Parallel Test Component finished.
08:48:48.530412 9819 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:48.530493 9814 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:48.530635 9814 - Port IPA_PORT was stopped.
08:48:48.530649 9819 - Port IPA_PORT was stopped.
08:48:48.530698 9819 - Port CFG_PORT was stopped.
08:48:48.530738 9814 - Port CFG_PORT was stopped.
08:48:48.530758 9819 - Port MTP3_SP_PORT was stopped.
08:48:48.530864 9817 - Port MGCP was unmapped from system:MGCP_CODEC_PT.
08:48:48.530886 9815 - Disconnected from MC.
08:48:48.530896 9819 - Port IPA_MGCP_PORT was stopped.
08:48:48.530946 9814 - Removing unterminated connection between port MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT.
08:48:48.530976 9815 - TTCN-3 Parallel Test Component finished.
08:48:48.530993 9817 - Port MGCP was stopped.
08:48:48.531055 9817 - Port MGCP_CLIENT was stopped.
08:48:48.531085 9819 - Port IPA_RSL_PORT was stopped.
08:48:48.531104 9814 - Port MTP3_SP_PORT was stopped.
08:48:48.531159 9817 - Port MGCP_CLIENT_MULTI was stopped.
08:48:48.531166 9819 - Port IPA_OML_PORT was stopped.
08:48:48.531177 9814 - Port IPA_MGCP_PORT was stopped.
08:48:48.531241 9814 - Port IPA_RSL_PORT was stopped.
08:48:48.531289 9819 - Port IPA_CTRL_PORT was stopped.
08:48:48.531307 9814 - Port IPA_OML_PORT was stopped.
08:48:48.531384 9819 - Port IPA_SP_PORT was stopped.
08:48:48.531409 9817 - Port MGCP_PROC was stopped.
08:48:48.531415 9814 - Port IPA_CTRL_PORT was stopped.
08:48:48.531476 9814 - Port IPA_SP_PORT was stopped.
08:48:48.531482 9817 - Component type MGCP_Emulation.MGCP_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.531550 9814 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.531552 9817 - Final verdict of PTC: none
08:48:48.531575 9819 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:48.531614 9814 - Final verdict of PTC: none
08:48:48.531644 9817 - Disconnected from MC.
08:48:48.531670 9819 - Final verdict of PTC: none
08:48:48.531676 9817 - TTCN-3 Parallel Test Component finished.
08:48:48.531726 9814 - Disconnected from MC.
08:48:48.531776 9814 - TTCN-3 Parallel Test Component finished.
08:48:48.531826 9718 BSC_Tests.ttcn:3193 Setting final verdict of the test case.
08:48:48.531852 9819 - Disconnected from MC.
08:48:48.531891 9718 BSC_Tests.ttcn:3193 Local verdict of MTC: pass
08:48:48.531929 9819 - TTCN-3 Parallel Test Component finished.
08:48:48.531931 9718 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-STATS(10): none (pass -> pass)
08:48:48.531972 9718 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-SCCP(11): none (pass -> pass)
08:48:48.532003 9718 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-IPA(12): none (pass -> pass)
08:48:48.532028 9718 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-IPA-WAIT(13): pass (pass -> pass)
08:48:48.532054 9718 BSC_Tests.ttcn:3193 Local verdict of PTC IPA-CTRL-CLI-IPA(14): none (pass -> pass)
08:48:48.532082 9718 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMGW-MGCP-0(15): none (pass -> pass)
08:48:48.532111 9718 BSC_Tests.ttcn:3193 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(16): none (pass -> pass)
08:48:48.532163 9718 BSC_Tests.ttcn:3193 Test case TC_ctrl_msc0_connection_status finished. Verdict: pass
08:48:48.532255 9718 BSC_Tests.ttcn:3193 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc0_connection_status pass'.
08:48:54.098796 9718 BSC_Tests.ttcn:3193 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc0_connection_status pass' was executed successfully (exit status: 0).
08:48:54.098942 9718 BSC_Tests.ttcn:3388 Switching to log file `BSC_Tests-TC_stat_num_bts_connected_1-cbea39017248-mtc-9718.log'
