08:48:27.681719 9718 BSC_Tests.ttcn:3177 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc_connection_status'.
08:48:28.695091 9718 BSC_Tests.ttcn:3177 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc_connection_status' was executed successfully (exit status: 0).
08:48:28.695158 9718 BSC_Tests.ttcn:3177 Test case TC_ctrl_msc_connection_status started.
08:48:28.695334 9718 BSC_Tests.ttcn:3177 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_ctrl_msc_connection_status.
08:48:28.696145 9718 BSC_Tests.ttcn:3177 Port IPA_CTRL was started.
08:48:28.696230 9718 BSC_Tests.ttcn:3177 Port RSL_CCHAN[0] was started.
08:48:28.696283 9718 BSC_Tests.ttcn:3177 Port RSL_CCHAN[1] was started.
08:48:28.696298 9718 BSC_Tests.ttcn:3177 Port RSL_CCHAN[2] was started.
08:48:28.696311 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[0][0] was started.
08:48:28.696324 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[0][1] was started.
08:48:28.696339 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[0][2] was started.
08:48:28.696352 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[0][3] was started.
08:48:28.696365 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[1][0] was started.
08:48:28.696378 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[1][1] was started.
08:48:28.696391 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[1][2] was started.
08:48:28.696404 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[1][3] was started.
08:48:28.696417 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[2][0] was started.
08:48:28.696430 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[2][1] was started.
08:48:28.696443 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[2][2] was started.
08:48:28.696456 9718 BSC_Tests.ttcn:3177 Port IPA_RSL[2][3] was started.
08:48:28.696472 9718 BSC_Tests.ttcn:3177 Port IPA was started.
08:48:28.696486 9718 BSC_Tests.ttcn:3177 Port SCCPLITE_IPA_CTRL was started.
08:48:28.696500 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[0][0] was started.
08:48:28.696513 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[0][1] was started.
08:48:28.696526 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[0][2] was started.
08:48:28.696539 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[0][3] was started.
08:48:28.696552 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[1][0] was started.
08:48:28.696566 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[1][1] was started.
08:48:28.696615 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[1][2] was started.
08:48:28.696657 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[1][3] was started.
08:48:28.696683 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[2][0] was started.
08:48:28.696706 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[2][1] was started.
08:48:28.696728 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[2][2] was started.
08:48:28.696763 9718 BSC_Tests.ttcn:3177 Port IPA_CFG_PORT[2][3] was started.
08:48:28.696780 9718 BSC_Tests.ttcn:3177 Port BSCVTY was started.
08:48:28.696793 9718 BSC_Tests.ttcn:3177 Port STPVTY was started.
08:48:28.696833 9718 BSC_Tests.ttcn:3177 Port SCCPLITE_IPA_CFG_PORT[0] was started.
08:48:28.696865 9718 BSC_Tests.ttcn:3177 Port SCCPLITE_IPA_CFG_PORT[1] was started.
08:48:28.696878 9718 BSC_Tests.ttcn:3177 Port SCCPLITE_IPA_CFG_PORT[2] was started.
08:48:28.696891 9718 BSC_Tests.ttcn:3177 Port BSSAP was started.
08:48:28.696904 9718 BSC_Tests.ttcn:3177 Port BSSAP_LE was started.
08:48:28.696922 9718 BSC_Tests.ttcn:3177 Component type BSC_Tests.test_CT was initialized.
08:48:28.697065 9718 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
08:48:28.697174 9718 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
08:48:28.697315 9718 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
08:48:28.697682 9718 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
08:48:28.697760 9718 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
08:48:28.697792 9718 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
08:48:28.697938 9718 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:28.698036 9718 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:28.698063 9718 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:28.698183 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
08:48:28.698243 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.698287 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:28.698302 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:28.698314 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:28.698334 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:28.698374 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:28.698428 9718 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
08:48:28.698515 9718 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
08:48:28.698551 9718 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
08:48:28.699056 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
08:48:28.699125 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.699161 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.699178 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:28.699198 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
08:48:28.699232 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.699405 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:28.699456 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.699591 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
08:48:28.699640 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.699664 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.699691 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.699705 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
08:48:28.699732 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
08:48:28.699750 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.699778 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
08:48:28.699805 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.699884 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
08:48:28.699916 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.699939 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.699973 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.699991 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
08:48:28.700009 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
08:48:28.700025 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.700068 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
08:48:28.700097 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.700137 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
08:48:28.700176 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.700200 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.700228 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.700246 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
08:48:28.700264 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
08:48:28.700294 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.700327 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
08:48:28.700351 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.700379 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
08:48:28.700403 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.700435 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.700460 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.700476 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
08:48:28.700490 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
08:48:28.700505 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.700520 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:28.700538 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.700558 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
08:48:28.700599 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.700635 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.700654 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
08:48:28.700671 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
08:48:28.700688 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.700722 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:28.700748 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.700777 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
08:48:28.700802 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.700822 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.700851 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.700867 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
08:48:28.700882 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
08:48:28.700898 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.700915 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:28.700934 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.700957 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
08:48:28.700981 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.701009 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.701037 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.701052 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
08:48:28.701067 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
08:48:28.701083 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.701098 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:28.701115 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.701146 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
08:48:28.701167 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.701187 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.701210 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.701227 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
08:48:28.701241 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
08:48:28.701256 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.701270 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:28.701287 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.701308 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
08:48:28.701328 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.701347 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.701370 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:28.701384 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
08:48:28.701398 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
08:48:28.701413 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.701427 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:28.701444 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.701462 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
08:48:28.701484 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.701504 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.701519 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
08:48:28.701533 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
08:48:28.701547 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.701641 9718 StatsD_Checker.ttcnpp:404 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:28.704066 9747 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:28.704189 9747 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-STATS(3), component type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS. Version: 11.1.0.
08:48:28.704218 9747 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:28.704255 9747 - Connected to MC.
08:48:28.704270 9747 - Initializing variables, timers and ports of component type StatsD_Checker.StatsD_Checker_CT inside testcase TC_ctrl_msc_connection_status.
08:48:28.704289 9718 StatsD_Checker.ttcnpp:404 PTC was created. Component reference: 3, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:28.704389 9718 StatsD_Checker.ttcnpp:405 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(3).
08:48:28.704542 9718 StatsD_Checker.ttcnpp:405 Function was started.
08:48:28.704601 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
08:48:28.704683 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.704826 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
08:48:28.704869 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.704902 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.704926 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
08:48:28.704944 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
08:48:28.704961 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.704979 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
08:48:28.705004 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.705065 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 1" id 14
08:48:28.705122 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
08:48:28.705177 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.705209 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.705232 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:28.705399 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:28.705594 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 1" with ? matched
08:48:28.705685 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 1" id 14
08:48:28.705766 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 14 was extracted from the queue of BSCVTY.
08:48:28.705905 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.706040 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.706044 9747 - Port STATSVTY was started.
08:48:28.706113 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
08:48:28.706186 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
08:48:28.706269 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.706382 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
08:48:28.706437 9747 - Port STATSD_PROC was started.
08:48:28.706492 9747 - Port STATS was started.
08:48:28.706570 9747 - Component type StatsD_Checker.StatsD_Checker_CT was initialized.
08:48:28.706629 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.706757 9747 - Starting function main("127.0.0.1", 8125, 5.000000).
08:48:28.706829 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 2" id 16
08:48:28.706908 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
08:48:28.706984 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.707039 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:28.707098 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:28.707156 9747 StatsD_Checker.ttcnpp:120 Mapping port VirtMSC-STATS(3):STATS to system:STATS.
08:48:28.707173 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:28.707199 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 2" with ? matched
08:48:28.707246 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 2" id 16
08:48:28.707264 9747 StatsD_Checker.ttcnpp:120 Port STATS was mapped to system:STATS.
08:48:28.707286 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
08:48:28.707377 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.707382 9747 StatsD_Checker.ttcnpp:120 Map operation of VirtMSC-STATS(3):STATS to system:STATS finished.
08:48:28.707427 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.707458 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
08:48:28.707492 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
08:48:28.707563 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.707643 9747 StatsD_Checker.ttcnpp:121 entering f__IPL4__PROVIDER__listen: 127.0.0.1:8125 / UDP
08:48:28.708756 9718 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:28.708830 9747 StatsD_Checker.ttcnpp:129 Mapping port VirtMSC-STATS(3):STATSVTY to system:STATSVTY.
08:48:28.709604 9747 StatsD_Checker.ttcnpp:129 Message enqueued on STATSVTY from system integer : 2 id 1
08:48:28.709814 9747 StatsD_Checker.ttcnpp:129 Port STATSVTY was mapped to system:STATSVTY.
08:48:28.709906 9747 StatsD_Checker.ttcnpp:129 Map operation of VirtMSC-STATS(3):STATSVTY to system:STATSVTY finished.
08:48:28.710245 9747 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:28.710332 9747 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:28.710361 9747 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:28.710514 9747 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "enable"
08:48:28.710589 9747 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.710650 9747 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:28.710680 9747 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:28.710696 9747 Osmocom_VTY_Functions.ttcn:74 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:28.710711 9747 Osmocom_VTY_Functions.ttcn:75 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:28.710739 9747 Osmocom_VTY_Functions.ttcn:85 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:28.710809 9747 Osmocom_VTY_Functions.ttcn:86 Matching on port STATSVTY succeeded: 2 with ? matched
08:48:28.710845 9747 Osmocom_VTY_Functions.ttcn:86 Receive operation on port STATSVTY succeeded, message from system(): integer : 2 id 1
08:48:28.710870 9747 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of STATSVTY.
08:48:28.710964 9747 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 2
08:48:28.711058 9747 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.711095 9747 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.711112 9747 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:28.711134 9747 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of STATSVTY.
08:48:28.711166 9747 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.711197 9747 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "stats reset"
08:48:28.711223 9747 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:28.711275 9747 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 3
08:48:28.711302 9747 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:28.711329 9747 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:28.711344 9747 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 3
08:48:28.711366 9747 Osmocom_VTY_Functions.ttcn:73 Message with id 3 was extracted from the queue of STATSVTY.
08:48:28.711381 9747 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:28.712540 9748 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:28.712611 9748 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-SCCP(4), component type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP. Version: 11.1.0.
08:48:28.712646 9748 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:28.712683 9748 - Connected to MC.
08:48:28.712698 9748 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_ctrl_msc_connection_status.
08:48:28.712719 9718 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 4, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:28.712845 9718 SCCP_Adapter.ttcnpp:131 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:28.713940 9748 - Port SCCP_SP_PORT was started.
08:48:28.713968 9748 - Port MTP3_SCCP_PORT was started.
08:48:28.713981 9748 - Component type SCCP_Emulation.SCCP_CT was initialized.
08:48:28.715519 9749 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:28.715579 9749 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-IPA(5), component type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA. Version: 11.1.0.
08:48:28.715596 9749 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:28.715633 9749 - Connected to MC.
08:48:28.715649 9749 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc_connection_status.
08:48:28.715665 9718 SCCP_Adapter.ttcnpp:131 PTC was created. Component reference: 5, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:28.715760 9718 SCCP_Adapter.ttcnpp:132 Mapping port VirtMSC-IPA(5):IPA_PORT to system:IPA_CODEC_PT.
08:48:28.716609 9749 - Port IPA_PORT was started.
08:48:28.716644 9749 - Port CFG_PORT was started.
08:48:28.716657 9749 - Port MTP3_SP_PORT was started.
08:48:28.716670 9749 - Port IPA_MGCP_PORT was started.
08:48:28.716682 9749 - Port IPA_RSL_PORT was started.
08:48:28.716694 9749 - Port IPA_OML_PORT was started.
08:48:28.716706 9749 - Port IPA_CTRL_PORT was started.
08:48:28.716719 9749 - Port IPA_SP_PORT was started.
08:48:28.716731 9749 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:28.716768 9749 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:28.716802 9718 SCCP_Adapter.ttcnpp:132 Map operation of VirtMSC-IPA(5):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:28.716868 9718 SCCP_Adapter.ttcnpp:134 Connecting ports VirtMSC-IPA(5):MTP3_SP_PORT and VirtMSC-SCCP(4):MTP3_SCCP_PORT.
08:48:28.717072 9748 - Port MTP3_SCCP_PORT is waiting for connection from VirtMSC-IPA(5):MTP3_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-c678f479.
08:48:28.717098 9749 - Port MTP3_SP_PORT has established the connection with VirtMSC-SCCP(4):MTP3_SCCP_PORT using transport type UNIX.
08:48:28.717130 9748 - Port MTP3_SCCP_PORT has accepted the connection from VirtMSC-IPA(5):MTP3_SP_PORT.
08:48:28.717141 9718 SCCP_Adapter.ttcnpp:134 Connect operation on VirtMSC-IPA(5):MTP3_SP_PORT and VirtMSC-SCCP(4):MTP3_SCCP_PORT finished.
08:48:28.717169 9718 SCCP_Adapter.ttcnpp:136 Creating new alive PTC with component type IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:28.719481 9750 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:28.719647 9750 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMSC-IPA-WAIT(6), component type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT. Version: 11.1.0.
08:48:28.719671 9750 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:28.719719 9750 - Connected to MC.
08:48:28.719735 9750 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_EventWaiter_CT inside testcase TC_ctrl_msc_connection_status.
08:48:28.719758 9718 SCCP_Adapter.ttcnpp:136 PTC was created. Component reference: 6, alive: yes, type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:28.719869 9718 SCCP_Adapter.ttcnpp:137 Connecting ports VirtMSC-IPA(5):IPA_SP_PORT and VirtMSC-IPA-WAIT(6):IPA_SP_PORT.
08:48:28.720124 9749 - Port IPA_SP_PORT is waiting for connection from VirtMSC-IPA-WAIT(6):IPA_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-e36bb20a.
08:48:28.720785 9750 - Port IPA_SP_PORT was started.
08:48:28.720816 9750 - Component type IPA_Emulation.IPA_EventWaiter_CT was initialized.
08:48:28.720854 9750 - Port IPA_SP_PORT has established the connection with VirtMSC-IPA(5):IPA_SP_PORT using transport type UNIX.
08:48:28.720934 9749 - Port IPA_SP_PORT has accepted the connection from VirtMSC-IPA-WAIT(6):IPA_SP_PORT.
08:48:28.720966 9718 SCCP_Adapter.ttcnpp:137 Connect operation on VirtMSC-IPA(5):IPA_SP_PORT and VirtMSC-IPA-WAIT(6):IPA_SP_PORT finished.
08:48:28.721093 9718 SCCP_Adapter.ttcnpp:138 Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}) on component VirtMSC-IPA-WAIT(6).
08:48:28.721791 9718 SCCP_Adapter.ttcnpp:138 Function was started.
08:48:28.722017 9750 - Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}).
08:48:28.722094 9718 SCCP_Adapter.ttcnpp:140 Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true) on component VirtMSC-IPA(5).
08:48:28.722540 9718 SCCP_Adapter.ttcnpp:140 Function was started.
08:48:28.722794 9749 - Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true).
08:48:28.723298 9749 IPA_Emulation.ttcnpp:332 entering f__IPL4__PROVIDER__listen: 127.0.0.1:5000 / TCP
08:48:32.274419 9749 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:32.274846 9749 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:32.275030 9749 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:32.275243 9749 IPA_Emulation.ttcnpp:830 Matching on port IPA_PORT succeeded:  matched
08:48:32.275431 9749 IPA_Emulation.ttcnpp:830 Receive operation on port IPA_PORT succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:32.275574 9749 IPA_Emulation.ttcnpp:830 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:32.275727 9749 IPA_Emulation.ttcnpp:832 Established a new IPA connection (conn_id=2)
08:48:32.276278 9749 IPA_Emulation.ttcnpp:381 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(6) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
}
08:48:32.276588 9750 IPA_Emulation.ttcnpp:965 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(5) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:32.276795 9750 IPA_Emulation.ttcnpp:966 Matching on port IPA_SP_PORT ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:32.276806 9749 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:32.276829 9750 IPA_Emulation.ttcnpp:969 Matching on port IPA_SP_PORT succeeded.
08:48:32.276850 9750 IPA_Emulation.ttcnpp:969 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(5): @IPA_Emulation.ASP_IPA_Event: {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:32.276875 9750 IPA_Emulation.ttcnpp:969 Message with id 1 was extracted from the queue of IPA_SP_PORT.
08:48:32.276902 9749 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:32.277058 9749 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:32.277286 9749 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:32.277401 9749 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:32.277452 9749 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:32.277468 9749 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:32.277483 9749 IPA_Emulation.ttcnpp:745 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:32.277548 9749 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:32.277591 9749 IPA_Emulation.ttcnpp:381 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(6) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
}
08:48:32.277625 9750 IPA_Emulation.ttcnpp:965 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(5) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:32.277646 9749 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE00'O
} id 3
08:48:32.277654 9750 IPA_Emulation.ttcnpp:966 Matching on port IPA_SP_PORT succeeded:  matched
08:48:32.277669 9750 IPA_Emulation.ttcnpp:966 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(5): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:32.277680 9749 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:32.277681 9750 IPA_Emulation.ttcnpp:966 Message with id 2 was extracted from the queue of IPA_SP_PORT.
08:48:32.277736 9749 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:32.277740 9750 IPA_Emulation.ttcnpp:967 setverdict(pass): none -> pass
08:48:32.277748 9749 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:32.277760 9749 IPA_Emulation.ttcnpp:745 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:32.277767 9750 - Function waiter_main finished. PTC remains alive and is waiting for next start.
08:48:32.277774 9749 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_PING (0),
    u := omit
}
08:48:32.277792 9749 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_PONG (1),
    u := omit
}
08:48:32.277805 9749 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '01'O
}
08:48:32.277837 9749 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE01'O
}
08:48:32.277871 9718 SCCP_Adapter.ttcnpp:151 PTC with component reference 6 is done.
08:48:32.277930 9718 SCCP_Adapter.ttcnpp:152 Disconnecting ports VirtMSC-IPA(5):IPA_SP_PORT and VirtMSC-IPA-WAIT(6):IPA_SP_PORT.
08:48:32.277966 9750 - Terminating the connection of port IPA_SP_PORT to VirtMSC-IPA(5):IPA_SP_PORT. No more messages can be sent through this connection.
08:48:32.277991 9749 IPA_Emulation.ttcnpp:743 Connection termination request was received on port IPA_SP_PORT from VirtMSC-IPA-WAIT(6):IPA_SP_PORT. No more data can be sent or received through this connection.
08:48:32.278011 9750 - Port IPA_SP_PORT was disconnected from VirtMSC-IPA(5):IPA_SP_PORT.
08:48:32.278033 9749 IPA_Emulation.ttcnpp:743 Port IPA_SP_PORT was disconnected from VirtMSC-IPA-WAIT(6):IPA_SP_PORT.
08:48:32.278061 9718 SCCP_Adapter.ttcnpp:152 Disconnect operation on VirtMSC-IPA(5):IPA_SP_PORT and VirtMSC-IPA-WAIT(6):IPA_SP_PORT finished.
08:48:32.278142 9718 BSC_Tests.ttcn:1221 Connecting ports mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(5):CFG_PORT.
08:48:32.278276 9718 BSC_Tests.ttcn:1221 Port SCCPLITE_IPA_CFG_PORT[0] is waiting for connection from VirtMSC-IPA(5):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-5607b44b.
08:48:32.278311 9749 IPA_Emulation.ttcnpp:743 Port CFG_PORT has established the connection with mtc:SCCPLITE_IPA_CFG_PORT[0] using transport type UNIX.
08:48:32.278330 9718 BSC_Tests.ttcn:1221 Port SCCPLITE_IPA_CFG_PORT[0] has accepted the connection from VirtMSC-IPA(5):CFG_PORT.
08:48:32.278345 9718 BSC_Tests.ttcn:1221 Connect operation on mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(5):CFG_PORT finished.
08:48:32.278361 9718 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(4):SCCP_SP_PORT.
08:48:32.278447 9718 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(4):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-457cb81d.
08:48:32.278489 9748 - Port SCCP_SP_PORT has established the connection with mtc:BSSAP using transport type UNIX.
08:48:32.278517 9718 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(4):SCCP_SP_PORT.
08:48:32.278531 9718 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(4):SCCP_SP_PORT finished.
08:48:32.278575 9718 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}) on component VirtMSC-SCCP(4).
08:48:32.278739 9718 SCCP_Adapter.ttcnpp:165 Function was started.
08:48:32.278863 9748 - Starting function SCCPStart({
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}).
08:48:32.279048 9748 SCCP_Emulation.ttcn:1453 v_sccp_pdu_maxlen:268
08:48:32.279109 9749 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0016FD090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:32.279154 9749 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:32.279271 9749 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_SCCP (253) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:32.279310 9749 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:32.279311 9718 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(4) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 0,
                        causeValue := '0000000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:48:32.279328 9749 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:32.279344 9749 IPA_Emulation.ttcnpp:761 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:32.279369 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 0,
                    causeValue := '0000000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:32.279571 9749 IPA_Emulation.ttcnpp:767 Sent on MTP3_SP_PORT to VirtMSC-SCCP(4) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
}
08:48:32.279573 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
08:48:32.279632 9718 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
}
08:48:32.279711 9748 SCCP_Emulation.ttcn:5439 Message enqueued on MTP3_SCCP_PORT from VirtMSC-IPA(5) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 1
08:48:32.279726 9718 BSC_Tests.ttcn:899 Start timer T: 5 s
08:48:32.280157 9748 SCCP_Emulation.ttcn:5439 Incoming message was mapped to @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:32.280230 9748 SCCP_Emulation.ttcn:5443 Matching on port MTP3_SCCP_PORT succeeded:  matched
08:48:32.280257 9748 SCCP_Emulation.ttcn:5443 Receive operation on port MTP3_SCCP_PORT succeeded, message from VirtMSC-IPA(5): @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:32.280288 9748 SCCP_Emulation.ttcn:5443 Message with id 1 was extracted from the queue of MTP3_SCCP_PORT.
08:48:32.280678 9748 SCCP_Emulation.ttcn:3464 Sent on SCCP_SP_PORT to mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
}
08:48:32.280886 9748 SCCP_Emulation.ttcn:5439 Message enqueued on SCCP_SP_PORT from mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:32.280901 9718 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(4) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
} id 1
08:48:32.280933 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000430040120'O
08:48:32.280948 9748 SCCP_Emulation.ttcn:5577 Matching on port SCCP_SP_PORT succeeded.
08:48:32.280971 9748 SCCP_Emulation.ttcn:5577 Check-receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req: {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:32.280988 9748 SCCP_Emulation.ttcn:5585 Matching on port SCCP_SP_PORT failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_DATA_req.
08:48:32.281047 9748 SCCP_Emulation.ttcn:5591 Matching on port SCCP_SP_PORT succeeded:  matched
08:48:32.281064 9748 SCCP_Emulation.ttcn:5591 Receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:32.281085 9748 SCCP_Emulation.ttcn:5591 Message with id 1 was extracted from the queue of SCCP_SP_PORT.
08:48:32.281594 9748 SCCP_Emulation.ttcn:5223 Sent on MTP3_SCCP_PORT to VirtMSC-IPA(5) @SCCP_Types.ASP_MTP3_TRANSFERreq_sccp : {
    sio := '83'O,
    opc := 185,
    dpc := 187,
    sls := 0,
    data := {
        unitdata := {
            messageType := 9,
            protClass := {
                class := '0000'B,
                messageHandling := '0000'B
            },
            pointer1 := 0,
            pointer2 := 0,
            pointer3 := 0,
            calledPAddress := {
                paramLength := 4,
                addr := '43BB00FE'O
            },
            callingPAddress := {
                paramLength := 4,
                addr := '43B900FE'O
            },
            data := {
                paramLength := 6,
                data := '000430040100'O
            }
        }
    }
}
08:48:32.281767 9748 SCCP_Emulation.ttcn:5223 Outgoing message was mapped to @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:32.281881 9749 IPA_Emulation.ttcnpp:743 Message enqueued on MTP3_SP_PORT from VirtMSC-SCCP(4) @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
} id 1
08:48:32.281960 9749 IPA_Emulation.ttcnpp:865 Matching on port MTP3_SP_PORT succeeded:  matched
08:48:32.281984 9749 IPA_Emulation.ttcnpp:865 Receive operation on port MTP3_SP_PORT succeeded, message from VirtMSC-SCCP(4): @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
} id 1
08:48:32.282005 9749 IPA_Emulation.ttcnpp:865 Message with id 1 was extracted from the queue of MTP3_SP_PORT.
08:48:32.282031 9749 IPA_Emulation.ttcnpp:868 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:32.282050 9749 IPA_Emulation.ttcnpp:868 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0016FD090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:32.282252 9749 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0013FD090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:32.282282 9749 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:32.282298 9749 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_SCCP (253) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:32.282322 9749 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:32.282345 9749 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:32.282366 9749 IPA_Emulation.ttcnpp:761 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:32.282391 9749 IPA_Emulation.ttcnpp:767 Sent on MTP3_SP_PORT to VirtMSC-SCCP(4) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE03000131'O
}
08:48:32.282452 9748 SCCP_Emulation.ttcn:5439 Message enqueued on MTP3_SCCP_PORT from VirtMSC-IPA(5) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE03000131'O
} id 2
08:48:32.282478 9748 SCCP_Emulation.ttcn:5439 Incoming message was mapped to @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 3,
            data := '000131'O
        }
    }
} id 2
08:48:32.282495 9748 SCCP_Emulation.ttcn:5443 Matching on port MTP3_SCCP_PORT succeeded:  matched
08:48:32.282511 9748 SCCP_Emulation.ttcn:5443 Receive operation on port MTP3_SCCP_PORT succeeded, message from VirtMSC-IPA(5): @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 3,
            data := '000131'O
        }
    }
} id 2
08:48:32.282528 9748 SCCP_Emulation.ttcn:5443 Message with id 2 was extracted from the queue of MTP3_SCCP_PORT.
08:48:32.282557 9748 SCCP_Emulation.ttcn:3464 Sent on SCCP_SP_PORT to mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
}
08:48:32.283055 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 4,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 1,
                    causeValue := '0100000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:32.283099 9718 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:32.283321 9718 BSC_Tests.ttcn:901 Matching on port BSSAP .userData.pdu.bssmap{
    reset := {
        messageType := '30'O ("0"),
        cause := {
            elementIdentifier := '04'O,
            lengthIndicator := 1,
            causeValue := '0100000'B,
            extensionCauseValue := '0'B,
            spare1 := omit
        },
        a_InterfaceSelectorForReset := omit,
        osmuxSupport := omit
    }
} with {
    resetAck := {
        messageType := '31'O ("1"),
        a_InterfaceSelectorForReset := *,
        osmuxSupport := omit
    }
} unmatched: First message in the queue does not match the template: 
08:48:32.283384 9718 BSC_Tests.ttcn:905 Matching on port BSSAP succeeded:  matched
08:48:32.283414 9718 BSC_Tests.ttcn:905 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(4): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:32.283435 9718 BSC_Tests.ttcn:905 Message with id 1 was extracted from the queue of BSSAP.
08:48:32.283461 9718 BSC_Tests.ttcn:906 BSSMAP: Respoding to inbound RESET with RESET-ACK
08:48:32.283515 9718 BSC_Tests.ttcn:907 Sent on BSSAP to VirtMSC-SCCP(4) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:48:32.283535 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:32.283557 9718 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000131'O
08:48:32.283573 9718 BSC_Tests.ttcn:907 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
}
08:48:32.283597 9748 SCCP_Emulation.ttcn:5439 Message enqueued on SCCP_SP_PORT from mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:32.283608 9718 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(4) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
} id 2
08:48:32.283615 9748 SCCP_Emulation.ttcn:5577 Matching on port SCCP_SP_PORT succeeded.
08:48:32.283626 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
08:48:32.283627 9748 SCCP_Emulation.ttcn:5577 Check-receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req: {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:32.283646 9748 SCCP_Emulation.ttcn:5585 Matching on port SCCP_SP_PORT failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_DATA_req.
08:48:32.283678 9748 SCCP_Emulation.ttcn:5591 Matching on port SCCP_SP_PORT succeeded:  matched
08:48:32.283688 9718 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 1,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:32.283695 9748 SCCP_Emulation.ttcn:5591 Receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:32.283709 9718 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 2
08:48:32.283711 9748 SCCP_Emulation.ttcn:5591 Message with id 2 was extracted from the queue of SCCP_SP_PORT.
08:48:32.283735 9718 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
08:48:32.283747 9748 SCCP_Emulation.ttcn:5223 Sent on MTP3_SCCP_PORT to VirtMSC-IPA(5) @SCCP_Types.ASP_MTP3_TRANSFERreq_sccp : {
    sio := '83'O,
    opc := 185,
    dpc := 187,
    sls := 0,
    data := {
        unitdata := {
            messageType := 9,
            protClass := {
                class := '0000'B,
                messageHandling := '0000'B
            },
            pointer1 := 0,
            pointer2 := 0,
            pointer3 := 0,
            calledPAddress := {
                paramLength := 4,
                addr := '43BB00FE'O
            },
            callingPAddress := {
                paramLength := 4,
                addr := '43B900FE'O
            },
            data := {
                paramLength := 3,
                data := '000131'O
            }
        }
    }
}
08:48:32.283753 9718 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(4): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 2
08:48:32.283770 9748 SCCP_Emulation.ttcn:5223 Outgoing message was mapped to @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:32.283770 9718 BSC_Tests.ttcn:901 Message with id 2 was extracted from the queue of BSSAP.
08:48:32.283789 9718 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
08:48:32.283803 9749 IPA_Emulation.ttcnpp:743 Message enqueued on MTP3_SP_PORT from VirtMSC-SCCP(4) @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 2
08:48:32.283809 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
08:48:32.283836 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:32.283859 9749 IPA_Emulation.ttcnpp:865 Matching on port MTP3_SP_PORT succeeded:  matched
08:48:32.283895 9749 IPA_Emulation.ttcnpp:865 Receive operation on port MTP3_SP_PORT succeeded, message from VirtMSC-SCCP(4): @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '10'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 2
08:48:32.283928 9749 IPA_Emulation.ttcnpp:865 Message with id 2 was extracted from the queue of MTP3_SP_PORT.
08:48:32.283962 9749 IPA_Emulation.ttcnpp:868 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:32.283990 9749 IPA_Emulation.ttcnpp:868 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0013FD090003070B0443BB00FE0443B900FE03000131'O
}
08:48:32.285082 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:32.285122 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 19
08:48:32.286191 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:32.287210 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:32.288181 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:32.289315 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:32.290424 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with ? matched
08:48:32.291615 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:32.291676 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 18 was extracted from the queue of BSCVTY.
08:48:32.291726 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:32.291771 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:32.291810 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 19
08:48:32.291836 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 19 was extracted from the queue of BSCVTY.
08:48:32.291863 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:32.292084 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:32.292139 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:32.292217 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 20
08:48:32.292267 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:32.292310 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:32.292359 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:32.292389 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 20
08:48:32.292417 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
08:48:32.292448 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:32.292477 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:32.292515 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:32.292570 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 21
08:48:32.292615 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:32.292690 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:32.292760 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:32.292781 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 21
08:48:32.292796 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
08:48:32.292810 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:32.292843 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
08:48:32.292877 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:32.292919 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 22
08:48:32.292944 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:32.292964 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:32.292990 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:32.293020 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 22
08:48:32.293042 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 22 was extracted from the queue of BSCVTY.
08:48:32.293059 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:32.293074 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:32.293093 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:32.293138 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
08:48:32.293169 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:32.293190 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:32.293214 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:32.293227 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
08:48:32.293241 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
08:48:32.293254 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:32.293266 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:32.293292 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:32.293320 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 24
08:48:32.293342 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:32.293363 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:32.293377 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 24
08:48:32.293392 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 24 was extracted from the queue of BSCVTY.
08:48:32.293406 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:32.293436 9718 BSC_Tests.ttcn:1191 msc 1 is not configured, skipping
08:48:32.293475 9718 BSC_Tests.ttcn:1191 msc 2 is not configured, skipping
08:48:32.293542 9718 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:32.296215 9752 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:32.296284 9752 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: IPA-CTRL-CLI-IPA(7), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA. Version: 11.1.0.
08:48:32.296302 9752 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:32.296353 9752 - Connected to MC.
08:48:32.296369 9752 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc_connection_status.
08:48:32.296388 9718 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 7, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:32.296429 9718 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(7):IPA_PORT to system:IPA_CODEC_PT.
08:48:32.297448 9752 - Port IPA_PORT was started.
08:48:32.297477 9752 - Port CFG_PORT was started.
08:48:32.297491 9752 - Port MTP3_SP_PORT was started.
08:48:32.297503 9752 - Port IPA_MGCP_PORT was started.
08:48:32.297516 9752 - Port IPA_RSL_PORT was started.
08:48:32.297528 9752 - Port IPA_OML_PORT was started.
08:48:32.297541 9752 - Port IPA_CTRL_PORT was started.
08:48:32.297553 9752 - Port IPA_SP_PORT was started.
08:48:32.297573 9752 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:32.297615 9752 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:32.297647 9718 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(7):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:32.297674 9718 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(7):IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:32.297862 9718 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(7):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-4937f21f.
08:48:32.297894 9752 - Port IPA_CTRL_PORT has established the connection with mtc:IPA_CTRL using transport type UNIX.
08:48:32.297925 9718 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(7):IPA_CTRL_PORT.
08:48:32.297942 9718 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(7):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
08:48:32.297980 9718 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false) on component IPA-CTRL-CLI-IPA(7).
08:48:32.298051 9718 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
08:48:32.298093 9718 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
08:48:32.298144 9752 - Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false).
08:48:32.298308 9752 IPA_Emulation.ttcnpp:316 entering f__IPL4__PROVIDER__connect: :0 -> 127.0.0.1:4249 / TCP
08:48:32.299257 9752 IPA_Emulation.ttcnpp:395 Sent on IPA_CTRL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:32.299454 9718 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(7) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:32.299576 9718 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
08:48:32.299601 9718 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(7): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:32.299623 9718 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
08:48:32.299702 9718 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:32.302346 9753 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:32.302419 9753 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: VirtMGW-MGCP-0(8), component type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0. Version: 11.1.0.
08:48:32.302439 9753 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:32.302488 9753 - Connected to MC.
08:48:32.302504 9753 - Initializing variables, timers and ports of component type MGCP_Emulation.MGCP_Emulation_CT inside testcase TC_ctrl_msc_connection_status.
08:48:32.302520 9718 BSC_Tests.ttcn:1073 PTC was created. Component reference: 8, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:32.302576 9718 BSC_Tests.ttcn:1074 Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(8).
08:48:32.302740 9718 BSC_Tests.ttcn:1074 Function was started.
08:48:32.302781 9718 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:32.302844 9718 Osmocom_CTRL_Functions.ttcn:30 Random number generator was initialized with seed 5.302844: srand48(566559059).
08:48:32.302863 9718 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.743431.
08:48:32.303049 9718 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(7) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "743431400",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:32.303115 9718 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:32.303195 9752 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "743431400",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:32.303291 9752 IPA_Emulation.ttcnpp:887 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:32.303324 9752 IPA_Emulation.ttcnpp:887 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "743431400",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:32.303347 9752 IPA_Emulation.ttcnpp:887 Message with id 1 was extracted from the queue of IPA_CTRL_PORT.
08:48:32.303589 9753 - Port MGCP was started.
08:48:32.303615 9753 - Port MGCP_CLIENT was started.
08:48:32.303630 9753 - Port MGCP_CLIENT_MULTI was started.
08:48:32.303643 9753 - Port MGCP_PROC was started.
08:48:32.303656 9753 - Component type MGCP_Emulation.MGCP_Emulation_CT was initialized.
08:48:32.303719 9753 - Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0").
08:48:32.303782 9752 IPA_Emulation.ttcnpp:890 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420373433343331343030206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 743431400 bts.0.oml-connection-state")
}
08:48:32.303925 9753 MGCP_Emulation.ttcn:279 Mapping port VirtMGW-MGCP-0(8):MGCP to system:MGCP_CODEC_PT.
08:48:32.303974 9753 MGCP_Emulation.ttcn:279 Port MGCP was mapped to system:MGCP_CODEC_PT.
08:48:32.303977 9752 IPA_Emulation.ttcnpp:890 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420373433343331343030206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:32.304009 9753 MGCP_Emulation.ttcn:279 Map operation of VirtMGW-MGCP-0(8):MGCP to system:MGCP_CODEC_PT finished.
08:48:32.304112 9753 MGCP_Emulation.ttcn:281 entering f__IPL4__PROVIDER__listen: 127.0.0.1:2427 / UDP
08:48:32.304260 9752 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 37783,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0038EE004745545F5245504C5920373433343331343030206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
} id 1
08:48:32.304380 9752 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920373433343331343030206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 743431400 bts.0.oml-connection-state degraded")
} id 1
08:48:32.304435 9752 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:32.304460 9752 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920373433343331343030206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 743431400 bts.0.oml-connection-state degraded")
} id 1
08:48:32.304481 9752 IPA_Emulation.ttcnpp:761 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:32.304658 9752 IPA_Emulation.ttcnpp:634 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "743431400",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
08:48:32.304741 9718 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(7) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "743431400",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:48:32.304796 9718 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:32.304816 9718 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(7): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "743431400",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:48:32.304832 9718 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
08:48:32.304874 9718 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:32.304896 9718 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:33.304920 9718 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:33.305189 9718 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:33.313572 9755 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:33.313752 9755 - TTCN-3 Parallel Test Component started on cbea39017248. Component reference: IPA-BTS0-TRX0-RSL-IPA(9), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA. Version: 11.1.0.
08:48:33.313827 9755 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:33.313913 9755 - Connected to MC.
08:48:33.313951 9755 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc_connection_status.
08:48:33.314091 9718 BSC_Tests.ttcn:951 PTC was created. Component reference: 9, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:33.314321 9718 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: {
    site_id := 1234,
    bts_id := 0,
    trx_id := 0
}
08:48:33.314636 9718 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
08:48:33.314704 9718 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(9):IPA_PORT to system:IPA_CODEC_PT.
08:48:33.316612 9755 - Port IPA_PORT was started.
08:48:33.316741 9755 - Port CFG_PORT was started.
08:48:33.316778 9755 - Port MTP3_SP_PORT was started.
08:48:33.316813 9755 - Port IPA_MGCP_PORT was started.
08:48:33.316845 9755 - Port IPA_RSL_PORT was started.
08:48:33.316897 9755 - Port IPA_OML_PORT was started.
08:48:33.316934 9755 - Port IPA_CTRL_PORT was started.
08:48:33.316968 9755 - Port IPA_SP_PORT was started.
08:48:33.317001 9755 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:33.317121 9755 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:33.317317 9718 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(9):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:33.317379 9718 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(9):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
08:48:33.317862 9718 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(9):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-49708b6e.
08:48:33.318024 9755 - Port CFG_PORT has established the connection with mtc:IPA_CFG_PORT[0][0] using transport type UNIX.
08:48:33.318248 9718 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(9):CFG_PORT.
08:48:33.318605 9718 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(9):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
08:48:33.318759 9718 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(9):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
08:48:33.319534 9718 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(9):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-2a6aab76.
08:48:33.319696 9755 - Port IPA_RSL_PORT has established the connection with mtc:IPA_RSL[0][0] using transport type UNIX.
08:48:33.319797 9718 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(9):IPA_RSL_PORT.
08:48:33.319877 9718 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(9):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
08:48:33.320050 9718 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true) on component IPA-BTS0-TRX0-RSL-IPA(9).
08:48:33.320223 9718 BSC_Tests.ttcn:969 Function was started.
08:48:33.320329 9718 BSC_Tests.ttcn:976 Start timer T: 10 s
08:48:33.320614 9755 - Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true).
08:48:33.321260 9755 IPA_Emulation.ttcnpp:316 entering f__IPL4__PROVIDER__connect: :10000 -> 127.0.0.1:3003 / TCP
08:48:33.325240 9755 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:33.325759 9755 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:33.326344 9755 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:33.327571 9755 IPA_Emulation.ttcnpp:385 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:33.327922 9718 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:33.328207 9718 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:33.328318 9718 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:33.328391 9718 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(9): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:33.328784 9718 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
08:48:33.330169 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0011FE0401080107010201030104010501010100'O
} id 1
08:48:33.330508 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:33.330595 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:33.330648 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:33.330829 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:33.330919 9755 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:33.330972 9755 IPA_Emulation.ttcnpp:745 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:33.331062 9755 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
08:48:33.331581 9755 IPA_Emulation.ttcnpp:479 CCM Tx:{
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
08:48:33.331752 9755 IPA_Emulation.ttcnpp:480 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:33.331814 9755 IPA_Emulation.ttcnpp:480 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:33.331930 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT succeeded:  matched
08:48:33.331978 9755 IPA_Emulation.ttcnpp:745 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:33.332017 9755 IPA_Emulation.ttcnpp:745 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:33.332054 9755 IPA_Emulation.ttcnpp:747 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:33.332099 9755 IPA_Emulation.ttcnpp:385 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
}
08:48:33.332173 9718 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:33.332278 9718 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:33.332382 9718 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(9): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:33.332497 9718 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
08:48:33.332823 9718 BSC_Tests.ttcn:979 Stop timer T: 10 s
08:48:33.333094 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:33.333208 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:33.333483 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.333640 9718 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:33.333748 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.333806 9718 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.152166.
08:48:33.333845 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:33.333898 9718 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(7) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "152166160",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:33.333968 9755 IPA_Emulation.ttcnpp:761 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:33.334024 9718 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:33.334124 9752 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "152166160",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:33.334397 9752 IPA_Emulation.ttcnpp:887 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:33.334545 9752 IPA_Emulation.ttcnpp:887 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "152166160",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:33.334686 9752 IPA_Emulation.ttcnpp:887 Message with id 2 was extracted from the queue of IPA_CTRL_PORT.
08:48:33.335032 9752 IPA_Emulation.ttcnpp:890 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420313532313636313630206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 152166160 bts.0.oml-connection-state")
}
08:48:33.335172 9752 IPA_Emulation.ttcnpp:890 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420313532313636313630206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:33.335451 9752 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 37783,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0039EE004745545F5245504C5920313532313636313630206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
} id 2
08:48:33.335627 9752 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313532313636313630206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 152166160 bts.0.oml-connection-state connected")
} id 2
08:48:33.335731 9752 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.335819 9752 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313532313636313630206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 152166160 bts.0.oml-connection-state connected")
} id 2
08:48:33.335948 9752 IPA_Emulation.ttcnpp:761 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:33.336113 9752 IPA_Emulation.ttcnpp:634 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "152166160",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
08:48:33.336287 9718 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(7) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "152166160",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:48:33.336545 9718 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:33.336698 9718 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(7): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "152166160",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:48:33.336825 9718 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
08:48:33.337009 9718 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:33.337096 9718 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:33.338386 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
}
08:48:33.338702 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:33.338765 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:33.338797 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0006000C1101801E0A'O
} id 5
08:48:33.338839 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:33.338876 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:33.338913 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:33.338948 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:33.338979 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:33.339134 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:33.339282 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:33.339361 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:33.339471 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
08:48:33.339492 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:33.339775 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:33.339897 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:33.340015 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:33.340108 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:33.340184 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '000400101A1E0D'O
} id 12
08:48:33.340256 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:33.340571 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.340686 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.340752 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:33.340815 9755 IPA_Emulation.ttcnpp:761 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:33.341100 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
}
08:48:33.341306 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.341406 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.341416 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
} id 4
08:48:33.341477 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:33.341583 9755 IPA_Emulation.ttcnpp:761 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:33.341881 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
}
08:48:33.342007 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.342116 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.342248 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
} id 5
08:48:33.342324 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:33.342420 9755 IPA_Emulation.ttcnpp:761 Message with id 6 was extracted from the queue of IPA_PORT.
08:48:33.342728 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:33.342840 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.342912 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
} id 6
08:48:33.342923 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.343180 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:33.343372 9755 IPA_Emulation.ttcnpp:761 Message with id 7 was extracted from the queue of IPA_PORT.
08:48:33.343770 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:33.344107 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.344255 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 7
08:48:33.344397 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.344773 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:33.344939 9755 IPA_Emulation.ttcnpp:761 Message with id 8 was extracted from the queue of IPA_PORT.
08:48:33.345240 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
}
08:48:33.345378 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.345456 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
} id 8
08:48:33.345610 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.345693 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:33.345769 9755 IPA_Emulation.ttcnpp:761 Message with id 9 was extracted from the queue of IPA_PORT.
08:48:33.345950 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:33.346078 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.346167 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.346170 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 9
08:48:33.346255 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:33.346343 9755 IPA_Emulation.ttcnpp:761 Message with id 10 was extracted from the queue of IPA_PORT.
08:48:33.346542 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:33.346639 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.346688 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 10
08:48:33.346937 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.347124 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:33.347363 9755 IPA_Emulation.ttcnpp:761 Message with id 11 was extracted from the queue of IPA_PORT.
08:48:33.347840 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:33.348094 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.348289 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.348391 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 11
08:48:33.348617 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:33.348834 9755 IPA_Emulation.ttcnpp:761 Message with id 12 was extracted from the queue of IPA_PORT.
08:48:33.349189 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
}
08:48:33.349476 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
} id 12
08:48:33.349511 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:33.349725 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:33.349877 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001400101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:33.349960 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:33.350057 9755 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:33.350148 9755 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:33.350239 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.350322 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.350400 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:33.350475 9755 IPA_Emulation.ttcnpp:761 Message with id 13 was extracted from the queue of IPA_PORT.
08:48:33.350663 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:33.350752 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.350813 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.350857 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 13
08:48:33.350875 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:33.351086 9755 IPA_Emulation.ttcnpp:761 Message with id 14 was extracted from the queue of IPA_PORT.
08:48:33.351322 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
}
08:48:33.351767 9755 IPA_Emulation.ttcnpp:745 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:33.351812 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
} id 14
08:48:33.351946 9755 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:33.352142 9755 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:33.352341 9755 IPA_Emulation.ttcnpp:761 Message with id 15 was extracted from the queue of IPA_PORT.
08:48:33.353163 9755 IPA_Emulation.ttcnpp:782 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:33.353653 9718 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(9) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 15
08:48:34.338086 9718 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:36.360344 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:36.361149 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:36.361686 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 25
08:48:36.362190 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.362241 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:36.362280 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:36.362352 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 25
08:48:36.362410 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
08:48:36.362515 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:36.362607 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:48:36.362697 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:36.362844 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 26
08:48:36.362939 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.362992 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:36.363042 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:48:36.363101 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 26
08:48:36.363138 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
08:48:36.363168 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:36.363392 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:48:36.363754 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:36.364040 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:36.364289 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.364540 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:36.364783 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:36.365079 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:36.365244 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 27 was extracted from the queue of BSCVTY.
08:48:36.365510 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:36.365837 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:36.366072 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:36.366470 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:36.366728 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.367021 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:36.367178 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:36.367264 9718 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:36.367463 9718 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
08:48:36.367569 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:36.367695 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:36.367840 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:36.367995 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 29
08:48:36.368160 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.368298 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:36.368378 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 29
08:48:36.368460 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 29 was extracted from the queue of BSCVTY.
08:48:36.368571 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:36.368951 9718 Osmocom_VTY_Functions.ttcn:333 "TC_ctrl_msc_connection_status() start"
08:48:36.369222 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_ctrl_msc_connection_status() start"
08:48:36.369382 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:36.369599 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 30
08:48:36.369744 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.369870 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:36.369972 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 30
08:48:36.370054 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 30 was extracted from the queue of BSCVTY.
08:48:36.370138 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:36.370372 9718 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.133656.
08:48:36.370505 9718 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(7) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "133656249",
        variable := "msc_connection_status",
        val := omit
    }
}
08:48:36.370741 9718 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:36.370820 9752 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "133656249",
        variable := "msc_connection_status",
        val := omit
    }
} id 3
08:48:36.371027 9752 IPA_Emulation.ttcnpp:887 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:36.371154 9752 IPA_Emulation.ttcnpp:887 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "133656249",
        variable := "msc_connection_status",
        val := omit
    }
} id 3
08:48:36.371438 9752 IPA_Emulation.ttcnpp:887 Message with id 3 was extracted from the queue of IPA_CTRL_PORT.
08:48:36.371629 9752 IPA_Emulation.ttcnpp:890 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420313333363536323439206D73635F636F6E6E656374696F6E5F737461747573'O ("GET 133656249 msc_connection_status")
}
08:48:36.371749 9752 IPA_Emulation.ttcnpp:890 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0024EE0047455420313333363536323439206D73635F636F6E6E656374696F6E5F737461747573'O
}
08:48:36.372099 9752 IPA_Emulation.ttcnpp:743 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 37783,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0034EE004745545F5245504C5920313333363536323439206D73635F636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O
} id 3
08:48:36.372218 9752 IPA_Emulation.ttcnpp:743 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313333363536323439206D73635F636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 133656249 msc_connection_status connected")
} id 3
08:48:36.372305 9752 IPA_Emulation.ttcnpp:761 Matching on port IPA_PORT succeeded:  matched
08:48:36.372390 9752 IPA_Emulation.ttcnpp:761 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313333363536323439206D73635F636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 133656249 msc_connection_status connected")
} id 3
08:48:36.372505 9752 IPA_Emulation.ttcnpp:761 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:36.372670 9752 IPA_Emulation.ttcnpp:634 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "133656249",
        variable := "msc_connection_status",
        val := "connected"
    }
}
08:48:36.372982 9718 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(7) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "133656249",
        variable := "msc_connection_status",
        val := "connected"
    }
} id 4
08:48:36.373300 9718 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:36.373441 9718 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(7): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "133656249",
        variable := "msc_connection_status",
        val := "connected"
    }
} id 4
08:48:36.373587 9718 Osmocom_CTRL_Functions.ttcn:41 Message with id 4 was extracted from the queue of IPA_CTRL.
08:48:36.374720 9718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
08:48:36.374904 9718 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:36.375994 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" id 31
08:48:36.376113 9718 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
08:48:36.376278 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.376541 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:36.376739 9718 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:36.376860 9718 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:36.376951 9718 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" with ? matched
08:48:36.377033 9718 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1407494 bytes in 1282 blocks)" id 31
08:48:36.377131 9718 Osmocom_VTY_Functions.ttcn:85 Message with id 31 was extracted from the queue of BSCVTY.
08:48:36.377328 9718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:36.377770 9718 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:36.377861 9718 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
08:48:36.377933 9718 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
08:48:36.378046 9718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:36.378357 9718 Osmocom_VTY_Functions.ttcn:260 talloc reports "struct bsc_subscr" x 0, expecting 0
08:48:36.378536 9718 Osmocom_VTY_Functions.ttcn:260 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
08:48:36.378700 9718 BSC_Tests.ttcn:888 Stopping all components.
08:48:36.378858 9747 StatsD_Checker.ttcnpp:138 Kill was requested from MC.
08:48:36.378870 9748 SCCP_Emulation.ttcn:5439 Stop was requested from MC.
08:48:36.378904 9749 IPA_Emulation.ttcnpp:743 Stop was requested from MC.
08:48:36.378919 9753 MGCP_Emulation.ttcn:301 Stop was requested from MC.
08:48:36.378928 9755 IPA_Emulation.ttcnpp:743 Stop was requested from MC.
08:48:36.378998 9752 IPA_Emulation.ttcnpp:743 Kill was requested from MC.
08:48:36.379028 9747 StatsD_Checker.ttcnpp:138 Terminating test component execution.
08:48:36.379080 9748 SCCP_Emulation.ttcn:5439 Stopping test component execution.
08:48:36.379128 9755 IPA_Emulation.ttcnpp:743 Stopping test component execution.
08:48:36.379177 9749 IPA_Emulation.ttcnpp:743 Stopping test component execution.
08:48:36.379229 9752 IPA_Emulation.ttcnpp:743 Terminating test component execution.
08:48:36.379372 9753 MGCP_Emulation.ttcn:301 Stopping test component execution.
08:48:36.381624 9747 - Function main was stopped. PTC terminates.
08:48:36.381637 9753 - Function main was stopped. PTC remains alive and is waiting for next start.
08:48:36.381686 9752 - Function main_client was stopped. PTC terminates.
08:48:36.381732 9755 - Function main_client was stopped. PTC remains alive and is waiting for next start.
08:48:36.381858 9747 - Terminating component type StatsD_Checker.StatsD_Checker_CT.
08:48:36.381949 9747 - Removing unterminated mapping between port STATSVTY and system:STATSVTY.
08:48:36.382178 9749 - Function main_server was stopped. PTC remains alive and is waiting for next start.
08:48:36.382256 9752 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:36.382364 9748 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
08:48:36.382523 9752 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:36.383008 9747 - Port STATSVTY was unmapped from system:STATSVTY.
08:48:36.383118 9747 - Port STATSVTY was stopped.
08:48:36.383178 9747 - Port STATSD_PROC was stopped.
08:48:36.383268 9747 - Removing unterminated mapping between port STATS and system:STATS.
08:48:36.384120 9747 - Port STATS was unmapped from system:STATS.
08:48:36.384205 9752 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:36.384236 9747 - Port STATS was stopped.
08:48:36.384300 9747 - Component type StatsD_Checker.StatsD_Checker_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.384381 9747 - Final verdict of PTC: none
08:48:36.384401 9752 - Port IPA_PORT was stopped.
08:48:36.384512 9752 - Port CFG_PORT was stopped.
08:48:36.384611 9747 - Disconnected from MC.
08:48:36.384683 9752 - Port MTP3_SP_PORT was stopped.
08:48:36.384766 9747 - TTCN-3 Parallel Test Component finished.
08:48:36.385010 9752 - Port IPA_MGCP_PORT was stopped.
08:48:36.385077 9752 - Port IPA_RSL_PORT was stopped.
08:48:36.385130 9752 - Port IPA_OML_PORT was stopped.
08:48:36.385222 9752 - Removing unterminated connection between port IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:36.385366 9752 - Port IPA_CTRL_PORT was stopped.
08:48:36.385409 9718 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(7):IPA_CTRL_PORT was closed unexpectedly by the peer.
08:48:36.385616 9752 - Port IPA_SP_PORT was stopped.
08:48:36.385628 9718 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(7):IPA_CTRL_PORT.
08:48:36.385733 9752 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.385804 9752 - Final verdict of PTC: none
08:48:36.385952 9718 BSC_Tests.ttcn:888 All components were stopped.
08:48:36.386093 9752 - Disconnected from MC.
08:48:36.386134 9718 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
08:48:36.386315 9718 BSC_Tests.ttcn:890 Stopping test component execution.
08:48:36.386326 9752 - TTCN-3 Parallel Test Component finished.
08:48:36.387795 9718 BSC_Tests.ttcn:3184 Test case TC_ctrl_msc_connection_status was stopped.
08:48:36.388282 9718 BSC_Tests.ttcn:3184 Terminating component type BSC_Tests.test_CT.
08:48:36.388675 9718 BSC_Tests.ttcn:3184 Default with id 1 (altstep as_Tguard) was deactivated.
08:48:36.388923 9718 BSC_Tests.ttcn:3184 Stop timer T_guard: 30 s
08:48:36.389084 9718 BSC_Tests.ttcn:3184 Port IPA_CTRL was stopped.
08:48:36.389317 9718 BSC_Tests.ttcn:3184 Port RSL_CCHAN[0] was stopped.
08:48:36.389698 9718 BSC_Tests.ttcn:3184 Port RSL_CCHAN[1] was stopped.
08:48:36.390011 9718 BSC_Tests.ttcn:3184 Port RSL_CCHAN[2] was stopped.
08:48:36.390155 9718 BSC_Tests.ttcn:3184 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(9):IPA_RSL_PORT.
08:48:36.390401 9755 - Connection of port IPA_RSL_PORT to mtc:IPA_RSL[0][0] was closed unexpectedly by the peer.
08:48:36.390582 9718 BSC_Tests.ttcn:3184 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
08:48:36.390665 9755 - Port IPA_RSL_PORT was disconnected from mtc:IPA_RSL[0][0].
08:48:36.390789 9718 BSC_Tests.ttcn:3184 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
08:48:36.390966 9718 BSC_Tests.ttcn:3184 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
08:48:36.391452 9718 BSC_Tests.ttcn:3184 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
08:48:36.391665 9718 BSC_Tests.ttcn:3184 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
08:48:36.391818 9718 BSC_Tests.ttcn:3184 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
08:48:36.392079 9718 BSC_Tests.ttcn:3184 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
08:48:36.392496 9718 BSC_Tests.ttcn:3184 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
08:48:36.392845 9718 BSC_Tests.ttcn:3184 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
08:48:36.393013 9718 BSC_Tests.ttcn:3184 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
08:48:36.393338 9718 BSC_Tests.ttcn:3184 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
08:48:36.393536 9718 BSC_Tests.ttcn:3184 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
08:48:36.393888 9718 BSC_Tests.ttcn:3184 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
08:48:36.394086 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[0][0] was stopped.
08:48:36.394218 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[0][1] was stopped.
08:48:36.394335 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[0][2] was stopped.
08:48:36.394446 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[0][3] was stopped.
08:48:36.394565 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[1][0] was stopped.
08:48:36.394680 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[1][1] was stopped.
08:48:36.394915 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[1][2] was stopped.
08:48:36.395208 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[1][3] was stopped.
08:48:36.395470 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[2][0] was stopped.
08:48:36.395780 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[2][1] was stopped.
08:48:36.395961 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[2][2] was stopped.
08:48:36.396080 9718 BSC_Tests.ttcn:3184 Port IPA_RSL[2][3] was stopped.
08:48:36.396207 9718 BSC_Tests.ttcn:3184 Port IPA was stopped.
08:48:36.396394 9718 BSC_Tests.ttcn:3184 Port SCCPLITE_IPA_CTRL was stopped.
08:48:36.396714 9718 BSC_Tests.ttcn:3184 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(9):CFG_PORT.
08:48:36.397016 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[0][0] was stopped.
08:48:36.397061 9755 - Connection of port CFG_PORT to mtc:IPA_CFG_PORT[0][0] was closed unexpectedly by the peer.
08:48:36.397282 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[0][1] was stopped.
08:48:36.397435 9755 - Port CFG_PORT was disconnected from mtc:IPA_CFG_PORT[0][0].
08:48:36.397514 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[0][2] was stopped.
08:48:36.397683 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[0][3] was stopped.
08:48:36.397797 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[1][0] was stopped.
08:48:36.397992 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[1][1] was stopped.
08:48:36.398174 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[1][2] was stopped.
08:48:36.398285 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[1][3] was stopped.
08:48:36.398504 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[2][0] was stopped.
08:48:36.398760 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[2][1] was stopped.
08:48:36.399073 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[2][2] was stopped.
08:48:36.399334 9718 BSC_Tests.ttcn:3184 Port IPA_CFG_PORT[2][3] was stopped.
08:48:36.399491 9718 BSC_Tests.ttcn:3184 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
08:48:36.399919 9718 BSC_Tests.ttcn:3184 Port BSCVTY was unmapped from system:BSCVTY.
08:48:36.400082 9718 BSC_Tests.ttcn:3184 Port BSCVTY was stopped.
08:48:36.400484 9718 BSC_Tests.ttcn:3184 Port STPVTY was stopped.
08:48:36.400776 9718 BSC_Tests.ttcn:3184 Removing unterminated connection between port SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(5):CFG_PORT.
08:48:36.401048 9718 BSC_Tests.ttcn:3184 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
08:48:36.401200 9749 - Connection of port CFG_PORT to mtc:SCCPLITE_IPA_CFG_PORT[0] was closed unexpectedly by the peer.
08:48:36.401451 9718 BSC_Tests.ttcn:3184 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
08:48:36.401555 9749 - Port CFG_PORT was disconnected from mtc:SCCPLITE_IPA_CFG_PORT[0].
08:48:36.401577 9718 BSC_Tests.ttcn:3184 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
08:48:36.401663 9718 BSC_Tests.ttcn:3184 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(4):SCCP_SP_PORT.
08:48:36.401912 9718 BSC_Tests.ttcn:3184 Port BSSAP was stopped.
08:48:36.402096 9748 - Connection of port SCCP_SP_PORT to mtc:BSSAP was closed unexpectedly by the peer.
08:48:36.402268 9718 BSC_Tests.ttcn:3184 Port BSSAP_LE was stopped.
08:48:36.402399 9718 BSC_Tests.ttcn:3184 Component type BSC_Tests.test_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.402445 9748 - Port SCCP_SP_PORT was disconnected from mtc:BSSAP.
08:48:36.403319 9718 BSC_Tests.ttcn:3184 Waiting for PTCs to finish.
08:48:36.403790 9748 - Kill was requested from MC. Terminating idle PTC.
08:48:36.403816 9750 - Kill was requested from MC. Terminating idle PTC.
08:48:36.403821 9749 - Kill was requested from MC. Terminating idle PTC.
08:48:36.403840 9753 - Kill was requested from MC. Terminating idle PTC.
08:48:36.403846 9755 - Kill was requested from MC. Terminating idle PTC.
08:48:36.403979 9750 - Terminating component type IPA_Emulation.IPA_EventWaiter_CT.
08:48:36.403982 9748 - Terminating component type SCCP_Emulation.SCCP_CT.
08:48:36.404064 9749 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:36.404081 9755 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:36.404162 9753 - Terminating component type MGCP_Emulation.MGCP_Emulation_CT.
08:48:36.404204 9755 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:36.404215 9750 - Port IPA_SP_PORT was stopped.
08:48:36.404248 9748 - Port SCCP_SP_PORT was stopped.
08:48:36.404322 9753 - Removing unterminated mapping between port MGCP and system:MGCP_CODEC_PT.
08:48:36.404338 9749 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:36.404350 9750 - Component type IPA_Emulation.IPA_EventWaiter_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.404479 9748 - Removing unterminated connection between port MTP3_SCCP_PORT and VirtMSC-IPA(5):MTP3_SP_PORT.
08:48:36.404530 9750 - Final verdict of PTC: pass
08:48:36.404812 9748 - Port MTP3_SCCP_PORT was stopped.
08:48:36.405169 9750 - Disconnected from MC.
08:48:36.405565 9750 - TTCN-3 Parallel Test Component finished.
08:48:36.405620 9755 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:36.405701 9748 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.405779 9755 - Port IPA_PORT was stopped.
08:48:36.405846 9755 - Port CFG_PORT was stopped.
08:48:36.405907 9748 - Final verdict of PTC: none
08:48:36.406055 9755 - Port MTP3_SP_PORT was stopped.
08:48:36.406161 9755 - Port IPA_MGCP_PORT was stopped.
08:48:36.406299 9755 - Port IPA_RSL_PORT was stopped.
08:48:36.406329 9748 - Disconnected from MC.
08:48:36.406444 9755 - Port IPA_OML_PORT was stopped.
08:48:36.406678 9749 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:36.406704 9748 - TTCN-3 Parallel Test Component finished.
08:48:36.406812 9753 - Port MGCP was unmapped from system:MGCP_CODEC_PT.
08:48:36.406899 9749 - Port IPA_PORT was stopped.
08:48:36.407012 9749 - Port CFG_PORT was stopped.
08:48:36.407025 9753 - Port MGCP was stopped.
08:48:36.407196 9755 - Port IPA_CTRL_PORT was stopped.
08:48:36.407246 9749 - Removing unterminated connection between port MTP3_SP_PORT and VirtMSC-SCCP(4):MTP3_SCCP_PORT.
08:48:36.407622 9755 - Port IPA_SP_PORT was stopped.
08:48:36.407696 9749 - Port MTP3_SP_PORT was stopped.
08:48:36.407768 9755 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.407888 9749 - Port IPA_MGCP_PORT was stopped.
08:48:36.407923 9753 - Port MGCP_CLIENT was stopped.
08:48:36.408153 9749 - Port IPA_RSL_PORT was stopped.
08:48:36.408309 9753 - Port MGCP_CLIENT_MULTI was stopped.
08:48:36.408426 9749 - Port IPA_OML_PORT was stopped.
08:48:36.408452 9755 - Final verdict of PTC: none
08:48:36.408611 9753 - Port MGCP_PROC was stopped.
08:48:36.408620 9749 - Port IPA_CTRL_PORT was stopped.
08:48:36.408873 9753 - Component type MGCP_Emulation.MGCP_Emulation_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.408941 9749 - Port IPA_SP_PORT was stopped.
08:48:36.408998 9755 - Disconnected from MC.
08:48:36.409124 9755 - TTCN-3 Parallel Test Component finished.
08:48:36.409141 9753 - Final verdict of PTC: none
08:48:36.409187 9749 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc_connection_status.
08:48:36.409346 9749 - Final verdict of PTC: none
08:48:36.409425 9753 - Disconnected from MC.
08:48:36.409539 9753 - TTCN-3 Parallel Test Component finished.
08:48:36.409728 9749 - Disconnected from MC.
08:48:36.409778 9718 BSC_Tests.ttcn:3184 Setting final verdict of the test case.
08:48:36.409829 9749 - TTCN-3 Parallel Test Component finished.
08:48:36.410118 9718 BSC_Tests.ttcn:3184 Local verdict of MTC: pass
08:48:36.410329 9718 BSC_Tests.ttcn:3184 Local verdict of PTC VirtMSC-STATS(3): none (pass -> pass)
08:48:36.410633 9718 BSC_Tests.ttcn:3184 Local verdict of PTC VirtMSC-SCCP(4): none (pass -> pass)
08:48:36.410958 9718 BSC_Tests.ttcn:3184 Local verdict of PTC VirtMSC-IPA(5): none (pass -> pass)
08:48:36.411118 9718 BSC_Tests.ttcn:3184 Local verdict of PTC VirtMSC-IPA-WAIT(6): pass (pass -> pass)
08:48:36.411261 9718 BSC_Tests.ttcn:3184 Local verdict of PTC IPA-CTRL-CLI-IPA(7): none (pass -> pass)
08:48:36.411463 9718 BSC_Tests.ttcn:3184 Local verdict of PTC VirtMGW-MGCP-0(8): none (pass -> pass)
08:48:36.411611 9718 BSC_Tests.ttcn:3184 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(9): none (pass -> pass)
08:48:36.411757 9718 BSC_Tests.ttcn:3184 Test case TC_ctrl_msc_connection_status finished. Verdict: pass
08:48:36.411898 9718 BSC_Tests.ttcn:3184 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc_connection_status pass'.
08:48:41.540916 9718 BSC_Tests.ttcn:3184 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc_connection_status pass' was executed successfully (exit status: 0).
08:48:41.540989 9718 BSC_Tests.ttcn:3187 Switching to log file `BSC_Tests-TC_ctrl_msc0_connection_status-cbea39017248-mtc-9718.log'
