(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "icE1usb")
    (date "2020-09-05")
    (rev "1.1")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.075)
    (pcbplotparams
      (layerselection 0x00210fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plot/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad4)")
  (net 5 "/e1A/rx_bias_p")
  (net 6 "/e1A/rx_bias_n")
  (net 7 "Net-(J4-Pad2)")
  (net 8 "Net-(J5-Pad6)")
  (net 9 "Net-(J5-Pad2)")
  (net 10 "Net-(J5-Pad7)")
  (net 11 "Net-(J5-Pad3)")
  (net 12 "/e1A/rx_hi_p")
  (net 13 "/e1A/rx_hi_n")
  (net 14 "/e1A/rx_lo_p")
  (net 15 "/e1A/rx_lo_n")
  (net 16 "Net-(R3-Pad2)")
  (net 17 "Net-(R2-Pad2)")
  (net 18 "/e1A_rj1")
  (net 19 "/e1B_rj1")
  (net 20 "Net-(C1-Pad2)")
  (net 21 "+3V3")
  (net 22 "Net-(C5-Pad1)")
  (net 23 "+1V2")
  (net 24 "/gps/RF")
  (net 25 "/e1B_rj7")
  (net 26 "/e1B_rj6")
  (net 27 "/e1B_rj5")
  (net 28 "/e1B_rj4")
  (net 29 "/e1B_rj8")
  (net 30 "/e1B_rj2")
  (net 31 "/e1B_rj3")
  (net 32 "/e1_led2")
  (net 33 "/e1_led0")
  (net 34 "/e1_led1")
  (net 35 "/e1A_rj8")
  (net 36 "/e1A_rj6")
  (net 37 "/e1A_rj4")
  (net 38 "/e1A_rj2")
  (net 39 "/e1A_rj7")
  (net 40 "/e1A_rj5")
  (net 41 "/e1A_rj3")
  (net 42 "+5V")
  (net 43 "Net-(F1-Pad2)")
  (net 44 "Net-(F2-Pad2)")
  (net 45 "Net-(F3-Pad2)")
  (net 46 "Net-(F4-Pad2)")
  (net 47 "Net-(F5-Pad2)")
  (net 48 "Net-(F6-Pad2)")
  (net 49 "Net-(F7-Pad2)")
  (net 50 "Net-(F8-Pad2)")
  (net 51 "/fpga/flash_mosi")
  (net 52 "/fpga/flash_miso")
  (net 53 "/fpga/~{creset}")
  (net 54 "/fpga/cdone")
  (net 55 "/fpga/~{flash_cs}")
  (net 56 "/fpga/~{boot_sw}")
  (net 57 "/fpga/flash_sck")
  (net 58 "/e1bias/bias_1")
  (net 59 "/usb_dn")
  (net 60 "/usb_dp")
  (net 61 "/dbg_rx")
  (net 62 "/dbg_tx")
  (net 63 "Net-(J4-Pad7)")
  (net 64 "Net-(J4-Pad6)")
  (net 65 "Net-(J4-Pad3)")
  (net 66 "/fpga/clk_tune_lo")
  (net 67 "/fpga/clk_tune_hi")
  (net 68 "Net-(RN1-Pad4)")
  (net 69 "Net-(RN1-Pad2)")
  (net 70 "Net-(RN1-Pad3)")
  (net 71 "Net-(RN1-Pad1)")
  (net 72 "/fpga/clk_30m72")
  (net 73 "Net-(C17-Pad1)")
  (net 74 "Net-(C10-Pad1)")
  (net 75 "Net-(J1-Pad8)")
  (net 76 "Net-(J1-Pad7)")
  (net 77 "Net-(J1-Pad6)")
  (net 78 "Net-(J1-Pad5)")
  (net 79 "Net-(J1-Pad4)")
  (net 80 "Net-(J1-Pad3)")
  (net 81 "Net-(J1-Pad2)")
  (net 82 "Net-(J1-Pad1)")
  (net 83 "Net-(RN2-Pad4)")
  (net 84 "Net-(RN2-Pad2)")
  (net 85 "Net-(RN2-Pad3)")
  (net 86 "Net-(RN2-Pad1)")
  (net 87 "/e1B/rx_hi_p")
  (net 88 "/e1B/rx_hi_n")
  (net 89 "/e1B/rx_lo_p")
  (net 90 "/e1B/rx_lo_n")
  (net 91 "/e1A/tx_hi")
  (net 92 "/e1A/tx_lo")
  (net 93 "/e1B/tx_hi")
  (net 94 "/e1B/tx_lo")
  (net 95 "unconnected-(TR1-Pad7)")
  (net 96 "unconnected-(TR1-Pad10)")
  (net 97 "unconnected-(TR1-Pad15)")
  (net 98 "unconnected-(TR2-Pad7)")
  (net 99 "/fpga/i2c_scl")
  (net 100 "/gpio2")
  (net 101 "/fpga/i2c_sda")
  (net 102 "/gpio1")
  (net 103 "/gpio0")
  (net 104 "unconnected-(TR2-Pad10)")
  (net 105 "unconnected-(TR2-Pad15)")
  (net 106 "unconnected-(U3-Pad9)")
  (net 107 "unconnected-(U7-Pad2)")
  (net 108 "/fpga/~{gps_reset}")
  (net 109 "/fpga/gps_pps")
  (net 110 "/fpga/gps_tx")
  (net 111 "/fpga/gps_rx")
  (net 112 "/fpga/usb_pu_i")
  (net 113 "/fpga/usb_dp_i")
  (net 114 "/e1_led3")
  (net 115 "/e1_led7")
  (net 116 "/e1_led6")
  (net 117 "/e1_led4")
  (net 118 "/e1_led5")
  (net 119 "/fpga/usb_dn_i")
  (net 120 "/fpga/dbg_rx_i")
  (net 121 "/fpga/dbg_tx_i")
  (net 122 "/fpga/e1_led_rclk")
  (net 123 "/gps/vbackup")
  (net 124 "Net-(D4-Pad1)")
  (net 125 "Net-(L1-Pad1)")
  (net 126 "Net-(C11-Pad1)")
  (net 127 "Net-(C16-Pad1)")
  (net 128 "Net-(C20-Pad1)")
  (net 129 "Net-(C21-Pad2)")
  (net 130 "/e1bias/bias_fixed")
  (net 131 "/e1bias/bias_0")
  (net 132 "Net-(C35-Pad1)")
  (net 133 "Net-(C36-Pad1)")
  (net 134 "Net-(C39-Pad1)")
  (net 135 "Net-(R16-Pad1)")
  (net 136 "Net-(R27-Pad1)")
  (net 137 "/e1bias/bias1")
  (net 138 "/e1bias/bias0")
  (net 139 "unconnected-(U7-Pad5)")
  (net 140 "unconnected-(U8-Pad5)")
  (net 141 "unconnected-(U8-Pad13)")
  (net 142 "unconnected-(U8-Pad18)")
  (net 143 "unconnected-(U9-Pad4)")
  (net 144 "unconnected-(U10-Pad4)")
  (net 145 "unconnected-(U12-Pad2)")
  (net 146 "unconnected-(U12-Pad5)")
  (net 147 "unconnected-(X4-PadA8)")
  (net 148 "unconnected-(X4-PadB8)")
  (net 149 "Net-(R12-Pad2)")
  (net 150 "Net-(R17-Pad1)")
  (net 151 "Net-(R28-Pad1)")
  (net 152 "Net-(RN6-Pad4)")
  (net 153 "Net-(RN6-Pad2)")
  (net 154 "Net-(RN6-Pad3)")
  (net 155 "Net-(RN6-Pad1)")
  (net 156 "Net-(U8-Pad16)")
  (net 157 "Net-(U8-Pad17)")
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at -13 13 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "MPN" "W25Q80DVSNIG")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "U5" (at 0 -3.4) (layer "F.SilkS") hide)
    (fp_text value "W25Q80" (at 0 -1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/fpga/~{flash_cs}") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/fpga/flash_miso") (pinfunction "SIO1/SO") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "SIO2/~{W}") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/fpga/flash_mosi") (pinfunction "SIO0/SI") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/fpga/flash_sck") (pinfunction "SCK") (pintype "input"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "SIO3/~{HOLD}") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "s47-device:LED_RGB_2020" (layer "F.Cu")
    (tedit 5F149206)
    (at -22.75 0 180)
    (descr "LED Tri SMD 2020, reflow soldering")
    (tags "tri led 2020")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "D1" (at 0 0) (layer "F.Fab"))
    (fp_text value "STATUS" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.95 -0.55 180) (size 0.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)") (pinfunction "RK") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 -0.55 180) (size 0.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)") (pinfunction "BK") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.95 0.55 180) (size 0.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A") (pintype "passive"))
    (pad "4" smd roundrect locked (at -0.95 0.55 180) (size 0.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad4)") (pinfunction "GK") (pintype "passive"))
    (model "${KIUSR3DMOD}/FOSHAN-FM-B2020RGBA-HG.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "s47-misc:LUMEX_LPF-C011303S" (layer "F.Cu")
    (tedit 5F148CB8)
    (at -22.75 0 -90)
    (descr "https://www.lumex.com/spec/LPF-C011303S.pdf")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr through_hole)
    (fp_text reference "LP1" (at 0 -4 90) (layer "F.SilkS") hide)
    (fp_text value "LightPipe" (at 3 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 0) (layer "F.Fab"))
    (pad "" np_thru_hole oval locked (at 3.575 0 270) (size 2 3) (drill oval 2 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval locked (at -3.575 0 270) (size 2 3) (drill oval 2 3) (layers *.Cu *.Mask))
    (model "${KIUSR3DMOD}/Lumex_LPF-C011303S.step"
      (offset (xyz 0 -2.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "s47-misc:SW_HYP_1TS003B" locked (layer "F.Cu")
    (tedit 5F149781)
    (at 41 20.5 -90)
    (descr "HYP (Hongyuan Precision) 1TS003B switches https://datasheet.lcsc.com/szlcsc/HYP-1TS003B-2600-3500A_C319399.pdf")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "SW1" (at 0 2.75 90) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0.87 0 270) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.85 0 270) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "1" smd rect locked (at -1.7 1.4 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 1.7 1.4 270) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/fpga/~{boot_sw}") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect locked (at 2.3 -0.6 270) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect locked (at -2.3 -0.6 270) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KIUSR3DMOD}/1TS003B.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "s47-misc:PULSE_BH" locked (layer "F.Cu")
    (tedit 5F1316D6)
    (at 17.5 -11.25 90)
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "TR1" (at 0 -8 90) (layer "F.SilkS") hide)
    (fp_text value "PULSE_T1094NL" (at 0 1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.165 -4.445 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at -4.165 -3.175 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "3" smd roundrect locked (at -4.165 -1.905 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "4" smd roundrect locked (at -4.165 -0.635 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "5" smd roundrect locked (at -4.165 0.635 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "6" smd roundrect locked (at -4.165 1.905 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "Net-(R16-Pad1)") (pintype "passive"))
    (pad "7" smd roundrect locked (at -4.165 3.175 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "unconnected-(TR1-Pad7)") (pintype "passive+no_connect"))
    (pad "8" smd roundrect locked (at -4.165 4.445 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(R17-Pad1)") (pintype "passive"))
    (pad "9" smd roundrect locked (at 4.165 4.445 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J4-Pad7)") (pintype "passive"))
    (pad "10" smd roundrect locked (at 4.165 3.175 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "unconnected-(TR1-Pad10)") (pintype "passive+no_connect"))
    (pad "11" smd roundrect locked (at 4.165 1.905 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(J4-Pad3)") (pintype "passive"))
    (pad "12" smd roundrect locked (at 4.165 0.635 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "13" smd roundrect locked (at 4.165 -0.635 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect locked (at 4.165 -1.905 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(J4-Pad6)") (pintype "passive"))
    (pad "15" smd roundrect locked (at 4.165 -3.175 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "unconnected-(TR1-Pad15)") (pintype "passive+no_connect"))
    (pad "16" smd roundrect locked (at 4.165 -4.445 90) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J4-Pad2)") (pintype "passive"))
    (model "${KIUSR3DMOD}/PULSE_BH1.step"
      (offset (xyz 0 0 6.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "s47-misc:Oscillator_SMD_VCXO-6Pin_7.0x5.0mm_P2.54mm" (layer "F.Cu")
    (tedit 5F259630)
    (at -5 -11 90)
    (descr "SMD Crystal Oscillator IDT https://www.idt.com/document/dst/xu-family-datasheet#page=17, 7.0x5.0mm")
    (tags "SMD SMT crystal oscillator")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "U4" (at 0 -4.63 90) (layer "F.SilkS") hide)
    (fp_text value "30M72" (at -0.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.1 -2.54) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(C11-Pad1)") (pinfunction "Vctrl") (pintype "input"))
    (pad "2" smd rect locked (at -2.1 0) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "OE") (pintype "input"))
    (pad "3" smd rect locked (at -2.1 2.54) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect locked (at 2.1 2.54) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(R12-Pad2)") (pinfunction "OUT") (pintype "output"))
    (pad "5" smd rect locked (at 2.1 0) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect locked (at 2.1 -2.54) (size 1.8 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "Vcc") (pintype "power_in"))
    (model "${KIUSR3DMOD}/Oscillator_SMD_VCXO-6Pin_7.0x5.0mm_P2.54mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "s47-misc:ublox_MAX" (layer "F.Cu")
    (tedit 5E9E8EA6)
    (at -21.75 -17.25 180)
    (descr "ublox MAX 6/7/8, (https://www.u-blox.com/sites/default/files/MAX-8-M8-FW3_HardwareIntegrationManual_%28UBX-15030059%29.pdf)")
    (tags "GPS ublox MAX 6/7/8")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "U8" (at 0 -6) (layer "F.SilkS") hide)
    (fp_text value "MAX-M8W" (at 0 1.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.75 -4.4 180) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -4.75 -3.3 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "Net-(RN6-Pad2)") (pinfunction "TXD") (pintype "output"))
    (pad "3" smd roundrect locked (at -4.75 -2.2 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(RN6-Pad1)") (pinfunction "RXD") (pintype "input"))
    (pad "4" smd roundrect locked (at -4.75 -1.1 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/fpga/gps_pps") (pinfunction "TIMEPULSE") (pintype "output"))
    (pad "5" smd roundrect locked (at -4.75 0 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "unconnected-(U8-Pad5)") (pinfunction "EXTINT") (pintype "input+no_connect"))
    (pad "6" smd roundrect locked (at -4.75 1.1 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "/gps/vbackup") (pinfunction "V_BCKP") (pintype "power_in"))
    (pad "7" smd roundrect locked (at -4.75 2.2 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VCC_IO") (pintype "power_in"))
    (pad "8" smd roundrect locked (at -4.75 3.3 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd roundrect locked (at -4.75 4.4 180) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "/fpga/~{gps_reset}") (pinfunction "~{RESET}") (pintype "input"))
    (pad "10" smd roundrect locked (at 4.75 4.4 180) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "11" smd roundrect locked (at 4.75 3.3 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/gps/RF") (pinfunction "RF_IN") (pintype "input"))
    (pad "12" smd roundrect locked (at 4.75 2.2 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "13" smd roundrect locked (at 4.75 1.1 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "unconnected-(U8-Pad13)") (pinfunction "Reserved") (pintype "no_connect"))
    (pad "14" smd roundrect locked (at 4.75 0 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(L1-Pad1)") (pinfunction "VCC_RF") (pintype "power_out"))
    (pad "15" smd roundrect locked (at 4.75 -1.1 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(C21-Pad2)") (pinfunction "V_ANT") (pintype "power_in"))
    (pad "16" smd roundrect locked (at 4.75 -2.2 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 156 "Net-(U8-Pad16)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at 4.75 -3.3 180) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 157 "Net-(U8-Pad17)") (pinfunction "SCL") (pintype "input"))
    (pad "18" smd roundrect locked (at 4.75 -4.4 180) (size 1.8 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "unconnected-(U8-Pad18)") (pinfunction "~{SAFEBOOT}") (pintype "input+no_connect"))
    (model "${KIUSR3DMOD}/ublox-MAX-M8.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "s47-misc:PULSE_BH" locked (layer "F.Cu")
    (tedit 5F1316D6)
    (at 17.5 11.25 -90)
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "TR2" (at 0 -8 90) (layer "F.SilkS") hide)
    (fp_text value "PULSE_T1094NL" (at 0 -1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.165 -4.445 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at -4.165 -3.175 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)") (pintype "passive"))
    (pad "3" smd roundrect locked (at -4.165 -1.905 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)") (pintype "passive"))
    (pad "4" smd roundrect locked (at -4.165 -0.635 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "5" smd roundrect locked (at -4.165 0.635 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "6" smd roundrect locked (at -4.165 1.905 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "7" smd roundrect locked (at -4.165 3.175 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "unconnected-(TR2-Pad7)") (pintype "passive+no_connect"))
    (pad "8" smd roundrect locked (at -4.165 4.445 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(R28-Pad1)") (pintype "passive"))
    (pad "9" smd roundrect locked (at 4.165 4.445 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J5-Pad7)") (pintype "passive"))
    (pad "10" smd roundrect locked (at 4.165 3.175 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "unconnected-(TR2-Pad10)") (pintype "passive+no_connect"))
    (pad "11" smd roundrect locked (at 4.165 1.905 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J5-Pad3)") (pintype "passive"))
    (pad "12" smd roundrect locked (at 4.165 0.635 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "13" smd roundrect locked (at 4.165 -0.635 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect locked (at 4.165 -1.905 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J5-Pad6)") (pintype "passive"))
    (pad "15" smd roundrect locked (at 4.165 -3.175 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "unconnected-(TR2-Pad15)") (pintype "passive+no_connect"))
    (pad "16" smd roundrect locked (at 4.165 -4.445 270) (size 1.9 0.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J5-Pad2)") (pintype "passive"))
    (model "${KIUSR3DMOD}/PULSE_BH1.step"
      (offset (xyz 0 0 6.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -31.75 2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -17.75 -2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -4.25 -2.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 -0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -4.25 4.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 0 -0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -4.25 1.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -4.25 0.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 -0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+1V2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -16 16.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at 13.69 -19.23 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr through_hole)
    (fp_text reference "J4" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "NT/TE" (at 0.52 3.81 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.02 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(F2-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J4-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(F4-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(F1-Pad2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J4-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J4-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(F3-Pad2)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -31.75 4.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "91k" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -31.75 -4.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -31.75 1.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 1.5 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -4.25 6.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "120R" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+1V2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at -28.25 -1.5 -90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.45 90) (layer "F.SilkS") hide)
    (fp_text value "IP4220CZ6" (at -1.25 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.16 -0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "/fpga/dbg_tx_i") (pintype "passive"))
    (pad "2" smd rect locked (at -1.16 0 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "3" smd rect locked (at -1.16 0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/fpga/dbg_rx_i") (pintype "passive"))
    (pad "4" smd rect locked (at 1.16 0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/fpga/usb_dp_i") (pintype "passive"))
    (pad "5" smd rect locked (at 1.16 0 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "+5V") (pintype "passive"))
    (pad "6" smd rect locked (at 1.16 -0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "/fpga/usb_dn_i") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 14.325 -3.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "U6" (at 0 -2.45 90) (layer "F.SilkS") hide)
    (fp_text value "IP4220CZ6" (at -1.25 0.175 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(R17-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at -1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "3" smd rect locked (at -1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "Net-(R16-Pad1)") (pintype "passive"))
    (pad "4" smd rect locked (at 1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "5" smd rect locked (at 1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (pad "6" smd rect locked (at 1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(C16-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 26 -20.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "U7" (at 0 -2.45 90) (layer "F.SilkS") hide)
    (fp_text value "IP4220CZ6" (at 1.25 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(F3-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at -1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "unconnected-(U7-Pad2)") (pintype "passive+no_connect"))
    (pad "3" smd rect locked (at -1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(F4-Pad2)") (pintype "passive"))
    (pad "4" smd rect locked (at 1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(F2-Pad2)") (pintype "passive"))
    (pad "5" smd rect locked (at 1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "unconnected-(U7-Pad5)") (pintype "passive+no_connect"))
    (pad "6" smd rect locked (at 1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(F1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at -12.32 21.35 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "SPI" (at 0.35 3.82 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.1 3.82) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "/fpga/~{flash_cs}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "/fpga/cdone") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "/fpga/flash_sck") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/fpga/~{creset}") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/fpga/flash_miso") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "+3V3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/fpga/flash_mosi") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -7.25 -15.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -10.5 -11.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1u" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -10.5 -8.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -25.5 7.25 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "psu")
    (attr smd)
    (fp_text reference "C29" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 0 -0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -20 7.25 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "psu")
    (attr smd)
    (fp_text reference "C30" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 0 -0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+1V2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 -21.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "F2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/e1A_rj2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(F2-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 -19.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "F3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/e1A_rj4") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(F3-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 -18.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "F4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/e1A_rj5") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(F4-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 18.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "F5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/e1B_rj1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(F5-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 19.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "F6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/e1B_rj2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(F6-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 21.25 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "F7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/e1B_rj4") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(F7-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 22.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "F8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/e1B_rj5") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(F8-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5A02FF57)
    (at -22.75 7.25)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "psu")
    (attr smd)
    (fp_text reference "U9" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MIC5504-1.2YM5" (at 1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "+5V") (pinfunction "EN") (pintype "input"))
    (pad "4" smd rect locked (at 1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "unconnected-(U9-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect locked (at 1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "+1V2") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -16 22)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "DONE" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/fpga/cdone") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at -22.48 18.81 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33) (layer "F.SilkS") hide)
    (fp_text value "EXT_OUT" (at 0.52 3.81 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.02 3.81 270) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -29.25 2 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1k5" (at 0 -0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "/fpga/usb_dp_i") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/fpga/usb_pu_i") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -10.5 -13 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "91k" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/fpga/clk_tune_lo") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -10.5 -10 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1k5" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 10.5 -1.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "27R" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(R17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "/e1A/tx_lo") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 10.5 5.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "27R" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(R28-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "/e1B/tx_lo") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 10.5 4.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "R27" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "27R" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "/e1B/tx_hi") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at -16 19.25 180)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "RN4" (at 0 -2.8) (layer "F.SilkS") hide)
    (fp_text value "10k" (at -1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/fpga/~{creset}") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/fpga/cdone") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/fpga/cdone") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/fpga/~{flash_cs}") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "R1.2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at 8 18.81 180)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -2.33) (layer "F.SilkS") hide)
    (fp_text value "EXT_IN" (at 0.5 3.81 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "/fpga/i2c_scl") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "/gpio2") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "/fpga/i2c_sda") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "/gpio1") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "+3V3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "/gpio0") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at -31.75 -1.5)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "RN3" (at 0 -2.8) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -1.25 -0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/dbg_rx") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/dbg_tx") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/usb_dn") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/usb_dp") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/fpga/usb_dp_i") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "/fpga/usb_dn_i") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "/fpga/dbg_tx_i") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "/fpga/dbg_rx_i") (pinfunction "R1.2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "s47-conn:SMA_TEConnectivity_619540-1_Horizontal" locked (layer "F.Cu")
    (tedit 5F259B65)
    (at -36 -20 90)
    (descr "https://www.amphenolrf.com/media/downloads/1769/132203-12.pdf")
    (tags "SMA THT Female Jack Horizontal")
    (property "MPN" "TEConnectivity 619540-1")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X1" (at -5.2 0) (layer "F.SilkS") hide)
    (fp_text value "GPS" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.25 2.25) (drill 1.5) (layers *.Cu *.Mask)
      (net 24 "/gps/RF") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 -2.54 90) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 2.54 90) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 -2.54 90) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 2.54 180) (size 2.5 2.5) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KIUSR3DMOD}/SMA_TEConnectivity_619540-1.step"
      (offset (xyz 0 15.8 6.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "s47-conn:USB_C_Receptacle_HRO_TYPE-C-31-M-12" locked (layer "F.Cu")
    (tedit 5F148CC8)
    (at -40.35 0 -90)
    (descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
    (tags "usb usb-c 2.0 pd")
    (property "MPN" "HRO_TYPE-C-31-M-12")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "X4" (at 0 -5.645 90) (layer "F.SilkS") hide)
    (fp_text value "USB" (at 2.5 0.15 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.5 0 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 2.89 -2.6 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -2.89 -2.6 270) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "A1" smd roundrect locked (at -3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd roundrect locked (at -2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 42 "+5V") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd roundrect locked (at -1.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(R2-Pad2)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd roundrect locked (at -0.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/usb_dp") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd roundrect locked (at 0.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/usb_dn") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd roundrect locked (at 1.25 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 147 "unconnected-(X4-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "A9" smd roundrect locked (at 2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 42 "+5V") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd roundrect locked (at 3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd roundrect locked (at 3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd roundrect locked (at 2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 42 "+5V") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd roundrect locked (at 1.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(R3-Pad2)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd roundrect locked (at 0.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/usb_dp") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd roundrect locked (at -0.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/usb_dn") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd roundrect locked (at -1.75 -4.045 270) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "unconnected-(X4-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "B9" smd roundrect locked (at -2.45 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 42 "+5V") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd roundrect locked (at -3.25 -4.045 270) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval locked (at -4.32 -3.13 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval locked (at -4.32 1.05 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval locked (at 4.32 1.05 270) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval locked (at 4.32 -3.13 270) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 20 "Net-(C1-Pad2)") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KIUSR3DMOD}/HRO_TYPE-C-31-M-12.step"
      (offset (xyz -4.465 -3.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ45_Amphenol_RJHSE5380" locked (layer "F.Cu")
    (tedit 5AD365F7)
    (at -36.5 18.57 90)
    (descr "Shielded, https://www.amphenolcanada.com/ProductSearch/drawings/AC/RJHSE538X.pdf")
    (tags "RJ45 8p8c ethernet cat5")
    (property "MPN" "Amphenol RJHSE5080")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X3" (at 3.56 -9.5 90) (layer "F.SilkS") hide)
    (fp_text value "GPIO" (at 3.57 -1.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.57 -4 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -2.79 -2.54 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 9.91 -2.54 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 82 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.02 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 81 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.04 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 80 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.06 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 79 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 4.08 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 78 "Net-(J1-Pad5)") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 5.1 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 77 "Net-(J1-Pad6)") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 6.12 0 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 76 "Net-(J1-Pad7)") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 7.14 1.78 90) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 75 "Net-(J1-Pad8)") (pintype "passive"))
    (pad "SH" thru_hole circle locked (at 11.69 0.89 90) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
    (pad "SH" thru_hole circle locked (at -4.57 0.89 90) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
    (model "${KIUSR3DMOD}/M-RJHSE-5080-REVT1.step"
      (offset (xyz 3.5 1.55 3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at 21.31 19.23 -90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr through_hole)
    (fp_text reference "J5" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "NT/TE" (at 2.02 3.81 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.52 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(F6-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(F8-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(F5-Pad2)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J5-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J5-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(F7-Pad2)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 11.25 2 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "R26" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "120R" (at 0 0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 5.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "C35" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/e1B/rx_hi_p") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 1.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "C38" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "Net-(C35-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/e1B/rx_lo_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "C37" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/e1B/rx_lo_p") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "C36" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(C36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/e1B/rx_hi_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 14.325 3.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "U11" (at 0 -2.45 90) (layer "F.SilkS") hide)
    (fp_text value "IP4220CZ6" (at 1.25 0.175 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(R28-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at -1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "3" smd rect locked (at -1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "4" smd rect locked (at 1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Net-(C36-Pad1)") (pintype "passive"))
    (pad "5" smd rect locked (at 1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (pad "6" smd rect locked (at 1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "Net-(C35-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 23.5 0 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.55) (layer "F.SilkS") hide)
    (fp_text value "74HC595" (at 0 -1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.95 -2.275 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/e1_led1") (pinfunction "QB") (pintype "tri_state"))
    (pad "2" smd rect locked (at -2.95 -1.625 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/e1_led2") (pinfunction "QC") (pintype "tri_state"))
    (pad "3" smd rect locked (at -2.95 -0.975 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/e1_led3") (pinfunction "QD") (pintype "tri_state"))
    (pad "4" smd rect locked (at -2.95 -0.325 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "/e1_led4") (pinfunction "QE") (pintype "tri_state"))
    (pad "5" smd rect locked (at -2.95 0.325 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "/e1_led5") (pinfunction "QF") (pintype "tri_state"))
    (pad "6" smd rect locked (at -2.95 0.975 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "/e1_led6") (pinfunction "QG") (pintype "tri_state"))
    (pad "7" smd rect locked (at -2.95 1.625 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "/e1_led7") (pinfunction "QH") (pintype "tri_state"))
    (pad "8" smd rect locked (at -2.95 2.275 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd rect locked (at 2.95 2.275 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "unconnected-(U3-Pad9)") (pinfunction "QH'") (pintype "output+no_connect"))
    (pad "10" smd rect locked (at 2.95 1.625 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/fpga/cdone") (pinfunction "~{SRCLR}") (pintype "input"))
    (pad "11" smd rect locked (at 2.95 0.975 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/fpga/flash_sck") (pinfunction "SRCLK") (pintype "input"))
    (pad "12" smd rect locked (at 2.95 0.325 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "/fpga/e1_led_rclk") (pinfunction "RCLK") (pintype "input"))
    (pad "13" smd rect locked (at 2.95 -0.325 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "~{OE}") (pintype "input"))
    (pad "14" smd rect locked (at 2.95 -0.975 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/fpga/flash_mosi") (pinfunction "SER") (pintype "input"))
    (pad "15" smd rect locked (at 2.95 -1.625 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/e1_led0") (pinfunction "QA") (pintype "tri_state"))
    (pad "16" smd rect locked (at 2.95 -2.275 180) (size 1.5 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at 26 -5 180)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RN1" (at 0 -2.8) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(RN1-Pad1)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(RN1-Pad2)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(RN1-Pad3)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(RN1-Pad4)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "/e1_led4") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "/e1_led5") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 116 "/e1_led6") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "/e1_led7") (pinfunction "R1.2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at 26 5 180)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RN2" (at 0 -2.8) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(RN2-Pad1)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(RN2-Pad2)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(RN2-Pad3)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(RN2-Pad4)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/e1_led1") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/e1_led2") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4 180) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/e1_led3") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2 180) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/e1_led0") (pinfunction "R1.2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ45_Amphenol_RJHSE538X-02" locked (layer "F.Cu")
    (tedit 5F32B9B7)
    (at 36.5 -11.435 -90)
    (descr "Shielded, 2 LED, 2 Ports, http://www.amphenolinfocom.eu/NavData/Drawings/RJHSE-538X-02-REVC.pdf")
    (tags "RJ45 8p8c dual ethernet cat5")
    (property "MPN" "AMPHENOL RJHSE508102")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X5" (at 11.43 -9.5 -90) (layer "F.SilkS") hide)
    (fp_text value "E1" (at 11.43 -1.5 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.435 -4 -90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -2.79 -2.54 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 25.66 -2.54 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 18 "/e1A_rj1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.016 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 38 "/e1A_rj2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.032 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 41 "/e1A_rj3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.048 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 37 "/e1A_rj4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 4.064 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 40 "/e1A_rj5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 5.08 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 36 "/e1A_rj6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 6.096 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 39 "/e1A_rj7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 7.112 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 35 "/e1A_rj8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at -3.3 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 68 "Net-(RN1-Pad4)") (pintype "passive"))
    (pad "10" thru_hole circle locked (at -1.01 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 70 "Net-(RN1-Pad3)") (pintype "passive"))
    (pad "11" thru_hole circle locked (at 8.13 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 69 "Net-(RN1-Pad2)") (pintype "passive"))
    (pad "12" thru_hole circle locked (at 10.42 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 71 "Net-(RN1-Pad1)") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 15.75 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 19 "/e1B_rj1") (pintype "passive"))
    (pad "14" thru_hole circle locked (at 16.766 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 30 "/e1B_rj2") (pintype "passive"))
    (pad "15" thru_hole circle locked (at 17.782 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 31 "/e1B_rj3") (pintype "passive"))
    (pad "16" thru_hole circle locked (at 18.798 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 28 "/e1B_rj4") (pintype "passive"))
    (pad "17" thru_hole circle locked (at 19.814 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 27 "/e1B_rj5") (pintype "passive"))
    (pad "18" thru_hole circle locked (at 20.83 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 26 "/e1B_rj6") (pintype "passive"))
    (pad "19" thru_hole circle locked (at 21.846 0 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 25 "/e1B_rj7") (pintype "passive"))
    (pad "20" thru_hole circle locked (at 22.862 1.78 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 29 "/e1B_rj8") (pintype "passive"))
    (pad "21" thru_hole circle locked (at 12.45 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 83 "Net-(RN2-Pad4)") (pintype "passive"))
    (pad "22" thru_hole circle locked (at 14.74 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 85 "Net-(RN2-Pad3)") (pintype "passive"))
    (pad "23" thru_hole circle locked (at 23.88 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 84 "Net-(RN2-Pad2)") (pintype "passive"))
    (pad "24" thru_hole circle locked (at 26.17 6.6 270) (size 1.5 1.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 86 "Net-(RN2-Pad1)") (pintype "passive"))
    (pad "SH" thru_hole circle locked (at -4.57 0.89 270) (size 2.3 2.3) (drill 1.57) (layers *.Cu *.Mask))
    (pad "SH" thru_hole circle locked (at 27.43 0.89 270) (size 2.3 2.3) (drill 1.57) (layers *.Cu *.Mask))
    (model "${KIUSR3DMOD}/M-RJHSE-X08X-02-REVT1.step"
      (offset (xyz 27.15 7.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 18.75 0 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Battery:Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles" (layer "F.Cu")
    (tedit 5C8577EF)
    (at -6.75 -19.25)
    (descr "Panasonic CR-1220/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D140.pdf")
    (tags "battery CR-1220 coin cell vertical")
    (property "DNP" "DNP")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr through_hole)
    (fp_text reference "BT1" (at 1.625 -4) (layer "F.SilkS") hide)
    (fp_text value "VL-1220/VCN" (at 1.625 -0.25) (layer "F.Fab") hide)
    (fp_text user "+" (at -1.46 -0.5) (layer "F.SilkS"))
    (fp_text user "DNP" (at 1.5 -1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.625 -1.2 180) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 1.09) (layers *.Cu *.Mask)
      (net 123 "/gps/vbackup") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 3.25 -2.45) (size 1.6 1.6) (drill 1.09) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KISYS3DMOD}/Battery.3dshapes/Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -30 -16.75 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DNP" "DNP")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "C21" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text user "DNP" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(C21-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -13.5 -20.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -13.5 -19)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "C23" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -13.5 -22)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1u" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -13.5 -17.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "C25" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "/gps/vbackup") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -30 -19.5 -90)
    (descr "Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "MPN" "Little Fuse PESD0402-140")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "PESD0402-140" (at -3 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/gps/RF") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "A2") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0402_1005Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -28.5 -19.5 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "MPN" "Murata LQW15AN47NG00D")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "L1" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "47n" (at 1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(L1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/gps/RF") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -28.5 -16.75 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DNP" "DNP")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10R" (at 0 0.75 90) (layer "F.Fab") hide)
    (fp_text user "DNP" (at 0 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(C21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(L1-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -7.5 -17.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DNP" "DNP")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330R" (at 1.75 0) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "DNP" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "/gps/vbackup") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 7.75 22.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "/fpga/i2c_sda") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 7.75 21.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "/fpga/i2c_scl") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -0.25 -11 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "27R" (at 0 0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/fpga/clk_30m72") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 -2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/e1A/rx_lo_p") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 -4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/e1A/rx_hi_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 -5.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/e1A/rx_hi_p") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 7 -1.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at -1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/e1A/rx_lo_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at 3.75 -3.5)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "RN5" (at 0 -2.8) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/e1A/rx_bias_n") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/e1A/rx_bias_n") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/e1A/rx_lo_n") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/e1A/rx_lo_p") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/e1A/rx_hi_n") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/e1A/rx_hi_p") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at 3.75 3.5)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "RN8" (at 0 -2.8) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/e1bias/bias_1") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/e1bias/bias_1") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/e1B/rx_hi_p") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/e1B/rx_hi_n") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/e1B/rx_lo_p") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/e1B/rx_lo_n") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 0.5 -4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 0.5 -2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 -0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/e1A/rx_bias_n") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 9 -9.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 1.75 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 0.5 4.25 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "C33" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 -0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 26 9.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "C39" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 0.5 2.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "C34" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/e1bias/bias_1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 9 -7.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 9 -10.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 26 10.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -4 12.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "C28" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 1.25 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/e1bias/bias_1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -5.5 12.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "C27" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 1.25 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "/e1bias/bias_0") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -1.25 9.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DNP" "DNP")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "0R" (at -1.25 0 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text user "DNP" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "/e1bias/bias_0") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -4.25 9.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "DNP" "DNP")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "0R" (at -1.25 0 90) (layer "F.Fab") hide)
    (fp_text user "DNP" (at 0 0 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/e1A/rx_bias_n") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/e1bias/bias_1") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 1.5 12.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "C26" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 1.25 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "/e1bias/bias_fixed") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at -1.25 12.5 -90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "RN7" (at 0 -2.8 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 1.25 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/e1bias/bias_fixed") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "/e1bias/bias_fixed") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "/e1bias/bias_0") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/e1bias/bias_1") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "/e1bias/bias1") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "/e1bias/bias0") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -2.75 9.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "0R" (at -1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/e1A/rx_bias_n") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "/e1bias/bias_0") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -17.75 -0.75 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+1V2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -8.5 6.75 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm" (layer "F.Cu")
    (tedit 5C26A111)
    (at -11 0)
    (descr "QFN, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2041_datasheet.pdf#page=62), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.8) (layer "F.SilkS") hide)
    (fp_text value "ICE40UP5K-SG48" (at 0 1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -0.66 -1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at -1.98 1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 1.98 -1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 1.98 0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 0.66 0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 0.66 1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at -0.66 0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at -0.66 1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at -1.98 -0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at -1.98 0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 0.66 -1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 0.66 -0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at -1.98 -1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 1.98 1.98) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at -0.66 -0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "" smd roundrect locked (at 1.98 -0.66) (size 1.07 1.07) (layers "F.Paste") (roundrect_rratio 0.233645))
    (pad "1" smd roundrect locked (at -3.45 -2.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VCC_IO2") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -3.45 -2.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "/fpga/gps_pps") (pinfunction "IOB_6A") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -3.45 -1.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "/fpga/i2c_sda") (pinfunction "IOB_9B") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -3.45 -1.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "/fpga/i2c_scl") (pinfunction "IOB_8A") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -3.45 -0.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+1V2") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd roundrect locked (at -3.45 -0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "/fpga/~{gps_reset}") (pinfunction "IOB_13B") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -3.45 0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/fpga/cdone") (pinfunction "CDONE") (pintype "open_collector"))
    (pad "8" smd roundrect locked (at -3.45 0.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/fpga/~{creset}") (pinfunction "~{CRESET_B}") (pintype "input"))
    (pad "9" smd roundrect locked (at -3.45 1.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "/fpga/usb_dn_i") (pinfunction "IOB_16A") (pintype "bidirectional"))
    (pad "10" smd roundrect locked (at -3.45 1.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "/fpga/usb_dp_i") (pinfunction "IOB_18A") (pintype "bidirectional"))
    (pad "11" smd roundrect locked (at -3.45 2.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/fpga/usb_pu_i") (pinfunction "IOB_20A") (pintype "bidirectional"))
    (pad "12" smd roundrect locked (at -3.45 2.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "/fpga/dbg_tx_i") (pinfunction "IOB_22A") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at -2.75 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "/gpio0") (pinfunction "IOB_24A") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at -2.25 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "/fpga/flash_mosi") (pinfunction "SPI_SDO/IOB_32A") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at -1.75 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/fpga/flash_sck") (pinfunction "SPI_SCK/IOB_34A") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at -1.25 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/fpga/~{flash_cs}") (pinfunction "~{SPI_CSn}/IOB_35B") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at -0.75 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/fpga/flash_miso") (pinfunction "SPI_SDI/IOB_33B") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at -0.25 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "/fpga/e1_led_rclk") (pinfunction "IOB_31B") (pintype "bidirectional"))
    (pad "19" smd roundrect locked (at 0.25 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "/gpio2") (pinfunction "IOB_29B") (pintype "bidirectional"))
    (pad "20" smd roundrect locked (at 0.75 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "/gpio1") (pinfunction "G3/IOB_25B") (pintype "bidirectional"))
    (pad "21" smd roundrect locked (at 1.25 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "/fpga/dbg_rx_i") (pinfunction "IOB_23B") (pintype "bidirectional"))
    (pad "22" smd roundrect locked (at 1.75 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VCC_IO1") (pintype "power_in"))
    (pad "23" smd roundrect locked (at 2.25 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/e1B/rx_hi_p") (pinfunction "IOT_37A") (pintype "bidirectional"))
    (pad "24" smd roundrect locked (at 2.75 3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VPP_2V5") (pintype "power_in"))
    (pad "25" smd roundrect locked (at 3.45 2.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/e1B/rx_hi_n") (pinfunction "IOT_36B") (pintype "bidirectional"))
    (pad "26" smd roundrect locked (at 3.45 2.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/e1B/rx_lo_p") (pinfunction "IOT_39A") (pintype "bidirectional"))
    (pad "27" smd roundrect locked (at 3.45 1.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/e1B/rx_lo_n") (pinfunction "IOT_38B") (pintype "bidirectional"))
    (pad "28" smd roundrect locked (at 3.45 1.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "/e1bias/bias0") (pinfunction "IOT_41A") (pintype "bidirectional"))
    (pad "29" smd roundrect locked (at 3.45 0.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(C5-Pad1)") (pinfunction "VCC_PLL") (pintype "power_in"))
    (pad "30" smd roundrect locked (at 3.45 0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+1V2") (pinfunction "VCC") (pintype "power_in"))
    (pad "31" smd roundrect locked (at 3.45 -0.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/e1A/rx_lo_n") (pinfunction "IOT_42B") (pintype "bidirectional"))
    (pad "32" smd roundrect locked (at 3.45 -0.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/e1A/rx_lo_p") (pinfunction "IOT_43A") (pintype "bidirectional"))
    (pad "33" smd roundrect locked (at 3.45 -1.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "VCC_IO0") (pintype "power_in"))
    (pad "34" smd roundrect locked (at 3.45 -1.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "/e1B/tx_hi") (pinfunction "IOT_44B") (pintype "bidirectional"))
    (pad "35" smd roundrect locked (at 3.45 -2.25) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "/e1bias/bias1") (pinfunction "G0/IOT_46B") (pintype "bidirectional"))
    (pad "36" smd roundrect locked (at 3.45 -2.75) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "/e1A/tx_lo") (pinfunction "IOT_48B") (pintype "bidirectional"))
    (pad "37" smd roundrect locked (at 2.75 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "/e1B/tx_lo") (pinfunction "G1/IOT_45A") (pintype "bidirectional"))
    (pad "38" smd roundrect locked (at 2.25 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/e1A/rx_hi_n") (pinfunction "IOT_50B") (pintype "bidirectional"))
    (pad "39" smd roundrect locked (at 1.75 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)") (pinfunction "RGB0") (pintype "open_collector"))
    (pad "40" smd roundrect locked (at 1.25 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad4)") (pinfunction "RGB1") (pintype "open_collector"))
    (pad "41" smd roundrect locked (at 0.75 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)") (pinfunction "RGB2") (pintype "open_collector"))
    (pad "42" smd roundrect locked (at 0.25 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/e1A/rx_hi_p") (pinfunction "IOT_51A") (pintype "bidirectional"))
    (pad "43" smd roundrect locked (at -0.25 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/e1A/tx_hi") (pinfunction "IOT_49A") (pintype "bidirectional"))
    (pad "44" smd roundrect locked (at -0.75 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/fpga/clk_30m72") (pinfunction "G6/IOB_3B") (pintype "bidirectional"))
    (pad "45" smd roundrect locked (at -1.25 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/fpga/clk_tune_lo") (pinfunction "IOB_5B") (pintype "bidirectional"))
    (pad "46" smd roundrect locked (at -1.75 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "/fpga/gps_tx") (pinfunction "IOB_0A") (pintype "bidirectional"))
    (pad "47" smd roundrect locked (at -2.25 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "/fpga/gps_rx") (pinfunction "IOB_2A") (pintype "bidirectional"))
    (pad "48" smd roundrect locked (at -2.75 -3.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/fpga/clk_tune_hi") (pinfunction "IOB_4A") (pintype "bidirectional"))
    (pad "49" smd roundrect locked (at 0 0) (size 5.3 5.3) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.04717)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -20 -7.25 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "psu")
    (attr smd)
    (fp_text reference "C32" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 0 -0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5A02FF57)
    (at -22.75 -7.25)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "psu")
    (attr smd)
    (fp_text reference "U10" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MIC5504-3.3YM5" (at 1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "+1V2") (pinfunction "EN") (pintype "input"))
    (pad "4" smd rect locked (at 1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(U10-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect locked (at 1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -25.5 -7.25 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "psu")
    (attr smd)
    (fp_text reference "C31" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1u" (at 0 -0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "s47-conn:Jack_2.5mm_CUI_SJ-2523-SMT_Horizontal" (layer "F.Cu")
    (tedit 5F32BCF4)
    (at -37.25 -10.5 90)
    (descr "2.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cuidevices.com/product/resource/sj-252x-smt.pdf))")
    (tags "2.5mm audio cui horizontal jack stereo")
    (property "MPN" "CUI SJ-2523-SMT")
    (property "Sheetfile" "icE1usb.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "X2" (at 0 -8.5 90) (layer "F.SilkS") hide)
    (fp_text value "Serial" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.75 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 -3 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 3 90) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "R" smd rect locked (at 3.3 -1.6 90) (size 2.8 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/dbg_tx") (pintype "passive"))
    (pad "S" smd rect locked (at -3.3 -4.3 90) (size 2.8 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "T" smd rect locked (at -3.45 5.4 90) (size 2.5 2.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/dbg_rx") (pintype "passive"))
    (model "${KIUSR3DMOD}/CUI_DEVICES_SJ-2523-SMT-TR.step"
      (offset (xyz 0 6 2.55))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 29.25 -22.75 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "Littlefuse 0603L010")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "300mA" (at -2 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/e1A_rj1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(F1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 26 20.5 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "U12" (at 0 -2.45 90) (layer "F.SilkS") hide)
    (fp_text value "IP4220CZ6" (at -1.25 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(F7-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at -1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "unconnected-(U12-Pad2)") (pintype "passive+no_connect"))
    (pad "3" smd rect locked (at -1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(F8-Pad2)") (pintype "passive"))
    (pad "4" smd rect locked (at 1.16 0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(F6-Pad2)") (pintype "passive"))
    (pad "5" smd rect locked (at 1.16 0 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "unconnected-(U12-Pad5)") (pintype "passive+no_connect"))
    (pad "6" smd rect locked (at 1.16 -0.95 90) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(F5-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 26 7.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1B")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(C39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 26 -7.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1k5" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "/fpga/e1_led_rclk") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/fpga/~{boot_sw}") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 0.25 9.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1bias.kicad_sch")
    (property "Sheetname" "e1bias")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "0R" (at -1.25 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/e1A/rx_bias_p") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "/e1bias/bias_fixed") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at -10.5 -17.5 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "DNP" "DNP")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "SDM02U30LP3" (at 0 -0.75) (layer "F.Fab") hide)
    (fp_text user "DNP" (at 0 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at -10.5 -14.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "fpga.kicad_sch")
    (property "Sheetname" "fpga")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1k5" (at 1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/fpga/clk_tune_hi") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x0603" (layer "F.Cu")
    (tedit 58E0A8B2)
    (at -16.5 -9.75 -90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr smd)
    (fp_text reference "RN6" (at 0 -2.8 90) (layer "F.SilkS") hide)
    (fp_text value "33R" (at -1.25 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.9 -1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(RN6-Pad1)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -0.9 -0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "Net-(RN6-Pad2)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -0.9 0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "Net-(RN6-Pad3)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -0.9 1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(RN6-Pad4)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 0.9 1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/fpga/i2c_scl") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 0.9 0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "/fpga/i2c_sda") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 0.9 -0.4 270) (size 0.8 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "/fpga/gps_rx") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 0.9 -1.2 270) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "/fpga/gps_tx") (pinfunction "R1.2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 10.5 -2.75 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "27R" (at -1.5 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "Net-(R16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/e1A/tx_hi") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 11.25 -5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "e1if.kicad_sch")
    (property "Sheetname" "e1A")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "120R" (at 0 0.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(C16-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 39 -25)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (attr smd board_only exclude_from_bom)
    (fp_text reference "FID_TR" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial_1mm_Mask2mm" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "s47-misc:J_0402" (layer "F.Cu")
    (tedit 5BF23F61)
    (at -21.75 -11.25)
    (descr "Jumper SMD 0402, reflow soldering")
    (tags "jumper 0402")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP2" (at 0 -1.1) (layer "F.Fab") hide)
    (fp_text value "GPS SDA" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.425 0) (size 0.65 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 156 "Net-(U8-Pad16)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.425 0) (size 0.65 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "Net-(RN6-Pad3)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at -39 25)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (attr smd board_only exclude_from_bom)
    (fp_text reference "FID_BL" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial_1mm_Mask2mm" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "s47-misc:J_0402" (layer "F.Cu")
    (tedit 5BF23F61)
    (at -21.75 -10.25)
    (descr "Jumper SMD 0402, reflow soldering")
    (tags "jumper 0402")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP3" (at 0 -1.1) (layer "F.Fab") hide)
    (fp_text value "GPS SCL" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.425 0) (size 0.65 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 157 "Net-(U8-Pad17)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.425 0) (size 0.65 0.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "Net-(RN6-Pad4)") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Fiducial:Fiducial_1mm_Mask2mm" (layer "F.Cu")
    (tedit 5C18CB26)
    (at 39 25)
    (descr "Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)")
    (tags "fiducial")
    (attr smd board_only exclude_from_bom)
    (fp_text reference "FID_BR" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Fiducial_1mm_Mask2mm" (at 0 2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd circle (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (footprint "s47-misc:J_NC_0603_30" (layer "B.Cu")
    (tedit 5BF2400B)
    (at -16.25 -18.25 -90)
    (descr "Jumper Normally Closed SMD 0603, 0.30mm connection, reflow soldering")
    (tags "jumper 0603")
    (property "Sheetfile" "gps.kicad_sch")
    (property "Sheetname" "gps")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "JP1" (at 0 1.1 90) (layer "B.Fab"))
    (fp_text value "BatBypass" (at 0 -1.2 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.575 0 270) (size 0.95 0.9) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "+3V3") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.575 0 270) (size 0.95 0.9) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "/gps/vbackup") (pinfunction "B") (pintype "passive"))
  )
  (gr_line (start -43 22.5) (end -43 -22.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 37.5 26.5) (end 40.5 26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 42 24.75) (mid 42.114181 24.175975) (end 42.43934 23.68934) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 42 25) (mid 41.56066 26.06066) (end 40.5 26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 37.5 26.5) (mid 36.925975 26.385819) (end 36.43934 26.06066) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 36.31066 25.93934) (end 36.43934 26.06066) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 42.56066 23.56066) (end 42.43934 23.68934) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 42 24.75) (end 42 25) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -36.31066 25.93934) (mid -35.824025 25.614181) (end -35.25 25.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -37.5 26.5) (end -40.5 26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -36.43934 26.06066) (mid -36.925975 26.385819) (end -37.5 26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -42 24.75) (end -42 25) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -36.31066 25.93934) (end -36.43934 26.06066) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -40.5 26.5) (mid -41.56066 26.06066) (end -42 25) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -42.56066 23.56066) (end -42.43934 23.68934) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -42.43934 23.68934) (mid -42.114181 24.175975) (end -42 24.75) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -42.56066 23.56066) (mid -42.885819 23.074025) (end -43 22.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 37.5 -26.5) (end 40.5 -26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 36.43934 -26.06066) (mid 36.925975 -26.385819) (end 37.5 -26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 36.31066 -25.93934) (end 36.43934 -26.06066) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 42 -24.75) (end 42 -25) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 36.31066 -25.93934) (mid 35.824025 -25.614181) (end 35.25 -25.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 40.5 -26.5) (mid 41.56066 -26.06066) (end 42 -25) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 42.56066 -23.56066) (end 42.43934 -23.68934) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 42.43934 -23.68934) (mid 42.114181 -24.175975) (end 42 -24.75) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 42.56066 -23.56066) (mid 42.885819 -23.074025) (end 43 -22.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -37.5 -26.5) (mid -36.925975 -26.385819) (end -36.43934 -26.06066) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -42 -24.75) (end -42 -25) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 35.25 25.5) (mid 35.824025 25.614181) (end 36.31066 25.93934) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -37.5 -26.5) (end -40.5 -26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -42 -25) (mid -41.56066 -26.06066) (end -40.5 -26.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -42.56066 -23.56066) (end -42.43934 -23.68934) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -35.25 -25.5) (mid -35.824025 -25.614181) (end -36.31066 -25.93934) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -43 -22.5) (mid -42.885819 -23.074025) (end -42.56066 -23.56066) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 43 -22.5) (end 43 22.5) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -36.31066 -25.93934) (end -36.43934 -26.06066) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start -42 -24.75) (mid -42.114181 -24.175975) (end -42.43934 -23.68934) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 35.25 25.5) (end -35.25 25.5) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 43 22.5) (mid 42.885819 23.074025) (end 42.56066 23.56066) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start -35.25 -25.5) (end 35.25 -25.5) (layer "Edge.Cuts") (width 0.05))
  (gr_text "rev 1.1 - 202209\n(c) 2020 - Munaut.S\nCERN-OHL-S" (at 0 -15) (layer "F.SilkS"))
  (gr_text "icE1usb" (at 0 -17.5) (layer "F.SilkS"))
  (gr_text "Serial" (at -47.5 -10.5 90) (layer "Eco1.User"))
  (gr_text "SMA" (at -57.5 -20 90) (layer "Eco1.User"))
  (gr_text "GPIO\nExt" (at -47.5 15 90) (layer "Eco1.User"))
  (gr_text "USB" (at -47.5 0 90) (layer "Eco1.User"))
  (gr_text "Back\nPanel" (at 44.75 -25.5) (layer "Eco1.User"))
  (gr_text "Front\nPanel" (at -44.75 -25.5) (layer "Eco1.User"))
  (zone (net 1) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 10 -11.25)
        (xy 28 -11.25)
        (xy 28 11.25)
        (xy 26.75 11.25)
        (xy 25.25 11.25)
        (xy 10 11.25)
        (xy 10 25)
        (xy -5.375 25)
        (xy -20.5 25)
        (xy -20.5 10.25)
        (xy -21.5 9.25)
        (xy -28 9.25)
        (xy -33 4.25)
        (xy -42.5 4.25)
        (xy -42.5 -22.5)
        (xy -41.5 -24.000292)
        (xy -41.5 -25)
        (xy 10 -25)
      )
    )
  )
  (zone (net 21) (net_name "+3V3") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 10 -11.25)
        (xy 28 -11.25)
        (xy 28 11.25)
        (xy 10 11.25)
        (xy 10 25)
        (xy -20.5 25)
        (xy -20.5 10.25)
        (xy -21.5 9.25)
        (xy -28 9.25)
        (xy -33 4.25)
        (xy -42.5 4.25)
        (xy -42.5 -22.501877)
        (xy -41.5 -24)
        (xy -41.5 -25)
        (xy 10 -25)
      )
    )
  )
  (zone (net 20) (net_name "Net-(C1-Pad2)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -35.75 -4.75)
        (xy -35.75 -4)
        (xy -36.25 -3.5)
        (xy -38.25 -3.5)
        (xy -38.5 -3.25)
        (xy -38.5 3.25)
        (xy -38.25 3.5)
        (xy -36.25 3.5)
        (xy -35.75 4)
        (xy -35.75 4.75)
        (xy -36.25 5.25)
        (xy -42 5.25)
        (xy -42.5 4.75)
        (xy -42.5 -4.75)
        (xy -42 -5.25)
        (xy -36.25 -5.25)
      )
    )
  )
)
