08:48:35.839291 9836 BSC_Tests.ttcn:3199 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc0_connection_status'.
08:48:37.385565 9836 BSC_Tests.ttcn:3199 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc0_connection_status' was executed successfully (exit status: 0).
08:48:37.385924 9836 BSC_Tests.ttcn:3199 Test case TC_ctrl_msc0_connection_status started.
08:48:37.386065 9836 BSC_Tests.ttcn:3199 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:37.387014 9836 BSC_Tests.ttcn:3199 Port IPA_CTRL was started.
08:48:37.387158 9836 BSC_Tests.ttcn:3199 Port RSL_CCHAN[0] was started.
08:48:37.387253 9836 BSC_Tests.ttcn:3199 Port RSL_CCHAN[1] was started.
08:48:37.387345 9836 BSC_Tests.ttcn:3199 Port RSL_CCHAN[2] was started.
08:48:37.387434 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[0][0] was started.
08:48:37.387525 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[0][1] was started.
08:48:37.387613 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[0][2] was started.
08:48:37.387863 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[0][3] was started.
08:48:37.387960 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[1][0] was started.
08:48:37.388019 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[1][1] was started.
08:48:37.388077 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[1][2] was started.
08:48:37.388135 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[1][3] was started.
08:48:37.388192 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[2][0] was started.
08:48:37.388249 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[2][1] was started.
08:48:37.388307 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[2][2] was started.
08:48:37.388365 9836 BSC_Tests.ttcn:3199 Port IPA_RSL[2][3] was started.
08:48:37.388425 9836 BSC_Tests.ttcn:3199 Port IPA was started.
08:48:37.388486 9836 BSC_Tests.ttcn:3199 Port SCCPLITE_IPA_CTRL was started.
08:48:37.388547 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[0][0] was started.
08:48:37.388607 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[0][1] was started.
08:48:37.388667 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[0][2] was started.
08:48:37.388727 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[0][3] was started.
08:48:37.388786 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[1][0] was started.
08:48:37.388847 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[1][1] was started.
08:48:37.388906 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[1][2] was started.
08:48:37.388966 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[1][3] was started.
08:48:37.389028 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[2][0] was started.
08:48:37.389087 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[2][1] was started.
08:48:37.389145 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[2][2] was started.
08:48:37.389205 9836 BSC_Tests.ttcn:3199 Port IPA_CFG_PORT[2][3] was started.
08:48:37.389265 9836 BSC_Tests.ttcn:3199 Port BSCVTY was started.
08:48:37.389326 9836 BSC_Tests.ttcn:3199 Port STPVTY was started.
08:48:37.389386 9836 BSC_Tests.ttcn:3199 Port SCCPLITE_IPA_CFG_PORT[0] was started.
08:48:37.389446 9836 BSC_Tests.ttcn:3199 Port SCCPLITE_IPA_CFG_PORT[1] was started.
08:48:37.389507 9836 BSC_Tests.ttcn:3199 Port SCCPLITE_IPA_CFG_PORT[2] was started.
08:48:37.389566 9836 BSC_Tests.ttcn:3199 Port BSSAP was started.
08:48:37.389625 9836 BSC_Tests.ttcn:3199 Port BSSAP_LE was started.
08:48:37.389687 9836 BSC_Tests.ttcn:3199 Component type BSC_Tests.test_CT was initialized.
08:48:37.389762 9836 BSC_Tests.ttcn:1277 Start timer T_guard: 30 s
08:48:37.389841 9836 BSC_Tests.ttcn:1278 Altstep as_Tguard was activated as default, id 1
08:48:37.389914 9836 BSC_Tests.ttcn:1100 Mapping port mtc:BSCVTY to system:BSCVTY.
08:48:37.390421 9836 BSC_Tests.ttcn:1100 Message enqueued on BSCVTY from system integer : 2 id 1
08:48:37.390513 9836 BSC_Tests.ttcn:1100 Port BSCVTY was mapped to system:BSCVTY.
08:48:37.390640 9836 BSC_Tests.ttcn:1100 Map operation of mtc:BSCVTY to system:BSCVTY finished.
08:48:37.390734 9836 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:37.390812 9836 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:37.390899 9836 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:37.391052 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
08:48:37.391159 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.391237 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:37.391304 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:37.391367 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:37.391429 9836 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:37.391491 9836 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:37.391560 9836 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
08:48:37.391631 9836 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
08:48:37.391721 9836 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
08:48:37.391920 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
08:48:37.392073 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.392195 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.392269 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:37.392342 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
08:48:37.392415 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.392496 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:37.392594 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.393241 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
08:48:37.393684 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.393899 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.394086 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.394174 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
08:48:37.394258 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
08:48:37.394348 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.394439 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
08:48:37.394565 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.394816 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
08:48:37.394936 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.395039 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.395163 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.395251 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
08:48:37.395324 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
08:48:37.395403 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.395479 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
08:48:37.395570 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.395789 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
08:48:37.395908 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.396011 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.396131 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.396201 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
08:48:37.396273 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
08:48:37.396350 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.396425 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
08:48:37.396510 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.396625 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
08:48:37.396731 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.396829 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.396953 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.397022 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
08:48:37.397093 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
08:48:37.397168 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.397238 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:37.397320 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.397413 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
08:48:37.397517 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.397621 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.397690 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
08:48:37.397761 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
08:48:37.397830 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.397905 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:37.397986 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.398109 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
08:48:37.398209 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.398305 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.398434 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.398507 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
08:48:37.398577 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
08:48:37.398652 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.398725 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:37.398807 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.398918 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
08:48:37.399022 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.399122 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.399238 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.399309 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
08:48:37.399378 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
08:48:37.399454 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.399524 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:37.399606 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.399746 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
08:48:37.399910 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.400043 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.400202 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.400277 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
08:48:37.400352 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
08:48:37.400431 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.400504 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:37.400604 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.400830 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
08:48:37.400945 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.401050 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.401179 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.401250 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
08:48:37.401321 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
08:48:37.401396 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.401468 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:37.401555 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.401669 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
08:48:37.401787 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.401892 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.401960 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
08:48:37.402029 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
08:48:37.402100 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.402173 9836 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:37.411951 9928 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:37.412161 9928 - TTCN-3 Parallel Test Component started on 5e318a98d888. Component reference: VirtMSC-STATS(10), component type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS. Version: 11.1.0.
08:48:37.412219 9928 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:37.412352 9928 - Connected to MC.
08:48:37.412396 9928 - Initializing variables, timers and ports of component type StatsD_Checker.StatsD_Checker_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:37.412464 9836 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 10, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:37.412517 9836 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(10).
08:48:37.412685 9836 StatsD_Checker.ttcnpp:417 Function was started.
08:48:37.412851 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
08:48:37.412992 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.413233 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
08:48:37.413413 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.413571 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.413669 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
08:48:37.413763 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
08:48:37.413859 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.413957 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
08:48:37.414075 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.414502 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 1" id 14
08:48:37.414611 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
08:48:37.414757 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.414894 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.415033 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:37.415145 9836 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:37.415282 9836 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 1" with ? matched
08:48:37.415495 9836 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 1" id 14
08:48:37.415731 9836 Osmocom_VTY_Functions.ttcn:85 Message with id 14 was extracted from the queue of BSCVTY.
08:48:37.415805 9928 - Port STATSVTY was started.
08:48:37.415936 9928 - Port STATSD_PROC was started.
08:48:37.416017 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.416060 9928 - Port STATS was started.
08:48:37.416122 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.416136 9928 - Component type StatsD_Checker.StatsD_Checker_CT was initialized.
08:48:37.416188 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
08:48:37.416254 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
08:48:37.416359 9928 - Starting function main("127.0.0.1", 8125, 5.000000).
08:48:37.416400 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.416542 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
08:48:37.416624 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.416795 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 2" id 16
08:48:37.416854 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
08:48:37.416893 9928 StatsD_Checker.ttcnpp:125 Mapping port VirtMSC-STATS(10):STATS to system:STATS.
08:48:37.416933 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.417010 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.417081 9928 StatsD_Checker.ttcnpp:125 Port STATS was mapped to system:STATS.
08:48:37.417088 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:37.417149 9836 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:37.417207 9836 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 2" with ? matched
08:48:37.417223 9928 StatsD_Checker.ttcnpp:125 Map operation of VirtMSC-STATS(10):STATS to system:STATS finished.
08:48:37.417263 9836 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 2" id 16
08:48:37.417323 9836 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
08:48:37.417401 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.417480 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.417541 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
08:48:37.417610 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
08:48:37.417645 9928 StatsD_Checker.ttcnpp:126 entering f__IPL4__PROVIDER__listen: 127.0.0.1:8125 / UDP
08:48:37.417678 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.417838 9836 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:37.420178 9928 StatsD_Checker.ttcnpp:134 Mapping port VirtMSC-STATS(10):STATSVTY to system:STATSVTY.
08:48:37.421160 9928 StatsD_Checker.ttcnpp:134 Message enqueued on STATSVTY from system integer : 2 id 1
08:48:37.421355 9928 StatsD_Checker.ttcnpp:134 Port STATSVTY was mapped to system:STATSVTY.
08:48:37.421455 9928 StatsD_Checker.ttcnpp:134 Map operation of VirtMSC-STATS(10):STATSVTY to system:STATSVTY finished.
08:48:37.421787 9928 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:37.421969 9928 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:37.422034 9928 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:37.422325 9928 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "enable"
08:48:37.422476 9928 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.422596 9928 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:37.422641 9928 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:37.422675 9928 Osmocom_VTY_Functions.ttcn:74 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:37.422711 9928 Osmocom_VTY_Functions.ttcn:75 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:37.422765 9928 Osmocom_VTY_Functions.ttcn:85 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:37.422892 9928 Osmocom_VTY_Functions.ttcn:86 Matching on port STATSVTY succeeded: 2 with ? matched
08:48:37.422959 9928 Osmocom_VTY_Functions.ttcn:86 Receive operation on port STATSVTY succeeded, message from system(): integer : 2 id 1
08:48:37.423015 9928 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of STATSVTY.
08:48:37.423177 9928 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 2
08:48:37.423316 9928 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.423381 9928 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.423413 9928 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:37.423453 9928 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of STATSVTY.
08:48:37.423507 9928 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.423561 9928 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "stats reset"
08:48:37.423610 9928 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.423697 9928 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 3
08:48:37.423749 9928 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.423796 9928 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.423827 9928 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 3
08:48:37.423860 9928 Osmocom_VTY_Functions.ttcn:73 Message with id 3 was extracted from the queue of STATSVTY.
08:48:37.423892 9928 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.423967 9929 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:37.424111 9929 - TTCN-3 Parallel Test Component started on 5e318a98d888. Component reference: VirtMSC-SCCP(11), component type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP. Version: 11.1.0.
08:48:37.424150 9929 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:37.424213 9929 - Connected to MC.
08:48:37.424244 9929 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:37.424285 9836 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 11, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:37.424328 9836 SCCP_Adapter.ttcnpp:131 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:37.426224 9929 - Port SCCP_SP_PORT was started.
08:48:37.426269 9929 - Port MTP3_SCCP_PORT was started.
08:48:37.426293 9929 - Component type SCCP_Emulation.SCCP_CT was initialized.
08:48:37.427711 9930 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:37.427795 9930 - TTCN-3 Parallel Test Component started on 5e318a98d888. Component reference: VirtMSC-IPA(12), component type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA. Version: 11.1.0.
08:48:37.427819 9930 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:37.427860 9930 - Connected to MC.
08:48:37.427880 9930 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:37.427894 9836 SCCP_Adapter.ttcnpp:131 PTC was created. Component reference: 12, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:37.427916 9836 SCCP_Adapter.ttcnpp:132 Mapping port VirtMSC-IPA(12):IPA_PORT to system:IPA_CODEC_PT.
08:48:37.429459 9930 - Port IPA_PORT was started.
08:48:37.429508 9930 - Port CFG_PORT was started.
08:48:37.429527 9930 - Port MTP3_SP_PORT was started.
08:48:37.429546 9930 - Port IPA_MGCP_PORT was started.
08:48:37.429563 9930 - Port IPA_RSL_PORT was started.
08:48:37.429582 9930 - Port IPA_OML_PORT was started.
08:48:37.429602 9930 - Port IPA_CTRL_PORT was started.
08:48:37.429621 9930 - Port IPA_SP_PORT was started.
08:48:37.429640 9930 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:37.429688 9930 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:37.429768 9836 SCCP_Adapter.ttcnpp:132 Map operation of VirtMSC-IPA(12):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:37.429800 9836 SCCP_Adapter.ttcnpp:134 Connecting ports VirtMSC-IPA(12):MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT.
08:48:37.430158 9929 - Port MTP3_SCCP_PORT is waiting for connection from VirtMSC-IPA(12):MTP3_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-1278f476.
08:48:37.430203 9930 - Port MTP3_SP_PORT has established the connection with VirtMSC-SCCP(11):MTP3_SCCP_PORT using transport type UNIX.
08:48:37.430281 9929 - Port MTP3_SCCP_PORT has accepted the connection from VirtMSC-IPA(12):MTP3_SP_PORT.
08:48:37.430328 9836 SCCP_Adapter.ttcnpp:134 Connect operation on VirtMSC-IPA(12):MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT finished.
08:48:37.430353 9836 SCCP_Adapter.ttcnpp:136 Creating new alive PTC with component type IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:37.433346 9931 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:37.433422 9931 - TTCN-3 Parallel Test Component started on 5e318a98d888. Component reference: VirtMSC-IPA-WAIT(13), component type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT. Version: 11.1.0.
08:48:37.433446 9931 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:37.433493 9931 - Connected to MC.
08:48:37.433509 9931 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_EventWaiter_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:37.433530 9836 SCCP_Adapter.ttcnpp:136 PTC was created. Component reference: 13, alive: yes, type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:37.433586 9836 SCCP_Adapter.ttcnpp:137 Connecting ports VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:37.433814 9930 - Port IPA_SP_PORT is waiting for connection from VirtMSC-IPA-WAIT(13):IPA_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-376bb203.
08:48:37.434535 9931 - Port IPA_SP_PORT was started.
08:48:37.434566 9931 - Component type IPA_Emulation.IPA_EventWaiter_CT was initialized.
08:48:37.434606 9931 - Port IPA_SP_PORT has established the connection with VirtMSC-IPA(12):IPA_SP_PORT using transport type UNIX.
08:48:37.434707 9930 - Port IPA_SP_PORT has accepted the connection from VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:37.434729 9836 SCCP_Adapter.ttcnpp:137 Connect operation on VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT finished.
08:48:37.434789 9836 SCCP_Adapter.ttcnpp:138 Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}) on component VirtMSC-IPA-WAIT(13).
08:48:37.434879 9836 SCCP_Adapter.ttcnpp:138 Function was started.
08:48:37.434926 9836 SCCP_Adapter.ttcnpp:140 Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true) on component VirtMSC-IPA(12).
08:48:37.434982 9836 SCCP_Adapter.ttcnpp:140 Function was started.
08:48:37.435007 9931 - Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}).
08:48:37.435081 9930 - Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true).
08:48:37.435329 9930 IPA_Emulation.ttcnpp:346 entering f__IPL4__PROVIDER__listen: 127.0.0.1:5000 / TCP
08:48:40.558270 9930 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:40.559162 9930 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:40.559472 9930 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:40.559983 9930 IPA_Emulation.ttcnpp:864 Matching on port IPA_PORT succeeded:  matched
08:48:40.560499 9930 IPA_Emulation.ttcnpp:864 Receive operation on port IPA_PORT succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:40.560940 9930 IPA_Emulation.ttcnpp:864 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:40.561372 9930 IPA_Emulation.ttcnpp:866 Established a new IPA connection (conn_id=2)
08:48:40.562872 9930 IPA_Emulation.ttcnpp:395 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(13) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
}
08:48:40.564257 9931 IPA_Emulation.ttcnpp:1007 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(12) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:40.564444 9930 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:40.565118 9930 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:40.565226 9931 IPA_Emulation.ttcnpp:1008 Matching on port IPA_SP_PORT ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:40.565389 9931 IPA_Emulation.ttcnpp:1011 Matching on port IPA_SP_PORT succeeded.
08:48:40.565584 9931 IPA_Emulation.ttcnpp:1011 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(12): @IPA_Emulation.ASP_IPA_Event: {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:40.565799 9931 IPA_Emulation.ttcnpp:1011 Message with id 1 was extracted from the queue of IPA_SP_PORT.
08:48:40.565894 9930 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:40.566881 9930 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:40.567706 9930 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:40.568278 9930 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:40.568606 9930 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:40.568730 9930 IPA_Emulation.ttcnpp:774 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:40.568840 9930 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:40.568951 9930 IPA_Emulation.ttcnpp:395 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(13) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
}
08:48:40.569061 9931 IPA_Emulation.ttcnpp:1007 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(12) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:40.569119 9930 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE00'O
} id 3
08:48:40.569228 9930 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:40.569257 9931 IPA_Emulation.ttcnpp:1008 Matching on port IPA_SP_PORT succeeded:  matched
08:48:40.569306 9930 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0016FD090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:40.569348 9931 IPA_Emulation.ttcnpp:1008 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(12): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:40.569380 9930 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:40.569432 9931 IPA_Emulation.ttcnpp:1008 Message with id 2 was extracted from the queue of IPA_SP_PORT.
08:48:40.569460 9930 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:40.569542 9930 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:40.569552 9931 IPA_Emulation.ttcnpp:1009 setverdict(pass): none -> pass
08:48:40.569613 9930 IPA_Emulation.ttcnpp:774 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:40.569680 9930 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_PING (0),
    u := omit
}
08:48:40.569687 9931 - Function waiter_main finished. PTC remains alive and is waiting for next start.
08:48:40.569771 9930 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_PONG (1),
    u := omit
}
08:48:40.569852 9930 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '01'O
}
08:48:40.569937 9930 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE01'O
}
08:48:40.569988 9836 SCCP_Adapter.ttcnpp:151 PTC with component reference 13 is done.
08:48:40.570265 9930 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_SCCP (253) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:40.570346 9836 SCCP_Adapter.ttcnpp:152 Disconnecting ports VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:40.570353 9930 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:40.570426 9930 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:40.570496 9930 IPA_Emulation.ttcnpp:790 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:40.570566 9931 - Terminating the connection of port IPA_SP_PORT to VirtMSC-IPA(12):IPA_SP_PORT. No more messages can be sent through this connection.
08:48:40.571500 9930 IPA_Emulation.ttcnpp:796 Sent on MTP3_SP_PORT to VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
}
08:48:40.571868 9930 IPA_Emulation.ttcnpp:772 Connection termination request was received on port IPA_SP_PORT from VirtMSC-IPA-WAIT(13):IPA_SP_PORT. No more data can be sent or received through this connection.
08:48:40.571975 9931 - Port IPA_SP_PORT was disconnected from VirtMSC-IPA(12):IPA_SP_PORT.
08:48:40.572081 9930 IPA_Emulation.ttcnpp:772 Port IPA_SP_PORT was disconnected from VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:40.572138 9836 SCCP_Adapter.ttcnpp:152 Disconnect operation on VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT finished.
08:48:40.572378 9836 BSC_Tests.ttcn:1225 Connecting ports mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT.
08:48:40.572493 9929 - Message enqueued on MTP3_SCCP_PORT from VirtMSC-IPA(12) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 1
08:48:40.573236 9836 BSC_Tests.ttcn:1225 Port SCCPLITE_IPA_CFG_PORT[0] is waiting for connection from VirtMSC-IPA(12):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-c504b44b.
08:48:40.573388 9930 IPA_Emulation.ttcnpp:772 Port CFG_PORT has established the connection with mtc:SCCPLITE_IPA_CFG_PORT[0] using transport type UNIX.
08:48:40.573622 9836 BSC_Tests.ttcn:1225 Port SCCPLITE_IPA_CFG_PORT[0] has accepted the connection from VirtMSC-IPA(12):CFG_PORT.
08:48:40.573720 9836 BSC_Tests.ttcn:1225 Connect operation on mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT finished.
08:48:40.573798 9836 BSC_Tests.ttcn:1227 Connecting ports mtc:BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:40.574532 9836 BSC_Tests.ttcn:1227 Port BSSAP is waiting for connection from VirtMSC-SCCP(11):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-d07fb81d.
08:48:40.574892 9929 - Incoming message was mapped to @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:40.575200 9929 - Port SCCP_SP_PORT has established the connection with mtc:BSSAP using transport type UNIX.
08:48:40.575395 9836 BSC_Tests.ttcn:1227 Port BSSAP has accepted the connection from VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:40.575475 9836 BSC_Tests.ttcn:1227 Connect operation on mtc:BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT finished.
08:48:40.575548 9836 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}) on component VirtMSC-SCCP(11).
08:48:40.575731 9836 SCCP_Adapter.ttcnpp:165 Function was started.
08:48:40.575875 9836 RAN_Emulation.ttcnpp:1403 Waiting for SCCP peer PC=187 to become available
08:48:40.575951 9836 RAN_Emulation.ttcnpp:1404 Start timer T: 3 s
08:48:40.576076 9929 - Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}).
08:48:40.576742 9929 SCCP_Emulation.ttcn:1453 v_sccp_pdu_maxlen:268
08:48:40.577750 9929 SCCP_Emulation.ttcn:5523 Matching on port MTP3_SCCP_PORT succeeded:  matched
08:48:40.577914 9929 SCCP_Emulation.ttcn:5523 Receive operation on port MTP3_SCCP_PORT succeeded, message from VirtMSC-IPA(12): @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:40.578079 9929 SCCP_Emulation.ttcn:5523 Message with id 1 was extracted from the queue of MTP3_SCCP_PORT.
08:48:40.579880 9929 SCCP_Emulation.ttcn:3464 Sent on SCCP_SP_PORT to mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
}
08:48:40.580364 9836 RAN_Emulation.ttcnpp:1406 Message enqueued on BSSAP from VirtMSC-SCCP(11) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
} id 1
08:48:40.580461 9836 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000430040120'O
08:48:40.581111 9836 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 4,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 1,
                    causeValue := '0100000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:40.581265 9836 RAN_Emulation.ttcnpp:1406 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:40.581388 9836 RAN_Emulation.ttcnpp:1407 Matching on port BSSAP failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_PCSTATE_ind.
08:48:40.581640 9836 RAN_Emulation.ttcnpp:1424 Matching on port BSSAP succeeded:  matched
08:48:40.581754 9836 RAN_Emulation.ttcnpp:1424 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(11): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:40.581868 9836 RAN_Emulation.ttcnpp:1424 Message with id 1 was extracted from the queue of BSSAP.
08:48:40.581948 9836 RAN_Emulation.ttcnpp:1425 Waiting for SCCP peer PC=187: Rx BSSMAP RANAP RESET, ACKing
08:48:40.582117 9836 RAN_Emulation.ttcnpp:1426 Sent on BSSAP to VirtMSC-SCCP(11) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:48:40.582202 9836 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:40.582307 9836 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000131'O
08:48:40.582388 9836 RAN_Emulation.ttcnpp:1426 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
}
08:48:40.582487 9836 RAN_Emulation.ttcnpp:1429 Stop timer T: 3 s
08:48:40.582590 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
08:48:40.582724 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:40.582919 9929 SCCP_Emulation.ttcn:5519 Message enqueued on SCCP_SP_PORT from mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 1
08:48:40.583214 9929 SCCP_Emulation.ttcn:5672 Matching on port SCCP_SP_PORT succeeded.
08:48:40.583332 9929 SCCP_Emulation.ttcn:5672 Check-receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req: {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 1
08:48:40.583422 9929 SCCP_Emulation.ttcn:5680 Matching on port SCCP_SP_PORT failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_DATA_req.
08:48:40.583741 9929 SCCP_Emulation.ttcn:5686 Matching on port SCCP_SP_PORT succeeded:  matched
08:48:40.583833 9929 SCCP_Emulation.ttcn:5686 Receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 1
08:48:40.583952 9929 SCCP_Emulation.ttcn:5686 Message with id 1 was extracted from the queue of SCCP_SP_PORT.
08:48:40.586378 9929 SCCP_Emulation.ttcn:5300 Sent on MTP3_SCCP_PORT to VirtMSC-IPA(12) @SCCP_Types.ASP_MTP3_TRANSFERreq_sccp : {
    sio := '03'O,
    opc := 185,
    dpc := 187,
    sls := 0,
    data := {
        unitdata := {
            messageType := 9,
            protClass := {
                class := '0000'B,
                messageHandling := '0000'B
            },
            pointer1 := 0,
            pointer2 := 0,
            pointer3 := 0,
            calledPAddress := {
                paramLength := 4,
                addr := '43BB00FE'O
            },
            callingPAddress := {
                paramLength := 4,
                addr := '43B900FE'O
            },
            data := {
                paramLength := 3,
                data := '000131'O
            }
        }
    }
}
08:48:40.587228 9929 SCCP_Emulation.ttcn:5300 Outgoing message was mapped to @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:40.587781 9930 IPA_Emulation.ttcnpp:772 Message enqueued on MTP3_SP_PORT from VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 1
08:48:40.588115 9930 IPA_Emulation.ttcnpp:899 Matching on port MTP3_SP_PORT succeeded:  matched
08:48:40.588225 9930 IPA_Emulation.ttcnpp:899 Receive operation on port MTP3_SP_PORT succeeded, message from VirtMSC-SCCP(11): @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 1
08:48:40.588332 9930 IPA_Emulation.ttcnpp:899 Message with id 1 was extracted from the queue of MTP3_SP_PORT.
08:48:40.588451 9930 IPA_Emulation.ttcnpp:902 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:40.588544 9930 IPA_Emulation.ttcnpp:902 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0013FD090003070B0443BB00FE0443B900FE03000131'O
}
08:48:40.589348 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:40.589587 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 19
08:48:40.594464 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:40.597615 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:40.599872 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:40.601636 9836 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:40.602878 9836 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with ? matched
08:48:40.603888 9836 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:40.603920 9836 Osmocom_VTY_Functions.ttcn:85 Message with id 18 was extracted from the queue of BSCVTY.
08:48:40.603946 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:40.603971 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:40.603987 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 19
08:48:40.604002 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 19 was extracted from the queue of BSCVTY.
08:48:40.604019 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:40.604039 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:40.604063 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:40.604115 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 20
08:48:40.604142 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:40.604164 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:40.604192 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:40.604207 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 20
08:48:40.604225 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
08:48:40.604240 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:40.604255 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:40.604276 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:40.604312 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 21
08:48:40.604334 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:40.604354 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:40.604379 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:40.604395 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 21
08:48:40.604411 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
08:48:40.604428 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:40.604458 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
08:48:40.604482 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:40.604508 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 22
08:48:40.604528 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:40.604547 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:40.604576 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:40.604590 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 22
08:48:40.604607 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 22 was extracted from the queue of BSCVTY.
08:48:40.604621 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:40.604637 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:40.604654 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:40.604678 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
08:48:40.604700 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:40.604722 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:40.604744 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:40.604759 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
08:48:40.604773 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
08:48:40.604788 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:40.604801 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:40.604820 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:40.604839 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 24
08:48:40.604860 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:40.604882 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:40.604896 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 24
08:48:40.604912 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 24 was extracted from the queue of BSCVTY.
08:48:40.604928 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:40.604946 9836 BSC_Tests.ttcn:1194 msc 1 is not configured, skipping
08:48:40.604971 9836 BSC_Tests.ttcn:1194 msc 2 is not configured, skipping
08:48:40.605008 9836 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:40.607769 9934 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:40.607856 9934 - TTCN-3 Parallel Test Component started on 5e318a98d888. Component reference: IPA-CTRL-CLI-IPA(14), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA. Version: 11.1.0.
08:48:40.607875 9934 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:40.607920 9934 - Connected to MC.
08:48:40.607934 9934 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:40.607951 9836 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 14, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:40.607973 9836 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(14):IPA_PORT to system:IPA_CODEC_PT.
08:48:40.609177 9934 - Port IPA_PORT was started.
08:48:40.609209 9934 - Port CFG_PORT was started.
08:48:40.609226 9934 - Port MTP3_SP_PORT was started.
08:48:40.609241 9934 - Port IPA_MGCP_PORT was started.
08:48:40.609256 9934 - Port IPA_RSL_PORT was started.
08:48:40.609270 9934 - Port IPA_OML_PORT was started.
08:48:40.609285 9934 - Port IPA_CTRL_PORT was started.
08:48:40.609301 9934 - Port IPA_SP_PORT was started.
08:48:40.609317 9934 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:40.609357 9934 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:40.609392 9836 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(14):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:40.609412 9836 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:40.609660 9836 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-da34f21f.
08:48:40.609693 9934 - Port IPA_CTRL_PORT has established the connection with mtc:IPA_CTRL using transport type UNIX.
08:48:40.609758 9836 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT.
08:48:40.609782 9836 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
08:48:40.609801 9836 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false) on component IPA-CTRL-CLI-IPA(14).
08:48:40.609844 9836 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
08:48:40.609863 9836 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
08:48:40.609984 9934 - Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false).
08:48:40.610229 9934 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :0 -> 127.0.0.1:4249 / TCP
08:48:40.611702 9934 IPA_Emulation.ttcnpp:409 Sent on IPA_CTRL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:40.611827 9836 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:40.611855 9836 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
08:48:40.611877 9836 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:40.611906 9836 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
08:48:40.611933 9836 BSC_Tests.ttcn:1076 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:40.616222 9935 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:40.616379 9935 - TTCN-3 Parallel Test Component started on 5e318a98d888. Component reference: VirtMGW-MGCP-0(15), component type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0. Version: 11.1.0.
08:48:40.616424 9935 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:40.616470 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 45607,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0029EE00545241502030206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O
} id 1
08:48:40.616525 9935 - Connected to MC.
08:48:40.616562 9935 - Initializing variables, timers and ports of component type MGCP_Emulation.MGCP_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:40.616580 9836 BSC_Tests.ttcn:1076 PTC was created. Component reference: 15, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:40.616623 9836 BSC_Tests.ttcn:1077 Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(15).
08:48:40.616723 9836 BSC_Tests.ttcn:1077 Function was started.
08:48:40.616761 9836 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:40.616804 9836 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.394023.
08:48:40.616856 9836 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:40.616902 9836 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:40.617066 9934 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '545241502030206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("TRAP 0 msc.0.connection_status connected")
} id 1
08:48:40.617161 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 45607,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0027EE00545241502030206D73635F636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O
} id 2
08:48:40.617222 9934 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '545241502030206D73635F636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("TRAP 0 msc_connection_status connected")
} id 2
08:48:40.617392 9934 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:40.617468 9934 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '545241502030206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("TRAP 0 msc.0.connection_status connected")
} id 1
08:48:40.617522 9934 IPA_Emulation.ttcnpp:790 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:40.618129 9934 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    trap := {
        variable := "msc.0.connection_status",
        val := "connected"
    }
}
08:48:40.618231 9934 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:40.618255 9836 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    trap := {
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 2
08:48:40.618392 9836 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL {
    trap := {
        variable := "msc.0.connection_status",
        val := "connected"
    }
} with {
    resp := {
        verb := "GET_REPLY",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := ?
    }
} unmatched: First message in the queue does not match the template: 
08:48:40.618454 9836 Osmocom_CTRL_Functions.ttcn:43 Matching on port IPA_CTRL succeeded:  matched
08:48:40.618501 9836 Osmocom_CTRL_Functions.ttcn:43 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    trap := {
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 2
08:48:40.618551 9836 Osmocom_CTRL_Functions.ttcn:43 Message with id 2 was extracted from the queue of IPA_CTRL.
08:48:40.618632 9934 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '545241502030206D73635F636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("TRAP 0 msc_connection_status connected")
} id 2
08:48:40.618686 9934 IPA_Emulation.ttcnpp:790 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:40.618745 9934 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    trap := {
        variable := "msc_connection_status",
        val := "connected"
    }
}
08:48:40.618797 9836 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    trap := {
        variable := "msc_connection_status",
        val := "connected"
    }
} id 3
08:48:40.618856 9836 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL {
    trap := {
        variable := "msc_connection_status",
        val := "connected"
    }
} with {
    resp := {
        verb := "GET_REPLY",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := ?
    }
} unmatched: First message in the queue does not match the template: 
08:48:40.618892 9836 Osmocom_CTRL_Functions.ttcn:43 Matching on port IPA_CTRL succeeded:  matched
08:48:40.618902 9935 - Port MGCP was started.
08:48:40.618937 9836 Osmocom_CTRL_Functions.ttcn:43 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    trap := {
        variable := "msc_connection_status",
        val := "connected"
    }
} id 3
08:48:40.618961 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:40.618967 9935 - Port MGCP_CLIENT was started.
08:48:40.618975 9836 Osmocom_CTRL_Functions.ttcn:43 Message with id 3 was extracted from the queue of IPA_CTRL.
08:48:40.619010 9935 - Port MGCP_CLIENT_MULTI was started.
08:48:40.619043 9935 - Port MGCP_PROC was started.
08:48:40.619075 9935 - Component type MGCP_Emulation.MGCP_Emulation_CT was initialized.
08:48:40.619164 9934 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:40.619236 9934 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:40.619240 9935 - Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0").
08:48:40.619309 9934 IPA_Emulation.ttcnpp:921 Message with id 1 was extracted from the queue of IPA_CTRL_PORT.
08:48:40.619812 9935 MGCP_Emulation.ttcn:279 Mapping port VirtMGW-MGCP-0(15):MGCP to system:MGCP_CODEC_PT.
08:48:40.619939 9935 MGCP_Emulation.ttcn:279 Port MGCP was mapped to system:MGCP_CODEC_PT.
08:48:40.620034 9935 MGCP_Emulation.ttcn:279 Map operation of VirtMGW-MGCP-0(15):MGCP to system:MGCP_CODEC_PT finished.
08:48:40.620320 9934 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420333934303233343731206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 394023471 bts.0.oml-connection-state")
}
08:48:40.620343 9935 MGCP_Emulation.ttcn:281 entering f__IPL4__PROVIDER__listen: 127.0.0.1:2427 / UDP
08:48:40.620652 9934 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420333934303233343731206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:40.620929 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 45607,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0038EE004745545F5245504C5920333934303233343731206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
} id 3
08:48:40.620997 9934 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920333934303233343731206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 394023471 bts.0.oml-connection-state degraded")
} id 3
08:48:40.621040 9934 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:40.621089 9934 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920333934303233343731206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 394023471 bts.0.oml-connection-state degraded")
} id 3
08:48:40.621130 9934 IPA_Emulation.ttcnpp:790 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:40.621241 9934 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
08:48:40.621305 9836 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 4
08:48:40.621353 9836 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:40.621396 9836 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "394023471",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 4
08:48:40.621435 9836 Osmocom_CTRL_Functions.ttcn:41 Message with id 4 was extracted from the queue of IPA_CTRL.
08:48:40.621473 9836 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:40.621515 9836 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:41.621580 9836 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:41.621780 9836 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:41.625366 9936 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:41.625563 9936 - TTCN-3 Parallel Test Component started on 5e318a98d888. Component reference: IPA-BTS0-TRX0-RSL-IPA(16), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA. Version: 11.1.0.
08:48:41.625692 9936 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:41.625855 9936 - Connected to MC.
08:48:41.625966 9936 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:41.625979 9836 BSC_Tests.ttcn:951 PTC was created. Component reference: 16, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:41.626046 9836 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: {
    site_id := 1234,
    bts_id := 0,
    trx_id := 0
}
08:48:41.626065 9836 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
08:48:41.626148 9836 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(16):IPA_PORT to system:IPA_CODEC_PT.
08:48:41.627429 9936 - Port IPA_PORT was started.
08:48:41.627472 9936 - Port CFG_PORT was started.
08:48:41.627485 9936 - Port MTP3_SP_PORT was started.
08:48:41.627497 9936 - Port IPA_MGCP_PORT was started.
08:48:41.627509 9936 - Port IPA_RSL_PORT was started.
08:48:41.627521 9936 - Port IPA_OML_PORT was started.
08:48:41.627532 9936 - Port IPA_CTRL_PORT was started.
08:48:41.627545 9936 - Port IPA_SP_PORT was started.
08:48:41.627556 9936 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:41.627600 9936 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:41.627627 9836 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(16):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:41.627645 9836 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
08:48:41.627897 9836 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-ca738b6e.
08:48:41.628003 9936 - Port CFG_PORT has established the connection with mtc:IPA_CFG_PORT[0][0] using transport type UNIX.
08:48:41.628118 9836 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT.
08:48:41.628203 9836 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
08:48:41.628216 9836 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
08:48:41.628326 9836 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-a969ab76.
08:48:41.628342 9936 - Port IPA_RSL_PORT has established the connection with mtc:IPA_RSL[0][0] using transport type UNIX.
08:48:41.628369 9836 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT.
08:48:41.628389 9836 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
08:48:41.628409 9836 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true) on component IPA-BTS0-TRX0-RSL-IPA(16).
08:48:41.628438 9836 BSC_Tests.ttcn:969 Function was started.
08:48:41.628449 9836 BSC_Tests.ttcn:976 Start timer T: 10 s
08:48:41.628566 9936 - Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true).
08:48:41.628781 9936 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :10000 -> 127.0.0.1:3003 / TCP
08:48:41.629946 9936 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:41.630068 9936 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:41.630217 9936 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:41.630569 9936 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:41.630645 9836 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:41.630667 9836 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:41.630682 9836 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:41.630706 9836 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(16): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:41.630735 9836 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
08:48:41.631325 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0011FE0401080107010201030104010501010100'O
} id 1
08:48:41.631452 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:41.631482 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:41.631501 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:41.631570 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:41.631598 9936 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:41.631614 9936 IPA_Emulation.ttcnpp:774 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:41.631682 9936 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
08:48:41.631939 9936 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
08:48:41.632019 9936 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:41.632039 9936 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:41.632080 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:41.632096 9936 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:41.632111 9936 IPA_Emulation.ttcnpp:774 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:41.632125 9936 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:41.632143 9936 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
}
08:48:41.632164 9836 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:41.632182 9836 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:41.632239 9836 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(16): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:41.632278 9836 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
08:48:41.632307 9836 BSC_Tests.ttcn:979 Stop timer T: 10 s
08:48:41.632337 9836 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:41.632367 9836 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.484451.
08:48:41.632403 9836 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "484451128",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:41.632440 9836 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:41.632462 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "484451128",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:41.632527 9934 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:41.632545 9934 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "484451128",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:41.632565 9934 IPA_Emulation.ttcnpp:921 Message with id 2 was extracted from the queue of IPA_CTRL_PORT.
08:48:41.632596 9934 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420343834343531313238206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 484451128 bts.0.oml-connection-state")
}
08:48:41.632622 9934 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420343834343531313238206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:41.632730 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:41.632750 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:41.632751 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 45607,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0039EE004745545F5245504C5920343834343531313238206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
} id 4
08:48:41.632777 9934 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920343834343531313238206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 484451128 bts.0.oml-connection-state connected")
} id 4
08:48:41.632791 9934 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.632804 9934 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920343834343531313238206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 484451128 bts.0.oml-connection-state connected")
} id 4
08:48:41.632815 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.632822 9934 IPA_Emulation.ttcnpp:790 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:41.632832 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.632845 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:41.632853 9934 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "484451128",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
08:48:41.632857 9936 IPA_Emulation.ttcnpp:790 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:41.632877 9836 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "484451128",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 5
08:48:41.632900 9836 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:41.632913 9836 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "484451128",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 5
08:48:41.632928 9836 Osmocom_CTRL_Functions.ttcn:41 Message with id 5 was extracted from the queue of IPA_CTRL.
08:48:41.632940 9836 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:41.632954 9836 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:41.634112 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
}
08:48:41.634275 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:41.634278 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
08:48:41.634297 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:41.634312 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0006000C1101801E0A'O
} id 5
08:48:41.634327 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:41.634342 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:41.634357 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:41.634371 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:41.634385 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:41.634400 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:41.634415 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:41.634429 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:41.634445 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:41.634460 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:41.634475 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:41.634490 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:41.634505 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:41.634519 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '000400101A1E0D'O
} id 12
08:48:41.634533 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:41.634548 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.634563 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.634577 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:41.634592 9936 IPA_Emulation.ttcnpp:790 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:41.634652 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
}
08:48:41.634673 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.634679 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
} id 4
08:48:41.634686 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.634697 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:41.634711 9936 IPA_Emulation.ttcnpp:790 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:41.634735 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
}
08:48:41.634750 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.634754 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
} id 5
08:48:41.634763 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.634777 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:41.634791 9936 IPA_Emulation.ttcnpp:790 Message with id 6 was extracted from the queue of IPA_PORT.
08:48:41.634815 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:41.634831 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.634836 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
} id 6
08:48:41.634844 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.634858 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:41.634873 9936 IPA_Emulation.ttcnpp:790 Message with id 7 was extracted from the queue of IPA_PORT.
08:48:41.634895 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:41.634910 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.634915 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 7
08:48:41.634924 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.634937 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:41.634950 9936 IPA_Emulation.ttcnpp:790 Message with id 8 was extracted from the queue of IPA_PORT.
08:48:41.634973 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
}
08:48:41.634989 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.634994 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
} id 8
08:48:41.635002 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.635016 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:41.635029 9936 IPA_Emulation.ttcnpp:790 Message with id 9 was extracted from the queue of IPA_PORT.
08:48:41.635049 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:41.635067 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.635072 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 9
08:48:41.635080 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.635094 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:41.635107 9936 IPA_Emulation.ttcnpp:790 Message with id 10 was extracted from the queue of IPA_PORT.
08:48:41.635128 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:41.635144 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.635149 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 10
08:48:41.635157 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.635171 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:41.635184 9936 IPA_Emulation.ttcnpp:790 Message with id 11 was extracted from the queue of IPA_PORT.
08:48:41.635249 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:41.635268 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.635273 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 11
08:48:41.635281 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.635294 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:41.635307 9936 IPA_Emulation.ttcnpp:790 Message with id 12 was extracted from the queue of IPA_PORT.
08:48:41.635325 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
}
08:48:41.635344 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
} id 12
08:48:41.635349 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:41.635365 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:41.635380 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001400101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:41.635394 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:41.635410 9936 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:41.635425 9936 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:41.635439 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.635452 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.635465 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:41.635478 9936 IPA_Emulation.ttcnpp:790 Message with id 13 was extracted from the queue of IPA_PORT.
08:48:41.635499 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:41.635514 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.635520 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 13
08:48:41.635527 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.635538 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:41.635551 9936 IPA_Emulation.ttcnpp:790 Message with id 14 was extracted from the queue of IPA_PORT.
08:48:41.635570 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
}
08:48:41.635587 9936 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:41.635601 9936 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:41.635608 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
} id 14
08:48:41.635615 9936 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:41.635630 9936 IPA_Emulation.ttcnpp:790 Message with id 15 was extracted from the queue of IPA_PORT.
08:48:41.635798 9936 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:41.635834 9836 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 15
08:48:42.633976 9836 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:42.634508 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:42.635002 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.635514 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 25
08:48:42.635802 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.636232 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.636702 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.637064 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 25
08:48:42.637421 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
08:48:42.637617 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.637709 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:48:42.637917 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.638256 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 26
08:48:42.638556 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.638692 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.638847 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.638953 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 26
08:48:42.639038 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
08:48:42.639132 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.639217 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:48:42.639332 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.639619 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:42.639779 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.639888 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.640017 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.640107 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:42.640182 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 27 was extracted from the queue of BSCVTY.
08:48:42.640291 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.640369 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:42.640474 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.640814 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:42.640925 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.641026 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.641150 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:42.641226 9836 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:42.641296 9836 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
08:48:42.641376 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.641448 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:42.641539 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.641784 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 29
08:48:42.641894 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.642022 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.642103 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 29
08:48:42.642176 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 29 was extracted from the queue of BSCVTY.
08:48:42.642255 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.642334 9836 Osmocom_VTY_Functions.ttcn:338 "TC_ctrl_msc0_connection_status() start"
08:48:42.642435 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_ctrl_msc0_connection_status() start"
08:48:42.642521 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.642873 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 30
08:48:42.643149 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.643367 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.643686 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 30
08:48:42.643921 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 30 was extracted from the queue of BSCVTY.
08:48:42.644198 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.644430 9836 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.133951.
08:48:42.644624 9836 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "133950738",
        variable := "msc.0.connection_status",
        val := omit
    }
}
08:48:42.644797 9836 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:42.644893 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "133950738",
        variable := "msc.0.connection_status",
        val := omit
    }
} id 3
08:48:42.645123 9934 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:42.645214 9934 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "133950738",
        variable := "msc.0.connection_status",
        val := omit
    }
} id 3
08:48:42.645290 9934 IPA_Emulation.ttcnpp:921 Message with id 3 was extracted from the queue of IPA_CTRL_PORT.
08:48:42.645420 9934 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420313333393530373338206D73632E302E636F6E6E656374696F6E5F737461747573'O ("GET 133950738 msc.0.connection_status")
}
08:48:42.645542 9934 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0026EE0047455420313333393530373338206D73632E302E636F6E6E656374696F6E5F737461747573'O
}
08:48:42.645991 9934 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 45607,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0036EE004745545F5245504C5920313333393530373338206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O
} id 5
08:48:42.646095 9934 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313333393530373338206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 133950738 msc.0.connection_status connected")
} id 5
08:48:42.646188 9934 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:42.646266 9934 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313333393530373338206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 133950738 msc.0.connection_status connected")
} id 5
08:48:42.646336 9934 IPA_Emulation.ttcnpp:790 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:42.646455 9934 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "133950738",
        variable := "msc.0.connection_status",
        val := "connected"
    }
}
08:48:42.646669 9836 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "133950738",
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 6
08:48:42.646987 9836 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:42.647250 9836 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "133950738",
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 6
08:48:42.647394 9836 Osmocom_CTRL_Functions.ttcn:41 Message with id 6 was extracted from the queue of IPA_CTRL.
08:48:42.647737 9836 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
08:48:42.647962 9836 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:42.649401 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1434657 bytes in 1306 blocks)" id 31
08:48:42.649477 9836 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
08:48:42.649634 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434657 bytes in 1306 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.649755 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434657 bytes in 1306 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:42.649866 9836 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434657 bytes in 1306 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:42.649946 9836 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434657 bytes in 1306 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:42.650020 9836 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1434657 bytes in 1306 blocks)" with ? matched
08:48:42.650089 9836 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1434657 bytes in 1306 blocks)" id 31
08:48:42.650158 9836 Osmocom_VTY_Functions.ttcn:85 Message with id 31 was extracted from the queue of BSCVTY.
08:48:42.650258 9836 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:42.650361 9836 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:42.650425 9836 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
08:48:42.650488 9836 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
08:48:42.650550 9836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:42.650618 9836 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
08:48:42.650698 9836 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
08:48:42.650776 9836 BSC_Tests.ttcn:888 Stopping all components.
08:48:42.650898 9928 StatsD_Checker.ttcnpp:143 Kill was requested from MC.
08:48:42.650919 9934 IPA_Emulation.ttcnpp:772 Kill was requested from MC.
08:48:42.650931 9929 SCCP_Emulation.ttcn:5519 Stop was requested from MC.
08:48:42.650968 9935 MGCP_Emulation.ttcn:301 Stop was requested from MC.
08:48:42.650982 9930 IPA_Emulation.ttcnpp:772 Stop was requested from MC.
08:48:42.650999 9934 IPA_Emulation.ttcnpp:772 Terminating test component execution.
08:48:42.651005 9928 StatsD_Checker.ttcnpp:143 Terminating test component execution.
08:48:42.651087 9930 IPA_Emulation.ttcnpp:772 Stopping test component execution.
08:48:42.651097 9936 IPA_Emulation.ttcnpp:772 Stop was requested from MC.
08:48:42.651160 9935 MGCP_Emulation.ttcn:301 Stopping test component execution.
08:48:42.651352 9936 IPA_Emulation.ttcnpp:772 Stopping test component execution.
08:48:42.651462 9929 SCCP_Emulation.ttcn:5519 Stopping test component execution.
08:48:42.652334 9928 - Function main was stopped. PTC terminates.
08:48:42.652362 9935 - Function main was stopped. PTC remains alive and is waiting for next start.
08:48:42.652414 9930 - Function main_server was stopped. PTC remains alive and is waiting for next start.
08:48:42.652420 9934 - Function main_client was stopped. PTC terminates.
08:48:42.652577 9928 - Terminating component type StatsD_Checker.StatsD_Checker_CT.
08:48:42.652606 9934 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:42.652666 9928 - Removing unterminated mapping between port STATSVTY and system:STATSVTY.
08:48:42.652670 9929 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
08:48:42.652678 9934 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:42.652897 9928 - Port STATSVTY was unmapped from system:STATSVTY.
08:48:42.652983 9928 - Port STATSVTY was stopped.
08:48:42.653050 9928 - Port STATSD_PROC was stopped.
08:48:42.653110 9928 - Removing unterminated mapping between port STATS and system:STATS.
08:48:42.653523 9936 - Function main_client was stopped. PTC remains alive and is waiting for next start.
08:48:42.653535 9934 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:42.653629 9934 - Port IPA_PORT was stopped.
08:48:42.653692 9934 - Port CFG_PORT was stopped.
08:48:42.653748 9934 - Port MTP3_SP_PORT was stopped.
08:48:42.653803 9934 - Port IPA_MGCP_PORT was stopped.
08:48:42.653858 9934 - Port IPA_RSL_PORT was stopped.
08:48:42.653911 9934 - Port IPA_OML_PORT was stopped.
08:48:42.653954 9928 - Port STATS was unmapped from system:STATS.
08:48:42.653967 9934 - Removing unterminated connection between port IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:42.654043 9928 - Port STATS was stopped.
08:48:42.654053 9934 - Port IPA_CTRL_PORT was stopped.
08:48:42.654077 9836 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT was closed unexpectedly by the peer.
08:48:42.654105 9928 - Component type StatsD_Checker.StatsD_Checker_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.654122 9934 - Port IPA_SP_PORT was stopped.
08:48:42.654179 9934 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.654187 9928 - Final verdict of PTC: none
08:48:42.654197 9836 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT.
08:48:42.654256 9934 - Final verdict of PTC: none
08:48:42.654341 9836 BSC_Tests.ttcn:888 All components were stopped.
08:48:42.654392 9928 - Disconnected from MC.
08:48:42.654459 9934 - Disconnected from MC.
08:48:42.654498 9836 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
08:48:42.654512 9928 - TTCN-3 Parallel Test Component finished.
08:48:42.654516 9934 - TTCN-3 Parallel Test Component finished.
08:48:42.654567 9836 BSC_Tests.ttcn:890 Stopping test component execution.
08:48:42.654797 9836 BSC_Tests.ttcn:3205 Test case TC_ctrl_msc0_connection_status was stopped.
08:48:42.654865 9836 BSC_Tests.ttcn:3205 Terminating component type BSC_Tests.test_CT.
08:48:42.654932 9836 BSC_Tests.ttcn:3205 Default with id 1 (altstep as_Tguard) was deactivated.
08:48:42.654999 9836 BSC_Tests.ttcn:3205 Stop timer T_guard: 30 s
08:48:42.655071 9836 BSC_Tests.ttcn:3205 Port IPA_CTRL was stopped.
08:48:42.655135 9836 BSC_Tests.ttcn:3205 Port RSL_CCHAN[0] was stopped.
08:48:42.655197 9836 BSC_Tests.ttcn:3205 Port RSL_CCHAN[1] was stopped.
08:48:42.655264 9836 BSC_Tests.ttcn:3205 Port RSL_CCHAN[2] was stopped.
08:48:42.655331 9836 BSC_Tests.ttcn:3205 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT.
08:48:42.655451 9836 BSC_Tests.ttcn:3205 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
08:48:42.655478 9936 - Connection of port IPA_RSL_PORT to mtc:IPA_RSL[0][0] was closed unexpectedly by the peer.
08:48:42.655686 9836 BSC_Tests.ttcn:3205 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
08:48:42.655812 9936 - Port IPA_RSL_PORT was disconnected from mtc:IPA_RSL[0][0].
08:48:42.655829 9836 BSC_Tests.ttcn:3205 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
08:48:42.655910 9836 BSC_Tests.ttcn:3205 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
08:48:42.655977 9836 BSC_Tests.ttcn:3205 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656040 9836 BSC_Tests.ttcn:3205 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656102 9836 BSC_Tests.ttcn:3205 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656164 9836 BSC_Tests.ttcn:3205 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656227 9836 BSC_Tests.ttcn:3205 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656288 9836 BSC_Tests.ttcn:3205 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656350 9836 BSC_Tests.ttcn:3205 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656412 9836 BSC_Tests.ttcn:3205 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656477 9836 BSC_Tests.ttcn:3205 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
08:48:42.656538 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[0][0] was stopped.
08:48:42.656598 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[0][1] was stopped.
08:48:42.656657 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[0][2] was stopped.
08:48:42.656716 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[0][3] was stopped.
08:48:42.656775 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[1][0] was stopped.
08:48:42.656835 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[1][1] was stopped.
08:48:42.656897 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[1][2] was stopped.
08:48:42.656956 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[1][3] was stopped.
08:48:42.657015 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[2][0] was stopped.
08:48:42.657074 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[2][1] was stopped.
08:48:42.657134 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[2][2] was stopped.
08:48:42.657192 9836 BSC_Tests.ttcn:3205 Port IPA_RSL[2][3] was stopped.
08:48:42.657253 9836 BSC_Tests.ttcn:3205 Port IPA was stopped.
08:48:42.657313 9836 BSC_Tests.ttcn:3205 Port SCCPLITE_IPA_CTRL was stopped.
08:48:42.657375 9836 BSC_Tests.ttcn:3205 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT.
08:48:42.657455 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[0][0] was stopped.
08:48:42.657538 9936 - Connection of port CFG_PORT to mtc:IPA_CFG_PORT[0][0] was closed unexpectedly by the peer.
08:48:42.657639 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[0][1] was stopped.
08:48:42.657704 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[0][2] was stopped.
08:48:42.657764 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[0][3] was stopped.
08:48:42.657805 9936 - Port CFG_PORT was disconnected from mtc:IPA_CFG_PORT[0][0].
08:48:42.657828 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[1][0] was stopped.
08:48:42.657908 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[1][1] was stopped.
08:48:42.657969 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[1][2] was stopped.
08:48:42.658029 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[1][3] was stopped.
08:48:42.658089 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[2][0] was stopped.
08:48:42.658148 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[2][1] was stopped.
08:48:42.658207 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[2][2] was stopped.
08:48:42.658265 9836 BSC_Tests.ttcn:3205 Port IPA_CFG_PORT[2][3] was stopped.
08:48:42.658324 9836 BSC_Tests.ttcn:3205 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
08:48:42.658446 9836 BSC_Tests.ttcn:3205 Port BSCVTY was unmapped from system:BSCVTY.
08:48:42.658516 9836 BSC_Tests.ttcn:3205 Port BSCVTY was stopped.
08:48:42.658576 9836 BSC_Tests.ttcn:3205 Port STPVTY was stopped.
08:48:42.658636 9836 BSC_Tests.ttcn:3205 Removing unterminated connection between port SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT.
08:48:42.658719 9836 BSC_Tests.ttcn:3205 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
08:48:42.658749 9930 - Connection of port CFG_PORT to mtc:SCCPLITE_IPA_CFG_PORT[0] was closed unexpectedly by the peer.
08:48:42.658861 9836 BSC_Tests.ttcn:3205 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
08:48:42.658904 9930 - Port CFG_PORT was disconnected from mtc:SCCPLITE_IPA_CFG_PORT[0].
08:48:42.658924 9836 BSC_Tests.ttcn:3205 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
08:48:42.658983 9836 BSC_Tests.ttcn:3205 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:42.659090 9836 BSC_Tests.ttcn:3205 Port BSSAP was stopped.
08:48:42.659105 9929 - Connection of port SCCP_SP_PORT to mtc:BSSAP was closed unexpectedly by the peer.
08:48:42.659345 9836 BSC_Tests.ttcn:3205 Port BSSAP_LE was stopped.
08:48:42.659360 9929 - Port SCCP_SP_PORT was disconnected from mtc:BSSAP.
08:48:42.659411 9836 BSC_Tests.ttcn:3205 Component type BSC_Tests.test_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.659483 9836 BSC_Tests.ttcn:3205 Waiting for PTCs to finish.
08:48:42.659609 9929 - Kill was requested from MC. Terminating idle PTC.
08:48:42.659628 9930 - Kill was requested from MC. Terminating idle PTC.
08:48:42.659675 9931 - Kill was requested from MC. Terminating idle PTC.
08:48:42.659689 9929 - Terminating component type SCCP_Emulation.SCCP_CT.
08:48:42.659696 9936 - Kill was requested from MC. Terminating idle PTC.
08:48:42.659742 9935 - Kill was requested from MC. Terminating idle PTC.
08:48:42.659757 9929 - Port SCCP_SP_PORT was stopped.
08:48:42.659830 9929 - Removing unterminated connection between port MTP3_SCCP_PORT and VirtMSC-IPA(12):MTP3_SP_PORT.
08:48:42.659837 9930 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:42.659897 9936 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:42.659914 9929 - Port MTP3_SCCP_PORT was stopped.
08:48:42.659967 9935 - Terminating component type MGCP_Emulation.MGCP_Emulation_CT.
08:48:42.659973 9930 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:42.660052 9929 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.660109 9931 - Terminating component type IPA_Emulation.IPA_EventWaiter_CT.
08:48:42.660111 9936 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:42.660120 9929 - Final verdict of PTC: none
08:48:42.660188 9935 - Removing unterminated mapping between port MGCP and system:MGCP_CODEC_PT.
08:48:42.660200 9931 - Port IPA_SP_PORT was stopped.
08:48:42.660394 9931 - Component type IPA_Emulation.IPA_EventWaiter_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.660537 9931 - Final verdict of PTC: pass
08:48:42.660749 9931 - Disconnected from MC.
08:48:42.660781 9929 - Disconnected from MC.
08:48:42.660929 9931 - TTCN-3 Parallel Test Component finished.
08:48:42.660940 9936 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:42.661034 9936 - Port IPA_PORT was stopped.
08:48:42.661080 9929 - TTCN-3 Parallel Test Component finished.
08:48:42.661103 9936 - Port CFG_PORT was stopped.
08:48:42.661165 9936 - Port MTP3_SP_PORT was stopped.
08:48:42.661244 9936 - Port IPA_MGCP_PORT was stopped.
08:48:42.661368 9936 - Port IPA_RSL_PORT was stopped.
08:48:42.661513 9936 - Port IPA_OML_PORT was stopped.
08:48:42.661812 9936 - Port IPA_CTRL_PORT was stopped.
08:48:42.661883 9936 - Port IPA_SP_PORT was stopped.
08:48:42.661995 9936 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.662043 9930 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:42.662089 9936 - Final verdict of PTC: none
08:48:42.662227 9930 - Port IPA_PORT was stopped.
08:48:42.662271 9935 - Port MGCP was unmapped from system:MGCP_CODEC_PT.
08:48:42.662311 9936 - Disconnected from MC.
08:48:42.662361 9930 - Port CFG_PORT was stopped.
08:48:42.662405 9936 - TTCN-3 Parallel Test Component finished.
08:48:42.662428 9935 - Port MGCP was stopped.
08:48:42.662526 9935 - Port MGCP_CLIENT was stopped.
08:48:42.662532 9930 - Removing unterminated connection between port MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT.
08:48:42.662677 9935 - Port MGCP_CLIENT_MULTI was stopped.
08:48:42.662744 9935 - Port MGCP_PROC was stopped.
08:48:42.662813 9930 - Port MTP3_SP_PORT was stopped.
08:48:42.662846 9935 - Component type MGCP_Emulation.MGCP_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.662933 9935 - Final verdict of PTC: none
08:48:42.662935 9930 - Port IPA_MGCP_PORT was stopped.
08:48:42.663039 9930 - Port IPA_RSL_PORT was stopped.
08:48:42.663182 9930 - Port IPA_OML_PORT was stopped.
08:48:42.663299 9935 - Disconnected from MC.
08:48:42.663589 9935 - TTCN-3 Parallel Test Component finished.
08:48:42.663758 9930 - Port IPA_CTRL_PORT was stopped.
08:48:42.663887 9930 - Port IPA_SP_PORT was stopped.
08:48:42.663964 9930 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:42.664058 9930 - Final verdict of PTC: none
08:48:42.664274 9930 - Disconnected from MC.
08:48:42.664322 9836 BSC_Tests.ttcn:3205 Setting final verdict of the test case.
08:48:42.664348 9930 - TTCN-3 Parallel Test Component finished.
08:48:42.664529 9836 BSC_Tests.ttcn:3205 Local verdict of MTC: pass
08:48:42.664649 9836 BSC_Tests.ttcn:3205 Local verdict of PTC VirtMSC-STATS(10): none (pass -> pass)
08:48:42.664817 9836 BSC_Tests.ttcn:3205 Local verdict of PTC VirtMSC-SCCP(11): none (pass -> pass)
08:48:42.664925 9836 BSC_Tests.ttcn:3205 Local verdict of PTC VirtMSC-IPA(12): none (pass -> pass)
08:48:42.665040 9836 BSC_Tests.ttcn:3205 Local verdict of PTC VirtMSC-IPA-WAIT(13): pass (pass -> pass)
08:48:42.665231 9836 BSC_Tests.ttcn:3205 Local verdict of PTC IPA-CTRL-CLI-IPA(14): none (pass -> pass)
08:48:42.665417 9836 BSC_Tests.ttcn:3205 Local verdict of PTC VirtMGW-MGCP-0(15): none (pass -> pass)
08:48:42.665521 9836 BSC_Tests.ttcn:3205 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(16): none (pass -> pass)
08:48:42.665650 9836 BSC_Tests.ttcn:3205 Test case TC_ctrl_msc0_connection_status finished. Verdict: pass
08:48:42.665768 9836 BSC_Tests.ttcn:3205 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc0_connection_status pass'.
08:48:47.919373 9836 BSC_Tests.ttcn:3205 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc0_connection_status pass' was executed successfully (exit status: 0).
08:48:47.919494 9836 BSC_Tests.ttcn:3400 Switching to log file `BSC_Tests-TC_stat_num_bts_connected_1-5e318a98d888-mtc-9836.log'
