module IPA_Emulation {

/* This module implements the IPA multiplex protocol on top of TCP, using the IPL4asp
 * test-port as provider.  It implements both client and server roles, as well was the CCM
 * handshake for establishing the identity of the client to the server.
 *
 * It already knows certain well-known sub-protocols such as A-bis RSL, MGCP and SCCP and
 * GSUP.  IT hence transcodes messages so the user can work with abstract data types rather
 * than binary messages.  It handles multiple packets inside one TCP segment.
 *
 * (C) 2017-2019 by Harald Welte <laforge@gnumonks.org>
 * contributions by sysmocom - s.f.m.c. GmbH
 * All rights reserved.
 *
 * Released under the terms of GNU General Public License, Version 2 or
 * (at your option) any later version.
 *
 * SPDX-License-Identifier: GPL-2.0-or-later
 */

import from IPA_Types all;
import from IPA_CodecPort all;
import from IPA_CodecPort_CtrlFunct all;
import from IPL4asp_Types all;
import from IPL4asp_PortType all;
import from Socket_API_Definitions all;

#ifdef IPA_EMULATION_SCCP
import from MTP3asp_Types all;
import from MTP3asp_PortType all;
#endif

#ifdef IPA_EMULATION_RSL
import from RSL_Types all;
#endif

#ifdef IPA_EMULATION_OML
import from AbisOML_Types all;
#endif

#ifdef IPA_EMULATION_MGCP
import from MGCP_Types all;
#endif

#ifdef IPA_EMULATION_GSUP
import from GSUP_Types all;
import from GSUP_Templates all;
#endif

#ifdef IPA_EMULATION_RSPRO
import from RSPRO all;
import from RSPRO_Types all;
#endif

#ifdef IPA_EMULATION_CTRL
import from Osmocom_CTRL_Types all;
#endif

#ifdef IPA_EMULATION_OSMO_PCU
import from PCUIF_Types all;
#endif

#ifdef IPA_EMULATION_TCAP_ROUTING
import from IPA_EXT_TCAP_ROUTING all;
#endif

modulepar {
	/* Use Osmocom extended IPA mux header */
	boolean mp_ipa_mgcp_uses_osmo_ext := true;
}

type enumerated IpaMode {
	IPA_MODE_CLIENT,
	IPA_MODE_SERVER
}

type enumerated IpaInitBehavior {
	IPA_INIT_SEND_IPA_ID_GET,
	IPA_INIT_SEND_IPA_ID_ACK
}

type record ASP_IPA_Unitdata {
	IpaStreamId	streamId,
	IpaExtStreamId	streamIdExt optional,
	octetstring	payload
}

type enumerated ASP_IPA_EventType {
	ASP_IPA_EVENT_DOWN,
	ASP_IPA_EVENT_UP,
	ASP_IPA_EVENT_ID_RESP,
	ASP_IPA_EVENT_ID_ACK
}

/* an event indicating us whether or not a connection is physically up or down,
 * and whether we have received an ID_RESP or ID_ACK */
type record ASP_IPA_Event {
	ASP_IPA_EventType	ev_type,
	integer			conn_id,

	/* Presence of these fields depends on event type */
	IpaCcmIdResp		id_resp optional  // ASP_IPA_EVENT_ID_RESP
}

template (value) ASP_IPA_Event ts_ASP_IPA_EV(ASP_IPA_EventType ev_type, integer conn_id,
					     template (omit) IpaCcmIdResp id_resp := omit) := {
	ev_type := ev_type,
	conn_id := conn_id,
	id_resp := id_resp
}

template ASP_IPA_Event tr_ASP_IPA_EV(template ASP_IPA_EventType ev_type,
				     template integer conn_id := ?,
				     template IpaCcmIdResp id_resp := *) := {
	ev_type := ev_type,
	conn_id := conn_id,
	id_resp := id_resp
}

template ASP_IPA_Unitdata t_ASP_IPA_UD(IpaStreamId sid, octetstring pl,
					template IpaExtStreamId esid := omit) := {
	streamId := sid,
	streamIdExt := esid,
	payload := pl
}

#ifdef IPA_EMULATION_RSL
/* like ASP_IPA_Unitdata, but with RSL_Message abstract type instead of octetstring */
type record ASP_RSL_Unitdata {
	integer		conn_id optional,
	IpaStreamId	streamId,
	RSL_Message	rsl
};

template (value) ASP_RSL_Unitdata ts_ASP_RSL_UD(template (value) RSL_Message rsl,
						IpaStreamId sid := IPAC_PROTO_RSL_TRX0,
						template (omit) integer conn_id := omit) := {
	conn_id := conn_id,
	streamId := sid,
	rsl := rsl
}

template ASP_RSL_Unitdata tr_ASP_RSL_UD(template (present) RSL_Message rsl,
					template IpaStreamId sid := IPAC_PROTO_RSL_TRX0,
					template integer conn_id := *) := {
	conn_id := conn_id,
	streamId := sid,
	rsl := rsl
}

template IpaStreamId t_IpaSidRSL := ( IPAC_PROTO_RSL_TRX0, IPAC_PROTO_RSL_TRX1,
				      IPAC_PROTO_RSL_TRX2, IPAC_PROTO_RSL_TRX3 );
#endif


/* Client port for general IPA messages, not further decoded */
type port IPA_SP_PT message {
	inout ASP_IPA_Unitdata, ASP_IPA_Event;
} with { extension "internal" }

#ifdef IPA_EMULATION_MGCP
/* Client port for MGCP inside IPA */
type port IPA_MGCP_PT message {
	inout MgcpCommand, MgcpResponse;
} with { extension "internal" }
#endif

#ifdef IPA_EMULATION_RSL
/* Client port for A-bis RSL inside IPA */
type port IPA_RSL_PT message {
	inout ASP_RSL_Unitdata, ASP_IPA_Event;
} with { extension "internal" }
#endif

#ifdef IPA_EMULATION_OML
/* Client port for A-bis OML inside IPA */
type port IPA_OML_PT message {
	inout OML_PDU, octetstring, ASP_IPA_Event;
} with { extension "internal" }
#endif

#ifdef IPA_EMULATION_CTRL
/* Client port for CTRL inside IPA */
type port IPA_CTRL_PT message {
	inout CtrlMessage, ASP_IPA_Event;
} with { extension "internal" }
#endif

#ifdef IPA_EMULATION_GSUP
/* Client port for CTRL inside IPA */
type port IPA_GSUP_PT message {
	inout GSUP_PDU, ASP_IPA_Event;
} with { extension "internal" }
#endif

#ifdef IPA_EMULATION_RSPRO
type port IPA_RSPRO_PT message {
	inout RsproPDU, ASP_IPA_Event;
} with { extension "internal" }
#endif

#ifdef IPA_EMULATION_OSMO_PCU
/* Client port for Osmocom PCU extension inside IPA */
type port IPA_OSMO_PCU_PT message {
	inout PCUIF_Message, ASP_IPA_Event;
} with { extension "internal" }
#endif

#ifdef IPA_EMULATION_TCAP_ROUTING
/* Client port for Osmocom PCU extension inside IPA */
type port IPA_TCAP_ROUTING_PT message {
	inout IPA_EXT_TCAP_ROUTING_Message, ASP_IPA_Event;
} with { extension "internal" }
#endif


type component IPA_Emulation_CT {
	/* down-facing port to IPA codec port */
	port IPA_CODEC_PT IPA_PORT;
	/* Down facing port to configure the component */
	port IPA_CFG_PT CFG_PORT;

#ifdef IPA_EMULATION_SCCP
	/* up-facing port to SCCP */
	port MTP3asp_SP_PT MTP3_SP_PORT;
#endif
#ifdef IPA_EMULATION_MGCP
	/* up-facing port for MGCP */
	port IPA_MGCP_PT IPA_MGCP_PORT;
#endif
#ifdef IPA_EMULATION_RSL
	/* up-facing port for RSL */
	port IPA_RSL_PT IPA_RSL_PORT;
#endif
#ifdef IPA_EMULATION_OML
	/* up-facing port for OML */
	port IPA_OML_PT IPA_OML_PORT;
#endif
#ifdef IPA_EMULATION_CTRL
	/* up-facing port for CTRL */
	port IPA_CTRL_PT IPA_CTRL_PORT;
#endif
#ifdef IPA_EMULATION_GSUP
	/* up-facing port for GSUP */
	port IPA_GSUP_PT IPA_GSUP_PORT;
#endif
#ifdef IPA_EMULATION_RSPRO
	/* up-facing port for RSPRO */
	port IPA_RSPRO_PT IPA_RSPRO_PORT;
#endif
#ifdef IPA_EMULATION_OSMO_PCU
	/* up-facing port for RSPRO */
	port IPA_OSMO_PCU_PT IPA_OSMO_PCU_PORT;
#endif
#ifdef IPA_EMULATION_TCAP_ROUTING
	/* up-facing port for RSPRO */
	port IPA_TCAP_ROUTING_PT IPA_TCAP_ROUTING_PORT;
#endif

	/* up-facing port for other streams */
	port IPA_SP_PT IPA_SP_PORT;

	var boolean g_initialized := false;
	/* Are we a BSC/MGW (truel) or MSC (false) */
	var boolean g_is_bsc_mgw;

	/* Connection identifier of the client / server itself */
	var IPL4asp_Types.ConnectionId g_self_conn_id := -1;
	/* Connection identifier of the last connected client (server only) */
	var IPL4asp_Types.ConnectionId g_last_conn_id := -1;

	var IpaMode g_mode;
	var boolean g_ccm_enabled;
	var IpaInitBehavior g_init_behavior;
	/* Shall we stop the component once the client disconnects, or keep
	 * running to let next user in ? */
	var boolean g_server_stop_on_ipa_ev_down := true;
	var IPA_CCM_Parameters	g_ccm_pars := c_IPA_default_ccm_pars;
}

type record IPA_CCM_Parameters {
	charstring	ser_nr optional,
	charstring	name optional,
	charstring	location1 optional,
	charstring	location2 optional,
	charstring	equip_version optional,
	charstring	sw_version optional,
	charstring	ip_addr optional,
	charstring	mac_addr optional,
	charstring	unit_id optional,
	charstring	osmo_rand optional
}

const IPA_CCM_Parameters c_IPA_default_ccm_pars := {
	ser_nr := "",
	name := "mahlzeit",
	location1 := "",
	location2 := "",
	equip_version := "",
	sw_version := "",
	ip_addr := "",
	mac_addr := "",
	unit_id := "0/1/2",
	osmo_rand := ""
};

signature IPA_CFG_disconnect(inout IPL4asp_Types.Result res);
signature IPA_CFG_chg_ccm_enabled(in boolean res);
type port IPA_CFG_PT procedure {
	inout IPA_CFG_disconnect;
	inout IPA_CFG_chg_ccm_enabled;
} with { extension "internal" };

function f_ipa_cfg_disconnect(IPA_CFG_PT pt, inout IPL4asp_Types.Result res) {
	pt.call(IPA_CFG_disconnect:{res}) {
		[] pt.getreply(IPA_CFG_disconnect:{?}) -> param (res) {};
	}
}
function f_ipa_cfg_chg_ccm_enabled(IPA_CFG_PT pt, boolean ccm_enabled) {
	pt.call(IPA_CFG_chg_ccm_enabled:{ccm_enabled}) {
		[] pt.getreply(IPA_CFG_chg_ccm_enabled:{ccm_enabled});
	}
}

/* Function to use to connect as client to a remote IPA Server */
function f_connect(charstring remote_host, IPL4asp_Types.PortNumber remote_port,
		   charstring local_host, IPL4asp_Types.PortNumber local_port,
		   IPA_CCM_Parameters ccm_pars := c_IPA_default_ccm_pars) runs on IPA_Emulation_CT {
	var IPL4asp_Types.Result res;
	res := IPA_CodecPort_CtrlFunct.f_IPL4_connect(IPA_PORT, remote_host, remote_port,
						local_host, local_port, 0, { tcp:={} });
	if (not ispresent(res.connId)) {
		setverdict(fail, "Could not connect IPA socket from ", local_host, " port ", local_port,
			   " to ", remote_host, " port ", remote_port, "; check your configuration");
		mtc.stop;
	}
	g_self_conn_id := res.connId;
	g_ccm_pars := ccm_pars;
	g_is_bsc_mgw := true;
}

/* Function to use to bind to a local port as IPA server, accepting remote clients */
function f_bind(charstring local_host, IPL4asp_Types.PortNumber local_port,
		IPA_CCM_Parameters ccm_pars := c_IPA_default_ccm_pars) runs on IPA_Emulation_CT {
	var IPL4asp_Types.Result res;
	res := IPA_CodecPort_CtrlFunct.f_IPL4_listen(IPA_PORT,
						local_host, local_port, { tcp:={} });
	if (not ispresent(res.connId)) {
		setverdict(fail, "Could not listen IPA socket ", local_host, ":", local_port, ", check your configuration");
		mtc.stop;
	}
	g_self_conn_id := res.connId;
	g_ccm_pars := ccm_pars;
	g_is_bsc_mgw := false;
}

private function f_close() runs on IPA_Emulation_CT return IPL4asp_Types.Result {
	var IPL4asp_Types.Result res;
	select (g_mode) {
	case (IPA_MODE_CLIENT) {
		res := IPA_CodecPort_CtrlFunct.f_IPL4_close(IPA_PORT, g_self_conn_id, {tcp := {}});
		g_self_conn_id := -1;
	}
	case (IPA_MODE_SERVER) {
		res := IPA_CodecPort_CtrlFunct.f_IPL4_close(IPA_PORT, g_last_conn_id, {tcp := {}});
		g_last_conn_id := -1;
	}
	case else {
		setverdict(fail, "Unknown mode");
		mtc.stop;
		}
	}
	return res;
}

#ifdef IPA_EMULATION_SCCP
template ASP_MTP3_TRANSFERind ts_MTP3_XFER_ind(integer opc, octetstring data) := {
	sio := { '10'B, '00'B, '0011'B },
	opc := opc,
	dpc := 0,
	sls := 0,
	data := data
}
#endif


private template IpaCcmRespPart t_IdRespPart(IpaCcmIdTag tag, charstring payload) := {
	len := 0,	/* overwritten by codec */
	tag := tag,
	data := char2oct(payload) & '00'O
}

private function f_send_IPA_EVT(template (value) ASP_IPA_Event evt) runs on IPA_Emulation_CT {
	if (IPA_SP_PORT.checkstate("Connected")) {
		IPA_SP_PORT.send(evt);
	}
#ifdef IPA_EMULATION_RSL
	if (IPA_RSL_PORT.checkstate("Connected")) {
		IPA_RSL_PORT.send(evt);
	}
#endif
#ifdef IPA_EMULATION_OML
	if (IPA_OML_PORT.checkstate("Connected")) {
		IPA_OML_PORT.send(evt);
	}
#endif
#ifdef IPA_EMULATION_CTRL
	if (IPA_CTRL_PORT.checkstate("Connected")) {
		IPA_CTRL_PORT.send(evt);
	}
#endif
#ifdef IPA_EMULATION_GSUP
	if (IPA_GSUP_PORT.checkstate("Connected")) {
		IPA_GSUP_PORT.send(evt);
	}
#endif
#ifdef IPA_EMULATION_RSPRO
	if (IPA_RSPRO_PORT.checkstate("Connected")) {
		IPA_RSPRO_PORT.send(evt);
	}
#endif
#ifdef IPA_EMULATION_OSMO_PCU
	if (IPA_OSMO_PCU_PORT.checkstate("Connected")) {
		IPA_OSMO_PCU_PORT.send(evt);
	}
#endif
#ifdef IPA_EMULATION_TCAP_ROUTING
	if (IPA_TCAP_ROUTING_PORT.checkstate("Connected")) {
		IPA_TCAP_ROUTING_PORT.send(evt);
	}
#endif
	/* FIXME: to other ports */
}

/* build IPA CCM ID RESP response from IPA CCM GET */
private function f_ccm_make_id_resp(PDU_IPA_CCM get) runs on IPA_Emulation_CT return PDU_IPA_CCM {
	var integer i;
	var PDU_IPA_CCM resp := {
		msg_type := IPAC_MSGT_ID_RESP,
		u := {
			resp := {}
		}
	}

	/* If no Tags were present in the received IPA message, .u = omit */
	if (not ispresent(get.u)) {
		return resp;
	}

	for (i := 0; i < sizeof(get.u.get); i := i + 1) {
		var IpaCcmIdTag tag := get.u.get[i].tag;
		var charstring foo;
		select (tag) {
			case (IPAC_IDTAG_SERNR) {
				foo := g_ccm_pars.ser_nr;
			}
			case (IPAC_IDTAG_UNITNAME) {
				foo := g_ccm_pars.name;
			}
			case (IPAC_IDTAG_LOCATION1) {
				foo := g_ccm_pars.location1;
			}
			case (IPAC_IDTAG_LOCATION2) {
				foo := g_ccm_pars.location2;
			}
			case (IPAC_IDTAG_EQUIPVERS) {
				foo := g_ccm_pars.equip_version;
			}
			case (IPAC_IDTAG_SWVERSION) {
				foo := g_ccm_pars.sw_version;
			}
			case (IPAC_IDTAG_IPADDR) {
				foo := g_ccm_pars.ip_addr;
			}
			case (IPAC_IDTAG_MACADDR) {
				foo := g_ccm_pars.mac_addr;
			}
			case (IPAC_IDTAG_UNITID) {
				foo := g_ccm_pars.unit_id;
			}
			case (IPAC_IDTAG_OSMO_RAND) {
				foo := g_ccm_pars.osmo_rand;
			}
			case else {
				foo := "unknown";
			}
		}
		resp.u.resp[sizeof(resp.u.resp)] := valueof(t_IdRespPart(tag, foo));
	}

	return resp;
}

/* transmit IPA CCM message */
private function f_ccm_tx(PDU_IPA_CCM ccm, IPL4asp_Types.ConnectionId conn_id)
runs on IPA_Emulation_CT {
	var IPA_Send ipa_tx := valueof(t_IPA_Send(conn_id, IPAC_PROTO_CCM, enc_PDU_IPA_CCM(ccm)));
	log("CCM Tx:", ccm);
	IPA_PORT.send(ipa_tx);
}

template PDU_IPA_CCM ts_IPA_PONG := {
	msg_type := IPAC_MSGT_PONG,
	u := omit
}

template PDU_IPA_CCM ts_IPA_ACK := {
	msg_type := IPAC_MSGT_ID_ACK,
	u := omit
}

template PDU_IPA_CCM ts_IPA_ID_GET := {
	msg_type := IPAC_MSGT_ID_GET,
	u := {
		get := {
			{ 1, IPAC_IDTAG_UNITNAME },
			{ 1, IPAC_IDTAG_UNITID }
		}
	}
}

template PDU_IPA_CCM tr_IPA_ID_RESP := {
	msg_type := IPAC_MSGT_ID_RESP,
	u := {
		resp := {
			{ ?, IPAC_IDTAG_UNITNAME, ? },
			{ ?, IPAC_IDTAG_UNITID, ? }
		}
	}
}

/* receive IPA CCM message */
private function f_ccm_rx_client(PDU_IPA_CCM ccm) runs on IPA_Emulation_CT {
	select (ccm.msg_type) {
		case (IPAC_MSGT_PING) {
			f_ccm_tx(valueof(ts_IPA_PONG), g_self_conn_id);
		}
		case (IPAC_MSGT_ID_ACK) {
			f_send_IPA_EVT(ts_ASP_IPA_EV(ASP_IPA_EVENT_ID_ACK, g_self_conn_id));
		}
		case (IPAC_MSGT_ID_GET) {
			f_ccm_tx(f_ccm_make_id_resp(ccm), g_self_conn_id);
		}
		case else {
			log("Unknown/unsupported IPA CCM message type", ccm);
		}
	}
}

private function f_ccm_rx_server(PDU_IPA_CCM ccm, IPL4asp_Types.ConnectionId conn_id)
runs on IPA_Emulation_CT {
	select (ccm.msg_type) {
		case (IPAC_MSGT_PING) {
			f_ccm_tx(valueof(ts_IPA_PONG), conn_id);
		}
		case (IPAC_MSGT_ID_ACK) {
			/* the IPA server should at some point receive an ID_ACK from the client,
			 * in case of RSL/OML from nanoBTS, this is actually the first message after
			 * the TCP connection is established.  Other implementations may differ.
			 * We currently ignore it completely - but actually we should make sure that
			 * one ID_ACK is received by the server at some point */
			f_send_IPA_EVT(ts_ASP_IPA_EV(ASP_IPA_EVENT_ID_ACK, conn_id));
		}
		case (IPAC_MSGT_ID_RESP) {
			log("IPA ID RESP: ", ccm.u.resp);

			/* make sure that the response contains all fields we requested */
			if (not match(ccm, tr_IPA_ID_RESP)) {
				log("IPA identity response ", ccm.u.resp, " mismatch");
				return;
			}

			/* forward to the upper layers, so they can map conn_id with unit_id */
			f_send_IPA_EVT(ts_ASP_IPA_EV(ASP_IPA_EVENT_ID_RESP, conn_id, ccm.u.resp));
			/* acknowledge any identity that the client may have sent */
			f_ccm_tx(valueof(ts_IPA_ACK), conn_id);
		}
		case else {
			log("Unknown/unsupported IPA CCM message type", ccm);
		}
	}
}

private function f_to_asp(IPA_RecvFrom ipa_rx) return ASP_IPA_Unitdata {
	var ASP_IPA_Unitdata ret := {
		streamId := ipa_rx.streamId,
		streamIdExt := ipa_rx.streamIdExt,
		payload := ipa_rx.msg
	}
	return ret;
}

private function f_from_asp(IPL4asp_Types.ConnectionId connId, ASP_IPA_Unitdata ipa_tx) return IPA_Send {
	var IPA_Send ret := valueof(t_IPA_Send(connId, ipa_tx.streamId, ipa_tx.payload,
						ipa_tx.streamIdExt));
	return ret;
}

#ifdef IPA_EMULATION_RSL
private function f_from_rsl(IPL4asp_Types.ConnectionId connId, ASP_RSL_Unitdata rsl_tx) return IPA_Send {
	var octetstring payload := enc_RSL_Message(rsl_tx.rsl);

	/* ASP_RSL_Unitdata may (optionally) contain TCP/IP connection ID */
	if (rsl_tx.conn_id != omit) {
		connId := rsl_tx.conn_id;
	}

	return valueof(t_IPA_Send(connId, rsl_tx.streamId, payload));
}
#endif

#ifdef IPA_EMULATION_OML
private function f_from_oml(IPL4asp_Types.ConnectionId connId, OML_PDU oml_tx) return IPA_Send {
	var octetstring payload := enc_OML_PDU(oml_tx);
	var IPA_Send ret := valueof(t_IPA_Send(connId, IPAC_PROTO_OML, payload));
	return ret;
}
#endif

/* main function to use for a client-side IPA implementation */
function main_client(charstring remote_host, IPL4asp_Types.PortNumber remote_port,
		     charstring local_host, IPL4asp_Types.PortNumber local_port,
		     IPA_CCM_Parameters ccm_pars := c_IPA_default_ccm_pars,
		     boolean ccm_enabled := true) runs on IPA_Emulation_CT {
	g_mode := IPA_MODE_CLIENT;
	g_ccm_enabled := ccm_enabled;
	f_connect(remote_host, remote_port, local_host, local_port, ccm_pars);
	if (g_ccm_enabled) {
		/* we're a client: Send ID_ACK immediately after connect */
		f_ccm_tx(valueof(ts_IPA_ACK), g_self_conn_id);
	}
	f_send_IPA_EVT(ts_ASP_IPA_EV(ASP_IPA_EVENT_UP, g_self_conn_id));
	ScanEvents();
}

/* main function to use for a server-side IPA implementation */
function main_server(charstring local_host, IPL4asp_Types.PortNumber local_port,
		     boolean ccm_enabled := true,
		     IpaInitBehavior init_behavior := IPA_INIT_SEND_IPA_ID_GET,
		     boolean server_stop_on_ipa_ev_down := true)
runs on IPA_Emulation_CT {
	g_mode := IPA_MODE_SERVER;
	g_ccm_enabled := ccm_enabled;
	g_init_behavior := init_behavior;
	g_server_stop_on_ipa_ev_down := server_stop_on_ipa_ev_down;
	f_bind(local_host, local_port);
	ScanEvents();
}

#ifdef IPA_EMULATION_CTRL
private function f_ctrl_to_user(octetstring msg) runs on IPA_Emulation_CT {
	var charstring msg_ch := oct2char(msg);
	IPA_CTRL_PORT.send(dec_CtrlMessage(msg_ch));
}
#endif

#ifdef IPA_EMULATION_GSUP
private function f_gsup_to_user(octetstring msg) runs on IPA_Emulation_CT {
	var GSUP_PDU gsup := dec_GSUP_PDU(msg);
	f_gsup_postprocess_decoded(gsup);
	IPA_GSUP_PORT.send(gsup);
}
#endif

#ifdef IPA_EMULATION_RSPRO
private function f_rspro_to_user(octetstring msg) runs on IPA_Emulation_CT {
	var RsproPDU rspro := dec_RsproPDU(msg);
	IPA_RSPRO_PORT.send(rspro);
}
#endif

#ifdef IPA_EMULATION_OSMO_PCU
private function f_osmo_pcu_to_user(octetstring msg) runs on IPA_Emulation_CT {
	var PCUIF_Message pcuif_msg := dec_PCUIF_Message(msg);
	IPA_OSMO_PCU_PORT.send(pcuif_msg);
}
#endif

#ifdef IPA_EMULATION_TCAP_ROUTING
private function f_tcap_routing_to_user(octetstring msg) runs on IPA_Emulation_CT {
	var IPA_EXT_TCAP_ROUTING_Message pcuif_msg := dec_IPA_EXT_TCAP_ROUTING_Message(msg);
	IPA_TCAP_ROUTING_PORT.send(pcuif_msg);
}
#endif

#ifdef IPA_EMULATION_MGCP
private function f_mgcp_to_user(octetstring msg) runs on IPA_Emulation_CT {
	var charstring msg_ch := oct2char(msg);
	if (g_is_bsc_mgw) {
		log("============");
		log(msg_ch);
		IPA_MGCP_PORT.send(dec_MgcpCommand(msg_ch));
	} else {
		IPA_MGCP_PORT.send(dec_MgcpResponse(msg_ch));
	}
}

private function f_mgcp_to_ud(octetstring payload) runs on IPA_Emulation_CT return ASP_IPA_Unitdata {
	if (mp_ipa_mgcp_uses_osmo_ext) {
		return valueof(t_ASP_IPA_UD(IPAC_PROTO_MGCP_OLD, payload));
	} else {
		return valueof(t_ASP_IPA_UD(IPAC_PROTO_OSMO, payload, IPAC_PROTO_EXT_MGCP));
	}
}
#endif

/* Resolve TCP/IP connection identifier depending on g_mode */
private function f_ipa_conn_id() runs on IPA_Emulation_CT
return IPL4asp_Types.ConnectionId {
	var IPL4asp_Types.ConnectionId conn_id;

	select (g_mode) {
	case (IPA_MODE_CLIENT) { conn_id := g_self_conn_id; }
	case (IPA_MODE_SERVER) { conn_id := g_last_conn_id; }
	case else {
		setverdict(fail, "Unknown mode");
		mtc.stop;
		}
	}

	if (conn_id == -1) { /* Just to be sure */
		setverdict(fail, "Connection is not established");
		mtc.stop;
	}

	return conn_id;
}

/* main loop function for both client and server. 'thread' of the component */
private function ScanEvents() runs on IPA_Emulation_CT {
	var IPA_RecvFrom ipa_rx;
	var ASP_Event asp_evt;
	var Socket_API_Definitions.PortEvent port_evt;
	var octetstring payload;
	var ASP_IPA_Unitdata ipa_ud;
	var IPL4asp_Types.Result res;
	var boolean cfg_chg_ccm_enabled;
#ifdef IPA_EMULATION_CTRL
	var CtrlMessage ctrl_msg;
#endif
#ifdef IPA_EMULATION_SCCP
	var ASP_MTP3_TRANSFERreq mtp_req;
#endif
#ifdef IPA_EMULATION_MGCP
	var MgcpCommand mgcp_cmd;
	var MgcpResponse mgcp_rsp;
#endif
#ifdef IPA_EMULATION_GSUP
	var GSUP_PDU gsup_msg;
#endif
#ifdef IPA_EMULATION_RSL
	var ASP_RSL_Unitdata rsl;
#endif
#ifdef IPA_EMULATION_OML
	var OML_PDU oml;
#endif
#ifdef IPA_EMULATION_RSPRO
	var RsproPDU rspro;
#endif
#ifdef IPA_EMULATION_OSMO_PCU
	var PCUIF_Message pcu;
#endif
#ifdef IPA_EMULATION_TCAP_ROUTING
	var IPA_EXT_TCAP_ROUTING_Message tcap_routing;
#endif

	/* Set function for dissecting the binary */
	var f_IPL4_getMsgLen vl_f := refers(f_IPL4_fixedMsgLen);
	IPA_CodecPort_CtrlFunct.f_IPL4_setGetMsgLen(IPA_PORT, g_self_conn_id, vl_f, {0, 2, 3, 1, 0});

	while (true) {
		alt {
		/* Received IPA -> up into SCCP stack */
		[g_ccm_enabled] IPA_PORT.receive(IPA_RecvFrom:{?,IPAC_PROTO_CCM,omit,?}) -> value ipa_rx {
			var PDU_IPA_CCM ccm := dec_PDU_IPA_CCM(ipa_rx.msg);
			log("CCM Rx:", ccm);
			select (g_mode) {
				case (IPA_MODE_CLIENT) {
					f_ccm_rx_client(ccm);
				}
				case (IPA_MODE_SERVER) {
					f_ccm_rx_server(ccm, ipa_rx.connId);
				}
				case else {
					setverdict(fail, "Unknown mode");
					mtc.stop;
				}
			}
			}
		[] IPA_PORT.receive(IPA_RecvFrom:?) -> value ipa_rx {
			select (ipa_rx.streamId) {
#ifdef IPA_EMULATION_SCCP
			case (IPAC_PROTO_SCCP) {
				var ASP_MTP3_TRANSFERind mtp;
				mtp := valueof(ts_MTP3_XFER_ind(0, ipa_rx.msg));
				MTP3_SP_PORT.send(mtp);
			}
#endif
#ifdef IPA_EMULATION_MGCP
			case (IPAC_PROTO_MGCP_OLD) {
				f_mgcp_to_user(ipa_rx.msg);
			}
#endif
#ifdef IPA_EMULATION_RSL
			case (t_IpaSidRSL) {
				rsl := valueof(ts_ASP_RSL_UD(
					rsl := dec_RSL_Message(ipa_rx.msg),
					sid := ipa_rx.streamId,
					conn_id := ipa_rx.connId
				));
				IPA_RSL_PORT.send(rsl);
			}
#endif
#ifdef IPA_EMULATION_OML
			case (IPAC_PROTO_OML) {
				oml := dec_OML_PDU(ipa_rx.msg)
				IPA_OML_PORT.send(oml);
			}
#endif
			case (IPAC_PROTO_OSMO) {
				select (ipa_rx.streamIdExt) {
#ifdef IPA_EMULATION_MGCP
					case (IPAC_PROTO_EXT_MGCP) {
						f_mgcp_to_user(ipa_rx.msg);
					}
#endif
#ifdef IPA_EMULATION_CTRL
					case (IPAC_PROTO_EXT_CTRL) {
						f_ctrl_to_user(ipa_rx.msg);
					}
#endif
#ifdef IPA_EMULATION_GSUP
					case (IPAC_PROTO_EXT_GSUP) {
						f_gsup_to_user(ipa_rx.msg);
					}
#endif
#ifdef IPA_EMULATION_RSPRO
					case (IPAC_PROTO_EXT_RSPRO) {
						f_rspro_to_user(ipa_rx.msg);
					}
#endif
#ifdef IPA_EMULATION_OSMO_PCU
					case (IPAC_PROTO_EXT_OSMO_PCU) {
						f_osmo_pcu_to_user(ipa_rx.msg);
					}
#endif
#ifdef IPA_EMULATION_TCAP_ROUTING
					case (IPAC_PROTO_EXT_TCAP_ROUTING) {
						f_tcap_routing_to_user(ipa_rx.msg);
					}
#endif
					case else {
						IPA_SP_PORT.send(f_to_asp(ipa_rx));
					}
				}
			}
			case else {
				IPA_SP_PORT.send(f_to_asp(ipa_rx));
				}
			}
		}

		/* server only */
		[] IPA_PORT.receive(ASP_Event:{connOpened:=?}) -> value asp_evt {
			g_last_conn_id := asp_evt.connOpened.connId;
			log("Established a new IPA connection (conn_id=", g_last_conn_id, ")");

			f_send_IPA_EVT(ts_ASP_IPA_EV(ASP_IPA_EVENT_UP, g_last_conn_id));
			if (g_mode == IPA_MODE_SERVER and g_ccm_enabled) {
				select (g_init_behavior) {
					case (IPA_INIT_SEND_IPA_ID_GET) {
						f_ccm_tx(valueof(ts_IPA_ID_GET), g_last_conn_id);
					}
					case (IPA_INIT_SEND_IPA_ID_ACK) {
						f_ccm_tx(valueof(ts_IPA_ACK), g_last_conn_id);
					}
				}
			}
		}

		[] IPA_PORT.receive(ASP_Event:{connClosed:=?}) -> value asp_evt {
			log("IPA: Closed");
			g_self_conn_id := -1;
			f_send_IPA_EVT(ts_ASP_IPA_EV(ASP_IPA_EVENT_DOWN, asp_evt.connClosed.connId));
			if (g_mode != IPA_MODE_SERVER or g_server_stop_on_ipa_ev_down) {
				self.stop;
			}
		}

		[] IPA_PORT.receive(Socket_API_Definitions.PortEvent:{result:={errorCode:=ERROR_SOCKET, connId:=?, os_error_code:=?, os_error_text:=?}}) -> value port_evt {
			log("PortEvent: ERROR_SOCKET: ", port_evt);
			g_self_conn_id := -1;
			f_send_IPA_EVT(ts_ASP_IPA_EV(ASP_IPA_EVENT_DOWN, port_evt.result.connId));
			self.stop;
		}

#ifdef IPA_EMULATION_SCCP
		/* Received SCCP -> down into IPA */
		[] MTP3_SP_PORT.receive(ASP_MTP3_TRANSFERreq: ?) -> value mtp_req {
			var IPA_Send ipa_tx := valueof(t_IPA_Send(f_ipa_conn_id(), IPAC_PROTO_SCCP,
							mtp_req.data));
			IPA_PORT.send(ipa_tx);
		}
#endif

#ifdef IPA_EMULATION_MGCP
		/* Received MGCP -> down into IPA */
		[] IPA_MGCP_PORT.receive(MgcpCommand:?) -> value mgcp_cmd {
			payload := char2oct(enc_MgcpCommand(mgcp_cmd));
			ipa_ud := f_mgcp_to_ud(payload);
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}
		[] IPA_MGCP_PORT.receive(MgcpResponse:?) -> value mgcp_rsp {
			payload := char2oct(enc_MgcpResponse(mgcp_rsp));
			ipa_ud := f_mgcp_to_ud(payload);
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}
#endif

#ifdef IPA_EMULATION_CTRL
		[] IPA_CTRL_PORT.receive(CtrlMessage:?) -> value ctrl_msg {
			payload := char2oct(enc_CtrlMessage(ctrl_msg));
			ipa_ud := valueof(t_ASP_IPA_UD(IPAC_PROTO_OSMO, payload, IPAC_PROTO_EXT_CTRL));
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}
#endif

#ifdef IPA_EMULATION_GSUP
		[] IPA_GSUP_PORT.receive(GSUP_PDU:?) -> value gsup_msg {
			f_gsup_preprocess_encoded(gsup_msg);
			payload := enc_GSUP_PDU(gsup_msg);
			ipa_ud := valueof(t_ASP_IPA_UD(IPAC_PROTO_OSMO, payload, IPAC_PROTO_EXT_GSUP));
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}
#endif

#ifdef IPA_EMULATION_RSPRO
		[] IPA_RSPRO_PORT.receive(RsproPDU:?) -> value rspro {
			payload := enc_RsproPDU(rspro);
			ipa_ud := valueof(t_ASP_IPA_UD(IPAC_PROTO_OSMO, payload, IPAC_PROTO_EXT_RSPRO));
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}
#endif

#ifdef IPA_EMULATION_OSMO_PCU
		[] IPA_OSMO_PCU_PORT.receive(PCUIF_Message:?) -> value pcu {
			payload := enc_PCUIF_Message(pcu);
			ipa_ud := valueof(t_ASP_IPA_UD(IPAC_PROTO_OSMO, payload, IPAC_PROTO_EXT_OSMO_PCU));
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}
#endif

#ifdef IPA_EMULATION_TCAP_ROUTING
		[] IPA_TCAP_ROUTING_PORT.receive(IPA_EXT_TCAP_ROUTING_Message:?) -> value tcap_routing {
			payload := enc_IPA_EXT_TCAP_ROUTING_Message(tcap_routing);
			ipa_ud := valueof(t_ASP_IPA_UD(IPAC_PROTO_OSMO, payload, IPAC_PROTO_EXT_TCAP_ROUTING));
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}
#endif

#ifdef IPA_EMULATION_RSL
		/* Received RSL -> down into IPA */
		[] IPA_RSL_PORT.receive(ASP_RSL_Unitdata:?) -> value rsl {
			IPA_PORT.send(f_from_rsl(f_ipa_conn_id(), rsl));
		}
#endif
#ifdef IPA_EMULATION_OML
		/* Received OML -> down into IPA */
		[] IPA_OML_PORT.receive(OML_PDU:?) -> value oml {
			IPA_PORT.send(f_from_oml(f_ipa_conn_id(), oml));
		}
		[] IPA_OML_PORT.receive(octetstring:?) -> value payload {
			IPA_PORT.send(t_IPA_Send(f_ipa_conn_id(), IPAC_PROTO_OML, payload));
		}
#endif
		/* Received MISC (OML/CTRL) -> down into IPA */
		[] IPA_SP_PORT.receive(ASP_IPA_Unitdata: ?) -> value ipa_ud {
			IPA_PORT.send(f_from_asp(f_ipa_conn_id(), ipa_ud));
		}

		/* Received call to configure/operate the component */
		[] CFG_PORT.getcall(IPA_CFG_disconnect:{?}) {
			res := f_close();
			CFG_PORT.reply(IPA_CFG_disconnect:{res});
		}

		[] CFG_PORT.getcall(IPA_CFG_chg_ccm_enabled:{?})-> param(cfg_chg_ccm_enabled) {
			g_ccm_enabled := cfg_chg_ccm_enabled;
			CFG_PORT.reply(IPA_CFG_chg_ccm_enabled:{cfg_chg_ccm_enabled});
		}

		}
	}
}

/***********************************************************************
 * IPA Event waiter component. Wait for ASP_IPA_EVENT_ID_ACK
 ***********************************************************************/

type component IPA_EventWaiter_CT {
	port IPA_SP_PT IPA_SP_PORT;
}

function waiter_main(template ASP_IPA_Event wait_for := tr_ASP_IPA_EV(ASP_IPA_EVENT_ID_ACK))
runs on IPA_EventWaiter_CT {

	alt {
	[] IPA_SP_PORT.receive(wait_for) {
		setverdict(pass);
		}
	[] IPA_SP_PORT.receive { repeat; }
	}
}


}
