dumpcap: '-n' is deprecated; use '-F pcapng' to set the output format to pcapng.
Capturing on 'any'
dumpcap: Promiscuous mode not supported on the "any" device.
File: /home/osmocom-build/jenkins/workspace/ttcn3-5gc-test-ogs/logs/testsuite/C5G_Tests.TC_ran_initiated_qos_flow_mobility.pcap

Packets captured: 616
Packets received/dropped on interface 'any': 616/0 (pcap:0/dumpcap:0/flushed:0/ps_ifdrop:0) (100.0%)
