08:48:33.070515 9738 BSC_Tests.ttcn:3187 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc0_connection_status'.
08:48:34.089982 9738 BSC_Tests.ttcn:3187 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-start.sh BSC_Tests.TC_ctrl_msc0_connection_status' was executed successfully (exit status: 0).
08:48:34.090300 9738 BSC_Tests.ttcn:3187 Test case TC_ctrl_msc0_connection_status started.
08:48:34.090387 9738 BSC_Tests.ttcn:3187 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:34.091042 9738 BSC_Tests.ttcn:3187 Port IPA_CTRL was started.
08:48:34.091131 9738 BSC_Tests.ttcn:3187 Port RSL_CCHAN[0] was started.
08:48:34.091195 9738 BSC_Tests.ttcn:3187 Port RSL_CCHAN[1] was started.
08:48:34.091259 9738 BSC_Tests.ttcn:3187 Port RSL_CCHAN[2] was started.
08:48:34.091324 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[0][0] was started.
08:48:34.091386 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[0][1] was started.
08:48:34.091449 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[0][2] was started.
08:48:34.091511 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[0][3] was started.
08:48:34.091572 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[1][0] was started.
08:48:34.091634 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[1][1] was started.
08:48:34.091723 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[1][2] was started.
08:48:34.091787 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[1][3] was started.
08:48:34.091850 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[2][0] was started.
08:48:34.091913 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[2][1] was started.
08:48:34.091976 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[2][2] was started.
08:48:34.092037 9738 BSC_Tests.ttcn:3187 Port IPA_RSL[2][3] was started.
08:48:34.092099 9738 BSC_Tests.ttcn:3187 Port IPA was started.
08:48:34.092161 9738 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CTRL was started.
08:48:34.092226 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][0] was started.
08:48:34.092290 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][1] was started.
08:48:34.092354 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][2] was started.
08:48:34.092564 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[0][3] was started.
08:48:34.092651 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][0] was started.
08:48:34.092718 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][1] was started.
08:48:34.092784 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][2] was started.
08:48:34.092847 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[1][3] was started.
08:48:34.092909 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][0] was started.
08:48:34.092971 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][1] was started.
08:48:34.093035 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][2] was started.
08:48:34.093097 9738 BSC_Tests.ttcn:3187 Port IPA_CFG_PORT[2][3] was started.
08:48:34.093161 9738 BSC_Tests.ttcn:3187 Port BSCVTY was started.
08:48:34.093225 9738 BSC_Tests.ttcn:3187 Port STPVTY was started.
08:48:34.093309 9738 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CFG_PORT[0] was started.
08:48:34.093367 9738 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CFG_PORT[1] was started.
08:48:34.093421 9738 BSC_Tests.ttcn:3187 Port SCCPLITE_IPA_CFG_PORT[2] was started.
08:48:34.093476 9738 BSC_Tests.ttcn:3187 Port BSSAP was started.
08:48:34.093530 9738 BSC_Tests.ttcn:3187 Port BSSAP_LE was started.
08:48:34.093584 9738 BSC_Tests.ttcn:3187 Component type BSC_Tests.test_CT was initialized.
08:48:34.093651 9738 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
08:48:34.093779 9738 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
08:48:34.093860 9738 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
08:48:34.094447 9738 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
08:48:34.094540 9738 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
08:48:34.094693 9738 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
08:48:34.094789 9738 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:34.094865 9738 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:34.094951 9738 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:34.095102 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
08:48:34.095208 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.095286 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:34.095353 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:34.095417 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:34.095481 9738 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:34.095543 9738 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:48:34.095614 9738 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
08:48:34.095685 9738 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
08:48:34.095758 9738 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
08:48:34.095954 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
08:48:34.096543 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.096906 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.097016 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:34.097153 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
08:48:34.097410 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.097550 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:34.097661 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.098188 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
08:48:34.098408 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.098725 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.099019 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.100178 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
08:48:34.100312 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
08:48:34.100545 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.100765 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
08:48:34.100936 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.101161 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
08:48:34.101411 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.101757 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.102001 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.102171 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
08:48:34.102271 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
08:48:34.102369 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.102467 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
08:48:34.102785 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.102990 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
08:48:34.103142 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.103274 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.103433 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.103515 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
08:48:34.103592 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
08:48:34.103677 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.103769 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
08:48:34.103882 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.104047 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
08:48:34.104190 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.104311 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.104461 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.104903 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
08:48:34.105044 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
08:48:34.105142 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.105281 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:34.105479 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.105845 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
08:48:34.106165 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.106398 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.106578 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
08:48:34.106716 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
08:48:34.106933 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.107058 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:34.107169 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.107431 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
08:48:34.107611 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.107958 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.108120 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.108194 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
08:48:34.108264 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
08:48:34.108338 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.108415 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:34.108517 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.108814 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
08:48:34.108931 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.109046 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.109176 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.109376 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
08:48:34.109609 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
08:48:34.109735 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.109832 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:34.109993 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.110203 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
08:48:34.110350 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.110458 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.110702 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.110805 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
08:48:34.110874 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
08:48:34.110985 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.111093 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:34.111265 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.111509 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
08:48:34.111637 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.111743 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.111914 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:34.111971 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
08:48:34.112029 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
08:48:34.112083 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.112144 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:34.112274 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.112456 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
08:48:34.112822 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.113055 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.113174 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
08:48:34.113279 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
08:48:34.113390 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.113566 9738 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:34.120799 9832 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:34.120919 9832 - TTCN-3 Parallel Test Component started on 801766a2a455. Component reference: VirtMSC-STATS(10), component type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS. Version: 11.1.0.
08:48:34.120957 9832 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:34.121013 9832 - Connected to MC.
08:48:34.121037 9832 - Initializing variables, timers and ports of component type StatsD_Checker.StatsD_Checker_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:34.121090 9738 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 10, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:48:34.121190 9738 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(10).
08:48:34.121289 9738 StatsD_Checker.ttcnpp:417 Function was started.
08:48:34.121345 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
08:48:34.121418 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.121527 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
08:48:34.121625 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.121712 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.121760 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
08:48:34.121814 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
08:48:34.121864 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.121915 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
08:48:34.121980 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.122071 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 1" id 14
08:48:34.122164 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
08:48:34.122226 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.122277 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.122319 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:34.122364 9738 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 1" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:34.122393 9738 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 1" with ? matched
08:48:34.122422 9738 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 1" id 14
08:48:34.122450 9738 Osmocom_VTY_Functions.ttcn:85 Message with id 14 was extracted from the queue of BSCVTY.
08:48:34.122485 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.122526 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.122555 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
08:48:34.122602 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
08:48:34.122635 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.122661 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
08:48:34.122693 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.122832 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "% No such MSC: nr 2" id 16
08:48:34.122857 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
08:48:34.122888 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.122917 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:34.122923 9832 - Port STATSVTY was started.
08:48:34.122946 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:34.122960 9832 - Port STATSD_PROC was started.
08:48:34.122971 9738 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "% No such MSC: nr 2" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:34.122986 9832 - Port STATS was started.
08:48:34.122995 9738 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "% No such MSC: nr 2" with ? matched
08:48:34.123019 9832 - Component type StatsD_Checker.StatsD_Checker_CT was initialized.
08:48:34.123032 9738 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "% No such MSC: nr 2" id 16
08:48:34.123080 9738 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
08:48:34.123134 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.123190 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.123194 9832 - Starting function main("127.0.0.1", 8125, 5.000000).
08:48:34.123231 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
08:48:34.123272 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
08:48:34.123315 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.123462 9738 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:34.123720 9832 StatsD_Checker.ttcnpp:125 Mapping port VirtMSC-STATS(10):STATS to system:STATS.
08:48:34.123900 9832 StatsD_Checker.ttcnpp:125 Port STATS was mapped to system:STATS.
08:48:34.124046 9832 StatsD_Checker.ttcnpp:125 Map operation of VirtMSC-STATS(10):STATS to system:STATS finished.
08:48:34.124319 9832 StatsD_Checker.ttcnpp:126 entering f__IPL4__PROVIDER__listen: 127.0.0.1:8125 / UDP
08:48:34.125198 9832 StatsD_Checker.ttcnpp:134 Mapping port VirtMSC-STATS(10):STATSVTY to system:STATSVTY.
08:48:34.125539 9832 StatsD_Checker.ttcnpp:134 Message enqueued on STATSVTY from system integer : 2 id 1
08:48:34.125607 9832 StatsD_Checker.ttcnpp:134 Port STATSVTY was mapped to system:STATSVTY.
08:48:34.125639 9832 StatsD_Checker.ttcnpp:134 Map operation of VirtMSC-STATS(10):STATSVTY to system:STATSVTY finished.
08:48:34.125774 9832 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:48:34.125841 9832 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:48:34.125864 9832 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:48:34.125986 9832 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "enable"
08:48:34.126045 9832 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.126089 9832 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:34.126102 9832 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:34.126112 9832 Osmocom_VTY_Functions.ttcn:74 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:34.126124 9832 Osmocom_VTY_Functions.ttcn:75 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:34.126142 9832 Osmocom_VTY_Functions.ttcn:85 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:48:34.126203 9832 Osmocom_VTY_Functions.ttcn:86 Matching on port STATSVTY succeeded: 2 with ? matched
08:48:34.126233 9832 Osmocom_VTY_Functions.ttcn:86 Receive operation on port STATSVTY succeeded, message from system(): integer : 2 id 1
08:48:34.126256 9832 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of STATSVTY.
08:48:34.126275 9833 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:34.126328 9832 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 2
08:48:34.126329 9833 - TTCN-3 Parallel Test Component started on 801766a2a455. Component reference: VirtMSC-SCCP(11), component type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP. Version: 11.1.0.
08:48:34.126347 9833 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:34.126376 9833 - Connected to MC.
08:48:34.126390 9833 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:34.126392 9832 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.126410 9738 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 11, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:48:34.126422 9832 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.126437 9832 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:48:34.126455 9832 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of STATSVTY.
08:48:34.126463 9738 SCCP_Adapter.ttcnpp:131 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:34.126481 9832 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.126505 9832 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "stats reset"
08:48:34.126527 9832 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:34.126591 9832 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 3
08:48:34.126615 9832 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:34.126636 9832 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:34.126649 9832 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 3
08:48:34.126668 9832 Osmocom_VTY_Functions.ttcn:73 Message with id 3 was extracted from the queue of STATSVTY.
08:48:34.126683 9832 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:34.127649 9833 - Port SCCP_SP_PORT was started.
08:48:34.127677 9833 - Port MTP3_SCCP_PORT was started.
08:48:34.127692 9833 - Component type SCCP_Emulation.SCCP_CT was initialized.
08:48:34.128579 9834 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:34.128642 9834 - TTCN-3 Parallel Test Component started on 801766a2a455. Component reference: VirtMSC-IPA(12), component type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA. Version: 11.1.0.
08:48:34.128686 9834 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:34.128722 9834 - Connected to MC.
08:48:34.128734 9834 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:34.128756 9738 SCCP_Adapter.ttcnpp:131 PTC was created. Component reference: 12, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: VirtMSC-IPA.
08:48:34.128798 9738 SCCP_Adapter.ttcnpp:132 Mapping port VirtMSC-IPA(12):IPA_PORT to system:IPA_CODEC_PT.
08:48:34.129625 9834 - Port IPA_PORT was started.
08:48:34.129650 9834 - Port CFG_PORT was started.
08:48:34.129665 9834 - Port MTP3_SP_PORT was started.
08:48:34.129678 9834 - Port IPA_MGCP_PORT was started.
08:48:34.129691 9834 - Port IPA_RSL_PORT was started.
08:48:34.129703 9834 - Port IPA_OML_PORT was started.
08:48:34.129716 9834 - Port IPA_CTRL_PORT was started.
08:48:34.129728 9834 - Port IPA_SP_PORT was started.
08:48:34.129740 9834 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:34.129771 9834 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:34.129806 9738 SCCP_Adapter.ttcnpp:132 Map operation of VirtMSC-IPA(12):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:34.129836 9738 SCCP_Adapter.ttcnpp:134 Connecting ports VirtMSC-IPA(12):MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT.
08:48:34.130040 9833 - Port MTP3_SCCP_PORT is waiting for connection from VirtMSC-IPA(12):MTP3_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-b278f476.
08:48:34.130075 9834 - Port MTP3_SP_PORT has established the connection with VirtMSC-SCCP(11):MTP3_SCCP_PORT using transport type UNIX.
08:48:34.130146 9833 - Port MTP3_SCCP_PORT has accepted the connection from VirtMSC-IPA(12):MTP3_SP_PORT.
08:48:34.130190 9738 SCCP_Adapter.ttcnpp:134 Connect operation on VirtMSC-IPA(12):MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT finished.
08:48:34.130275 9738 SCCP_Adapter.ttcnpp:136 Creating new alive PTC with component type IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:34.132521 9835 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:34.132589 9835 - TTCN-3 Parallel Test Component started on 801766a2a455. Component reference: VirtMSC-IPA-WAIT(13), component type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT. Version: 11.1.0.
08:48:34.132606 9835 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:34.132679 9835 - Connected to MC.
08:48:34.132692 9835 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_EventWaiter_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:34.132713 9738 SCCP_Adapter.ttcnpp:136 PTC was created. Component reference: 13, alive: yes, type: IPA_Emulation.IPA_EventWaiter_CT, component name: VirtMSC-IPA-WAIT.
08:48:34.132758 9738 SCCP_Adapter.ttcnpp:137 Connecting ports VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:34.132915 9834 - Port IPA_SP_PORT is waiting for connection from VirtMSC-IPA-WAIT(13):IPA_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-976bb203.
08:48:34.133668 9835 - Port IPA_SP_PORT was started.
08:48:34.133697 9835 - Component type IPA_Emulation.IPA_EventWaiter_CT was initialized.
08:48:34.133733 9835 - Port IPA_SP_PORT has established the connection with VirtMSC-IPA(12):IPA_SP_PORT using transport type UNIX.
08:48:34.133787 9834 - Port IPA_SP_PORT has accepted the connection from VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:34.133811 9738 SCCP_Adapter.ttcnpp:137 Connect operation on VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT finished.
08:48:34.133850 9738 SCCP_Adapter.ttcnpp:138 Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}) on component VirtMSC-IPA-WAIT(13).
08:48:34.133932 9738 SCCP_Adapter.ttcnpp:138 Function was started.
08:48:34.133956 9738 SCCP_Adapter.ttcnpp:140 Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true) on component VirtMSC-IPA(12).
08:48:34.134051 9835 - Starting function waiter_main({
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := ?,
    id_resp := *
}).
08:48:34.134058 9738 SCCP_Adapter.ttcnpp:140 Function was started.
08:48:34.134227 9834 - Starting function main_server("127.0.0.1", 5000, true, IPA_INIT_SEND_IPA_ID_ACK (1), true).
08:48:34.134669 9834 IPA_Emulation.ttcnpp:346 entering f__IPL4__PROVIDER__listen: 127.0.0.1:5000 / TCP
08:48:37.775466 9834 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:37.776380 9834 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:37.776705 9834 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT failed: Type of the first message in the queue is not @IPA_CodecPort.IPA_RecvFrom.
08:48:37.777229 9834 IPA_Emulation.ttcnpp:864 Matching on port IPA_PORT succeeded:  matched
08:48:37.777682 9834 IPA_Emulation.ttcnpp:864 Receive operation on port IPA_PORT succeeded, message from system(): @Socket_API_Definitions.PortEvent : {
    connOpened := {
        connId := 2,
        remName := "127.0.0.1",
        remPort := 4000,
        locName := "127.0.0.1",
        locPort := 5000,
        proto := {
            tcp := { }
        },
        userData := 0
    }
} id 1
08:48:37.778266 9834 IPA_Emulation.ttcnpp:864 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:37.778596 9834 IPA_Emulation.ttcnpp:866 Established a new IPA connection (conn_id=2)
08:48:37.780239 9834 IPA_Emulation.ttcnpp:395 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(13) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
}
08:48:37.781506 9835 IPA_Emulation.ttcnpp:1007 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(12) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:37.781715 9834 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:37.782357 9834 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:37.782572 9835 IPA_Emulation.ttcnpp:1008 Matching on port IPA_SP_PORT ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:37.782812 9835 IPA_Emulation.ttcnpp:1011 Matching on port IPA_SP_PORT succeeded.
08:48:37.782997 9835 IPA_Emulation.ttcnpp:1011 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(12): @IPA_Emulation.ASP_IPA_Event: {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 2,
    id_resp := omit
} id 1
08:48:37.783112 9834 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:37.783207 9835 IPA_Emulation.ttcnpp:1011 Message with id 1 was extracted from the queue of IPA_SP_PORT.
08:48:37.785152 9834 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:37.785796 9834 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:37.786156 9834 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:37.786344 9834 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:37.786421 9834 IPA_Emulation.ttcnpp:774 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:37.786515 9834 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:37.786666 9834 IPA_Emulation.ttcnpp:395 Sent on IPA_SP_PORT to VirtMSC-IPA-WAIT(13) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
}
08:48:37.786819 9835 IPA_Emulation.ttcnpp:1007 Message enqueued on IPA_SP_PORT from VirtMSC-IPA(12) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:37.786841 9834 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE00'O
} id 3
08:48:37.786975 9834 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:37.787063 9834 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0016FD090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:37.787136 9835 IPA_Emulation.ttcnpp:1008 Matching on port IPA_SP_PORT succeeded:  matched
08:48:37.787149 9834 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:37.787232 9834 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:37.787238 9835 IPA_Emulation.ttcnpp:1008 Receive operation on port IPA_SP_PORT succeeded, message from VirtMSC-IPA(12): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 2,
    id_resp := omit
} id 2
08:48:37.787300 9834 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '00'O
} id 3
08:48:37.787321 9835 IPA_Emulation.ttcnpp:1008 Message with id 2 was extracted from the queue of IPA_SP_PORT.
08:48:37.787382 9834 IPA_Emulation.ttcnpp:774 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:37.787424 9835 IPA_Emulation.ttcnpp:1009 setverdict(pass): none -> pass
08:48:37.787452 9834 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_PING (0),
    u := omit
}
08:48:37.787556 9835 - Function waiter_main finished. PTC remains alive and is waiting for next start.
08:48:37.787561 9834 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_PONG (1),
    u := omit
}
08:48:37.787644 9834 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '01'O
}
08:48:37.787745 9834 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0001FE01'O
}
08:48:37.787797 9738 SCCP_Adapter.ttcnpp:151 PTC with component reference 13 is done.
08:48:37.788015 9738 SCCP_Adapter.ttcnpp:152 Disconnecting ports VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:37.788098 9834 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_SCCP (253) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:37.788191 9834 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:37.788212 9835 - Terminating the connection of port IPA_SP_PORT to VirtMSC-IPA(12):IPA_SP_PORT. No more messages can be sent through this connection.
08:48:37.788267 9834 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 4
08:48:37.788337 9834 IPA_Emulation.ttcnpp:790 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:37.789463 9834 IPA_Emulation.ttcnpp:796 Sent on MTP3_SP_PORT to VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
}
08:48:37.789857 9834 IPA_Emulation.ttcnpp:772 Connection termination request was received on port IPA_SP_PORT from VirtMSC-IPA-WAIT(13):IPA_SP_PORT. No more data can be sent or received through this connection.
08:48:37.789966 9835 - Port IPA_SP_PORT was disconnected from VirtMSC-IPA(12):IPA_SP_PORT.
08:48:37.790074 9834 IPA_Emulation.ttcnpp:772 Port IPA_SP_PORT was disconnected from VirtMSC-IPA-WAIT(13):IPA_SP_PORT.
08:48:37.790201 9738 SCCP_Adapter.ttcnpp:152 Disconnect operation on VirtMSC-IPA(12):IPA_SP_PORT and VirtMSC-IPA-WAIT(13):IPA_SP_PORT finished.
08:48:37.790480 9833 - Message enqueued on MTP3_SCCP_PORT from VirtMSC-IPA(12) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE06000430040120'O
} id 1
08:48:37.790519 9738 BSC_Tests.ttcn:1221 Connecting ports mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT.
08:48:37.791536 9738 BSC_Tests.ttcn:1221 Port SCCPLITE_IPA_CFG_PORT[0] is waiting for connection from VirtMSC-IPA(12):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-a304b44b.
08:48:37.791666 9834 IPA_Emulation.ttcnpp:772 Port CFG_PORT has established the connection with mtc:SCCPLITE_IPA_CFG_PORT[0] using transport type UNIX.
08:48:37.791929 9738 BSC_Tests.ttcn:1221 Port SCCPLITE_IPA_CFG_PORT[0] has accepted the connection from VirtMSC-IPA(12):CFG_PORT.
08:48:37.792082 9738 BSC_Tests.ttcn:1221 Connect operation on mtc:SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT finished.
08:48:37.792207 9738 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:37.792969 9833 - Incoming message was mapped to @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:37.792972 9738 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(11):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-b67fb81d.
08:48:37.793284 9833 - Port SCCP_SP_PORT has established the connection with mtc:BSSAP using transport type UNIX.
08:48:37.793433 9738 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:37.793569 9738 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT finished.
08:48:37.793689 9738 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}) on component VirtMSC-SCCP(11).
08:48:37.793889 9738 SCCP_Adapter.ttcnpp:165 Function was started.
08:48:37.794257 9833 - Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}).
08:48:37.794259 9738 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(11) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 0,
                        causeValue := '0000000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:48:37.794407 9738 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 0,
                    causeValue := '0000000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:37.794579 9738 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
08:48:37.794714 9738 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
}
08:48:37.794903 9738 BSC_Tests.ttcn:899 Start timer T: 5 s
08:48:37.794996 9833 SCCP_Emulation.ttcn:1453 v_sccp_pdu_maxlen:268
08:48:37.796053 9833 SCCP_Emulation.ttcn:5443 Matching on port MTP3_SCCP_PORT succeeded:  matched
08:48:37.796204 9833 SCCP_Emulation.ttcn:5443 Receive operation on port MTP3_SCCP_PORT succeeded, message from VirtMSC-IPA(12): @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 6,
            data := '000430040120'O
        }
    }
} id 1
08:48:37.796377 9833 SCCP_Emulation.ttcn:5443 Message with id 1 was extracted from the queue of MTP3_SCCP_PORT.
08:48:37.798235 9833 SCCP_Emulation.ttcn:3464 Sent on SCCP_SP_PORT to mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
}
08:48:37.798790 9738 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(11) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000430040120'O,
    importance := omit
} id 1
08:48:37.798946 9738 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000430040120'O
08:48:37.799421 9833 SCCP_Emulation.ttcn:5439 Message enqueued on SCCP_SP_PORT from mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:37.799715 9833 SCCP_Emulation.ttcn:5577 Matching on port SCCP_SP_PORT succeeded.
08:48:37.799796 9738 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 4,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 1,
                    causeValue := '0100000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:37.799844 9833 SCCP_Emulation.ttcn:5577 Check-receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req: {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:37.799944 9833 SCCP_Emulation.ttcn:5585 Matching on port SCCP_SP_PORT failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_DATA_req.
08:48:37.800019 9738 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:37.800260 9833 SCCP_Emulation.ttcn:5591 Matching on port SCCP_SP_PORT succeeded:  matched
08:48:37.800276 9738 BSC_Tests.ttcn:901 Matching on port BSSAP .userData.pdu.bssmap{
    reset := {
        messageType := '30'O ("0"),
        cause := {
            elementIdentifier := '04'O,
            lengthIndicator := 1,
            causeValue := '0100000'B,
            extensionCauseValue := '0'B,
            spare1 := omit
        },
        a_InterfaceSelectorForReset := omit,
        osmuxSupport := omit
    }
} with {
    resetAck := {
        messageType := '31'O ("1"),
        a_InterfaceSelectorForReset := *,
        osmuxSupport := omit
    }
} unmatched: First message in the queue does not match the template: 
08:48:37.800364 9833 SCCP_Emulation.ttcn:5591 Receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
} id 1
08:48:37.800490 9738 BSC_Tests.ttcn:905 Matching on port BSSAP succeeded:  matched
08:48:37.800505 9833 SCCP_Emulation.ttcn:5591 Message with id 1 was extracted from the queue of SCCP_SP_PORT.
08:48:37.800665 9738 BSC_Tests.ttcn:905 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(11): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 4,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 1,
                        causeValue := '0100000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:48:37.800818 9738 BSC_Tests.ttcn:905 Message with id 1 was extracted from the queue of BSSAP.
08:48:37.800944 9738 BSC_Tests.ttcn:906 BSSMAP: Respoding to inbound RESET with RESET-ACK
08:48:37.801182 9738 BSC_Tests.ttcn:907 Sent on BSSAP to VirtMSC-SCCP(11) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:48:37.801331 9738 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:37.801477 9738 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000131'O
08:48:37.801597 9738 BSC_Tests.ttcn:907 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
}
08:48:37.802782 9833 SCCP_Emulation.ttcn:5223 Sent on MTP3_SCCP_PORT to VirtMSC-IPA(12) @SCCP_Types.ASP_MTP3_TRANSFERreq_sccp : {
    sio := '03'O,
    opc := 185,
    dpc := 187,
    sls := 0,
    data := {
        unitdata := {
            messageType := 9,
            protClass := {
                class := '0000'B,
                messageHandling := '0000'B
            },
            pointer1 := 0,
            pointer2 := 0,
            pointer3 := 0,
            calledPAddress := {
                paramLength := 4,
                addr := '43BB00FE'O
            },
            callingPAddress := {
                paramLength := 4,
                addr := '43B900FE'O
            },
            data := {
                paramLength := 6,
                data := '000430040100'O
            }
        }
    }
}
08:48:37.803509 9833 SCCP_Emulation.ttcn:5223 Outgoing message was mapped to @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:37.803928 9834 IPA_Emulation.ttcnpp:772 Message enqueued on MTP3_SP_PORT from VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
} id 1
08:48:37.804065 9833 SCCP_Emulation.ttcn:5439 Message enqueued on SCCP_SP_PORT from mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:37.804146 9833 SCCP_Emulation.ttcn:5577 Matching on port SCCP_SP_PORT succeeded.
08:48:37.804184 9834 IPA_Emulation.ttcnpp:899 Matching on port MTP3_SP_PORT succeeded:  matched
08:48:37.804237 9833 SCCP_Emulation.ttcn:5577 Check-receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req: {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:37.804285 9834 IPA_Emulation.ttcnpp:899 Receive operation on port MTP3_SP_PORT succeeded, message from VirtMSC-SCCP(11): @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE06000430040100'O
} id 1
08:48:37.804326 9833 SCCP_Emulation.ttcn:5585 Matching on port SCCP_SP_PORT failed: Type of the first message in the queue is not @SCCPasp_Types.ASP_SCCP_N_DATA_req.
08:48:37.804399 9834 IPA_Emulation.ttcnpp:899 Message with id 1 was extracted from the queue of MTP3_SP_PORT.
08:48:37.804433 9833 SCCP_Emulation.ttcn:5591 Matching on port SCCP_SP_PORT succeeded:  matched
08:48:37.804537 9833 SCCP_Emulation.ttcn:5591 Receive operation on port SCCP_SP_PORT succeeded, message from mtc: @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000131'O,
    importance := omit
} id 2
08:48:37.804561 9834 IPA_Emulation.ttcnpp:902 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:37.804591 9833 SCCP_Emulation.ttcn:5591 Message with id 2 was extracted from the queue of SCCP_SP_PORT.
08:48:37.804670 9834 IPA_Emulation.ttcnpp:902 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0016FD090003070B0443BB00FE0443B900FE06000430040100'O
}
08:48:37.804732 9833 SCCP_Emulation.ttcn:5223 Sent on MTP3_SCCP_PORT to VirtMSC-IPA(12) @SCCP_Types.ASP_MTP3_TRANSFERreq_sccp : {
    sio := '03'O,
    opc := 185,
    dpc := 187,
    sls := 0,
    data := {
        unitdata := {
            messageType := 9,
            protClass := {
                class := '0000'B,
                messageHandling := '0000'B
            },
            pointer1 := 0,
            pointer2 := 0,
            pointer3 := 0,
            calledPAddress := {
                paramLength := 4,
                addr := '43BB00FE'O
            },
            callingPAddress := {
                paramLength := 4,
                addr := '43B900FE'O
            },
            data := {
                paramLength := 3,
                data := '000131'O
            }
        }
    }
}
08:48:37.804955 9833 SCCP_Emulation.ttcn:5223 Outgoing message was mapped to @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:37.805031 9834 IPA_Emulation.ttcnpp:772 Message enqueued on MTP3_SP_PORT from VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 2
08:48:37.805090 9834 IPA_Emulation.ttcnpp:899 Matching on port MTP3_SP_PORT succeeded:  matched
08:48:37.805137 9834 IPA_Emulation.ttcnpp:899 Receive operation on port MTP3_SP_PORT succeeded, message from VirtMSC-SCCP(11): @MTP3asp_Types.ASP_MTP3_TRANSFERreq : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    data := '090003070B0443BB00FE0443B900FE03000131'O
} id 2
08:48:37.805468 9834 IPA_Emulation.ttcnpp:899 Message with id 2 was extracted from the queue of MTP3_SP_PORT.
08:48:37.805524 9834 IPA_Emulation.ttcnpp:902 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443BB00FE0443B900FE03000131'O
}
08:48:37.805585 9834 IPA_Emulation.ttcnpp:902 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 2,
    proto := {
        tcp := { }
    },
    msg := '0013FD090003070B0443BB00FE0443B900FE03000131'O
}
08:48:37.829730 9834 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 2,
    remName := "127.0.0.1",
    remPort := 4000,
    locName := "127.0.0.1",
    locPort := 5000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0013FD090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:37.829959 9834 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:37.830198 9834 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_SCCP (253) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:37.830365 9834 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:37.830670 9834 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 2,
    streamId := IPAC_PROTO_SCCP (253),
    streamIdExt := omit,
    msg := '090003070B0443B900FE0443BB00FE03000131'O
} id 5
08:48:37.830788 9834 IPA_Emulation.ttcnpp:790 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:37.831008 9834 IPA_Emulation.ttcnpp:796 Sent on MTP3_SP_PORT to VirtMSC-SCCP(11) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE03000131'O
}
08:48:37.831200 9833 SCCP_Emulation.ttcn:5439 Message enqueued on MTP3_SCCP_PORT from VirtMSC-IPA(12) @MTP3asp_Types.ASP_MTP3_TRANSFERind : {
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 0,
    dpc := 0,
    sls := 0,
    data := '090003070B0443B900FE0443BB00FE03000131'O
} id 2
08:48:37.831421 9833 SCCP_Emulation.ttcn:5439 Incoming message was mapped to @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 3,
            data := '000131'O
        }
    }
} id 2
08:48:37.831591 9833 SCCP_Emulation.ttcn:5443 Matching on port MTP3_SCCP_PORT succeeded:  matched
08:48:37.831682 9833 SCCP_Emulation.ttcn:5443 Receive operation on port MTP3_SCCP_PORT succeeded, message from VirtMSC-IPA(12): @SCCP_Types.PDU_SCCP : {
    unitdata := {
        messageType := 9,
        protClass := {
            class := '0000'B,
            messageHandling := '0000'B
        },
        pointer1 := 3,
        pointer2 := 7,
        pointer3 := 11,
        calledPAddress := {
            paramLength := 4,
            addr := '43B900FE'O
        },
        callingPAddress := {
            paramLength := 4,
            addr := '43BB00FE'O
        },
        data := {
            paramLength := 3,
            data := '000131'O
        }
    }
} id 2
08:48:37.832080 9833 SCCP_Emulation.ttcn:5443 Message with id 2 was extracted from the queue of MTP3_SCCP_PORT.
08:48:37.832567 9833 SCCP_Emulation.ttcn:3464 Sent on SCCP_SP_PORT to mtc @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
}
08:48:37.833053 9738 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(11) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
} id 2
08:48:37.833418 9738 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
08:48:37.834050 9738 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 1,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:48:37.834397 9738 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 2
08:48:37.834810 9738 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
08:48:37.835137 9738 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(11): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 2
08:48:37.835473 9738 BSC_Tests.ttcn:901 Message with id 2 was extracted from the queue of BSSAP.
08:48:37.835697 9738 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
08:48:37.835906 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
08:48:37.836084 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.842448 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:37.842895 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 19
08:48:37.848805 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.854479 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.859197 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:37.862495 9738 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:37.864598 9738 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" with ? matched
08:48:37.866052 9738 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm info
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 5000 4000 ipa
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  transport-role client
  no tcp-param keepalive
  no shutdown
 as as-clnt-msc-0 ipa
  asp asp-clnt-msc-0
  routing-key 0 0.23.3
  point-code override opc 0.23.1
 sccp-address addr-dyn-msc-default
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr addr-dyn-msc-default
 asp-protocol ipa
 lcls-mode disabled
 lcls-codec-mismatch forbidden
bsc
 mid-call-timeout 0
end" id 18
08:48:37.866095 9738 Osmocom_VTY_Functions.ttcn:85 Message with id 18 was extracted from the queue of BSCVTY.
08:48:37.866128 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.866158 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.866180 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 19
08:48:37.866199 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 19 was extracted from the queue of BSCVTY.
08:48:37.866219 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.866247 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:37.866329 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.866432 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 20
08:48:37.866476 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.866502 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.866537 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.866555 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 20
08:48:37.866572 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
08:48:37.866593 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.866631 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:48:37.866659 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.866767 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 21
08:48:37.866793 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.866816 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.866844 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.866861 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 21
08:48:37.866878 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
08:48:37.866900 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.866918 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
08:48:37.866938 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.867025 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 22
08:48:37.867048 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.867070 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.867096 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.867113 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 22
08:48:37.867129 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 22 was extracted from the queue of BSCVTY.
08:48:37.867145 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.867161 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:37.867180 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.867258 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
08:48:37.867281 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.867303 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:37.867328 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:37.867348 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
08:48:37.867374 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
08:48:37.867393 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.867411 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:48:37.867431 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:37.867508 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 24
08:48:37.867530 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:37.867554 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:37.867573 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 24
08:48:37.867588 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 24 was extracted from the queue of BSCVTY.
08:48:37.867605 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:37.867623 9738 BSC_Tests.ttcn:1191 msc 1 is not configured, skipping
08:48:37.867641 9738 BSC_Tests.ttcn:1191 msc 2 is not configured, skipping
08:48:37.867674 9738 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:37.870653 9837 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:37.870868 9837 - TTCN-3 Parallel Test Component started on 801766a2a455. Component reference: IPA-CTRL-CLI-IPA(14), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA. Version: 11.1.0.
08:48:37.870910 9837 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:37.870992 9837 - Connected to MC.
08:48:37.871018 9837 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:37.871050 9738 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 14, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:48:37.871080 9738 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(14):IPA_PORT to system:IPA_CODEC_PT.
08:48:37.872696 9837 - Port IPA_PORT was started.
08:48:37.872748 9837 - Port CFG_PORT was started.
08:48:37.872776 9837 - Port MTP3_SP_PORT was started.
08:48:37.872802 9837 - Port IPA_MGCP_PORT was started.
08:48:37.872829 9837 - Port IPA_RSL_PORT was started.
08:48:37.872858 9837 - Port IPA_OML_PORT was started.
08:48:37.872884 9837 - Port IPA_CTRL_PORT was started.
08:48:37.872910 9837 - Port IPA_SP_PORT was started.
08:48:37.872936 9837 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:37.873003 9837 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:37.873071 9738 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(14):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:37.873106 9738 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:37.873495 9738 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-bc34f21f.
08:48:37.873554 9837 - Port IPA_CTRL_PORT has established the connection with mtc:IPA_CTRL using transport type UNIX.
08:48:37.873623 9738 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT.
08:48:37.873664 9738 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
08:48:37.873696 9738 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false) on component IPA-CTRL-CLI-IPA(14).
08:48:37.873774 9738 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
08:48:37.873887 9738 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
08:48:37.873965 9837 - Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false).
08:48:37.874300 9837 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :0 -> 127.0.0.1:4249 / TCP
08:48:37.876356 9837 IPA_Emulation.ttcnpp:409 Sent on IPA_CTRL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:37.876584 9738 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:37.876705 9738 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
08:48:37.876805 9738 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:37.876897 9738 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
08:48:37.876972 9738 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:37.883229 9838 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:37.883407 9838 - TTCN-3 Parallel Test Component started on 801766a2a455. Component reference: VirtMGW-MGCP-0(15), component type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0. Version: 11.1.0.
08:48:37.883456 9838 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:37.883557 9838 - Connected to MC.
08:48:37.883591 9838 - Initializing variables, timers and ports of component type MGCP_Emulation.MGCP_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:37.883659 9738 BSC_Tests.ttcn:1073 PTC was created. Component reference: 15, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:48:37.883793 9738 BSC_Tests.ttcn:1074 Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(15).
08:48:37.883971 9738 BSC_Tests.ttcn:1074 Function was started.
08:48:37.884071 9738 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:37.884124 9738 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.132172.
08:48:37.884191 9738 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "132171665",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:37.884249 9738 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:37.884514 9837 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "132171665",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:37.884813 9837 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:37.884978 9837 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "132171665",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:48:37.885042 9837 IPA_Emulation.ttcnpp:921 Message with id 1 was extracted from the queue of IPA_CTRL_PORT.
08:48:37.886044 9838 - Port MGCP was started.
08:48:37.886109 9838 - Port MGCP_CLIENT was started.
08:48:37.886143 9838 - Port MGCP_CLIENT_MULTI was started.
08:48:37.886178 9838 - Port MGCP_PROC was started.
08:48:37.886208 9838 - Component type MGCP_Emulation.MGCP_Emulation_CT was initialized.
08:48:37.886261 9837 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420313332313731363635206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 132171665 bts.0.oml-connection-state")
}
08:48:37.886378 9838 - Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := true
}, "VirtMGW-MGCP-0").
08:48:37.886825 9837 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420313332313731363635206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:37.886935 9838 MGCP_Emulation.ttcn:279 Mapping port VirtMGW-MGCP-0(15):MGCP to system:MGCP_CODEC_PT.
08:48:37.887101 9838 MGCP_Emulation.ttcn:279 Port MGCP was mapped to system:MGCP_CODEC_PT.
08:48:37.887247 9838 MGCP_Emulation.ttcn:279 Map operation of VirtMGW-MGCP-0(15):MGCP to system:MGCP_CODEC_PT finished.
08:48:37.887564 9838 MGCP_Emulation.ttcn:281 entering f__IPL4__PROVIDER__listen: 127.0.0.1:2427 / UDP
08:48:37.887770 9837 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 37637,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0038EE004745545F5245504C5920313332313731363635206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
} id 1
08:48:37.888148 9837 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313332313731363635206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 132171665 bts.0.oml-connection-state degraded")
} id 1
08:48:37.888329 9837 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:37.888411 9837 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920313332313731363635206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 132171665 bts.0.oml-connection-state degraded")
} id 1
08:48:37.888478 9837 IPA_Emulation.ttcnpp:790 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:37.889022 9837 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "132171665",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
08:48:37.889177 9738 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "132171665",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:48:37.889255 9738 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:37.889316 9738 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "132171665",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:48:37.889375 9738 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
08:48:37.889430 9738 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:37.889480 9738 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:38.889532 9738 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:38.889996 9738 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:38.900482 9840 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:48:38.900916 9840 - TTCN-3 Parallel Test Component started on 801766a2a455. Component reference: IPA-BTS0-TRX0-RSL-IPA(16), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA. Version: 11.1.0.
08:48:38.901154 9840 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=LOG_ALL | MATCHING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:48:38.901456 9840 - Connected to MC.
08:48:38.901604 9840 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_ctrl_msc0_connection_status.
08:48:38.901786 9738 BSC_Tests.ttcn:951 PTC was created. Component reference: 16, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:48:38.902124 9738 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: {
    site_id := 1234,
    bts_id := 0,
    trx_id := 0
}
08:48:38.902412 9738 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
08:48:38.902497 9738 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(16):IPA_PORT to system:IPA_CODEC_PT.
08:48:38.905375 9840 - Port IPA_PORT was started.
08:48:38.905552 9840 - Port CFG_PORT was started.
08:48:38.905615 9840 - Port MTP3_SP_PORT was started.
08:48:38.905673 9840 - Port IPA_MGCP_PORT was started.
08:48:38.905730 9840 - Port IPA_RSL_PORT was started.
08:48:38.905786 9840 - Port IPA_OML_PORT was started.
08:48:38.905842 9840 - Port IPA_CTRL_PORT was started.
08:48:38.905896 9840 - Port IPA_SP_PORT was started.
08:48:38.905946 9840 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:48:38.906106 9840 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:48:38.906412 9738 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(16):IPA_PORT to system:IPA_CODEC_PT finished.
08:48:38.906599 9738 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
08:48:38.907585 9738 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-ac738b6e.
08:48:38.907726 9840 - Port CFG_PORT has established the connection with mtc:IPA_CFG_PORT[0][0] using transport type UNIX.
08:48:38.907887 9738 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT.
08:48:38.907977 9738 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
08:48:38.908056 9738 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
08:48:38.909111 9738 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-cf69ab76.
08:48:38.909323 9840 - Port IPA_RSL_PORT has established the connection with mtc:IPA_RSL[0][0] using transport type UNIX.
08:48:38.909866 9738 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT.
08:48:38.910060 9738 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
08:48:38.910152 9738 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true) on component IPA-BTS0-TRX0-RSL-IPA(16).
08:48:38.910452 9738 BSC_Tests.ttcn:969 Function was started.
08:48:38.910660 9738 BSC_Tests.ttcn:976 Start timer T: 10 s
08:48:38.910787 9840 - Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true).
08:48:38.911621 9840 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :10000 -> 127.0.0.1:3003 / TCP
08:48:38.916377 9840 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:38.916938 9840 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:48:38.917551 9840 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:48:38.918997 9840 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:48:38.919345 9738 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:38.919520 9738 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:48:38.919780 9738 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:38.919925 9738 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(16): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:48:38.920077 9738 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
08:48:38.921638 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0011FE0401080107010201030104010501010100'O
} id 1
08:48:38.922023 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:38.922108 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:48:38.922163 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:38.922373 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:38.922462 9840 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:48:38.922513 9840 IPA_Emulation.ttcnpp:774 Message with id 1 was extracted from the queue of IPA_PORT.
08:48:38.922602 9840 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
08:48:38.923188 9840 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
08:48:38.923384 9840 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:38.923435 9840 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:48:38.923539 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:48:38.923605 9840 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:48:38.923692 9840 IPA_Emulation.ttcnpp:774 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:38.923732 9840 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:48:38.923776 9840 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
}
08:48:38.923863 9738 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:38.924018 9738 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
08:48:38.924102 9738 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(16): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:48:38.924179 9738 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
08:48:38.924238 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:38.924249 9738 BSC_Tests.ttcn:979 Stop timer T: 10 s
08:48:38.924285 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:38.924327 9738 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:48:38.924403 9738 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.690972.
08:48:38.924452 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.924503 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.924517 9738 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "690971945",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:48:38.924542 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:48:38.924582 9840 IPA_Emulation.ttcnpp:790 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:38.924622 9738 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:38.924698 9837 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "690971945",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:38.924888 9837 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:38.924971 9837 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "690971945",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:48:38.925042 9837 IPA_Emulation.ttcnpp:921 Message with id 2 was extracted from the queue of IPA_CTRL_PORT.
08:48:38.925175 9837 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420363930393731393435206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 690971945 bts.0.oml-connection-state")
}
08:48:38.925277 9837 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420363930393731393435206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:48:38.925559 9837 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 37637,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0039EE004745545F5245504C5920363930393731393435206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
} id 2
08:48:38.925666 9837 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920363930393731393435206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 690971945 bts.0.oml-connection-state connected")
} id 2
08:48:38.925736 9837 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.925814 9837 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920363930393731393435206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 690971945 bts.0.oml-connection-state connected")
} id 2
08:48:38.925933 9837 IPA_Emulation.ttcnpp:790 Message with id 2 was extracted from the queue of IPA_PORT.
08:48:38.926177 9837 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "690971945",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
08:48:38.926354 9738 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "690971945",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:48:38.926501 9738 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:38.926579 9738 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "690971945",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:48:38.926670 9738 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
08:48:38.926744 9738 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:48:38.926811 9738 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:48:38.928026 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
}
08:48:38.928330 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:38.928344 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
08:48:38.928371 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:38.928399 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0006000C1101801E0A'O
} id 5
08:48:38.928424 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:38.928451 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:38.928493 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:38.928520 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:38.928545 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:38.928573 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:38.928596 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:38.928620 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:38.928652 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:38.928676 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:38.928706 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:38.928733 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:38.928770 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:38.928793 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '000400101A1E0D'O
} id 12
08:48:38.928816 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:38.928840 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.928863 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.928886 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000FFE50400'O
} id 4
08:48:38.928909 9840 IPA_Emulation.ttcnpp:790 Message with id 4 was extracted from the queue of IPA_PORT.
08:48:38.929012 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
}
08:48:38.929052 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.929075 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.929097 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:48:38.929108 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000FFE50400'O
                    }
                }
            }
        }
    }
} id 4
08:48:38.929137 9840 IPA_Emulation.ttcnpp:790 Message with id 5 was extracted from the queue of IPA_PORT.
08:48:38.929178 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
}
08:48:38.929204 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.929226 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.929249 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:48:38.929269 9840 IPA_Emulation.ttcnpp:790 Message with id 6 was extracted from the queue of IPA_PORT.
08:48:38.929277 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
} id 5
08:48:38.929335 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:38.929367 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.929388 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.929409 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:48:38.929429 9840 IPA_Emulation.ttcnpp:790 Message with id 7 was extracted from the queue of IPA_PORT.
08:48:38.929476 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:38.929509 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
} id 6
08:48:38.929521 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.929543 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.929564 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:48:38.929574 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 7
08:48:38.929586 9840 IPA_Emulation.ttcnpp:790 Message with id 8 was extracted from the queue of IPA_PORT.
08:48:38.929623 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
}
08:48:38.929648 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.929657 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
} id 8
08:48:38.929670 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.929691 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:48:38.929710 9840 IPA_Emulation.ttcnpp:790 Message with id 9 was extracted from the queue of IPA_PORT.
08:48:38.929744 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:38.929771 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.929780 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 9
08:48:38.929791 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.929813 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:48:38.929833 9840 IPA_Emulation.ttcnpp:790 Message with id 10 was extracted from the queue of IPA_PORT.
08:48:38.929870 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:48:38.929897 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.929906 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 10
08:48:38.929941 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.929972 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:48:38.929997 9840 IPA_Emulation.ttcnpp:790 Message with id 11 was extracted from the queue of IPA_PORT.
08:48:38.930144 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:38.930180 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.930187 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 11
08:48:38.930201 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.930220 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:48:38.930239 9840 IPA_Emulation.ttcnpp:790 Message with id 12 was extracted from the queue of IPA_PORT.
08:48:38.930269 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
}
08:48:38.930356 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:38.930357 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
} id 12
08:48:38.930402 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:38.930427 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001400101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:38.930454 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:38.930477 9840 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:38.930500 9840 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:38.930522 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.930543 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.930563 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:48:38.930583 9840 IPA_Emulation.ttcnpp:790 Message with id 13 was extracted from the queue of IPA_PORT.
08:48:38.930643 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:38.930670 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.930689 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.930696 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 13
08:48:38.930729 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197FF2B'O
} id 14
08:48:38.930754 9840 IPA_Emulation.ttcnpp:790 Message with id 14 was extracted from the queue of IPA_PORT.
08:48:38.930785 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
}
08:48:38.930822 9840 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:48:38.930845 9840 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:38.930847 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197FF2B'O
                    }
                }
            }
        }
    }
} id 14
08:48:38.930866 9840 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:48:38.930886 9840 IPA_Emulation.ttcnpp:790 Message with id 15 was extracted from the queue of IPA_PORT.
08:48:38.931112 9840 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:48:38.931180 9738 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(16) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 15
08:48:39.927504 9738 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:48:39.928031 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:48:39.928569 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:39.929225 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 25
08:48:39.929748 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.930255 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:39.930715 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:48:39.931099 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 25
08:48:39.931428 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
08:48:39.931740 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:39.931946 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:48:39.932097 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:39.932523 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 26
08:48:39.932751 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.932877 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:39.933057 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:48:39.933242 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 26
08:48:39.933327 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
08:48:39.933496 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:39.933602 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:48:39.933883 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:39.934262 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:39.934453 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.934592 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:39.934734 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:39.934809 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 27
08:48:39.934895 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 27 was extracted from the queue of BSCVTY.
08:48:39.934969 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:39.935088 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:48:39.935193 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:39.935364 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:39.935490 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.935621 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:39.935770 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:48:39.935844 9738 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 28
08:48:39.935919 9738 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
08:48:39.935996 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:39.936075 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:48:39.936168 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:39.936381 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 29
08:48:39.936493 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.936614 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:39.936719 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 29
08:48:39.936798 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 29 was extracted from the queue of BSCVTY.
08:48:39.936878 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:39.936955 9738 Osmocom_VTY_Functions.ttcn:338 "TC_ctrl_msc0_connection_status() start"
08:48:39.937128 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_ctrl_msc0_connection_status() start"
08:48:39.937245 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:39.937651 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 30
08:48:39.937792 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.937908 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:39.937977 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 30
08:48:39.938046 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 30 was extracted from the queue of BSCVTY.
08:48:39.938113 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:39.938190 9738 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.636290.
08:48:39.938288 9738 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "636290195",
        variable := "msc.0.connection_status",
        val := omit
    }
}
08:48:39.938374 9738 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:48:39.938431 9837 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "636290195",
        variable := "msc.0.connection_status",
        val := omit
    }
} id 3
08:48:39.938560 9837 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:48:39.938642 9837 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "636290195",
        variable := "msc.0.connection_status",
        val := omit
    }
} id 3
08:48:39.938734 9837 IPA_Emulation.ttcnpp:921 Message with id 3 was extracted from the queue of IPA_CTRL_PORT.
08:48:39.938858 9837 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420363336323930313935206D73632E302E636F6E6E656374696F6E5F737461747573'O ("GET 636290195 msc.0.connection_status")
}
08:48:39.938961 9837 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0026EE0047455420363336323930313935206D73632E302E636F6E6E656374696F6E5F737461747573'O
}
08:48:39.939276 9837 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 37637,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0036EE004745545F5245504C5920363336323930313935206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O
} id 3
08:48:39.939391 9837 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920363336323930313935206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 636290195 msc.0.connection_status connected")
} id 3
08:48:39.939461 9837 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:48:39.939541 9837 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920363336323930313935206D73632E302E636F6E6E656374696F6E5F73746174757320636F6E6E6563746564'O ("GET_REPLY 636290195 msc.0.connection_status connected")
} id 3
08:48:39.939608 9837 IPA_Emulation.ttcnpp:790 Message with id 3 was extracted from the queue of IPA_PORT.
08:48:39.939722 9837 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "636290195",
        variable := "msc.0.connection_status",
        val := "connected"
    }
}
08:48:39.939834 9738 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(14) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "636290195",
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 4
08:48:39.939916 9738 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:48:39.939997 9738 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(14): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "636290195",
        variable := "msc.0.connection_status",
        val := "connected"
    }
} id 4
08:48:39.940080 9738 Osmocom_CTRL_Functions.ttcn:41 Message with id 4 was extracted from the queue of IPA_CTRL.
08:48:39.940194 9738 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
08:48:39.940389 9738 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:48:39.941504 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1434269 bytes in 1321 blocks)" id 31
08:48:39.941581 9738 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
08:48:39.941752 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434269 bytes in 1321 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.941863 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434269 bytes in 1321 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:48:39.941973 9738 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434269 bytes in 1321 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:48:39.942054 9738 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1434269 bytes in 1321 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:48:39.942126 9738 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1434269 bytes in 1321 blocks)" with ? matched
08:48:39.942202 9738 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1434269 bytes in 1321 blocks)" id 31
08:48:39.942268 9738 Osmocom_VTY_Functions.ttcn:85 Message with id 31 was extracted from the queue of BSCVTY.
08:48:39.942440 9738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:48:39.942600 9738 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:48:39.942723 9738 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
08:48:39.942816 9738 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
08:48:39.943006 9738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:48:39.943262 9738 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
08:48:39.943347 9738 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
08:48:39.943441 9738 BSC_Tests.ttcn:888 Stopping all components.
08:48:39.943753 9832 StatsD_Checker.ttcnpp:143 Kill was requested from MC.
08:48:39.943767 9833 SCCP_Emulation.ttcn:5439 Stop was requested from MC.
08:48:39.943776 9837 IPA_Emulation.ttcnpp:772 Kill was requested from MC.
08:48:39.943777 9834 IPA_Emulation.ttcnpp:772 Stop was requested from MC.
08:48:39.943792 9838 MGCP_Emulation.ttcn:301 Stop was requested from MC.
08:48:39.943877 9840 IPA_Emulation.ttcnpp:772 Stop was requested from MC.
08:48:39.943992 9832 StatsD_Checker.ttcnpp:143 Terminating test component execution.
08:48:39.944044 9838 MGCP_Emulation.ttcn:301 Stopping test component execution.
08:48:39.944062 9837 IPA_Emulation.ttcnpp:772 Terminating test component execution.
08:48:39.944073 9834 IPA_Emulation.ttcnpp:772 Stopping test component execution.
08:48:39.944144 9840 IPA_Emulation.ttcnpp:772 Stopping test component execution.
08:48:39.944176 9833 SCCP_Emulation.ttcn:5439 Stopping test component execution.
08:48:39.945177 9832 - Function main was stopped. PTC terminates.
08:48:39.945288 9838 - Function main was stopped. PTC remains alive and is waiting for next start.
08:48:39.945326 9837 - Function main_client was stopped. PTC terminates.
08:48:39.945332 9834 - Function main_server was stopped. PTC remains alive and is waiting for next start.
08:48:39.945403 9840 - Function main_client was stopped. PTC remains alive and is waiting for next start.
08:48:39.945441 9832 - Terminating component type StatsD_Checker.StatsD_Checker_CT.
08:48:39.945480 9837 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:39.945582 9832 - Removing unterminated mapping between port STATSVTY and system:STATSVTY.
08:48:39.945591 9837 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:39.945819 9832 - Port STATSVTY was unmapped from system:STATSVTY.
08:48:39.946034 9832 - Port STATSVTY was stopped.
08:48:39.946164 9833 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
08:48:39.946217 9832 - Port STATSD_PROC was stopped.
08:48:39.946321 9832 - Removing unterminated mapping between port STATS and system:STATS.
08:48:39.946366 9837 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:39.946458 9837 - Port IPA_PORT was stopped.
08:48:39.946750 9837 - Port CFG_PORT was stopped.
08:48:39.946896 9837 - Port MTP3_SP_PORT was stopped.
08:48:39.947125 9837 - Port IPA_MGCP_PORT was stopped.
08:48:39.947187 9832 - Port STATS was unmapped from system:STATS.
08:48:39.947262 9837 - Port IPA_RSL_PORT was stopped.
08:48:39.947283 9832 - Port STATS was stopped.
08:48:39.947350 9832 - Component type StatsD_Checker.StatsD_Checker_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.947435 9832 - Final verdict of PTC: none
08:48:39.947487 9837 - Port IPA_OML_PORT was stopped.
08:48:39.947588 9832 - Disconnected from MC.
08:48:39.947615 9837 - Removing unterminated connection between port IPA_CTRL_PORT and mtc:IPA_CTRL.
08:48:39.947653 9832 - TTCN-3 Parallel Test Component finished.
08:48:39.947782 9837 - Port IPA_CTRL_PORT was stopped.
08:48:39.947801 9738 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT was closed unexpectedly by the peer.
08:48:39.947886 9837 - Port IPA_SP_PORT was stopped.
08:48:39.947896 9738 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(14):IPA_CTRL_PORT.
08:48:39.947983 9837 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.948215 9837 - Final verdict of PTC: none
08:48:39.948278 9738 BSC_Tests.ttcn:888 All components were stopped.
08:48:39.948342 9738 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
08:48:39.948415 9738 BSC_Tests.ttcn:890 Stopping test component execution.
08:48:39.948455 9837 - Disconnected from MC.
08:48:39.948508 9738 BSC_Tests.ttcn:3193 Test case TC_ctrl_msc0_connection_status was stopped.
08:48:39.948549 9837 - TTCN-3 Parallel Test Component finished.
08:48:39.948576 9738 BSC_Tests.ttcn:3193 Terminating component type BSC_Tests.test_CT.
08:48:39.948688 9738 BSC_Tests.ttcn:3193 Default with id 1 (altstep as_Tguard) was deactivated.
08:48:39.948858 9738 BSC_Tests.ttcn:3193 Stop timer T_guard: 30 s
08:48:39.948951 9738 BSC_Tests.ttcn:3193 Port IPA_CTRL was stopped.
08:48:39.949019 9738 BSC_Tests.ttcn:3193 Port RSL_CCHAN[0] was stopped.
08:48:39.949091 9738 BSC_Tests.ttcn:3193 Port RSL_CCHAN[1] was stopped.
08:48:39.949150 9738 BSC_Tests.ttcn:3193 Port RSL_CCHAN[2] was stopped.
08:48:39.949217 9738 BSC_Tests.ttcn:3193 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(16):IPA_RSL_PORT.
08:48:39.949397 9738 BSC_Tests.ttcn:3193 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
08:48:39.949506 9840 - Connection of port IPA_RSL_PORT to mtc:IPA_RSL[0][0] was closed unexpectedly by the peer.
08:48:39.949541 9738 BSC_Tests.ttcn:3193 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
08:48:39.949629 9840 - Port IPA_RSL_PORT was disconnected from mtc:IPA_RSL[0][0].
08:48:39.949631 9738 BSC_Tests.ttcn:3193 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
08:48:39.949711 9738 BSC_Tests.ttcn:3193 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
08:48:39.949781 9738 BSC_Tests.ttcn:3193 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
08:48:39.949864 9738 BSC_Tests.ttcn:3193 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
08:48:39.949932 9738 BSC_Tests.ttcn:3193 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
08:48:39.949999 9738 BSC_Tests.ttcn:3193 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
08:48:39.950067 9738 BSC_Tests.ttcn:3193 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
08:48:39.950133 9738 BSC_Tests.ttcn:3193 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
08:48:39.950198 9738 BSC_Tests.ttcn:3193 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
08:48:39.950263 9738 BSC_Tests.ttcn:3193 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
08:48:39.950330 9738 BSC_Tests.ttcn:3193 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
08:48:39.950393 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[0][0] was stopped.
08:48:39.950462 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[0][1] was stopped.
08:48:39.950581 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[0][2] was stopped.
08:48:39.950665 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[0][3] was stopped.
08:48:39.950724 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[1][0] was stopped.
08:48:39.950781 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[1][1] was stopped.
08:48:39.950836 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[1][2] was stopped.
08:48:39.950892 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[1][3] was stopped.
08:48:39.950949 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[2][0] was stopped.
08:48:39.951005 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[2][1] was stopped.
08:48:39.951065 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[2][2] was stopped.
08:48:39.951122 9738 BSC_Tests.ttcn:3193 Port IPA_RSL[2][3] was stopped.
08:48:39.951177 9738 BSC_Tests.ttcn:3193 Port IPA was stopped.
08:48:39.951238 9738 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CTRL was stopped.
08:48:39.951298 9738 BSC_Tests.ttcn:3193 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(16):CFG_PORT.
08:48:39.951463 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][0] was stopped.
08:48:39.951492 9840 - Connection of port CFG_PORT to mtc:IPA_CFG_PORT[0][0] was closed unexpectedly by the peer.
08:48:39.951623 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][1] was stopped.
08:48:39.951690 9840 - Port CFG_PORT was disconnected from mtc:IPA_CFG_PORT[0][0].
08:48:39.951690 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][2] was stopped.
08:48:39.951756 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[0][3] was stopped.
08:48:39.951822 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][0] was stopped.
08:48:39.951889 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][1] was stopped.
08:48:39.952089 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][2] was stopped.
08:48:39.952215 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[1][3] was stopped.
08:48:39.952314 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][0] was stopped.
08:48:39.952412 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][1] was stopped.
08:48:39.952507 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][2] was stopped.
08:48:39.952602 9738 BSC_Tests.ttcn:3193 Port IPA_CFG_PORT[2][3] was stopped.
08:48:39.952725 9738 BSC_Tests.ttcn:3193 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
08:48:39.952915 9738 BSC_Tests.ttcn:3193 Port BSCVTY was unmapped from system:BSCVTY.
08:48:39.953086 9738 BSC_Tests.ttcn:3193 Port BSCVTY was stopped.
08:48:39.953190 9738 BSC_Tests.ttcn:3193 Port STPVTY was stopped.
08:48:39.953288 9738 BSC_Tests.ttcn:3193 Removing unterminated connection between port SCCPLITE_IPA_CFG_PORT[0] and VirtMSC-IPA(12):CFG_PORT.
08:48:39.953433 9738 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
08:48:39.953457 9834 - Connection of port CFG_PORT to mtc:SCCPLITE_IPA_CFG_PORT[0] was closed unexpectedly by the peer.
08:48:39.953559 9738 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
08:48:39.953588 9834 - Port CFG_PORT was disconnected from mtc:SCCPLITE_IPA_CFG_PORT[0].
08:48:39.953683 9738 BSC_Tests.ttcn:3193 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
08:48:39.953783 9738 BSC_Tests.ttcn:3193 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(11):SCCP_SP_PORT.
08:48:39.953969 9738 BSC_Tests.ttcn:3193 Port BSSAP was stopped.
08:48:39.953984 9833 - Connection of port SCCP_SP_PORT to mtc:BSSAP was closed unexpectedly by the peer.
08:48:39.954156 9738 BSC_Tests.ttcn:3193 Port BSSAP_LE was stopped.
08:48:39.954160 9833 - Port SCCP_SP_PORT was disconnected from mtc:BSSAP.
08:48:39.954274 9738 BSC_Tests.ttcn:3193 Component type BSC_Tests.test_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.954423 9738 BSC_Tests.ttcn:3193 Waiting for PTCs to finish.
08:48:39.954595 9833 - Kill was requested from MC. Terminating idle PTC.
08:48:39.954612 9834 - Kill was requested from MC. Terminating idle PTC.
08:48:39.954634 9838 - Kill was requested from MC. Terminating idle PTC.
08:48:39.954651 9835 - Kill was requested from MC. Terminating idle PTC.
08:48:39.954653 9840 - Kill was requested from MC. Terminating idle PTC.
08:48:39.954776 9833 - Terminating component type SCCP_Emulation.SCCP_CT.
08:48:39.954785 9834 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:39.954801 9840 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:48:39.954838 9835 - Terminating component type IPA_Emulation.IPA_EventWaiter_CT.
08:48:39.954841 9838 - Terminating component type MGCP_Emulation.MGCP_Emulation_CT.
08:48:39.954904 9833 - Port SCCP_SP_PORT was stopped.
08:48:39.954996 9834 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:39.955006 9833 - Removing unterminated connection between port MTP3_SCCP_PORT and VirtMSC-IPA(12):MTP3_SP_PORT.
08:48:39.955006 9840 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:48:39.955019 9835 - Port IPA_SP_PORT was stopped.
08:48:39.955025 9838 - Removing unterminated mapping between port MGCP and system:MGCP_CODEC_PT.
08:48:39.955189 9833 - Port MTP3_SCCP_PORT was stopped.
08:48:39.955295 9833 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.955297 9835 - Component type IPA_Emulation.IPA_EventWaiter_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.955457 9833 - Final verdict of PTC: none
08:48:39.955493 9835 - Final verdict of PTC: pass
08:48:39.955781 9833 - Disconnected from MC.
08:48:39.955995 9833 - TTCN-3 Parallel Test Component finished.
08:48:39.956026 9835 - Disconnected from MC.
08:48:39.956311 9835 - TTCN-3 Parallel Test Component finished.
08:48:39.956797 9838 - Port MGCP was unmapped from system:MGCP_CODEC_PT.
08:48:39.956934 9838 - Port MGCP was stopped.
08:48:39.957015 9840 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:39.957098 9838 - Port MGCP_CLIENT was stopped.
08:48:39.957225 9840 - Port IPA_PORT was stopped.
08:48:39.957317 9834 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:48:39.957335 9838 - Port MGCP_CLIENT_MULTI was stopped.
08:48:39.957362 9840 - Port CFG_PORT was stopped.
08:48:39.957481 9838 - Port MGCP_PROC was stopped.
08:48:39.957490 9834 - Port IPA_PORT was stopped.
08:48:39.957585 9840 - Port MTP3_SP_PORT was stopped.
08:48:39.957776 9838 - Component type MGCP_Emulation.MGCP_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.957789 9834 - Port CFG_PORT was stopped.
08:48:39.957908 9840 - Port IPA_MGCP_PORT was stopped.
08:48:39.957968 9838 - Final verdict of PTC: none
08:48:39.958041 9840 - Port IPA_RSL_PORT was stopped.
08:48:39.958193 9834 - Removing unterminated connection between port MTP3_SP_PORT and VirtMSC-SCCP(11):MTP3_SCCP_PORT.
08:48:39.958260 9840 - Port IPA_OML_PORT was stopped.
08:48:39.958400 9840 - Port IPA_CTRL_PORT was stopped.
08:48:39.958448 9834 - Port MTP3_SP_PORT was stopped.
08:48:39.958452 9838 - Disconnected from MC.
08:48:39.958571 9834 - Port IPA_MGCP_PORT was stopped.
08:48:39.958588 9840 - Port IPA_SP_PORT was stopped.
08:48:39.958730 9834 - Port IPA_RSL_PORT was stopped.
08:48:39.958785 9838 - TTCN-3 Parallel Test Component finished.
08:48:39.958885 9840 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.959038 9840 - Final verdict of PTC: none
08:48:39.959072 9834 - Port IPA_OML_PORT was stopped.
08:48:39.959316 9834 - Port IPA_CTRL_PORT was stopped.
08:48:39.959420 9840 - Disconnected from MC.
08:48:39.959525 9834 - Port IPA_SP_PORT was stopped.
08:48:39.959621 9840 - TTCN-3 Parallel Test Component finished.
08:48:39.959701 9834 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_ctrl_msc0_connection_status.
08:48:39.960001 9834 - Final verdict of PTC: none
08:48:39.960314 9834 - Disconnected from MC.
08:48:39.960348 9738 BSC_Tests.ttcn:3193 Setting final verdict of the test case.
08:48:39.960434 9834 - TTCN-3 Parallel Test Component finished.
08:48:39.960504 9738 BSC_Tests.ttcn:3193 Local verdict of MTC: pass
08:48:39.960644 9738 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-STATS(10): none (pass -> pass)
08:48:39.960812 9738 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-SCCP(11): none (pass -> pass)
08:48:39.960943 9738 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-IPA(12): none (pass -> pass)
08:48:39.961251 9738 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMSC-IPA-WAIT(13): pass (pass -> pass)
08:48:39.961495 9738 BSC_Tests.ttcn:3193 Local verdict of PTC IPA-CTRL-CLI-IPA(14): none (pass -> pass)
08:48:39.961655 9738 BSC_Tests.ttcn:3193 Local verdict of PTC VirtMGW-MGCP-0(15): none (pass -> pass)
08:48:39.961812 9738 BSC_Tests.ttcn:3193 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(16): none (pass -> pass)
08:48:39.962022 9738 BSC_Tests.ttcn:3193 Test case TC_ctrl_msc0_connection_status finished. Verdict: pass
08:48:39.962173 9738 BSC_Tests.ttcn:3193 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc0_connection_status pass'.
08:48:45.206269 9738 BSC_Tests.ttcn:3193 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test-sccplite/ttcn3-tcpdump-stop.sh BSC_Tests.TC_ctrl_msc0_connection_status pass' was executed successfully (exit status: 0).
08:48:45.206446 9738 BSC_Tests.ttcn:3388 Switching to log file `BSC_Tests-TC_stat_num_bts_connected_1-801766a2a455-mtc-9738.log'
