Metadata-Version: 2.2
Name: smpplib
Version: 2.2.4
Summary: SMPP library for python
Home-page: https://github.com/python-smpplib/python-smpplib
Classifier: Development Status :: 5 - Production/Stable
Classifier: Intended Audience :: Telecommunications Industry
Classifier: License :: OSI Approved :: GNU Lesser General Public License v3 (LGPLv3)
Classifier: Operating System :: OS Independent
Classifier: Programming Language :: Python :: 2
Classifier: Programming Language :: Python :: 2.7
Classifier: Programming Language :: Python :: 3
Classifier: Programming Language :: Python :: 3.9
Classifier: Programming Language :: Python :: 3.10
Classifier: Programming Language :: Python :: 3.11
Classifier: Programming Language :: Python :: 3.12
Classifier: Programming Language :: Python :: 3.13
Classifier: Programming Language :: Python
Classifier: Topic :: Communications :: Telephony
Classifier: Topic :: Communications
Classifier: Topic :: Software Development :: Libraries :: Python Modules
Classifier: Topic :: Software Development :: Libraries
Description-Content-Type: text/markdown
License-File: LICENSE
Requires-Dist: six
Provides-Extra: tests
Requires-Dist: typing; python_version < "3.5" and extra == "tests"
Requires-Dist: pytest; extra == "tests"
Requires-Dist: mock; extra == "tests"
Dynamic: classifier
Dynamic: description
Dynamic: description-content-type
Dynamic: home-page
Dynamic: provides-extra
Dynamic: requires-dist
Dynamic: summary

`python-smpplib`
================

[![Version](https://img.shields.io/pypi/v/smpplib.svg?style=flat)](https://pypi.org/project/smpplib/#history)
[![Python versions](https://img.shields.io/pypi/pyversions/smpplib.svg?style=flat)](https://pypi.org/project/smpplib/)
[![PyPI downloads](https://img.shields.io/pypi/dm/smpplib.svg?style=flat)](https://pypi.org/project/smpplib/#files)
![License](https://img.shields.io/pypi/l/smpplib.svg?style=flat)
[![CircleCI](https://circleci.com/gh/python-smpplib/python-smpplib.svg?style=svg)](https://circleci.com/gh/python-smpplib/python-smpplib)

SMPP library for Python. Forked from [Google Code](https://code.google.com/p/smpplib/).

Example:

```python
import logging
import sys

import smpplib.gsm
import smpplib.client
import smpplib.consts

# if you want to know what's happening
logging.basicConfig(level='DEBUG')

# Two parts, UCS2, SMS with UDH
parts, encoding_flag, msg_type_flag = smpplib.gsm.make_parts(u'Привет мир!\n'*10)

client = smpplib.client.Client('example.com', SOMEPORTNUMBER, allow_unknown_opt_params=True)

# Print when obtain message_id
client.set_message_sent_handler(
    lambda pdu: sys.stdout.write('sent {} {}\n'.format(pdu.sequence, pdu.message_id)))
client.set_message_received_handler(
    lambda pdu: sys.stdout.write('delivered {}\n'.format(pdu.receipted_message_id)))

client.connect()
client.bind_transceiver(system_id='login', password='secret')

for part in parts:
    pdu = client.send_message(
        source_addr_ton=smpplib.consts.SMPP_TON_INTL,
        #source_addr_npi=smpplib.consts.SMPP_NPI_ISDN,
        # Make sure it is a byte string, not unicode:
        source_addr='SENDERPHONENUM',

        dest_addr_ton=smpplib.consts.SMPP_TON_INTL,
        #dest_addr_npi=smpplib.consts.SMPP_NPI_ISDN,
        # Make sure thease two params are byte strings, not unicode:
        destination_addr='PHONENUMBER',
        short_message=part,

        data_coding=encoding_flag,
        esm_class=msg_type_flag,
        registered_delivery=True,
    )
    print(pdu.sequence)
    
# Enters a loop, waiting for incoming PDUs
client.listen()
```
You also may want to listen in a thread:
```python
from threading import Thread
t = Thread(target=client.listen)
t.start()
```
**Note:** When listening, the client will automatically send an `enquire_link` command when the socket timeouts. You may override that behavior by passing `auto_send_enquire_link=False` as an argument to `listen()`. In that case, `socket.timeout` exceptions will bubble up.

The client supports setting a custom generator that produces sequence numbers for the PDU packages. Per default a simple in memory generator is used which in conclusion is reset on (re)instantiation of the client, e.g. by an application restart. If you want to keep the sequence number to be persisted across restarts you can implement your own storage backed generator.

Example:

```python
import smpplib.client

import mymodule

generator = mymodule.PersistentSequenceGenerator()
client = smpplib.client.Client('example.com', SOMEPORTNUMBER, sequence_generator=generator)
...
```
