08:47:43.748574 9884 BSC_Tests.ttcn:3129 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_si2_ncc_permitted'.
08:47:44.760851 9884 BSC_Tests.ttcn:3129 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_si2_ncc_permitted' was executed successfully (exit status: 0).
08:47:44.761242 9884 BSC_Tests.ttcn:3129 Test case TC_si2_ncc_permitted started.
08:47:44.761372 9884 BSC_Tests.ttcn:3129 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_si2_ncc_permitted.
08:47:44.761725 9884 BSC_Tests.ttcn:3129 Port IPA_CTRL was started.
08:47:44.761819 9884 BSC_Tests.ttcn:3129 Port RSL_CCHAN[0] was started.
08:47:44.762001 9884 BSC_Tests.ttcn:3129 Port RSL_CCHAN[1] was started.
08:47:44.762163 9884 BSC_Tests.ttcn:3129 Port RSL_CCHAN[2] was started.
08:47:44.762346 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][0] was started.
08:47:44.762633 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][1] was started.
08:47:44.762960 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][2] was started.
08:47:44.763234 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[0][3] was started.
08:47:44.763427 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][0] was started.
08:47:44.763589 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][1] was started.
08:47:44.763743 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][2] was started.
08:47:44.763905 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[1][3] was started.
08:47:44.764062 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][0] was started.
08:47:44.764152 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][1] was started.
08:47:44.764237 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][2] was started.
08:47:44.764312 9884 BSC_Tests.ttcn:3129 Port IPA_RSL[2][3] was started.
08:47:44.764387 9884 BSC_Tests.ttcn:3129 Port IPA was started.
08:47:44.764463 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CTRL was started.
08:47:44.764540 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][0] was started.
08:47:44.764617 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][1] was started.
08:47:44.764692 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][2] was started.
08:47:44.764765 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[0][3] was started.
08:47:44.764838 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][0] was started.
08:47:44.764913 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][1] was started.
08:47:44.764984 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][2] was started.
08:47:44.765058 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[1][3] was started.
08:47:44.765133 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][0] was started.
08:47:44.765206 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][1] was started.
08:47:44.765279 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][2] was started.
08:47:44.765352 9884 BSC_Tests.ttcn:3129 Port IPA_CFG_PORT[2][3] was started.
08:47:44.765425 9884 BSC_Tests.ttcn:3129 Port BSCVTY was started.
08:47:44.765501 9884 BSC_Tests.ttcn:3129 Port STPVTY was started.
08:47:44.765575 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CFG_PORT[0] was started.
08:47:44.765650 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CFG_PORT[1] was started.
08:47:44.765723 9884 BSC_Tests.ttcn:3129 Port SCCPLITE_IPA_CFG_PORT[2] was started.
08:47:44.765797 9884 BSC_Tests.ttcn:3129 Port BSSAP was started.
08:47:44.765871 9884 BSC_Tests.ttcn:3129 Port BSSAP_LE was started.
08:47:44.765945 9884 BSC_Tests.ttcn:3129 Component type BSC_Tests.test_CT was initialized.
08:47:44.766053 9884 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
08:47:44.766684 9884 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
08:47:44.766819 9884 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
08:47:44.766985 9884 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
08:47:44.767115 9884 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:47:44.767215 9884 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:47:44.767309 9884 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:47:44.767520 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
08:47:44.767674 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.767791 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:47:44.767876 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:47:44.767959 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:47:44.768040 9884 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:47:44.768119 9884 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:47:44.768206 9884 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
08:47:44.768294 9884 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
08:47:44.768379 9884 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
08:47:44.768496 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
08:47:44.768706 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.768876 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.768970 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:47:44.769056 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
08:47:44.769147 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.769251 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:44.769379 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.769638 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
08:47:44.769809 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.769963 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.770147 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.770246 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
08:47:44.770487 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
08:47:44.770637 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.770744 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
08:47:44.770841 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.771068 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
08:47:44.771228 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.771574 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.771819 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.771931 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
08:47:44.772030 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
08:47:44.772151 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.772264 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
08:47:44.772422 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.772607 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
08:47:44.772766 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.772910 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.773083 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.773178 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
08:47:44.773261 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
08:47:44.773347 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.773437 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
08:47:44.773557 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.773704 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
08:47:44.773848 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.773985 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.774149 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.774242 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
08:47:44.774348 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
08:47:44.774447 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.774536 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:47:44.774657 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.774777 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
08:47:44.775015 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.775238 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.775353 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
08:47:44.775451 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
08:47:44.775542 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.775640 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:44.775766 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.775956 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
08:47:44.776105 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.776248 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.776420 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.776520 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
08:47:44.776632 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
08:47:44.776726 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.776819 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:47:44.776954 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.777118 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 9
08:47:44.777279 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.777431 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.777603 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.777703 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 9
08:47:44.777796 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
08:47:44.777892 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.777991 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:47:44.778125 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.778284 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 10
08:47:44.778623 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.778856 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.779038 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.779114 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 10
08:47:44.779183 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
08:47:44.779252 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.779327 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "ncc-permitted 6 7 8"
08:47:44.779439 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.779726 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 11
08:47:44.779955 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.780082 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.780224 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.780295 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 11
08:47:44.780362 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
08:47:44.780431 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.780502 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:47:44.780598 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.780970 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
08:47:44.781081 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.781211 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.781277 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
08:47:44.781340 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
08:47:44.781402 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.781466 9884 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
08:47:44.781533 9884 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
08:47:44.781603 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:44.781692 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.781912 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 13
08:47:44.782020 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.782115 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.782242 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.782336 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 13
08:47:44.782401 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 13 was extracted from the queue of BSCVTY.
08:47:44.782467 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.782531 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:47:44.782615 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.782729 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 14
08:47:44.782827 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.782917 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.783031 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.783095 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 14
08:47:44.783157 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 14 was extracted from the queue of BSCVTY.
08:47:44.783220 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.783280 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:47:44.783355 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.783750 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 15
08:47:44.783859 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.783950 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.784062 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.784126 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 15
08:47:44.784187 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 15 was extracted from the queue of BSCVTY.
08:47:44.784249 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.784311 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:44.784403 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.784509 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 16
08:47:44.784601 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.784691 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:44.784797 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:44.784859 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 16
08:47:44.784918 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 16 was extracted from the queue of BSCVTY.
08:47:44.784980 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.785038 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:44.785111 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.785193 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
08:47:44.785612 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.785716 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.785791 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
08:47:44.785846 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
08:47:44.785901 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.785962 9884 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:47:44.798371 11670 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:44.798582 11670 - TTCN-3 Parallel Test Component started on 8fbedb33933a. Component reference: VirtMSC-STATS(251), component type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS. Version: 11.1.0.
08:47:44.798684 11670 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:47:44.798858 11670 - Connected to MC.
08:47:44.798955 11670 - Initializing variables, timers and ports of component type StatsD_Checker.StatsD_Checker_CT inside testcase TC_si2_ncc_permitted.
08:47:44.799019 9884 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 251, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:47:44.799339 9884 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(251).
08:47:44.799466 9884 StatsD_Checker.ttcnpp:417 Function was started.
08:47:44.799525 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
08:47:44.799595 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.799816 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 18
08:47:44.799915 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.799999 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.800051 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 18
08:47:44.800101 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 18 was extracted from the queue of BSCVTY.
08:47:44.800149 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.800200 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
08:47:44.800262 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.800385 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 19
08:47:44.800462 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.800537 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.800586 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 19
08:47:44.800632 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 19 was extracted from the queue of BSCVTY.
08:47:44.800698 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.800748 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
08:47:44.800806 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.801209 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 20
08:47:44.801284 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.801739 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.801915 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 20
08:47:44.802073 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 20 was extracted from the queue of BSCVTY.
08:47:44.802157 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.802445 9884 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:47:44.804012 11670 - Port STATSVTY was started.
08:47:44.804223 11670 - Port STATSD_PROC was started.
08:47:44.804300 11670 - Port STATS was started.
08:47:44.804345 11670 - Component type StatsD_Checker.StatsD_Checker_CT was initialized.
08:47:44.804655 11670 - Starting function main("127.0.0.1", 8125, 5.000000).
08:47:44.805314 11670 StatsD_Checker.ttcnpp:125 Mapping port VirtMSC-STATS(251):STATS to system:STATS.
08:47:44.805512 11670 StatsD_Checker.ttcnpp:125 Port STATS was mapped to system:STATS.
08:47:44.805719 11670 StatsD_Checker.ttcnpp:125 Map operation of VirtMSC-STATS(251):STATS to system:STATS finished.
08:47:44.806178 11670 StatsD_Checker.ttcnpp:126 entering f__IPL4__PROVIDER__listen: 127.0.0.1:8125 / UDP
08:47:44.808794 11670 StatsD_Checker.ttcnpp:134 Mapping port VirtMSC-STATS(251):STATSVTY to system:STATSVTY.
08:47:44.809711 11670 StatsD_Checker.ttcnpp:134 Message enqueued on STATSVTY from system integer : 2 id 1
08:47:44.809888 11670 StatsD_Checker.ttcnpp:134 Port STATSVTY was mapped to system:STATSVTY.
08:47:44.809957 11670 StatsD_Checker.ttcnpp:134 Map operation of VirtMSC-STATS(251):STATSVTY to system:STATSVTY finished.
08:47:44.810280 11670 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 1,
        prompt := "OsmoBSC> ",
        has_wildcards := false
    }
}
08:47:44.810451 11670 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 2,
        prompt := "OsmoBSC# ",
        has_wildcards := false
    }
}
08:47:44.810502 11670 Osmocom_VTY_Functions.ttcn:59 Sent on STATSVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : {
    prompt := {
        id := 3,
        prompt := "OsmoBSC(*)",
        has_wildcards := true
    }
}
08:47:44.810777 11670 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "enable"
08:47:44.810912 11670 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.811012 11670 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:47:44.811040 11670 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:47:44.811064 11670 Osmocom_VTY_Functions.ttcn:74 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:47:44.811086 11670 Osmocom_VTY_Functions.ttcn:75 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:47:44.811219 11670 Osmocom_VTY_Functions.ttcn:85 Matching on port STATSVTY failed: Type of the first message in the queue is not charstring.
08:47:44.811336 11670 Osmocom_VTY_Functions.ttcn:86 Matching on port STATSVTY succeeded: 2 with ? matched
08:47:44.811391 11670 Osmocom_VTY_Functions.ttcn:86 Receive operation on port STATSVTY succeeded, message from system(): integer : 2 id 1
08:47:44.811424 11670 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of STATSVTY.
08:47:44.811476 11671 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:44.811580 11670 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 2
08:47:44.811617 11671 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_si2_ncc_permitted.
08:47:44.811684 9884 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 252, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:47:44.811725 9884 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
08:47:44.811740 11670 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.811810 11670 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.811836 11670 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:47:44.811867 11670 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of STATSVTY.
08:47:44.811916 11670 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.811959 11670 Osmocom_VTY_Functions.ttcn:105 Sent on STATSVTY to system charstring : "stats reset"
08:47:44.811996 11670 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:44.812059 11670 Osmocom_VTY_Functions.ttcn:71 Message enqueued on STATSVTY from system charstring : "OsmoBSC# " id 3
08:47:44.812099 11670 Osmocom_VTY_Functions.ttcn:72 Matching on port STATSVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:44.812137 11670 Osmocom_VTY_Functions.ttcn:73 Matching on port STATSVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:44.812159 11670 Osmocom_VTY_Functions.ttcn:73 Receive operation on port STATSVTY succeeded, message from system(): charstring : "OsmoBSC# " id 3
08:47:44.812180 11670 Osmocom_VTY_Functions.ttcn:73 Message with id 3 was extracted from the queue of STATSVTY.
08:47:44.812202 11670 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:44.813670 11671 - Component type SCCP_Emulation.SCCP_CT was initialized.
08:47:44.816556 11672 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:44.816659 11672 - Initializing variables, timers and ports of component type M3UA_Emulation.M3UA_CT inside testcase TC_si2_ncc_permitted.
08:47:44.816685 9884 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 253, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
08:47:44.816707 9884 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(253):SCTP_PORT to system:sctp.
08:47:44.818211 11672 - Component type M3UA_Emulation.M3UA_CT was initialized.
08:47:44.818264 9884 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(253):SCTP_PORT to system:sctp finished.
08:47:44.818287 9884 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(253):MTP3_SP_PORT and VirtMSC-SCCP(252):MTP3_SCCP_PORT.
08:47:44.818661 9884 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(253):MTP3_SP_PORT and VirtMSC-SCCP(252):MTP3_SCCP_PORT finished.
08:47:44.818682 9884 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({
    local_sctp_port := 23905,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 1) on component VirtMSC-M3UA(253).
08:47:44.818726 9884 SCCP_Adapter.ttcnpp:127 Function was started.
08:47:44.818748 9884 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(252):SCCP_SP_PORT.
08:47:44.818789 11672 - Starting function f_M3UA_Emulation({
    local_sctp_port := 23905,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 1).
08:47:44.818941 9884 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(252):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-d77fb81d.
08:47:44.819034 9884 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(252):SCCP_SP_PORT.
08:47:44.819057 9884 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(252):SCCP_SP_PORT finished.
08:47:44.819078 9884 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}) on component VirtMSC-SCCP(252).
08:47:44.819127 9884 SCCP_Adapter.ttcnpp:165 Function was started.
08:47:44.819240 9884 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(252) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 0,
        pdu := {
            bssmap := {
                reset := {
                    messageType := '30'O ("0"),
                    cause := {
                        elementIdentifier := '04'O,
                        lengthIndicator := 0,
                        causeValue := '0000000'B,
                        extensionCauseValue := '0'B,
                        spare1 := omit
                    },
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
}
08:47:44.819274 9884 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 0,
    pdu := {
        bssmap := {
            reset := {
                messageType := '30'O ("0"),
                cause := {
                    elementIdentifier := '04'O,
                    lengthIndicator := 0,
                    causeValue := '0000000'B,
                    extensionCauseValue := '0'B,
                    spare1 := omit
                },
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:47:44.819320 9884 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
08:47:44.819329 11671 - Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 185,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 254
}).
08:47:44.819347 9884 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := omit,
    returnOption := omit,
    userData := '000430040100'O,
    importance := omit
}
08:47:44.819381 9884 BSC_Tests.ttcn:899 Start timer T: 5 s
08:47:45.027690 9884 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(252) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := '000131'O,
    importance := omit
} id 1
08:47:45.027739 9884 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
08:47:45.027880 9884 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: {
    discriminator := '0'B,
    spare := '0000000'B,
    dlci := omit,
    lengthIndicator := 1,
    pdu := {
        bssmap := {
            resetAck := {
                messageType := '31'O ("1"),
                a_InterfaceSelectorForReset := omit,
                osmuxSupport := omit
            }
        }
    }
}
08:47:45.027977 9884 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:47:45.028030 9884 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
08:47:45.028057 9884 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(252): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : {
    calledAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111001'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    callingAddress := {
        addressIndicator := {
            pointCodeIndic := '1'B,
            ssnIndicator := '1'B,
            globalTitleIndic := '0000'B,
            routingIndicator := '1'B
        },
        signPointCode := '00000010111011'B,
        subsystemNumber := 254,
        globalTitle := omit
    },
    sequenceControl := '00000000'B,
    returnOption := '00000000'B,
    userData := {
        discriminator := '0'B,
        spare := '0000000'B,
        dlci := omit,
        lengthIndicator := 1,
        pdu := {
            bssmap := {
                resetAck := {
                    messageType := '31'O ("1"),
                    a_InterfaceSelectorForReset := omit,
                    osmuxSupport := omit
                }
            }
        }
    },
    importance := omit
} id 1
08:47:45.028083 9884 BSC_Tests.ttcn:901 Message with id 1 was extracted from the queue of BSSAP.
08:47:45.028106 9884 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
08:47:45.028148 9884 BSSAP_LE_Adapter.ttcn:95 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
08:47:45.041066 11673 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:45.041230 11673 - TTCN-3 Parallel Test Component started on 8fbedb33933a. Component reference: VirtSMLC-SCCP(254), component type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP. Version: 11.1.0.
08:47:45.041307 11673 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:47:45.041506 11673 - Connected to MC.
08:47:45.041574 11673 - Initializing variables, timers and ports of component type SCCP_Emulation.SCCP_CT inside testcase TC_si2_ncc_permitted.
08:47:45.041668 9884 BSSAP_LE_Adapter.ttcn:95 PTC was created. Component reference: 254, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
08:47:45.041793 9884 BSSAP_LE_Adapter.ttcn:101 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
08:47:45.045785 11673 - Port SCCP_SP_PORT was started.
08:47:45.045938 11673 - Port MTP3_SCCP_PORT was started.
08:47:45.046068 11673 - Component type SCCP_Emulation.SCCP_CT was initialized.
08:47:45.050218 11674 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:45.050293 11674 - TTCN-3 Parallel Test Component started on 8fbedb33933a. Component reference: VirtSMLC-M3UA(255), component type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA. Version: 11.1.0.
08:47:45.050336 11674 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:47:45.050396 11674 - Connected to MC.
08:47:45.050425 11674 - Initializing variables, timers and ports of component type M3UA_Emulation.M3UA_CT inside testcase TC_si2_ncc_permitted.
08:47:45.050446 9884 BSSAP_LE_Adapter.ttcn:101 PTC was created. Component reference: 255, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
08:47:45.050483 9884 BSSAP_LE_Adapter.ttcn:102 Mapping port VirtSMLC-M3UA(255):SCTP_PORT to system:sctp.
08:47:45.052401 11674 - Port MTP3_SP_PORT was started.
08:47:45.052475 11674 - Port SCTP_PORT was started.
08:47:45.052502 11674 - Component type M3UA_Emulation.M3UA_CT was initialized.
08:47:45.052540 11674 - Port SCTP_PORT was mapped to system:sctp.
08:47:45.052593 9884 BSSAP_LE_Adapter.ttcn:102 Map operation of VirtSMLC-M3UA(255):SCTP_PORT to system:sctp finished.
08:47:45.052619 9884 BSSAP_LE_Adapter.ttcn:104 Connecting ports VirtSMLC-M3UA(255):MTP3_SP_PORT and VirtSMLC-SCCP(254):MTP3_SCCP_PORT.
08:47:45.052940 11673 - Port MTP3_SCCP_PORT is waiting for connection from VirtSMLC-M3UA(255):MTP3_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-b173f483.
08:47:45.053013 11674 - Port MTP3_SP_PORT has established the connection with VirtSMLC-SCCP(254):MTP3_SCCP_PORT using transport type UNIX.
08:47:45.053102 11673 - Port MTP3_SCCP_PORT has accepted the connection from VirtSMLC-M3UA(255):MTP3_SP_PORT.
08:47:45.053120 9884 BSSAP_LE_Adapter.ttcn:104 Connect operation on VirtSMLC-M3UA(255):MTP3_SP_PORT and VirtSMLC-SCCP(254):MTP3_SCCP_PORT finished.
08:47:45.053146 9884 BSSAP_LE_Adapter.ttcn:105 Starting function f_M3UA_Emulation({
    local_sctp_port := 23908,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 6) on component VirtSMLC-M3UA(255).
08:47:45.053206 9884 BSSAP_LE_Adapter.ttcn:105 Function was started.
08:47:45.053244 9884 BSC_Tests.ttcn:1290 Connecting ports mtc:BSSAP_LE and VirtSMLC-SCCP(254):SCCP_SP_PORT.
08:47:45.053322 11674 - Starting function f_M3UA_Emulation({
    local_sctp_port := 23908,
    local_ip_addr := "127.0.0.1",
    remote_sctp_port := 2905,
    remote_ip_addr := "127.0.0.1"
}, 6).
08:47:45.053623 9884 BSC_Tests.ttcn:1290 Port BSSAP_LE is waiting for connection from VirtSMLC-SCCP(254):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-9033e71d.
08:47:45.053679 11673 - Port SCCP_SP_PORT has established the connection with mtc:BSSAP_LE using transport type UNIX.
08:47:45.053785 9884 BSC_Tests.ttcn:1290 Port BSSAP_LE has accepted the connection from VirtSMLC-SCCP(254):SCCP_SP_PORT.
08:47:45.053822 9884 BSC_Tests.ttcn:1290 Connect operation on mtc:BSSAP_LE and VirtSMLC-SCCP(254):SCCP_SP_PORT finished.
08:47:45.053856 9884 BSSAP_LE_Adapter.ttcn:122 Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 190,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 252
}) on component VirtSMLC-SCCP(254).
08:47:45.053928 9884 BSSAP_LE_Adapter.ttcn:122 Function was started.
08:47:45.053968 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
08:47:45.054031 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.054034 11674 M3UA_Emulation.ttcn:512 *************************************************
08:47:45.054088 11674 M3UA_Emulation.ttcn:513 M3UA emulation initiated, the test can be started
08:47:45.054120 11674 M3UA_Emulation.ttcn:514 *************************************************
08:47:45.054229 11673 - Starting function SCCPStart({
    sio := {
        ni := '00'B,
        prio := '00'B,
        si := '0011'B
    },
    opc := 190,
    dpc := 187,
    sls := 0,
    sccp_serviceType := "mtp3_itu",
    ssn := 252
}).
08:47:45.054800 11673 SCCP_Emulation.ttcn:1453 v_sccp_pdu_maxlen:268
08:47:45.054857 11674 M3UA_Emulation.ttcn:554 Sent on SCTP_PORT to system @SCTPasp_Types.ASP_SCTP_ConnectFrom : {
    local_hostname := "127.0.0.1",
    local_portnumber := 23908,
    peer_hostname := "127.0.0.1",
    peer_portnumber := 2905
}
08:47:45.058283 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" id 21
08:47:45.058449 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 22
08:47:45.062603 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.066098 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.068429 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:47:45.070516 9884 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:47:45.071933 9884 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" with ? matched
08:47:45.073125 9884 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "
Current configuration:
!
password foo
!
log stderr
 logging filter all 1
 logging color 1
 logging print category-hex 0
 logging print category 1
 logging print thread-id 0
 logging print extended-timestamp 1
 logging print level 1
 logging print file basename last
 logging level rll notice
 logging level mm notice
 logging level rr notice
 logging level rsl notice
 logging level nm notice
 logging level pag notice
 logging level meas notice
 logging level msc notice
 logging level ho notice
 logging level hodec notice
 logging level ref notice
 logging level ctrl notice
 logging level filter debug
 logging level pcu debug
 logging level lcls notice
 logging level chan notice
 logging level ts notice
 logging level as notice
 logging level cbs notice
 logging level lcs notice
 logging level asci notice
 logging level reset notice
 logging level loop notice
 logging level lglobal notice
 logging level llapd notice
 logging level linp notice
 logging level lmux notice
 logging level lmi notice
 logging level lmib notice
 logging level lsms notice
 logging level lctrl notice
 logging level lgtp notice
 logging level lstats notice
 logging level lgsup notice
 logging level loap notice
 logging level lss7 notice
 logging level lsccp notice
 logging level lsua notice
 logging level lm3ua notice
 logging level lmgcp notice
 logging level ljibuf notice
 logging level lrspro notice
 logging level lns notice
 logging level lbssgp notice
 logging level lnsdata notice
 logging level lnssignal notice
 logging level liuup notice
 logging level lpfcp notice
 logging level lcsn1 notice
 logging level lio notice
 logging level ltcap notice
log gsmtap 127.0.0.1
 logging filter all 1
 logging color 1
 logging print category-hex 1
 logging print category 0
 logging print thread-id 0
 logging timestamp 0
 logging print file 1
 logging level rll debug
 logging level mm debug
 logging level rr debug
 logging level rsl debug
 logging level nm debug
 logging level pag debug
 logging level meas debug
 logging level msc debug
 logging level ho debug
 logging level hodec debug
 logging level ref debug
 logging level ctrl debug
 logging level filter debug
 logging level pcu debug
 logging level lcls debug
 logging level chan debug
 logging level ts debug
 logging level as debug
 logging level cbs debug
 logging level lcs debug
 logging level asci debug
 logging level reset debug
 logging level loop debug
 logging level lglobal debug
 logging level llapd debug
 logging level linp debug
 logging level lmux debug
 logging level lmi debug
 logging level lmib debug
 logging level lsms debug
 logging level lctrl debug
 logging level lgtp debug
 logging level lstats debug
 logging level lgsup debug
 logging level loap debug
 logging level lss7 debug
 logging level lsccp debug
 logging level lsua debug
 logging level lm3ua debug
 logging level lmgcp debug
 logging level ljibuf debug
 logging level lrspro debug
 logging level lns debug
 logging level lbssgp debug
 logging level lnsdata debug
 logging level lnssignal debug
 logging level liuup debug
 logging level lpfcp debug
 logging level lcsn1 debug
 logging level lio debug
 logging level ltcap debug
!
stats interval 0
stats reporter statsd
  remote-ip 127.0.0.1
  remote-port 8125
  mtu 1024
  level subscriber
  prefix TTCN3
  flush-period 1
  enable
!
line vty
 no login
!
e1_input
 e1_line 0 driver ipa
 e1_line 0 port 0
 no e1_line 0 keepalive
 ipa bind 127.0.0.1
ctrl
 bind 127.0.0.1
cs7 instance 0
 network-indicator international
 point-code 0.23.3
 asp asp-clnt-msc-0 2905 1905 m3ua
  local-ip 0.0.0.0
  remote-ip 127.0.0.1
  role asp
  sctp-role client
  no shutdown
 sccp-address msc0
  routing-indicator PC
  point-code 0.23.1
  subsystem-number 254
 sccp-address msc1
  routing-indicator PC
  point-code 0.0.2
  subsystem-number 254
 sccp-address msc2
  routing-indicator PC
  point-code 0.0.3
  subsystem-number 254
network
 network country code 001
 mobile network code 01
 encryption a5 0 1 3
 neci 1
 paging any use tch 0
 handover 1
 handover1 window rxlev averaging 10
 handover1 window rxqual averaging 1
 handover1 window rxlev neighbor averaging 10
 handover1 power budget interval 6
 handover1 power budget hysteresis 3
 handover1 maximum distance 9999
 timer net T3113 10
 timer net T3212 30
 nri null add 0 1
 mgw 0
  remote-ip 127.0.0.1
 bts 0
  type osmo-bts
  band DCS1800
  cell_identity 0
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 10
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  access-control-class-rotate-quantum 1
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1234 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 4 7
  amr tch-f threshold ms 32 32 32
  amr tch-f hysteresis ms 8 8 8
  amr tch-f threshold bts 32 32 32
  amr tch-f hysteresis bts 8 8 8
  amr tch-f start-mode auto
  amr tch-h modes 0 2 4
  amr tch-h threshold ms 32 32
  amr tch-h hysteresis ms 8 8
  amr tch-h threshold bts 32 32
  amr tch-h hysteresis bts 8 8
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1234
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1234
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1234
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  ncc-permitted 6 7 8
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 1
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0001
  dtx uplink force
  dtx downlink
  base_station_id_code 11
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1235 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1235
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1235
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1235
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 2
  type osmo-bts
  band DCS1800
  cell_identity 1
  location_area_code 0x0002
  dtx uplink force
  dtx downlink
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 1236 0
  oml ipa stream-id 255 line 0
  neighbor-list mode manual-si5
  neighbor-list add arfcn 100
  neighbor-list add arfcn 200
  si5 neighbor-list add arfcn 10
  si5 neighbor-list add arfcn 20
  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode gprs
  gprs routing area 0
  gprs network-control-order nc0
  gprs power-control alpha 0
  gprs cell bvci 1236
  gprs cell timer blocking-timer 3
  gprs cell timer blocking-retries 3
  gprs cell timer unblocking-retries 3
  gprs cell timer reset-timer 3
  gprs cell timer reset-retries 3
  gprs cell timer suspend-timer 10
  gprs cell timer suspend-retries 3
  gprs cell timer resume-timer 10
  gprs cell timer resume-retries 3
  gprs cell timer capability-update-timer 10
  gprs cell timer capability-update-retries 3
  gprs nsei 1236
  gprs ns timer tns-block 3
  gprs ns timer tns-block-retries 3
  gprs ns timer tns-reset 3
  gprs ns timer tns-reset-retries 3
  gprs ns timer tns-test 30
  gprs ns timer tns-alive 3
  gprs ns timer tns-alive-retries 10
  gprs nsvc 0 nsvci 1236
  gprs nsvc 0 local udp port 23000
  gprs nsvc 0 remote ip 192.168.100.239
  gprs nsvc 0 remote udp port 23000
  gprs nsvc 1 nsvci 0
  gprs nsvc 1 local udp port 0
  gprs nsvc 1 remote ip 0.0.0.0
  gprs nsvc 1 remote udp port 0
  no force-combined-si
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4+CBCH
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 1
   rf_locked 0
   arfcn 873
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 2
   rf_locked 0
   arfcn 875
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
  trx 3
   rf_locked 0
   arfcn 877
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
 bts 3
  type osmo-bts
  band DCS1800
  cell_identity 3
  location_area_code 0x0003
  base_station_id_code 12
  ms max power 15
  cell reselection hysteresis 4
  rxlev access min 0
  radio-link-timeout 32
  channel allocator mode chan-req ascending
  channel allocator mode assignment ascending
  channel allocator mode handover ascending
  channel allocator mode vgcs-vbs ascending
  rach tx integer 9
  rach max transmission 7
  rach max-delay 63
  rach expiry-timeout 32
  channel-description attach 1
  channel-description bs-pa-mfrms 5
  channel-description bs-ag-blks-res 1
  no nch-position
  no access-control-class-ramping
  early-classmark-sending forbidden
  early-classmark-sending-3g allowed
  ipa unit-id 0 0
  oml ipa stream-id 255 line 0
  neighbor-list mode automatic
  codec-support fr hr efr amr
  amr tch-f modes 0 2 5 7
  amr tch-f threshold ms 13 25 37
  amr tch-f hysteresis ms 4 4 4
  amr tch-f threshold bts 13 25 37
  amr tch-f hysteresis bts 4 4 4
  amr tch-f start-mode auto
  amr tch-h modes 0 2 3 5
  amr tch-h threshold ms 16 24 32
  amr tch-h hysteresis ms 4 4 4
  amr tch-h threshold bts 16 24 32
  amr tch-h hysteresis bts 4 4 4
  amr tch-h start-mode auto
  gprs mode none
  bs-power-control
   mode static
  ms-power-control
   mode dyn-bts
   ctrl-interval 2
   step-size inc 4 red 2
   rxlev-thresh lower 32 upper 38
   rxlev-thresh-comp lower 10 12 upper 19 20
   rxqual-thresh lower 3 upper 0
   rxqual-thresh-comp lower 5 7 upper 15 18
   ci-thresh fr-efr disable
   ci-thresh fr-efr lower 13 upper 17
   ci-thresh-comp fr-efr lower 5 7 upper 15 18
   ci-thresh hr disable
   ci-thresh hr lower 16 upper 21
   ci-thresh-comp hr lower 5 7 upper 15 18
   ci-thresh amr-fr disable
   ci-thresh amr-fr lower 7 upper 11
   ci-thresh-comp amr-fr lower 5 7 upper 15 18
   ci-thresh amr-hr disable
   ci-thresh amr-hr lower 13 upper 17
   ci-thresh-comp amr-hr lower 5 7 upper 15 18
   ci-thresh sdcch disable
   ci-thresh sdcch lower 12 upper 16
   ci-thresh-comp sdcch lower 5 7 upper 15 18
   ci-thresh gprs disable
   ci-thresh gprs lower 18 upper 24
   ci-thresh-comp gprs lower 5 7 upper 15 18
  trx 0
   rf_locked 0
   arfcn 871
   nominal power 23
   max_power_red 20
   rsl e1 tei 0
   timeslot 0
    phys_chan_config CCCH+SDCCH4
    hopping enabled 0
   timeslot 1
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 2
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 3
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 4
    phys_chan_config TCH/F
    hopping enabled 0
   timeslot 5
    phys_chan_config TCH/H
    hopping enabled 0
   timeslot 6
    phys_chan_config PDCH
    hopping enabled 0
   timeslot 7
    phys_chan_config PDCH
    hopping enabled 0
msc 0
 codec-list fr1 fr2 fr3 hr1 hr3
 allow-emergency allow
 amr-config 12_2k forbidden
 amr-config 10_2k forbidden
 amr-config 7_95k forbidden
 amr-config 7_40k forbidden
 amr-config 6_70k forbidden
 amr-config 5_90k allowed
 amr-config 5_15k forbidden
 amr-config 4_75k forbidden
 amr-payload octet-aligned
 msc-addr msc0
 asp-protocol m3ua
 lcls-mode mgw-loop
 lcls-codec-mismatch forbidden
 nri add 1 255
msc 1
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc1
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 256 511
 no allow-attach
msc 2
 codec-list fr1 hr1 fr2 fr3 hr3
 allow-emergency deny
 amr-config 12_2k allowed
 amr-config 10_2k allowed
 amr-config 7_95k allowed
 amr-config 7_40k allowed
 amr-config 6_70k allowed
 amr-config 5_90k allowed
 amr-config 5_15k allowed
 amr-config 4_75k allowed
 amr-payload octet-aligned
 msc-addr msc2
 asp-protocol m3ua
 lcls-mode disabled
 lcls-codec-mismatch forbidden
 nri add 512 767
 no allow-attach
bsc
 mid-call-timeout 0
cbc
 mode disabled
 server
  local-port 48050
 client
  remote-ip 127.0.0.1
smlc
 enable
end" id 21
08:47:45.073150 9884 Osmocom_VTY_Functions.ttcn:85 Message with id 21 was extracted from the queue of BSCVTY.
08:47:45.073173 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.073192 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:45.073203 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 22
08:47:45.073214 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 22 was extracted from the queue of BSCVTY.
08:47:45.073224 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.073241 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:45.073261 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.073334 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
08:47:45.073352 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.073369 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.073391 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.073402 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
08:47:45.073413 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
08:47:45.073426 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.073436 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:47:45.073452 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.073492 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 24
08:47:45.073509 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.073524 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.073543 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.073553 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 24
08:47:45.073562 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 24 was extracted from the queue of BSCVTY.
08:47:45.073572 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.073583 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
08:47:45.073596 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.073630 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 25
08:47:45.073645 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.073660 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.073677 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.073687 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 25
08:47:45.073697 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
08:47:45.073707 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.073717 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:45.073728 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.073754 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 26
08:47:45.073769 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.073783 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.073801 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.073810 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 26
08:47:45.073820 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
08:47:45.073830 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.073839 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:45.073851 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.073873 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 27
08:47:45.073887 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.073903 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:45.073913 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 27
08:47:45.073922 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 27 was extracted from the queue of BSCVTY.
08:47:45.073934 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.073946 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:45.073958 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.073990 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 28
08:47:45.074005 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074019 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074047 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074059 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 28
08:47:45.074069 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
08:47:45.074079 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074089 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1"
08:47:45.074101 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074143 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 29
08:47:45.074158 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074173 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074191 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074201 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 29
08:47:45.074210 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 29 was extracted from the queue of BSCVTY.
08:47:45.074220 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074230 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
08:47:45.074242 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074271 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 30
08:47:45.074286 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074304 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074322 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074332 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 30
08:47:45.074342 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 30 was extracted from the queue of BSCVTY.
08:47:45.074351 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074361 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:45.074373 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074388 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 31
08:47:45.074403 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074416 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074435 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074444 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 31
08:47:45.074453 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 31 was extracted from the queue of BSCVTY.
08:47:45.074462 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074471 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:45.074482 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074495 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
08:47:45.074509 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074523 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:45.074533 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
08:47:45.074542 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
08:47:45.074551 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074561 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:45.074572 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074595 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 33
08:47:45.074609 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074623 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074640 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074649 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 33
08:47:45.074658 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 33 was extracted from the queue of BSCVTY.
08:47:45.074668 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074677 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2"
08:47:45.074688 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074704 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 34
08:47:45.074717 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074731 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074748 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074758 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 34
08:47:45.074767 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 34 was extracted from the queue of BSCVTY.
08:47:45.074777 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074786 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
08:47:45.074797 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074812 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 35
08:47:45.074827 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074842 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074858 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074868 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 35
08:47:45.074877 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 35 was extracted from the queue of BSCVTY.
08:47:45.074886 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.074895 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:45.074906 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.074921 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 36
08:47:45.074935 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.074949 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:45.074966 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:45.074975 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 36
08:47:45.074984 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 36 was extracted from the queue of BSCVTY.
08:47:45.074993 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.075002 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:47:45.075013 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:45.075026 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 37
08:47:45.075039 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:45.075054 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:45.075063 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 37
08:47:45.075072 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 37 was extracted from the queue of BSCVTY.
08:47:45.075081 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:45.075091 9884 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:47:45.078179 11675 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:45.078214 11675 - TTCN-3 Parallel Test Component started on 8fbedb33933a. Component reference: IPA-CTRL-CLI-IPA(256), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA. Version: 11.1.0.
08:47:45.078228 11675 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:47:45.078269 11675 - Connected to MC.
08:47:45.078283 11675 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_si2_ncc_permitted.
08:47:45.078354 9884 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 256, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:47:45.078371 9884 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(256):IPA_PORT to system:IPA_CODEC_PT.
08:47:45.079453 11675 - Port IPA_PORT was started.
08:47:45.079477 11675 - Port CFG_PORT was started.
08:47:45.079489 11675 - Port MTP3_SP_PORT was started.
08:47:45.079501 11675 - Port IPA_MGCP_PORT was started.
08:47:45.079512 11675 - Port IPA_RSL_PORT was started.
08:47:45.079523 11675 - Port IPA_OML_PORT was started.
08:47:45.079534 11675 - Port IPA_CTRL_PORT was started.
08:47:45.079545 11675 - Port IPA_SP_PORT was started.
08:47:45.079555 11675 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:47:45.079591 11675 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:47:45.079677 9884 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(256):IPA_PORT to system:IPA_CODEC_PT finished.
08:47:45.079692 9884 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT and mtc:IPA_CTRL.
08:47:45.079900 9884 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-2435f21f.
08:47:45.079972 11675 - Port IPA_CTRL_PORT has established the connection with mtc:IPA_CTRL using transport type UNIX.
08:47:45.080014 9884 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT.
08:47:45.080066 9884 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
08:47:45.080080 9884 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false) on component IPA-CTRL-CLI-IPA(256).
08:47:45.080157 9884 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
08:47:45.080173 9884 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
08:47:45.080273 11675 - Starting function main_client("127.0.0.1", 4249, "", 0, {
    ser_nr := "",
    name := "mahlzeit",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "0/1/2",
    osmo_rand := ""
}, false).
08:47:45.080490 11675 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :0 -> 127.0.0.1:4249 / TCP
08:47:45.081860 11675 IPA_Emulation.ttcnpp:409 Sent on IPA_CTRL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:47:45.081969 9884 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(256) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:47:45.081989 9884 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
08:47:45.082005 9884 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(256): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:47:45.082021 9884 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
08:47:45.082042 9884 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:47:45.087752 11676 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:45.087818 11676 - TTCN-3 Parallel Test Component started on 8fbedb33933a. Component reference: VirtMGW-MGCP-0(257), component type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0. Version: 11.1.0.
08:47:45.087846 11676 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:47:45.088053 11676 - Connected to MC.
08:47:45.088187 11676 - Initializing variables, timers and ports of component type MGCP_Emulation.MGCP_Emulation_CT inside testcase TC_si2_ncc_permitted.
08:47:45.088255 9884 BSC_Tests.ttcn:1073 PTC was created. Component reference: 257, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:47:45.088295 9884 BSC_Tests.ttcn:1074 Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := false
}, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(257).
08:47:45.088488 9884 BSC_Tests.ttcn:1074 Function was started.
08:47:45.088571 9884 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:47:45.088605 9884 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.815763.
08:47:45.088650 9884 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:47:45.088734 9884 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:47:45.088923 11675 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:47:45.089102 11675 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:47:45.089160 11675 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 1
08:47:45.089204 11675 IPA_Emulation.ttcnpp:921 Message with id 1 was extracted from the queue of IPA_CTRL_PORT.
08:47:45.089259 11675 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Encoding @Osmocom_CTRL_Types.CtrlMessage: {
    cmd := {
        verb := "GET",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:47:45.089428 11675 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Stream after encoding: "GET 815763297 bts.0.oml-connection-state"
08:47:45.090161 11675 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 815763297 bts.0.oml-connection-state")
}
08:47:45.090323 11675 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '47455420383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 815763297 bts.0.oml-connection-state")
}
08:47:45.090351 11676 - Port MGCP was started.
08:47:45.090406 11676 - Port MGCP_CLIENT was started.
08:47:45.090520 11676 - Port MGCP_CLIENT_MULTI was started.
08:47:45.090562 11676 - Port MGCP_PROC was started.
08:47:45.090611 11675 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0029EE0047455420383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
08:47:45.090681 11676 - Component type MGCP_Emulation.MGCP_Emulation_CT was initialized.
08:47:45.090728 11675 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:47:45.090813 11676 - Starting function main({
    create_cb := refers(MGCP_Emulation.ExpectedCreateCallback),
    unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback)
}, {
    callagent_ip := "127.0.0.1",
    callagent_udp_port := -1,
    mgw_ip := "127.0.0.1",
    mgw_udp_port := 2427,
    multi_conn_mode := false
}, "VirtMGW-MGCP-0").
08:47:45.091146 11676 MGCP_Emulation.ttcn:279 Mapping port VirtMGW-MGCP-0(257):MGCP to system:MGCP_CODEC_PT.
08:47:45.091214 11675 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 40295,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0038EE004745545F5245504C5920383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
} id 1
08:47:45.091266 11675 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0038EE004745545F5245504C5920383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O
08:47:45.091270 11676 MGCP_Emulation.ttcn:279 Port MGCP was mapped to system:MGCP_CODEC_PT.
08:47:45.091369 11676 MGCP_Emulation.ttcn:279 Map operation of VirtMGW-MGCP-0(257):MGCP to system:MGCP_CODEC_PT finished.
08:47:45.091447 11675 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 56,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '4745545F5245504C5920383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 815763297 bts.0.oml-connection-state degraded")
}
08:47:45.091499 11675 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 815763297 bts.0.oml-connection-state degraded")
} id 1
08:47:45.091528 11676 MGCP_Emulation.ttcn:281 entering f__IPL4__PROVIDER__listen: 127.0.0.1:2427 / UDP
08:47:45.091593 11675 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:45.091634 11675 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920383135373633323937206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465206465677261646564'O ("GET_REPLY 815763297 bts.0.oml-connection-state degraded")
} id 1
08:47:45.091662 11675 IPA_Emulation.ttcnpp:790 Message with id 1 was extracted from the queue of IPA_PORT.
08:47:45.091704 11675 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Stream before decoding: "GET_REPLY 815763297 bts.0.oml-connection-state degraded"
08:47:45.091805 11675 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 815763297 bts.0.oml-connection-state degraded
08:47:45.091828 11675 IPA_Emulation.ttcnpp:653 match_begin token: null_match
08:47:45.091849 11675 IPA_Emulation.ttcnpp:653 match_begin result: 0
08:47:45.091940 11675 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 815763297 bts.0.oml-connection-state degraded
08:47:45.091964 11675 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET)|(SET)))"
08:47:45.091987 11675 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
08:47:45.092007 11675 IPA_Emulation.ttcnpp:653 match_begin result: 3
08:47:45.092028 11675 IPA_Emulation.ttcnpp:653 match_begin data: _REPLY 815763297 bts.0.oml-connection-state degraded
08:47:45.092048 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:45.092068 11675 IPA_Emulation.ttcnpp:653 match_begin result: -1
08:47:45.092129 11675 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 815763297 bts.0.oml-connection-state degraded
08:47:45.092151 11675 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET_REPLY)|(SET_REPLY)))"
08:47:45.092171 11675 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
08:47:45.092189 11675 IPA_Emulation.ttcnpp:653 match_begin result: 9
08:47:45.092208 11675 IPA_Emulation.ttcnpp:653 match_begin data:  815763297 bts.0.oml-connection-state degraded
08:47:45.092226 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:45.092244 11675 IPA_Emulation.ttcnpp:653 match_begin result: 1
08:47:45.092265 11675 IPA_Emulation.ttcnpp:653 match_first data: 815763297 bts.0.oml-connection-state degraded
08:47:45.092283 11675 IPA_Emulation.ttcnpp:653 match_first token: " "
08:47:45.092301 11675 IPA_Emulation.ttcnpp:653 match_first result: 9
08:47:45.092320 11675 IPA_Emulation.ttcnpp:653 match_list data: 815763297 bts.0.oml-connection-state degraded
08:47:45.092338 11675 IPA_Emulation.ttcnpp:653 match_list result: 9
08:47:45.092356 11675 IPA_Emulation.ttcnpp:653 match_begin data:  bts.0.oml-connection-state degraded
08:47:45.092375 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:45.092393 11675 IPA_Emulation.ttcnpp:653 match_begin result: 1
08:47:45.092410 11675 IPA_Emulation.ttcnpp:653 match_first data: bts.0.oml-connection-state degraded
08:47:45.092434 11675 IPA_Emulation.ttcnpp:653 match_first token: " "
08:47:45.092452 11675 IPA_Emulation.ttcnpp:653 match_first result: 26
08:47:45.092469 11675 IPA_Emulation.ttcnpp:653 match_list data: bts.0.oml-connection-state degraded
08:47:45.092487 11675 IPA_Emulation.ttcnpp:653 match_list result: 26
08:47:45.092504 11675 IPA_Emulation.ttcnpp:653 match_begin data:  degraded
08:47:45.092522 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:45.092540 11675 IPA_Emulation.ttcnpp:653 match_begin result: 1
08:47:45.092557 11675 IPA_Emulation.ttcnpp:653 match_first data: degraded
08:47:45.092575 11675 IPA_Emulation.ttcnpp:653 match_first token: " "
08:47:45.092595 11675 IPA_Emulation.ttcnpp:653 match_first result: -1
08:47:45.092627 11675 IPA_Emulation.ttcnpp:653 match_list data: degraded
08:47:45.092641 11675 IPA_Emulation.ttcnpp:653 match_list result: -1
08:47:45.092693 11675 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Decoded @Osmocom_CTRL_Types.CtrlMessage: {
    resp := {
        verb := "GET_REPLY",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
08:47:45.092740 11675 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
}
08:47:45.092795 9884 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:47:45.092815 9884 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:47:45.092832 9884 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(256): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "815763297",
        variable := "bts.0.oml-connection-state",
        val := "degraded"
    }
} id 2
08:47:45.092847 9884 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
08:47:45.092861 9884 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:47:45.092875 9884 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:47:45.256247 11674 M3UA_Emulation.ttcn:560 Start timer T_Timer: 2 s
08:47:45.257084 11674 M3UA_Emulation.ttcn:561 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP_RESULT : {
    client_id := 8,
    error_status := false,
    error_message := omit
} id 1
08:47:45.257552 11674 M3UA_Emulation.ttcn:562 Matching on port SCTP_PORT succeeded:  matched
08:47:45.257668 11674 M3UA_Emulation.ttcn:562 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP_RESULT : {
    client_id := 8,
    error_status := false,
    error_message := omit
} id 1
08:47:45.257770 11674 M3UA_Emulation.ttcn:562 Message with id 1 was extracted from the queue of SCTP_PORT.
08:47:45.257841 11674 M3UA_Emulation.ttcn:569 SCTP_ConnectResult -> connection established from: "127.0.0.1":23908 to server: "127.0.0.1":2905 association #8
08:47:45.258024 11674 M3UA_Emulation.ttcn:579 Stop timer T_Timer: 2 s
08:47:45.258084 11674 M3UA_Emulation.ttcn:537 Start timer T_Assoc_restart: 60 s
08:47:45.258197 11674 M3UA_Emulation.ttcn:542 Start timer T_ASPUP_resend: 2 s
08:47:45.258250 11674 M3UA_Emulation.ttcn:543 Start timer T_ASPAC_resend: 2 s
08:47:45.259113 11674 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE : {
    client_id := 8,
    sac_state := SCTP_COMM_UP (0)
} id 2
08:47:45.259303 11674 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT succeeded:  matched
08:47:45.259368 11674 M3UA_Emulation.ttcn:668 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE : {
    client_id := 8,
    sac_state := SCTP_COMM_UP (0)
} id 2
08:47:45.259424 11674 M3UA_Emulation.ttcn:668 Message with id 2 was extracted from the queue of SCTP_PORT.
08:47:45.260645 11674 M3UA_Emulation.ttcn:959 enc_PDU_M3UA(): Encoding @M3UA_Types.PDU_M3UA: {
    m3UA_ASPUP := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0301'O,
        messageLength := 0,
        messageParameters := {
            aSP_Identifier := omit,
            info_String := omit
        }
    }
}
08:47:45.261566 11674 M3UA_Emulation.ttcn:959 enc_PDU_M3UA(): Stream after encoding: '0100030100000008'O
08:47:45.262079 11674 M3UA_Emulation.ttcn:959 Sent on SCTP_PORT to system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030100000008'O
}
08:47:45.263176 11674 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030400000008'O
} id 3
08:47:45.263472 11674 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
08:47:45.263666 11674 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
08:47:45.263809 11674 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030400000008'O
} id 3
08:47:45.263954 11674 M3UA_Emulation.ttcn:711 Message with id 3 was extracted from the queue of SCTP_PORT.
08:47:45.264155 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100030400000008'O
08:47:45.264725 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_ASPUP_Ack := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0304'O,
        messageLength := 8,
        messageParameters := {
            info_String := omit
        }
    }
}
08:47:45.265777 11674 M3UA_Emulation.ttcn:1189 enc_PDU_M3UA(): Encoding @M3UA_Types.PDU_M3UA: {
    m3UA_ASPAC := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0401'O,
        messageLength := 0,
        messageParameters := {
            traffic_Mode_Type := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
08:47:45.266135 11674 M3UA_Emulation.ttcn:1189 enc_PDU_M3UA(): Stream after encoding: '01000401000000100006000800000006'O
08:47:45.266215 11674 M3UA_Emulation.ttcn:1189 Sent on SCTP_PORT to system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '01000401000000100006000800000006'O
}
08:47:45.266583 11674 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030300000008'O
} id 4
08:47:45.266843 11674 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
08:47:45.267025 11674 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
08:47:45.267177 11674 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100030300000008'O
} id 4
08:47:45.267248 11674 M3UA_Emulation.ttcn:711 Message with id 4 was extracted from the queue of SCTP_PORT.
08:47:45.267315 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100030300000008'O
08:47:45.267554 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_BEAT := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0303'O,
        messageLength := 8,
        messageParameters := {
            heartbeat_Data := omit
        }
    }
}
08:47:45.267879 11674 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100020006000800000006'O
} id 5
08:47:45.267946 11674 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
08:47:45.268003 11674 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
08:47:45.268157 11674 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100020006000800000006'O
} id 5
08:47:45.268310 11674 M3UA_Emulation.ttcn:711 Message with id 5 was extracted from the queue of SCTP_PORT.
08:47:45.268453 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100000100000018000D0008000100020006000800000006'O
08:47:45.269124 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_NOTIFY := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0001'O,
        messageLength := 24,
        messageParameters := {
            status := {
                tag := '000D'O,
                lengthInd := 8,
                statusType := '0001'O,
                statusInfo := '0002'O
            },
            aSP_Identifier := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
08:47:45.269512 11674 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '01000403000000100006000800000006'O
} id 6
08:47:45.269661 11674 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
08:47:45.269805 11674 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
08:47:45.269959 11674 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '01000403000000100006000800000006'O
} id 6
08:47:45.270024 11674 M3UA_Emulation.ttcn:711 Message with id 6 was extracted from the queue of SCTP_PORT.
08:47:45.270082 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '01000403000000100006000800000006'O
08:47:45.270379 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_ASPAC_Ack := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0403'O,
        messageLength := 16,
        messageParameters := {
            traffic_Mode_Type := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
08:47:45.270861 11674 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100030006000800000006'O
} id 7
08:47:45.270943 11674 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
08:47:45.271003 11674 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
08:47:45.271064 11674 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '0100000100000018000D0008000100030006000800000006'O
} id 7
08:47:45.271120 11674 M3UA_Emulation.ttcn:711 Message with id 7 was extracted from the queue of SCTP_PORT.
08:47:45.271177 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '0100000100000018000D0008000100030006000800000006'O
08:47:45.271270 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_NOTIFY := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0001'O,
        messageLength := 24,
        messageParameters := {
            status := {
                tag := '000D'O,
                lengthInd := 8,
                statusType := '0001'O,
                statusInfo := '0003'O
            },
            aSP_Identifier := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            info_String := omit
        }
    }
}
08:47:45.271378 11674 M3UA_Emulation.ttcn:596 Message enqueued on SCTP_PORT from system @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '010002010000003000060008000000060012000C0000000200000003000400125246433436363620342E352E31000000'O
} id 8
08:47:45.271436 11674 M3UA_Emulation.ttcn:668 Matching on port SCTP_PORT failed: Type of the first message in the queue is not @SCTPasp_Types.ASP_SCTP_ASSOC_CHANGE.
08:47:45.271492 11674 M3UA_Emulation.ttcn:711 Matching on port SCTP_PORT succeeded:  matched
08:47:45.271552 11674 M3UA_Emulation.ttcn:711 Receive operation on port SCTP_PORT succeeded, message from system(): @SCTPasp_Types.ASP_SCTP : {
    client_id := 8,
    sinfo_stream := 0,
    sinfo_ppid := 3,
    data := '010002010000003000060008000000060012000C0000000200000003000400125246433436363620342E352E31000000'O
} id 8
08:47:45.271606 11674 M3UA_Emulation.ttcn:711 Message with id 8 was extracted from the queue of SCTP_PORT.
08:47:45.271658 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Stream before decoding: '010002010000003000060008000000060012000C0000000200000003000400125246433436363620342E352E31000000'O
08:47:45.271901 11674 M3UA_Emulation.ttcn:724 dec_PDU_M3UA(): Decoded @M3UA_Types.PDU_M3UA: {
    m3UA_DUNA := {
        version := '01'O,
        reserved := '00'O,
        messageClassAndType := '0201'O,
        messageLength := 48,
        messageParameters := {
            network_Appearance := omit,
            routing_Context := {
                tag := '0006'O,
                lengthInd := 8,
                routingContext := '00000006'O
            },
            affected_Point_Codes := {
                tag := '0012'O,
                lengthInd := 12,
                pointCodes := {
                    {
                        mask := '00'O,
                        affected_Point_Code := '000002'O
                    },
                    {
                        mask := '00'O,
                        affected_Point_Code := '000003'O
                    }
                }
            },
            info_String := {
                tag := '0004'O,
                lengthInd := 18,
                infoString := '5246433436363620342E352E3100'O
            }
        }
    }
}
08:47:46.092925 9884 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:47:46.093267 9884 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:47:46.106235 11677 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
08:47:46.106367 11677 - TTCN-3 Parallel Test Component started on 8fbedb33933a. Component reference: IPA-BTS0-TRX0-RSL-IPA(258), component type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA. Version: 11.1.0.
08:47:46.106475 11677 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
08:47:46.106639 11677 - Connected to MC.
08:47:46.106741 11677 - Initializing variables, timers and ports of component type IPA_Emulation.IPA_Emulation_CT inside testcase TC_si2_ncc_permitted.
08:47:46.106814 9884 BSC_Tests.ttcn:951 PTC was created. Component reference: 258, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:47:46.106916 9884 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: {
    site_id := 1234,
    bts_id := 0,
    trx_id := 0
}
08:47:46.106981 9884 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
08:47:46.107023 9884 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(258):IPA_PORT to system:IPA_CODEC_PT.
08:47:46.110007 11677 - Port IPA_PORT was started.
08:47:46.110095 11677 - Port CFG_PORT was started.
08:47:46.110141 11677 - Port MTP3_SP_PORT was started.
08:47:46.110181 11677 - Port IPA_MGCP_PORT was started.
08:47:46.110222 11677 - Port IPA_RSL_PORT was started.
08:47:46.110263 11677 - Port IPA_OML_PORT was started.
08:47:46.110347 11677 - Port IPA_CTRL_PORT was started.
08:47:46.110482 11677 - Port IPA_SP_PORT was started.
08:47:46.110534 11677 - Component type IPA_Emulation.IPA_Emulation_CT was initialized.
08:47:46.110690 11677 - Port IPA_PORT was mapped to system:IPA_CODEC_PT.
08:47:46.110895 9884 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(258):IPA_PORT to system:IPA_CODEC_PT finished.
08:47:46.110962 9884 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
08:47:46.111527 9884 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-28728b6e.
08:47:46.111720 11677 - Port CFG_PORT has established the connection with mtc:IPA_CFG_PORT[0][0] using transport type UNIX.
08:47:46.111846 9884 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT.
08:47:46.111951 9884 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
08:47:46.112012 9884 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
08:47:46.112498 9884 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-4b68ab76.
08:47:46.112665 11677 - Port IPA_RSL_PORT has established the connection with mtc:IPA_RSL[0][0] using transport type UNIX.
08:47:46.112806 9884 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT.
08:47:46.112917 9884 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
08:47:46.112972 9884 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true) on component IPA-BTS0-TRX0-RSL-IPA(258).
08:47:46.113373 9884 BSC_Tests.ttcn:969 Function was started.
08:47:46.113485 9884 BSC_Tests.ttcn:976 Start timer T: 10 s
08:47:46.113775 11677 - Starting function main_client("127.0.0.1", 3003, "", 10000, {
    ser_nr := "",
    name := "Osmocom TTCN-3 BTS Simulator",
    location1 := "",
    location2 := "",
    equip_version := "",
    sw_version := "",
    ip_addr := "",
    mac_addr := "",
    unit_id := "1234/0/0",
    osmo_rand := ""
}, true).
08:47:46.114449 11677 IPA_Emulation.ttcnpp:330 entering f__IPL4__PROVIDER__connect: :10000 -> 127.0.0.1:3003 / TCP
08:47:46.117579 11677 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Encoding @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:47:46.117875 11677 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Stream after encoding: '06'O
08:47:46.118355 11677 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:47:46.118596 11677 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
}
08:47:46.118762 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '06'O
}
08:47:46.118859 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0001FE06'O
08:47:46.118998 11677 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0001FE06'O
}
08:47:46.119899 11677 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
}
08:47:46.120058 9884 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:47:46.120117 9884 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:47:46.120147 9884 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
08:47:46.120171 9884 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_UP (1),
    conn_id := 1,
    id_resp := omit
} id 1
08:47:46.120195 9884 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
08:47:46.121242 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0011FE0401080107010201030104010501010100'O
} id 1
08:47:46.121273 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0011FE0401080107010201030104010501010100'O
08:47:46.121450 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 17,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '0401080107010201030104010501010100'O
}
08:47:46.121485 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:47:46.121519 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0001FE06'O
} id 2
08:47:46.121545 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0001FE06'O
08:47:46.121563 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '06'O
}
08:47:46.121581 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:47:46.121684 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:47:46.121764 11677 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '0401080107010201030104010501010100'O
} id 1
08:47:46.121790 11677 IPA_Emulation.ttcnpp:774 Message with id 1 was extracted from the queue of IPA_PORT.
08:47:46.121834 11677 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Stream before decoding: '0401080107010201030104010501010100'O
08:47:46.121890 11677 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Decoded @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
08:47:46.121931 11677 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_GET (4),
    u := {
        get := {
            {
                len := 1,
                tag := IPAC_IDTAG_UNITID (8)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_MACADDR (7)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION1 (2)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_LOCATION2 (3)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_EQUIPVERS (4)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SWVERSION (5)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_UNITNAME (1)
            },
            {
                len := 1,
                tag := IPAC_IDTAG_SERNR (0)
            }
        }
    }
}
08:47:46.122214 11677 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Encoding @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
08:47:46.122285 11677 IPA_Emulation.ttcnpp:497 enc_PDU_IPA_CCM(): Stream after encoding: '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
08:47:46.122340 11677 IPA_Emulation.ttcnpp:498 CCM Tx:{
    msg_type := IPAC_MSGT_ID_RESP (5),
    u := {
        resp := {
            {
                len := 0,
                tag := IPAC_IDTAG_UNITID (8),
                data := '313233342F302F3000'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_MACADDR (7),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION1 (2),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_LOCATION2 (3),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_EQUIPVERS (4),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SWVERSION (5),
                data := '00'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_UNITNAME (1),
                data := '4F736D6F636F6D205454434E2D33204254532053696D756C61746F7200'O
            },
            {
                len := 0,
                tag := IPAC_IDTAG_SERNR (0),
                data := '00'O
            }
        }
    }
}
08:47:46.122436 11677 IPA_Emulation.ttcnpp:499 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:47:46.122455 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    payloadData := '05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:47:46.122485 11677 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
08:47:46.122511 11677 IPA_Emulation.ttcnpp:499 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0045FE05000A08313233342F302F30000002070000020200000203000002040000020500001E014F736D6F636F6D205454434E2D33204254532053696D756C61746F720000020000'O
}
08:47:46.122576 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT succeeded:  matched
08:47:46.122597 11677 IPA_Emulation.ttcnpp:774 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_CCM (254),
    streamIdExt := omit,
    msg := '06'O
} id 2
08:47:46.122614 11677 IPA_Emulation.ttcnpp:774 Message with id 2 was extracted from the queue of IPA_PORT.
08:47:46.122630 11677 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Stream before decoding: '06'O
08:47:46.122646 11677 IPA_Emulation.ttcnpp:775 dec_PDU_IPA_CCM(): Decoded @IPA_Types.PDU_IPA_CCM: {
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:47:46.122662 11677 IPA_Emulation.ttcnpp:776 CCM Rx:{
    msg_type := IPAC_MSGT_ID_ACK (6),
    u := omit
}
08:47:46.122689 11677 IPA_Emulation.ttcnpp:399 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
}
08:47:46.122727 9884 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:47:46.122771 9884 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
08:47:46.122795 9884 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_IPA_Event : {
    ev_type := ASP_IPA_EVENT_ID_ACK (3),
    conn_id := 1,
    id_resp := omit
} id 2
08:47:46.122814 9884 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
08:47:46.122831 9884 BSC_Tests.ttcn:979 Stop timer T: 10 s
08:47:46.122853 9884 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:47:46.122874 9884 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.848471.
08:47:46.122909 9884 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:47:46.122935 9884 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:47:46.122959 11675 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_CTRL_PORT from mtc @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:47:46.122990 11675 IPA_Emulation.ttcnpp:921 Matching on port IPA_CTRL_PORT succeeded:  matched
08:47:46.123056 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:47:46.123067 11675 IPA_Emulation.ttcnpp:921 Receive operation on port IPA_CTRL_PORT succeeded, message from mtc: @Osmocom_CTRL_Types.CtrlMessage : {
    cmd := {
        verb := "GET",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
} id 2
08:47:46.123085 11675 IPA_Emulation.ttcnpp:921 Message with id 2 was extracted from the queue of IPA_CTRL_PORT.
08:47:46.123102 11675 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Encoding @Osmocom_CTRL_Types.CtrlMessage: {
    cmd := {
        verb := "GET",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := omit
    }
}
08:47:46.123123 11675 IPA_Emulation.ttcnpp:922 enc_CtrlMessage(): Stream after encoding: "GET 848470909 bts.0.oml-connection-state"
08:47:46.123135 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E0127175506198FB38000000000000000000000000000E504002B'O
08:47:46.123155 11675 IPA_Emulation.ttcnpp:924 Sent on IPA_PORT to system @IPA_CodecPort.IPA_Send : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '47455420383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 848470909 bts.0.oml-connection-state")
}
08:47:46.123172 11675 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Encoding @IPA_Types.PDU_IPA: {
    lengthInd := 0,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '47455420383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O ("GET 848470909 bts.0.oml-connection-state")
}
08:47:46.123179 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
}
08:47:46.123202 11675 IPA_CodecPort.ttcn:54 enc_PDU_IPA(): Stream after encoding: '0029EE0047455420383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
08:47:46.123206 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:47:46.123225 11675 IPA_Emulation.ttcnpp:924 Outgoing message was mapped to @IPL4asp_Types.ASP_Send : {
    connId := 1,
    proto := {
        tcp := { }
    },
    msg := '0029EE0047455420383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D7374617465'O
}
08:47:46.123235 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E02271759061A00000000000000000000000000000000E0E50400'O
} id 4
08:47:46.123252 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E02271759061A00000000000000000000000000000000E0E50400'O
08:47:46.123271 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
}
08:47:46.123299 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
} id 4
08:47:46.123302 11675 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 4249,
    locName := "127.0.0.1",
    locPort := 40295,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0039EE004745545F5245504C5920383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
} id 2
08:47:46.123318 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '0006000C1101801E0A'O
} id 5
08:47:46.123321 11675 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0039EE004745545F5245504C5920383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O
08:47:46.123335 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '0006000C1101801E0A'O
08:47:46.123372 11675 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 57,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    payloadData := '4745545F5245504C5920383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 848470909 bts.0.oml-connection-state connected")
}
08:47:46.123372 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 6,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E0A'O
}
08:47:46.123397 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:47:46.123405 11675 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 848470909 bts.0.oml-connection-state connected")
} id 2
08:47:46.123423 11675 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.123463 11675 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_OSMO (238),
    streamIdExt := IPAC_PROTO_EXT_CTRL (0),
    msg := '4745545F5245504C5920383438343730393039206274732E302E6F6D6C2D636F6E6E656374696F6E2D737461746520636F6E6E6563746564'O ("GET_REPLY 848470909 bts.0.oml-connection-state connected")
} id 2
08:47:46.123482 11675 IPA_Emulation.ttcnpp:790 Message with id 2 was extracted from the queue of IPA_PORT.
08:47:46.123495 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.123499 11675 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Stream before decoding: "GET_REPLY 848470909 bts.0.oml-connection-state connected"
08:47:46.123520 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.123522 11675 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 848470909 bts.0.oml-connection-state connected
08:47:46.123540 11675 IPA_Emulation.ttcnpp:653 match_begin token: null_match
08:47:46.123540 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
} id 3
08:47:46.123557 11675 IPA_Emulation.ttcnpp:653 match_begin result: 0
08:47:46.123562 11677 IPA_Emulation.ttcnpp:790 Message with id 3 was extracted from the queue of IPA_PORT.
08:47:46.123583 11675 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 848470909 bts.0.oml-connection-state connected
08:47:46.123598 11675 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET)|(SET)))"
08:47:46.123617 11675 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
08:47:46.123632 11675 IPA_Emulation.ttcnpp:653 match_begin result: 3
08:47:46.123648 11675 IPA_Emulation.ttcnpp:653 match_begin data: _REPLY 848470909 bts.0.oml-connection-state connected
08:47:46.123654 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E0127175506198FB38000000000000000000000000000E504002B'O
08:47:46.123663 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:46.123679 11675 IPA_Emulation.ttcnpp:653 match_begin result: -1
08:47:46.123699 11675 IPA_Emulation.ttcnpp:653 match_begin data: GET_REPLY 848470909 bts.0.oml-connection-state connected
08:47:46.123715 11675 IPA_Emulation.ttcnpp:653 match_begin token: "^(((GET_REPLY)|(SET_REPLY)))"
08:47:46.123732 11675 IPA_Emulation.ttcnpp:653 match_begin regexec result: 0, Success
08:47:46.123747 11675 IPA_Emulation.ttcnpp:653 match_begin result: 9
08:47:46.123762 11675 IPA_Emulation.ttcnpp:653 match_begin data:  848470909 bts.0.oml-connection-state connected
08:47:46.123777 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:46.123793 11675 IPA_Emulation.ttcnpp:653 match_begin result: 1
08:47:46.123811 11675 IPA_Emulation.ttcnpp:653 match_first data: 848470909 bts.0.oml-connection-state connected
08:47:46.123826 11675 IPA_Emulation.ttcnpp:653 match_first token: " "
08:47:46.123841 11675 IPA_Emulation.ttcnpp:653 match_first result: 9
08:47:46.123856 11675 IPA_Emulation.ttcnpp:653 match_list data: 848470909 bts.0.oml-connection-state connected
08:47:46.123872 11675 IPA_Emulation.ttcnpp:653 match_list result: 9
08:47:46.123887 11675 IPA_Emulation.ttcnpp:653 match_begin data:  bts.0.oml-connection-state connected
08:47:46.123902 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:46.123917 11675 IPA_Emulation.ttcnpp:653 match_begin result: 1
08:47:46.123932 11675 IPA_Emulation.ttcnpp:653 match_first data: bts.0.oml-connection-state connected
08:47:46.123947 11675 IPA_Emulation.ttcnpp:653 match_first token: " "
08:47:46.123963 11675 IPA_Emulation.ttcnpp:653 match_first result: 26
08:47:46.123977 11675 IPA_Emulation.ttcnpp:653 match_list data: bts.0.oml-connection-state connected
08:47:46.123993 11675 IPA_Emulation.ttcnpp:653 match_list result: 26
08:47:46.124008 11675 IPA_Emulation.ttcnpp:653 match_begin data:  connected
08:47:46.124023 11675 IPA_Emulation.ttcnpp:653 match_begin token: " "
08:47:46.124038 11675 IPA_Emulation.ttcnpp:653 match_begin result: 1
08:47:46.124053 11675 IPA_Emulation.ttcnpp:653 match_first data: connected
08:47:46.124068 11675 IPA_Emulation.ttcnpp:653 match_first token: " "
08:47:46.124086 11675 IPA_Emulation.ttcnpp:653 match_first result: -1
08:47:46.124101 11675 IPA_Emulation.ttcnpp:653 match_list data: connected
08:47:46.124116 11675 IPA_Emulation.ttcnpp:653 match_list result: -1
08:47:46.124132 11675 IPA_Emulation.ttcnpp:653 dec_CtrlMessage(): Decoded @Osmocom_CTRL_Types.CtrlMessage: {
    resp := {
        verb := "GET_REPLY",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
08:47:46.124154 11675 IPA_Emulation.ttcnpp:653 Sent on IPA_CTRL_PORT to mtc @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
}
08:47:46.124189 9884 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(256) @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:47:46.124216 9884 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:47:46.124238 9884 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(256): @Osmocom_CTRL_Types.CtrlMessage : {
    resp := {
        verb := "GET_REPLY",
        id := "848470909",
        variable := "bts.0.oml-connection-state",
        val := "connected"
    }
} id 3
08:47:46.124257 9884 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
08:47:46.124276 9884 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:47:46.124279 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_1 (1)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '5506198FB38000000000000000000000000000E504002B'O
                }
            }
        }
    }
}
08:47:46.124292 9884 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:47:46.125728 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
}
08:47:46.125982 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.126012 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.126021 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
08:47:46.126036 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
} id 4
08:47:46.126059 11677 IPA_Emulation.ttcnpp:790 Message with id 4 was extracted from the queue of IPA_PORT.
08:47:46.126080 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E02271759061A00000000000000000000000000000000E0E50400'O
08:47:46.126115 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2 (2)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '59061A00000000000000000000000000000000E0E50400'O
                }
            }
        }
    }
}
08:47:46.126213 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000E0E50400'O
                    }
                }
            }
        }
    }
}
08:47:46.126255 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.126266 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000E0E50400'O
                    }
                }
            }
        }
    }
} id 4
08:47:46.126285 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.126316 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0A'O
} id 5
08:47:46.126338 11677 IPA_Emulation.ttcnpp:790 Message with id 5 was extracted from the queue of IPA_PORT.
08:47:46.126360 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E0A'O
08:47:46.126388 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
            }
        }
    }
}
08:47:46.126432 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
}
08:47:46.126503 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2bis (10)
                }
            }
        }
    }
} id 5
08:47:46.126519 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:47:46.126544 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
08:47:46.126587 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
}
08:47:46.126632 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:47:46.126659 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:47:46.126682 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
08:47:46.126709 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
}
08:47:46.126738 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:47:46.126766 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:47:46.126793 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
08:47:46.126819 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
}
08:47:46.126847 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:47:46.126872 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:47:46.126893 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
08:47:46.126921 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
}
08:47:46.126948 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:47:46.126972 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001F000C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:47:46.126993 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001F000C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
08:47:46.127017 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 31,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
}
08:47:46.127044 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:47:46.127068 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:47:46.127089 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001A00101A1E050B001349061D10000000000000000000000000000000'O
08:47:46.127113 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 26,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E050B001349061D10000000000000000000000000000000'O
}
08:47:46.127141 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:47:46.127169 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '000400101A1E0D'O
} id 12
08:47:46.127192 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '000400101A1E0D'O
08:47:46.127215 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 4,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E0D'O
}
08:47:46.127244 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:47:46.127270 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:47:46.127293 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001A00101A1E0E0B00134906069E050020000000000000000000000000'O
08:47:46.127319 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 26,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E0E0B00134906069E050020000000000000000000000000'O
}
08:47:46.127347 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:47:46.127372 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '001400101A1E060B000D2D061E000000F110000197E02B'O
} id 14
08:47:46.127394 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '001400101A1E060B000D2D061E000000F110000197E02B'O
08:47:46.127419 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 20,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '101A1E060B000D2D061E000000F110000197E02B'O
}
08:47:46.127447 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197E02B'O
} id 14
08:47:46.127476 11677 IPA_Emulation.ttcnpp:772 Message enqueued on IPA_PORT from system @IPL4asp_Types.ASP_RecvFrom : {
    connId := 1,
    remName := "127.0.0.1",
    remPort := 3003,
    locName := "127.0.0.1",
    locPort := 10000,
    proto := {
        tcp := { }
    },
    userData := 0,
    msg := '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:47:46.127500 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Stream before decoding: '003F0010600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
08:47:46.127530 11677 IPA_CodecPort.ttcn:43 dec_PDU_IPA(): Decoded @IPA_Types.PDU_IPA: {
    lengthInd := 63,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    payloadData := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
}
08:47:46.127566 11677 IPA_Emulation.ttcnpp:772 Incoming message was mapped to @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:47:46.127595 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.127621 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.127647 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
} id 6
08:47:46.127671 11677 IPA_Emulation.ttcnpp:790 Message with id 6 was extracted from the queue of IPA_PORT.
08:47:46.127695 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E0B27174906038E3200000000000000000000000008002B2B2B2B'O
08:47:46.127734 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                }
            }
        }
    }
}
08:47:46.127802 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:47:46.127839 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.127858 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2ter (11)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '4906038E3200000000000000000000000008002B2B2B2B'O
                    }
                }
            }
        }
    }
} id 6
08:47:46.127863 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.127891 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
} id 7
08:47:46.127916 11677 IPA_Emulation.ttcnpp:790 Message with id 7 was extracted from the queue of IPA_PORT.
08:47:46.127939 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E292717590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
08:47:46.127973 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                }
            }
        }
    }
}
08:47:46.128025 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:47:46.128058 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.128075 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2quater (41)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 7
08:47:46.128082 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.128109 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
} id 8
08:47:46.128132 11677 IPA_Emulation.ttcnpp:790 Message with id 8 was extracted from the queue of IPA_PORT.
08:47:46.128155 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E03271749061B000000F1100001C9031E174740E504000C132B2B'O
08:47:46.128188 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_3 (3)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                }
            }
        }
    }
}
08:47:46.128246 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
}
08:47:46.128279 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.128293 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_3 (3)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '49061B000000F1100001C9031E174740E504000C132B2B'O
                    }
                }
            }
        }
    }
} id 8
08:47:46.128305 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.128335 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
} id 9
08:47:46.128360 11677 IPA_Emulation.ttcnpp:790 Message with id 9 was extracted from the queue of IPA_PORT.
08:47:46.128384 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E04271741061C00F11000014740E5040064304367012B2B2B2B2B'O
08:47:46.128418 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_4 (4)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                }
            }
        }
    }
}
08:47:46.128494 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:47:46.128535 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.128548 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_4 (4)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 9
08:47:46.128565 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.128596 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
} id 10
08:47:46.128629 11677 IPA_Emulation.ttcnpp:790 Message with id 10 was extracted from the queue of IPA_PORT.
08:47:46.128661 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '0C1101801E2827170106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
08:47:46.128703 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_CCHAN (6),
        transparent := false
    },
    msg_type := RSL_MT_BCCH_INFO (17),
    ies := {
        {
            iei := RSL_IE_CHAN_NR (1),
            body := {
                chan_nr := {
                    u := {
                        ch0 := RSL_CHAN_NR_BCCH (16)
                    },
                    tn := 0
                }
            }
        },
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_13 (40)
            }
        },
        {
            iei := RSL_IE_FULL_BCCH_INFO (39),
            body := {
                other := {
                    len := 23,
                    payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                }
            }
        }
    }
}
08:47:46.128773 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
}
08:47:46.128813 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.128828 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_13 (40)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
                    }
                }
            }
        }
    }
} id 10
08:47:46.128846 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.128876 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E050B001349061D10000000000000000000000000000000'O
} id 11
08:47:46.128908 11677 IPA_Emulation.ttcnpp:790 Message with id 11 was extracted from the queue of IPA_PORT.
08:47:46.128940 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E050B001349061D10000000000000000000000000000000'O
08:47:46.129016 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_5 (5)
            }
        },
        {
            iei := RSL_IE_L3_INFO (11),
            body := {
                l3_info := {
                    len := 19,
                    payload := '49061D10000000000000000000000000000000'O
                }
            }
        }
    }
}
08:47:46.129150 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:47:46.129198 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.129216 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5 (5)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '49061D10000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 11
08:47:46.129231 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.129259 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0D'O
} id 12
08:47:46.129291 11677 IPA_Emulation.ttcnpp:790 Message with id 12 was extracted from the queue of IPA_PORT.
08:47:46.129324 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E0D'O
08:47:46.129358 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
            }
        }
    }
}
08:47:46.129407 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
}
08:47:46.129447 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.129458 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5bis (13)
                }
            }
        }
    }
} id 12
08:47:46.129488 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.129523 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E0E0B00134906069E050020000000000000000000000000'O
} id 13
08:47:46.129558 11677 IPA_Emulation.ttcnpp:790 Message with id 13 was extracted from the queue of IPA_PORT.
08:47:46.129593 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E0E0B00134906069E050020000000000000000000000000'O
08:47:46.129635 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
            }
        },
        {
            iei := RSL_IE_L3_INFO (11),
            body := {
                l3_info := {
                    len := 19,
                    payload := '4906069E050020000000000000000000000000'O
                }
            }
        }
    }
}
08:47:46.129696 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:47:46.129741 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.129755 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_5ter (14)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 19,
                        payload := '4906069E050020000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 13
08:47:46.129778 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.129817 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '101A1E060B000D2D061E000000F110000197E02B'O
} id 14
08:47:46.129854 11677 IPA_Emulation.ttcnpp:790 Message with id 14 was extracted from the queue of IPA_PORT.
08:47:46.129897 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '101A1E060B000D2D061E000000F110000197E02B'O
08:47:46.129941 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_SACCH_FILL (26),
    ies := {
        {
            iei := RSL_IE_SYSINFO_TYPE (30),
            body := {
                sysinfo_type := RSL_SYSTEM_INFO_6 (6)
            }
        },
        {
            iei := RSL_IE_L3_INFO (11),
            body := {
                l3_info := {
                    len := 13,
                    payload := '2D061E000000F110000197E02B'O
                }
            }
        }
    }
}
08:47:46.130003 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197E02B'O
                    }
                }
            }
        }
    }
}
08:47:46.130057 11677 IPA_Emulation.ttcnpp:774 Matching on port IPA_PORT IPAC_PROTO_RSL_TRX0 (0) with IPAC_PROTO_CCM (254) unmatched: First message in the queue does not match the template: 
08:47:46.130069 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_SACCH_FILL (26),
        ies := {
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_6 (6)
                }
            },
            {
                iei := RSL_IE_L3_INFO (11),
                body := {
                    l3_info := {
                        len := 13,
                        payload := '2D061E000000F110000197E02B'O
                    }
                }
            }
        }
    }
} id 14
08:47:46.130095 11677 IPA_Emulation.ttcnpp:790 Matching on port IPA_PORT succeeded:  matched
08:47:46.130137 11677 IPA_Emulation.ttcnpp:790 Receive operation on port IPA_PORT succeeded, message from system(): @IPA_CodecPort.IPA_RecvFrom : {
    connId := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    streamIdExt := omit,
    msg := '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
} id 15
08:47:46.130174 11677 IPA_Emulation.ttcnpp:790 Message with id 15 was extracted from the queue of IPA_PORT.
08:47:46.130216 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Stream before decoding: '10600D0004001F37062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
08:47:46.130384 11677 IPA_Emulation.ttcnpp:806 dec_RSL_Message(): Decoded @RSL_Types.RSL_Message: {
    msg_disc := {
        msg_group := RSL_MDISC_TRX_MGMT (8),
        transparent := false
    },
    msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
    ies := {
        {
            iei := RSL_IE_MS_POWER (13),
            body := {
                ms_power := {
                    reserved := 0,
                    fpc_epc := false,
                    power_level := 0
                }
            }
        },
        {
            iei := RSL_IE_BS_POWER (4),
            body := {
                bs_power := {
                    reserved := 0,
                    epc := false,
                    fpc := false,
                    power_level := 0
                }
            }
        },
        {
            iei := RSL_IE_MS_POWER_PARAM (31),
            body := {
                ms_power_params := {
                    len := 55,
                    params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                }
            }
        }
    }
}
08:47:46.130729 11677 IPA_Emulation.ttcnpp:811 Sent on IPA_RSL_PORT to mtc @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
}
08:47:46.130825 9884 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(258) @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_TRX_MGMT (8),
            transparent := false
        },
        msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96),
        ies := {
            {
                iei := RSL_IE_MS_POWER (13),
                body := {
                    ms_power := {
                        reserved := 0,
                        fpc_epc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_BS_POWER (4),
                body := {
                    bs_power := {
                        reserved := 0,
                        epc := false,
                        fpc := false,
                        power_level := 0
                    }
                }
            },
            {
                iei := RSL_IE_MS_POWER_PARAM (31),
                body := {
                    ms_power_params := {
                        len := 55,
                        params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O
                    }
                }
            }
        }
    }
} id 15
08:47:47.124901 9884 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:47:47.125181 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:47.125405 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.125815 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 38
08:47:47.126052 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.126184 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.126356 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.126500 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 38
08:47:47.126653 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 38 was extracted from the queue of BSCVTY.
08:47:47.126803 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.126948 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:47:47.127041 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.127307 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 39
08:47:47.127413 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.127510 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.127629 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.127696 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 39
08:47:47.127760 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 39 was extracted from the queue of BSCVTY.
08:47:47.127824 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.127887 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:47:47.128113 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.128423 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 40
08:47:47.128601 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.128720 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.128857 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.128924 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 40
08:47:47.128990 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 40 was extracted from the queue of BSCVTY.
08:47:47.129057 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.129123 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:47:47.129214 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.129534 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 41
08:47:47.129632 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.129724 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.129838 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.129906 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 41
08:47:47.129997 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 41 was extracted from the queue of BSCVTY.
08:47:47.130065 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.130123 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:47:47.130219 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.130482 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 42
08:47:47.130592 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.130690 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:47.130752 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 42
08:47:47.130812 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 42 was extracted from the queue of BSCVTY.
08:47:47.130872 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.130931 9884 Osmocom_VTY_Functions.ttcn:338 "TC_si2_ncc_permitted() start"
08:47:47.131024 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_si2_ncc_permitted() start"
08:47:47.131100 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.131502 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 43
08:47:47.131617 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.131714 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:47.131775 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 43
08:47:47.131833 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 43 was extracted from the queue of BSCVTY.
08:47:47.131894 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.131952 9884 BSC_Tests.ttcn:3143 Start timer T: 5 s
08:47:47.132222 9884 BSC_Tests.ttcn:3147 Matching on port IPA_RSL[0][0] .rsl.ies{
    {
        iei := RSL_IE_CHAN_NR (1),
        body := {
            chan_nr := {
                u := {
                    ch0 := RSL_CHAN_NR_BCCH (16)
                },
                tn := 0
            }
        }
    },
    {
        iei := RSL_IE_SYSINFO_TYPE (30),
        body := {
            sysinfo_type := RSL_SYSTEM_INFO_1 (1)
        }
    },
    {
        iei := RSL_IE_FULL_BCCH_INFO (39),
        body := {
            other := {
                len := 23,
                payload := '5506198FB38000000000000000000000000000E504002B'O
            }
        }
    }
} with {
    {
        iei := ?,
        body := {
            chan_nr := {
                u := {
                    ch0 := RSL_CHAN_NR_BCCH (16)
                },
                tn := 0
            }
        }
    },
    {
        iei := ?,
        body := {
            sysinfo_type := RSL_SYSTEM_INFO_2 (2)
        }
    },
    {
        iei := ?,
        body := {
            other := {
                len := ?,
                payload := ?
            }
        }
    },
    *
} unmatched: First message in the queue does not match the template: 
08:47:47.132301 9884 BSC_Tests.ttcn:3162 Matching on port IPA_RSL[0][0] succeeded.
08:47:47.132378 9884 BSC_Tests.ttcn:3162 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_RSL_Unitdata: {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_1 (1)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '5506198FB38000000000000000000000000000E504002B'O
                    }
                }
            }
        }
    }
} id 3
08:47:47.132448 9884 BSC_Tests.ttcn:3162 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
08:47:47.132541 9884 BSC_Tests.ttcn:3147 Matching on port IPA_RSL[0][0] succeeded:  matched
08:47:47.132614 9884 BSC_Tests.ttcn:3147 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(258): @IPA_Emulation.ASP_RSL_Unitdata : {
    conn_id := 1,
    streamId := IPAC_PROTO_RSL_TRX0 (0),
    rsl := {
        msg_disc := {
            msg_group := RSL_MDISC_CCHAN (6),
            transparent := false
        },
        msg_type := RSL_MT_BCCH_INFO (17),
        ies := {
            {
                iei := RSL_IE_CHAN_NR (1),
                body := {
                    chan_nr := {
                        u := {
                            ch0 := RSL_CHAN_NR_BCCH (16)
                        },
                        tn := 0
                    }
                }
            },
            {
                iei := RSL_IE_SYSINFO_TYPE (30),
                body := {
                    sysinfo_type := RSL_SYSTEM_INFO_2 (2)
                }
            },
            {
                iei := RSL_IE_FULL_BCCH_INFO (39),
                body := {
                    other := {
                        len := 23,
                        payload := '59061A00000000000000000000000000000000E0E50400'O
                    }
                }
            }
        }
    }
} id 4
08:47:47.132764 9884 BSC_Tests.ttcn:3147 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
08:47:47.132908 9884 BSC_Tests.ttcn:3149 dec_SystemInformation(): Stream before decoding: '59061A00000000000000000000000000000000E0E50400'O
08:47:47.133019 9884 BSC_Tests.ttcn:3149 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: {
    header := {
        l2_plen := {
            l2_plen := 22,
            zero_one := '01'B
        },
        skip_indicator := 0,
        rr_protocol_discriminator := 6,
        message_type := SYSTEM_INFORMATION_TYPE_2 (26)
    },
    payload := {
        si2 := {
            bcch_freq_list := '00000000000000000000000000000000'O,
            ncc_permitted := '11100000'B,
            rach_control := {
                max_retrans := RACH_MAX_RETRANS_7 (3),
                tx_integer := '1001'B,
                cell_barr_access := false,
                re_not_allowed := true,
                acc := '0000010000000000'B
            }
        }
    }
}
08:47:47.133148 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:47:47.133325 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.133637 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 44
08:47:47.133750 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.133845 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.133963 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.134027 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 44
08:47:47.134085 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 44 was extracted from the queue of BSCVTY.
08:47:47.134147 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.134206 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:47:47.134281 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.134571 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 45
08:47:47.134712 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.134810 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.134925 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.134985 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 45
08:47:47.135042 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 45 was extracted from the queue of BSCVTY.
08:47:47.135103 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.135164 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:47:47.135251 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.135392 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 46
08:47:47.135483 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.135568 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.135674 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.135730 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 46
08:47:47.135806 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 46 was extracted from the queue of BSCVTY.
08:47:47.135863 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.135918 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "ncc-permitted all"
08:47:47.135989 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.136127 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 47
08:47:47.136212 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.136293 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.136394 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:47:47.136451 9884 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 47
08:47:47.136503 9884 Osmocom_VTY_Functions.ttcn:74 Message with id 47 was extracted from the queue of BSCVTY.
08:47:47.136557 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.136607 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:47:47.136672 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.136761 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 48
08:47:47.136843 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.136927 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:47.136980 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 48
08:47:47.137032 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 48 was extracted from the queue of BSCVTY.
08:47:47.137175 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.137298 9884 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
08:47:47.137453 9884 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:47:47.138554 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1454615 bytes in 1329 blocks)" id 49
08:47:47.138693 9884 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 50
08:47:47.138887 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454615 bytes in 1329 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.138990 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454615 bytes in 1329 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:47:47.139086 9884 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454615 bytes in 1329 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:47:47.139162 9884 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454615 bytes in 1329 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:47:47.139226 9884 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1454615 bytes in 1329 blocks)" with ? matched
08:47:47.139287 9884 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1454615 bytes in 1329 blocks)" id 49
08:47:47.139359 9884 Osmocom_VTY_Functions.ttcn:85 Message with id 49 was extracted from the queue of BSCVTY.
08:47:47.139445 9884 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:47:47.139536 9884 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:47:47.139596 9884 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 50
08:47:47.139656 9884 Osmocom_VTY_Functions.ttcn:73 Message with id 50 was extracted from the queue of BSCVTY.
08:47:47.139715 9884 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:47:47.139775 9884 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
08:47:47.139864 9884 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
08:47:47.139940 9884 BSC_Tests.ttcn:888 Stopping all components.
08:47:47.140080 11672 M3UA_Emulation.ttcn:596 Stopping test component execution.
08:47:47.140090 11671 SCCP_Emulation.ttcn:5439 Stopping test component execution.
08:47:47.140117 11673 SCCP_Emulation.ttcn:5439 Stop was requested from MC.
08:47:47.140119 11674 M3UA_Emulation.ttcn:596 Stop was requested from MC.
08:47:47.140158 11676 MGCP_Emulation.ttcn:301 Stop was requested from MC.
08:47:47.140160 11675 IPA_Emulation.ttcnpp:772 Kill was requested from MC.
08:47:47.140235 11670 StatsD_Checker.ttcnpp:143 Kill was requested from MC.
08:47:47.140283 11677 IPA_Emulation.ttcnpp:772 Stop was requested from MC.
08:47:47.140316 11674 M3UA_Emulation.ttcn:596 Stopping test component execution.
08:47:47.140403 11673 SCCP_Emulation.ttcn:5439 Stopping test component execution.
08:47:47.140403 11676 MGCP_Emulation.ttcn:301 Stopping test component execution.
08:47:47.140498 11675 IPA_Emulation.ttcnpp:772 Terminating test component execution.
08:47:47.140503 11677 IPA_Emulation.ttcnpp:772 Stopping test component execution.
08:47:47.140544 11670 StatsD_Checker.ttcnpp:143 Terminating test component execution.
08:47:47.141134 11672 - Function f_M3UA_Emulation was stopped. PTC remains alive and is waiting for next start.
08:47:47.141294 11674 - Function f_M3UA_Emulation was stopped. PTC remains alive and is waiting for next start.
08:47:47.141342 11671 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
08:47:47.141663 11670 - Function main was stopped. PTC terminates.
08:47:47.141704 11677 - Function main_client was stopped. PTC remains alive and is waiting for next start.
08:47:47.141879 11670 - Terminating component type StatsD_Checker.StatsD_Checker_CT.
08:47:47.141964 11670 - Removing unterminated mapping between port STATSVTY and system:STATSVTY.
08:47:47.142174 11670 - Port STATSVTY was unmapped from system:STATSVTY.
08:47:47.142363 11675 - Function main_client was stopped. PTC terminates.
08:47:47.142401 11670 - Port STATSVTY was stopped.
08:47:47.142496 11676 - Function main was stopped. PTC remains alive and is waiting for next start.
08:47:47.142550 11670 - Port STATSD_PROC was stopped.
08:47:47.142591 11673 - Function SCCPStart was stopped. PTC remains alive and is waiting for next start.
08:47:47.142599 11670 - Removing unterminated mapping between port STATS and system:STATS.
08:47:47.142695 11675 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:47:47.142816 11675 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:47:47.143491 11670 - Port STATS was unmapped from system:STATS.
08:47:47.143587 11670 - Port STATS was stopped.
08:47:47.143634 11670 - Component type StatsD_Checker.StatsD_Checker_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.143699 11670 - Final verdict of PTC: none
08:47:47.143866 11670 - Disconnected from MC.
08:47:47.143916 11670 - TTCN-3 Parallel Test Component finished.
08:47:47.144089 11675 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:47:47.144252 11675 - Port IPA_PORT was stopped.
08:47:47.144333 11675 - Port CFG_PORT was stopped.
08:47:47.144404 11675 - Port MTP3_SP_PORT was stopped.
08:47:47.144474 11675 - Port IPA_MGCP_PORT was stopped.
08:47:47.144544 11675 - Port IPA_RSL_PORT was stopped.
08:47:47.144612 11675 - Port IPA_OML_PORT was stopped.
08:47:47.144680 11675 - Removing unterminated connection between port IPA_CTRL_PORT and mtc:IPA_CTRL.
08:47:47.144798 11675 - Port IPA_CTRL_PORT was stopped.
08:47:47.144823 9884 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT was closed unexpectedly by the peer.
08:47:47.144875 11675 - Port IPA_SP_PORT was stopped.
08:47:47.144902 9884 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(256):IPA_CTRL_PORT.
08:47:47.144946 11675 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.145037 11675 - Final verdict of PTC: none
08:47:47.145081 9884 BSC_Tests.ttcn:888 All components were stopped.
08:47:47.145144 9884 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
08:47:47.145208 9884 BSC_Tests.ttcn:890 Stopping test component execution.
08:47:47.145243 11675 - Disconnected from MC.
08:47:47.145296 9884 BSC_Tests.ttcn:3174 Test case TC_si2_ncc_permitted was stopped.
08:47:47.145323 11675 - TTCN-3 Parallel Test Component finished.
08:47:47.145347 9884 BSC_Tests.ttcn:3174 Terminating component type BSC_Tests.test_CT.
08:47:47.145402 9884 BSC_Tests.ttcn:3174 Default with id 1 (altstep as_Tguard) was deactivated.
08:47:47.145456 9884 BSC_Tests.ttcn:3174 Stop timer T_guard: 30 s
08:47:47.145512 9884 BSC_Tests.ttcn:3174 Port IPA_CTRL was stopped.
08:47:47.145564 9884 BSC_Tests.ttcn:3174 Port RSL_CCHAN[0] was stopped.
08:47:47.145619 9884 BSC_Tests.ttcn:3174 Port RSL_CCHAN[1] was stopped.
08:47:47.145666 9884 BSC_Tests.ttcn:3174 Port RSL_CCHAN[2] was stopped.
08:47:47.145713 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(258):IPA_RSL_PORT.
08:47:47.145792 9884 BSC_Tests.ttcn:3174 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
08:47:47.145814 11677 - Connection of port IPA_RSL_PORT to mtc:IPA_RSL[0][0] was closed unexpectedly by the peer.
08:47:47.145878 9884 BSC_Tests.ttcn:3174 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
08:47:47.145906 11677 - Port IPA_RSL_PORT was disconnected from mtc:IPA_RSL[0][0].
08:47:47.145929 9884 BSC_Tests.ttcn:3174 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
08:47:47.145980 9884 BSC_Tests.ttcn:3174 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146028 9884 BSC_Tests.ttcn:3174 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146075 9884 BSC_Tests.ttcn:3174 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146126 9884 BSC_Tests.ttcn:3174 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146173 9884 BSC_Tests.ttcn:3174 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146221 9884 BSC_Tests.ttcn:3174 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146269 9884 BSC_Tests.ttcn:3174 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146345 9884 BSC_Tests.ttcn:3174 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
08:47:47.146402 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][0] was stopped.
08:47:47.146485 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][1] was stopped.
08:47:47.146533 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][2] was stopped.
08:47:47.146580 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[0][3] was stopped.
08:47:47.146626 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][0] was stopped.
08:47:47.146673 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][1] was stopped.
08:47:47.146728 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][2] was stopped.
08:47:47.146829 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[1][3] was stopped.
08:47:47.146916 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][0] was stopped.
08:47:47.147196 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][1] was stopped.
08:47:47.147301 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][2] was stopped.
08:47:47.147365 9884 BSC_Tests.ttcn:3174 Port IPA_RSL[2][3] was stopped.
08:47:47.147448 9884 BSC_Tests.ttcn:3174 Port IPA was stopped.
08:47:47.147503 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CTRL was stopped.
08:47:47.147570 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(258):CFG_PORT.
08:47:47.147652 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][0] was stopped.
08:47:47.147706 11677 - Connection of port CFG_PORT to mtc:IPA_CFG_PORT[0][0] was closed unexpectedly by the peer.
08:47:47.147836 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][1] was stopped.
08:47:47.147893 11677 - Port CFG_PORT was disconnected from mtc:IPA_CFG_PORT[0][0].
08:47:47.147894 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][2] was stopped.
08:47:47.147950 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[0][3] was stopped.
08:47:47.148007 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][0] was stopped.
08:47:47.148061 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][1] was stopped.
08:47:47.148115 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][2] was stopped.
08:47:47.148168 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[1][3] was stopped.
08:47:47.148221 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][0] was stopped.
08:47:47.148274 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][1] was stopped.
08:47:47.148327 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][2] was stopped.
08:47:47.148380 9884 BSC_Tests.ttcn:3174 Port IPA_CFG_PORT[2][3] was stopped.
08:47:47.148433 9884 BSC_Tests.ttcn:3174 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
08:47:47.148545 9884 BSC_Tests.ttcn:3174 Port BSCVTY was unmapped from system:BSCVTY.
08:47:47.148613 9884 BSC_Tests.ttcn:3174 Port BSCVTY was stopped.
08:47:47.148669 9884 BSC_Tests.ttcn:3174 Port STPVTY was stopped.
08:47:47.148725 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
08:47:47.148779 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
08:47:47.148833 9884 BSC_Tests.ttcn:3174 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
08:47:47.148888 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(252):SCCP_SP_PORT.
08:47:47.148969 9884 BSC_Tests.ttcn:3174 Port BSSAP was stopped.
08:47:47.149098 9884 BSC_Tests.ttcn:3174 Removing unterminated connection between port BSSAP_LE and VirtSMLC-SCCP(254):SCCP_SP_PORT.
08:47:47.149175 9884 BSC_Tests.ttcn:3174 Port BSSAP_LE was stopped.
08:47:47.149220 11673 - Connection of port SCCP_SP_PORT to mtc:BSSAP_LE was closed unexpectedly by the peer.
08:47:47.149294 9884 BSC_Tests.ttcn:3174 Component type BSC_Tests.test_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.149323 11673 - Port SCCP_SP_PORT was disconnected from mtc:BSSAP_LE.
08:47:47.149357 9884 BSC_Tests.ttcn:3174 Waiting for PTCs to finish.
08:47:47.149472 11671 - Kill was requested from MC. Terminating idle PTC.
08:47:47.149480 11672 - Kill was requested from MC. Terminating idle PTC.
08:47:47.149481 11673 - Kill was requested from MC. Terminating idle PTC.
08:47:47.149534 11674 - Kill was requested from MC. Terminating idle PTC.
08:47:47.149546 11676 - Kill was requested from MC. Terminating idle PTC.
08:47:47.149578 11677 - Kill was requested from MC. Terminating idle PTC.
08:47:47.149624 11672 - Terminating component type M3UA_Emulation.M3UA_CT.
08:47:47.149658 11671 - Terminating component type SCCP_Emulation.SCCP_CT.
08:47:47.149690 11674 - Terminating component type M3UA_Emulation.M3UA_CT.
08:47:47.149708 11676 - Terminating component type MGCP_Emulation.MGCP_Emulation_CT.
08:47:47.149747 11671 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.149755 11673 - Terminating component type SCCP_Emulation.SCCP_CT.
08:47:47.149795 11677 - Terminating component type IPA_Emulation.IPA_Emulation_CT.
08:47:47.149950 11676 - Removing unterminated mapping between port MGCP and system:MGCP_CODEC_PT.
08:47:47.149970 11671 - Final verdict of PTC: none
08:47:47.149974 11674 - Stop timer T_ASPUP_resend: 2 s
08:47:47.149995 11672 - Component type M3UA_Emulation.M3UA_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.150026 11673 - Port SCCP_SP_PORT was stopped.
08:47:47.150067 11672 - Final verdict of PTC: none
08:47:47.150080 11674 - Stop timer T_ASPAC_resend: 2 s
08:47:47.150103 11677 - Removing unterminated mapping between port IPA_PORT and system:IPA_CODEC_PT.
08:47:47.150203 11673 - Removing unterminated connection between port MTP3_SCCP_PORT and VirtSMLC-M3UA(255):MTP3_SP_PORT.
08:47:47.150206 11674 - Stop timer T_Assoc_restart: 60 s
08:47:47.150360 11674 - Removing unterminated connection between port MTP3_SP_PORT and VirtSMLC-SCCP(254):MTP3_SCCP_PORT.
08:47:47.150460 11673 - Port MTP3_SCCP_PORT was stopped.
08:47:47.150849 11674 - Port MTP3_SP_PORT was stopped.
08:47:47.150969 11673 - Component type SCCP_Emulation.SCCP_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.151113 11677 - Port IPA_PORT was unmapped from system:IPA_CODEC_PT.
08:47:47.151217 11677 - Port IPA_PORT was stopped.
08:47:47.151284 11677 - Port CFG_PORT was stopped.
08:47:47.151311 11673 - Final verdict of PTC: none
08:47:47.151322 11674 - Removing unterminated mapping between port SCTP_PORT and system:sctp.
08:47:47.151560 11677 - Port MTP3_SP_PORT was stopped.
08:47:47.151648 11673 - Disconnected from MC.
08:47:47.151711 11677 - Port IPA_MGCP_PORT was stopped.
08:47:47.151843 11676 - Port MGCP was unmapped from system:MGCP_CODEC_PT.
08:47:47.151940 11674 - Port SCTP_PORT was unmapped from system:sctp.
08:47:47.152313 11677 - Port IPA_RSL_PORT was stopped.
08:47:47.152328 11676 - Port MGCP was stopped.
08:47:47.152429 11676 - Port MGCP_CLIENT was stopped.
08:47:47.152442 11674 - Port SCTP_PORT was stopped.
08:47:47.152445 11677 - Port IPA_OML_PORT was stopped.
08:47:47.152498 11676 - Port MGCP_CLIENT_MULTI was stopped.
08:47:47.152562 11673 - TTCN-3 Parallel Test Component finished.
08:47:47.152569 11677 - Port IPA_CTRL_PORT was stopped.
08:47:47.152614 11676 - Port MGCP_PROC was stopped.
08:47:47.152641 11677 - Port IPA_SP_PORT was stopped.
08:47:47.152674 11676 - Component type MGCP_Emulation.MGCP_Emulation_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.152702 11674 - Component type M3UA_Emulation.M3UA_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.152703 11677 - Component type IPA_Emulation.IPA_Emulation_CT was shut down inside testcase TC_si2_ncc_permitted.
08:47:47.152745 11676 - Final verdict of PTC: none
08:47:47.152800 11677 - Final verdict of PTC: none
08:47:47.152820 11674 - Final verdict of PTC: none
08:47:47.152929 11676 - Disconnected from MC.
08:47:47.152980 11676 - TTCN-3 Parallel Test Component finished.
08:47:47.153023 11677 - Disconnected from MC.
08:47:47.153117 9884 BSC_Tests.ttcn:3174 Setting final verdict of the test case.
08:47:47.153118 11677 - TTCN-3 Parallel Test Component finished.
08:47:47.153142 11674 - Disconnected from MC.
08:47:47.153646 11674 - TTCN-3 Parallel Test Component finished.
08:47:47.153761 9884 BSC_Tests.ttcn:3174 Local verdict of MTC: pass
08:47:47.154420 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMSC-STATS(251): none (pass -> pass)
08:47:47.154922 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMSC-SCCP(252): none (pass -> pass)
08:47:47.155272 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMSC-M3UA(253): none (pass -> pass)
08:47:47.155517 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtSMLC-SCCP(254): none (pass -> pass)
08:47:47.155655 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtSMLC-M3UA(255): none (pass -> pass)
08:47:47.155987 9884 BSC_Tests.ttcn:3174 Local verdict of PTC IPA-CTRL-CLI-IPA(256): none (pass -> pass)
08:47:47.156187 9884 BSC_Tests.ttcn:3174 Local verdict of PTC VirtMGW-MGCP-0(257): none (pass -> pass)
08:47:47.156321 9884 BSC_Tests.ttcn:3174 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(258): none (pass -> pass)
08:47:47.156469 9884 BSC_Tests.ttcn:3174 Test case TC_si2_ncc_permitted finished. Verdict: pass
08:47:47.156612 9884 BSC_Tests.ttcn:3174 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_si2_ncc_permitted pass'.
08:47:52.431400 9884 BSC_Tests.ttcn:3174 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_si2_ncc_permitted pass' was executed successfully (exit status: 0).
08:47:52.431490 9884 BSC_Tests.ttcn:1399 Switching to log file `BSC_Tests-TC_chan_act_noreply-8fbedb33933a-mtc-9884.log'
