08:43:42.643571 BSC_Tests.ttcn:2895 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_si2quater_3_earfcns'.
08:43:43.659426 BSC_Tests.ttcn:2895 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_si2quater_3_earfcns' was executed successfully (exit status: 0).
08:43:43.659705 BSC_Tests.ttcn:2895 Test case TC_si2quater_3_earfcns started.
08:43:43.659821 BSC_Tests.ttcn:2895 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_si2quater_3_earfcns.
08:43:43.660141 BSC_Tests.ttcn:2895 Port IPA_CTRL was started.
08:43:43.660371 BSC_Tests.ttcn:2895 Port RSL_CCHAN[0] was started.
08:43:43.660436 BSC_Tests.ttcn:2895 Port RSL_CCHAN[1] was started.
08:43:43.660593 BSC_Tests.ttcn:2895 Port RSL_CCHAN[2] was started.
08:43:43.660750 BSC_Tests.ttcn:2895 Port IPA_RSL[0][0] was started.
08:43:43.660810 BSC_Tests.ttcn:2895 Port IPA_RSL[0][1] was started.
08:43:43.660943 BSC_Tests.ttcn:2895 Port IPA_RSL[0][2] was started.
08:43:43.661092 BSC_Tests.ttcn:2895 Port IPA_RSL[0][3] was started.
08:43:43.661150 BSC_Tests.ttcn:2895 Port IPA_RSL[1][0] was started.
08:43:43.661203 BSC_Tests.ttcn:2895 Port IPA_RSL[1][1] was started.
08:43:43.661253 BSC_Tests.ttcn:2895 Port IPA_RSL[1][2] was started.
08:43:43.661302 BSC_Tests.ttcn:2895 Port IPA_RSL[1][3] was started.
08:43:43.661352 BSC_Tests.ttcn:2895 Port IPA_RSL[2][0] was started.
08:43:43.661401 BSC_Tests.ttcn:2895 Port IPA_RSL[2][1] was started.
08:43:43.661450 BSC_Tests.ttcn:2895 Port IPA_RSL[2][2] was started.
08:43:43.661499 BSC_Tests.ttcn:2895 Port IPA_RSL[2][3] was started.
08:43:43.661550 BSC_Tests.ttcn:2895 Port IPA was started.
08:43:43.661599 BSC_Tests.ttcn:2895 Port SCCPLITE_IPA_CTRL was started.
08:43:43.661651 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[0][0] was started.
08:43:43.661702 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[0][1] was started.
08:43:43.661752 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[0][2] was started.
08:43:43.661805 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[0][3] was started.
08:43:43.661854 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[1][0] was started.
08:43:43.661903 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[1][1] was started.
08:43:43.661952 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[1][2] was started.
08:43:43.662002 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[1][3] was started.
08:43:43.662050 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[2][0] was started.
08:43:43.662101 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[2][1] was started.
08:43:43.662153 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[2][2] was started.
08:43:43.662202 BSC_Tests.ttcn:2895 Port IPA_CFG_PORT[2][3] was started.
08:43:43.662253 BSC_Tests.ttcn:2895 Port BSCVTY was started.
08:43:43.662407 BSC_Tests.ttcn:2895 Port STPVTY was started.
08:43:43.662469 BSC_Tests.ttcn:2895 Port SCCPLITE_IPA_CFG_PORT[0] was started.
08:43:43.662520 BSC_Tests.ttcn:2895 Port SCCPLITE_IPA_CFG_PORT[1] was started.
08:43:43.662571 BSC_Tests.ttcn:2895 Port SCCPLITE_IPA_CFG_PORT[2] was started.
08:43:43.662621 BSC_Tests.ttcn:2895 Port BSSAP was started.
08:43:43.662671 BSC_Tests.ttcn:2895 Port BSSAP_LE was started.
08:43:43.662722 BSC_Tests.ttcn:2895 Component type BSC_Tests.test_CT was initialized.
08:43:43.663352 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
08:43:43.663443 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
08:43:43.663511 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
08:43:43.664238 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
08:43:43.664320 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
08:43:43.664502 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
08:43:43.664585 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 1, prompt := "OsmoBSC> ", has_wildcards := false } }
08:43:43.664652 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 2, prompt := "OsmoBSC# ", has_wildcards := false } }
08:43:43.664745 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 3, prompt := "OsmoBSC(*)", has_wildcards := true } }
08:43:43.664886 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
08:43:43.664984 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.665053 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:43:43.665110 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:43:43.665165 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:43:43.665217 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:43:43.665272 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
08:43:43.665332 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
08:43:43.665393 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
08:43:43.665454 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
08:43:43.665624 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
08:43:43.665776 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.665887 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.665947 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
08:43:43.666008 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
08:43:43.666069 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.666138 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:43.666221 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.666620 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
08:43:43.666738 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.666839 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.666967 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.667036 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
08:43:43.667097 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
08:43:43.667160 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.667224 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
08:43:43.667300 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.667574 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
08:43:43.667670 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.667760 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.667873 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.667938 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
08:43:43.668011 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
08:43:43.668073 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.668134 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
08:43:43.668206 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.668465 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
08:43:43.668558 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.668648 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.668754 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.668817 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
08:43:43.668875 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
08:43:43.668935 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.668994 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
08:43:43.669062 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.669308 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
08:43:43.669398 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.669486 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.669591 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.669655 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
08:43:43.669711 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
08:43:43.669770 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.669827 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:43:43.669896 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.670109 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
08:43:43.670197 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.670288 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.670367 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
08:43:43.670425 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
08:43:43.670486 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.670548 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:43.670620 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.670889 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
08:43:43.670979 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.671067 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.671171 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.671246 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
08:43:43.671304 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
08:43:43.671365 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.671424 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:43:43.671494 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.671744 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
08:43:43.671834 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.671920 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.672022 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.672082 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
08:43:43.672140 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
08:43:43.672199 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.672258 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:43:43.672325 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.672580 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
08:43:43.672668 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.672752 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.672852 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.672914 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
08:43:43.672971 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
08:43:43.673031 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.673087 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.673153 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.673387 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
08:43:43.673475 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.673560 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.673663 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.673724 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
08:43:43.673781 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
08:43:43.673840 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.673895 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.673962 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.674186 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
08:43:43.674274 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.674743 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.674992 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
08:43:43.675111 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
08:43:43.675216 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.675325 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:43:43.686969 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 147, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
08:43:43.687123 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(147).
08:43:43.687417 StatsD_Checker.ttcnpp:417 Function was started.
08:43:43.687572 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
08:43:43.687708 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.688039 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
08:43:43.688253 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.688413 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.688526 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
08:43:43.688620 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
08:43:43.688712 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.688817 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
08:43:43.688958 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.689492 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 14
08:43:43.689673 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.689820 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.689908 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 14
08:43:43.689989 Osmocom_VTY_Functions.ttcn:73 Message with id 14 was extracted from the queue of BSCVTY.
08:43:43.690070 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.690160 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
08:43:43.690280 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.690671 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
08:43:43.690824 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.690968 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.691060 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
08:43:43.691142 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
08:43:43.691225 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.691411 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:43:43.693998 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 148, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
08:43:43.694028 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
08:43:43.697313 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 149, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
08:43:43.697348 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(149):SCTP_PORT to system:sctp.
08:43:43.698718 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(149):SCTP_PORT to system:sctp finished.
08:43:43.698753 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(149):MTP3_SP_PORT and VirtMSC-SCCP(148):MTP3_SCCP_PORT.
08:43:43.699054 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(149):MTP3_SP_PORT and VirtMSC-SCCP(148):MTP3_SCCP_PORT finished.
08:43:43.699087 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({ local_sctp_port := 23905, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 1) on component VirtMSC-M3UA(149).
08:43:43.699151 SCCP_Adapter.ttcnpp:127 Function was started.
08:43:43.699185 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(148):SCCP_SP_PORT.
08:43:43.699380 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(148):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-197fb81d.
08:43:43.699471 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(148):SCCP_SP_PORT.
08:43:43.699513 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(148):SCCP_SP_PORT finished.
08:43:43.699547 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 185, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 254 }) on component VirtMSC-SCCP(148).
08:43:43.699625 SCCP_Adapter.ttcnpp:165 Function was started.
08:43:43.699757 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(148) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit }
08:43:43.699805 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
08:43:43.699879 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
08:43:43.699938 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := '000430040100'O, importance := omit }
08:43:43.700000 BSC_Tests.ttcn:899 Start timer T: 5 s
08:43:43.908058 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(148) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := '000131'O, importance := omit } id 1
08:43:43.908231 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
08:43:43.908782 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
08:43:43.908984 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
08:43:43.909213 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
08:43:43.909349 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(148): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
08:43:43.909460 BSC_Tests.ttcn:901 Message with id 1 was extracted from the queue of BSSAP.
08:43:43.909565 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
08:43:43.909751 BSSAP_LE_Adapter.ttcn:95 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
08:43:43.917190 BSSAP_LE_Adapter.ttcn:95 PTC was created. Component reference: 150, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
08:43:43.917239 BSSAP_LE_Adapter.ttcn:101 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
08:43:43.925902 BSSAP_LE_Adapter.ttcn:101 PTC was created. Component reference: 151, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
08:43:43.926026 BSSAP_LE_Adapter.ttcn:102 Mapping port VirtSMLC-M3UA(151):SCTP_PORT to system:sctp.
08:43:43.928668 BSSAP_LE_Adapter.ttcn:102 Map operation of VirtSMLC-M3UA(151):SCTP_PORT to system:sctp finished.
08:43:43.928828 BSSAP_LE_Adapter.ttcn:104 Connecting ports VirtSMLC-M3UA(151):MTP3_SP_PORT and VirtSMLC-SCCP(150):MTP3_SCCP_PORT.
08:43:43.929850 BSSAP_LE_Adapter.ttcn:104 Connect operation on VirtSMLC-M3UA(151):MTP3_SP_PORT and VirtSMLC-SCCP(150):MTP3_SCCP_PORT finished.
08:43:43.930048 BSSAP_LE_Adapter.ttcn:105 Starting function f_M3UA_Emulation({ local_sctp_port := 23908, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 6) on component VirtSMLC-M3UA(151).
08:43:43.930260 BSSAP_LE_Adapter.ttcn:105 Function was started.
08:43:43.930415 BSC_Tests.ttcn:1290 Connecting ports mtc:BSSAP_LE and VirtSMLC-SCCP(150):SCCP_SP_PORT.
08:43:43.931216 BSC_Tests.ttcn:1290 Port BSSAP_LE is waiting for connection from VirtSMLC-SCCP(150):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-5e33e71d.
08:43:43.932216 BSC_Tests.ttcn:1290 Port BSSAP_LE has accepted the connection from VirtSMLC-SCCP(150):SCCP_SP_PORT.
08:43:43.932457 BSC_Tests.ttcn:1290 Connect operation on mtc:BSSAP_LE and VirtSMLC-SCCP(150):SCCP_SP_PORT finished.
08:43:43.932610 BSSAP_LE_Adapter.ttcn:122 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 190, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 252 }) on component VirtSMLC-SCCP(150).
08:43:43.932839 BSSAP_LE_Adapter.ttcn:122 Function was started.
08:43:43.932981 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
08:43:43.933173 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.938896 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
08:43:43.939012 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
08:43:43.941961 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.944005 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.945620 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:43:43.946983 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:43:43.948101 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with ? matched
08:43:43.949054 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
08:43:43.949078 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
08:43:43.949100 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.949121 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.949133 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
08:43:43.949144 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
08:43:43.949156 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.949172 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:43.949192 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.949249 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 18
08:43:43.949270 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.949289 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.949308 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.949319 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 18
08:43:43.949330 Osmocom_VTY_Functions.ttcn:74 Message with id 18 was extracted from the queue of BSCVTY.
08:43:43.949340 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.949350 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
08:43:43.949365 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.949390 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 19
08:43:43.949406 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.949422 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.949440 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.949451 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 19
08:43:43.949461 Osmocom_VTY_Functions.ttcn:74 Message with id 19 was extracted from the queue of BSCVTY.
08:43:43.949471 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.949482 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
08:43:43.949494 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.949515 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 20
08:43:43.949530 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.949545 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.949563 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.949575 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 20
08:43:43.949585 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
08:43:43.949595 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.949605 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.949616 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.949632 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 21
08:43:43.949647 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.949661 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.949678 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.949689 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 21
08:43:43.949698 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
08:43:43.949708 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.949718 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.949730 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.949744 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 22
08:43:43.949759 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.949774 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.949785 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 22
08:43:43.949795 Osmocom_VTY_Functions.ttcn:73 Message with id 22 was extracted from the queue of BSCVTY.
08:43:43.949804 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.949817 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:43.949829 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.949855 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
08:43:43.949871 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.949886 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.949904 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.949915 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
08:43:43.949925 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
08:43:43.949935 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.949945 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1"
08:43:43.949957 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.949974 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 24
08:43:43.949989 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.950004 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.950024 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.950035 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 24
08:43:43.950045 Osmocom_VTY_Functions.ttcn:74 Message with id 24 was extracted from the queue of BSCVTY.
08:43:43.950055 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.950065 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
08:43:43.950077 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.950094 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 25
08:43:43.950109 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.950124 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.950141 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.950152 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 25
08:43:43.950161 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
08:43:43.950172 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.950181 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.950193 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.950209 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 26
08:43:43.950224 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.950239 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.950256 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.950266 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 26
08:43:43.950276 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
08:43:43.950286 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.950295 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.950313 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.950400 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 27
08:43:43.950512 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.950600 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.950694 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 27
08:43:43.950706 Osmocom_VTY_Functions.ttcn:73 Message with id 27 was extracted from the queue of BSCVTY.
08:43:43.950800 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.950820 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:43.950833 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.950854 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 28
08:43:43.950869 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.950887 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.950905 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.950916 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 28
08:43:43.950926 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
08:43:43.950936 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.950946 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2"
08:43:43.950959 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.950976 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 29
08:43:43.950991 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.951006 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.951024 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.951035 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 29
08:43:43.951045 Osmocom_VTY_Functions.ttcn:74 Message with id 29 was extracted from the queue of BSCVTY.
08:43:43.951055 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.951065 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
08:43:43.951077 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.951094 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 30
08:43:43.951109 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.951124 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.951141 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.951152 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 30
08:43:43.951162 Osmocom_VTY_Functions.ttcn:74 Message with id 30 was extracted from the queue of BSCVTY.
08:43:43.951172 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.951182 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.951193 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.951209 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 31
08:43:43.951224 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.951239 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.951256 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.951267 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 31
08:43:43.951277 Osmocom_VTY_Functions.ttcn:74 Message with id 31 was extracted from the queue of BSCVTY.
08:43:43.951286 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.951296 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
08:43:43.951310 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.951324 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
08:43:43.951339 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.951355 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.951365 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
08:43:43.951375 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
08:43:43.951385 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.951396 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:43:43.954284 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 152, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
08:43:43.954313 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(152):IPA_PORT to system:IPA_CODEC_PT.
08:43:43.955345 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(152):IPA_PORT to system:IPA_CODEC_PT finished.
08:43:43.955356 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(152):IPA_CTRL_PORT and mtc:IPA_CTRL.
08:43:43.955471 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(152):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-1a34f21f.
08:43:43.955514 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(152):IPA_CTRL_PORT.
08:43:43.955527 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(152):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
08:43:43.955537 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, { ser_nr := "", name := "mahlzeit", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "0/1/2", osmo_rand := "" }, false) on component IPA-CTRL-CLI-IPA(152).
08:43:43.955565 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
08:43:43.955575 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
08:43:43.956877 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(152) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
08:43:43.956890 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
08:43:43.956901 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(152): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
08:43:43.956911 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
08:43:43.956927 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:43:43.959929 BSC_Tests.ttcn:1073 PTC was created. Component reference: 153, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
08:43:43.959943 BSC_Tests.ttcn:1074 Starting function main({ create_cb := refers(MGCP_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback) }, { callagent_ip := "127.0.0.1", callagent_udp_port := -1, mgw_ip := "127.0.0.1", mgw_udp_port := 2427, multi_conn_mode := false }, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(153).
08:43:43.959989 BSC_Tests.ttcn:1074 Function was started.
08:43:43.960000 Osmocom_VTY_Functions.ttcn:338 "TC_si2quater_3_earfcns() start"
08:43:43.960017 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_si2quater_3_earfcns() start"
08:43:43.960038 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960079 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 33
08:43:43.960116 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.960138 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.960149 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 33
08:43:43.960160 Osmocom_VTY_Functions.ttcn:73 Message with id 33 was extracted from the queue of BSCVTY.
08:43:43.960171 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.960186 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:43.960202 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960228 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 34
08:43:43.960246 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.960262 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.960284 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.960295 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 34
08:43:43.960306 Osmocom_VTY_Functions.ttcn:74 Message with id 34 was extracted from the queue of BSCVTY.
08:43:43.960317 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.960327 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:43:43.960340 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960359 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 35
08:43:43.960376 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.960392 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.960411 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.960422 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 35
08:43:43.960432 Osmocom_VTY_Functions.ttcn:74 Message with id 35 was extracted from the queue of BSCVTY.
08:43:43.960442 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.960453 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:43:43.960465 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960489 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 36
08:43:43.960505 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.960521 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.960539 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.960550 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 36
08:43:43.960560 Osmocom_VTY_Functions.ttcn:74 Message with id 36 was extracted from the queue of BSCVTY.
08:43:43.960570 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.960586 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "si2quater neighbor-list add earfcn 1 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3"
08:43:43.960598 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960650 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 37
08:43:43.960667 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.960681 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.960700 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.960710 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 37
08:43:43.960720 Osmocom_VTY_Functions.ttcn:74 Message with id 37 was extracted from the queue of BSCVTY.
08:43:43.960730 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.960740 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:43:43.960752 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960766 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 38
08:43:43.960781 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.960797 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.960807 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 38
08:43:43.960817 Osmocom_VTY_Functions.ttcn:73 Message with id 38 was extracted from the queue of BSCVTY.
08:43:43.960826 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.960837 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:43.960850 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960870 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 39
08:43:43.960886 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.960902 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.960920 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.960932 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 39
08:43:43.960942 Osmocom_VTY_Functions.ttcn:74 Message with id 39 was extracted from the queue of BSCVTY.
08:43:43.960952 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.960962 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:43:43.960974 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.960991 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 40
08:43:43.961006 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.961023 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.961041 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.961052 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 40
08:43:43.961063 Osmocom_VTY_Functions.ttcn:74 Message with id 40 was extracted from the queue of BSCVTY.
08:43:43.961074 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.961084 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:43:43.961096 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.961113 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 41
08:43:43.961128 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.961144 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.961162 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.961173 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 41
08:43:43.961182 Osmocom_VTY_Functions.ttcn:74 Message with id 41 was extracted from the queue of BSCVTY.
08:43:43.961192 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.961205 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "si2quater neighbor-list add earfcn 0 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3"
08:43:43.961217 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.961250 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 42
08:43:43.961265 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.961279 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:43.961297 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:43.961308 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 42
08:43:43.961317 Osmocom_VTY_Functions.ttcn:74 Message with id 42 was extracted from the queue of BSCVTY.
08:43:43.961327 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.961337 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:43:43.961349 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:43.961363 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 43
08:43:43.961378 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:43.961394 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:43.961404 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 43
08:43:43.961414 Osmocom_VTY_Functions.ttcn:73 Message with id 43 was extracted from the queue of BSCVTY.
08:43:43.961423 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:43.961434 BSC_Tests.ttcn:1344 Altstep as_catch_RSL_sysinfo was activated as default, id 2
08:43:43.961445 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:43:43.961457 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.019395.
08:43:43.961477 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(152) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "19394662", variable := "bts.0.oml-connection-state", val := omit } }
08:43:43.961491 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:43:43.963511 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(152) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "19394662", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
08:43:43.963529 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:43:43.963541 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(152): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "19394662", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
08:43:43.963552 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
08:43:43.963562 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:43:43.963572 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:43:44.963713 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:43:44.964151 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:43:44.973326 BSC_Tests.ttcn:951 PTC was created. Component reference: 154, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
08:43:44.973503 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1234, bts_id := 0, trx_id := 0 }
08:43:44.973641 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
08:43:44.973946 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(154):IPA_PORT to system:IPA_CODEC_PT.
08:43:44.978631 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(154):IPA_PORT to system:IPA_CODEC_PT finished.
08:43:44.978799 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(154):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
08:43:44.979892 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(154):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-16738b6e.
08:43:44.980478 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(154):CFG_PORT.
08:43:44.980651 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(154):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
08:43:44.980758 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(154):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
08:43:44.981544 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(154):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-7569ab76.
08:43:44.981892 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(154):IPA_RSL_PORT.
08:43:44.982066 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(154):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
08:43:44.982133 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1234/0/0", osmo_rand := "" }, true) on component IPA-BTS0-TRX0-RSL-IPA(154).
08:43:44.982293 BSC_Tests.ttcn:969 Function was started.
08:43:44.982390 BSC_Tests.ttcn:976 Start timer T: 10 s
08:43:44.991303 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
08:43:44.991381 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
08:43:44.991440 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:44.991491 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
08:43:44.991545 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
08:43:44.996642 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
08:43:44.996701 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:44.996736 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
08:43:44.996771 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
08:43:44.996804 BSC_Tests.ttcn:979 Stop timer T: 10 s
08:43:44.996840 BSC_Tests.ttcn:1016 Start timer T: 5 s
08:43:44.996878 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.630194.
08:43:44.996935 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(152) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "630193967", variable := "bts.0.oml-connection-state", val := omit } }
08:43:44.996975 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
08:43:44.999264 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(152) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "630193967", variable := "bts.0.oml-connection-state", val := "connected" } } id 3
08:43:44.999299 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
08:43:44.999329 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(152): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "630193967", variable := "bts.0.oml-connection-state", val := "connected" } } id 3
08:43:44.999356 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
08:43:44.999383 BSC_Tests.ttcn:1019 Stop timer T: 5 s
08:43:44.999408 BSC_Tests.ttcn:1022 Start timer T: 1 s
08:43:45.000370 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 3
08:43:45.000421 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.000458 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.000486 BSC_Tests.ttcn:1148 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 3
08:43:45.000510 BSC_Tests.ttcn:1148 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
08:43:45.000547 BSC_Tests.ttcn:527 dec_SystemInformation(): Stream before decoding: '5506198FB38000000000000000000000000000E504002B'O
08:43:45.000598 BSC_Tests.ttcn:527 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 21, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_1 (25) }, payload := { si1 := { cell_chan_desc := '8FB38000000000000000000000000000'O, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, rest_octets := '2B'O ("+") } } }
08:43:45.000642 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.000716 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 4
08:43:45.000751 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.000783 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.000810 BSC_Tests.ttcn:1148 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 4
08:43:45.000834 BSC_Tests.ttcn:1148 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
08:43:45.000859 BSC_Tests.ttcn:533 dec_SystemInformation(): Stream before decoding: '59061A00000000000000000000000000000000FFE50400'O
08:43:45.000892 BSC_Tests.ttcn:533 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 22, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_2 (26) }, payload := { si2 := { bcch_freq_list := '00000000000000000000000000000000'O, ncc_permitted := '11111111'B, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B } } } }
08:43:45.000924 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.000985 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 5
08:43:45.001024 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 6
08:43:45.001054 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.001079 BSC_Tests.ttcn:1144 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 5
08:43:45.001101 BSC_Tests.ttcn:1144 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
08:43:45.001126 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.001159 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.001190 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.001215 BSC_Tests.ttcn:1148 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 6
08:43:45.001236 BSC_Tests.ttcn:1148 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
08:43:45.001258 BSC_Tests.ttcn:545 dec_SystemInformation(): Stream before decoding: '4906038E3200000000000000000000000008002B2B2B2B'O
08:43:45.001288 BSC_Tests.ttcn:545 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 18, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_2ter (3) }, payload := { si2ter := { extd_bcch_freq_list := '8E320000000000000000000000000800'O, rest_octets := '2B2B2B2B'O ("++++") } } }
08:43:45.001315 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.001973 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB8000DC0002D74AB602B2B'O } } } } } } id 7
08:43:45.002009 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB8000DC0002D74AB602B2B'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.002037 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.002064 BSC_Tests.ttcn:1148 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB8000DC0002D74AB602B2B'O } } } } } } id 7
08:43:45.002089 BSC_Tests.ttcn:1148 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
08:43:45.002111 BSC_Tests.ttcn:551 dec_SystemInformation(): Stream before decoding: '590607400004870000B3006FB8000DC0002D74AB602B2B'O
08:43:45.002198 BSC_Tests.ttcn:551 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 22, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_2quater (7) }, payload := { si2quater := { rest_octets := { ba_ind := '0'B, ba_3g_ind := '1'B, mp_change_mark := '0'B, si2quater_index := 0, si2quater_count := 0, meas_params_desc := { presence := '0'B, desc := omit }, gprs := { rt_diff_desc := { presence := '0'B, desc := omit }, bsic_desc := { presence := '0'B, desc := omit }, rep_prio_desc := { presence := '0'B, desc := omit }, meas_params_desc := { presence := '0'B, desc := omit } }, nc_meas_params := { presence := '0'B, params := omit }, ext_info := { presence := '0'B, info := omit }, utran_neigh_desc := { presence := '0'B, desc := omit }, utran_meas_params_desc := { presence := '0'B, desc := omit }, utran_gprs_meas_params_desc := { presence := '0'B, desc := omit }, rel_additions := { rel5_presence := '1'B, rel5 := { umts_add_meas_params_desc := { presence := '0'B, desc := omit }, umts_add_meas_params_desc2 := { presence := '0'B, desc := omit }, rel6_presence := '1'B, rel6 := { umts_ccn_active := '0'B, rel7_presence := '1'B, rel7 := { rep700 := { presence := '0'B, val := omit }, rep810 := { presence := '0'B, val := omit }, rel8_presence := '1'B, rel8 := { prio_eutran_params_desc := { presence := '1'B, desc := { sc_prio_params_desc := { presence := '1'B, desc := { geran_priority := 0, thresh_priority_search := 0, thresh_gsm_low := 0, h_prio := 0, t_reselection := 0 } }, utran_prio_params_desc := { presence := '0'B, desc := omit }, eutran_params_desc := { presence := '1'B, desc := { ccn_active := '0'B, e_start := '1'B, e_stop := '1'B, meas_params_desc := { presence := '0'B, desc := omit }, gprs_meas_params_desc := { presence := '0'B, desc := omit }, repeated_neigh_cells := { { item_ind := '1'B, cell_desc_list := { { item_ind := '1'B, e_arfcn := 111, meas_bw_presence := '1'B, meas_bw := 3 }, { item_ind := '1'B, e_arfcn := 1, meas_bw_presence := '1'B, meas_bw := 3 }, { item_ind := '1'B, e_arfcn := 0, meas_bw_presence := '1'B, meas_bw := 3 } }, cell_desc_list_term := '0'B, prio_presence := '1'B, prio := 3, thresh_high := 20, thresh_low_presence := '1'B, thresh_low := 10, qrxlevmin_presence := '1'B, qrxlevmin := 22 } }, repeated_neigh_cells_term := '0'B, repeated_not_allowed_cells := omit, repeated_not_allowed_cells_term := '0'B, pcid2ta_map_list := omit, pcid2ta_map_list_term := '0'B } } } }, utran_csg_desc := { presence := '0'B, desc := omit }, eutran_csg_desc := { presence := '0'B, desc := omit } } } } } } } } } }
08:43:45.002268 BSC_Tests.ttcn:551 Warning: dec_SystemInformation(): Data remained at the end of the stream after successful decoding: '2B'O ("+")
08:43:45.002334 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.002414 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } } } id 8
08:43:45.002442 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } } } id 9
08:43:45.002474 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.002506 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.002530 BSC_Tests.ttcn:1148 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } } } id 8
08:43:45.002550 BSC_Tests.ttcn:1148 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
08:43:45.002573 BSC_Tests.ttcn:559 dec_SystemInformation(): Stream before decoding: '49061B000000F1100001C9031E174740E504000C132B2B'O
08:43:45.002620 BSC_Tests.ttcn:559 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 18, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_3 (27) }, payload := { si3 := { cell_id := 0, lai := { mcc_mnc := '001F01'H, lac := 1 }, ctrl_chan_desc := { msc_r99 := true, att := true, bs_ag_blks_res := 1, ccch_conf := CCHAN_DESC_1CCCH_COMBINED (1), si22ind := false, cbq3 := CBQ3_IU_MODE_NOT_SUPPORTED (0), spare := '00'B, bs_pa_mfrms := 3, t3212 := 30 }, cell_options := { dn_ind := false, pwrc := false, dtx := MS_SHALL_USE_UL_DTX (1), radio_link_tout_div4 := 7 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, si_2ter_ind := '1'B, early_cm_ind := '0'B, sched_where := { presence := '0'B, where := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, umts_early_cm_ind := '1'B, si2_quater_ind := { presence := '1'B, ind := '0'B }, iu_mode_ind := omit, si21_ind := { presence := '0'B, pos := omit } } } } }
08:43:45.002670 BSC_Tests.ttcn:559 Warning: dec_SystemInformation(): Data remained at the end of the stream after successful decoding: '2B2B'O ("++")
08:43:45.002707 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.002740 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.002767 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.002792 BSC_Tests.ttcn:1148 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } } } id 9
08:43:45.002814 BSC_Tests.ttcn:1148 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
08:43:45.002838 BSC_Tests.ttcn:565 dec_SystemInformation(): Stream before decoding: '41061C00F11000014740E5040064304367012B2B2B2B2B'O
08:43:45.002874 BSC_Tests.ttcn:565 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 16, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_4 (28) }, payload := { si4 := { lai := { mcc_mnc := '001F01'H, lac := 1 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, cbch_chan_desc := { iei := '64'O ("d"), v := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, tsc := 2, h := false, arfcn := 871, maio_hsn := omit } }, cbch_mobile_alloc := omit, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, s_presence := '0'B, s := omit } } } }
08:43:45.002916 BSC_Tests.ttcn:565 Warning: dec_SystemInformation(): Data remained at the end of the stream after successful decoding: '2B2B2B2B2B'O ("+++++")
08:43:45.002947 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.003012 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 10
08:43:45.003037 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 11
08:43:45.003059 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 12
08:43:45.003081 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 13
08:43:45.003114 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.003141 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.003164 BSC_Tests.ttcn:1148 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 10
08:43:45.003186 BSC_Tests.ttcn:1148 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
08:43:45.003208 BSC_Tests.ttcn:571 dec_SystemInformation(): Stream before decoding: '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O
08:43:45.003244 BSC_Tests.ttcn:571 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 0, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_13 (0) }, payload := { si13 := { rest_octets := { presence := '1'B, bcch_change_mark := 1, si_change_field := '0000'B, presence2 := '0'B, si13_change_mark := omit, gprs_ma := omit, zero := '0'B, rac := 0, spgc_ccch_sup := '0'B, priority_access_thr := '110'B, network_control_order := '00'B, gprs_cell_opts := { nmo := '01'B, t3168 := '011'B, t3192 := '010'B, drx_timer_max := '011'B, access_burst_type := '0'B, control_ack_type := '1'B, bs_cv_max := 15, pan_presence := '1'B, pan_dec := 1, pan_inc := 1, pan_max := '111'B, ext_info_presence := '1'B, ext_info_length := '000101'B, ext_info := { egprs_supported := '0'B, egprs_pkt_channel_req := omit, bep_period := omit, pfc_feature_mode := '0'B, dtm_support := '0'B, bss_paging_coordination := '1'B, ccn_active := '1'B, nw_ext_utbf := '0'B } }, gprs_pwr_ctrl_params := { alpha := 0, t_avg_w := '10000'B, t_avg_t := '10000'B, pc_meas_chan := '0'B, n_avg_i := '1000'B } } } } }
08:43:45.003282 BSC_Tests.ttcn:571 Warning: dec_SystemInformation(): Data remained at the end of the stream after successful decoding: '2B2B2B2B2B2B2B2B2B'O ("+++++++++")
08:43:45.003312 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.003342 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies[0].body{ sysinfo_type := RSL_SYSTEM_INFO_5 (5) } with { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } unmatched.rsl.ies[1].body{ l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } with { sysinfo_type := ? } unmatched: First message in the queue does not match the template: 
08:43:45.003371 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:45.003396 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.003419 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.003441 BSC_Tests.ttcn:1156 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 11
08:43:45.003459 BSC_Tests.ttcn:1156 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
08:43:45.003482 BSC_Tests.ttcn:583 dec_SystemInformation(): Stream before decoding: '49061D10000000000000000000000000000000'O
08:43:45.003503 BSC_Tests.ttcn:583 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 18, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_5 (29) }, payload := { si5 := { bcch_freq_list := '10000000000000000000000000000000'O } } }
08:43:45.003526 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.003549 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.003575 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:45.003595 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.003613 BSC_Tests.ttcn:1152 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 12
08:43:45.003630 BSC_Tests.ttcn:1152 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
08:43:45.003648 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.003672 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies[0].body{ sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } with { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } unmatched.rsl.ies[1].body{ l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } with { sysinfo_type := ? } unmatched: First message in the queue does not match the template: 
08:43:45.003698 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:45.003720 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.003744 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.003763 BSC_Tests.ttcn:1156 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 13
08:43:45.003779 BSC_Tests.ttcn:1156 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
08:43:45.003798 BSC_Tests.ttcn:595 dec_SystemInformation(): Stream before decoding: '4906069E050020000000000000000000000000'O
08:43:45.003817 BSC_Tests.ttcn:595 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 18, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_5ter (6) }, payload := { si5ter := { extd_bcch_freq_list := '9E050020000000000000000000000000'O } } }
08:43:45.003838 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.003891 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } } } id 14
08:43:45.003918 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 15
08:43:45.003945 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies[0].body{ sysinfo_type := RSL_SYSTEM_INFO_6 (6) } with { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } unmatched.rsl.ies[1].body{ l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } with { sysinfo_type := ? } unmatched: First message in the queue does not match the template: 
08:43:45.003972 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_SACCH_FILL (26) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:45.003995 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] .rsl.ies{ { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.004019 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:45.004037 BSC_Tests.ttcn:1156 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } } } id 14
08:43:45.004054 BSC_Tests.ttcn:1156 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
08:43:45.004073 BSC_Tests.ttcn:601 dec_SystemInformation(): Stream before decoding: '2D061E000000F110000197FF2B'O
08:43:45.004102 BSC_Tests.ttcn:601 dec_SystemInformation(): Decoded @GSM_SystemInformation.SystemInformation: { header := { l2_plen := { l2_plen := 11, zero_one := '01'B }, skip_indicator := 0, rr_protocol_discriminator := 6, message_type := SYSTEM_INFORMATION_TYPE_6 (30) }, payload := { si6 := { cell_id := 0, lai := { mcc_mnc := '001F01'H, lac := 1 }, cell_options := { dtx_ext := '1'B, pwrc := false, dtx := '01'B, radio_link_timeout := '0111'B }, ncc_permitted := '11111111'B, rest_octets := { pch_nch_info := { presence := '0'B, info := omit }, vbs_vgcs_options := { presence := '0'B, options := omit }, dtm_support := '0'B, rac := omit, max_lapdm := omit, band_ind := '0'B } } } }
08:43:45.004133 BSC_Tests.ttcn:1023 Default with id 2 (altstep as_catch_RSL_sysinfo) has reached a break statement. Skipping current alt statement or receiving operation.
08:43:45.004163 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.004192 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:45.004219 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:45.004247 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies[0].body{ ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } with { sysinfo_type := ? } unmatched.rsl.ies[1].body{ bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } with { l3_info := { len := ?, payload := ? } } unmatched: First message in the queue does not match the template: 
08:43:46.000390 BSC_Tests.ttcn:1023 Timeout T: 1 s
08:43:46.000828 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:46.001251 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:46.001766 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.002279 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:46.002791 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.003248 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies[0].body{ ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } with { sysinfo_type := ? } unmatched.rsl.ies[1].body{ bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } with { l3_info := { len := ?, payload := ? } } unmatched: First message in the queue does not match the template: 
08:43:46.003713 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 44
08:43:46.004008 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:46.004224 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:46.004445 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:46.004606 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 44
08:43:46.004781 Osmocom_VTY_Functions.ttcn:74 Message with id 44 was extracted from the queue of BSCVTY.
08:43:46.004847 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:46.004915 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:43:46.005027 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:46.005338 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.005603 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:46.005787 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.005954 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies[0].body{ ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } with { sysinfo_type := ? } unmatched.rsl.ies[1].body{ bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } with { l3_info := { len := ?, payload := ? } } unmatched: First message in the queue does not match the template: 
08:43:46.006211 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 45
08:43:46.006513 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:46.006622 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:46.006745 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:43:46.006817 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 45
08:43:46.006883 Osmocom_VTY_Functions.ttcn:74 Message with id 45 was extracted from the queue of BSCVTY.
08:43:46.006945 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:46.007006 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:43:46.007098 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:46.007317 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.007504 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:46.007608 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.007700 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies[0].body{ ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } with { sysinfo_type := ? } unmatched.rsl.ies[1].body{ bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } with { l3_info := { len := ?, payload := ? } } unmatched: First message in the queue does not match the template: 
08:43:46.007882 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 46
08:43:46.008000 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:46.008096 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:46.008211 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:46.008275 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 46
08:43:46.008338 Osmocom_VTY_Functions.ttcn:74 Message with id 46 was extracted from the queue of BSCVTY.
08:43:46.008400 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:46.008461 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
08:43:46.008555 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:46.008680 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.008789 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:46.008885 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.008972 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies[0].body{ ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } with { sysinfo_type := ? } unmatched.rsl.ies[1].body{ bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } with { l3_info := { len := ?, payload := ? } } unmatched: First message in the queue does not match the template: 
08:43:46.009135 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 47
08:43:46.009245 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:46.009337 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:46.009450 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:46.009512 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 47
08:43:46.009573 Osmocom_VTY_Functions.ttcn:74 Message with id 47 was extracted from the queue of BSCVTY.
08:43:46.009634 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:46.009692 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:43:46.009772 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:46.009885 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.009993 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:46.010088 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.010172 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies[0].body{ ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } with { sysinfo_type := ? } unmatched.rsl.ies[1].body{ bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } with { l3_info := { len := ?, payload := ? } } unmatched: First message in the queue does not match the template: 
08:43:46.010330 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 48
08:43:46.010446 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:46.010553 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:46.010615 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 48
08:43:46.010683 Osmocom_VTY_Functions.ttcn:73 Message with id 48 was extracted from the queue of BSCVTY.
08:43:46.010751 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:46.010818 Osmocom_Types.ttcn:126 Start timer T: 5 s
08:43:46.010924 BSC_Tests.ttcn:1144 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.011027 BSC_Tests.ttcn:1148 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_CCHAN (6) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_BCCH_INFO (17) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := ?, body := { sysinfo_type := ? } }, { iei := ?, body := { other := { len := ?, payload := ? } } }, * } unmatched: First message in the queue does not match the template: 
08:43:46.011116 BSC_Tests.ttcn:1152 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies{ { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } with { { iei := ?, body := { sysinfo_type := ? } } } unmatched: First message in the queue does not match the template: 
08:43:46.011199 BSC_Tests.ttcn:1156 Matching on port IPA_RSL[0][0] RSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_SACCH_FILL (26) unmatched.rsl.ies[0].body{ ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } with { sysinfo_type := ? } unmatched.rsl.ies[1].body{ bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } with { l3_info := { len := ?, payload := ? } } unmatched: First message in the queue does not match the template: 
08:43:51.015494 Osmocom_Types.ttcn:127 Timeout T: 5 s
08:43:51.016004 BSC_Tests.ttcn:1353 RSL 0 SYSTEM INFORMATION: { si1 := { cell_chan_desc := '8FB38000000000000000000000000000'O, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, rest_octets := '2B'O ("+") }, si2 := { bcch_freq_list := '00000000000000000000000000000000'O, ncc_permitted := '11111111'B, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B } }, si2bis := omit, si2ter := { extd_bcch_freq_list := '8E320000000000000000000000000800'O, rest_octets := '2B2B2B2B'O ("++++") }, si2quater := { { ba_ind := '0'B, ba_3g_ind := '1'B, mp_change_mark := '0'B, si2quater_index := 0, si2quater_count := 0, meas_params_desc := { presence := '0'B, desc := omit }, gprs := { rt_diff_desc := { presence := '0'B, desc := omit }, bsic_desc := { presence := '0'B, desc := omit }, rep_prio_desc := { presence := '0'B, desc := omit }, meas_params_desc := { presence := '0'B, desc := omit } }, nc_meas_params := { presence := '0'B, params := omit }, ext_info := { presence := '0'B, info := omit }, utran_neigh_desc := { presence := '0'B, desc := omit }, utran_meas_params_desc := { presence := '0'B, desc := omit }, utran_gprs_meas_params_desc := { presence := '0'B, desc := omit }, rel_additions := { rel5_presence := '1'B, rel5 := { umts_add_meas_params_desc := { presence := '0'B, desc := omit }, umts_add_meas_params_desc2 := { presence := '0'B, desc := omit }, rel6_presence := '1'B, rel6 := { umts_ccn_active := '0'B, rel7_presence := '1'B, rel7 := { rep700 := { presence := '0'B, val := omit }, rep810 := { presence := '0'B, val := omit }, rel8_presence := '1'B, rel8 := { prio_eutran_params_desc := { presence := '1'B, desc := { sc_prio_params_desc := { presence := '1'B, desc := { geran_priority := 0, thresh_priority_search := 0, thresh_gsm_low := 0, h_prio := 0, t_reselection := 0 } }, utran_prio_params_desc := { presence := '0'B, desc := omit }, eutran_params_desc := { presence := '1'B, desc := { ccn_active := '0'B, e_start := '1'B, e_stop := '1'B, meas_params_desc := { presence := '0'B, desc := omit }, gprs_meas_params_desc := { presence := '0'B, desc := omit }, repeated_neigh_cells := { { item_ind := '1'B, cell_desc_list := { { item_ind := '1'B, e_arfcn := 111, meas_bw_presence := '1'B, meas_bw := 3 }, { item_ind := '1'B, e_arfcn := 1, meas_bw_presence := '1'B, meas_bw := 3 }, { item_ind := '1'B, e_arfcn := 0, meas_bw_presence := '1'B, meas_bw := 3 } }, cell_desc_list_term := '0'B, prio_presence := '1'B, prio := 3, thresh_high := 20, thresh_low_presence := '1'B, thresh_low := 10, qrxlevmin_presence := '1'B, qrxlevmin := 22 } }, repeated_neigh_cells_term := '0'B, repeated_not_allowed_cells := omit, repeated_not_allowed_cells_term := '0'B, pcid2ta_map_list := omit, pcid2ta_map_list_term := '0'B } } } }, utran_csg_desc := { presence := '0'B, desc := omit }, eutran_csg_desc := { presence := '0'B, desc := omit } } } } } } } }, si3 := { cell_id := 0, lai := { mcc_mnc := '001F01'H, lac := 1 }, ctrl_chan_desc := { msc_r99 := true, att := true, bs_ag_blks_res := 1, ccch_conf := CCHAN_DESC_1CCCH_COMBINED (1), si22ind := false, cbq3 := CBQ3_IU_MODE_NOT_SUPPORTED (0), spare := '00'B, bs_pa_mfrms := 3, t3212 := 30 }, cell_options := { dn_ind := false, pwrc := false, dtx := MS_SHALL_USE_UL_DTX (1), radio_link_tout_div4 := 7 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, si_2ter_ind := '1'B, early_cm_ind := '0'B, sched_where := { presence := '0'B, where := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, umts_early_cm_ind := '1'B, si2_quater_ind := { presence := '1'B, ind := '0'B }, iu_mode_ind := omit, si21_ind := { presence := '0'B, pos := omit } } }, si4 := { lai := { mcc_mnc := '001F01'H, lac := 1 }, cell_sel_par := { cell_resel_hyst_2dB := 2, ms_txpwr_max_cch := 7, acs := '0'B, neci := true, rxlev_access_min := 0 }, rach_control := { max_retrans := RACH_MAX_RETRANS_7 (3), tx_integer := '1001'B, cell_barr_access := false, re_not_allowed := true, acc := '0000010000000000'B }, cbch_chan_desc := { iei := '64'O ("d"), v := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 2 } }, tn := 0 }, tsc := 2, h := false, arfcn := 871, maio_hsn := omit } }, cbch_mobile_alloc := omit, rest_octets := { sel_params := { presence := '0'B, params := omit }, pwr_offset := { presence := '0'B, offset := omit }, gprs_ind := { presence := '1'B, ind := { ra_colour := 0, si13_pos := '0'B } }, s_presence := '0'B, s := omit } }, si13 := { rest_octets := { presence := '1'B, bcch_change_mark := 1, si_change_field := '0000'B, presence2 := '0'B, si13_change_mark := omit, gprs_ma := omit, zero := '0'B, rac := 0, spgc_ccch_sup := '0'B, priority_access_thr := '110'B, network_control_order := '00'B, gprs_cell_opts := { nmo := '01'B, t3168 := '011'B, t3192 := '010'B, drx_timer_max := '011'B, access_burst_type := '0'B, control_ack_type := '1'B, bs_cv_max := 15, pan_presence := '1'B, pan_dec := 1, pan_inc := 1, pan_max := '111'B, ext_info_presence := '1'B, ext_info_length := '000101'B, ext_info := { egprs_supported := '0'B, egprs_pkt_channel_req := omit, bep_period := omit, pfc_feature_mode := '0'B, dtm_support := '0'B, bss_paging_coordination := '1'B, ccn_active := '1'B, nw_ext_utbf := '0'B } }, gprs_pwr_ctrl_params := { alpha := 0, t_avg_w := '10000'B, t_avg_t := '10000'B, pc_meas_chan := '0'B, n_avg_i := '1000'B } } }, si5 := { bcch_freq_list := '10000000000000000000000000000000'O }, si5bis := omit, si5ter := { extd_bcch_freq_list := '9E050020000000000000000000000000'O }, si6 := { cell_id := 0, lai := { mcc_mnc := '001F01'H, lac := 1 }, cell_options := { dtx_ext := '1'B, pwrc := false, dtx := '01'B, radio_link_timeout := '0111'B }, ncc_permitted := '11111111'B, rest_octets := { pch_nch_info := { presence := '0'B, info := omit }, vbs_vgcs_options := { presence := '0'B, options := omit }, dtm_support := '0'B, rac := omit, max_lapdm := omit, band_ind := '0'B } } }
08:43:51.018082 BSC_Tests.ttcn:1355 Default with id 2 (altstep as_catch_RSL_sysinfo) was deactivated.
08:43:51.018769 BSC_Tests.ttcn:1358 setverdict(pass): none -> pass
08:43:51.019215 Osmocom_Types.ttcn:65 Function rnd() returned 0.189231.
08:43:51.019551 Osmocom_Types.ttcn:65 Function rnd() returned 0.957026.
08:43:51.019901 Osmocom_Types.ttcn:65 Function rnd() returned 0.485822.
08:43:51.020080 Osmocom_Types.ttcn:65 Function rnd() returned 0.908316.
08:43:51.020231 Osmocom_Types.ttcn:65 Function rnd() returned 0.383604.
08:43:51.020304 Osmocom_Types.ttcn:65 Function rnd() returned 0.896630.
08:43:51.020638 Osmocom_Types.ttcn:65 Function rnd() returned 0.588232.
08:43:51.020971 Osmocom_Types.ttcn:65 Function rnd() returned 0.570166.
08:43:51.021157 Osmocom_Types.ttcn:65 Function rnd() returned 0.817663.
08:43:51.021300 Osmocom_Types.ttcn:65 Function rnd() returned 0.031040.
08:43:51.021649 BSC_Tests.ttcn:618 enc_PDU_ML3_MS_NW(): Encoding @MobileL3_Types.PDU_ML3_MS_NW: { discriminator := '0000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { mm := { locationUpdateRequest := { messageType := '000000'B, nsd := '00'B, locationUpdatingType := { lut := '10'B, spare1_1 := '0'B, fop := '0'B }, cipheringKeySequenceNumber := { keySequence := '000'B, spare := '0'B }, locationAreaIdentification := { mcc_mnc := '123456'O, lac := '172A'O }, mobileStationClassmark1 := { rf_PowerCapability := '010'B, a5_1 := '0'B, esind := '1'B, revisionLevel := '10'B, spare1_1 := '0'B }, mobileIdentityLV := { lengthIndicator := 0, mobileIdentityV := { typeOfIdentity := '001'B, oddEvenInd_identity := { imsi := { oddevenIndicator := '1'B, digits := '001011949385580'H, fillerDigit := omit } } } }, classmarkInformationType2_forUMTS := omit, additionalUpdateParameterTV := omit, deviceProperties := omit, mS_NetworkFeatureSupport := omit } } } }
08:43:51.021910 BSC_Tests.ttcn:618 enc_PDU_ML3_MS_NW(): Stream after encoding: '050802123456172A52080910109194835508'O
08:43:51.022217 BSC_Tests.ttcn:1394 Sent on IPA_RSL[0][0] to IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_CHAN_RQD (19), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_RACH (17) }, tn := 0 } } }, { iei := RSL_IE_REQ_REFERENCE (19), body := { req_ref := { ra := '23'O ("#"), frame_nr := { t1_p := 0, t3 := 23, t2 := 23 } } } }, { iei := RSL_IE_ACCESS_DELAY (17), body := { access_delay := 0 } } } } }
08:43:51.022424 BSC_Tests.ttcn:1375 Start timer T: 2 s
08:43:51.022537 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] RSL_MDISC_TRX_MGMT (8) with RSL_MDISC_DCHAN (4) unmatchedRSL_MT_IPAC_MEAS_PREPROC_DFT (96) with RSL_MT_CHAN_ACTIV (33) unmatched: First message in the queue does not match the template: 
08:43:51.022618 BSC_Tests.ttcn:1380 Matching on port IPA_RSL[0][0] succeeded.
08:43:51.022714 BSC_Tests.ttcn:1380 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata: { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 15
08:43:51.022788 BSC_Tests.ttcn:1380 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
08:43:51.031455 BSC_Tests.ttcn:1376 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_CHAN_ACTIV (33), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_ACT_TYPE (3), body := { act_type := { reactivation := false, reserved := 0, a_bits := ACT_REL_TO_IMM_ASSIGN (0) } } }, { iei := RSL_IE_CHAN_MODE (6), body := { chan_mode := { len := 4, reserved := '000000'B, dtx_d := true, dtx_u := true, spd_ind := RSL_SPDI_SIGN (3), ch_rate_type := RSL_CHRT_SDCCH (1), u := { sign := RSL_CMOD_NO_RESOURCE (0) } } } }, { iei := RSL_IE_CHAN_IDENT (5), body := { chan_ident := { len := 6, ch_desc := { iei := '64'O ("d"), v := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, tsc := 2, h := false, arfcn := 871, maio_hsn := omit } }, ma := { iei := '72'O ("r"), v := { len := 0, ma := ''B } } } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 7 } } }, { iei := RSL_IE_TIMING_ADVANCE (24), body := { timing_adv := 0 } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 0, params := ''O } } } } } } id 16
08:43:51.031598 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:51.031708 BSC_Tests.ttcn:1377 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_CHAN_ACTIV (33), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_ACT_TYPE (3), body := { act_type := { reactivation := false, reserved := 0, a_bits := ACT_REL_TO_IMM_ASSIGN (0) } } }, { iei := RSL_IE_CHAN_MODE (6), body := { chan_mode := { len := 4, reserved := '000000'B, dtx_d := true, dtx_u := true, spd_ind := RSL_SPDI_SIGN (3), ch_rate_type := RSL_CHRT_SDCCH (1), u := { sign := RSL_CMOD_NO_RESOURCE (0) } } } }, { iei := RSL_IE_CHAN_IDENT (5), body := { chan_ident := { len := 6, ch_desc := { iei := '64'O ("d"), v := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 }, tsc := 2, h := false, arfcn := 871, maio_hsn := omit } }, ma := { iei := '72'O ("r"), v := { len := 0, ma := ''B } } } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 7 } } }, { iei := RSL_IE_TIMING_ADVANCE (24), body := { timing_adv := 0 } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 0, params := ''O } } } } } } id 16
08:43:51.031800 BSC_Tests.ttcn:1377 Message with id 16 was extracted from the queue of IPA_RSL[0][0].
08:43:51.031869 BSC_Tests.ttcn:1378 Stop timer T: 2 s
08:43:51.032031 BSC_Tests.ttcn:1394 Sent on IPA_RSL[0][0] to IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_CHAN_ACTIV_ACK (34), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_FRAME_NUMBER (8), body := { frame_nr := { t1_p := 0, t3 := 33, t2 := 7 } } } } } }
08:43:51.032147 BSC_Tests.ttcn:1375 Start timer T: 2 s
08:43:51.034240 BSC_Tests.ttcn:1376 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_IMMEDIATE_ASSIGN_CMD (22), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_FULL_IMM_ASS_INFO (43), body := { full_imm_ass_info := { len := 23, payload := '2D063F032043672302F700002B2B2B2B2B2B2B2B2B2B2B'O } } } } } } id 17
08:43:51.034354 BSC_Tests.ttcn:1377 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:51.034447 BSC_Tests.ttcn:1377 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_IMMEDIATE_ASSIGN_CMD (22), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_PCH_AGCH (18) }, tn := 0 } } }, { iei := RSL_IE_FULL_IMM_ASS_INFO (43), body := { full_imm_ass_info := { len := 23, payload := '2D063F032043672302F700002B2B2B2B2B2B2B2B2B2B2B'O } } } } } } id 17
08:43:51.034517 BSC_Tests.ttcn:1377 Message with id 17 was extracted from the queue of IPA_RSL[0][0].
08:43:51.034588 BSC_Tests.ttcn:1378 Stop timer T: 2 s
08:43:51.034766 BSC_Tests.ttcn:1394 Sent on IPA_RSL[0][0] to IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_RLL (1), transparent := false }, msg_type := RSL_MT_EST_IND (6), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_LINK_IDENT (2), body := { link_id := { c := FACCH_SDCCH (0), na := false, prio := SAPI0_PRIO_NORMAL (0), sapi := 0 } } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 0, payload := '050802123456172A52080910109194835508'O } } } } } }
08:43:51.039992 BSC_Tests.ttcn:1971 Message enqueued on BSSAP from VirtMSC-SCCP(148) @SCCPasp_Types.ASP_SCCP_N_CONNECT_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, qualityOfService := omit, userData := '002A5705080000F110000100001712050802123456172A520809101091948355087D09808283045781840407'O, connectionId := 4990300, importance := omit } id 2
08:43:51.040111 BSSAP_CodecPort.ttcn:233 dec_PDU_BSSAP(): Stream before decoding: '002A5705080000F110000100001712050802123456172A520809101091948355087D09808283045781840407'O
08:43:51.040674 BSSAP_CodecPort.ttcn:233 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 42, pdu := { bssmap := { completeLayer3Information := { messageType := '57'O ("W"), cellIdentifier := { elementIdentifier := '05'O, lengthIndicator := 8, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_CGI := { mcc_mnc := '00F110'O, lac := '0001'O, ci := '0000'O } } }, layer3Information := { elementIdentifier := '17'O, lengthIndicator := 18, layer3info := '050802123456172A52080910109194835508'O }, chosenChannel := omit, lSAIdentifier := omit, aPDU := omit, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 9, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '01010111'B }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '00000111'B } } }, redirectAttemptFlag := omit, sendSequenceNumber := omit, iMSI := omit } } } }
08:43:51.040917 BSC_Tests.ttcn:1971 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_CONNECT_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, qualityOfService := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 42, pdu := { bssmap := { completeLayer3Information := { messageType := '57'O ("W"), cellIdentifier := { elementIdentifier := '05'O, lengthIndicator := 8, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_CGI := { mcc_mnc := '00F110'O, lac := '0001'O, ci := '0000'O } } }, layer3Information := { elementIdentifier := '17'O, lengthIndicator := 18, layer3info := '050802123456172A52080910109194835508'O }, chosenChannel := omit, lSAIdentifier := omit, aPDU := omit, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 9, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '01010111'B }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '00000111'B } } }, redirectAttemptFlag := omit, sendSequenceNumber := omit, iMSI := omit } } } }, connectionId := 4990300, importance := omit } id 2
08:43:51.041202 BSC_Tests.ttcn:1971 Matching on port BSSAP succeeded:  matched
08:43:51.041399 BSC_Tests.ttcn:1971 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(148): @BSSAP_CodecPort.BSSAP_N_CONNECT_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, qualityOfService := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 42, pdu := { bssmap := { completeLayer3Information := { messageType := '57'O ("W"), cellIdentifier := { elementIdentifier := '05'O, lengthIndicator := 8, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_CGI := { mcc_mnc := '00F110'O, lac := '0001'O, ci := '0000'O } } }, layer3Information := { elementIdentifier := '17'O, lengthIndicator := 18, layer3info := '050802123456172A52080910109194835508'O }, chosenChannel := omit, lSAIdentifier := omit, aPDU := omit, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 9, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '01010111'B }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '00000111'B } } }, redirectAttemptFlag := omit, sendSequenceNumber := omit, iMSI := omit } } } }, connectionId := 4990300, importance := omit } id 2
08:43:51.041563 BSC_Tests.ttcn:1971 Message with id 2 was extracted from the queue of BSSAP.
08:43:51.041756 BSC_Tests.ttcn:1973 Sent on BSSAP to VirtMSC-SCCP(148) @BSSAP_CodecPort.BSSAP_N_CONNECT_res : { respondingAddress := omit, expeditedDataSel := omit, qualityOfService := omit, userData := omit, connectionId := 4990300, importance := omit }
08:43:51.041822 BSC_Tests.ttcn:1973 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_CONNECT_res : { respondingAddress := omit, expeditedDataSel := omit, qualityOfService := omit, userData := omit, connectionId := 4990300, importance := omit }
08:43:51.042023 BSC_Tests.ttcn:2831 Sent on BSSAP to VirtMSC-SCCP(148) @BSSAP_CodecPort.BSSAP_N_DATA_req : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { commonID := { messageType := '2F'O ("/"), iMSI := { elementIdentifier := '08'O ("\b"), lengthIndicator := 0, typeOfIdentity := '001'B, oddEvenIndicator := '1'B, digits := '001019876543210'H }, sNAAccessInformation := omit, selectedPLMNId := omit, lastUsedEUTRANPLMNId := { elementIdentifier := '95'O, mcc_mnc := '323454'O ("24T") } } } } }, connectionId := 4990300, importance := omit }
08:43:51.042087 BSSAP_CodecPort.ttcn:327 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { commonID := { messageType := '2F'O ("/"), iMSI := { elementIdentifier := '08'O ("\b"), lengthIndicator := 0, typeOfIdentity := '001'B, oddEvenIndicator := '1'B, digits := '001019876543210'H }, sNAAccessInformation := omit, selectedPLMNId := omit, lastUsedEUTRANPLMNId := { elementIdentifier := '95'O, mcc_mnc := '323454'O ("24T") } } } } }
08:43:51.042219 BSSAP_CodecPort.ttcn:327 enc_PDU_BSSAP(): Stream after encoding: '000F2F0808091010896745230195323454'O
08:43:51.042284 BSC_Tests.ttcn:2831 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_DATA_req : { userData := '000F2F0808091010896745230195323454'O, connectionId := 4990300, importance := omit }
08:43:51.042454 BSC_Tests.ttcn:2835 Sent on BSSAP to VirtMSC-SCCP(148) @BSSAP_CodecPort.BSSAP_N_DATA_req : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { clearCommand := { messageType := '20'O (" "), layer3HeaderInfo := omit, cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, cSFB_Indication := { elementIdentifier := '8F'O } } } } }, connectionId := 4990300, importance := omit }
08:43:51.042512 BSSAP_CodecPort.ttcn:327 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { clearCommand := { messageType := '20'O (" "), layer3HeaderInfo := omit, cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, cSFB_Indication := { elementIdentifier := '8F'O } } } } }
08:43:51.042603 BSSAP_CodecPort.ttcn:327 enc_PDU_BSSAP(): Stream after encoding: '0005200401008F'O
08:43:51.042662 BSC_Tests.ttcn:2835 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_DATA_req : { userData := '0005200401008F'O, connectionId := 4990300, importance := omit }
08:43:51.249361 BSC_Tests.ttcn:2838 Message enqueued on BSSAP from VirtMSC-SCCP(148) @SCCPasp_Types.ASP_SCCP_N_DATA_ind : { userData := '000121'O, connectionId := 4990300, importance := omit } id 3
08:43:51.249773 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Stream before decoding: '000121'O
08:43:51.250115 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { clearComplete := { messageType := '21'O ("!") } } } }
08:43:51.250327 BSC_Tests.ttcn:2838 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { clearComplete := { messageType := '21'O ("!") } } } }, connectionId := 4990300, importance := omit } id 3
08:43:51.250758 BSC_Tests.ttcn:2838 Matching on port BSSAP succeeded:  matched
08:43:51.251032 BSC_Tests.ttcn:2838 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(148): @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { clearComplete := { messageType := '21'O ("!") } } } }, connectionId := 4990300, importance := omit } id 3
08:43:51.251402 BSC_Tests.ttcn:2838 Message with id 3 was extracted from the queue of BSSAP.
08:43:51.251772 BSC_Tests.ttcn:2840 Sent on BSSAP to VirtMSC-SCCP(148) @BSSAP_CodecPort.BSSAP_N_DISCONNECT_req : { respondingAddress := omit, reason := 0, userData := omit, connectionId := 4990300, importance := omit }
08:43:51.251913 BSC_Tests.ttcn:2840 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_DISCONNECT_req : { respondingAddress := omit, reason := 0, userData := omit, connectionId := 4990300, importance := omit }
08:43:51.252105 BSC_Tests.ttcn:2210 f_expect_chan_rel() expecting: expect_deact_sacch=true expect_rr_chan_rel=true expect_rll_rel_req=false
08:43:51.252892 BSC_Tests.ttcn:2212 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_RLL (1), transparent := true }, msg_type := RSL_MT_DATA_REQ (1), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_LINK_IDENT (2), body := { link_id := { c := FACCH_SDCCH (0), na := false, prio := SAPI0_PRIO_NORMAL (0), sapi := 0 } } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 15, payload := '060D6F770A7006FB20003640002C00'O } } } } } } id 18
08:43:51.253240 BSC_Tests.ttcn:2213 Matching on port IPA_RSL[0][0] RSL_MDISC_RLL (1) with RSL_MDISC_DCHAN (4) unmatched.rsl.msg_disc.transparent := true with false unmatchedRSL_MT_DATA_REQ (1) with RSL_MT_DEACTIVATE_SACCH (37) unmatched.rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_LINK_IDENT (2), body := { link_id := { c := FACCH_SDCCH (0), na := false, prio := SAPI0_PRIO_NORMAL (0), sapi := 0 } } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 15, payload := '060D6F770A7006FB20003640002C00'O } } } } with { { iei := ?, body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } unmatched: First message in the queue does not match the template: 
08:43:51.253786 BSC_Tests.ttcn:2217 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:51.253943 BSC_Tests.ttcn:2217 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_RLL (1), transparent := true }, msg_type := RSL_MT_DATA_REQ (1), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := RSL_IE_LINK_IDENT (2), body := { link_id := { c := FACCH_SDCCH (0), na := false, prio := SAPI0_PRIO_NORMAL (0), sapi := 0 } } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 15, payload := '060D6F770A7006FB20003640002C00'O } } } } } } id 18
08:43:51.254365 BSC_Tests.ttcn:2217 Message with id 18 was extracted from the queue of IPA_RSL[0][0].
08:43:51.254533 BSC_Tests.ttcn:2224 dec_PDU_ML3_NW_MS(): Stream before decoding: '060D6F770A7006FB20003640002C00'O
08:43:51.254826 BSC_Tests.ttcn:2224 dec_PDU_ML3_NW_MS(): Decoded @MobileL3_Types.PDU_ML3_NW_MS: { discriminator := '0110'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { rrm := { channelRelease := { messageType := '00001101'B, rRCause := { valuePart := '6F'O ("o") }, bARange := omit, groupChannelDescription := omit, groupCipherKeyNumber := omit, gPRSResumption := omit, bAListPref := omit, uTRANFrequencyList := omit, cellChannelDescr := omit, cellSelectionIndicator := { elementIdentifier := '77'O ("w"), lengthIndicator := 10, cellSelectionIndicatorValue := '7006FB20003640002C00'O }, enhanced_DTM_CS_Release_Indication := omit, vGCS_Ciphering_Parameters := omit, group_Channel_Description_2 := omit, talkerIdentity := omit, talkerPriorityStatus := omit, vGCS_AMR_Configuration := omit, individual_Priorities := omit } } } }
08:43:51.255015 BSC_Tests.ttcn:2227 dec_CellSelIndValue(): Stream before decoding: '7006FB20003640002C00'O
08:43:51.255204 BSC_Tests.ttcn:2227 dec_CellSelIndValue(): Decoded @GSM_RR_Types.CellSelIndValue: { discr := '011'B, value_list := { eutran := { { item_ind := '1'B, earfcn := 111, meas_bw_presence := '1'B, meas_bw := 3, not_allowed_cells_presence := '0'B, not_allowed_cells := omit, target_pcid_presence := '0'B, target_pcid := omit }, { item_ind := '1'B, earfcn := 1, meas_bw_presence := '1'B, meas_bw := 3, not_allowed_cells_presence := '0'B, not_allowed_cells := omit, target_pcid_presence := '0'B, target_pcid := omit }, { item_ind := '1'B, earfcn := 0, meas_bw_presence := '1'B, meas_bw := 3, not_allowed_cells_presence := '0'B, not_allowed_cells := omit, target_pcid_presence := '0'B, target_pcid := omit } } }, value_list_term := '0'B }
08:43:51.255383 BSC_Tests.ttcn:2227 Warning: dec_CellSelIndValue(): Data remained at the end of the stream after successful decoding: '00'O
08:43:51.255468 BSC_Tests.ttcn:2230 GOT RR CHANNEL RELEASE WITH CELLS: { discr := '011'B, value_list := { eutran := { { item_ind := '1'B, earfcn := 111, meas_bw_presence := '1'B, meas_bw := 3, not_allowed_cells_presence := '0'B, not_allowed_cells := omit, target_pcid_presence := '0'B, target_pcid := omit }, { item_ind := '1'B, earfcn := 1, meas_bw_presence := '1'B, meas_bw := 3, not_allowed_cells_presence := '0'B, not_allowed_cells := omit, target_pcid_presence := '0'B, target_pcid := omit }, { item_ind := '1'B, earfcn := 0, meas_bw_presence := '1'B, meas_bw := 3, not_allowed_cells_presence := '0'B, not_allowed_cells := omit, target_pcid_presence := '0'B, target_pcid := omit } } }, value_list_term := '0'B }
08:43:51.255706 BSC_Tests.ttcn:2232 setverdict(pass): pass -> pass, component reason not changed
08:43:51.255803 BSC_Tests.ttcn:2240 GOT CAUSE CODE: '6F'O ("o") = GSM48_RR_CAUSE_PROT_ERROR_UNSPC (111)
08:43:51.255903 BSC_Tests.ttcn:2242 setverdict(pass): pass -> pass, component reason not changed
08:43:51.256292 BSC_Tests.ttcn:2212 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_DEACTIVATE_SACCH (37), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } } } id 19
08:43:51.256403 BSC_Tests.ttcn:2213 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:51.256483 BSC_Tests.ttcn:2213 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_DEACTIVATE_SACCH (37), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } } } id 19
08:43:51.256555 BSC_Tests.ttcn:2213 Message with id 19 was extracted from the queue of IPA_RSL[0][0].
08:43:53.251642 BSC_Tests.ttcn:2212 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_RF_CHAN_REL (46), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } } } id 20
08:43:53.252018 BSC_Tests.ttcn:2213 Matching on port IPA_RSL[0][0] RSL_MT_RF_CHAN_REL (46) with RSL_MT_DEACTIVATE_SACCH (37) unmatched: First message in the queue does not match the template: 
08:43:53.252490 BSC_Tests.ttcn:2217 Matching on port IPA_RSL[0][0] RSL_MDISC_DCHAN (4) with RSL_MDISC_RLL (1) unmatched.rsl.msg_disc.transparent := false with true unmatchedRSL_MT_RF_CHAN_REL (46) with RSL_MT_DATA_REQ (1) unmatched.rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } with { { iei := ?, body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := ?, body := { link_id := ? } }, { iei := ?, body := { l3_info := { len := ?, payload := decmatch PDU_ML3_NW_MS: { discriminator := '0110'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { rrm := { channelRelease := { messageType := '00001101'B, rRCause := { valuePart := ? }, bARange := *, groupChannelDescription := *, groupCipherKeyNumber := *, gPRSResumption := *, bAListPref := *, uTRANFrequencyList := *, cellChannelDescr := *, cellSelectionIndicator := *, enhanced_DTM_CS_Release_Indication := *, vGCS_Ciphering_Parameters := *, group_Channel_Description_2 := *, talkerIdentity := *, talkerPriorityStatus := *, vGCS_AMR_Configuration := *, individual_Priorities := * } } } } } } } } unmatched: First message in the queue does not match the template: 
08:43:53.252742 BSC_Tests.ttcn:2249 Matching on port IPA_RSL[0][0] RSL_MDISC_DCHAN (4) with RSL_MDISC_RLL (1) unmatchedRSL_MT_RF_CHAN_REL (46) with RSL_MT_REL_REQ (7) unmatched.rsl.ies{ { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } with { { iei := ?, body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } }, { iei := ?, body := { link_id := ? } }, { iei := ?, body := { release_mode := ? } } } unmatched: First message in the queue does not match the template: 
08:43:53.252929 BSC_Tests.ttcn:2257 Matching on port IPA_RSL[0][0] succeeded:  matched
08:43:53.253048 BSC_Tests.ttcn:2257 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(154): @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_RF_CHAN_REL (46), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } } } id 20
08:43:53.253148 BSC_Tests.ttcn:2257 Message with id 20 was extracted from the queue of IPA_RSL[0][0].
08:43:53.253347 BSC_Tests.ttcn:1394 Sent on IPA_RSL[0][0] to IPA-BTS0-TRX0-RSL-IPA(154) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := omit, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_DCHAN (4), transparent := false }, msg_type := RSL_MT_RF_CHAN_REL_ACK (51), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { sdcch4 := { tag := '001'B, sub_chan := 0 } }, tn := 0 } } } } } }
08:43:53.253499 BSC_Tests.ttcn:2267 f_expect_chan_rel() summary: got_deact_sacch=true got_rr_chan_rel=true got_rll_rel_req=false
08:43:53.253678 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:53.253847 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.254229 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 49
08:43:53.254453 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.254621 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.254809 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.254910 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 49
08:43:53.255004 Osmocom_VTY_Functions.ttcn:74 Message with id 49 was extracted from the queue of BSCVTY.
08:43:53.255096 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.255189 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:43:53.255322 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.255598 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 50
08:43:53.255761 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.255915 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.256089 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.256187 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 50
08:43:53.256273 Osmocom_VTY_Functions.ttcn:74 Message with id 50 was extracted from the queue of BSCVTY.
08:43:53.256362 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.256451 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:43:53.256579 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.256867 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 51
08:43:53.257021 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.257187 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.257357 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.257451 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 51
08:43:53.257537 Osmocom_VTY_Functions.ttcn:74 Message with id 51 was extracted from the queue of BSCVTY.
08:43:53.257624 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.257720 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "si2quater neighbor-list del earfcn 1"
08:43:53.257838 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.258038 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 52
08:43:53.258072 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.258103 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.258140 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.258160 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 52
08:43:53.258178 Osmocom_VTY_Functions.ttcn:74 Message with id 52 was extracted from the queue of BSCVTY.
08:43:53.258197 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.258216 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:43:53.258242 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.258327 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 53
08:43:53.258362 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.258393 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:53.258413 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 53
08:43:53.258431 Osmocom_VTY_Functions.ttcn:73 Message with id 53 was extracted from the queue of BSCVTY.
08:43:53.258450 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.258470 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
08:43:53.258497 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.258596 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 54
08:43:53.258630 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.258662 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.258698 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.258719 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 54
08:43:53.258738 Osmocom_VTY_Functions.ttcn:74 Message with id 54 was extracted from the queue of BSCVTY.
08:43:53.258757 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.258777 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
08:43:53.258802 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.258890 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 55
08:43:53.258924 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.258956 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.258992 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.259013 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 55
08:43:53.259032 Osmocom_VTY_Functions.ttcn:74 Message with id 55 was extracted from the queue of BSCVTY.
08:43:53.259051 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.259070 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
08:43:53.259096 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.259172 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 56
08:43:53.259205 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.259236 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.259272 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.259293 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 56
08:43:53.259312 Osmocom_VTY_Functions.ttcn:74 Message with id 56 was extracted from the queue of BSCVTY.
08:43:53.259330 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.259351 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "si2quater neighbor-list del earfcn 0"
08:43:53.259376 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.259463 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 57
08:43:53.259496 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.259527 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.259563 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
08:43:53.259584 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 57
08:43:53.259602 Osmocom_VTY_Functions.ttcn:74 Message with id 57 was extracted from the queue of BSCVTY.
08:43:53.259621 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.259639 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
08:43:53.259665 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.259740 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 58
08:43:53.259773 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.259805 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:53.259825 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 58
08:43:53.259843 Osmocom_VTY_Functions.ttcn:73 Message with id 58 was extracted from the queue of BSCVTY.
08:43:53.259865 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.259975 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
08:43:53.260008 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
08:43:53.260212 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" id 59
08:43:53.260234 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 60
08:43:53.260270 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.260301 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
08:43:53.260333 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
08:43:53.260356 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
08:43:53.260376 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with ? matched
08:43:53.260395 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" id 59
08:43:53.260413 Osmocom_VTY_Functions.ttcn:85 Message with id 59 was extracted from the queue of BSCVTY.
08:43:53.260441 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
08:43:53.260470 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
08:43:53.260489 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 60
08:43:53.260506 Osmocom_VTY_Functions.ttcn:73 Message with id 60 was extracted from the queue of BSCVTY.
08:43:53.260524 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
08:43:53.260542 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
08:43:53.260567 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
08:43:53.260591 BSC_Tests.ttcn:888 Stopping all components.
08:43:53.262890 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(152):IPA_CTRL_PORT was closed unexpectedly by the peer.
08:43:53.262990 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(152):IPA_CTRL_PORT.
08:43:53.263111 BSC_Tests.ttcn:888 All components were stopped.
08:43:53.263194 BSC_Tests.ttcn:889 setverdict(pass): pass -> pass, component reason not changed
08:43:53.263270 BSC_Tests.ttcn:890 Stopping test component execution.
08:43:53.263454 BSC_Tests.ttcn:2897 Test case TC_si2quater_3_earfcns was stopped.
08:43:53.263560 BSC_Tests.ttcn:2897 Terminating component type BSC_Tests.test_CT.
08:43:53.263625 BSC_Tests.ttcn:2897 Default with id 1 (altstep as_Tguard) was deactivated.
08:43:53.263683 BSC_Tests.ttcn:2897 Stop timer T_guard: 30 s
08:43:53.263755 BSC_Tests.ttcn:2897 Port IPA_CTRL was stopped.
08:43:53.263813 BSC_Tests.ttcn:2897 Port RSL_CCHAN[0] was stopped.
08:43:53.263868 BSC_Tests.ttcn:2897 Port RSL_CCHAN[1] was stopped.
08:43:53.263926 BSC_Tests.ttcn:2897 Port RSL_CCHAN[2] was stopped.
08:43:53.263984 BSC_Tests.ttcn:2897 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(154):IPA_RSL_PORT.
08:43:53.264104 BSC_Tests.ttcn:2897 Port IPA_RSL[0][0] was stopped.
08:43:53.264230 BSC_Tests.ttcn:2897 Port IPA_RSL[0][1] was stopped.
08:43:53.264297 BSC_Tests.ttcn:2897 Port IPA_RSL[0][2] was stopped.
08:43:53.264362 BSC_Tests.ttcn:2897 Port IPA_RSL[0][3] was stopped.
08:43:53.264425 BSC_Tests.ttcn:2897 Port IPA_RSL[1][0] was stopped.
08:43:53.264490 BSC_Tests.ttcn:2897 Port IPA_RSL[1][1] was stopped.
08:43:53.264554 BSC_Tests.ttcn:2897 Port IPA_RSL[1][2] was stopped.
08:43:53.264617 BSC_Tests.ttcn:2897 Port IPA_RSL[1][3] was stopped.
08:43:53.264680 BSC_Tests.ttcn:2897 Port IPA_RSL[2][0] was stopped.
08:43:53.264743 BSC_Tests.ttcn:2897 Port IPA_RSL[2][1] was stopped.
08:43:53.264806 BSC_Tests.ttcn:2897 Port IPA_RSL[2][2] was stopped.
08:43:53.264870 BSC_Tests.ttcn:2897 Port IPA_RSL[2][3] was stopped.
08:43:53.264935 BSC_Tests.ttcn:2897 Port IPA was stopped.
08:43:53.264998 BSC_Tests.ttcn:2897 Port SCCPLITE_IPA_CTRL was stopped.
08:43:53.265061 BSC_Tests.ttcn:2897 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(154):CFG_PORT.
08:43:53.265159 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[0][0] was stopped.
08:43:53.265250 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[0][1] was stopped.
08:43:53.265316 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[0][2] was stopped.
08:43:53.265381 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[0][3] was stopped.
08:43:53.265445 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[1][0] was stopped.
08:43:53.265510 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[1][1] was stopped.
08:43:53.265574 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[1][2] was stopped.
08:43:53.265637 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[1][3] was stopped.
08:43:53.265701 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[2][0] was stopped.
08:43:53.265764 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[2][1] was stopped.
08:43:53.265828 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[2][2] was stopped.
08:43:53.265892 BSC_Tests.ttcn:2897 Port IPA_CFG_PORT[2][3] was stopped.
08:43:53.265958 BSC_Tests.ttcn:2897 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
08:43:53.266087 BSC_Tests.ttcn:2897 Port BSCVTY was unmapped from system:BSCVTY.
08:43:53.266179 BSC_Tests.ttcn:2897 Port BSCVTY was stopped.
08:43:53.266247 BSC_Tests.ttcn:2897 Port STPVTY was stopped.
08:43:53.266401 BSC_Tests.ttcn:2897 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
08:43:53.266600 BSC_Tests.ttcn:2897 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
08:43:53.266683 BSC_Tests.ttcn:2897 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
08:43:53.266749 BSC_Tests.ttcn:2897 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(148):SCCP_SP_PORT.
08:43:53.266883 BSC_Tests.ttcn:2897 Port BSSAP was stopped.
08:43:53.266956 BSC_Tests.ttcn:2897 Removing unterminated connection between port BSSAP_LE and VirtSMLC-SCCP(150):SCCP_SP_PORT.
08:43:53.267060 BSC_Tests.ttcn:2897 Port BSSAP_LE was stopped.
08:43:53.267124 BSC_Tests.ttcn:2897 Component type BSC_Tests.test_CT was shut down inside testcase TC_si2quater_3_earfcns.
08:43:53.267186 BSC_Tests.ttcn:2897 Waiting for PTCs to finish.
08:43:53.271729 BSC_Tests.ttcn:2897 Setting final verdict of the test case.
08:43:53.271979 BSC_Tests.ttcn:2897 Local verdict of MTC: pass
08:43:53.272169 BSC_Tests.ttcn:2897 Local verdict of PTC VirtMSC-STATS(147): none (pass -> pass)
08:43:53.272427 BSC_Tests.ttcn:2897 Local verdict of PTC VirtMSC-SCCP(148): none (pass -> pass)
08:43:53.272626 BSC_Tests.ttcn:2897 Local verdict of PTC VirtMSC-M3UA(149): none (pass -> pass)
08:43:53.272762 BSC_Tests.ttcn:2897 Local verdict of PTC VirtSMLC-SCCP(150): none (pass -> pass)
08:43:53.272911 BSC_Tests.ttcn:2897 Local verdict of PTC VirtSMLC-M3UA(151): none (pass -> pass)
08:43:53.273027 BSC_Tests.ttcn:2897 Local verdict of PTC IPA-CTRL-CLI-IPA(152): none (pass -> pass)
08:43:53.273058 BSC_Tests.ttcn:2897 Local verdict of PTC VirtMGW-MGCP-0(153): none (pass -> pass)
08:43:53.273087 BSC_Tests.ttcn:2897 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(154): none (pass -> pass)
08:43:53.273133 BSC_Tests.ttcn:2897 Test case TC_si2quater_3_earfcns finished. Verdict: pass
08:43:53.273182 BSC_Tests.ttcn:2897 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_si2quater_3_earfcns pass'.
08:43:58.509263 BSC_Tests.ttcn:2897 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_si2quater_3_earfcns pass' was executed successfully (exit status: 0).
08:43:58.509353 BSC_Tests.ttcn:2900 Switching to log file `BSC_Tests-TC_si2quater_4_earfcns-d5b21e48044a-mtc-9786.log'
