09:00:37.216534 BSC_Tests.ttcn:5024 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_assignment_codec_amr_h_S024'.
09:00:38.231830 BSC_Tests.ttcn:5024 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_assignment_codec_amr_h_S024' was executed successfully (exit status: 0).
09:00:38.232128 BSC_Tests.ttcn:5024 Test case TC_assignment_codec_amr_h_S024 started.
09:00:38.232247 BSC_Tests.ttcn:5024 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_assignment_codec_amr_h_S024.
09:00:38.232522 BSC_Tests.ttcn:5024 Port IPA_CTRL was started.
09:00:38.232616 BSC_Tests.ttcn:5024 Port RSL_CCHAN[0] was started.
09:00:38.232898 BSC_Tests.ttcn:5024 Port RSL_CCHAN[1] was started.
09:00:38.233174 BSC_Tests.ttcn:5024 Port RSL_CCHAN[2] was started.
09:00:38.233454 BSC_Tests.ttcn:5024 Port IPA_RSL[0][0] was started.
09:00:38.233740 BSC_Tests.ttcn:5024 Port IPA_RSL[0][1] was started.
09:00:38.233945 BSC_Tests.ttcn:5024 Port IPA_RSL[0][2] was started.
09:00:38.234027 BSC_Tests.ttcn:5024 Port IPA_RSL[0][3] was started.
09:00:38.234102 BSC_Tests.ttcn:5024 Port IPA_RSL[1][0] was started.
09:00:38.234174 BSC_Tests.ttcn:5024 Port IPA_RSL[1][1] was started.
09:00:38.234246 BSC_Tests.ttcn:5024 Port IPA_RSL[1][2] was started.
09:00:38.234471 BSC_Tests.ttcn:5024 Port IPA_RSL[1][3] was started.
09:00:38.234564 BSC_Tests.ttcn:5024 Port IPA_RSL[2][0] was started.
09:00:38.234615 BSC_Tests.ttcn:5024 Port IPA_RSL[2][1] was started.
09:00:38.234661 BSC_Tests.ttcn:5024 Port IPA_RSL[2][2] was started.
09:00:38.234707 BSC_Tests.ttcn:5024 Port IPA_RSL[2][3] was started.
09:00:38.234754 BSC_Tests.ttcn:5024 Port IPA was started.
09:00:38.234801 BSC_Tests.ttcn:5024 Port SCCPLITE_IPA_CTRL was started.
09:00:38.234849 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[0][0] was started.
09:00:38.234896 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[0][1] was started.
09:00:38.234942 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[0][2] was started.
09:00:38.234988 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[0][3] was started.
09:00:38.235033 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[1][0] was started.
09:00:38.235080 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[1][1] was started.
09:00:38.235125 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[1][2] was started.
09:00:38.235172 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[1][3] was started.
09:00:38.235217 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[2][0] was started.
09:00:38.235263 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[2][1] was started.
09:00:38.235309 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[2][2] was started.
09:00:38.235354 BSC_Tests.ttcn:5024 Port IPA_CFG_PORT[2][3] was started.
09:00:38.235400 BSC_Tests.ttcn:5024 Port BSCVTY was started.
09:00:38.235446 BSC_Tests.ttcn:5024 Port STPVTY was started.
09:00:38.235492 BSC_Tests.ttcn:5024 Port SCCPLITE_IPA_CFG_PORT[0] was started.
09:00:38.235538 BSC_Tests.ttcn:5024 Port SCCPLITE_IPA_CFG_PORT[1] was started.
09:00:38.235584 BSC_Tests.ttcn:5024 Port SCCPLITE_IPA_CFG_PORT[2] was started.
09:00:38.235632 BSC_Tests.ttcn:5024 Port BSSAP was started.
09:00:38.235679 BSC_Tests.ttcn:5024 Port BSSAP_LE was started.
09:00:38.235727 BSC_Tests.ttcn:5024 Component type BSC_Tests.test_CT was initialized.
09:00:38.235931 Osmocom_Types.ttcn:65 Function rnd() returned 0.185748.
09:00:38.236005 Osmocom_Types.ttcn:65 Function rnd() returned 0.374412.
09:00:38.236058 Osmocom_Types.ttcn:65 Function rnd() returned 0.143229.
09:00:38.236110 Osmocom_Types.ttcn:65 Function rnd() returned 0.082683.
09:00:38.236163 Osmocom_Types.ttcn:65 Function rnd() returned 0.654085.
09:00:38.236214 Osmocom_Types.ttcn:65 Function rnd() returned 0.450696.
09:00:38.236265 Osmocom_Types.ttcn:65 Function rnd() returned 0.233092.
09:00:38.236316 Osmocom_Types.ttcn:65 Function rnd() returned 0.438190.
09:00:38.236366 Osmocom_Types.ttcn:65 Function rnd() returned 0.013016.
09:00:38.236416 Osmocom_Types.ttcn:65 Function rnd() returned 0.155085.
09:00:38.236469 Osmocom_Types.ttcn:65 Function rnd() returned 0.613857.
09:00:38.236520 Osmocom_Types.ttcn:65 Function rnd() returned 0.674956.
09:00:38.236593 Osmocom_Types.ttcn:65 Function rnd() returned 0.567726.
09:00:38.236645 Osmocom_Types.ttcn:65 Function rnd() returned 0.214449.
09:00:38.236696 Osmocom_Types.ttcn:65 Function rnd() returned 0.500874.
09:00:38.236747 Osmocom_Types.ttcn:65 Function rnd() returned 0.577131.
09:00:38.236797 Osmocom_Types.ttcn:65 Function rnd() returned 0.674249.
09:00:38.236848 Osmocom_Types.ttcn:65 Function rnd() returned 0.140954.
09:00:38.236898 Osmocom_Types.ttcn:65 Function rnd() returned 0.212912.
09:00:38.236950 BSC_Tests.ttcn:738 "TC_assignment_codec_amr_h_S024": using IMSI '001011310642401'H
09:00:38.237160 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
09:00:38.237223 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
09:00:38.237282 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
09:00:38.237958 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
09:00:38.238036 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
09:00:38.238231 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
09:00:38.238331 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 1, prompt := "OsmoBSC> ", has_wildcards := false } }
09:00:38.238406 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 2, prompt := "OsmoBSC# ", has_wildcards := false } }
09:00:38.238462 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 3, prompt := "OsmoBSC(*)", has_wildcards := true } }
09:00:38.238601 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
09:00:38.238694 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.238761 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:00:38.238815 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:00:38.238864 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:00:38.238913 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:00:38.238962 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:00:38.239017 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
09:00:38.239074 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
09:00:38.239131 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
09:00:38.239294 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
09:00:38.239438 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.239548 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.239605 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
09:00:38.239660 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
09:00:38.239718 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.239783 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:38.239864 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.240220 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
09:00:38.240321 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.240435 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.240559 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.240621 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
09:00:38.240679 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
09:00:38.240738 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.240797 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
09:00:38.240871 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.241134 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
09:00:38.241227 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.241314 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.241423 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.241483 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
09:00:38.241537 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
09:00:38.241594 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.241652 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
09:00:38.241719 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.241969 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
09:00:38.242059 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.242143 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.242246 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.242326 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
09:00:38.242383 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
09:00:38.242441 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.242496 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
09:00:38.242564 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.242817 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
09:00:38.242902 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.242985 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.243085 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.243144 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
09:00:38.243198 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
09:00:38.243254 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.243306 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:00:38.243383 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.243599 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
09:00:38.243684 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.243770 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.243827 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
09:00:38.243881 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
09:00:38.243937 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.243994 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:38.244060 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.244335 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
09:00:38.244421 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.244505 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.244606 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.244665 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
09:00:38.244720 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
09:00:38.244776 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.244832 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
09:00:38.244898 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.244992 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
09:00:38.245077 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.245159 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.245257 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.245315 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
09:00:38.245379 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
09:00:38.245437 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.245499 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
09:00:38.245575 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.245680 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
09:00:38.245787 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.245872 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.245975 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.246032 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
09:00:38.246087 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
09:00:38.246154 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.246208 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.246277 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.246391 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
09:00:38.246480 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.246563 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.246663 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.246719 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
09:00:38.246773 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
09:00:38.246828 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.246879 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.246946 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.247023 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
09:00:38.247105 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.247189 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.247246 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
09:00:38.247300 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
09:00:38.247354 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.247411 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
09:00:38.260980 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 835, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
09:00:38.261044 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(835).
09:00:38.261237 StatsD_Checker.ttcnpp:417 Function was started.
09:00:38.261295 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
09:00:38.261365 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.261701 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
09:00:38.261803 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.261917 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.261978 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
09:00:38.262035 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
09:00:38.262094 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.262153 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
09:00:38.262229 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.262609 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 14
09:00:38.262734 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.262819 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.262877 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 14
09:00:38.262943 Osmocom_VTY_Functions.ttcn:73 Message with id 14 was extracted from the queue of BSCVTY.
09:00:38.262998 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.263053 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
09:00:38.263124 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.264030 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
09:00:38.264120 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.264205 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.264261 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
09:00:38.264315 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
09:00:38.264369 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.264530 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
09:00:38.270619 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 836, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
09:00:38.270655 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
09:00:38.275586 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 837, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
09:00:38.275609 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(837):SCTP_PORT to system:sctp.
09:00:38.277109 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(837):SCTP_PORT to system:sctp finished.
09:00:38.277130 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(837):MTP3_SP_PORT and VirtMSC-SCCP(836):MTP3_SCCP_PORT.
09:00:38.277785 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(837):MTP3_SP_PORT and VirtMSC-SCCP(836):MTP3_SCCP_PORT finished.
09:00:38.277813 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({ local_sctp_port := 23905, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 1) on component VirtMSC-M3UA(837).
09:00:38.277862 SCCP_Adapter.ttcnpp:127 Function was started.
09:00:38.277890 RAN_Adapter.ttcnpp:57 Creating new alive PTC with component type RAN_Emulation.RAN_Emulation_CT, component name: VirtMSC-RAN.
09:00:38.282189 RAN_Adapter.ttcnpp:57 PTC was created. Component reference: 838, alive: yes, type: RAN_Emulation.RAN_Emulation_CT, component name: VirtMSC-RAN.
09:00:38.282208 RAN_Adapter.ttcnpp:60 Start timer T: 5 s
09:00:38.282224 RAN_Adapter.ttcnpp:72 Connecting BSSAP RAN_Emulation to SCCP_SP_PORT
09:00:38.282241 RAN_Adapter.ttcnpp:73 Connecting ports VirtMSC-RAN(838):BSSAP and VirtMSC-SCCP(836):SCCP_SP_PORT.
09:00:38.283898 RAN_Adapter.ttcnpp:73 Connect operation on VirtMSC-RAN(838):BSSAP and VirtMSC-SCCP(836):SCCP_SP_PORT finished.
09:00:38.283922 RAN_Adapter.ttcnpp:90 Starting RAN_Emulation
09:00:38.283941 RAN_Adapter.ttcnpp:91 Starting function main({ create_cb := refers(RAN_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MSC_ConnectionHandler.UnitdataCallback), decode_dtap := false, role_ms := false, protocol := RAN_PROTOCOL_BSSAP (0), transport := BSSAP_TRANSPORT_AoIP (0), use_osmux := false, bssap_reset_retries := 1, sccp_addr_local := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sccp_addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit } }, "") on component VirtMSC-RAN(838).
09:00:38.284020 RAN_Adapter.ttcnpp:91 Function was started.
09:00:38.284043 BSC_Tests.ttcn:1216 Connecting ports mtc:SCCPLITE_IPA_CTRL and VirtMSC-RAN(838):CTRL_CLIENT.
09:00:38.284264 BSC_Tests.ttcn:1216 Port SCCPLITE_IPA_CTRL is waiting for connection from VirtMSC-RAN(838):CTRL_CLIENT on UNIX pathname /tmp/ttcn3-portconn-893ae002.
09:00:38.288418 BSC_Tests.ttcn:1216 Port SCCPLITE_IPA_CTRL has accepted the connection from VirtMSC-RAN(838):CTRL_CLIENT.
09:00:38.288456 BSC_Tests.ttcn:1216 Connect operation on mtc:SCCPLITE_IPA_CTRL and VirtMSC-RAN(838):CTRL_CLIENT finished.
09:00:38.288489 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 185, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 254 }) on component VirtMSC-SCCP(836).
09:00:38.288554 SCCP_Adapter.ttcnpp:165 Function was started.
09:00:38.288620 BSSAP_LE_Adapter.ttcn:95 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
09:00:38.294041 BSSAP_LE_Adapter.ttcn:95 PTC was created. Component reference: 839, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
09:00:38.294096 BSSAP_LE_Adapter.ttcn:97 Creating new alive PTC with component type BSSAP_LE_Emulation.BSSAP_LE_Emulation_CT, component name: VirtSMLC-BSSAP_LE.
09:00:38.297769 BSSAP_LE_Adapter.ttcn:97 PTC was created. Component reference: 840, alive: yes, type: BSSAP_LE_Emulation.BSSAP_LE_Emulation_CT, component name: VirtSMLC-BSSAP_LE.
09:00:38.297788 BSSAP_LE_Adapter.ttcn:101 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
09:00:38.300673 BSSAP_LE_Adapter.ttcn:101 PTC was created. Component reference: 841, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
09:00:38.300691 BSSAP_LE_Adapter.ttcn:102 Mapping port VirtSMLC-M3UA(841):SCTP_PORT to system:sctp.
09:00:38.301925 BSSAP_LE_Adapter.ttcn:102 Map operation of VirtSMLC-M3UA(841):SCTP_PORT to system:sctp finished.
09:00:38.301942 BSSAP_LE_Adapter.ttcn:104 Connecting ports VirtSMLC-M3UA(841):MTP3_SP_PORT and VirtSMLC-SCCP(839):MTP3_SCCP_PORT.
09:00:38.302216 BSSAP_LE_Adapter.ttcn:104 Connect operation on VirtSMLC-M3UA(841):MTP3_SP_PORT and VirtSMLC-SCCP(839):MTP3_SCCP_PORT finished.
09:00:38.302236 BSSAP_LE_Adapter.ttcn:105 Starting function f_M3UA_Emulation({ local_sctp_port := 23908, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 6) on component VirtSMLC-M3UA(841).
09:00:38.302272 BSSAP_LE_Adapter.ttcn:105 Function was started.
09:00:38.302290 BSSAP_LE_Adapter.ttcn:109 Start timer T: 5 s
09:00:38.302315 BSSAP_LE_Adapter.ttcn:112 Connecting BSSAP_LE_Emulation to SCCP_SP_PORT
09:00:38.302346 BSSAP_LE_Adapter.ttcn:113 Connecting ports VirtSMLC-BSSAP_LE(840):BSSAP_LE and VirtSMLC-SCCP(839):SCCP_SP_PORT.
09:00:38.302645 BSSAP_LE_Adapter.ttcn:113 Connect operation on VirtSMLC-BSSAP_LE(840):BSSAP_LE and VirtSMLC-SCCP(839):SCCP_SP_PORT finished.
09:00:38.302678 BSSAP_LE_Adapter.ttcn:114 Starting BSSAP_LE_Emulation
09:00:38.302711 BSSAP_LE_Adapter.ttcn:115 Starting function main({ create_cb := refers(BSSAP_LE_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MSC_ConnectionHandler.BSSAP_LE_UnitdataCallback), decode_dtap := false, role_ms := false, bssap_le_reset_retries := 1, sccp_addr_local := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111110'B, subsystemNumber := 252, globalTitle := omit }, sccp_addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 250, globalTitle := omit } }, "") on component VirtSMLC-BSSAP_LE(840).
09:00:38.302778 BSSAP_LE_Adapter.ttcn:115 Function was started.
09:00:38.302804 BSSAP_LE_Adapter.ttcn:122 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 190, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 252 }) on component VirtSMLC-SCCP(839).
09:00:38.302855 BSSAP_LE_Adapter.ttcn:122 Function was started.
09:00:38.302878 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
09:00:38.302920 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.304940 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
09:00:38.304984 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
09:00:38.306187 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.307504 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.309110 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
09:00:38.311225 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
09:00:38.313023 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with ? matched
09:00:38.314560 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
09:00:38.314594 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
09:00:38.314625 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.314651 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.314669 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
09:00:38.314684 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
09:00:38.314699 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.314721 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:38.314743 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.314851 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 18
09:00:38.314877 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.314901 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.314930 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.314946 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 18
09:00:38.314962 Osmocom_VTY_Functions.ttcn:74 Message with id 18 was extracted from the queue of BSCVTY.
09:00:38.314978 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.314994 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
09:00:38.315013 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.315104 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 19
09:00:38.315127 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.315148 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.315173 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.315188 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 19
09:00:38.315202 Osmocom_VTY_Functions.ttcn:74 Message with id 19 was extracted from the queue of BSCVTY.
09:00:38.315216 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.315231 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
09:00:38.315247 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.315333 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 20
09:00:38.315353 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.315374 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.315398 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.315413 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 20
09:00:38.315426 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
09:00:38.315440 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.315454 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.315471 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.315551 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 21
09:00:38.315572 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.315595 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.315619 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.315634 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 21
09:00:38.315648 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
09:00:38.315662 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.315675 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.315692 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.315768 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 22
09:00:38.315788 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.315809 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.315824 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 22
09:00:38.315838 Osmocom_VTY_Functions.ttcn:73 Message with id 22 was extracted from the queue of BSCVTY.
09:00:38.315852 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.315868 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:38.315885 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.315970 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
09:00:38.315991 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.316011 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.316035 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.316050 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
09:00:38.316064 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
09:00:38.316078 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.316092 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1"
09:00:38.316109 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.316131 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 24
09:00:38.316154 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.316174 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.316196 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.316210 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 24
09:00:38.316224 Osmocom_VTY_Functions.ttcn:74 Message with id 24 was extracted from the queue of BSCVTY.
09:00:38.316238 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.316251 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
09:00:38.316268 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.316289 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 25
09:00:38.316311 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.316330 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.316353 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.316367 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 25
09:00:38.316380 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
09:00:38.316393 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.316406 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.316422 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.316499 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 26
09:00:38.316518 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.316537 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.316560 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.316574 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 26
09:00:38.316587 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
09:00:38.316601 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.316614 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.316629 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.316647 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 27
09:00:38.316667 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.316687 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.316701 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 27
09:00:38.316715 Osmocom_VTY_Functions.ttcn:73 Message with id 27 was extracted from the queue of BSCVTY.
09:00:38.316728 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.316743 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:38.316760 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.316784 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 28
09:00:38.316804 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.316824 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.316847 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.316861 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 28
09:00:38.316875 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
09:00:38.316888 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.316902 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2"
09:00:38.316921 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.316943 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 29
09:00:38.316965 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.316984 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.317007 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.317021 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 29
09:00:38.317034 Osmocom_VTY_Functions.ttcn:74 Message with id 29 was extracted from the queue of BSCVTY.
09:00:38.317047 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.317061 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
09:00:38.317076 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.317097 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 30
09:00:38.317116 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.317134 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.317156 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.317170 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 30
09:00:38.317183 Osmocom_VTY_Functions.ttcn:74 Message with id 30 was extracted from the queue of BSCVTY.
09:00:38.317196 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.317209 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.317224 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.317244 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 31
09:00:38.317263 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.317285 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:38.317306 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:38.317320 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 31
09:00:38.317332 Osmocom_VTY_Functions.ttcn:74 Message with id 31 was extracted from the queue of BSCVTY.
09:00:38.317345 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.317357 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:00:38.317372 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:38.317389 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
09:00:38.317408 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:38.317427 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:38.317440 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
09:00:38.317453 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
09:00:38.317468 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:38.317481 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
09:00:38.320918 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 842, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
09:00:38.320938 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(842):IPA_PORT to system:IPA_CODEC_PT.
09:00:38.322424 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(842):IPA_PORT to system:IPA_CODEC_PT finished.
09:00:38.322445 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(842):IPA_CTRL_PORT and mtc:IPA_CTRL.
09:00:38.322723 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(842):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-c837f21f.
09:00:38.322856 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(842):IPA_CTRL_PORT.
09:00:38.322916 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(842):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
09:00:38.322936 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, { ser_nr := "", name := "mahlzeit", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "0/1/2", osmo_rand := "" }, false) on component IPA-CTRL-CLI-IPA(842).
09:00:38.322980 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
09:00:38.323000 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
09:00:38.324898 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(842) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:00:38.324926 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
09:00:38.324949 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(842): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:00:38.324972 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
09:00:38.325047 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
09:00:38.331870 BSC_Tests.ttcn:1073 PTC was created. Component reference: 843, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
09:00:38.331916 BSC_Tests.ttcn:1074 Starting function main({ create_cb := refers(MGCP_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback) }, { callagent_ip := "127.0.0.1", callagent_udp_port := -1, mgw_ip := "127.0.0.1", mgw_udp_port := 2427, multi_conn_mode := false }, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(843).
09:00:38.332060 BSC_Tests.ttcn:1074 Function was started.
09:00:38.332091 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:00:38.332122 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.028860.
09:00:38.332177 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "28860469", variable := "bts.0.oml-connection-state", val := omit } }
09:00:38.332213 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:00:38.338364 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "28860469", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
09:00:38.338423 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:00:38.338468 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(842): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "28860469", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
09:00:38.338519 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
09:00:38.338560 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:00:38.338598 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:00:38.488078 BSC_Tests.ttcn:1023 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc.0.connection_status", val := "connected" } } id 3
09:00:38.490108 BSC_Tests.ttcn:1023 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc_connection_status", val := "connected" } } id 4
09:00:39.339228 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:00:39.339718 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
09:00:39.348732 BSC_Tests.ttcn:951 PTC was created. Component reference: 844, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
09:00:39.348781 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1234, bts_id := 0, trx_id := 0 }
09:00:39.348902 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
09:00:39.348995 BSC_Tests.ttcn:956 Creating new alive PTC with component type RSL_Emulation.RSL_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-RSL.
09:00:39.358419 BSC_Tests.ttcn:956 PTC was created. Component reference: 845, alive: yes, type: RSL_Emulation.RSL_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-RSL.
09:00:39.358500 BSC_Tests.ttcn:957 Connecting ports IPA-BTS0-TRX0-RSL-RSL(845):CCHAN_PT and mtc:RSL_CCHAN[0].
09:00:39.358984 BSC_Tests.ttcn:957 Port RSL_CCHAN[0] is waiting for connection from IPA-BTS0-TRX0-RSL-RSL(845):CCHAN_PT on UNIX pathname /tmp/ttcn3-portconn-9358f91e.
09:00:39.360996 BSC_Tests.ttcn:957 Port RSL_CCHAN[0] has accepted the connection from IPA-BTS0-TRX0-RSL-RSL(845):CCHAN_PT.
09:00:39.361100 BSC_Tests.ttcn:957 Connect operation on IPA-BTS0-TRX0-RSL-RSL(845):CCHAN_PT and mtc:RSL_CCHAN[0] finished.
09:00:39.361268 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(844):IPA_PORT to system:IPA_CODEC_PT.
09:00:39.361645 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(844):IPA_PORT to system:IPA_CODEC_PT finished.
09:00:39.361682 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(844):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
09:00:39.362058 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(844):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-c0708b6e.
09:00:39.362269 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(844):CFG_PORT.
09:00:39.362327 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(844):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
09:00:39.362360 BSC_Tests.ttcn:963 Connecting ports IPA-BTS0-TRX0-RSL-IPA(844):IPA_RSL_PORT and IPA-BTS0-TRX0-RSL-RSL(845):IPA_PT.
09:00:39.362914 BSC_Tests.ttcn:963 Connect operation on IPA-BTS0-TRX0-RSL-IPA(844):IPA_RSL_PORT and IPA-BTS0-TRX0-RSL-RSL(845):IPA_PT finished.
09:00:39.362950 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1234/0/0", osmo_rand := "" }, true) on component IPA-BTS0-TRX0-RSL-IPA(844).
09:00:39.363033 BSC_Tests.ttcn:969 Function was started.
09:00:39.363067 BSC_Tests.ttcn:971 Starting function main(true) on component IPA-BTS0-TRX0-RSL-RSL(845).
09:00:39.363129 BSC_Tests.ttcn:971 Function was started.
09:00:39.363162 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:00:39.363202 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.115856.
09:00:39.363262 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "115856039", variable := "bts.0.oml-connection-state", val := omit } }
09:00:39.363306 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:00:39.363366 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL { trap := { variable := "msc.0.connection_status", val := "connected" } } with { resp := { verb := "GET_REPLY", id := "115856039", variable := "bts.0.oml-connection-state", val := ? } } unmatched: First message in the queue does not match the template: 
09:00:39.363407 Osmocom_CTRL_Functions.ttcn:43 Matching on port IPA_CTRL succeeded:  matched
09:00:39.363442 Osmocom_CTRL_Functions.ttcn:43 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(842): @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc.0.connection_status", val := "connected" } } id 3
09:00:39.363479 Osmocom_CTRL_Functions.ttcn:43 Message with id 3 was extracted from the queue of IPA_CTRL.
09:00:39.363521 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL { trap := { variable := "msc_connection_status", val := "connected" } } with { resp := { verb := "GET_REPLY", id := "115856039", variable := "bts.0.oml-connection-state", val := ? } } unmatched: First message in the queue does not match the template: 
09:00:39.363554 Osmocom_CTRL_Functions.ttcn:43 Matching on port IPA_CTRL succeeded:  matched
09:00:39.363587 Osmocom_CTRL_Functions.ttcn:43 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(842): @Osmocom_CTRL_Types.CtrlMessage : { trap := { variable := "msc_connection_status", val := "connected" } } id 4
09:00:39.363626 Osmocom_CTRL_Functions.ttcn:43 Message with id 4 was extracted from the queue of IPA_CTRL.
09:00:39.366078 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "115856039", variable := "bts.0.oml-connection-state", val := "degraded" } } id 5
09:00:39.366121 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:00:39.366158 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(842): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "115856039", variable := "bts.0.oml-connection-state", val := "degraded" } } id 5
09:00:39.366191 Osmocom_CTRL_Functions.ttcn:41 Message with id 5 was extracted from the queue of IPA_CTRL.
09:00:39.366229 Osmocom_Types.ttcn:126 Start timer T: 0.1 s
09:00:39.380325 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 1
09:00:39.380755 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 2
09:00:39.381192 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 3
09:00:39.381452 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 4
09:00:39.381794 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O } } } } } } id 5
09:00:39.382026 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } } } id 6
09:00:39.382248 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } } } id 7
09:00:39.382595 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 8
09:00:39.382791 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 9
09:00:39.382980 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 10
09:00:39.383236 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 11
09:00:39.383407 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } } } id 12
09:00:39.383700 Osmocom_Types.ttcn:127 Message enqueued on RSL_CCHAN[0] from IPA-BTS0-TRX0-RSL-RSL(845) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 13
09:00:39.466269 Osmocom_Types.ttcn:127 Timeout T: 0.1 s
09:00:39.466653 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.013063.
09:00:39.467010 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "13063262", variable := "bts.0.oml-connection-state", val := omit } }
09:00:39.467361 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:00:39.473458 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(842) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "13063262", variable := "bts.0.oml-connection-state", val := "connected" } } id 6
09:00:39.473649 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:00:39.473767 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(842): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "13063262", variable := "bts.0.oml-connection-state", val := "connected" } } id 6
09:00:39.473872 Osmocom_CTRL_Functions.ttcn:41 Message with id 6 was extracted from the queue of IPA_CTRL.
09:00:39.473976 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:00:39.474075 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:00:40.474335 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:00:40.474765 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:40.475184 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.475723 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 33
09:00:40.476167 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.476598 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.477089 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.477293 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 33
09:00:40.477463 Osmocom_VTY_Functions.ttcn:74 Message with id 33 was extracted from the queue of BSCVTY.
09:00:40.477638 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.477823 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
09:00:40.478047 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.478381 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 34
09:00:40.478516 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.478624 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.478743 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.478812 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 34
09:00:40.478875 Osmocom_VTY_Functions.ttcn:74 Message with id 34 was extracted from the queue of BSCVTY.
09:00:40.478942 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.479005 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
09:00:40.479088 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.479368 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 35
09:00:40.479464 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.479553 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.479663 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.479723 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 35
09:00:40.479778 Osmocom_VTY_Functions.ttcn:74 Message with id 35 was extracted from the queue of BSCVTY.
09:00:40.479836 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.479894 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
09:00:40.479964 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.480279 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 36
09:00:40.480368 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.480453 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.480558 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.480617 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 36
09:00:40.480672 Osmocom_VTY_Functions.ttcn:74 Message with id 36 was extracted from the queue of BSCVTY.
09:00:40.480729 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.480785 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:00:40.480852 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.481120 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 37
09:00:40.481221 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.481311 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:40.481369 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 37
09:00:40.481422 Osmocom_VTY_Functions.ttcn:73 Message with id 37 was extracted from the queue of BSCVTY.
09:00:40.481478 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.481533 Osmocom_VTY_Functions.ttcn:338 "TC_assignment_codec_amr_h_S024() start"
09:00:40.481632 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_assignment_codec_amr_h_S024() start"
09:00:40.481705 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.482055 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 38
09:00:40.482149 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.482238 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:40.482296 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 38
09:00:40.482503 Osmocom_VTY_Functions.ttcn:73 Message with id 38 was extracted from the queue of BSCVTY.
09:00:40.482584 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.482757 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:40.482941 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.483240 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 39
09:00:40.483424 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.483609 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.483813 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.483889 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 39
09:00:40.483947 Osmocom_VTY_Functions.ttcn:74 Message with id 39 was extracted from the queue of BSCVTY.
09:00:40.484006 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.484065 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
09:00:40.484133 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.484388 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 40
09:00:40.484476 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.484560 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.484664 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.484722 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 40
09:00:40.484777 Osmocom_VTY_Functions.ttcn:74 Message with id 40 was extracted from the queue of BSCVTY.
09:00:40.484834 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.484890 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 12_2k allowed"
09:00:40.484955 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.485225 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 41
09:00:40.485311 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.485395 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.485495 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.485554 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 41
09:00:40.485609 Osmocom_VTY_Functions.ttcn:74 Message with id 41 was extracted from the queue of BSCVTY.
09:00:40.485666 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.485722 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 10_2k forbidden"
09:00:40.485788 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.486052 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 42
09:00:40.486138 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.486223 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.486338 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.486398 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 42
09:00:40.486453 Osmocom_VTY_Functions.ttcn:74 Message with id 42 was extracted from the queue of BSCVTY.
09:00:40.486511 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.486567 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 7_95k forbidden"
09:00:40.486633 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.486887 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 43
09:00:40.486972 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.487055 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.487156 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.487215 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 43
09:00:40.487269 Osmocom_VTY_Functions.ttcn:74 Message with id 43 was extracted from the queue of BSCVTY.
09:00:40.487325 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.487381 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 7_40k allowed"
09:00:40.487446 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.487701 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 44
09:00:40.487785 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.487868 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.487965 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.488033 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 44
09:00:40.488088 Osmocom_VTY_Functions.ttcn:74 Message with id 44 was extracted from the queue of BSCVTY.
09:00:40.488145 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.488201 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 6_70k forbidden"
09:00:40.488267 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.488521 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 45
09:00:40.488608 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.488691 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.488789 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.488846 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 45
09:00:40.488900 Osmocom_VTY_Functions.ttcn:74 Message with id 45 was extracted from the queue of BSCVTY.
09:00:40.488956 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.489011 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 5_90k allowed"
09:00:40.489075 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.489335 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 46
09:00:40.489420 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.489503 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.489601 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.489660 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 46
09:00:40.489714 Osmocom_VTY_Functions.ttcn:74 Message with id 46 was extracted from the queue of BSCVTY.
09:00:40.489770 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.489825 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 5_15k forbidden"
09:00:40.489890 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.490147 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 47
09:00:40.490282 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.490562 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.490782 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.490873 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 47
09:00:40.491101 Osmocom_VTY_Functions.ttcn:74 Message with id 47 was extracted from the queue of BSCVTY.
09:00:40.491417 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.491596 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 4_75k allowed"
09:00:40.491802 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.492115 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 48
09:00:40.492376 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.492551 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.492765 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.492877 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 48
09:00:40.492968 Osmocom_VTY_Functions.ttcn:74 Message with id 48 was extracted from the queue of BSCVTY.
09:00:40.493057 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.493150 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:00:40.493279 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.493528 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 49
09:00:40.493688 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.493843 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:40.493938 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 49
09:00:40.494023 Osmocom_VTY_Functions.ttcn:73 Message with id 49 was extracted from the queue of BSCVTY.
09:00:40.494110 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.494217 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:40.494380 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.494648 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 50
09:00:40.494809 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.494956 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.495129 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.495224 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 50
09:00:40.495310 Osmocom_VTY_Functions.ttcn:74 Message with id 50 was extracted from the queue of BSCVTY.
09:00:40.495398 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.495491 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
09:00:40.495611 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.495873 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 51
09:00:40.496028 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.496169 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.496336 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.496431 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 51
09:00:40.496516 Osmocom_VTY_Functions.ttcn:74 Message with id 51 was extracted from the queue of BSCVTY.
09:00:40.496605 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.496694 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
09:00:40.496834 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.497085 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 52
09:00:40.497120 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.497151 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.497188 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.497209 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 52
09:00:40.497228 Osmocom_VTY_Functions.ttcn:74 Message with id 52 was extracted from the queue of BSCVTY.
09:00:40.497246 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.497267 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr tch-h start-mode 1"
09:00:40.497293 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.497382 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 53
09:00:40.497416 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.497447 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:40.497484 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:00:40.497504 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 53
09:00:40.497523 Osmocom_VTY_Functions.ttcn:74 Message with id 53 was extracted from the queue of BSCVTY.
09:00:40.497542 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.497561 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:00:40.497587 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:40.497664 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 54
09:00:40.497697 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:40.497729 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:40.497750 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 54
09:00:40.497768 Osmocom_VTY_Functions.ttcn:73 Message with id 54 was extracted from the queue of BSCVTY.
09:00:40.497787 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:40.497806 Osmocom_Types.ttcn:126 Start timer T: 1 s
09:00:41.498087 Osmocom_Types.ttcn:127 Timeout T: 1 s
09:00:41.499030 BSC_Tests.ttcn:4122 Creating new PTC with component type MSC_ConnectionHandler.MSC_ConnHdlr, component name: TC_assignment_codec_amr_h_S024.
09:00:41.507842 BSC_Tests.ttcn:4122 PTC was created. Component reference: 846, alive: no, type: MSC_ConnectionHandler.MSC_ConnHdlr, component name: TC_assignment_codec_amr_h_S024.
09:00:41.508061 BSC_Tests.ttcn:4089 Connecting ports TC_assignment_codec_amr_h_S024(846):RAN and VirtMSC-RAN(838):PROC.
09:00:41.513987 BSC_Tests.ttcn:4089 Connect operation on TC_assignment_codec_amr_h_S024(846):RAN and VirtMSC-RAN(838):PROC finished.
09:00:41.514038 BSC_Tests.ttcn:4090 Connecting ports TC_assignment_codec_amr_h_S024(846):RSL and IPA-BTS0-TRX0-RSL-RSL(845):CLIENT_PT.
09:00:41.514424 BSC_Tests.ttcn:4090 Connect operation on TC_assignment_codec_amr_h_S024(846):RSL and IPA-BTS0-TRX0-RSL-RSL(845):CLIENT_PT finished.
09:00:41.514477 BSC_Tests.ttcn:4091 Connecting ports TC_assignment_codec_amr_h_S024(846):RSL_PROC and IPA-BTS0-TRX0-RSL-RSL(845):RSL_PROC.
09:00:41.515106 BSC_Tests.ttcn:4091 Connect operation on TC_assignment_codec_amr_h_S024(846):RSL_PROC and IPA-BTS0-TRX0-RSL-RSL(845):RSL_PROC finished.
09:00:41.515311 BSC_Tests.ttcn:4100 Connecting ports TC_assignment_codec_amr_h_S024(846):RAN_CONN and VirtMSC-RAN(838):CLIENT.
09:00:41.516349 BSC_Tests.ttcn:4100 Connect operation on TC_assignment_codec_amr_h_S024(846):RAN_CONN and VirtMSC-RAN(838):CLIENT finished.
09:00:41.516544 BSC_Tests.ttcn:4102 Connecting ports TC_assignment_codec_amr_h_S024(846):BSSAP_LE and VirtSMLC-BSSAP_LE(840):CLIENT.
09:00:41.517798 BSC_Tests.ttcn:4102 Connect operation on TC_assignment_codec_amr_h_S024(846):BSSAP_LE and VirtSMLC-BSSAP_LE(840):CLIENT finished.
09:00:41.517992 BSC_Tests.ttcn:4103 Connecting ports TC_assignment_codec_amr_h_S024(846):BSSAP_LE_PROC and VirtSMLC-BSSAP_LE(840):PROC.
09:00:41.518863 BSC_Tests.ttcn:4103 Connect operation on TC_assignment_codec_amr_h_S024(846):BSSAP_LE_PROC and VirtSMLC-BSSAP_LE(840):PROC finished.
09:00:41.519059 BSC_Tests.ttcn:4105 Connecting ports TC_assignment_codec_amr_h_S024(846):STATSD_PROC and VirtMSC-STATS(835):STATSD_PROC.
09:00:41.520093 BSC_Tests.ttcn:4105 Connect operation on TC_assignment_codec_amr_h_S024(846):STATSD_PROC and VirtMSC-STATS(835):STATSD_PROC finished.
09:00:41.520288 BSC_Tests.ttcn:4106 Connecting ports TC_assignment_codec_amr_h_S024(846):MGCP_PROC and VirtMGW-MGCP-0(843):MGCP_PROC.
09:00:41.521151 BSC_Tests.ttcn:4106 Connect operation on TC_assignment_codec_amr_h_S024(846):MGCP_PROC and VirtMGW-MGCP-0(843):MGCP_PROC finished.
09:00:41.521343 BSC_Tests.ttcn:4107 Connecting ports TC_assignment_codec_amr_h_S024(846):MGCP and VirtMGW-MGCP-0(843):MGCP_CLIENT.
09:00:41.522162 BSC_Tests.ttcn:4107 Connect operation on TC_assignment_codec_amr_h_S024(846):MGCP and VirtMGW-MGCP-0(843):MGCP_CLIENT finished.
09:00:41.522412 BSC_Tests.ttcn:4108 Connecting ports TC_assignment_codec_amr_h_S024(846):MGCP_MULTI and VirtMGW-MGCP-0(843):MGCP_CLIENT_MULTI.
09:00:41.523252 BSC_Tests.ttcn:4108 Connect operation on TC_assignment_codec_amr_h_S024(846):MGCP_MULTI and VirtMGW-MGCP-0(843):MGCP_CLIENT_MULTI finished.
09:00:41.523447 BSC_Tests.ttcn:4130 Starting function f_handler_init(refers(BSC_Tests.f_TC_assignment_codec), "TC_assignment_codec_amr_h_S024", { ra := '23'O ("#"), fn := 23, imsi := '001011310642401'H, imei := '00101665255612'H, link_id := { c := FACCH_SDCCH (0), na := false, prio := SAPI0_PRIO_NORMAL (0), sapi := 0 }, media_nr := 1, ass_codec_list := { elementIdentifier := '7D'O ("}"), lengthIndicator := 0, codecElements := { { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00010101'B, s8_15 := '00000111'B } } }, expect_mr_conf_ie := { multirate_cfg := { len := 5, mr_speech_ver := 1, nscb := false, icmi := true, spare := '0'B, start_mode := 0, codec_modes := '00010101'B, parameters := '208820'O } }, expect_mr_s0_s7 := '00010101'B, encr := omit, lcls := { gcr := omit, cfg := omit, csc := omit, exp_sts := omit, adjust_cx_exp := true }, sccp_addr_msc := omit, sccp_addr_bsc := omit, exp_ms_power_level := 7, exp_ms_power_params := false, aoip := true, use_osmux_cn := false, use_osmux_bts := false, host_aoip_tla := "1.2.3.4", mscpool := { bssap_idx := 0, rsl_idx := 0, l3_info := omit }, mgwpool_idx := 0, media_mgw_offer_ipv6 := true, last_used_eutran_plmn := omit, exp_fast_return := false, expect_channel_mode_modify := false, expect_tsc := 2, cell_id_source := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0001'O } } }, expect_ho_fail := false, expect_ho_fail_lchan_est := false, inter_bsc_ho_in__ho_req_in_initial_sccp_cr := true, ignore_mgw_mdcx := false, fail_on_dlcx := true, ignore_ipa_media := false, asci_test := { vgcs_setup_ok := false, vgcs_assign_ok := false, vgcs_assign_fail := false, vgcs_talker_req := false, vgcs_talker_fail := false, vgcs_talker_est := false, vgcs_talker_rel := false, vgcs_uplink_reject := false, vgcs_uplink_seized := false, vgcs_uplink_release := false, delay_bts := false, delay_msc := false } }) on component TC_assignment_codec_amr_h_S024(846).
09:00:41.523887 BSC_Tests.ttcn:4130 Function was started.
09:00:45.853615 BSC_Tests.ttcn:4914 PTC with component reference 846 is done.
09:00:45.854223 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:45.854514 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.854877 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 55
09:00:45.855038 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.855155 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.855283 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.855348 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 55
09:00:45.855411 Osmocom_VTY_Functions.ttcn:74 Message with id 55 was extracted from the queue of BSCVTY.
09:00:45.855474 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.855538 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
09:00:45.855621 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.855893 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 56
09:00:45.855989 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.856079 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.856189 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.856250 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 56
09:00:45.856306 Osmocom_VTY_Functions.ttcn:74 Message with id 56 was extracted from the queue of BSCVTY.
09:00:45.856364 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.856422 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 12_2k forbidden"
09:00:45.856495 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.856767 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 57
09:00:45.856860 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.856945 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.857048 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.857115 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 57
09:00:45.857172 Osmocom_VTY_Functions.ttcn:74 Message with id 57 was extracted from the queue of BSCVTY.
09:00:45.857229 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.857285 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 10_2k forbidden"
09:00:45.857352 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.857519 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 58
09:00:45.857535 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.857561 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.857579 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.857590 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 58
09:00:45.857600 Osmocom_VTY_Functions.ttcn:74 Message with id 58 was extracted from the queue of BSCVTY.
09:00:45.857610 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.857620 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 7_95k forbidden"
09:00:45.857633 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.857651 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 59
09:00:45.857666 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.857682 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.857700 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.857711 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 59
09:00:45.857721 Osmocom_VTY_Functions.ttcn:74 Message with id 59 was extracted from the queue of BSCVTY.
09:00:45.857731 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.857741 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 7_40k forbidden"
09:00:45.857753 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.857770 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 60
09:00:45.857785 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.857800 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.857819 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.857830 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 60
09:00:45.857839 Osmocom_VTY_Functions.ttcn:74 Message with id 60 was extracted from the queue of BSCVTY.
09:00:45.857850 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.857860 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 6_70k forbidden"
09:00:45.857872 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.857889 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 61
09:00:45.857904 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.857919 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.857937 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.857948 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 61
09:00:45.857960 Osmocom_VTY_Functions.ttcn:74 Message with id 61 was extracted from the queue of BSCVTY.
09:00:45.857971 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.857981 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 5_90k allowed"
09:00:45.857993 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858010 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 62
09:00:45.858025 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.858042 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.858060 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.858071 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 62
09:00:45.858081 Osmocom_VTY_Functions.ttcn:74 Message with id 62 was extracted from the queue of BSCVTY.
09:00:45.858091 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.858101 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 5_15k forbidden"
09:00:45.858114 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858130 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 63
09:00:45.858146 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.858161 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.858179 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.858190 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 63
09:00:45.858199 Osmocom_VTY_Functions.ttcn:74 Message with id 63 was extracted from the queue of BSCVTY.
09:00:45.858220 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.858232 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr-config 4_75k forbidden"
09:00:45.858247 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858266 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 64
09:00:45.858284 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.858305 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.858328 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.858340 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 64
09:00:45.858352 Osmocom_VTY_Functions.ttcn:74 Message with id 64 was extracted from the queue of BSCVTY.
09:00:45.858364 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.858376 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:00:45.858390 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858406 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 65
09:00:45.858423 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.858442 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:45.858456 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 65
09:00:45.858468 Osmocom_VTY_Functions.ttcn:73 Message with id 65 was extracted from the queue of BSCVTY.
09:00:45.858480 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.858495 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:00:45.858510 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858529 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 66
09:00:45.858547 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.858565 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.858585 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.858598 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 66
09:00:45.858610 Osmocom_VTY_Functions.ttcn:74 Message with id 66 was extracted from the queue of BSCVTY.
09:00:45.858622 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.858634 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
09:00:45.858648 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858667 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 67
09:00:45.858685 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.858701 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.858722 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.858735 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 67
09:00:45.858746 Osmocom_VTY_Functions.ttcn:74 Message with id 67 was extracted from the queue of BSCVTY.
09:00:45.858758 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.858770 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
09:00:45.858784 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858808 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 68
09:00:45.858826 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.858843 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.858864 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.858877 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 68
09:00:45.858889 Osmocom_VTY_Functions.ttcn:74 Message with id 68 was extracted from the queue of BSCVTY.
09:00:45.858901 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.858914 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "amr tch-h start-mode auto"
09:00:45.858928 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.858971 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 69
09:00:45.858991 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.859009 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.859029 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:00:45.859043 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 69
09:00:45.859056 Osmocom_VTY_Functions.ttcn:74 Message with id 69 was extracted from the queue of BSCVTY.
09:00:45.859068 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.859080 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:00:45.859094 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.859110 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 70
09:00:45.859128 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.859147 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:45.859160 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 70
09:00:45.859172 Osmocom_VTY_Functions.ttcn:73 Message with id 70 was extracted from the queue of BSCVTY.
09:00:45.859184 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.859212 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
09:00:45.859226 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:00:45.859435 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" id 71
09:00:45.859448 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 72
09:00:45.859466 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.859484 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:00:45.859501 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
09:00:45.859516 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
09:00:45.859530 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" with ? matched
09:00:45.859543 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1454287 bytes in 1328 blocks)" id 71
09:00:45.859554 Osmocom_VTY_Functions.ttcn:85 Message with id 71 was extracted from the queue of BSCVTY.
09:00:45.859571 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:00:45.859588 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:00:45.859599 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 72
09:00:45.859613 Osmocom_VTY_Functions.ttcn:73 Message with id 72 was extracted from the queue of BSCVTY.
09:00:45.859624 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:00:45.859637 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
09:00:45.859654 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
09:00:45.859670 BSC_Tests.ttcn:888 Stopping all components.
09:00:45.860762 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(842):IPA_CTRL_PORT was closed unexpectedly by the peer.
09:00:45.860778 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(842):IPA_CTRL_PORT.
09:00:45.860806 BSC_Tests.ttcn:888 All components were stopped.
09:00:45.860838 BSC_Tests.ttcn:889 setverdict(pass): none -> pass
09:00:45.860852 BSC_Tests.ttcn:890 Stopping test component execution.
09:00:45.860893 BSC_Tests.ttcn:5028 Test case TC_assignment_codec_amr_h_S024 was stopped.
09:00:45.860906 BSC_Tests.ttcn:5028 Terminating component type BSC_Tests.test_CT.
09:00:45.860916 BSC_Tests.ttcn:5028 Default with id 1 (altstep as_Tguard) was deactivated.
09:00:45.860926 BSC_Tests.ttcn:5028 Stop timer T_guard: 30 s
09:00:45.860937 BSC_Tests.ttcn:5028 Port IPA_CTRL was stopped.
09:00:45.860947 BSC_Tests.ttcn:5028 Removing unterminated connection between port RSL_CCHAN[0] and IPA-BTS0-TRX0-RSL-RSL(845):CCHAN_PT.
09:00:45.860968 BSC_Tests.ttcn:5028 Message with id 1 was extracted from the queue of RSL_CCHAN[0].
09:00:45.860987 BSC_Tests.ttcn:5028 Message with id 2 was extracted from the queue of RSL_CCHAN[0].
09:00:45.860997 BSC_Tests.ttcn:5028 Message with id 3 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861007 BSC_Tests.ttcn:5028 Message with id 4 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861016 BSC_Tests.ttcn:5028 Message with id 5 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861025 BSC_Tests.ttcn:5028 Message with id 6 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861034 BSC_Tests.ttcn:5028 Message with id 7 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861043 BSC_Tests.ttcn:5028 Message with id 8 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861052 BSC_Tests.ttcn:5028 Message with id 9 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861061 BSC_Tests.ttcn:5028 Message with id 10 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861070 BSC_Tests.ttcn:5028 Message with id 11 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861079 BSC_Tests.ttcn:5028 Message with id 12 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861089 BSC_Tests.ttcn:5028 Message with id 13 was extracted from the queue of RSL_CCHAN[0].
09:00:45.861097 BSC_Tests.ttcn:5028 Port RSL_CCHAN[0] was stopped.
09:00:45.861106 BSC_Tests.ttcn:5028 Port RSL_CCHAN[1] was stopped.
09:00:45.861114 BSC_Tests.ttcn:5028 Port RSL_CCHAN[2] was stopped.
09:00:45.861122 BSC_Tests.ttcn:5028 Port IPA_RSL[0][0] was stopped.
09:00:45.861131 BSC_Tests.ttcn:5028 Port IPA_RSL[0][1] was stopped.
09:00:45.861139 BSC_Tests.ttcn:5028 Port IPA_RSL[0][2] was stopped.
09:00:45.861148 BSC_Tests.ttcn:5028 Port IPA_RSL[0][3] was stopped.
09:00:45.861157 BSC_Tests.ttcn:5028 Port IPA_RSL[1][0] was stopped.
09:00:45.861165 BSC_Tests.ttcn:5028 Port IPA_RSL[1][1] was stopped.
09:00:45.861174 BSC_Tests.ttcn:5028 Port IPA_RSL[1][2] was stopped.
09:00:45.861182 BSC_Tests.ttcn:5028 Port IPA_RSL[1][3] was stopped.
09:00:45.861190 BSC_Tests.ttcn:5028 Port IPA_RSL[2][0] was stopped.
09:00:45.861199 BSC_Tests.ttcn:5028 Port IPA_RSL[2][1] was stopped.
09:00:45.861207 BSC_Tests.ttcn:5028 Port IPA_RSL[2][2] was stopped.
09:00:45.861216 BSC_Tests.ttcn:5028 Port IPA_RSL[2][3] was stopped.
09:00:45.861225 BSC_Tests.ttcn:5028 Port IPA was stopped.
09:00:45.861233 BSC_Tests.ttcn:5028 Removing unterminated connection between port SCCPLITE_IPA_CTRL and VirtMSC-RAN(838):CTRL_CLIENT.
09:00:45.861277 BSC_Tests.ttcn:5028 Port SCCPLITE_IPA_CTRL was stopped.
09:00:45.861324 BSC_Tests.ttcn:5028 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(844):CFG_PORT.
09:00:45.861369 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[0][0] was stopped.
09:00:45.861405 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[0][1] was stopped.
09:00:45.861434 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[0][2] was stopped.
09:00:45.861462 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[0][3] was stopped.
09:00:45.861495 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[1][0] was stopped.
09:00:45.861519 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[1][1] was stopped.
09:00:45.861546 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[1][2] was stopped.
09:00:45.861572 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[1][3] was stopped.
09:00:45.861597 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[2][0] was stopped.
09:00:45.861622 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[2][1] was stopped.
09:00:45.861648 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[2][2] was stopped.
09:00:45.861673 BSC_Tests.ttcn:5028 Port IPA_CFG_PORT[2][3] was stopped.
09:00:45.861698 BSC_Tests.ttcn:5028 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
09:00:45.861760 BSC_Tests.ttcn:5028 Port BSCVTY was unmapped from system:BSCVTY.
09:00:45.861793 BSC_Tests.ttcn:5028 Port BSCVTY was stopped.
09:00:45.861820 BSC_Tests.ttcn:5028 Port STPVTY was stopped.
09:00:45.861845 BSC_Tests.ttcn:5028 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
09:00:45.861870 BSC_Tests.ttcn:5028 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
09:00:45.861895 BSC_Tests.ttcn:5028 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
09:00:45.861921 BSC_Tests.ttcn:5028 Port BSSAP was stopped.
09:00:45.861947 BSC_Tests.ttcn:5028 Port BSSAP_LE was stopped.
09:00:45.861973 BSC_Tests.ttcn:5028 Component type BSC_Tests.test_CT was shut down inside testcase TC_assignment_codec_amr_h_S024.
09:00:45.862001 BSC_Tests.ttcn:5028 Waiting for PTCs to finish.
09:00:45.867772 BSC_Tests.ttcn:5028 Setting final verdict of the test case.
09:00:45.868069 BSC_Tests.ttcn:5028 Local verdict of MTC: pass
09:00:45.868292 BSC_Tests.ttcn:5028 Local verdict of PTC VirtMSC-STATS(835): none (pass -> pass)
09:00:45.868410 BSC_Tests.ttcn:5028 Local verdict of PTC VirtMSC-SCCP(836): none (pass -> pass)
09:00:45.868562 BSC_Tests.ttcn:5028 Local verdict of PTC VirtMSC-M3UA(837): none (pass -> pass)
09:00:45.868798 BSC_Tests.ttcn:5028 Local verdict of PTC VirtMSC-RAN(838): none (pass -> pass)
09:00:45.868990 BSC_Tests.ttcn:5028 Local verdict of PTC VirtSMLC-SCCP(839): none (pass -> pass)
09:00:45.869190 BSC_Tests.ttcn:5028 Local verdict of PTC VirtSMLC-BSSAP_LE(840): none (pass -> pass)
09:00:45.869350 BSC_Tests.ttcn:5028 Local verdict of PTC VirtSMLC-M3UA(841): none (pass -> pass)
09:00:45.869699 BSC_Tests.ttcn:5028 Local verdict of PTC IPA-CTRL-CLI-IPA(842): none (pass -> pass)
09:00:45.870140 BSC_Tests.ttcn:5028 Local verdict of PTC VirtMGW-MGCP-0(843): none (pass -> pass)
09:00:45.870177 BSC_Tests.ttcn:5028 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(844): none (pass -> pass)
09:00:45.870226 BSC_Tests.ttcn:5028 Local verdict of PTC IPA-BTS0-TRX0-RSL-RSL(845): none (pass -> pass)
09:00:45.870256 BSC_Tests.ttcn:5028 Local verdict of PTC TC_assignment_codec_amr_h_S024(846): pass (pass -> pass)
09:00:45.870311 BSC_Tests.ttcn:5028 Test case TC_assignment_codec_amr_h_S024 finished. Verdict: pass
09:00:45.870356 BSC_Tests.ttcn:5028 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_assignment_codec_amr_h_S024 pass'.
09:00:51.081516 BSC_Tests.ttcn:5028 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_assignment_codec_amr_h_S024 pass' was executed successfully (exit status: 0).
09:00:51.081660 BSC_Tests.ttcn:5037 Switching to log file `BSC_Tests-TC_assignment_codec_amr_h_S0247-d5b21e48044a-mtc-9786.log'
