09:15:35.524151 BSC_Tests.ttcn:3694 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_paging_imsi_nochan_cgi_unknown_cid'.
09:15:36.537677 BSC_Tests.ttcn:3694 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-start.sh BSC_Tests.TC_paging_imsi_nochan_cgi_unknown_cid' was executed successfully (exit status: 0).
09:15:36.537945 BSC_Tests.ttcn:3694 Test case TC_paging_imsi_nochan_cgi_unknown_cid started.
09:15:36.538020 BSC_Tests.ttcn:3694 Initializing variables, timers and ports of component type BSC_Tests.test_CT inside testcase TC_paging_imsi_nochan_cgi_unknown_cid.
09:15:36.538247 BSC_Tests.ttcn:3694 Port IPA_CTRL was started.
09:15:36.538405 BSC_Tests.ttcn:3694 Port RSL_CCHAN[0] was started.
09:15:36.538481 BSC_Tests.ttcn:3694 Port RSL_CCHAN[1] was started.
09:15:36.538661 BSC_Tests.ttcn:3694 Port RSL_CCHAN[2] was started.
09:15:36.538738 BSC_Tests.ttcn:3694 Port IPA_RSL[0][0] was started.
09:15:36.538922 BSC_Tests.ttcn:3694 Port IPA_RSL[0][1] was started.
09:15:36.538998 BSC_Tests.ttcn:3694 Port IPA_RSL[0][2] was started.
09:15:36.539160 BSC_Tests.ttcn:3694 Port IPA_RSL[0][3] was started.
09:15:36.539211 BSC_Tests.ttcn:3694 Port IPA_RSL[1][0] was started.
09:15:36.539257 BSC_Tests.ttcn:3694 Port IPA_RSL[1][1] was started.
09:15:36.539303 BSC_Tests.ttcn:3694 Port IPA_RSL[1][2] was started.
09:15:36.539350 BSC_Tests.ttcn:3694 Port IPA_RSL[1][3] was started.
09:15:36.539396 BSC_Tests.ttcn:3694 Port IPA_RSL[2][0] was started.
09:15:36.539442 BSC_Tests.ttcn:3694 Port IPA_RSL[2][1] was started.
09:15:36.539487 BSC_Tests.ttcn:3694 Port IPA_RSL[2][2] was started.
09:15:36.539534 BSC_Tests.ttcn:3694 Port IPA_RSL[2][3] was started.
09:15:36.539580 BSC_Tests.ttcn:3694 Port IPA was started.
09:15:36.539627 BSC_Tests.ttcn:3694 Port SCCPLITE_IPA_CTRL was started.
09:15:36.539674 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[0][0] was started.
09:15:36.539722 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[0][1] was started.
09:15:36.539767 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[0][2] was started.
09:15:36.539814 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[0][3] was started.
09:15:36.539859 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[1][0] was started.
09:15:36.539905 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[1][1] was started.
09:15:36.539950 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[1][2] was started.
09:15:36.539996 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[1][3] was started.
09:15:36.540041 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[2][0] was started.
09:15:36.540087 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[2][1] was started.
09:15:36.540132 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[2][2] was started.
09:15:36.540178 BSC_Tests.ttcn:3694 Port IPA_CFG_PORT[2][3] was started.
09:15:36.540224 BSC_Tests.ttcn:3694 Port BSCVTY was started.
09:15:36.540270 BSC_Tests.ttcn:3694 Port STPVTY was started.
09:15:36.540316 BSC_Tests.ttcn:3694 Port SCCPLITE_IPA_CFG_PORT[0] was started.
09:15:36.540361 BSC_Tests.ttcn:3694 Port SCCPLITE_IPA_CFG_PORT[1] was started.
09:15:36.540406 BSC_Tests.ttcn:3694 Port SCCPLITE_IPA_CFG_PORT[2] was started.
09:15:36.540452 BSC_Tests.ttcn:3694 Port BSSAP was started.
09:15:36.540498 BSC_Tests.ttcn:3694 Port BSSAP_LE was started.
09:15:36.540543 BSC_Tests.ttcn:3694 Component type BSC_Tests.test_CT was initialized.
09:15:36.540653 BSC_Tests.ttcn:1265 Start timer T_guard: 30 s
09:15:36.540718 BSC_Tests.ttcn:1266 Altstep as_Tguard was activated as default, id 1
09:15:36.540780 BSC_Tests.ttcn:1097 Mapping port mtc:BSCVTY to system:BSCVTY.
09:15:36.541346 BSC_Tests.ttcn:1097 Message enqueued on BSCVTY from system integer : 2 id 1
09:15:36.541423 BSC_Tests.ttcn:1097 Port BSCVTY was mapped to system:BSCVTY.
09:15:36.541525 BSC_Tests.ttcn:1097 Map operation of mtc:BSCVTY to system:BSCVTY finished.
09:15:36.541601 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 1, prompt := "OsmoBSC> ", has_wildcards := false } }
09:15:36.541665 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 2, prompt := "OsmoBSC# ", has_wildcards := false } }
09:15:36.541745 Osmocom_VTY_Functions.ttcn:59 Sent on BSCVTY to system @TELNETasp_PortType.ASP_TelnetDynamicConfig : { prompt := { id := 3, prompt := "OsmoBSC(*)", has_wildcards := true } }
09:15:36.541881 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "enable"
09:15:36.541973 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.542037 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:15:36.542090 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:15:36.542141 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:15:36.542190 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:15:36.542239 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY failed: Type of the first message in the queue is not charstring.
09:15:36.542294 Osmocom_VTY_Functions.ttcn:86 Matching on port BSCVTY succeeded: 2 with ? matched
09:15:36.542489 Osmocom_VTY_Functions.ttcn:86 Receive operation on port BSCVTY succeeded, message from system(): integer : 2 id 1
09:15:36.542571 Osmocom_VTY_Functions.ttcn:86 Message with id 1 was extracted from the queue of BSCVTY.
09:15:36.542772 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 2
09:15:36.542927 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.543049 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.543112 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 2
09:15:36.543174 Osmocom_VTY_Functions.ttcn:73 Message with id 2 was extracted from the queue of BSCVTY.
09:15:36.543232 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.543304 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:36.543411 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.543612 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 3
09:15:36.543718 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.543814 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.543937 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.544000 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 3
09:15:36.544059 Osmocom_VTY_Functions.ttcn:74 Message with id 3 was extracted from the queue of BSCVTY.
09:15:36.544118 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.544178 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "cs7 instance 0"
09:15:36.544254 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.544363 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 4
09:15:36.544456 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.544543 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.544653 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.544739 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 4
09:15:36.544795 Osmocom_VTY_Functions.ttcn:74 Message with id 4 was extracted from the queue of BSCVTY.
09:15:36.544853 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.544912 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer ias 420"
09:15:36.544982 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.545082 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 5
09:15:36.545171 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.545256 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.545359 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.545417 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 5
09:15:36.545472 Osmocom_VTY_Functions.ttcn:74 Message with id 5 was extracted from the queue of BSCVTY.
09:15:36.545528 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.545585 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "sccp-timer iar 900"
09:15:36.545651 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.545745 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-cs7)# " id 6
09:15:36.545831 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.545914 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-cs7)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.546014 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-cs7)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.546073 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-cs7)# " id 6
09:15:36.546127 Osmocom_VTY_Functions.ttcn:74 Message with id 6 was extracted from the queue of BSCVTY.
09:15:36.546184 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.546236 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:15:36.546374 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.546498 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 7
09:15:36.546588 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.546677 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.546735 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 7
09:15:36.546790 Osmocom_VTY_Functions.ttcn:73 Message with id 7 was extracted from the queue of BSCVTY.
09:15:36.546845 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.546904 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:36.546973 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.547117 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 8
09:15:36.547205 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.547289 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.547403 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.547462 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 8
09:15:36.547517 Osmocom_VTY_Functions.ttcn:74 Message with id 8 was extracted from the queue of BSCVTY.
09:15:36.547575 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.547630 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
09:15:36.547697 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.547794 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 9
09:15:36.547878 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.547962 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.548060 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.548118 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 9
09:15:36.548172 Osmocom_VTY_Functions.ttcn:74 Message with id 9 was extracted from the queue of BSCVTY.
09:15:36.548229 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.548284 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
09:15:36.548350 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.548442 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 10
09:15:36.548526 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.548608 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.548704 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.548760 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 10
09:15:36.548815 Osmocom_VTY_Functions.ttcn:74 Message with id 10 was extracted from the queue of BSCVTY.
09:15:36.548871 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.548923 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.548989 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.549076 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 11
09:15:36.549159 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.549240 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.549336 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.549392 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 11
09:15:36.549444 Osmocom_VTY_Functions.ttcn:74 Message with id 11 was extracted from the queue of BSCVTY.
09:15:36.549499 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.549551 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.549614 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.549688 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 12
09:15:36.549781 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.549866 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.549922 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 12
09:15:36.549976 Osmocom_VTY_Functions.ttcn:73 Message with id 12 was extracted from the queue of BSCVTY.
09:15:36.550031 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.550089 StatsD_Checker.ttcnpp:416 Creating new PTC with component type StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
09:15:36.563905 StatsD_Checker.ttcnpp:416 PTC was created. Component reference: 1476, alive: no, type: StatsD_Checker.StatsD_Checker_CT, component name: VirtMSC-STATS.
09:15:36.563980 StatsD_Checker.ttcnpp:417 Starting function main("127.0.0.1", 8125, 5.000000) on component VirtMSC-STATS(1476).
09:15:36.564102 StatsD_Checker.ttcnpp:417 Function was started.
09:15:36.564167 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0 bssmap reset"
09:15:36.564249 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.564435 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 13
09:15:36.564539 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.564633 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.564689 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 13
09:15:36.564744 Osmocom_VTY_Functions.ttcn:73 Message with id 13 was extracted from the queue of BSCVTY.
09:15:36.564800 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.564856 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1 bssmap reset"
09:15:36.564925 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.565035 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 14
09:15:36.565122 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.565206 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.565260 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 14
09:15:36.565313 Osmocom_VTY_Functions.ttcn:73 Message with id 14 was extracted from the queue of BSCVTY.
09:15:36.565367 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.565421 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2 bssmap reset"
09:15:36.565485 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.565999 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 15
09:15:36.566332 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.566477 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.566548 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 15
09:15:36.566619 Osmocom_VTY_Functions.ttcn:73 Message with id 15 was extracted from the queue of BSCVTY.
09:15:36.566688 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.566844 SCCP_Adapter.ttcnpp:114 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
09:15:36.570413 SCCP_Adapter.ttcnpp:114 PTC was created. Component reference: 1477, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtMSC-SCCP.
09:15:36.570437 SCCP_Adapter.ttcnpp:123 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
09:15:36.573995 SCCP_Adapter.ttcnpp:123 PTC was created. Component reference: 1478, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtMSC-M3UA.
09:15:36.574015 SCCP_Adapter.ttcnpp:124 Mapping port VirtMSC-M3UA(1478):SCTP_PORT to system:sctp.
09:15:36.575537 SCCP_Adapter.ttcnpp:124 Map operation of VirtMSC-M3UA(1478):SCTP_PORT to system:sctp finished.
09:15:36.575560 SCCP_Adapter.ttcnpp:126 Connecting ports VirtMSC-M3UA(1478):MTP3_SP_PORT and VirtMSC-SCCP(1477):MTP3_SCCP_PORT.
09:15:36.575875 SCCP_Adapter.ttcnpp:126 Connect operation on VirtMSC-M3UA(1478):MTP3_SP_PORT and VirtMSC-SCCP(1477):MTP3_SCCP_PORT finished.
09:15:36.575896 SCCP_Adapter.ttcnpp:127 Starting function f_M3UA_Emulation({ local_sctp_port := 23905, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 1) on component VirtMSC-M3UA(1478).
09:15:36.575937 SCCP_Adapter.ttcnpp:127 Function was started.
09:15:36.575958 BSC_Tests.ttcn:1223 Connecting ports mtc:BSSAP and VirtMSC-SCCP(1477):SCCP_SP_PORT.
09:15:36.576120 BSC_Tests.ttcn:1223 Port BSSAP is waiting for connection from VirtMSC-SCCP(1477):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-487ab81d.
09:15:36.576192 BSC_Tests.ttcn:1223 Port BSSAP has accepted the connection from VirtMSC-SCCP(1477):SCCP_SP_PORT.
09:15:36.576218 BSC_Tests.ttcn:1223 Connect operation on mtc:BSSAP and VirtMSC-SCCP(1477):SCCP_SP_PORT finished.
09:15:36.576239 SCCP_Adapter.ttcnpp:165 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 185, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 254 }) on component VirtMSC-SCCP(1477).
09:15:36.576286 SCCP_Adapter.ttcnpp:165 Function was started.
09:15:36.576400 BSC_Tests.ttcn:897 Sent on BSSAP to VirtMSC-SCCP(1477) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit }
09:15:36.576427 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
09:15:36.576555 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
09:15:36.576669 BSC_Tests.ttcn:897 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := '000430040100'O, importance := omit }
09:15:36.576779 BSC_Tests.ttcn:899 Start timer T: 5 s
09:15:36.785685 BSC_Tests.ttcn:900 Message enqueued on BSSAP from VirtMSC-SCCP(1477) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := '000131'O, importance := omit } id 1
09:15:36.786188 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
09:15:36.786974 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
09:15:36.787398 BSC_Tests.ttcn:900 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
09:15:36.787863 BSC_Tests.ttcn:901 Matching on port BSSAP succeeded:  matched
09:15:36.788099 BSC_Tests.ttcn:901 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(1477): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
09:15:36.788278 BSC_Tests.ttcn:901 Message with id 1 was extracted from the queue of BSSAP.
09:15:36.788462 BSC_Tests.ttcn:903 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
09:15:36.788605 BSSAP_LE_Adapter.ttcn:95 Creating new alive PTC with component type SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
09:15:36.795890 BSSAP_LE_Adapter.ttcn:95 PTC was created. Component reference: 1479, alive: yes, type: SCCP_Emulation.SCCP_CT, component name: VirtSMLC-SCCP.
09:15:36.795922 BSSAP_LE_Adapter.ttcn:101 Creating new alive PTC with component type M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
09:15:36.803584 BSSAP_LE_Adapter.ttcn:101 PTC was created. Component reference: 1480, alive: yes, type: M3UA_Emulation.M3UA_CT, component name: VirtSMLC-M3UA.
09:15:36.803602 BSSAP_LE_Adapter.ttcn:102 Mapping port VirtSMLC-M3UA(1480):SCTP_PORT to system:sctp.
09:15:36.806227 BSSAP_LE_Adapter.ttcn:102 Map operation of VirtSMLC-M3UA(1480):SCTP_PORT to system:sctp finished.
09:15:36.806265 BSSAP_LE_Adapter.ttcn:104 Connecting ports VirtSMLC-M3UA(1480):MTP3_SP_PORT and VirtSMLC-SCCP(1479):MTP3_SCCP_PORT.
09:15:36.807103 BSSAP_LE_Adapter.ttcn:104 Connect operation on VirtSMLC-M3UA(1480):MTP3_SP_PORT and VirtSMLC-SCCP(1479):MTP3_SCCP_PORT finished.
09:15:36.807141 BSSAP_LE_Adapter.ttcn:105 Starting function f_M3UA_Emulation({ local_sctp_port := 23908, local_ip_addr := "127.0.0.1", remote_sctp_port := 2905, remote_ip_addr := "127.0.0.1" }, 6) on component VirtSMLC-M3UA(1480).
09:15:36.807288 BSSAP_LE_Adapter.ttcn:105 Function was started.
09:15:36.807328 BSC_Tests.ttcn:1290 Connecting ports mtc:BSSAP_LE and VirtSMLC-SCCP(1479):SCCP_SP_PORT.
09:15:36.807732 BSC_Tests.ttcn:1290 Port BSSAP_LE is waiting for connection from VirtSMLC-SCCP(1479):SCCP_SP_PORT on UNIX pathname /tmp/ttcn3-portconn-f36e71d.
09:15:36.807975 BSC_Tests.ttcn:1290 Port BSSAP_LE has accepted the connection from VirtSMLC-SCCP(1479):SCCP_SP_PORT.
09:15:36.808072 BSC_Tests.ttcn:1290 Connect operation on mtc:BSSAP_LE and VirtSMLC-SCCP(1479):SCCP_SP_PORT finished.
09:15:36.808112 BSSAP_LE_Adapter.ttcn:122 Starting function SCCPStart({ sio := { ni := '00'B, prio := '00'B, si := '0011'B }, opc := 190, dpc := 187, sls := 0, sccp_serviceType := "mtp3_itu", ssn := 252 }) on component VirtSMLC-SCCP(1479).
09:15:36.808318 BSSAP_LE_Adapter.ttcn:122 Function was started.
09:15:36.808381 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show running-config"
09:15:36.808477 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.815190 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
09:15:36.815472 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 17
09:15:36.821232 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.825494 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.828305 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
09:15:36.830632 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
09:15:36.832185 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" with ? matched
09:15:36.833494 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "\nCurrent configuration:\n!\npassword foo\n!\nlog stderr\n logging filter all 1\n logging color 1\n logging print category-hex 0\n logging print category 1\n logging print thread-id 0\n logging print extended-timestamp 1\n logging print level 1\n logging print file basename last\n logging level rll notice\n logging level mm notice\n logging level rr notice\n logging level rsl notice\n logging level nm notice\n logging level pag notice\n logging level meas notice\n logging level msc notice\n logging level ho notice\n logging level hodec notice\n logging level ref notice\n logging level ctrl notice\n logging level filter debug\n logging level pcu debug\n logging level lcls notice\n logging level chan notice\n logging level ts notice\n logging level as notice\n logging level cbs notice\n logging level lcs notice\n logging level asci notice\n logging level reset notice\n logging level loop notice\n logging level lglobal notice\n logging level llapd notice\n logging level linp notice\n logging level lmux notice\n logging level lmi notice\n logging level lmib notice\n logging level lsms notice\n logging level lctrl notice\n logging level lgtp notice\n logging level lstats notice\n logging level lgsup notice\n logging level loap notice\n logging level lss7 notice\n logging level lsccp notice\n logging level lsua notice\n logging level lm3ua notice\n logging level lmgcp notice\n logging level ljibuf notice\n logging level lrspro notice\n logging level lns notice\n logging level lbssgp notice\n logging level lnsdata notice\n logging level lnssignal notice\n logging level liuup notice\n logging level lpfcp notice\n logging level lcsn1 notice\n logging level lio notice\n logging level ltcap notice\nlog gsmtap 127.0.0.1\n logging filter all 1\n logging color 1\n logging print category-hex 1\n logging print category 0\n logging print thread-id 0\n logging timestamp 0\n logging print file 1\n logging level rll debug\n logging level mm debug\n logging level rr debug\n logging level rsl debug\n logging level nm debug\n logging level pag debug\n logging level meas debug\n logging level msc debug\n logging level ho debug\n logging level hodec debug\n logging level ref debug\n logging level ctrl debug\n logging level filter debug\n logging level pcu debug\n logging level lcls debug\n logging level chan debug\n logging level ts debug\n logging level as debug\n logging level cbs debug\n logging level lcs debug\n logging level asci debug\n logging level reset debug\n logging level loop debug\n logging level lglobal debug\n logging level llapd debug\n logging level linp debug\n logging level lmux debug\n logging level lmi debug\n logging level lmib debug\n logging level lsms debug\n logging level lctrl debug\n logging level lgtp debug\n logging level lstats debug\n logging level lgsup debug\n logging level loap debug\n logging level lss7 debug\n logging level lsccp debug\n logging level lsua debug\n logging level lm3ua debug\n logging level lmgcp debug\n logging level ljibuf debug\n logging level lrspro debug\n logging level lns debug\n logging level lbssgp debug\n logging level lnsdata debug\n logging level lnssignal debug\n logging level liuup debug\n logging level lpfcp debug\n logging level lcsn1 debug\n logging level lio debug\n logging level ltcap debug\n!\nstats interval 0\nstats reporter statsd\n  remote-ip 127.0.0.1\n  remote-port 8125\n  mtu 1024\n  level subscriber\n  prefix TTCN3\n  flush-period 1\n  enable\n!\nline vty\n no login\n!\ne1_input\n e1_line 0 driver ipa\n e1_line 0 port 0\n no e1_line 0 keepalive\n ipa bind 127.0.0.1\nctrl\n bind 127.0.0.1\ncs7 instance 0\n network-indicator international\n point-code 0.23.3\n asp asp-clnt-msc-0 2905 1905 m3ua\n  local-ip 0.0.0.0\n  remote-ip 127.0.0.1\n  role asp\n  sctp-role client\n  no shutdown\n sccp-address msc0\n  routing-indicator PC\n  point-code 0.23.1\n  subsystem-number 254\n sccp-address msc1\n  routing-indicator PC\n  point-code 0.0.2\n  subsystem-number 254\n sccp-address msc2\n  routing-indicator PC\n  point-code 0.0.3\n  subsystem-number 254\nnetwork\n network country code 001\n mobile network code 01\n encryption a5 0 1 3\n neci 1\n paging any use tch 0\n handover 1\n handover1 window rxlev averaging 10\n handover1 window rxqual averaging 1\n handover1 window rxlev neighbor averaging 10\n handover1 power budget interval 6\n handover1 power budget hysteresis 3\n handover1 maximum distance 9999\n timer net T3113 10\n timer net T3212 30\n nri null add 0 1\n mgw 0\n  remote-ip 127.0.0.1\n bts 0\n  type osmo-bts\n  band DCS1800\n  cell_identity 0\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 10\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  access-control-class-rotate-quantum 1\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1234 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 4 7\n  amr tch-f threshold ms 32 32 32\n  amr tch-f hysteresis ms 8 8 8\n  amr tch-f threshold bts 32 32 32\n  amr tch-f hysteresis bts 8 8 8\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 4\n  amr tch-h threshold ms 32 32\n  amr tch-h hysteresis ms 8 8\n  amr tch-h threshold bts 32 32\n  amr tch-h hysteresis bts 8 8\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1234\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1234\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1234\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 1\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0001\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 11\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1235 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1235\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1235\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1235\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 2\n  type osmo-bts\n  band DCS1800\n  cell_identity 1\n  location_area_code 0x0002\n  dtx uplink force\n  dtx downlink\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 1236 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode manual-si5\n  neighbor-list add arfcn 100\n  neighbor-list add arfcn 200\n  si5 neighbor-list add arfcn 10\n  si5 neighbor-list add arfcn 20\n  si2quater neighbor-list add earfcn 111 thresh-hi 20 thresh-lo 10 prio 3 qrxlv 22 meas 3\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode gprs\n  gprs routing area 0\n  gprs network-control-order nc0\n  gprs power-control alpha 0\n  gprs cell bvci 1236\n  gprs cell timer blocking-timer 3\n  gprs cell timer blocking-retries 3\n  gprs cell timer unblocking-retries 3\n  gprs cell timer reset-timer 3\n  gprs cell timer reset-retries 3\n  gprs cell timer suspend-timer 10\n  gprs cell timer suspend-retries 3\n  gprs cell timer resume-timer 10\n  gprs cell timer resume-retries 3\n  gprs cell timer capability-update-timer 10\n  gprs cell timer capability-update-retries 3\n  gprs nsei 1236\n  gprs ns timer tns-block 3\n  gprs ns timer tns-block-retries 3\n  gprs ns timer tns-reset 3\n  gprs ns timer tns-reset-retries 3\n  gprs ns timer tns-test 30\n  gprs ns timer tns-alive 3\n  gprs ns timer tns-alive-retries 10\n  gprs nsvc 0 nsvci 1236\n  gprs nsvc 0 local udp port 23000\n  gprs nsvc 0 remote ip 192.168.100.239\n  gprs nsvc 0 remote udp port 23000\n  gprs nsvc 1 nsvci 0\n  gprs nsvc 1 local udp port 0\n  gprs nsvc 1 remote ip 0.0.0.0\n  gprs nsvc 1 remote udp port 0\n  no force-combined-si\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4+CBCH\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 1\n   rf_locked 0\n   arfcn 873\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 2\n   rf_locked 0\n   arfcn 875\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n  trx 3\n   rf_locked 0\n   arfcn 877\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\n bts 3\n  type osmo-bts\n  band DCS1800\n  cell_identity 3\n  location_area_code 0x0003\n  base_station_id_code 12\n  ms max power 15\n  cell reselection hysteresis 4\n  rxlev access min 0\n  radio-link-timeout 32\n  channel allocator mode chan-req ascending\n  channel allocator mode assignment ascending\n  channel allocator mode handover ascending\n  channel allocator mode vgcs-vbs ascending\n  rach tx integer 9\n  rach max transmission 7\n  rach max-delay 63\n  rach expiry-timeout 32\n  channel-description attach 1\n  channel-description bs-pa-mfrms 5\n  channel-description bs-ag-blks-res 1\n  no nch-position\n  no access-control-class-ramping\n  early-classmark-sending forbidden\n  early-classmark-sending-3g allowed\n  ipa unit-id 0 0\n  oml ipa stream-id 255 line 0\n  neighbor-list mode automatic\n  codec-support fr hr efr amr\n  amr tch-f modes 0 2 5 7\n  amr tch-f threshold ms 13 25 37\n  amr tch-f hysteresis ms 4 4 4\n  amr tch-f threshold bts 13 25 37\n  amr tch-f hysteresis bts 4 4 4\n  amr tch-f start-mode auto\n  amr tch-h modes 0 2 3 5\n  amr tch-h threshold ms 16 24 32\n  amr tch-h hysteresis ms 4 4 4\n  amr tch-h threshold bts 16 24 32\n  amr tch-h hysteresis bts 4 4 4\n  amr tch-h start-mode auto\n  gprs mode none\n  bs-power-control\n   mode static\n  ms-power-control\n   mode dyn-bts\n   ctrl-interval 2\n   step-size inc 4 red 2\n   rxlev-thresh lower 32 upper 38\n   rxlev-thresh-comp lower 10 12 upper 19 20\n   rxqual-thresh lower 3 upper 0\n   rxqual-thresh-comp lower 5 7 upper 15 18\n   ci-thresh fr-efr disable\n   ci-thresh fr-efr lower 13 upper 17\n   ci-thresh-comp fr-efr lower 5 7 upper 15 18\n   ci-thresh hr disable\n   ci-thresh hr lower 16 upper 21\n   ci-thresh-comp hr lower 5 7 upper 15 18\n   ci-thresh amr-fr disable\n   ci-thresh amr-fr lower 7 upper 11\n   ci-thresh-comp amr-fr lower 5 7 upper 15 18\n   ci-thresh amr-hr disable\n   ci-thresh amr-hr lower 13 upper 17\n   ci-thresh-comp amr-hr lower 5 7 upper 15 18\n   ci-thresh sdcch disable\n   ci-thresh sdcch lower 12 upper 16\n   ci-thresh-comp sdcch lower 5 7 upper 15 18\n   ci-thresh gprs disable\n   ci-thresh gprs lower 18 upper 24\n   ci-thresh-comp gprs lower 5 7 upper 15 18\n  trx 0\n   rf_locked 0\n   arfcn 871\n   nominal power 23\n   max_power_red 20\n   rsl e1 tei 0\n   timeslot 0\n    phys_chan_config CCCH+SDCCH4\n    hopping enabled 0\n   timeslot 1\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 2\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 3\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 4\n    phys_chan_config TCH/F\n    hopping enabled 0\n   timeslot 5\n    phys_chan_config TCH/H\n    hopping enabled 0\n   timeslot 6\n    phys_chan_config PDCH\n    hopping enabled 0\n   timeslot 7\n    phys_chan_config PDCH\n    hopping enabled 0\nmsc 0\n codec-list fr1 fr2 fr3 hr1 hr3\n allow-emergency allow\n amr-config 12_2k forbidden\n amr-config 10_2k forbidden\n amr-config 7_95k forbidden\n amr-config 7_40k forbidden\n amr-config 6_70k forbidden\n amr-config 5_90k allowed\n amr-config 5_15k forbidden\n amr-config 4_75k forbidden\n amr-payload octet-aligned\n msc-addr msc0\n asp-protocol m3ua\n lcls-mode mgw-loop\n lcls-codec-mismatch forbidden\n nri add 1 255\nmsc 1\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc1\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 256 511\n no allow-attach\nmsc 2\n codec-list fr1 hr1 fr2 fr3 hr3\n allow-emergency deny\n amr-config 12_2k allowed\n amr-config 10_2k allowed\n amr-config 7_95k allowed\n amr-config 7_40k allowed\n amr-config 6_70k allowed\n amr-config 5_90k allowed\n amr-config 5_15k allowed\n amr-config 4_75k allowed\n amr-payload octet-aligned\n msc-addr msc2\n asp-protocol m3ua\n lcls-mode disabled\n lcls-codec-mismatch forbidden\n nri add 512 767\n no allow-attach\nbsc\n mid-call-timeout 0\ncbc\n mode disabled\n server\n  local-port 48050\n client\n  remote-ip 127.0.0.1\nsmlc\n enable\nend" id 16
09:15:36.833567 Osmocom_VTY_Functions.ttcn:85 Message with id 16 was extracted from the queue of BSCVTY.
09:15:36.833651 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.833735 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.833807 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 17
09:15:36.833822 Osmocom_VTY_Functions.ttcn:73 Message with id 17 was extracted from the queue of BSCVTY.
09:15:36.833908 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.833987 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:36.834006 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.834116 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 18
09:15:36.834135 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.834152 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.834173 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.834184 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 18
09:15:36.834194 Osmocom_VTY_Functions.ttcn:74 Message with id 18 was extracted from the queue of BSCVTY.
09:15:36.834205 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.834219 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 0"
09:15:36.834234 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.834332 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 19
09:15:36.834351 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.834368 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.834388 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.834399 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 19
09:15:36.834410 Osmocom_VTY_Functions.ttcn:74 Message with id 19 was extracted from the queue of BSCVTY.
09:15:36.834420 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.834431 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "allow-attach"
09:15:36.834445 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.834529 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 20
09:15:36.834546 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.834568 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.834587 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.834597 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 20
09:15:36.834607 Osmocom_VTY_Functions.ttcn:74 Message with id 20 was extracted from the queue of BSCVTY.
09:15:36.834618 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.834628 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.834640 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.834712 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 21
09:15:36.834728 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.834743 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.834761 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.834772 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 21
09:15:36.834782 Osmocom_VTY_Functions.ttcn:74 Message with id 21 was extracted from the queue of BSCVTY.
09:15:36.834792 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.834802 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.834814 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.834883 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 22
09:15:36.834899 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.834914 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.834925 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 22
09:15:36.834935 Osmocom_VTY_Functions.ttcn:73 Message with id 22 was extracted from the queue of BSCVTY.
09:15:36.834946 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.834959 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:36.834971 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.834994 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 23
09:15:36.835010 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835025 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835044 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835055 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 23
09:15:36.835065 Osmocom_VTY_Functions.ttcn:74 Message with id 23 was extracted from the queue of BSCVTY.
09:15:36.835076 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835086 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 1"
09:15:36.835102 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835119 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 24
09:15:36.835136 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835151 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835169 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835179 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 24
09:15:36.835189 Osmocom_VTY_Functions.ttcn:74 Message with id 24 was extracted from the queue of BSCVTY.
09:15:36.835199 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835209 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
09:15:36.835221 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835238 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 25
09:15:36.835253 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835268 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835285 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835296 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 25
09:15:36.835305 Osmocom_VTY_Functions.ttcn:74 Message with id 25 was extracted from the queue of BSCVTY.
09:15:36.835315 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835325 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.835337 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835352 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 26
09:15:36.835367 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835382 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835400 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835410 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 26
09:15:36.835423 Osmocom_VTY_Functions.ttcn:74 Message with id 26 was extracted from the queue of BSCVTY.
09:15:36.835433 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835442 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.835453 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835466 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 27
09:15:36.835480 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835495 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.835504 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 27
09:15:36.835514 Osmocom_VTY_Functions.ttcn:73 Message with id 27 was extracted from the queue of BSCVTY.
09:15:36.835523 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835534 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:36.835549 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835564 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 28
09:15:36.835579 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835593 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835610 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835621 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 28
09:15:36.835630 Osmocom_VTY_Functions.ttcn:74 Message with id 28 was extracted from the queue of BSCVTY.
09:15:36.835640 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835649 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "msc 2"
09:15:36.835661 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835676 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 29
09:15:36.835691 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835705 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835722 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835732 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 29
09:15:36.835741 Osmocom_VTY_Functions.ttcn:74 Message with id 29 was extracted from the queue of BSCVTY.
09:15:36.835751 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835760 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "no allow-attach"
09:15:36.835771 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835787 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-msc)# " id 30
09:15:36.835801 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835815 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-msc)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835832 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-msc)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835842 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-msc)# " id 30
09:15:36.835851 Osmocom_VTY_Functions.ttcn:74 Message with id 30 was extracted from the queue of BSCVTY.
09:15:36.835860 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835869 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.835880 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.835895 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 31
09:15:36.835910 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.835923 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:36.835940 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:36.835951 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 31
09:15:36.835960 Osmocom_VTY_Functions.ttcn:74 Message with id 31 was extracted from the queue of BSCVTY.
09:15:36.835970 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.835979 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "exit"
09:15:36.835990 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:36.836003 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 32
09:15:36.836017 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:36.836032 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:36.836041 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 32
09:15:36.836051 Osmocom_VTY_Functions.ttcn:73 Message with id 32 was extracted from the queue of BSCVTY.
09:15:36.836060 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:36.836071 Osmocom_CTRL_Adapter.ttcn:69 Creating new PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
09:15:36.839083 Osmocom_CTRL_Adapter.ttcn:69 PTC was created. Component reference: 1481, alive: no, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-CTRL-CLI-IPA.
09:15:36.839100 Osmocom_CTRL_Adapter.ttcn:71 Mapping port IPA-CTRL-CLI-IPA(1481):IPA_PORT to system:IPA_CODEC_PT.
09:15:36.840417 Osmocom_CTRL_Adapter.ttcn:71 Map operation of IPA-CTRL-CLI-IPA(1481):IPA_PORT to system:IPA_CODEC_PT finished.
09:15:36.840434 Osmocom_CTRL_Adapter.ttcn:72 Connecting ports IPA-CTRL-CLI-IPA(1481):IPA_CTRL_PORT and mtc:IPA_CTRL.
09:15:36.840648 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL is waiting for connection from IPA-CTRL-CLI-IPA(1481):IPA_CTRL_PORT on UNIX pathname /tmp/ttcn3-portconn-4b31f21f.
09:15:36.840779 Osmocom_CTRL_Adapter.ttcn:72 Port IPA_CTRL has accepted the connection from IPA-CTRL-CLI-IPA(1481):IPA_CTRL_PORT.
09:15:36.840840 Osmocom_CTRL_Adapter.ttcn:72 Connect operation on IPA-CTRL-CLI-IPA(1481):IPA_CTRL_PORT and mtc:IPA_CTRL finished.
09:15:36.840856 Osmocom_CTRL_Adapter.ttcn:74 Starting function main_client("127.0.0.1", 4249, "", 0, { ser_nr := "", name := "mahlzeit", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "0/1/2", osmo_rand := "" }, false) on component IPA-CTRL-CLI-IPA(1481).
09:15:36.840947 Osmocom_CTRL_Adapter.ttcn:74 Function was started.
09:15:36.840963 Osmocom_CTRL_Adapter.ttcn:37 Start timer T: 10 s
09:15:36.842873 Osmocom_CTRL_Adapter.ttcn:38 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(1481) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:36.842897 Osmocom_CTRL_Adapter.ttcn:39 Matching on port IPA_CTRL succeeded:  matched
09:15:36.842915 Osmocom_CTRL_Adapter.ttcn:39 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(1481): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:36.842934 Osmocom_CTRL_Adapter.ttcn:39 Message with id 1 was extracted from the queue of IPA_CTRL.
09:15:36.842959 BSC_Tests.ttcn:1073 Creating new alive PTC with component type MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
09:15:36.849219 BSC_Tests.ttcn:1073 PTC was created. Component reference: 1482, alive: yes, type: MGCP_Emulation.MGCP_Emulation_CT, component name: VirtMGW-MGCP-0.
09:15:36.849249 BSC_Tests.ttcn:1074 Starting function main({ create_cb := refers(MGCP_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MGCP_Emulation.DummyUnitdataCallback) }, { callagent_ip := "127.0.0.1", callagent_udp_port := -1, mgw_ip := "127.0.0.1", mgw_udp_port := 2427, multi_conn_mode := false }, "VirtMGW-MGCP-0") on component VirtMGW-MGCP-0(1482).
09:15:36.849344 BSC_Tests.ttcn:1074 Function was started.
09:15:36.849373 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:15:36.849403 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.618225.
09:15:36.849452 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "618225305", variable := "bts.0.oml-connection-state", val := omit } }
09:15:36.849487 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:15:36.856204 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "618225305", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
09:15:36.856258 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:15:36.856303 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(1481): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "618225305", variable := "bts.0.oml-connection-state", val := "degraded" } } id 2
09:15:36.856344 Osmocom_CTRL_Functions.ttcn:41 Message with id 2 was extracted from the queue of IPA_CTRL.
09:15:36.856386 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:15:36.856424 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:15:37.856657 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:15:37.857115 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
09:15:37.866801 BSC_Tests.ttcn:951 PTC was created. Component reference: 1483, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS0-TRX0-RSL-IPA.
09:15:37.866997 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1234, bts_id := 0, trx_id := 0 }
09:15:37.867338 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1234/0/0"
09:15:37.867444 BSC_Tests.ttcn:960 Mapping port IPA-BTS0-TRX0-RSL-IPA(1483):IPA_PORT to system:IPA_CODEC_PT.
09:15:37.871446 BSC_Tests.ttcn:960 Map operation of IPA-BTS0-TRX0-RSL-IPA(1483):IPA_PORT to system:IPA_CODEC_PT finished.
09:15:37.871475 BSC_Tests.ttcn:961 Connecting ports IPA-BTS0-TRX0-RSL-IPA(1483):CFG_PORT and mtc:IPA_CFG_PORT[0][0].
09:15:37.871664 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(1483):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-47768b6e.
09:15:37.871716 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(1483):CFG_PORT.
09:15:37.871731 BSC_Tests.ttcn:961 Connect operation on IPA-BTS0-TRX0-RSL-IPA(1483):CFG_PORT and mtc:IPA_CFG_PORT[0][0] finished.
09:15:37.871742 BSC_Tests.ttcn:965 Connecting ports IPA-BTS0-TRX0-RSL-IPA(1483):IPA_RSL_PORT and mtc:IPA_RSL[0][0].
09:15:37.871824 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] is waiting for connection from IPA-BTS0-TRX0-RSL-IPA(1483):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-246cab76.
09:15:37.871856 BSC_Tests.ttcn:965 Port IPA_RSL[0][0] has accepted the connection from IPA-BTS0-TRX0-RSL-IPA(1483):IPA_RSL_PORT.
09:15:37.871867 BSC_Tests.ttcn:965 Connect operation on IPA-BTS0-TRX0-RSL-IPA(1483):IPA_RSL_PORT and mtc:IPA_RSL[0][0] finished.
09:15:37.871877 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 10000, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1234/0/0", osmo_rand := "" }, true) on component IPA-BTS0-TRX0-RSL-IPA(1483).
09:15:37.871903 BSC_Tests.ttcn:969 Function was started.
09:15:37.871913 BSC_Tests.ttcn:976 Start timer T: 10 s
09:15:37.879214 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:37.879294 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
09:15:37.879362 BSC_Tests.ttcn:981 Matching on port IPA_RSL[0][0] succeeded:  matched
09:15:37.879410 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(1483): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:37.879457 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[0][0].
09:15:37.883726 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:37.884097 BSC_Tests.ttcn:978 Matching on port IPA_RSL[0][0] succeeded:  matched
09:15:37.884183 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[0][0] succeeded, message from IPA-BTS0-TRX0-RSL-IPA(1483): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:37.884250 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[0][0].
09:15:37.884306 BSC_Tests.ttcn:979 Stop timer T: 10 s
09:15:37.884386 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:15:37.884464 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.526561.
09:15:37.884568 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "526561476", variable := "bts.0.oml-connection-state", val := omit } }
09:15:37.884653 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:15:37.886561 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "526561476", variable := "bts.0.oml-connection-state", val := "connected" } } id 3
09:15:37.886664 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:15:37.886720 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(1481): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "526561476", variable := "bts.0.oml-connection-state", val := "connected" } } id 3
09:15:37.886768 Osmocom_CTRL_Functions.ttcn:41 Message with id 3 was extracted from the queue of IPA_CTRL.
09:15:37.886827 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:15:37.886869 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:15:37.887157 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 3
09:15:37.888080 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 4
09:15:37.888215 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 5
09:15:37.888354 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 6
09:15:37.888491 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O } } } } } } id 7
09:15:37.888625 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000000F1100001C9031E174740E504000C132B2B'O } } } } } } id 8
09:15:37.888759 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064304367012B2B2B2B2B'O } } } } } } id 9
09:15:37.888890 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106008000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 10
09:15:37.889083 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 11
09:15:37.889196 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 12
09:15:37.889524 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 13
09:15:37.889634 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000000F110000197FF2B'O } } } } } } id 14
09:15:37.889937 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[0][0] from IPA-BTS0-TRX0-RSL-IPA(1483) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 15
09:15:38.887123 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:15:38.887690 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:38.888284 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:38.888951 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 33
09:15:38.889488 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:38.890046 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:38.890665 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:38.890918 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 33
09:15:38.891024 Osmocom_VTY_Functions.ttcn:74 Message with id 33 was extracted from the queue of BSCVTY.
09:15:38.891437 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:38.891612 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
09:15:38.891809 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:38.892191 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 34
09:15:38.892412 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:38.892597 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:38.892805 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
09:15:38.892951 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 34
09:15:38.893054 Osmocom_VTY_Functions.ttcn:74 Message with id 34 was extracted from the queue of BSCVTY.
09:15:38.893151 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:38.893249 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 0"
09:15:38.893377 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:38.893679 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 35
09:15:38.893843 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:38.893989 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:38.894164 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:15:38.894262 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 35
09:15:38.894386 Osmocom_VTY_Functions.ttcn:74 Message with id 35 was extracted from the queue of BSCVTY.
09:15:38.894478 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:38.894572 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
09:15:38.894694 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:38.895031 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 36
09:15:38.895187 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:38.895328 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:38.895495 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:15:38.895588 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 36
09:15:38.895671 Osmocom_VTY_Functions.ttcn:74 Message with id 36 was extracted from the queue of BSCVTY.
09:15:38.895757 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:38.895845 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:15:38.895963 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:38.896243 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 37
09:15:38.896392 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:38.896536 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:38.896626 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 37
09:15:38.896709 Osmocom_VTY_Functions.ttcn:73 Message with id 37 was extracted from the queue of BSCVTY.
09:15:38.896795 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:38.896884 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:15:38.896974 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.716483.
09:15:38.897102 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "716483430", variable := "bts.1.oml-connection-state", val := omit } }
09:15:38.897226 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:15:38.901323 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "716483430", variable := "bts.1.oml-connection-state", val := "degraded" } } id 4
09:15:38.901481 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:15:38.901580 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(1481): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "716483430", variable := "bts.1.oml-connection-state", val := "degraded" } } id 4
09:15:38.901669 Osmocom_CTRL_Functions.ttcn:41 Message with id 4 was extracted from the queue of IPA_CTRL.
09:15:38.901757 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:15:38.901837 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:15:39.902203 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:15:39.902751 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS1-TRX0-RSL-IPA.
09:15:39.911893 BSC_Tests.ttcn:951 PTC was created. Component reference: 1484, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS1-TRX0-RSL-IPA.
09:15:39.911958 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1235, bts_id := 0, trx_id := 0 }
09:15:39.912036 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1235/0/0"
09:15:39.912164 BSC_Tests.ttcn:960 Mapping port IPA-BTS1-TRX0-RSL-IPA(1484):IPA_PORT to system:IPA_CODEC_PT.
09:15:39.916856 BSC_Tests.ttcn:960 Map operation of IPA-BTS1-TRX0-RSL-IPA(1484):IPA_PORT to system:IPA_CODEC_PT finished.
09:15:39.917059 BSC_Tests.ttcn:961 Connecting ports IPA-BTS1-TRX0-RSL-IPA(1484):CFG_PORT and mtc:IPA_CFG_PORT[1][0].
09:15:39.918204 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[1][0] is waiting for connection from IPA-BTS1-TRX0-RSL-IPA(1484):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-40768a6e.
09:15:39.918700 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[1][0] has accepted the connection from IPA-BTS1-TRX0-RSL-IPA(1484):CFG_PORT.
09:15:39.918867 BSC_Tests.ttcn:961 Connect operation on IPA-BTS1-TRX0-RSL-IPA(1484):CFG_PORT and mtc:IPA_CFG_PORT[1][0] finished.
09:15:39.918986 BSC_Tests.ttcn:965 Connecting ports IPA-BTS1-TRX0-RSL-IPA(1484):IPA_RSL_PORT and mtc:IPA_RSL[1][0].
09:15:39.919915 BSC_Tests.ttcn:965 Port IPA_RSL[1][0] is waiting for connection from IPA-BTS1-TRX0-RSL-IPA(1484):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-236cab77.
09:15:39.920340 BSC_Tests.ttcn:965 Port IPA_RSL[1][0] has accepted the connection from IPA-BTS1-TRX0-RSL-IPA(1484):IPA_RSL_PORT.
09:15:39.920507 BSC_Tests.ttcn:965 Connect operation on IPA-BTS1-TRX0-RSL-IPA(1484):IPA_RSL_PORT and mtc:IPA_RSL[1][0] finished.
09:15:39.920624 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 11000, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1235/0/0", osmo_rand := "" }, true) on component IPA-BTS1-TRX0-RSL-IPA(1484).
09:15:39.920913 BSC_Tests.ttcn:969 Function was started.
09:15:39.921004 BSC_Tests.ttcn:976 Start timer T: 10 s
09:15:39.929948 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:39.930093 BSC_Tests.ttcn:978 Matching on port IPA_RSL[1][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
09:15:39.930189 BSC_Tests.ttcn:981 Matching on port IPA_RSL[1][0] succeeded:  matched
09:15:39.930274 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[1][0] succeeded, message from IPA-BTS1-TRX0-RSL-IPA(1484): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:39.930374 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[1][0].
09:15:39.934894 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:39.935085 BSC_Tests.ttcn:978 Matching on port IPA_RSL[1][0] succeeded:  matched
09:15:39.935244 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[1][0] succeeded, message from IPA-BTS1-TRX0-RSL-IPA(1484): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:39.935363 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[1][0].
09:15:39.935487 BSC_Tests.ttcn:979 Stop timer T: 10 s
09:15:39.935628 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:15:39.935772 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.418741.
09:15:39.935915 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "418741002", variable := "bts.1.oml-connection-state", val := omit } }
09:15:39.936010 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:15:39.938825 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "418741002", variable := "bts.1.oml-connection-state", val := "connected" } } id 5
09:15:39.938887 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:15:39.938937 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(1481): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "418741002", variable := "bts.1.oml-connection-state", val := "connected" } } id 5
09:15:39.938980 Osmocom_CTRL_Functions.ttcn:41 Message with id 5 was extracted from the queue of IPA_CTRL.
09:15:39.939023 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:15:39.939063 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:15:39.939716 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB38000000000000000000000000000E504002B'O } } } } } } id 3
09:15:39.940742 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 4
09:15:39.940892 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 5
09:15:39.941050 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 6
09:15:39.941201 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O } } } } } } id 7
09:15:39.941344 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000100F1100001C9031E174740E504000C132B2B'O } } } } } } id 8
09:15:39.941490 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000014740E5040064306367012B2B2B2B2B'O } } } } } } id 9
09:15:39.941632 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 10
09:15:39.941831 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 11
09:15:39.941962 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 12
09:15:39.942369 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 13
09:15:39.942501 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000100F110000197FF2B'O } } } } } } id 14
09:15:39.942831 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[1][0] from IPA-BTS1-TRX0-RSL-IPA(1484) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 15
09:15:40.940071 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:15:40.940543 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:40.940940 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:40.941456 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 38
09:15:40.941852 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:40.942223 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:40.942637 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:40.942845 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 38
09:15:40.942953 Osmocom_VTY_Functions.ttcn:74 Message with id 38 was extracted from the queue of BSCVTY.
09:15:40.943131 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:40.943309 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
09:15:40.943528 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:40.943855 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 39
09:15:40.944069 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:40.944254 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:40.944438 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
09:15:40.944537 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 39
09:15:40.944633 Osmocom_VTY_Functions.ttcn:74 Message with id 39 was extracted from the queue of BSCVTY.
09:15:40.944732 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:40.944837 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 1"
09:15:40.944974 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:40.945274 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 40
09:15:40.945465 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:40.945620 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:40.945789 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:15:40.945887 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 40
09:15:40.945981 Osmocom_VTY_Functions.ttcn:74 Message with id 40 was extracted from the queue of BSCVTY.
09:15:40.946075 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:40.946176 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
09:15:40.946365 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:40.946648 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 41
09:15:40.946812 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:40.946959 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:40.947130 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:15:40.947226 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 41
09:15:40.947311 Osmocom_VTY_Functions.ttcn:74 Message with id 41 was extracted from the queue of BSCVTY.
09:15:40.947399 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:40.947486 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:15:40.947608 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:40.947890 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 42
09:15:40.948041 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:40.948186 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:40.948280 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 42
09:15:40.948363 Osmocom_VTY_Functions.ttcn:73 Message with id 42 was extracted from the queue of BSCVTY.
09:15:40.948448 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:40.948539 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:15:40.948628 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.618455.
09:15:40.948757 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "618455466", variable := "bts.2.oml-connection-state", val := omit } }
09:15:40.948879 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:15:40.953404 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "618455466", variable := "bts.2.oml-connection-state", val := "degraded" } } id 6
09:15:40.953541 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:15:40.953639 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(1481): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "618455466", variable := "bts.2.oml-connection-state", val := "degraded" } } id 6
09:15:40.953726 Osmocom_CTRL_Functions.ttcn:41 Message with id 6 was extracted from the queue of IPA_CTRL.
09:15:40.953836 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:15:40.953921 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:15:41.954262 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:15:41.954751 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX0-RSL-IPA.
09:15:41.964006 BSC_Tests.ttcn:951 PTC was created. Component reference: 1485, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX0-RSL-IPA.
09:15:41.964139 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1236, bts_id := 0, trx_id := 0 }
09:15:41.964291 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1236/0/0"
09:15:41.964416 BSC_Tests.ttcn:960 Mapping port IPA-BTS2-TRX0-RSL-IPA(1485):IPA_PORT to system:IPA_CODEC_PT.
09:15:41.969241 BSC_Tests.ttcn:960 Map operation of IPA-BTS2-TRX0-RSL-IPA(1485):IPA_PORT to system:IPA_CODEC_PT finished.
09:15:41.969398 BSC_Tests.ttcn:961 Connecting ports IPA-BTS2-TRX0-RSL-IPA(1485):CFG_PORT and mtc:IPA_CFG_PORT[2][0].
09:15:41.970596 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][0] is waiting for connection from IPA-BTS2-TRX0-RSL-IPA(1485):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-4176896e.
09:15:41.971286 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][0] has accepted the connection from IPA-BTS2-TRX0-RSL-IPA(1485):CFG_PORT.
09:15:41.971517 BSC_Tests.ttcn:961 Connect operation on IPA-BTS2-TRX0-RSL-IPA(1485):CFG_PORT and mtc:IPA_CFG_PORT[2][0] finished.
09:15:41.971633 BSC_Tests.ttcn:965 Connecting ports IPA-BTS2-TRX0-RSL-IPA(1485):IPA_RSL_PORT and mtc:IPA_RSL[2][0].
09:15:41.972603 BSC_Tests.ttcn:965 Port IPA_RSL[2][0] is waiting for connection from IPA-BTS2-TRX0-RSL-IPA(1485):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-226cab74.
09:15:41.973068 BSC_Tests.ttcn:965 Port IPA_RSL[2][0] has accepted the connection from IPA-BTS2-TRX0-RSL-IPA(1485):IPA_RSL_PORT.
09:15:41.973213 BSC_Tests.ttcn:965 Connect operation on IPA-BTS2-TRX0-RSL-IPA(1485):IPA_RSL_PORT and mtc:IPA_RSL[2][0] finished.
09:15:41.973307 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 12000, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1236/0/0", osmo_rand := "" }, true) on component IPA-BTS2-TRX0-RSL-IPA(1485).
09:15:41.973589 BSC_Tests.ttcn:969 Function was started.
09:15:41.973676 BSC_Tests.ttcn:976 Start timer T: 10 s
09:15:41.982760 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:41.982905 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][0] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
09:15:41.983004 BSC_Tests.ttcn:981 Matching on port IPA_RSL[2][0] succeeded:  matched
09:15:41.983093 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[2][0] succeeded, message from IPA-BTS2-TRX0-RSL-IPA(1485): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:41.983179 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[2][0].
09:15:41.987758 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:41.987840 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][0] succeeded:  matched
09:15:41.987899 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[2][0] succeeded, message from IPA-BTS2-TRX0-RSL-IPA(1485): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:41.987962 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[2][0].
09:15:41.988020 BSC_Tests.ttcn:979 Stop timer T: 10 s
09:15:41.988090 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX1-RSL-IPA.
09:15:41.991807 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_1 (1) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '5506198FB3AA00000000000000000000000000E504002B'O } } } } } } id 3
09:15:41.992881 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2 (2) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '59061A00000000000000000000000000000000FFE50400'O } } } } } } id 4
09:15:41.993041 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2bis (10) } } } } } id 5
09:15:41.993220 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2ter (11) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '4906038E3200000000000000000000000008002B2B2B2B'O } } } } } } id 6
09:15:41.993374 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_2quater (41) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '590607400004870000B3006FB5D2AD812B2B2B2B2B2B2B'O } } } } } } id 7
09:15:41.993530 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_3 (3) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '49061B000100F1100002C9031E174740E504000C132B2B'O } } } } } } id 8
09:15:41.993678 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_4 (4) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '41061C00F11000024740E5040064308367012B2B2B2B2B'O } } } } } } id 9
09:15:41.993830 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_CCHAN (6), transparent := false }, msg_type := RSL_MT_BCCH_INFO (17), ies := { { iei := RSL_IE_CHAN_NR (1), body := { chan_nr := { u := { ch0 := RSL_CHAN_NR_BCCH (16) }, tn := 0 } } }, { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_13 (40) } }, { iei := RSL_IE_FULL_BCCH_INFO (39), body := { other := { len := 23, payload := '0106009000185A6FC9F14608411B2B2B2B2B2B2B2B2B2B'O } } } } } } id 10
09:15:41.994045 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 11
09:15:41.994179 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 12
09:15:41.994310 BSC_Tests.ttcn:951 PTC was created. Component reference: 1486, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX1-RSL-IPA.
09:15:41.994367 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1236, bts_id := 0, trx_id := 1 }
09:15:41.994404 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1236/0/1"
09:15:41.994436 BSC_Tests.ttcn:960 Mapping port IPA-BTS2-TRX1-RSL-IPA(1486):IPA_PORT to system:IPA_CODEC_PT.
09:15:41.994577 BSC_Tests.ttcn:960 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 13
09:15:41.994690 BSC_Tests.ttcn:960 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000100F110000297FF2B'O } } } } } } id 14
09:15:41.995020 BSC_Tests.ttcn:960 Message enqueued on IPA_RSL[2][0] from IPA-BTS2-TRX0-RSL-IPA(1485) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 15
09:15:41.995902 BSC_Tests.ttcn:960 Map operation of IPA-BTS2-TRX1-RSL-IPA(1486):IPA_PORT to system:IPA_CODEC_PT finished.
09:15:41.995935 BSC_Tests.ttcn:961 Connecting ports IPA-BTS2-TRX1-RSL-IPA(1486):CFG_PORT and mtc:IPA_CFG_PORT[2][1].
09:15:41.996121 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][1] is waiting for connection from IPA-BTS2-TRX1-RSL-IPA(1486):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-4276896f.
09:15:41.996204 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][1] has accepted the connection from IPA-BTS2-TRX1-RSL-IPA(1486):CFG_PORT.
09:15:41.996244 BSC_Tests.ttcn:961 Connect operation on IPA-BTS2-TRX1-RSL-IPA(1486):CFG_PORT and mtc:IPA_CFG_PORT[2][1] finished.
09:15:41.996276 BSC_Tests.ttcn:965 Connecting ports IPA-BTS2-TRX1-RSL-IPA(1486):IPA_RSL_PORT and mtc:IPA_RSL[2][1].
09:15:41.996440 BSC_Tests.ttcn:965 Port IPA_RSL[2][1] is waiting for connection from IPA-BTS2-TRX1-RSL-IPA(1486):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-206cab74.
09:15:41.996523 BSC_Tests.ttcn:965 Port IPA_RSL[2][1] has accepted the connection from IPA-BTS2-TRX1-RSL-IPA(1486):IPA_RSL_PORT.
09:15:41.996563 BSC_Tests.ttcn:965 Connect operation on IPA-BTS2-TRX1-RSL-IPA(1486):IPA_RSL_PORT and mtc:IPA_RSL[2][1] finished.
09:15:41.996595 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 12001, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1236/0/1", osmo_rand := "" }, true) on component IPA-BTS2-TRX1-RSL-IPA(1486).
09:15:41.996657 BSC_Tests.ttcn:969 Function was started.
09:15:41.996688 BSC_Tests.ttcn:976 Start timer T: 10 s
09:15:42.000142 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][1] from IPA-BTS2-TRX1-RSL-IPA(1486) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:42.000210 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][1] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
09:15:42.000261 BSC_Tests.ttcn:981 Matching on port IPA_RSL[2][1] succeeded:  matched
09:15:42.000309 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[2][1] succeeded, message from IPA-BTS2-TRX1-RSL-IPA(1486): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:42.000353 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[2][1].
09:15:42.002872 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][1] from IPA-BTS2-TRX1-RSL-IPA(1486) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:42.002922 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][1] succeeded:  matched
09:15:42.002959 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[2][1] succeeded, message from IPA-BTS2-TRX1-RSL-IPA(1486): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:42.002993 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[2][1].
09:15:42.003027 BSC_Tests.ttcn:979 Stop timer T: 10 s
09:15:42.003069 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX2-RSL-IPA.
09:15:42.005020 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][1] from IPA-BTS2-TRX1-RSL-IPA(1486) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 3
09:15:42.005442 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][1] from IPA-BTS2-TRX1-RSL-IPA(1486) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 4
09:15:42.005557 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][1] from IPA-BTS2-TRX1-RSL-IPA(1486) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 5
09:15:42.005665 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][1] from IPA-BTS2-TRX1-RSL-IPA(1486) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000100F110000297FF2B'O } } } } } } id 6
09:15:42.005942 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][1] from IPA-BTS2-TRX1-RSL-IPA(1486) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 7
09:15:42.007356 BSC_Tests.ttcn:951 PTC was created. Component reference: 1487, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX2-RSL-IPA.
09:15:42.007390 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1236, bts_id := 0, trx_id := 2 }
09:15:42.007423 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1236/0/2"
09:15:42.007451 BSC_Tests.ttcn:960 Mapping port IPA-BTS2-TRX2-RSL-IPA(1487):IPA_PORT to system:IPA_CODEC_PT.
09:15:42.008784 BSC_Tests.ttcn:960 Map operation of IPA-BTS2-TRX2-RSL-IPA(1487):IPA_PORT to system:IPA_CODEC_PT finished.
09:15:42.008818 BSC_Tests.ttcn:961 Connecting ports IPA-BTS2-TRX2-RSL-IPA(1487):CFG_PORT and mtc:IPA_CFG_PORT[2][2].
09:15:42.008991 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][2] is waiting for connection from IPA-BTS2-TRX2-RSL-IPA(1487):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-4376896c.
09:15:42.009075 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][2] has accepted the connection from IPA-BTS2-TRX2-RSL-IPA(1487):CFG_PORT.
09:15:42.009117 BSC_Tests.ttcn:961 Connect operation on IPA-BTS2-TRX2-RSL-IPA(1487):CFG_PORT and mtc:IPA_CFG_PORT[2][2] finished.
09:15:42.009152 BSC_Tests.ttcn:965 Connecting ports IPA-BTS2-TRX2-RSL-IPA(1487):IPA_RSL_PORT and mtc:IPA_RSL[2][2].
09:15:42.009316 BSC_Tests.ttcn:965 Port IPA_RSL[2][2] is waiting for connection from IPA-BTS2-TRX2-RSL-IPA(1487):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-226cab74.
09:15:42.009400 BSC_Tests.ttcn:965 Port IPA_RSL[2][2] has accepted the connection from IPA-BTS2-TRX2-RSL-IPA(1487):IPA_RSL_PORT.
09:15:42.009443 BSC_Tests.ttcn:965 Connect operation on IPA-BTS2-TRX2-RSL-IPA(1487):IPA_RSL_PORT and mtc:IPA_RSL[2][2] finished.
09:15:42.009479 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 12002, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1236/0/2", osmo_rand := "" }, true) on component IPA-BTS2-TRX2-RSL-IPA(1487).
09:15:42.009554 BSC_Tests.ttcn:969 Function was started.
09:15:42.009590 BSC_Tests.ttcn:976 Start timer T: 10 s
09:15:42.013226 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][2] from IPA-BTS2-TRX2-RSL-IPA(1487) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:42.013320 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][2] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
09:15:42.013374 BSC_Tests.ttcn:981 Matching on port IPA_RSL[2][2] succeeded:  matched
09:15:42.013421 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[2][2] succeeded, message from IPA-BTS2-TRX2-RSL-IPA(1487): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:42.013466 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[2][2].
09:15:42.016940 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][2] from IPA-BTS2-TRX2-RSL-IPA(1487) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:42.017096 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][2] succeeded:  matched
09:15:42.017342 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[2][2] succeeded, message from IPA-BTS2-TRX2-RSL-IPA(1487): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:42.017428 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[2][2].
09:15:42.017496 BSC_Tests.ttcn:979 Stop timer T: 10 s
09:15:42.017591 BSC_Tests.ttcn:951 Creating new alive PTC with component type IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX3-RSL-IPA.
09:15:42.021215 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][2] from IPA-BTS2-TRX2-RSL-IPA(1487) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 3
09:15:42.021976 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][2] from IPA-BTS2-TRX2-RSL-IPA(1487) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 4
09:15:42.022188 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][2] from IPA-BTS2-TRX2-RSL-IPA(1487) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 5
09:15:42.022385 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][2] from IPA-BTS2-TRX2-RSL-IPA(1487) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000100F110000297FF2B'O } } } } } } id 6
09:15:42.022838 BSC_Tests.ttcn:951 Message enqueued on IPA_RSL[2][2] from IPA-BTS2-TRX2-RSL-IPA(1487) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 7
09:15:42.025060 BSC_Tests.ttcn:951 PTC was created. Component reference: 1488, alive: yes, type: IPA_Emulation.IPA_Emulation_CT, component name: IPA-BTS2-TRX3-RSL-IPA.
09:15:42.025119 BSC_Tests.ttcn:954 enc_IpaUnitId(): Encoding @IPA_Types.IpaUnitId: { site_id := 1236, bts_id := 0, trx_id := 3 }
09:15:42.025164 BSC_Tests.ttcn:954 enc_IpaUnitId(): Stream after encoding: "1236/0/3"
09:15:42.025204 BSC_Tests.ttcn:960 Mapping port IPA-BTS2-TRX3-RSL-IPA(1488):IPA_PORT to system:IPA_CODEC_PT.
09:15:42.027008 BSC_Tests.ttcn:960 Map operation of IPA-BTS2-TRX3-RSL-IPA(1488):IPA_PORT to system:IPA_CODEC_PT finished.
09:15:42.027069 BSC_Tests.ttcn:961 Connecting ports IPA-BTS2-TRX3-RSL-IPA(1488):CFG_PORT and mtc:IPA_CFG_PORT[2][3].
09:15:42.027388 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][3] is waiting for connection from IPA-BTS2-TRX3-RSL-IPA(1488):CFG_PORT on UNIX pathname /tmp/ttcn3-portconn-5c76896d.
09:15:42.027516 BSC_Tests.ttcn:961 Port IPA_CFG_PORT[2][3] has accepted the connection from IPA-BTS2-TRX3-RSL-IPA(1488):CFG_PORT.
09:15:42.027573 BSC_Tests.ttcn:961 Connect operation on IPA-BTS2-TRX3-RSL-IPA(1488):CFG_PORT and mtc:IPA_CFG_PORT[2][3] finished.
09:15:42.027619 BSC_Tests.ttcn:965 Connecting ports IPA-BTS2-TRX3-RSL-IPA(1488):IPA_RSL_PORT and mtc:IPA_RSL[2][3].
09:15:42.027858 BSC_Tests.ttcn:965 Port IPA_RSL[2][3] is waiting for connection from IPA-BTS2-TRX3-RSL-IPA(1488):IPA_RSL_PORT on UNIX pathname /tmp/ttcn3-portconn-3c6cab74.
09:15:42.027975 BSC_Tests.ttcn:965 Port IPA_RSL[2][3] has accepted the connection from IPA-BTS2-TRX3-RSL-IPA(1488):IPA_RSL_PORT.
09:15:42.028032 BSC_Tests.ttcn:965 Connect operation on IPA-BTS2-TRX3-RSL-IPA(1488):IPA_RSL_PORT and mtc:IPA_RSL[2][3] finished.
09:15:42.028081 BSC_Tests.ttcn:969 Starting function main_client("127.0.0.1", 3003, "", 12003, { ser_nr := "", name := "Osmocom TTCN-3 BTS Simulator", location1 := "", location2 := "", equip_version := "", sw_version := "", ip_addr := "", mac_addr := "", unit_id := "1236/0/3", osmo_rand := "" }, true) on component IPA-BTS2-TRX3-RSL-IPA(1488).
09:15:42.028179 BSC_Tests.ttcn:969 Function was started.
09:15:42.028229 BSC_Tests.ttcn:976 Start timer T: 10 s
09:15:42.033325 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][3] from IPA-BTS2-TRX3-RSL-IPA(1488) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:42.033418 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][3] ASP_IPA_EVENT_UP (1) with ASP_IPA_EVENT_ID_ACK (3) unmatched: First message in the queue does not match the template: 
09:15:42.033483 BSC_Tests.ttcn:981 Matching on port IPA_RSL[2][3] succeeded:  matched
09:15:42.033544 BSC_Tests.ttcn:981 Receive operation on port IPA_RSL[2][3] succeeded, message from IPA-BTS2-TRX3-RSL-IPA(1488): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_UP (1), conn_id := 1, id_resp := omit } id 1
09:15:42.033602 BSC_Tests.ttcn:981 Message with id 1 was extracted from the queue of IPA_RSL[2][3].
09:15:42.036861 BSC_Tests.ttcn:977 Message enqueued on IPA_RSL[2][3] from IPA-BTS2-TRX3-RSL-IPA(1488) @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:42.036922 BSC_Tests.ttcn:978 Matching on port IPA_RSL[2][3] succeeded:  matched
09:15:42.036970 BSC_Tests.ttcn:978 Receive operation on port IPA_RSL[2][3] succeeded, message from IPA-BTS2-TRX3-RSL-IPA(1488): @IPA_Emulation.ASP_IPA_Event : { ev_type := ASP_IPA_EVENT_ID_ACK (3), conn_id := 1, id_resp := omit } id 2
09:15:42.037036 BSC_Tests.ttcn:978 Message with id 2 was extracted from the queue of IPA_RSL[2][3].
09:15:42.037081 BSC_Tests.ttcn:979 Stop timer T: 10 s
09:15:42.037127 BSC_Tests.ttcn:1016 Start timer T: 5 s
09:15:42.037174 Osmocom_CTRL_Functions.ttcn:30 Function rnd() returned 0.090585.
09:15:42.037242 Osmocom_CTRL_Functions.ttcn:38 Sent on IPA_CTRL to IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { cmd := { verb := "GET", id := "90584852", variable := "bts.2.oml-connection-state", val := omit } }
09:15:42.037301 Osmocom_CTRL_Functions.ttcn:39 Start timer T: 2 s
09:15:42.038706 Osmocom_CTRL_Functions.ttcn:40 Message enqueued on IPA_CTRL from IPA-CTRL-CLI-IPA(1481) @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "90584852", variable := "bts.2.oml-connection-state", val := "connected" } } id 7
09:15:42.038763 Osmocom_CTRL_Functions.ttcn:41 Matching on port IPA_CTRL succeeded:  matched
09:15:42.038806 Osmocom_CTRL_Functions.ttcn:41 Receive operation on port IPA_CTRL succeeded, message from IPA-CTRL-CLI-IPA(1481): @Osmocom_CTRL_Types.CtrlMessage : { resp := { verb := "GET_REPLY", id := "90584852", variable := "bts.2.oml-connection-state", val := "connected" } } id 7
09:15:42.038843 Osmocom_CTRL_Functions.ttcn:41 Message with id 7 was extracted from the queue of IPA_CTRL.
09:15:42.038879 BSC_Tests.ttcn:1019 Stop timer T: 5 s
09:15:42.038913 BSC_Tests.ttcn:1022 Start timer T: 1 s
09:15:42.039313 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[2][3] from IPA-BTS2-TRX3-RSL-IPA(1488) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5 (5) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '49061D10000000000000000000000000000000'O } } } } } } id 3
09:15:42.039798 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[2][3] from IPA-BTS2-TRX3-RSL-IPA(1488) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5bis (13) } } } } } id 4
09:15:42.039939 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[2][3] from IPA-BTS2-TRX3-RSL-IPA(1488) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_5ter (14) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 19, payload := '4906069E050020000000000000000000000000'O } } } } } } id 5
09:15:42.040070 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[2][3] from IPA-BTS2-TRX3-RSL-IPA(1488) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_SACCH_FILL (26), ies := { { iei := RSL_IE_SYSINFO_TYPE (30), body := { sysinfo_type := RSL_SYSTEM_INFO_6 (6) } }, { iei := RSL_IE_L3_INFO (11), body := { l3_info := { len := 13, payload := '2D061E000100F110000297FF2B'O } } } } } } id 6
09:15:42.040382 BSC_Tests.ttcn:1023 Message enqueued on IPA_RSL[2][3] from IPA-BTS2-TRX3-RSL-IPA(1488) @IPA_Emulation.ASP_RSL_Unitdata : { conn_id := 1, streamId := IPAC_PROTO_RSL_TRX0 (0), rsl := { msg_disc := { msg_group := RSL_MDISC_TRX_MGMT (8), transparent := false }, msg_type := RSL_MT_IPAC_MEAS_PREPROC_DFT (96), ies := { { iei := RSL_IE_MS_POWER (13), body := { ms_power := { reserved := 0, fpc_epc := false, power_level := 0 } } }, { iei := RSL_IE_BS_POWER (4), body := { bs_power := { reserved := 0, epc := false, fpc := false, power_level := 0 } } }, { iei := RSL_IE_MS_POWER_PARAM (31), body := { ms_power_params := { len := 55, params := '062026300A0A0C131405070F120242F10C000000000000000000000000F218000000000000000000000000000000000000000000000000'O } } } } } } id 7
09:15:43.039634 BSC_Tests.ttcn:1023 Timeout T: 1 s
09:15:43.040223 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "configure terminal"
09:15:43.040827 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:43.041321 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config)# " id 43
09:15:43.041639 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:43.041917 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:43.042209 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config)# " with pattern "[\w-]+\(*\)\# " matched
09:15:43.042439 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config)# " id 43
09:15:43.042830 Osmocom_VTY_Functions.ttcn:74 Message with id 43 was extracted from the queue of BSCVTY.
09:15:43.043267 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:43.043538 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "network"
09:15:43.043825 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:43.044278 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net)# " id 44
09:15:43.044494 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:43.044662 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:43.044850 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net)# " with pattern "[\w-]+\(*\)\# " matched
09:15:43.044953 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net)# " id 44
09:15:43.045060 Osmocom_VTY_Functions.ttcn:74 Message with id 44 was extracted from the queue of BSCVTY.
09:15:43.045153 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:43.045249 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "bts 2"
09:15:43.045379 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:43.045690 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 45
09:15:43.045852 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:43.046002 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:43.046175 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:15:43.046270 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 45
09:15:43.046383 Osmocom_VTY_Functions.ttcn:74 Message with id 45 was extracted from the queue of BSCVTY.
09:15:43.046472 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:43.046563 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "osmux off"
09:15:43.046685 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:43.047036 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC(config-net-bts)# " id 46
09:15:43.047189 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:43.047366 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:43.047537 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY succeeded: "OsmoBSC(config-net-bts)# " with pattern "[\w-]+\(*\)\# " matched
09:15:43.047632 Osmocom_VTY_Functions.ttcn:74 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC(config-net-bts)# " id 46
09:15:43.047716 Osmocom_VTY_Functions.ttcn:74 Message with id 46 was extracted from the queue of BSCVTY.
09:15:43.047802 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:43.047889 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "end"
09:15:43.048011 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:43.048303 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 47
09:15:43.048452 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:43.048598 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:43.048689 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 47
09:15:43.048772 Osmocom_VTY_Functions.ttcn:73 Message with id 47 was extracted from the queue of BSCVTY.
09:15:43.048857 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:43.048944 Osmocom_VTY_Functions.ttcn:338 "TC_paging_imsi_nochan_cgi_unknown_cid() start"
09:15:43.049085 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "logp lglobal notice TTCN3 f_logp(): TC_paging_imsi_nochan_cgi_unknown_cid() start"
09:15:43.049209 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:43.049572 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 48
09:15:43.049726 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:43.049873 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:43.049966 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 48
09:15:43.050053 Osmocom_VTY_Functions.ttcn:73 Message with id 48 was extracted from the queue of BSCVTY.
09:15:43.050137 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:43.050247 BSC_Tests.ttcn:3508 Message with id 3 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050352 BSC_Tests.ttcn:3508 Message with id 4 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050434 BSC_Tests.ttcn:3508 Message with id 5 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050514 BSC_Tests.ttcn:3508 Message with id 6 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050593 BSC_Tests.ttcn:3508 Message with id 7 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050671 BSC_Tests.ttcn:3508 Message with id 8 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050748 BSC_Tests.ttcn:3508 Message with id 9 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050824 BSC_Tests.ttcn:3508 Message with id 10 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050903 BSC_Tests.ttcn:3508 Message with id 11 was extracted from the queue of IPA_RSL[0][0].
09:15:43.050978 BSC_Tests.ttcn:3508 Message with id 12 was extracted from the queue of IPA_RSL[0][0].
09:15:43.051053 BSC_Tests.ttcn:3508 Message with id 13 was extracted from the queue of IPA_RSL[0][0].
09:15:43.051130 BSC_Tests.ttcn:3508 Message with id 14 was extracted from the queue of IPA_RSL[0][0].
09:15:43.051209 BSC_Tests.ttcn:3508 Message with id 15 was extracted from the queue of IPA_RSL[0][0].
09:15:43.051282 BSC_Tests.ttcn:3508 Port IPA_RSL[0][0] was cleared.
09:15:43.051390 BSC_Tests.ttcn:3508 Message with id 3 was extracted from the queue of IPA_RSL[1][0].
09:15:43.051472 BSC_Tests.ttcn:3508 Message with id 4 was extracted from the queue of IPA_RSL[1][0].
09:15:43.051550 BSC_Tests.ttcn:3508 Message with id 5 was extracted from the queue of IPA_RSL[1][0].
09:15:43.051626 BSC_Tests.ttcn:3508 Message with id 6 was extracted from the queue of IPA_RSL[1][0].
09:15:43.051702 BSC_Tests.ttcn:3508 Message with id 7 was extracted from the queue of IPA_RSL[1][0].
09:15:43.051779 BSC_Tests.ttcn:3508 Message with id 8 was extracted from the queue of IPA_RSL[1][0].
09:15:43.051995 BSC_Tests.ttcn:3508 Message with id 9 was extracted from the queue of IPA_RSL[1][0].
09:15:43.052186 BSC_Tests.ttcn:3508 Message with id 10 was extracted from the queue of IPA_RSL[1][0].
09:15:43.052362 BSC_Tests.ttcn:3508 Message with id 11 was extracted from the queue of IPA_RSL[1][0].
09:15:43.052546 BSC_Tests.ttcn:3508 Message with id 12 was extracted from the queue of IPA_RSL[1][0].
09:15:43.052733 BSC_Tests.ttcn:3508 Message with id 13 was extracted from the queue of IPA_RSL[1][0].
09:15:43.052923 BSC_Tests.ttcn:3508 Message with id 14 was extracted from the queue of IPA_RSL[1][0].
09:15:43.053103 BSC_Tests.ttcn:3508 Message with id 15 was extracted from the queue of IPA_RSL[1][0].
09:15:43.053182 BSC_Tests.ttcn:3508 Port IPA_RSL[1][0] was cleared.
09:15:43.053263 BSC_Tests.ttcn:3508 Message with id 3 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053342 BSC_Tests.ttcn:3508 Message with id 4 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053420 BSC_Tests.ttcn:3508 Message with id 5 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053498 BSC_Tests.ttcn:3508 Message with id 6 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053575 BSC_Tests.ttcn:3508 Message with id 7 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053651 BSC_Tests.ttcn:3508 Message with id 8 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053727 BSC_Tests.ttcn:3508 Message with id 9 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053804 BSC_Tests.ttcn:3508 Message with id 10 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053880 BSC_Tests.ttcn:3508 Message with id 11 was extracted from the queue of IPA_RSL[2][0].
09:15:43.053955 BSC_Tests.ttcn:3508 Message with id 12 was extracted from the queue of IPA_RSL[2][0].
09:15:43.054030 BSC_Tests.ttcn:3508 Message with id 13 was extracted from the queue of IPA_RSL[2][0].
09:15:43.054105 BSC_Tests.ttcn:3508 Message with id 14 was extracted from the queue of IPA_RSL[2][0].
09:15:43.054182 BSC_Tests.ttcn:3508 Message with id 15 was extracted from the queue of IPA_RSL[2][0].
09:15:43.054258 BSC_Tests.ttcn:3508 Port IPA_RSL[2][0] was cleared.
09:15:43.054713 BSC_Tests.ttcn:3518 Sent on BSSAP to VirtMSC-SCCP(1477) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { paging := { messageType := '52'O ("R"), iMSI := { elementIdentifier := '08'O ("\b"), lengthIndicator := 0, typeOfIdentity := '001'B, oddEvenIndicator := '1'B, digits := '001010000000006'H }, tMSI := omit, cellIdentifierList := { elementIdentifier := '1A'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentificationList := { cIl_CGI := { { mcc_mnc := '76089F'O, lac := '0001'O, ci := '0000'O } } } }, channelNeeded := omit, eMLPP_Priority := omit, pagingInformation := omit } } } }, importance := omit }
09:15:43.054845 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { paging := { messageType := '52'O ("R"), iMSI := { elementIdentifier := '08'O ("\b"), lengthIndicator := 0, typeOfIdentity := '001'B, oddEvenIndicator := '1'B, digits := '001010000000006'H }, tMSI := omit, cellIdentifierList := { elementIdentifier := '1A'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentificationList := { cIl_CGI := { { mcc_mnc := '76089F'O, lac := '0001'O, ci := '0000'O } } } }, channelNeeded := omit, eMLPP_Priority := omit, pagingInformation := omit } } } }
09:15:43.055051 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '001552080809101000000000601A080076089F00010000'O
09:15:43.055173 BSC_Tests.ttcn:3518 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := '001552080809101000000000601A080076089F00010000'O, importance := omit }
09:15:43.055384 Osmocom_Types.ttcn:126 Start timer T: 2 s
09:15:45.056744 Osmocom_Types.ttcn:127 Timeout T: 2 s
09:15:45.057313 BSC_Tests.ttcn:3545 Start timer T: 0.1 s
09:15:45.157995 BSC_Tests.ttcn:3551 Timeout T: 0.1 s
09:15:45.158542 BSC_Tests.ttcn:3545 Start timer T: 0.1 s
09:15:45.259215 BSC_Tests.ttcn:3551 Timeout T: 0.1 s
09:15:45.259773 BSC_Tests.ttcn:3545 Start timer T: 0.1 s
09:15:45.360457 BSC_Tests.ttcn:3551 Timeout T: 0.1 s
09:15:45.361016 BSC_Tests.ttcn:3555 setverdict(pass): none -> pass
09:15:45.361664 Osmocom_VTY_Functions.ttcn:105 Sent on BSCVTY to system charstring : "show talloc-context application full filter \\<struct.bsc_subscr\\>\\|\\<struct.gsm_subscriber_connection\\>"
09:15:45.362177 Osmocom_VTY_Functions.ttcn:70 Start timer T: 2 s
09:15:45.363621 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "full talloc report on 'osmo-bsc' (total 1458717 bytes in 1353 blocks)" id 49
09:15:45.364089 Osmocom_VTY_Functions.ttcn:71 Message enqueued on BSCVTY from system charstring : "OsmoBSC# " id 50
09:15:45.364637 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1458717 bytes in 1353 blocks)" with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:45.364963 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1458717 bytes in 1353 blocks)" with pattern "[\w-]+\# " unmatched: First message in the queue does not match the template: 
09:15:45.365235 Osmocom_VTY_Functions.ttcn:74 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1458717 bytes in 1353 blocks)" with pattern "[\w-]+\(*\)\# " unmatched: First message in the queue does not match the template: 
09:15:45.365455 Osmocom_VTY_Functions.ttcn:75 Matching on port BSCVTY "full talloc report on 'osmo-bsc' (total 1458717 bytes in 1353 blocks)" with pattern "*% Unknown command." unmatched: First message in the queue does not match the template: 
09:15:45.365653 Osmocom_VTY_Functions.ttcn:85 Matching on port BSCVTY succeeded: "full talloc report on 'osmo-bsc' (total 1458717 bytes in 1353 blocks)" with ? matched
09:15:45.365851 Osmocom_VTY_Functions.ttcn:85 Receive operation on port BSCVTY succeeded, message from system(): charstring : "full talloc report on 'osmo-bsc' (total 1458717 bytes in 1353 blocks)" id 49
09:15:45.365943 Osmocom_VTY_Functions.ttcn:85 Message with id 49 was extracted from the queue of BSCVTY.
09:15:45.366081 Osmocom_VTY_Functions.ttcn:72 Matching on port BSCVTY "OsmoBSC# " with pattern "[\w-]+> " unmatched: First message in the queue does not match the template: 
09:15:45.366254 Osmocom_VTY_Functions.ttcn:73 Matching on port BSCVTY succeeded: "OsmoBSC# " with pattern "[\w-]+\# " matched
09:15:45.366505 Osmocom_VTY_Functions.ttcn:73 Receive operation on port BSCVTY succeeded, message from system(): charstring : "OsmoBSC# " id 50
09:15:45.366757 Osmocom_VTY_Functions.ttcn:73 Message with id 50 was extracted from the queue of BSCVTY.
09:15:45.366937 Osmocom_VTY_Functions.ttcn:99 Stop timer T: 2 s
09:15:45.367114 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct bsc_subscr" x 0, expecting 0
09:15:45.367321 Osmocom_VTY_Functions.ttcn:265 talloc reports "struct gsm_subscriber_connection" x 0, expecting 0
09:15:45.367503 BSC_Tests.ttcn:888 Stopping all components.
09:15:45.371433 BSC_Tests.ttcn:888 Connection of port IPA_CTRL to IPA-CTRL-CLI-IPA(1481):IPA_CTRL_PORT was closed unexpectedly by the peer.
09:15:45.371641 BSC_Tests.ttcn:888 Port IPA_CTRL was disconnected from IPA-CTRL-CLI-IPA(1481):IPA_CTRL_PORT.
09:15:45.374073 BSC_Tests.ttcn:888 All components were stopped.
09:15:45.374219 BSC_Tests.ttcn:889 setverdict(pass): pass -> pass, component reason not changed
09:15:45.374432 BSC_Tests.ttcn:890 Stopping test component execution.
09:15:45.374717 BSC_Tests.ttcn:3698 Test case TC_paging_imsi_nochan_cgi_unknown_cid was stopped.
09:15:45.374860 BSC_Tests.ttcn:3698 Terminating component type BSC_Tests.test_CT.
09:15:45.374971 BSC_Tests.ttcn:3698 Default with id 1 (altstep as_Tguard) was deactivated.
09:15:45.375074 BSC_Tests.ttcn:3698 Stop timer T_guard: 30 s
09:15:45.375178 BSC_Tests.ttcn:3698 Port IPA_CTRL was stopped.
09:15:45.375264 BSC_Tests.ttcn:3698 Port RSL_CCHAN[0] was stopped.
09:15:45.375345 BSC_Tests.ttcn:3698 Port RSL_CCHAN[1] was stopped.
09:15:45.375422 BSC_Tests.ttcn:3698 Port RSL_CCHAN[2] was stopped.
09:15:45.375499 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_RSL[0][0] and IPA-BTS0-TRX0-RSL-IPA(1483):IPA_RSL_PORT.
09:15:45.375645 BSC_Tests.ttcn:3698 Port IPA_RSL[0][0] was stopped.
09:15:45.375762 BSC_Tests.ttcn:3698 Port IPA_RSL[0][1] was stopped.
09:15:45.375844 BSC_Tests.ttcn:3698 Port IPA_RSL[0][2] was stopped.
09:15:45.375922 BSC_Tests.ttcn:3698 Port IPA_RSL[0][3] was stopped.
09:15:45.375999 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_RSL[1][0] and IPA-BTS1-TRX0-RSL-IPA(1484):IPA_RSL_PORT.
09:15:45.376119 BSC_Tests.ttcn:3698 Port IPA_RSL[1][0] was stopped.
09:15:45.376446 BSC_Tests.ttcn:3698 Port IPA_RSL[1][1] was stopped.
09:15:45.376586 BSC_Tests.ttcn:3698 Port IPA_RSL[1][2] was stopped.
09:15:45.376670 BSC_Tests.ttcn:3698 Port IPA_RSL[1][3] was stopped.
09:15:45.376746 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_RSL[2][0] and IPA-BTS2-TRX0-RSL-IPA(1485):IPA_RSL_PORT.
09:15:45.376869 BSC_Tests.ttcn:3698 Port IPA_RSL[2][0] was stopped.
09:15:45.377012 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_RSL[2][1] and IPA-BTS2-TRX1-RSL-IPA(1486):IPA_RSL_PORT.
09:15:45.377144 BSC_Tests.ttcn:3698 Message with id 3 was extracted from the queue of IPA_RSL[2][1].
09:15:45.377228 BSC_Tests.ttcn:3698 Message with id 4 was extracted from the queue of IPA_RSL[2][1].
09:15:45.377309 BSC_Tests.ttcn:3698 Message with id 5 was extracted from the queue of IPA_RSL[2][1].
09:15:45.377390 BSC_Tests.ttcn:3698 Message with id 6 was extracted from the queue of IPA_RSL[2][1].
09:15:45.377474 BSC_Tests.ttcn:3698 Message with id 7 was extracted from the queue of IPA_RSL[2][1].
09:15:45.377548 BSC_Tests.ttcn:3698 Port IPA_RSL[2][1] was stopped.
09:15:45.377621 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_RSL[2][2] and IPA-BTS2-TRX2-RSL-IPA(1487):IPA_RSL_PORT.
09:15:45.377739 BSC_Tests.ttcn:3698 Message with id 3 was extracted from the queue of IPA_RSL[2][2].
09:15:45.377826 BSC_Tests.ttcn:3698 Message with id 4 was extracted from the queue of IPA_RSL[2][2].
09:15:45.377914 BSC_Tests.ttcn:3698 Message with id 5 was extracted from the queue of IPA_RSL[2][2].
09:15:45.378018 BSC_Tests.ttcn:3698 Message with id 6 was extracted from the queue of IPA_RSL[2][2].
09:15:45.378099 BSC_Tests.ttcn:3698 Message with id 7 was extracted from the queue of IPA_RSL[2][2].
09:15:45.378173 BSC_Tests.ttcn:3698 Port IPA_RSL[2][2] was stopped.
09:15:45.378247 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_RSL[2][3] and IPA-BTS2-TRX3-RSL-IPA(1488):IPA_RSL_PORT.
09:15:45.378388 BSC_Tests.ttcn:3698 Message with id 3 was extracted from the queue of IPA_RSL[2][3].
09:15:45.378510 BSC_Tests.ttcn:3698 Message with id 4 was extracted from the queue of IPA_RSL[2][3].
09:15:45.378584 BSC_Tests.ttcn:3698 Message with id 5 was extracted from the queue of IPA_RSL[2][3].
09:15:45.378663 BSC_Tests.ttcn:3698 Message with id 6 was extracted from the queue of IPA_RSL[2][3].
09:15:45.378740 BSC_Tests.ttcn:3698 Message with id 7 was extracted from the queue of IPA_RSL[2][3].
09:15:45.378813 BSC_Tests.ttcn:3698 Port IPA_RSL[2][3] was stopped.
09:15:45.378888 BSC_Tests.ttcn:3698 Port IPA was stopped.
09:15:45.378961 BSC_Tests.ttcn:3698 Port SCCPLITE_IPA_CTRL was stopped.
09:15:45.379033 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_CFG_PORT[0][0] and IPA-BTS0-TRX0-RSL-IPA(1483):CFG_PORT.
09:15:45.379140 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[0][0] was stopped.
09:15:45.379222 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[0][1] was stopped.
09:15:45.379293 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[0][2] was stopped.
09:15:45.379364 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[0][3] was stopped.
09:15:45.379437 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_CFG_PORT[1][0] and IPA-BTS1-TRX0-RSL-IPA(1484):CFG_PORT.
09:15:45.379544 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[1][0] was stopped.
09:15:45.379624 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[1][1] was stopped.
09:15:45.379698 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[1][2] was stopped.
09:15:45.379770 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[1][3] was stopped.
09:15:45.379842 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_CFG_PORT[2][0] and IPA-BTS2-TRX0-RSL-IPA(1485):CFG_PORT.
09:15:45.379949 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[2][0] was stopped.
09:15:45.380023 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_CFG_PORT[2][1] and IPA-BTS2-TRX1-RSL-IPA(1486):CFG_PORT.
09:15:45.380143 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[2][1] was stopped.
09:15:45.380225 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_CFG_PORT[2][2] and IPA-BTS2-TRX2-RSL-IPA(1487):CFG_PORT.
09:15:45.380347 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[2][2] was stopped.
09:15:45.380424 BSC_Tests.ttcn:3698 Removing unterminated connection between port IPA_CFG_PORT[2][3] and IPA-BTS2-TRX3-RSL-IPA(1488):CFG_PORT.
09:15:45.380540 BSC_Tests.ttcn:3698 Port IPA_CFG_PORT[2][3] was stopped.
09:15:45.380618 BSC_Tests.ttcn:3698 Removing unterminated mapping between port BSCVTY and system:BSCVTY.
09:15:45.380780 BSC_Tests.ttcn:3698 Port BSCVTY was unmapped from system:BSCVTY.
09:15:45.380889 BSC_Tests.ttcn:3698 Port BSCVTY was stopped.
09:15:45.380969 BSC_Tests.ttcn:3698 Port STPVTY was stopped.
09:15:45.381044 BSC_Tests.ttcn:3698 Port SCCPLITE_IPA_CFG_PORT[0] was stopped.
09:15:45.381120 BSC_Tests.ttcn:3698 Port SCCPLITE_IPA_CFG_PORT[1] was stopped.
09:15:45.381194 BSC_Tests.ttcn:3698 Port SCCPLITE_IPA_CFG_PORT[2] was stopped.
09:15:45.381268 BSC_Tests.ttcn:3698 Removing unterminated connection between port BSSAP and VirtMSC-SCCP(1477):SCCP_SP_PORT.
09:15:45.381384 BSC_Tests.ttcn:3698 Port BSSAP was stopped.
09:15:45.381466 BSC_Tests.ttcn:3698 Removing unterminated connection between port BSSAP_LE and VirtSMLC-SCCP(1479):SCCP_SP_PORT.
09:15:45.381581 BSC_Tests.ttcn:3698 Port BSSAP_LE was stopped.
09:15:45.381663 BSC_Tests.ttcn:3698 Component type BSC_Tests.test_CT was shut down inside testcase TC_paging_imsi_nochan_cgi_unknown_cid.
09:15:45.381746 BSC_Tests.ttcn:3698 Waiting for PTCs to finish.
09:15:45.386858 BSC_Tests.ttcn:3698 Setting final verdict of the test case.
09:15:45.387076 BSC_Tests.ttcn:3698 Local verdict of MTC: pass
09:15:45.387302 BSC_Tests.ttcn:3698 Local verdict of PTC VirtMSC-STATS(1476): none (pass -> pass)
09:15:45.387473 BSC_Tests.ttcn:3698 Local verdict of PTC VirtMSC-SCCP(1477): none (pass -> pass)
09:15:45.387998 BSC_Tests.ttcn:3698 Local verdict of PTC VirtMSC-M3UA(1478): none (pass -> pass)
09:15:45.388269 BSC_Tests.ttcn:3698 Local verdict of PTC VirtSMLC-SCCP(1479): none (pass -> pass)
09:15:45.388505 BSC_Tests.ttcn:3698 Local verdict of PTC VirtSMLC-M3UA(1480): none (pass -> pass)
09:15:45.388830 BSC_Tests.ttcn:3698 Local verdict of PTC IPA-CTRL-CLI-IPA(1481): none (pass -> pass)
09:15:45.388997 BSC_Tests.ttcn:3698 Local verdict of PTC VirtMGW-MGCP-0(1482): none (pass -> pass)
09:15:45.389099 BSC_Tests.ttcn:3698 Local verdict of PTC IPA-BTS0-TRX0-RSL-IPA(1483): none (pass -> pass)
09:15:45.389207 BSC_Tests.ttcn:3698 Local verdict of PTC IPA-BTS1-TRX0-RSL-IPA(1484): none (pass -> pass)
09:15:45.389433 BSC_Tests.ttcn:3698 Local verdict of PTC IPA-BTS2-TRX0-RSL-IPA(1485): none (pass -> pass)
09:15:45.389775 BSC_Tests.ttcn:3698 Local verdict of PTC IPA-BTS2-TRX1-RSL-IPA(1486): none (pass -> pass)
09:15:45.390053 BSC_Tests.ttcn:3698 Local verdict of PTC IPA-BTS2-TRX2-RSL-IPA(1487): none (pass -> pass)
09:15:45.390284 BSC_Tests.ttcn:3698 Local verdict of PTC IPA-BTS2-TRX3-RSL-IPA(1488): none (pass -> pass)
09:15:45.390589 BSC_Tests.ttcn:3698 Test case TC_paging_imsi_nochan_cgi_unknown_cid finished. Verdict: pass
09:15:45.390786 BSC_Tests.ttcn:3698 Starting external command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_paging_imsi_nochan_cgi_unknown_cid pass'.
09:15:50.373134 BSC_Tests.ttcn:3698 External command `/home/osmocom-build/jenkins/workspace/ttcn3-bsc-test/ttcn3-tcpdump-stop.sh BSC_Tests.TC_paging_imsi_nochan_cgi_unknown_cid pass' was executed successfully (exit status: 0).
09:15:50.373225 BSC_Tests.ttcn:3829 Switching to log file `BSC_Tests-TC_paging_imsi_a_reset-d5b21e48044a-mtc-9786.log'
