09:28:29.695501 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:28:29.695559 - TTCN-3 Parallel Test Component started on d5b21e48044a. Component reference: VirtMSC-RAN(2014), component type: RAN_Emulation.RAN_Emulation_CT, component name: VirtMSC-RAN. Version: 11.1.0.
09:28:29.695586 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING | DEBUG; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:28:29.695645 - Connected to MC.
09:28:29.695663 - Initializing variables, timers and ports of component type RAN_Emulation.RAN_Emulation_CT inside testcase TC_ho_in_fail_mgw_mdcx_timeout.
09:28:29.696931 - Port BSSAP was started.
09:28:29.696956 - Port CLIENT was started.
09:28:29.696969 - Port MGCP was started.
09:28:29.696980 - Port CTRL was started.
09:28:29.696992 - Port CTRL_CLIENT was started.
09:28:29.697003 - Port PROC was started.
09:28:29.697014 - Component type RAN_Emulation.RAN_Emulation_CT was initialized.
09:28:29.697052 - Port BSSAP has established the connection with VirtMSC-SCCP(2012):SCCP_SP_PORT using transport type UNIX.
09:28:29.697660 - Starting function main({ create_cb := refers(RAN_Emulation.ExpectedCreateCallback), unitdata_cb := refers(MSC_ConnectionHandler.UnitdataCallback), decode_dtap := false, role_ms := false, protocol := RAN_PROTOCOL_BSSAP (0), transport := BSSAP_TRANSPORT_AoIP (0), use_osmux := false, bssap_reset_retries := 1, sccp_addr_local := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sccp_addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit } }, "").
09:28:29.699787 RAN_Emulation.ttcnpp:600 Sent on BSSAP to VirtMSC-SCCP(2012) @BSSAP_CodecPort.BSSAP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit }
09:28:29.699875 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { reset := { messageType := '30'O ("0"), cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
09:28:29.700222 BSSAP_CodecPort.ttcn:349 enc_PDU_BSSAP(): Stream after encoding: '000430040100'O
09:28:29.700342 RAN_Emulation.ttcnpp:600 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_UNITDATA_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := omit, returnOption := omit, userData := '000430040100'O, importance := omit }
09:28:29.700687 RAN_Emulation.ttcnpp:601 Start timer T: 5 s
09:28:29.700953 RAN_Emulation.ttcnpp:602 Port CTRL_CLIENT has established the connection with mtc:SCCPLITE_IPA_CTRL using transport type UNIX.
09:28:29.901002 RAN_Emulation.ttcnpp:602 Message enqueued on BSSAP from VirtMSC-SCCP(2012) @SCCPasp_Types.ASP_SCCP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := '000131'O, importance := omit } id 1
09:28:29.901059 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Stream before decoding: '000131'O
09:28:29.906221 BSSAP_CodecPort.ttcn:281 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }
09:28:29.906475 RAN_Emulation.ttcnpp:602 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
09:28:29.906628 RAN_Emulation.ttcnpp:603 Matching on port BSSAP succeeded:  matched
09:28:29.906656 RAN_Emulation.ttcnpp:603 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(2012): @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, sequenceControl := '00000000'B, returnOption := '00000000'B, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { resetAck := { messageType := '31'O ("1"), a_InterfaceSelectorForReset := omit, osmuxSupport := omit } } } }, importance := omit } id 1
09:28:29.906670 RAN_Emulation.ttcnpp:603 Message with id 1 was extracted from the queue of BSSAP.
09:28:29.906690 RAN_Emulation.ttcnpp:604 BSSMAP: Received RESET-ACK in response to RESET, we're ready to go!
09:28:33.067408 RAN_Emulation.ttcnpp:1377 Port PROC is waiting for connection from TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN on UNIX pathname /tmp/ttcn3-portconn-3105b1db.
09:28:33.069255 RAN_Emulation.ttcnpp:1377 Port PROC has accepted the connection from TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN.
09:28:33.069739 RAN_Emulation.ttcnpp:1377 Port CLIENT is waiting for connection from TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN_CONN on UNIX pathname /tmp/ttcn3-portconn-744cb597.
09:28:33.069779 RAN_Emulation.ttcnpp:1377 Port CLIENT has accepted the connection from TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN_CONN.
09:28:34.100030 RAN_Emulation.ttcnpp:1377 Message enqueued on CLIENT from TC_ho_in_fail_mgw_mdcx_timeout(2022) @RAN_Emulation.BSSAP_Conn_Req : { addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, addr_own := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, bssap := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { handoverRequest := { messageType := '10'O, channelType := { elementIdentifier := '0B'O ("\v"), lengthIndicator := 0, speechOrDataIndicator := '0001'B, spare1_4 := '0000'B, channelRateAndType := '08'O ("\b"), speechId_DataIndicator := '01'O }, encryptionInformation := { elementIdentifier := '0A'O ("\n"), lengthIndicator := 0, permittedAlgorithms := '01'O, key := '0000000000000000'O }, classmarkInformationType := { classmarkInformationType1 := { elementIdentifier := '1D'O, rf_PowerCapability := '000'B, a5_1 := '0'B, esind := '0'B, revisionLevel := '10'B, spare1_1 := '0'B } }, cellIdentifierSource := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0001'O } } }, priority := omit, circuitIdentityCode := omit, downLinkDTX_Flag := omit, cellIdentifierTarget := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0000'O } } }, interferenceBandToBeUsed := omit, cause := omit, classmarkInformationType3 := omit, currentChannelType1 := omit, speechVersion := omit, groupCallReference := omit, talkerFlag := omit, configurationEvolutionIndication := omit, chosenEncryptionAlgorithm := omit, oldToNewBSSInfo := omit, lSAInformation := omit, lSAAccessControlSuppression := omit, serviceHandover := omit, iMSI_bssmap := omit, sourceToTargetRNCTransparentInfo := omit, sourceToTargetRNCTransparentInfoCDMA := omit, sNAAccessInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '01020304'O }, uDPPortValue := 2342 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 0, codecElements := { { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '11111111'B, s8_15 := '01010111'B }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00111111'B, s8_15 := '00000111'B }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, callIdentifier := omit, kC128 := omit, globalCallReference := omit, lCLS_Configuration := omit, connectionStatusControl := omit } } } } } id 1
09:28:34.100605 RAN_Emulation.ttcnpp:1020 Matching on port CLIENT failed: Type of the first message in the queue is not @BSSAP_Types.PDU_BSSAP.
09:28:34.100642 RAN_Emulation.ttcnpp:1026 Matching on port CLIENT failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_UNITDATA_req.
09:28:34.100680 RAN_Emulation.ttcnpp:1031 Matching on port CLIENT failed: Type of the first message in the queue is not @RAN_Emulation.RAN_Conn_Prim.
09:28:34.100807 RAN_Emulation.ttcnpp:1038 Matching on port CLIENT succeeded:  matched
09:28:34.100901 RAN_Emulation.ttcnpp:1038 Receive operation on port CLIENT succeeded, message from TC_ho_in_fail_mgw_mdcx_timeout(2022): @RAN_Emulation.BSSAP_Conn_Req : { addr_peer := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, addr_own := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, bssap := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { handoverRequest := { messageType := '10'O, channelType := { elementIdentifier := '0B'O ("\v"), lengthIndicator := 0, speechOrDataIndicator := '0001'B, spare1_4 := '0000'B, channelRateAndType := '08'O ("\b"), speechId_DataIndicator := '01'O }, encryptionInformation := { elementIdentifier := '0A'O ("\n"), lengthIndicator := 0, permittedAlgorithms := '01'O, key := '0000000000000000'O }, classmarkInformationType := { classmarkInformationType1 := { elementIdentifier := '1D'O, rf_PowerCapability := '000'B, a5_1 := '0'B, esind := '0'B, revisionLevel := '10'B, spare1_1 := '0'B } }, cellIdentifierSource := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0001'O } } }, priority := omit, circuitIdentityCode := omit, downLinkDTX_Flag := omit, cellIdentifierTarget := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0000'O } } }, interferenceBandToBeUsed := omit, cause := omit, classmarkInformationType3 := omit, currentChannelType1 := omit, speechVersion := omit, groupCallReference := omit, talkerFlag := omit, configurationEvolutionIndication := omit, chosenEncryptionAlgorithm := omit, oldToNewBSSInfo := omit, lSAInformation := omit, lSAAccessControlSuppression := omit, serviceHandover := omit, iMSI_bssmap := omit, sourceToTargetRNCTransparentInfo := omit, sourceToTargetRNCTransparentInfoCDMA := omit, sNAAccessInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '01020304'O }, uDPPortValue := 2342 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 0, codecElements := { { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '11111111'B, s8_15 := '01010111'B }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00111111'B, s8_15 := '00000111'B }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, callIdentifier := omit, kC128 := omit, globalCallReference := omit, lCLS_Configuration := omit, connectionStatusControl := omit } } } } } id 1
09:28:34.100991 RAN_Emulation.ttcnpp:1038 Message with id 1 was extracted from the queue of CLIENT.
09:28:34.101101 RAN_Emulation.ttcnpp:431 Random number generator was initialized with seed 2832.101100: srand48(-257528254).
09:28:34.101151 RAN_Emulation.ttcnpp:431 Function rnd() returned 0.041010.
09:28:34.101265 RAN_Emulation.ttcnpp:468 Added conn table entry 0TC_ho_in_fail_mgw_mdcx_timeout(2022)688032
09:28:34.103283 RAN_Emulation.ttcnpp:1049 Sent on BSSAP to VirtMSC-SCCP(2012) @BSSAP_CodecPort.BSSAP_N_CONNECT_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, expeditedDataSel := omit, qualityOfService := omit, userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { handoverRequest := { messageType := '10'O, channelType := { elementIdentifier := '0B'O ("\v"), lengthIndicator := 0, speechOrDataIndicator := '0001'B, spare1_4 := '0000'B, channelRateAndType := '08'O ("\b"), speechId_DataIndicator := '01'O }, encryptionInformation := { elementIdentifier := '0A'O ("\n"), lengthIndicator := 0, permittedAlgorithms := '01'O, key := '0000000000000000'O }, classmarkInformationType := { classmarkInformationType1 := { elementIdentifier := '1D'O, rf_PowerCapability := '000'B, a5_1 := '0'B, esind := '0'B, revisionLevel := '10'B, spare1_1 := '0'B } }, cellIdentifierSource := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0001'O } } }, priority := omit, circuitIdentityCode := omit, downLinkDTX_Flag := omit, cellIdentifierTarget := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0000'O } } }, interferenceBandToBeUsed := omit, cause := omit, classmarkInformationType3 := omit, currentChannelType1 := omit, speechVersion := omit, groupCallReference := omit, talkerFlag := omit, configurationEvolutionIndication := omit, chosenEncryptionAlgorithm := omit, oldToNewBSSInfo := omit, lSAInformation := omit, lSAAccessControlSuppression := omit, serviceHandover := omit, iMSI_bssmap := omit, sourceToTargetRNCTransparentInfo := omit, sourceToTargetRNCTransparentInfoCDMA := omit, sNAAccessInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '01020304'O }, uDPPortValue := 2342 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 0, codecElements := { { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '11111111'B, s8_15 := '01010111'B }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00111111'B, s8_15 := '00000111'B }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, callIdentifier := omit, kC128 := omit, globalCallReference := omit, lCLS_Configuration := omit, connectionStatusControl := omit } } } }, connectionId := 688032, importance := omit }
09:28:34.103376 BSSAP_CodecPort.ttcn:303 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { handoverRequest := { messageType := '10'O, channelType := { elementIdentifier := '0B'O ("\v"), lengthIndicator := 0, speechOrDataIndicator := '0001'B, spare1_4 := '0000'B, channelRateAndType := '08'O ("\b"), speechId_DataIndicator := '01'O }, encryptionInformation := { elementIdentifier := '0A'O ("\n"), lengthIndicator := 0, permittedAlgorithms := '01'O, key := '0000000000000000'O }, classmarkInformationType := { classmarkInformationType1 := { elementIdentifier := '1D'O, rf_PowerCapability := '000'B, a5_1 := '0'B, esind := '0'B, revisionLevel := '10'B, spare1_1 := '0'B } }, cellIdentifierSource := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0001'O } } }, priority := omit, circuitIdentityCode := omit, downLinkDTX_Flag := omit, cellIdentifierTarget := { elementIdentifier := '05'O, lengthIndicator := 0, cellIdentifierDiscriminator := '0000'B, spare1_4 := '0000'B, cellIdentification := { cI_LAC_CI := { lac := '0001'O, ci := '0000'O } } }, interferenceBandToBeUsed := omit, cause := omit, classmarkInformationType3 := omit, currentChannelType1 := omit, speechVersion := omit, groupCallReference := omit, talkerFlag := omit, configurationEvolutionIndication := omit, chosenEncryptionAlgorithm := omit, oldToNewBSSInfo := omit, lSAInformation := omit, lSAAccessControlSuppression := omit, serviceHandover := omit, iMSI_bssmap := omit, sourceToTargetRNCTransparentInfo := omit, sourceToTargetRNCTransparentInfoCDMA := omit, sNAAccessInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '01020304'O }, uDPPortValue := 2342 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 0, codecElements := { { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '11111111'B, s8_15 := '01010111'B }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00111111'B, s8_15 := '00000111'B }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, callIdentifier := omit, kC128 := omit, globalCallReference := omit, lCLS_Configuration := omit, connectionStatusControl := omit } } } }
09:28:34.104124 BSSAP_CodecPort.ttcn:303 enc_PDU_BSSAP(): Stream after encoding: '0034100B030108010A090100000000000000001D4005050100010001050501000100007C060102030409267D0983FF57843F07828081'O
09:28:34.104227 RAN_Emulation.ttcnpp:1049 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_CONNECT_req : { calledAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111011'B, subsystemNumber := 254, globalTitle := omit }, callingAddress := { addressIndicator := { pointCodeIndic := '1'B, ssnIndicator := '1'B, globalTitleIndic := '0000'B, routingIndicator := '1'B }, signPointCode := '00000010111001'B, subsystemNumber := 254, globalTitle := omit }, expeditedDataSel := omit, qualityOfService := omit, userData := '0034100B030108010A090100000000000000001D4005050100010001050501000100007C060102030409267D0983FF57843F07828081'O, connectionId := 688032, importance := omit }
09:28:34.106213 RAN_Emulation.ttcnpp:1377 Message enqueued on BSSAP from VirtMSC-SCCP(2012) @SCCPasp_Types.ASP_SCCP_N_CONNECT_cfm : { respondingAddress := omit, qualityOfService := omit, userData := omit, connectionId := 688032, importance := omit } id 2
09:28:34.106369 RAN_Emulation.ttcnpp:1377 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_CONNECT_cfm : { respondingAddress := omit, qualityOfService := omit, userData := omit, connectionId := 688032, importance := omit } id 2
09:28:34.106505 RAN_Emulation.ttcnpp:972 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind.
09:28:34.106653 RAN_Emulation.ttcnpp:982 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_CONNECT_ind.
09:28:34.106698 RAN_Emulation.ttcnpp:992 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_DATA_ind.
09:28:34.106845 RAN_Emulation.ttcnpp:999 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_DISCONNECT_ind.
09:28:34.106892 RAN_Emulation.ttcnpp:1011 Matching on port BSSAP succeeded:  matched
09:28:34.106935 RAN_Emulation.ttcnpp:1011 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(2012): @BSSAP_CodecPort.BSSAP_N_CONNECT_cfm : { respondingAddress := omit, qualityOfService := omit, userData := omit, connectionId := 688032, importance := omit } id 2
09:28:34.106993 RAN_Emulation.ttcnpp:1011 Message with id 2 was extracted from the queue of BSSAP.
09:28:34.107364 RAN_Emulation.ttcnpp:1014 Sent on CLIENT to TC_ho_in_fail_mgw_mdcx_timeout(2022) @RAN_Emulation.RAN_Conn_Prim : { conf_ind := { } }
09:28:34.135574 RAN_Emulation.ttcnpp:1377 Message enqueued on BSSAP from VirtMSC-SCCP(2012) @SCCPasp_Types.ASP_SCCP_N_DATA_ind : { userData := '002C12170D062BCA670943671A07D063019021982C0140017C067F0000052AFA7D098082830457818404077E0180'O, connectionId := 688032, importance := omit } id 3
09:28:34.135604 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Stream before decoding: '002C12170D062BCA670943671A07D063019021982C0140017C067F0000052AFA7D098082830457818404077E0180'O
09:28:34.136831 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 44, pdu := { bssmap := { handoverRequestAck := { messageType := '12'O, layer3Information := { elementIdentifier := '17'O, lengthIndicator := 13, layer3info := '062BCA670943671A07D0630190'O }, chosenChannel := { elementIdentifier := '21'O ("!"), channel := '1000'B, channelMode := '1001'B }, chosenEncryptionAlgorithm := { elementIdentifier := '2C'O (","), algorithmIdentifier := '01'O }, circuitPool := omit, speechVersion := { elementIdentifier := '40'O ("@"), speechVersionIdentifier := '0000001'B, spare1_1 := '0'B }, circuitIdentityCode := omit, lSAIdentifier := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '7F000005'O }, uDPPortValue := 11002 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 9, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '01010111'B }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '00000111'B } } }, speechCodec := { elementIdentifier := '7E'O ("~"), lengthIndicator := 1, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, lCLS_bSS_Status := omit } } } }
09:28:34.137105 RAN_Emulation.ttcnpp:1377 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 44, pdu := { bssmap := { handoverRequestAck := { messageType := '12'O, layer3Information := { elementIdentifier := '17'O, lengthIndicator := 13, layer3info := '062BCA670943671A07D0630190'O }, chosenChannel := { elementIdentifier := '21'O ("!"), channel := '1000'B, channelMode := '1001'B }, chosenEncryptionAlgorithm := { elementIdentifier := '2C'O (","), algorithmIdentifier := '01'O }, circuitPool := omit, speechVersion := { elementIdentifier := '40'O ("@"), speechVersionIdentifier := '0000001'B, spare1_1 := '0'B }, circuitIdentityCode := omit, lSAIdentifier := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '7F000005'O }, uDPPortValue := 11002 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 9, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '01010111'B }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '00000111'B } } }, speechCodec := { elementIdentifier := '7E'O ("~"), lengthIndicator := 1, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, lCLS_bSS_Status := omit } } } }, connectionId := 688032, importance := omit } id 3
09:28:34.137140 RAN_Emulation.ttcnpp:972 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind.
09:28:34.137155 RAN_Emulation.ttcnpp:982 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_CONNECT_ind.
09:28:34.137178 RAN_Emulation.ttcnpp:992 Matching on port BSSAP succeeded:  matched
09:28:34.137204 RAN_Emulation.ttcnpp:992 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(2012): @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 44, pdu := { bssmap := { handoverRequestAck := { messageType := '12'O, layer3Information := { elementIdentifier := '17'O, lengthIndicator := 13, layer3info := '062BCA670943671A07D0630190'O }, chosenChannel := { elementIdentifier := '21'O ("!"), channel := '1000'B, channelMode := '1001'B }, chosenEncryptionAlgorithm := { elementIdentifier := '2C'O (","), algorithmIdentifier := '01'O }, circuitPool := omit, speechVersion := { elementIdentifier := '40'O ("@"), speechVersionIdentifier := '0000001'B, spare1_1 := '0'B }, circuitIdentityCode := omit, lSAIdentifier := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '7F000005'O }, uDPPortValue := 11002 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 9, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '01010111'B }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '00000111'B } } }, speechCodec := { elementIdentifier := '7E'O ("~"), lengthIndicator := 1, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, lCLS_bSS_Status := omit } } } }, connectionId := 688032, importance := omit } id 3
09:28:34.137222 RAN_Emulation.ttcnpp:992 Message with id 3 was extracted from the queue of BSSAP.
09:28:34.137290 RAN_Emulation.ttcnpp:547 Sent on CLIENT to TC_ho_in_fail_mgw_mdcx_timeout(2022) @BSSAP_Types.PDU_BSSAP : { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 44, pdu := { bssmap := { handoverRequestAck := { messageType := '12'O, layer3Information := { elementIdentifier := '17'O, lengthIndicator := 13, layer3info := '062BCA670943671A07D0630190'O }, chosenChannel := { elementIdentifier := '21'O ("!"), channel := '1000'B, channelMode := '1001'B }, chosenEncryptionAlgorithm := { elementIdentifier := '2C'O (","), algorithmIdentifier := '01'O }, circuitPool := omit, speechVersion := { elementIdentifier := '40'O ("@"), speechVersionIdentifier := '0000001'B, spare1_1 := '0'B }, circuitIdentityCode := omit, lSAIdentifier := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, aoIPTransportLayer := { elementIdentifier := '7C'O ("|"), lengthIndicator := 6, ipAddress := { ipv4 := '7F000005'O }, uDPPortValue := 11002 }, codecList := { elementIdentifier := '7D'O ("}"), lengthIndicator := 9, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := GSM_EFR (2), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := FR_AMR (3), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '01010111'B }, { codecType := GSM_HR (1), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit }, { codecType := HR_AMR (4), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := '00000100'B, s8_15 := '00000111'B } } }, speechCodec := { elementIdentifier := '7E'O ("~"), lengthIndicator := 1, codecElements := { { codecType := GSM_FR (0), tF := '0'B, pT := '0'B, pI := '0'B, fI := '1'B, extendedCodecType := omit, s0_7 := omit, s8_15 := omit } } }, lCLS_bSS_Status := omit } } } }
09:28:37.114086 RAN_Emulation.ttcnpp:1377 Message enqueued on BSSAP from VirtMSC-SCCP(2012) @SCCPasp_Types.ASP_SCCP_N_DATA_ind : { userData := '000416040100'O, connectionId := 688032, importance := omit } id 4
09:28:37.114146 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Stream before decoding: '000416040100'O
09:28:37.114442 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { handoverFailure := { messageType := '16'O, cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, rR_Cause := omit, circuitPool := omit, circuitPoolList := omit, gERANClassmark := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, codecList := omit } } } }
09:28:37.114704 RAN_Emulation.ttcnpp:1377 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { handoverFailure := { messageType := '16'O, cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, rR_Cause := omit, circuitPool := omit, circuitPoolList := omit, gERANClassmark := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, codecList := omit } } } }, connectionId := 688032, importance := omit } id 4
09:28:37.114743 RAN_Emulation.ttcnpp:972 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind.
09:28:37.114762 RAN_Emulation.ttcnpp:982 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_CONNECT_ind.
09:28:37.114782 RAN_Emulation.ttcnpp:992 Matching on port BSSAP succeeded:  matched
09:28:37.114804 RAN_Emulation.ttcnpp:992 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(2012): @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { handoverFailure := { messageType := '16'O, cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, rR_Cause := omit, circuitPool := omit, circuitPoolList := omit, gERANClassmark := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, codecList := omit } } } }, connectionId := 688032, importance := omit } id 4
09:28:37.114826 RAN_Emulation.ttcnpp:992 Message with id 4 was extracted from the queue of BSSAP.
09:28:37.114844 RAN_Emulation.ttcnpp:547 Sent on CLIENT to TC_ho_in_fail_mgw_mdcx_timeout(2022) @BSSAP_Types.PDU_BSSAP : { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { handoverFailure := { messageType := '16'O, cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, rR_Cause := omit, circuitPool := omit, circuitPoolList := omit, gERANClassmark := omit, newBSSToOldBSSInfo := omit, interSystemInformation := omit, talkerPriority := omit, codecList := omit } } } }
09:28:37.114960 RAN_Emulation.ttcnpp:1377 Message enqueued on BSSAP from VirtMSC-SCCP(2012) @SCCPasp_Types.ASP_SCCP_N_DATA_ind : { userData := '000422040120'O, connectionId := 688032, importance := omit } id 5
09:28:37.114976 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Stream before decoding: '000422040120'O
09:28:37.115047 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { clearRequest := { messageType := '22'O ("\""), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit } } } } }
09:28:37.115084 RAN_Emulation.ttcnpp:1377 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { clearRequest := { messageType := '22'O ("\""), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit } } } } }, connectionId := 688032, importance := omit } id 5
09:28:37.115099 RAN_Emulation.ttcnpp:972 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind.
09:28:37.115149 RAN_Emulation.ttcnpp:982 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_CONNECT_ind.
09:28:37.115182 RAN_Emulation.ttcnpp:992 Matching on port BSSAP succeeded:  matched
09:28:37.115199 RAN_Emulation.ttcnpp:992 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(2012): @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { clearRequest := { messageType := '22'O ("\""), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit } } } } }, connectionId := 688032, importance := omit } id 5
09:28:37.115212 RAN_Emulation.ttcnpp:992 Message with id 5 was extracted from the queue of BSSAP.
09:28:37.115230 RAN_Emulation.ttcnpp:547 Sent on CLIENT to TC_ho_in_fail_mgw_mdcx_timeout(2022) @BSSAP_Types.PDU_BSSAP : { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 4, pdu := { bssmap := { clearRequest := { messageType := '22'O ("\""), cause := { elementIdentifier := '04'O, lengthIndicator := 1, causeValue := '0100000'B, extensionCauseValue := '0'B, spare1 := omit } } } } }
09:28:38.156518 RAN_Emulation.ttcnpp:1377 Message enqueued on CLIENT from TC_ho_in_fail_mgw_mdcx_timeout(2022) @BSSAP_Types.PDU_BSSAP : { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { clearCommand := { messageType := '20'O (" "), layer3HeaderInfo := omit, cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, cSFB_Indication := omit } } } } id 2
09:28:38.157297 RAN_Emulation.ttcnpp:1020 Matching on port CLIENT succeeded:  matched
09:28:38.157639 RAN_Emulation.ttcnpp:1020 Receive operation on port CLIENT succeeded, message from TC_ho_in_fail_mgw_mdcx_timeout(2022): @BSSAP_Types.PDU_BSSAP : { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { clearCommand := { messageType := '20'O (" "), layer3HeaderInfo := omit, cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, cSFB_Indication := omit } } } } id 2
09:28:38.157984 RAN_Emulation.ttcnpp:1020 Message with id 2 was extracted from the queue of CLIENT.
09:28:38.158746 RAN_Emulation.ttcnpp:1023 Sent on BSSAP to VirtMSC-SCCP(2012) @BSSAP_CodecPort.BSSAP_N_DATA_req : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { clearCommand := { messageType := '20'O (" "), layer3HeaderInfo := omit, cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, cSFB_Indication := omit } } } }, connectionId := 688032, importance := omit }
09:28:38.158925 BSSAP_CodecPort.ttcn:327 enc_PDU_BSSAP(): Encoding @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 0, pdu := { bssmap := { clearCommand := { messageType := '20'O (" "), layer3HeaderInfo := omit, cause := { elementIdentifier := '04'O, lengthIndicator := 0, causeValue := '0000000'B, extensionCauseValue := '0'B, spare1 := omit }, cSFB_Indication := omit } } } }
09:28:38.159295 BSSAP_CodecPort.ttcn:327 enc_PDU_BSSAP(): Stream after encoding: '000420040100'O
09:28:38.159448 RAN_Emulation.ttcnpp:1023 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_DATA_req : { userData := '000420040100'O, connectionId := 688032, importance := omit }
09:28:38.162661 RAN_Emulation.ttcnpp:1377 Message enqueued on BSSAP from VirtMSC-SCCP(2012) @SCCPasp_Types.ASP_SCCP_N_DATA_ind : { userData := '000121'O, connectionId := 688032, importance := omit } id 6
09:28:38.162836 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Stream before decoding: '000121'O
09:28:38.163083 BSSAP_CodecPort.ttcn:256 dec_PDU_BSSAP(): Decoded @BSSAP_Types.PDU_BSSAP: { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { clearComplete := { messageType := '21'O ("!") } } } }
09:28:38.163237 RAN_Emulation.ttcnpp:1377 Incoming message was mapped to @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { clearComplete := { messageType := '21'O ("!") } } } }, connectionId := 688032, importance := omit } id 6
09:28:38.163324 RAN_Emulation.ttcnpp:972 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_UNITDATA_ind.
09:28:38.163389 RAN_Emulation.ttcnpp:982 Matching on port BSSAP failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_CONNECT_ind.
09:28:38.163456 RAN_Emulation.ttcnpp:992 Matching on port BSSAP succeeded:  matched
09:28:38.163529 RAN_Emulation.ttcnpp:992 Receive operation on port BSSAP succeeded, message from VirtMSC-SCCP(2012): @BSSAP_CodecPort.BSSAP_N_DATA_ind : { userData := { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { clearComplete := { messageType := '21'O ("!") } } } }, connectionId := 688032, importance := omit } id 6
09:28:38.163599 RAN_Emulation.ttcnpp:992 Message with id 6 was extracted from the queue of BSSAP.
09:28:38.163669 RAN_Emulation.ttcnpp:547 Sent on CLIENT to TC_ho_in_fail_mgw_mdcx_timeout(2022) @BSSAP_Types.PDU_BSSAP : { discriminator := '0'B, spare := '0000000'B, dlci := omit, lengthIndicator := 1, pdu := { bssmap := { clearComplete := { messageType := '21'O ("!") } } } }
09:28:38.166292 RAN_Emulation.ttcnpp:1377 Message enqueued on CLIENT from TC_ho_in_fail_mgw_mdcx_timeout(2022) @RAN_Emulation.RAN_Conn_Prim : { disc_req := { reason := 0 } } id 3
09:28:38.166535 RAN_Emulation.ttcnpp:1020 Matching on port CLIENT failed: Type of the first message in the queue is not @BSSAP_Types.PDU_BSSAP.
09:28:38.166602 RAN_Emulation.ttcnpp:1026 Matching on port CLIENT failed: Type of the first message in the queue is not @BSSAP_CodecPort.BSSAP_N_UNITDATA_req.
09:28:38.166828 RAN_Emulation.ttcnpp:1031 Matching on port CLIENT succeeded:  matched
09:28:38.166930 RAN_Emulation.ttcnpp:1031 Receive operation on port CLIENT succeeded, message from TC_ho_in_fail_mgw_mdcx_timeout(2022): @RAN_Emulation.RAN_Conn_Prim : { disc_req := { reason := 0 } } id 3
09:28:38.166987 RAN_Emulation.ttcnpp:1031 Message with id 3 was extracted from the queue of CLIENT.
09:28:38.167232 RAN_Emulation.ttcnpp:1033 Sent on BSSAP to VirtMSC-SCCP(2012) @BSSAP_CodecPort.BSSAP_N_DISCONNECT_req : { respondingAddress := omit, reason := 0, userData := omit, connectionId := 688032, importance := omit }
09:28:38.167379 RAN_Emulation.ttcnpp:1033 Outgoing message was mapped to @SCCPasp_Types.ASP_SCCP_N_DISCONNECT_req : { respondingAddress := omit, reason := 0, userData := omit, connectionId := 688032, importance := omit }
09:28:38.168227 RAN_Emulation.ttcnpp:480 Deleted conn table entry 0TC_ho_in_fail_mgw_mdcx_timeout(2022)688032
09:28:38.169654 RAN_Emulation.ttcnpp:1377 Connection of port CLIENT to TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN_CONN was closed unexpectedly by the peer.
09:28:38.169733 RAN_Emulation.ttcnpp:1377 Port CLIENT was disconnected from TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN_CONN.
09:28:38.170210 RAN_Emulation.ttcnpp:1377 Connection of port PROC to TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN was closed unexpectedly by the peer.
09:28:38.170272 RAN_Emulation.ttcnpp:1377 Port PROC was disconnected from TC_ho_in_fail_mgw_mdcx_timeout(2022):RAN.
09:28:38.305810 RAN_Emulation.ttcnpp:1377 Stop was requested from MC.
09:28:38.305927 RAN_Emulation.ttcnpp:1377 Stopping test component execution.
09:28:38.306185 - Function main was stopped. PTC remains alive and is waiting for next start.
09:28:38.307925 - Connection of port CTRL_CLIENT to mtc:SCCPLITE_IPA_CTRL was closed unexpectedly by the peer.
09:28:38.307945 - Port CTRL_CLIENT was disconnected from mtc:SCCPLITE_IPA_CTRL.
09:28:38.308184 - Kill was requested from MC. Terminating idle PTC.
09:28:38.308199 - Terminating component type RAN_Emulation.RAN_Emulation_CT.
09:28:38.308209 - Removing unterminated connection between port BSSAP and VirtMSC-SCCP(2012):SCCP_SP_PORT.
09:28:38.308225 - Port BSSAP was stopped.
09:28:38.308303 - Port CLIENT was stopped.
09:28:38.308396 - Port MGCP was stopped.
09:28:38.308428 - Port CTRL was stopped.
09:28:38.308487 - Port CTRL_CLIENT was stopped.
09:28:38.308547 - Port PROC was stopped.
09:28:38.308648 - Component type RAN_Emulation.RAN_Emulation_CT was shut down inside testcase TC_ho_in_fail_mgw_mdcx_timeout.
09:28:38.308702 - Final verdict of PTC: none
09:28:38.308843 - Disconnected from MC.
09:28:38.308934 - TTCN-3 Parallel Test Component finished.
