+ CONFIG=generic
+ SITE_ID=1235
+ TRX_NUM=1
+ BTS_FEATURES=-fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX
+ respawn.sh osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
respawn: 0: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;31mDLINP[0;m[38;5;23m stream_cli.c:424 CLICONN(ts-0-1-oml,){CONNECTING} connect failed (-111)[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x557be4ec8090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36773){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x557be4ec7790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x557be4ec7790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x557be4ec7790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 0: stopped pid 9740 with status 0
respawn: 1: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558cf8735090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43175){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558cf8734790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558cf8734790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558cf8734790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 1: stopped pid 10236 with status 0
respawn: 2: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5600a3209090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37403){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5600a3208790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5600a3208790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5600a3208790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 2: stopped pid 10323 with status 0
respawn: 3: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x555eacc08090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34703){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x555eacc07790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x555eacc07790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x555eacc07790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 3: stopped pid 18185 with status 0
respawn: 4: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ba38682090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46663){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ba38681790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ba38681790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ba38681790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 4: stopped pid 18265 with status 0
respawn: 5: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55636bd0a090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46349){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55636bd09790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55636bd09790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55636bd09790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 5: stopped pid 18351 with status 0
respawn: 6: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f2970b0090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43101){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f2970af790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f2970af790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f2970af790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 6: stopped pid 18432 with status 0
respawn: 7: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d516f84090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39103){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d516f83790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d516f83790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d516f83790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 7: stopped pid 18511 with status 0
respawn: 8: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f693193090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40637){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f693192790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f693192790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f693192790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 8: stopped pid 18598 with status 0
respawn: 9: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ca7e913090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43359){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ca7e912790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ca7e912790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ca7e912790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 9: stopped pid 18678 with status 0
respawn: 10: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e1c7543090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38437){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e1c7542790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e1c7542790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e1c7542790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 10: stopped pid 18767 with status 0
respawn: 11: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5557cf21f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35427){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5557cf21e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5557cf21e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5557cf21e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 11: stopped pid 18848 with status 0
respawn: 12: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b2935f0090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37053){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b2935ef790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b2935ef790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b2935ef790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 12: stopped pid 18929 with status 0
respawn: 13: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ad03022090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33691){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ad03021790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ad03021790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ad03021790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 13: stopped pid 19015 with status 0
respawn: 14: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d1baeec090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33501){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d1baeeb790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d1baeeb790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d1baeeb790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 14: stopped pid 19095 with status 0
respawn: 15: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c933b17090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34973){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c933b16790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c933b16790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c933b16790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 15: stopped pid 19173 with status 0
respawn: 16: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562a859f7090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45339){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562a859f6790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562a859f6790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562a859f6790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 16: stopped pid 19250 with status 0
respawn: 17: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x560c2ee1a090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36879){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x560c2ee19790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x560c2ee19790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x560c2ee19790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 17: stopped pid 19327 with status 0
respawn: 18: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558d99678090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33183){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558d99677790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558d99677790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558d99677790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 18: stopped pid 19410 with status 0
respawn: 19: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5570124d9090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39835){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5570124d8790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5570124d8790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5570124d8790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 19: stopped pid 19484 with status 0
respawn: 20: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a543274090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41627){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a543273790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a543273790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a543273790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 20: stopped pid 19562 with status 0
respawn: 21: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5641c2c65090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40155){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5641c2c64790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5641c2c64790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5641c2c64790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 21: stopped pid 19641 with status 0
respawn: 22: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5594d6b56090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44291){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5594d6b55790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5594d6b55790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5594d6b55790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 22: stopped pid 19722 with status 0
respawn: 23: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564f5e236090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43627){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564f5e235790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564f5e235790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564f5e235790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 23: stopped pid 19805 with status 0
respawn: 24: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5611a8d26090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46105){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5611a8d25790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5611a8d25790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5611a8d25790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 24: stopped pid 20117 with status 0
respawn: 25: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55660b1bd090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44311){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55660b1bc790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55660b1bc790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55660b1bc790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 25: stopped pid 20878 with status 0
respawn: 26: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56528b9f9090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41045){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56528b9f8790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56528b9f8790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56528b9f8790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 26: stopped pid 20951 with status 0
respawn: 27: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fa7f629090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33293){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fa7f628790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fa7f628790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fa7f628790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 27: stopped pid 21027 with status 0
respawn: 28: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561d6ec7b090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45861){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561d6ec7a790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561d6ec7a790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561d6ec7a790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 28: stopped pid 21106 with status 0
respawn: 29: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5652cd0cd090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45725){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5652cd0cc790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5652cd0cc790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5652cd0cc790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 29: stopped pid 21184 with status 0
respawn: 30: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5565b4385090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40309){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5565b4384790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5565b4384790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5565b4384790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 30: stopped pid 21261 with status 0
respawn: 31: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5566a1ce9090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35959){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5566a1ce8790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5566a1ce8790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5566a1ce8790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 31: stopped pid 23152 with status 0
respawn: 32: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a217eb8090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38487){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a217eb7790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a217eb7790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a217eb7790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 32: stopped pid 23246 with status 0
respawn: 33: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c575bae090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37865){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c575bad790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c575bad790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c575bad790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 33: stopped pid 23338 with status 0
respawn: 34: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55b754323090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45395){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55b754322790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55b754322790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55b754322790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 34: stopped pid 23432 with status 0
respawn: 35: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x556572eb4090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33801){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x556572eb3790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x556572eb3790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x556572eb3790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 35: stopped pid 23522 with status 0
respawn: 36: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f2b4f15090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43419){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f2b4f14790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f2b4f14790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f2b4f14790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 36: stopped pid 23609 with status 0
respawn: 37: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55db16152090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38841){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55db16151790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55db16151790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55db16151790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 37: stopped pid 23705 with status 0
respawn: 38: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559402554090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45525){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559402553790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559402553790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559402553790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 38: stopped pid 23781 with status 0
respawn: 39: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55fbcde50090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:36325){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55fbcde4f790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55fbcde4f790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55fbcde4f790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 39: stopped pid 23874 with status 0
respawn: 40: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5624c8fc5090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42679){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5624c8fc4790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5624c8fc4790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5624c8fc4790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 40: stopped pid 23959 with status 0
respawn: 41: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c32c59a090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37169){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c32c599790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c32c599790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c32c599790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 41: stopped pid 25037 with status 0
respawn: 42: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5584da9e4090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:37851){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5584da9e3790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5584da9e3790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5584da9e3790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 42: stopped pid 25130 with status 0
respawn: 43: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e886955090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39469){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e886954790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e886954790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e886954790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 43: stopped pid 25227 with status 0
respawn: 44: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55a87395a090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38337){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55a873959790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55a873959790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55a873959790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 44: stopped pid 25321 with status 0
respawn: 45: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d8eef1b090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43449){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d8eef1a790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d8eef1a790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d8eef1a790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 45: stopped pid 25416 with status 0
respawn: 46: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564d3ef4f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43553){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564d3ef4e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564d3ef4e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564d3ef4e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 46: stopped pid 25513 with status 0
respawn: 47: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5607a5dfe090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33603){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5607a5dfd790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5607a5dfd790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5607a5dfd790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 47: stopped pid 25610 with status 0
respawn: 48: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x557a73452090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45025){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x557a73451790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x557a73451790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x557a73451790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 48: stopped pid 25709 with status 0
respawn: 49: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e3531a6090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43293){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e3531a5790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e3531a5790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e3531a5790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 49: stopped pid 25966 with status 0
respawn: 50: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55cf3e938090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41175){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55cf3e937790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55cf3e937790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55cf3e937790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 50: stopped pid 26056 with status 0
respawn: 51: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e9d2efc090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44033){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e9d2efb790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e9d2efb790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e9d2efb790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 51: stopped pid 26154 with status 0
respawn: 52: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561f22efd090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44965){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561f22efc790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561f22efc790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561f22efc790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 52: stopped pid 26250 with status 0
respawn: 53: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5648ca305090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41783){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;31mDABIS[0;m abis.c:105 OML link was closed early within 5 seconds. If this situation persists, please check your BTS and BSC configuration files for errors. A common error is a mismatch between unit_id configuration parameters of BTS and BSC.
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5648ca304790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5648ca304790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5648ca304790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 53: stopped pid 27062 with status 0
respawn: 54: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x562b23b10090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40741){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x562b23b0f790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x562b23b0f790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x562b23b0f790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 54: stopped pid 27079 with status 0
respawn: 55: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55f2a8788090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44883){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55f2a8787790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55f2a8787790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55f2a8787790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 55: stopped pid 27813 with status 0
respawn: 56: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ae066ce090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Unlocked -> Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1486 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM state already was Locked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35331){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ae066cd790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ae066cd790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ae066cd790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 56: stopped pid 28464 with status 0
respawn: 57: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55bbe8482090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38843){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55bbe8481790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55bbe8481790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55bbe8481790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 57: stopped pid 28886 with status 0
respawn: 58: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x557fbedcf090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43981){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x557fbedce790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x557fbedce790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x557fbedce790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 58: stopped pid 29287 with status 0
respawn: 59: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55deeecc0090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44063){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55deeecbf790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55deeecbf790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55deeecbf790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 59: stopped pid 29367 with status 0
respawn: 60: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ce660e6090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45369){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ce660e5790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ce660e5790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ce660e5790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 60: stopped pid 29453 with status 0
respawn: 61: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559fa60ef090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35061){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;31mDABIS[0;m abis.c:105 OML link was closed early within 10 seconds. If this situation persists, please check your BTS and BSC configuration files for errors. A common error is a mismatch between unit_id configuration parameters of BTS and BSC.
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559fa60ee790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559fa60ee790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559fa60ee790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 61: stopped pid 31157 with status 0
respawn: 62: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564a95ab5090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39145){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564a95ab4790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564a95ab4790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564a95ab4790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 62: stopped pid 31233 with status 0
respawn: 63: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558674862090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41687){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558674861790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558674861790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558674861790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 63: stopped pid 31315 with status 0
respawn: 64: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5587ab570090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:45835){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5587ab56f790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5587ab56f790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5587ab56f790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 64: stopped pid 31391 with status 0
respawn: 65: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56142833c090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41859){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56142833b790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56142833b790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56142833b790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 65: stopped pid 31471 with status 0
respawn: 66: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x564611369090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:38987){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x564611368790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x564611368790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x564611368790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 66: stopped pid 31551 with status 0
respawn: 67: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55ece0fc3090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42805){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55ece0fc2790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55ece0fc2790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55ece0fc2790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 67: stopped pid 31629 with status 0
respawn: 68: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55d792246090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43779){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55d792245790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55d792245790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55d792245790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 68: stopped pid 31720 with status 0
respawn: 69: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55989bc94090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:35709){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55989bc93790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55989bc93790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55989bc93790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 69: stopped pid 31793 with status 0
respawn: 70: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x561c99e1f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40887){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x561c99e1e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x561c99e1e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x561c99e1e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 70: stopped pid 31875 with status 0
respawn: 71: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55836e571090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46135){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55836e570790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55836e570790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55836e570790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 71: stopped pid 31956 with status 0
respawn: 72: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56328fd90090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:42355){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56328fd8f790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56328fd8f790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56328fd8f790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 72: stopped pid 32038 with status 0
respawn: 73: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5602deb3c090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40717){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5602deb3b790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5602deb3b790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5602deb3b790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 73: stopped pid 32122 with status 0
respawn: 74: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558860fa9090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40107){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558860fa8790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558860fa8790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558860fa8790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 74: stopped pid 32202 with status 0
respawn: 75: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55efa0701090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34239){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55efa0700790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55efa0700790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55efa0700790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 75: stopped pid 32282 with status 0
respawn: 76: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5647194b9090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43413){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5647194b8790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5647194b8790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5647194b8790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 76: stopped pid 32365 with status 0
respawn: 77: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56528b291090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:33553){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56528b290790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56528b290790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56528b290790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 77: stopped pid 32455 with status 0
respawn: 78: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55e85d05f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34221){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55e85d05e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55e85d05e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55e85d05e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 78: stopped pid 32536 with status 0
respawn: 79: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558b99711090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44283){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558b99710790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558b99710790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558b99710790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 79: stopped pid 32610 with status 0
respawn: 80: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5564c4216090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:43381){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5564c4215790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5564c4215790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5564c4215790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 80: stopped pid 32688 with status 0
respawn: 81: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x559e489c2090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34161){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x559e489c1790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x559e489c1790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x559e489c1790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 81: stopped pid 32772 with status 0
respawn: 82: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x56093f455090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:44551){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x56093f454790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x56093f454790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x56093f454790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 82: stopped pid 32849 with status 0
respawn: 83: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55c7050f1090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41435){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55c7050f0790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55c7050f0790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55c7050f0790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 83: stopped pid 32928 with status 0
respawn: 84: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x558dec889090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34445){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x558dec888790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x558dec888790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x558dec888790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 84: stopped pid 33005 with status 0
respawn: 85: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5606c4d85090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:46751){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x5606c4d84790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x5606c4d84790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x5606c4d84790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 85: stopped pid 33085 with status 0
respawn: 86: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55565c93f090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:41313){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55565c93e790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55565c93e790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55565c93e790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 86: stopped pid 33160 with status 0
respawn: 87: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x557d30077090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:40663){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x557d30076790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x557d30076790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x557d30076790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 87: stopped pid 33248 with status 0
respawn: 88: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55efa6ded090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:39749){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55efa6dec790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55efa6dec790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55efa6dec790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 88: stopped pid 33326 with status 0
respawn: 89: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x55558feba090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m stream_cli.c:548 CLICONN(ts-0-1-oml,r=127.0.0.1:3002<->l=127.0.0.1:34037){CONNECTED} connection closed with srv[0;m
[1;31mDABIS[0;m abis.c:429 E1L(0) Signalling link down
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:268 BTS_SHUTDOWN(bts0)[0x55558feb9790]{NONE}: Shutting down BTS, exit 1, reason: Abis close[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:926 E1TS(0:1) failed reading from socket: 0[0;m
[1;36m[1;31mDOML[0;m[1;36m bts_shutdown_fsm.c:228 BTS_SHUTDOWN(bts0)[0x55558feb9790]{WAIT_TRX_CLOSED}: Timer expired waiting for TRX close[0;m
[1;36m[1;33mDOML[0;m[1;36m bts_shutdown_fsm.c:171 BTS_SHUTDOWN(bts0)[0x55558feb9790]{EXIT}: Shutdown process completed successfully, exiting process[0;m
respawn: 89: stopped pid 33405 with status 0
respawn: 90: starting: osmo-bts-omldummy -fCCN,EGPRS,GPRS,IPv6_NSVC,PAGING_COORDINATION,OSMUX 127.0.0.1 1235 1
[1;33mDABIS[0;m abis.c:170 A-bis connection establishment to BSC (127.0.0.1) in progress...
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:1078 E1TS(0:1) enabling ipaccess BTS mode, OML connecting to 127.0.0.1:3002[0;m
[38;5;23m[1;33mDLINP[0;m[38;5;23m input/ipaccess.c:893 received ID_GET for unit ID 1235/0/0[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=GPRS-CELL INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-CELL(f1) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSE(f0) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=GPRS-NSVC(f2) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=RADIO-CARRIER INST=(00,00,ff): O&M Get Attributes [0], SW Configuration is unsupported[0;m
[1;33mDL1C[0;m bts_model.c:87 Unimplemented vbts_set_trx
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=RADIO-CARRIER(02) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;31mDOML[0;m[1;36m oml.c:631 OC=BASEBAND-TRANSCEIVER INST=(00,00,ff): O&M Get Attributes [0], Manufacturer Dependent State is unsupported[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,00): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,01): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,02): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,03): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,04): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,05): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,06): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=CHANNEL(03) INST=(00,00,07): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BTS(01) INST=(00,ff,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m oml.c:1490 OC=BASEBAND-TRANSCEIVER(04) INST=(00,00,ff): ADM STATE Locked -> Unlocked[0;m
[1;36m[1;33mDOML[0;m[1;36m nm_bb_transc_fsm.c:151 NM_BBTRANSC_OP(bts0-trx0)[0x5588f8797090]{DISABLED_OFFLINE}: Not connecting RSL in OML-DUMMY![0;m
