-- 3GPP TS 38.413 V19.1.0 (2025-12)
-- 9.4.4	PDU Definitions
-- **************************************************************
--
-- PDU definitions for NGAP.
--
-- **************************************************************

NGAP-PDU-Contents {
itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)
ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- **************************************************************
--
-- IE parameter types from other modules.
--
-- **************************************************************

IMPORTS

	A2X-PC5-QoS-Parameters,
	AerialUEsubscriptionInformation,
	AdditionalULI,
	AIoT-CorrelationIdentifier,
	AIOTFIdentifier,
	AIOTFName,
	AIOTSessionReleaseCommandTransfer,
	AIOTSessionReleaseCompleteTransfer,
	AIOTSessionReleaseRequestTransfer,
	AIoT-Support,
	AllowedNSSAI,
	AMFName,
	AMFSetID,
	AMF-TNLAssociationSetupList,
	AMF-TNLAssociationToAddList,
	AMF-TNLAssociationToRemoveList,
	AMF-TNLAssociationToUpdateList,
	AMF-UE-NGAP-ID,
	AssistanceDataForPaging,
	AssociatedSessionID,
	AUN3DeviceAccessInfo,
	AuthenticatedIndication,
	BroadcastCancelledAreaList,
	BroadcastCompletedAreaList,
	BroadcastTransportFailureTransfer,
	BroadcastTransportRequestTransfer,
	BroadcastTransportResponseTransfer,
	CancelAllWarningMessages,
	Cause,
	CellIDListForRestart,
	CEmodeBrestricted,
	CEmodeBSupport-Indicator,
	CNAssistedRANTuning,
	CommandRequestTransfer,
	CommandResponseTransfer,
	CommandFailureTransfer,	ConcurrentWarningMessageInd,
	CoreNetworkAssistanceInformationForInactive,
	CPTransportLayerInformation,
	CriticalityDiagnostics,
	DataCodingScheme,
	DirectForwardingPathAvailability,
	DL-CP-SecurityInformation,
	DL-Signalling,
	EarlyStatusTransfer-TransparentContainer,
	EDT-Session,
	EmergencyAreaIDListForRestart,
	EmergencyFallbackIndicator,
	EN-DCSONConfigurationTransfer,
	EndIndication,
	Enhanced-CoverageRestriction,
	ERedCapIndication,
	EUTRA-CGI,
	EUTRA-PagingeDRXInformation,
	Extended-AMFName,
	Extended-ConnectedTime,
	Extended-RANNodeName,
	FiveGCAction,
	FiveG-ProSeAuthorized,
	FiveG-ProSePC5QoSParameters,
	FiveG-S-TMSI,
	GlobalRANNodeID,
	GUAMI,
	GUAMIList,
	GUAMIType,
	GW-Context-Release-Indication,
	HandoverFlag,
	HandoverType,
	IAB-Authorized,
	IABNodeIndication,
	IAB-Supported,
	IMSVoiceSupportIndicator,
	IndexToRFSP,
	InfoOnRecommendedCellsAndRANNodesForPaging,
	IntersystemSONConfigurationTransfer,
	InventoryRequestTransfer,
	InventoryResponseTransfer,
	InventoryFailureTransfer,
	InventoryReportTransfer,
	LAI,
	LocationReportingRequestType,
	LPWUSPSAssistanceInformation,
	LPWUSDisableIndication,
	LTE-A2X-ServicesAuthorized,
	LTEM-Indication,
	LTEUESidelinkAggregateMaximumBitrate,
	LTEV2XServicesAuthorized,
	MaskedIMEISV,
	MBS-AreaSessionID,
	MBS-DistributionReleaseRequestTransfer,
	MBS-DistributionSetupRequestTransfer,
	MBS-DistributionSetupResponseTransfer,
	MBS-DistributionSetupUnsuccessfulTransfer,
	MBS-ServiceArea,
	MBS-SessionID,
	MBSSessionReleaseResponseTransfer,
	MBSSessionSetupOrModFailureTransfer,
	MBSSessionSetupOrModRequestTransfer,
	MBSSessionSetupOrModResponseTransfer,
	MDTPLMNList,
	MDTPLMNModificationList,
	MessageIdentifier,
	MobileIAB-Authorized,
	MobileIABNodeIndication,
	MobileIAB-Supported,
	MobilityRestrictionList,
	MulticastGroupPagingAreaList,
	MulticastSessionActivationRequestTransfer,
	MulticastSessionDeactivationRequestTransfer,
	MulticastSessionUpdateRequestTransfer,
	NAS-PDU,
	NASSecurityParametersFromNGRAN,
	NB-IoT-DefaultPagingDRX,
	NB-IoT-PagingDRX,
	NB-IoT-Paging-eDRXInfo,
	NB-IoT-UEPriority,
	NetworkControlledRepeaterAuthorized,
	NewSecurityContextInd,
	NGRAN-CGI,
	NGRAN-TNLAssociationToRemoveList,
	NGRANTraceID,
	NID,
	NoPDUSessionIndication,
	NotifySourceNGRANNode,
	NPN-AccessInformation,
	NR-A2X-ServicesAuthorized,
	NR-CGI,
	NR-PagingeDRXInformation,
	NRPPa-PDU,
	NRUESidelinkAggregateMaximumBitrate,
	NRV2XServicesAuthorized,
	NumberOfBroadcastsRequested,
	OverloadResponse,
	OverloadStartNSSAIList,
	PagingAssisDataforCEcapabUE,
	PagingCause,
	PagingDRX,
	PagingOrigin,
	PagingPolicyDifferentiation,
	PagingPriority,
	Partially-Allowed-NSSAI,
	PC5QoSParameters,
	PDUSessionAggregateMaximumBitRate,
	PDUSessionListMTCommHReq,
	PDUSessionResourceAdmittedList,
	PDUSessionResourceFailedToModifyListModCfm,
	PDUSessionResourceFailedToModifyListModRes,
	PDUSessionResourceFailedToResumeListRESReq,
	PDUSessionResourceFailedToResumeListRESRes,
	PDUSessionResourceFailedToSetupListCxtFail,
	PDUSessionResourceFailedToSetupListCxtRes,
	PDUSessionResourceFailedToSetupListHOAck,
	PDUSessionResourceFailedToSetupListPSReq,
	PDUSessionResourceFailedToSetupListSURes,
	PDUSessionResourceHandoverList,
	PDUSessionResourceListCxtRelCpl,
	PDUSessionResourceListCxtRelReq,
	PDUSessionResourceListHORqd,
	PDUSessionResourceModifyListModCfm,
	PDUSessionResourceModifyListModInd,
	PDUSessionResourceModifyListModReq,
	PDUSessionResourceModifyListModRes,
	PDUSessionResourceNotifyList,
	PDUSessionResourceReleasedListNot,
	PDUSessionResourceReleasedListPSAck,
	PDUSessionResourceReleasedListPSFail,
	PDUSessionResourceReleasedListRelRes,
	PDUSessionResourceResumeListRESReq,
	PDUSessionResourceResumeListRESRes,
	PDUSessionResourceSecondaryRATUsageList,
	PDUSessionResourceSetupListCxtReq,
	PDUSessionResourceSetupListCxtRes,
	PDUSessionResourceSetupListHOReq,
	PDUSessionResourceSetupListSUReq,
	PDUSessionResourceSetupListSURes,
	PDUSessionResourceSuspendListSUSReq,
	PDUSessionResourceSwitchedList,
	PDUSessionResourceToBeSwitchedDLList,
	PDUSessionResourceToReleaseListHOCmd,
	PDUSessionResourceToReleaseListRelCmd,
	PEIPSassistanceInformation,
	PLMNIdentity,
	PLMNSupportList,
	PrivacyIndicator,
	PWSFailedCellIDList,
	QMCConfigInfo,
	QMCDeactivation,
	RAN-AIOT-Device-NGAP-ID,
	RANNodeName,
	RANPagingPriority,
	RANStatusTransfer-TransparentContainer,
	RANTimingSynchronisationStatusInfo,
	RAN-TSSRequestType,
	RAN-TSSScope,
	RAN-UE-NGAP-ID,
	RedCapIndication,
	RedirectionVoiceFallback,
	RelativeAMFCapacity,
	RepetitionPeriod,
	RequestedNSSAI,
	ResetType,
	RGLevelWirelineAccessCharacteristics,
	RIMInformationTransfer,
	RoutingID,
	RRCEstablishmentCause,
	RRCInactiveTransitionReportRequest,
	RRCState,
	SecurityContext,
	SecurityKey,
	SerialNumber,
	ServedGUAMIList,
	SliceSupportList,
	SLPositioningRangingServiceInfo,
	S-NSSAI,
	SONConfigurationTransfer,
	SourceToTarget-AMFInformationReroute,
	SourceToTarget-TransparentContainer,
	SRVCCOperationPossible,
	SupportedTAList,
	Suspend-Request-Indication,
	Suspend-Response-Indication,
	TAI,
	TAIListForPaging,
	TAIListForRestart,
	TargetID,
	TargetNSSAIInformation,
	TargettoSource-Failure-TransparentContainer,
	TargetToSource-TransparentContainer,
	TimeSyncAssistanceInfo,
	TimeToWait,
	TNLAssociationList,
	TraceActivation,
	TrafficLoadReductionIndication,
	TransportLayerAddress,
	UEAggregateMaximumBitRate,
	UE-associatedLogicalNG-connectionList,
	UECapabilityInfoRequest,
	UEContextRequest,
	UE-DifferentiationInfo,
	UE-NGAP-IDs,
	UEPagingIdentity,
	UEPresenceInAreaOfInterestList,
	UERadioCapability,
	UERadioCapabilityForPaging,
	UERadioCapabilityID,
	UERetentionInformation,
	UESecurityCapabilities,
	UESliceMaximumBitRateList,
	UE-UP-CIoT-Support,
	UL-CP-SecurityInformation,
	UnavailableGUAMIList,
	URI-address,
	UserLocationInformation,
	WarningAreaCoordinates,
	WarningAreaList,
	WarningMessageContents,
	WarningSecurityInfo,
	WarningType,
	WUS-Assistance-Information,
	XrDeviceWith2Rx

FROM NGAP-IEs

	PrivateIE-Container{},
	ProtocolExtensionContainer{},
	ProtocolIE-Container{},
	ProtocolIE-ContainerList{},
	ProtocolIE-ContainerPair{},
	ProtocolIE-SingleContainer{},
	NGAP-PRIVATE-IES,
	NGAP-PROTOCOL-EXTENSION,
	NGAP-PROTOCOL-IES,
	NGAP-PROTOCOL-IES-PAIR

FROM NGAP-Containers

	id-A2X-PC5-QoS-Parameters,
	id-AerialUEsubscriptionInformation,
	id-AdditionalULI,
	id-AIoT-CorrelationIdentifier,
	id-AIOTFIdentifier,
	id-AIOTFName,
	id-AIOTSessionReleaseCommandTransfer,
	id-AIOTSessionReleaseCompleteTransfer,
	id-AIOTSessionReleaseRequestTransfer,
	id-AIoT-Support,
	id-AllowedNSSAI,
	id-AMFName,
	id-AMFOverloadResponse,
	id-AMFSetID,
	id-AMF-TNLAssociationFailedToSetupList,
	id-AMF-TNLAssociationSetupList,
	id-AMF-TNLAssociationToAddList,
	id-AMF-TNLAssociationToRemoveList,
	id-AMF-TNLAssociationToUpdateList,
	id-AMFTrafficLoadReductionIndication,
	id-AMF-UE-NGAP-ID,
	id-AMF-UE-NGAP-ID2,
	id-AssistanceDataForPaging,
	id-AssociatedSessionID,
	id-AUN3DeviceAccessInfo,
	id-AuthenticatedIndication,
	id-BroadcastCancelledAreaList,
	id-BroadcastCompletedAreaList,
	id-BroadcastTransportFailureTransfer,
	id-BroadcastTransportRequestTransfer,
	id-BroadcastTransportResponseTransfer,
	id-CancelAllWarningMessages,
	id-Cause,
	id-CellIDListForRestart,
	id-CEmodeBrestricted,
	id-CEmodeBSupport-Indicator,
	id-CNAssistedRANTuning,
	id-CommandRequestTransfer,
	id-CommandResponseTransfer,
	id-CommandFailureTransfer,
	id-ConcurrentWarningMessageInd,
	id-CoreNetworkAssistanceInformationForInactive,
	id-CriticalityDiagnostics,
	id-DataCodingScheme,
	id-DefaultPagingDRX,
	id-DirectForwardingPathAvailability,
	id-DL-CP-SecurityInformation,
	id-DL-Signalling,
	id-EarlyStatusTransfer-TransparentContainer,
	id-EDT-Session,
	id-EmergencyAreaIDListForRestart,
	id-EmergencyFallbackIndicator,
	id-ENDC-SONConfigurationTransferDL,
	id-ENDC-SONConfigurationTransferUL,
	id-EndIndication,
	id-Enhanced-CoverageRestriction,
	id-ERedCapIndication,
	id-EUTRA-CGI,
	id-EUTRA-PagingeDRXInformation,
	id-Extended-AMFName,
	id-Extended-ConnectedTime,
	id-Extended-RANNodeName,
	id-FiveGCAction,
	id-FiveG-ProSeAuthorized,
	id-FiveG-ProSePC5QoSParameters,
	id-FiveG-ProSeUEPC5AggregateMaximumBitRate,
	id-FiveG-S-TMSI,
	id-GlobalRANNodeID,
	id-GUAMI,
	id-GUAMIList,
	id-GUAMIType,
	id-GW-Context-Release-Indication,
	id-HandoverFlag,
	id-HandoverType,
	id-IAB-Authorized,
	id-IABNodeIndication,
	id-IAB-Supported,
	id-IMSVoiceSupportIndicator,
	id-IndexToRFSP,
	id-InfoOnRecommendedCellsAndRANNodesForPaging,
	id-IntersystemSONConfigurationTransferDL,
	id-IntersystemSONConfigurationTransferUL,
	id-InventoryRequestTransfer,
	id-InventoryResponseTransfer,
	id-InventoryFailureTransfer,
	id-InventoryReportTransfer,
	id-LocationReportingRequestType,
	id-LPWUSPSAssistanceInformation,
	id-LPWUSDisableIndication,
	id-LTE-A2X-ServicesAuthorized,
	id-LTE-A2X-UE-PC5-AggregateMaximumBitRate,
	id-LTEM-Indication,
	id-LTEUESidelinkAggregateMaximumBitrate,
	id-LTEV2XServicesAuthorized,
	id-ManagementBasedMDTPLMNList,
	id-ManagementBasedMDTPLMNModificationList,
	id-MaskedIMEISV,
	id-MBS-AreaSessionID,
	id-MBS-DistributionReleaseRequestTransfer,
	id-MBS-DistributionSetupRequestTransfer,
	id-MBS-DistributionSetupResponseTransfer,
	id-MBS-DistributionSetupUnsuccessfulTransfer,
	id-MBS-ServiceArea,
	id-MBS-SessionID,
	id-MBSSessionModificationFailureTransfer,
	id-MBSSessionModificationRequestTransfer,
	id-MBSSessionModificationResponseTransfer,
	id-MBSSessionReleaseResponseTransfer,
	id-MBSSessionSetupFailureTransfer,
	id-MBSSessionSetupRequestTransfer,
	id-MBSSessionSetupResponseTransfer,
	id-MessageIdentifier,
	id-MobileIAB-Authorized,
	id-MobileIABNodeIndication,
	id-MobileIAB-Supported,
	id-MobilityRestrictionList,
	id-MulticastGroupPagingAreaList,
	id-MulticastSessionActivationRequestTransfer,
	id-MulticastSessionDeactivationRequestTransfer,
	id-MulticastSessionUpdateRequestTransfer,
	id-NASC,
	id-NAS-PDU,
	id-NASSecurityParametersFromNGRAN,
	id-NB-IoT-DefaultPagingDRX,
	id-NB-IoT-PagingDRX,
	id-NB-IoT-Paging-eDRXInfo,
	id-NB-IoT-UEPriority,
	id-NetworkControlledRepeaterAuthorized,
	id-NewAMF-UE-NGAP-ID,
	id-NewGUAMI,
	id-NewSecurityContextInd,
	id-NGAP-Message,
	id-NGRAN-CGI,
	id-NGRAN-TNLAssociationToRemoveList,
	id-NGRANTraceID,
	id-NoPDUSessionIndication,
	id-NotifySourceNGRANNode,
	id-NPN-AccessInformation,
	id-NR-A2X-ServicesAuthorized,
	id-NR-A2X-UE-PC5-AggregateMaximumBitRate,
	id-NR-PagingeDRXInformation,
	id-NRPPa-PDU,
	id-NRUESidelinkAggregateMaximumBitrate,
	id-NRV2XServicesAuthorized,
	id-NumberOfBroadcastsRequested,
	id-OldAMF,
	id-OverloadStartNSSAIList,
	id-PagingAssisDataforCEcapabUE,
	id-PagingCause,
	id-PagingDRX,
	id-PagingOrigin,
	id-PagingPolicyDifferentiation,
	id-PagingPriority,
	id-Partially-Allowed-NSSAI,
	id-PC5QoSParameters,
	id-PDUSessionListMTCommHReq,
	id-PDUSessionResourceAdmittedList,
	id-PDUSessionResourceFailedToModifyListModCfm,
	id-PDUSessionResourceFailedToModifyListModRes,
	id-PDUSessionResourceFailedToResumeListRESReq,
	id-PDUSessionResourceFailedToResumeListRESRes,
	id-PDUSessionResourceFailedToSetupListCxtFail,
	id-PDUSessionResourceFailedToSetupListCxtRes,
	id-PDUSessionResourceFailedToSetupListHOAck,
	id-PDUSessionResourceFailedToSetupListPSReq,
	id-PDUSessionResourceFailedToSetupListSURes,
	id-PDUSessionResourceHandoverList,
	id-PDUSessionResourceListCxtRelCpl,
	id-PDUSessionResourceListCxtRelReq,
	id-PDUSessionResourceListHORqd,
	id-PDUSessionResourceModifyListModCfm,
	id-PDUSessionResourceModifyListModInd,
	id-PDUSessionResourceModifyListModReq,
	id-PDUSessionResourceModifyListModRes,
	id-PDUSessionResourceNotifyList,
	id-PDUSessionResourceReleasedListNot,
	id-PDUSessionResourceReleasedListPSAck,
	id-PDUSessionResourceReleasedListPSFail,
	id-PDUSessionResourceReleasedListRelRes,
	id-PDUSessionResourceResumeListRESReq,
	id-PDUSessionResourceResumeListRESRes,
	id-PDUSessionResourceSecondaryRATUsageList,
	id-PDUSessionResourceSetupListCxtReq,
	id-PDUSessionResourceSetupListCxtRes,
	id-PDUSessionResourceSetupListHOReq,
	id-PDUSessionResourceSetupListSUReq,
	id-PDUSessionResourceSetupListSURes,
	id-PDUSessionResourceSuspendListSUSReq,
	id-PDUSessionResourceSwitchedList,
	id-PDUSessionResourceToBeSwitchedDLList,
	id-PDUSessionResourceToReleaseListHOCmd,
	id-PDUSessionResourceToReleaseListRelCmd,
	id-PEIPSassistanceInformation,
	id-PLMNSupportList,
	id-PrivacyIndicator,
	id-PWSFailedCellIDList,
	id-QMCConfigInfo,
	id-QMCDeactivation,
	id-RAN-AIOT-Device-NGAP-ID,
	id-RANNodeName,
	id-RANPagingPriority,
	id-RANStatusTransfer-TransparentContainer,
	id-RANTimingSynchronisationStatusInfo,
	id-RAN-TSSRequestType,
	id-RAN-TSSScope,
	id-RAN-UE-NGAP-ID,
	id-RedCapIndication,
	id-RedirectionVoiceFallback,
	id-RelativeAMFCapacity,
	id-RepetitionPeriod,
	id-RequestedNSSAI,
	id-ResetType,
	id-RGLevelWirelineAccessCharacteristics,
	id-RIMInformationTransfer,
	id-RoutingID,
	id-RRCEstablishmentCause,
	id-RRCInactiveTransitionReportRequest,
	id-RRC-Resume-Cause,
	id-RRCState,
	id-SecurityContext,
	id-SecurityKey,
	id-SelectedNID,
	id-SelectedPLMNIdentity,
	id-SerialNumber,
	id-ServedGUAMIList,
	id-SliceSupportList,
	id-S-NSSAI,
	id-SONConfigurationTransferDL,
	id-SONConfigurationTransferUL,
	id-SourceAMF-GUAMI,
	id-SourceAMF-UE-NGAP-ID,
	id-SourceToTarget-AMFInformationReroute,
	id-SourceToTarget-TransparentContainer,
	id-SRVCCOperationPossible,
	id-SupportedTAList,
	id-Suspend-Request-Indication,
	id-Suspend-Response-Indication,
	id-Target-RAN-Node-ID,
	id-TAI,
	id-TAIListForPaging,
	id-TAIListForRestart,
	id-TargetID,
	id-TargetNSSAIInformation,
	id-TargettoSource-Failure-TransparentContainer,
	id-TargetToSource-TransparentContainer,
	id-TimeSyncAssistanceInfo,
	id-TimeToWait,
	id-TNGFIdentityInformation,
	id-TraceActivation,
	id-TraceCollectionEntityIPAddress,
	id-TraceCollectionEntityURI,
	id-TWIFIdentityInformation,
	id-UEAggregateMaximumBitRate,
	id-UE-associatedLogicalNG-connectionList,
	id-UECapabilityInfoRequest,
	id-UEContextRequest,
	id-UE-DifferentiationInfo,
	id-UE-NGAP-IDs,
	id-UEPagingIdentity,
	id-UEPresenceInAreaOfInterestList,
	id-UERadioCapability,
	id-UERadioCapability-EUTRA-Format,
	id-UERadioCapabilityForPaging,
	id-UERadioCapabilityID,
	id-UERetentionInformation,
	id-UESecurityCapabilities,
	id-UESliceMaximumBitRateList,
	id-UE-UP-CIoT-Support,
	id-UL-CP-SecurityInformation,
	id-UnavailableGUAMIList,
	id-UserLocationInformation,
	id-W-AGFIdentityInformation,
	id-WarningAreaCoordinates,
	id-WarningAreaList,
	id-WarningMessageContents,
	id-WarningSecurityInfo,
	id-WarningType,
	id-WUS-Assistance-Information,
	id-XrDeviceWith2Rx,
	id-SLPositioningRangingServiceInfo,
	id-ExtendedOldAMF,
	id-Aerial-UE-FlightInformationOngoingReporting-failed


FROM NGAP-Constants;

-- **************************************************************
--
-- PDU SESSION MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- PDU Session Resource Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE SETUP REQUEST
--
-- **************************************************************

PDUSessionResourceSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceSetupRequestIEs} },
	...
}

PDUSessionResourceSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RANPagingPriority						CRITICALITY ignore	TYPE RANPagingPriority							PRESENCE optional		}|
	{ ID id-NAS-PDU									CRITICALITY reject	TYPE NAS-PDU									PRESENCE optional		}|
	{ ID id-PDUSessionResourceSetupListSUReq		CRITICALITY reject	TYPE PDUSessionResourceSetupListSUReq		PRESENCE mandatory	}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY ignore	TYPE UEAggregateMaximumBitRate				PRESENCE optional		}|
	{ ID id-UESliceMaximumBitRateList				CRITICALITY ignore	TYPE UESliceMaximumBitRateList				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE SETUP RESPONSE
--
-- **************************************************************

PDUSessionResourceSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceSetupResponseIEs} },
	...
}

PDUSessionResourceSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSetupListSURes			CRITICALITY ignore	TYPE PDUSessionResourceSetupListSURes				PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToSetupListSURes	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListSURes		PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation							PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PDU Session Resource Release Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE RELEASE COMMAND
--
-- **************************************************************

PDUSessionResourceReleaseCommand ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceReleaseCommandIEs} },
	...
}

PDUSessionResourceReleaseCommandIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RANPagingPriority							CRITICALITY ignore	TYPE RANPagingPriority								PRESENCE optional		}|
	{ ID id-NAS-PDU										CRITICALITY ignore	TYPE NAS-PDU											PRESENCE optional		}|
	{ ID id-PDUSessionResourceToReleaseListRelCmd		CRITICALITY reject	TYPE PDUSessionResourceToReleaseListRelCmd		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE RELEASE RESPONSE
--
-- **************************************************************

PDUSessionResourceReleaseResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceReleaseResponseIEs} },
	...
}

PDUSessionResourceReleaseResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceReleasedListRelRes			CRITICALITY ignore	TYPE PDUSessionResourceReleasedListRelRes		PRESENCE mandatory	}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation						PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PDU Session Resource Modify Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY REQUEST
--
-- **************************************************************

PDUSessionResourceModifyRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyRequestIEs} },
	...
}

PDUSessionResourceModifyRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RANPagingPriority						CRITICALITY ignore	TYPE RANPagingPriority							PRESENCE optional		}|
	{ ID id-PDUSessionResourceModifyListModReq		CRITICALITY reject	TYPE PDUSessionResourceModifyListModReq	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY RESPONSE
--
-- **************************************************************

PDUSessionResourceModifyResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyResponseIEs} },
	...
}

PDUSessionResourceModifyResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID									CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID									CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceModifyListModRes				CRITICALITY ignore	TYPE PDUSessionResourceModifyListModRes			PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToModifyListModRes		CRITICALITY ignore	TYPE PDUSessionResourceFailedToModifyListModRes		PRESENCE optional	}|
	{ ID id-UserLocationInformation							CRITICALITY ignore	TYPE UserLocationInformation							PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics							CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PDU Session Resource Notify Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE NOTIFY
--
-- **************************************************************

PDUSessionResourceNotify ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceNotifyIEs} },
	...
}

PDUSessionResourceNotifyIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceNotifyList			CRITICALITY reject	TYPE PDUSessionResourceNotifyList				PRESENCE optional		}|
	{ ID id-PDUSessionResourceReleasedListNot		CRITICALITY ignore	TYPE PDUSessionResourceReleasedListNot		PRESENCE optional		}|
	{ ID id-UserLocationInformation					CRITICALITY ignore	TYPE UserLocationInformation						PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PDU Session Resource Modify Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY INDICATION
--
-- **************************************************************

PDUSessionResourceModifyIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyIndicationIEs} },
	...
}

PDUSessionResourceModifyIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceModifyListModInd		CRITICALITY reject	TYPE PDUSessionResourceModifyListModInd		PRESENCE mandatory	}|
	{ ID id-UserLocationInformation					CRITICALITY ignore	TYPE UserLocationInformation						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PDU SESSION RESOURCE MODIFY CONFIRM
--
-- **************************************************************

PDUSessionResourceModifyConfirm ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PDUSessionResourceModifyConfirmIEs} },
	...
}

PDUSessionResourceModifyConfirmIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceModifyListModCfm			CRITICALITY ignore	TYPE PDUSessionResourceModifyListModCfm		PRESENCE optional	}|
	{ ID id-PDUSessionResourceFailedToModifyListModCfm	CRITICALITY ignore	TYPE PDUSessionResourceFailedToModifyListModCfm		PRESENCE optional	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Initial Context Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- INITIAL CONTEXT SETUP REQUEST
--
-- **************************************************************

InitialContextSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialContextSetupRequestIEs} },
	...
}

InitialContextSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-OldAMF									CRITICALITY reject	TYPE AMFName											PRESENCE optional		}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY reject	TYPE UEAggregateMaximumBitRate						PRESENCE conditional	}|
-- The above IE shall be present if the PDU Session Resource Setup List IE is present
	{ ID id-CoreNetworkAssistanceInformationForInactive		CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive		PRESENCE optional		}|
	{ ID id-GUAMI									CRITICALITY reject	TYPE GUAMI												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSetupListCxtReq		CRITICALITY reject	TYPE PDUSessionResourceSetupListCxtReq			PRESENCE optional		}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI										PRESENCE mandatory	}|
	{ ID id-UESecurityCapabilities					CRITICALITY reject	TYPE UESecurityCapabilities							PRESENCE mandatory	}|
	{ ID id-SecurityKey								CRITICALITY reject	TYPE SecurityKey										PRESENCE mandatory	}|
	{ ID id-TraceActivation							CRITICALITY ignore	TYPE TraceActivation									PRESENCE optional		}|
	{ ID id-MobilityRestrictionList					CRITICALITY ignore	TYPE MobilityRestrictionList							PRESENCE optional		}|
	{ ID id-UERadioCapability						CRITICALITY ignore	TYPE UERadioCapability									PRESENCE optional		}|
	{ ID id-IndexToRFSP								CRITICALITY ignore	TYPE IndexToRFSP										PRESENCE optional		}|
	{ ID id-MaskedIMEISV							CRITICALITY ignore	TYPE MaskedIMEISV										PRESENCE optional		}|
	{ ID id-NAS-PDU									CRITICALITY ignore	TYPE NAS-PDU											PRESENCE optional		}|
	{ ID id-EmergencyFallbackIndicator				CRITICALITY reject	TYPE EmergencyFallbackIndicator						PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest		CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest			PRESENCE optional		}|
	{ ID id-UERadioCapabilityForPaging				CRITICALITY ignore	TYPE UERadioCapabilityForPaging						PRESENCE optional		}|
	{ ID id-RedirectionVoiceFallback				CRITICALITY ignore	TYPE RedirectionVoiceFallback						PRESENCE optional		}|
	{ ID id-LocationReportingRequestType			CRITICALITY ignore	TYPE LocationReportingRequestType					PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning						CRITICALITY ignore	TYPE CNAssistedRANTuning								PRESENCE optional		}|
	{ ID id-SRVCCOperationPossible					CRITICALITY ignore	TYPE SRVCCOperationPossible							PRESENCE optional		}|
	{ ID id-IAB-Authorized							CRITICALITY ignore	TYPE IAB-Authorized										PRESENCE optional		}|
	{ ID id-Enhanced-CoverageRestriction			CRITICALITY ignore	TYPE Enhanced-CoverageRestriction					PRESENCE optional		}|
	{ ID id-Extended-ConnectedTime					CRITICALITY ignore	TYPE Extended-ConnectedTime							PRESENCE optional		}|
	{ ID id-UE-DifferentiationInfo					CRITICALITY ignore	TYPE UE-DifferentiationInfo							PRESENCE optional		}|
	{ ID id-NRV2XServicesAuthorized					CRITICALITY ignore	TYPE NRV2XServicesAuthorized							PRESENCE optional		}|
	{ ID id-LTEV2XServicesAuthorized				CRITICALITY ignore	TYPE LTEV2XServicesAuthorized						PRESENCE optional		}|
	{ ID id-NRUESidelinkAggregateMaximumBitrate		CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate			PRESENCE optional		}|
	{ ID id-LTEUESidelinkAggregateMaximumBitrate	CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-PC5QoSParameters						CRITICALITY ignore	TYPE PC5QoSParameters									PRESENCE optional 	}|
	{ ID id-CEmodeBrestricted						CRITICALITY ignore	TYPE CEmodeBrestricted									PRESENCE optional		}|
	{ ID id-UE-UP-CIoT-Support						CRITICALITY ignore	TYPE UE-UP-CIoT-Support									PRESENCE optional		}|
	{ ID id-RGLevelWirelineAccessCharacteristics	CRITICALITY ignore	TYPE RGLevelWirelineAccessCharacteristics		PRESENCE optional		}|
	{ ID id-ManagementBasedMDTPLMNList				CRITICALITY ignore	TYPE MDTPLMNList										PRESENCE optional		}|
	{ ID id-UERadioCapabilityID						CRITICALITY reject	TYPE UERadioCapabilityID								PRESENCE optional		}|
	{ ID id-TimeSyncAssistanceInfo					CRITICALITY ignore	TYPE TimeSyncAssistanceInfo							PRESENCE optional		}|
	{ ID id-QMCConfigInfo							CRITICALITY ignore	TYPE QMCConfigInfo										PRESENCE optional		}|
	{ ID id-TargetNSSAIInformation					CRITICALITY ignore	TYPE TargetNSSAIInformation							PRESENCE optional		}|
	{ ID id-UESliceMaximumBitRateList				CRITICALITY ignore	TYPE UESliceMaximumBitRateList						PRESENCE optional		}|
	{ ID id-FiveG-ProSeAuthorized					CRITICALITY ignore	TYPE FiveG-ProSeAuthorized							PRESENCE optional		}|
	{ ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate	CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate			PRESENCE optional		}|
	{ ID id-FiveG-ProSePC5QoSParameters				CRITICALITY ignore	TYPE FiveG-ProSePC5QoSParameters					PRESENCE optional		}|
	{ ID id-NetworkControlledRepeaterAuthorized 	CRITICALITY ignore	TYPE NetworkControlledRepeaterAuthorized 		PRESENCE optional		}|
	{ ID id-AerialUEsubscriptionInformation			CRITICALITY ignore	TYPE AerialUEsubscriptionInformation				PRESENCE optional		}|
	{ ID id-NR-A2X-ServicesAuthorized				CRITICALITY ignore	TYPE NR-A2X-ServicesAuthorized						PRESENCE optional		}|
	{ ID id-LTE-A2X-ServicesAuthorized				CRITICALITY ignore	TYPE LTE-A2X-ServicesAuthorized						PRESENCE optional		}|
	{ ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate	CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate			PRESENCE optional		}|
	{ ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate	CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-A2X-PC5-QoS-Parameters					CRITICALITY ignore	TYPE A2X-PC5-QoS-Parameters							PRESENCE optional		}|
	{ ID id-MobileIAB-Authorized					CRITICALITY ignore	TYPE MobileIAB-Authorized								PRESENCE optional		}|
	{ ID id-Partially-Allowed-NSSAI					CRITICALITY ignore	TYPE Partially-Allowed-NSSAI							PRESENCE optional		}|
	{ ID id-SLPositioningRangingServiceInfo			CRITICALITY ignore	TYPE SLPositioningRangingServiceInfo				PRESENCE optional		}|
	{ ID id-ExtendedOldAMF							CRITICALITY ignore	TYPE Extended-AMFName									PRESENCE optional		}|
	{ ID id-AMF-UE-NGAP-ID2							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE optional		},
	...
}

-- **************************************************************
--
-- INITIAL CONTEXT SETUP RESPONSE
--
-- **************************************************************

InitialContextSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialContextSetupResponseIEs} },
	...
}

InitialContextSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSetupListCxtRes			CRITICALITY ignore	TYPE PDUSessionResourceSetupListCxtRes					PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToSetupListCxtRes	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListCxtRes		PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics									PRESENCE optional		},
	...
}


-- **************************************************************
--
-- INITIAL CONTEXT SETUP FAILURE
--
-- **************************************************************

InitialContextSetupFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialContextSetupFailureIEs} },
	...
}

InitialContextSetupFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceFailedToSetupListCxtFail	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListCxtFail		PRESENCE optional		}|
	{ ID id-Cause										CRITICALITY ignore	TYPE Cause														PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics									PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Context Release Request Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT RELEASE REQUEST
--
-- **************************************************************

UEContextReleaseRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextReleaseRequest-IEs} },
	...
}

UEContextReleaseRequest-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID						CRITICALITY reject	TYPE RAN-UE-NGAP-ID								PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceListCxtRelReq		CRITICALITY reject	TYPE PDUSessionResourceListCxtRelReq		PRESENCE optional		}|
	{ ID id-Cause								CRITICALITY ignore	TYPE Cause										PRESENCE mandatory	}|
	{ ID id-GW-Context-Release-Indication		CRITICALITY reject	TYPE GW-Context-Release-Indication			PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Context Release Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT RELEASE COMMAND
--
-- **************************************************************

UEContextReleaseCommand ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextReleaseCommand-IEs} },
	...
}

UEContextReleaseCommand-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UE-NGAP-IDs				CRITICALITY reject	TYPE UE-NGAP-IDs			PRESENCE mandatory	}|
	{ ID id-Cause					CRITICALITY ignore	TYPE Cause					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE CONTEXT RELEASE COMPLETE
--
-- **************************************************************

UEContextReleaseComplete ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextReleaseComplete-IEs} },
	...
}

UEContextReleaseComplete-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation							PRESENCE optional		}|
	{ ID id-InfoOnRecommendedCellsAndRANNodesForPaging	CRITICALITY ignore	TYPE InfoOnRecommendedCellsAndRANNodesForPaging	PRESENCE optional		}|
	{ ID id-PDUSessionResourceListCxtRelCpl				CRITICALITY	reject	TYPE PDUSessionResourceListCxtRelCpl					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		}|
	{ ID id-PagingAssisDataforCEcapabUE					CRITICALITY ignore	TYPE PagingAssisDataforCEcapabUE						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Context Resume Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT RESUME REQUEST
--
-- **************************************************************

UEContextResumeRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextResumeRequestIEs} },
	...
}

UEContextResumeRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RRC-Resume-Cause						CRITICALITY ignore	TYPE RRCEstablishmentCause							PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceResumeListRESReq		CRITICALITY reject	TYPE PDUSessionResourceResumeListRESReq			PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToResumeListRESReq		CRITICALITY reject	TYPE PDUSessionResourceFailedToResumeListRESReq			PRESENCE optional		}|
	{ ID id-Suspend-Request-Indication				CRITICALITY ignore	TYPE Suspend-Request-Indication						PRESENCE optional		}|
	{ ID id-InfoOnRecommendedCellsAndRANNodesForPaging	CRITICALITY ignore	TYPE InfoOnRecommendedCellsAndRANNodesForPaging		PRESENCE optional		}|
	{ ID id-PagingAssisDataforCEcapabUE					CRITICALITY ignore	TYPE PagingAssisDataforCEcapabUE				PRESENCE optional		}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation					PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT RESUME RESPONSE
--
-- **************************************************************

UEContextResumeResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextResumeResponseIEs} },
	...
}

UEContextResumeResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceResumeListRESRes		CRITICALITY reject	TYPE PDUSessionResourceResumeListRESRes			PRESENCE optional		}|
	{ ID id-PDUSessionResourceFailedToResumeListRESRes		CRITICALITY reject	TYPE PDUSessionResourceFailedToResumeListRESRes			PRESENCE optional		}|
	{ ID id-SecurityContext							CRITICALITY reject	TYPE SecurityContext									PRESENCE optional		}|
	{ ID id-Suspend-Response-Indication				CRITICALITY ignore	TYPE Suspend-Response-Indication					PRESENCE optional		}|
	{ ID id-Extended-ConnectedTime					CRITICALITY ignore	TYPE Extended-ConnectedTime							PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT RESUME FAILURE
--
-- **************************************************************

UEContextResumeFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { UEContextResumeFailureIEs} },
	...
}

UEContextResumeFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}


-- **************************************************************
--
-- UE Context Suspend Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT SUSPEND REQUEST
--
-- **************************************************************

UEContextSuspendRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextSuspendRequestIEs} },
	...
}

UEContextSuspendRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-InfoOnRecommendedCellsAndRANNodesForPaging	CRITICALITY ignore	TYPE InfoOnRecommendedCellsAndRANNodesForPaging		PRESENCE optional		}|
	{ ID id-PagingAssisDataforCEcapabUE					CRITICALITY ignore	TYPE PagingAssisDataforCEcapabUE							PRESENCE optional		}|
	{ ID id-PDUSessionResourceSuspendListSUSReq			CRITICALITY reject	TYPE PDUSessionResourceSuspendListSUSReq				PRESENCE optional		}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT SUSPEND RESPONSE
--
-- **************************************************************

UEContextSuspendResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextSuspendResponseIEs} },
	...
}

UEContextSuspendResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-SecurityContext							CRITICALITY reject	TYPE SecurityContext									PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT SUSPEND FAILURE
--
-- **************************************************************

UEContextSuspendFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { UEContextSuspendFailureIEs} },
	...
}

UEContextSuspendFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Context Modification Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE CONTEXT MODIFICATION REQUEST
--
-- **************************************************************

UEContextModificationRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextModificationRequestIEs} },
	...
}

UEContextModificationRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RANPagingPriority						CRITICALITY ignore	TYPE RANPagingPriority								PRESENCE optional		}|
	{ ID id-SecurityKey								CRITICALITY reject	TYPE SecurityKey									PRESENCE optional		}|
	{ ID id-IndexToRFSP								CRITICALITY ignore	TYPE IndexToRFSP									PRESENCE optional		}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY ignore	TYPE UEAggregateMaximumBitRate					PRESENCE optional		}|
	{ ID id-UESecurityCapabilities					CRITICALITY reject	TYPE UESecurityCapabilities						PRESENCE optional		}|
	{ ID id-CoreNetworkAssistanceInformationForInactive		CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive		PRESENCE optional		}|
	{ ID id-EmergencyFallbackIndicator				CRITICALITY reject	TYPE EmergencyFallbackIndicator					PRESENCE optional		}|
	{ ID id-NewAMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest		CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest		PRESENCE optional		}|
	{ ID id-NewGUAMI								CRITICALITY reject	TYPE GUAMI											PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning						CRITICALITY ignore	TYPE CNAssistedRANTuning							PRESENCE optional		}|
	{ ID id-SRVCCOperationPossible					CRITICALITY ignore	TYPE SRVCCOperationPossible						PRESENCE optional		}|
	{ ID id-IAB-Authorized							CRITICALITY ignore	TYPE IAB-Authorized									PRESENCE optional		}|
	{ ID id-NRV2XServicesAuthorized					CRITICALITY ignore	TYPE NRV2XServicesAuthorized						PRESENCE optional		}|
	{ ID id-LTEV2XServicesAuthorized				CRITICALITY ignore	TYPE LTEV2XServicesAuthorized					PRESENCE optional		}|
	{ ID id-NRUESidelinkAggregateMaximumBitrate		CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-LTEUESidelinkAggregateMaximumBitrate	CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate	PRESENCE optional		}|
	{ ID id-PC5QoSParameters						CRITICALITY ignore	TYPE PC5QoSParameters								PRESENCE optional 	}|
	{ ID id-UERadioCapabilityID						CRITICALITY reject	TYPE UERadioCapabilityID							PRESENCE optional		}|
	{ ID id-RGLevelWirelineAccessCharacteristics	CRITICALITY ignore	TYPE RGLevelWirelineAccessCharacteristics	PRESENCE optional		}|
	{ ID id-TimeSyncAssistanceInfo					CRITICALITY ignore	TYPE TimeSyncAssistanceInfo						PRESENCE optional		}|
	{ ID id-QMCConfigInfo							CRITICALITY ignore	TYPE QMCConfigInfo									PRESENCE optional		}|
	{ ID id-QMCDeactivation							CRITICALITY ignore	TYPE QMCDeactivation								PRESENCE optional		}|
	{ ID id-UESliceMaximumBitRateList				CRITICALITY ignore	TYPE UESliceMaximumBitRateList					PRESENCE optional		}|
	{ ID id-ManagementBasedMDTPLMNModificationList	CRITICALITY ignore	TYPE MDTPLMNModificationList						PRESENCE optional		}|
	{ ID id-FiveG-ProSeAuthorized					CRITICALITY ignore	TYPE FiveG-ProSeAuthorized						PRESENCE optional		}|
	{ ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate	CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-FiveG-ProSePC5QoSParameters				CRITICALITY ignore	TYPE FiveG-ProSePC5QoSParameters				PRESENCE optional		}|
	{ ID id-NetworkControlledRepeaterAuthorized 	CRITICALITY ignore	TYPE NetworkControlledRepeaterAuthorized 	PRESENCE optional		}|
	{ ID id-AerialUEsubscriptionInformation			CRITICALITY ignore	TYPE AerialUEsubscriptionInformation			PRESENCE optional		}|
	{ ID id-NR-A2X-ServicesAuthorized				CRITICALITY ignore	TYPE NR-A2X-ServicesAuthorized					PRESENCE optional		}|
	{ ID id-LTE-A2X-ServicesAuthorized				CRITICALITY ignore	TYPE LTE-A2X-ServicesAuthorized					PRESENCE optional		}|
	{ ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate	CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate	CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate	PRESENCE optional		}|
	{ ID id-A2X-PC5-QoS-Parameters					CRITICALITY ignore	TYPE A2X-PC5-QoS-Parameters						PRESENCE optional		}|
	{ ID id-MobileIAB-Authorized					CRITICALITY ignore	TYPE MobileIAB-Authorized							PRESENCE optional		}|
	{ ID id-SLPositioningRangingServiceInfo			CRITICALITY ignore	TYPE SLPositioningRangingServiceInfo			PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT MODIFICATION RESPONSE
--
-- **************************************************************

UEContextModificationResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextModificationResponseIEs} },
	...
}

UEContextModificationResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RRCState					CRITICALITY ignore	TYPE RRCState					PRESENCE optional		}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation	PRESENCE optional 	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE CONTEXT MODIFICATION FAILURE
--
-- **************************************************************

UEContextModificationFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UEContextModificationFailureIEs} },
	...
}

UEContextModificationFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- RRC INACTIVE TRANSITION REPORT
--
-- **************************************************************

RRCInactiveTransitionReport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RRCInactiveTransitionReportIEs} },
	...
}

RRCInactiveTransitionReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RRCState					CRITICALITY ignore	TYPE RRCState						PRESENCE mandatory	}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- Retrieve UE Information
--
-- **************************************************************

RetrieveUEInformation ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container       { { RetrieveUEInformationIEs} },
	...
}

RetrieveUEInformationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-FiveG-S-TMSI					CRITICALITY reject	TYPE FiveG-S-TMSI				PRESENCE mandatory	},
	...

}

-- **************************************************************

-- UE Information Transfer
--
-- **************************************************************

UEInformationTransfer ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container       { {  UEInformationTransferIEs} },
	...
}

UEInformationTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-FiveG-S-TMSI				CRITICALITY reject 	TYPE FiveG-S-TMSI				PRESENCE mandatory	}|
	{ ID id-NB-IoT-UEPriority			CRITICALITY ignore	TYPE NB-IoT-UEPriority			PRESENCE optional		}|
	{ ID id-UERadioCapability			CRITICALITY ignore	TYPE UERadioCapability			PRESENCE optional		}|
	{ ID id-S-NSSAI						CRITICALITY ignore	TYPE S-NSSAI					PRESENCE optional		}|
	{ ID id-AllowedNSSAI				CRITICALITY ignore	TYPE AllowedNSSAI				PRESENCE optional		}|
	{ ID id-UE-DifferentiationInfo		CRITICALITY ignore	TYPE UE-DifferentiationInfo		PRESENCE optional		}|
	{ ID id-MaskedIMEISV				CRITICALITY ignore	TYPE MaskedIMEISV				PRESENCE optional		}|
	{ ID id-Partially-Allowed-NSSAI		CRITICALITY ignore	TYPE Partially-Allowed-NSSAI	PRESENCE optional		},
	...
}

-- **************************************************************
--
-- RAN CP Relocation Indication
--
-- **************************************************************

RANCPRelocationIndication ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container { { RANCPRelocationIndicationIEs} },
	...
}

RANCPRelocationIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-FiveG-S-TMSI					CRITICALITY reject	TYPE FiveG-S-TMSI					PRESENCE mandatory	}|
	{ ID id-EUTRA-CGI						CRITICALITY ignore	TYPE EUTRA-CGI						PRESENCE mandatory	}|
	{ ID id-TAI								CRITICALITY ignore	TYPE TAI							PRESENCE mandatory	}|
	{ ID id-UL-CP-SecurityInformation		CRITICALITY reject	TYPE UL-CP-SecurityInformation		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE MOBILITY MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Handover Preparation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER REQUIRED
--
-- **************************************************************

HandoverRequired ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverRequiredIEs} },
	...
}

HandoverRequiredIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-HandoverType							CRITICALITY reject	TYPE HandoverType									PRESENCE mandatory	}|
	{ ID id-Cause									CRITICALITY ignore	TYPE Cause											PRESENCE mandatory	}|
	{ ID id-TargetID								CRITICALITY reject	TYPE TargetID										PRESENCE mandatory	}|
	{ ID id-DirectForwardingPathAvailability		CRITICALITY ignore	TYPE DirectForwardingPathAvailability			PRESENCE optional		}|
	{ ID id-PDUSessionResourceListHORqd				CRITICALITY reject	TYPE PDUSessionResourceListHORqd				PRESENCE mandatory	}|
	{ ID id-SourceToTarget-TransparentContainer		CRITICALITY reject	TYPE SourceToTarget-TransparentContainer		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- HANDOVER COMMAND
--
-- **************************************************************

HandoverCommand ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverCommandIEs} },
	...
}

HandoverCommandIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-HandoverType								CRITICALITY reject	TYPE HandoverType											PRESENCE mandatory	}|
	{ ID id-NASSecurityParametersFromNGRAN				CRITICALITY reject	TYPE NASSecurityParametersFromNGRAN					PRESENCE conditional	}|
-- The above IE shall be present if the HandoverType IE is set to the value “5GStoEPPS” or “5GStoUTRAN”
	{ ID id-PDUSessionResourceHandoverList				CRITICALITY ignore	TYPE PDUSessionResourceHandoverList					PRESENCE optional		}|
	{ ID id-PDUSessionResourceToReleaseListHOCmd		CRITICALITY ignore	TYPE PDUSessionResourceToReleaseListHOCmd			PRESENCE optional		}|
	{ ID id-TargetToSource-TransparentContainer			CRITICALITY reject	TYPE TargetToSource-TransparentContainer			PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}


-- **************************************************************
--
-- HANDOVER PREPARATION FAILURE
--
-- **************************************************************

HandoverPreparationFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverPreparationFailureIEs} },
	...
}

HandoverPreparationFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		}|
	{ ID id-TargettoSource-Failure-TransparentContainer		CRITICALITY ignore	TYPE TargettoSource-Failure-TransparentContainer		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Handover Resource Allocation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER REQUEST
--
-- **************************************************************

HandoverRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverRequestIEs} },
	...
}

HandoverRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-HandoverType							CRITICALITY reject	TYPE HandoverType									PRESENCE mandatory	}|
	{ ID id-Cause									CRITICALITY ignore	TYPE Cause											PRESENCE mandatory	}|
	{ ID id-UEAggregateMaximumBitRate				CRITICALITY reject	TYPE UEAggregateMaximumBitRate					PRESENCE mandatory	}|
	{ ID id-CoreNetworkAssistanceInformationForInactive		CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive		PRESENCE optional		}|
	{ ID id-UESecurityCapabilities					CRITICALITY reject	TYPE UESecurityCapabilities						PRESENCE mandatory	}|
	{ ID id-SecurityContext							CRITICALITY reject	TYPE SecurityContext								PRESENCE mandatory	}|
	{ ID id-NewSecurityContextInd					CRITICALITY reject	TYPE NewSecurityContextInd						PRESENCE optional		}|
	{ ID id-NASC									CRITICALITY reject	TYPE NAS-PDU										PRESENCE optional		}|
	{ ID id-PDUSessionResourceSetupListHOReq		CRITICALITY reject	TYPE PDUSessionResourceSetupListHOReq			PRESENCE mandatory	}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI									PRESENCE mandatory	}|
	{ ID id-TraceActivation							CRITICALITY ignore	TYPE TraceActivation								PRESENCE optional		}|
	{ ID id-MaskedIMEISV							CRITICALITY ignore	TYPE MaskedIMEISV									PRESENCE optional		}|
	{ ID id-SourceToTarget-TransparentContainer		CRITICALITY reject	TYPE SourceToTarget-TransparentContainer		PRESENCE mandatory	}|
	{ ID id-MobilityRestrictionList					CRITICALITY ignore	TYPE MobilityRestrictionList						PRESENCE optional		}|
	{ ID id-LocationReportingRequestType			CRITICALITY ignore	TYPE LocationReportingRequestType				PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest		CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest		PRESENCE optional		}|
	{ ID id-GUAMI									CRITICALITY reject	TYPE GUAMI											PRESENCE mandatory	}|
	{ ID id-RedirectionVoiceFallback				CRITICALITY ignore	TYPE RedirectionVoiceFallback					PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning						CRITICALITY ignore	TYPE CNAssistedRANTuning							PRESENCE optional		}|
	{ ID id-SRVCCOperationPossible					CRITICALITY ignore	TYPE SRVCCOperationPossible						PRESENCE optional		}|
	{ ID id-IAB-Authorized							CRITICALITY reject	TYPE IAB-Authorized									PRESENCE optional		}|
	{ ID id-Enhanced-CoverageRestriction			CRITICALITY ignore	TYPE Enhanced-CoverageRestriction				PRESENCE optional		}|
	{ ID id-UE-DifferentiationInfo					CRITICALITY ignore	TYPE UE-DifferentiationInfo						PRESENCE optional		}|
	{ ID id-NRV2XServicesAuthorized					CRITICALITY ignore	TYPE NRV2XServicesAuthorized						PRESENCE optional		}|
	{ ID id-LTEV2XServicesAuthorized				CRITICALITY ignore	TYPE LTEV2XServicesAuthorized					PRESENCE optional		}|
	{ ID id-NRUESidelinkAggregateMaximumBitrate		CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-LTEUESidelinkAggregateMaximumBitrate	CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate	PRESENCE optional		}|
	{ ID id-PC5QoSParameters						CRITICALITY ignore	TYPE PC5QoSParameters								PRESENCE optional 	}|
	{ ID id-CEmodeBrestricted						CRITICALITY ignore	TYPE CEmodeBrestricted								PRESENCE optional		}|
	{ ID id-UE-UP-CIoT-Support						CRITICALITY ignore	TYPE UE-UP-CIoT-Support								PRESENCE optional		}|
	{ ID id-ManagementBasedMDTPLMNList				CRITICALITY ignore	TYPE MDTPLMNList									PRESENCE optional		}|
	{ ID id-UERadioCapabilityID						CRITICALITY reject	TYPE UERadioCapabilityID							PRESENCE optional		}|
	{ ID id-Extended-ConnectedTime					CRITICALITY ignore	TYPE Extended-ConnectedTime						PRESENCE optional		}|
	{ ID id-TimeSyncAssistanceInfo					CRITICALITY ignore	TYPE TimeSyncAssistanceInfo						PRESENCE optional		}|
	{ ID id-UESliceMaximumBitRateList				CRITICALITY ignore	TYPE UESliceMaximumBitRateList					PRESENCE optional		}|
	{ ID id-FiveG-ProSeAuthorized					CRITICALITY ignore	TYPE FiveG-ProSeAuthorized						PRESENCE optional		}|
	{ ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate	CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-FiveG-ProSePC5QoSParameters				CRITICALITY ignore	TYPE FiveG-ProSePC5QoSParameters				PRESENCE optional		}|
	{ ID id-AerialUEsubscriptionInformation			CRITICALITY ignore	TYPE AerialUEsubscriptionInformation			PRESENCE optional		}|
	{ ID id-NR-A2X-ServicesAuthorized				CRITICALITY ignore	TYPE NR-A2X-ServicesAuthorized					PRESENCE optional		}|
	{ ID id-LTE-A2X-ServicesAuthorized				CRITICALITY ignore	TYPE LTE-A2X-ServicesAuthorized					PRESENCE optional		}|
	{ ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate	CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate	CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate	PRESENCE optional		}|
	{ ID id-A2X-PC5-QoS-Parameters					CRITICALITY ignore	TYPE A2X-PC5-QoS-Parameters						PRESENCE optional		}|
	{ ID id-MobileIAB-Authorized					CRITICALITY ignore	TYPE MobileIAB-Authorized							PRESENCE optional		}|
	{ ID id-NoPDUSessionIndication					CRITICALITY ignore	TYPE NoPDUSessionIndication 						PRESENCE optional		}|
	{ ID id-Partially-Allowed-NSSAI					CRITICALITY ignore	TYPE Partially-Allowed-NSSAI						PRESENCE optional		}|
	{ ID id-SLPositioningRangingServiceInfo			CRITICALITY ignore	TYPE SLPositioningRangingServiceInfo			PRESENCE optional		}|
	{ ID id-AMF-UE-NGAP-ID2							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID									PRESENCE optional		}|
	{ ID id-Target-RAN-Node-ID						CRITICALITY ignore	TYPE GlobalRANNodeID								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- HANDOVER REQUEST ACKNOWLEDGE
--
-- **************************************************************

HandoverRequestAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {HandoverRequestAcknowledgeIEs} },
	...
}

HandoverRequestAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceAdmittedList				CRITICALITY ignore	TYPE PDUSessionResourceAdmittedList					PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceFailedToSetupListHOAck	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListHOAck		PRESENCE optional		}|
	{ ID id-TargetToSource-TransparentContainer			CRITICALITY reject	TYPE TargetToSource-TransparentContainer			PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		}|
	{ ID id-NPN-AccessInformation						CRITICALITY reject	TYPE NPN-AccessInformation								PRESENCE optional		}|
	{ ID id-RedCapIndication							CRITICALITY ignore	TYPE RedCapIndication										PRESENCE optional		}|
	{ ID id-ERedCapIndication							CRITICALITY ignore	TYPE ERedCapIndication									PRESENCE optional		},
	...
}


-- **************************************************************
--
-- HANDOVER FAILURE
--
-- **************************************************************

HandoverFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverFailureIEs} },
	...
}

HandoverFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		}|
	{ ID id-TargettoSource-Failure-TransparentContainer		CRITICALITY ignore	TYPE TargettoSource-Failure-TransparentContainer		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Handover Notification Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER NOTIFY
--
-- **************************************************************

HandoverNotify ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverNotifyIEs} },
	...
}

HandoverNotifyIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation	PRESENCE mandatory	}|
	{ ID id-NotifySourceNGRANNode		CRITICALITY ignore	TYPE NotifySourceNGRANNode		PRESENCE optional   	},
	...
}

-- **************************************************************
--
-- Path Switch Request Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PATH SWITCH REQUEST
--
-- **************************************************************

PathSwitchRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { PathSwitchRequestIEs} },
	...
}

PathSwitchRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-SourceAMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation							PRESENCE mandatory	}|
	{ ID id-UESecurityCapabilities						CRITICALITY ignore	TYPE UESecurityCapabilities								PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceToBeSwitchedDLList		CRITICALITY reject	TYPE PDUSessionResourceToBeSwitchedDLList			PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceFailedToSetupListPSReq	CRITICALITY ignore	TYPE PDUSessionResourceFailedToSetupListPSReq		PRESENCE optional		}|
	{ ID id-RRC-Resume-Cause							CRITICALITY ignore	TYPE RRCEstablishmentCause								PRESENCE optional		}|
	{ ID id-RedCapIndication							CRITICALITY ignore	TYPE RedCapIndication										PRESENCE optional		}|
	{ ID id-ERedCapIndication							CRITICALITY ignore	TYPE ERedCapIndication									PRESENCE optional		}|
	{ ID id-SourceAMF-GUAMI							CRITICALITY ignore	TYPE GUAMI													PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PATH SWITCH REQUEST ACKNOWLEDGE
--
-- **************************************************************

PathSwitchRequestAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { PathSwitchRequestAcknowledgeIEs} },
	...
}

PathSwitchRequestAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-UESecurityCapabilities						CRITICALITY reject	TYPE UESecurityCapabilities							PRESENCE optional		}|
	{ ID id-SecurityContext								CRITICALITY reject	TYPE SecurityContext									PRESENCE mandatory	}|
	{ ID id-NewSecurityContextInd						CRITICALITY reject	TYPE NewSecurityContextInd							PRESENCE optional		}|
	{ ID id-PDUSessionResourceSwitchedList				CRITICALITY ignore	TYPE PDUSessionResourceSwitchedList				PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceReleasedListPSAck			CRITICALITY ignore	TYPE PDUSessionResourceReleasedListPSAck		PRESENCE optional		}|
	{ ID id-AllowedNSSAI								CRITICALITY reject	TYPE AllowedNSSAI										PRESENCE mandatory	}|
	{ ID id-CoreNetworkAssistanceInformationForInactive		CRITICALITY ignore	TYPE CoreNetworkAssistanceInformationForInactive		PRESENCE optional		}|
	{ ID id-RRCInactiveTransitionReportRequest			CRITICALITY ignore	TYPE RRCInactiveTransitionReportRequest			PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		}|
	{ ID id-RedirectionVoiceFallback					CRITICALITY ignore	TYPE RedirectionVoiceFallback						PRESENCE optional		}|
	{ ID id-CNAssistedRANTuning							CRITICALITY ignore	TYPE CNAssistedRANTuning								PRESENCE optional		}|
	{ ID id-SRVCCOperationPossible						CRITICALITY ignore	TYPE SRVCCOperationPossible							PRESENCE optional		}|
	{ ID id-Enhanced-CoverageRestriction				CRITICALITY ignore	TYPE Enhanced-CoverageRestriction					PRESENCE optional		}|
	{ ID id-Extended-ConnectedTime						CRITICALITY ignore	TYPE Extended-ConnectedTime							PRESENCE optional		}|
	{ ID id-UE-DifferentiationInfo						CRITICALITY ignore	TYPE UE-DifferentiationInfo							PRESENCE optional		}|
	{ ID id-NRV2XServicesAuthorized						CRITICALITY ignore	TYPE NRV2XServicesAuthorized						PRESENCE optional		}|
	{ ID id-LTEV2XServicesAuthorized					CRITICALITY ignore	TYPE LTEV2XServicesAuthorized						PRESENCE optional		}|
	{ ID id-NRUESidelinkAggregateMaximumBitrate			CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-LTEUESidelinkAggregateMaximumBitrate		CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-PC5QoSParameters							CRITICALITY ignore	TYPE PC5QoSParameters									PRESENCE optional 	}|
	{ ID id-CEmodeBrestricted							CRITICALITY ignore	TYPE CEmodeBrestricted								PRESENCE optional		}|
	{ ID id-UE-UP-CIoT-Support							CRITICALITY ignore	TYPE UE-UP-CIoT-Support								PRESENCE optional		}|
	{ ID id-UERadioCapabilityID							CRITICALITY reject	TYPE UERadioCapabilityID								PRESENCE optional		}|
	{ ID id-ManagementBasedMDTPLMNList					CRITICALITY ignore	TYPE MDTPLMNList										PRESENCE optional		}|
	{ ID id-TimeSyncAssistanceInfo						CRITICALITY ignore	TYPE TimeSyncAssistanceInfo							PRESENCE optional		}|
	{ ID id-FiveG-ProSeAuthorized						CRITICALITY ignore	TYPE FiveG-ProSeAuthorized							PRESENCE optional		}|
	{ ID id-FiveG-ProSeUEPC5AggregateMaximumBitRate		CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-FiveG-ProSePC5QoSParameters					CRITICALITY ignore	TYPE FiveG-ProSePC5QoSParameters					PRESENCE optional		}|
	{ ID id-ManagementBasedMDTPLMNModificationList		CRITICALITY ignore	TYPE MDTPLMNModificationList						PRESENCE optional		}|
	{ ID id-IAB-Authorized								CRITICALITY ignore	TYPE IAB-Authorized										PRESENCE optional		}|
	{ ID id-AerialUEsubscriptionInformation				CRITICALITY ignore	TYPE AerialUEsubscriptionInformation				PRESENCE optional		}|
	{ ID id-NR-A2X-ServicesAuthorized					CRITICALITY ignore	TYPE NR-A2X-ServicesAuthorized						PRESENCE optional		}|
	{ ID id-LTE-A2X-ServicesAuthorized					CRITICALITY ignore	TYPE LTE-A2X-ServicesAuthorized					PRESENCE optional		}|
	{ ID id-NR-A2X-UE-PC5-AggregateMaximumBitRate		CRITICALITY ignore	TYPE NRUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-LTE-A2X-UE-PC5-AggregateMaximumBitRate		CRITICALITY ignore	TYPE LTEUESidelinkAggregateMaximumBitrate		PRESENCE optional		}|
	{ ID id-A2X-PC5-QoS-Parameters						CRITICALITY ignore	TYPE A2X-PC5-QoS-Parameters							PRESENCE optional		}|
	{ ID id-MobileIAB-Authorized				   	    CRITICALITY ignore	TYPE MobileIAB-Authorized							PRESENCE optional		}|
	{ ID id-Partially-Allowed-NSSAI						CRITICALITY ignore	TYPE Partially-Allowed-NSSAI						PRESENCE optional		}|
	{ ID id-SLPositioningRangingServiceInfo				CRITICALITY ignore	TYPE SLPositioningRangingServiceInfo				PRESENCE optional		}|
	{ ID id-AMF-UE-NGAP-ID2								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID										PRESENCE optional		},
	...
}


-- **************************************************************
--
-- PATH SWITCH REQUEST FAILURE
--
-- **************************************************************

PathSwitchRequestFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { PathSwitchRequestFailureIEs} },
	...
}

PathSwitchRequestFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY ignore	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceReleasedListPSFail	CRITICALITY ignore	TYPE PDUSessionResourceReleasedListPSFail	PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Handover Cancellation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER CANCEL
--
-- **************************************************************

HandoverCancel ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverCancelIEs} },
	...
}

HandoverCancelIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID		CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID		CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-Cause				CRITICALITY ignore	TYPE Cause				PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- HANDOVER CANCEL ACKNOWLEDGE
--
-- **************************************************************

HandoverCancelAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { HandoverCancelAcknowledgeIEs} },
	...
}

HandoverCancelAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- HANDOVER SUCCESS ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- HANDOVER SUCCESS
--
-- **************************************************************

HandoverSuccess ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container       { { HandoverSuccessIEs} },
	...
}

HandoverSuccessIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID		CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID		CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UPLINK RAN EARLY STATUS TRANSFER ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- Uplink RAN Early Status Transfer
--
-- **************************************************************

UplinkRANEarlyStatusTransfer ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container       { {UplinkRANEarlyStatusTransferIEs} },
	...
}

UplinkRANEarlyStatusTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-EarlyStatusTransfer-TransparentContainer    CRITICALITY reject  TYPE EarlyStatusTransfer-TransparentContainer		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- DOWNLINK RAN EARLY STATUS TRANSFER ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- Downlink RAN Early Status Transfer
--
-- **************************************************************

DownlinkRANEarlyStatusTransfer ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container       { {DownlinkRANEarlyStatusTransferIEs} },
	...
}

DownlinkRANEarlyStatusTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-EarlyStatusTransfer-TransparentContainer	CRITICALITY reject	TYPE EarlyStatusTransfer-TransparentContainer		PRESENCE mandatory	},
	...
}


-- **************************************************************
--
-- Uplink RAN Status Transfer Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UPLINK RAN STATUS TRANSFER
--
-- **************************************************************

UplinkRANStatusTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkRANStatusTransferIEs} },
	...
}

UplinkRANStatusTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RANStatusTransfer-TransparentContainer		CRITICALITY reject	TYPE RANStatusTransfer-TransparentContainer	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- Downlink RAN Status Transfer Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- DOWNLINK RAN STATUS TRANSFER
--
-- **************************************************************

DownlinkRANStatusTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkRANStatusTransferIEs} },
	...
}

DownlinkRANStatusTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY reject	TYPE AMF-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY reject	TYPE RAN-UE-NGAP-ID											PRESENCE mandatory	}|
	{ ID id-RANStatusTransfer-TransparentContainer		CRITICALITY reject	TYPE RANStatusTransfer-TransparentContainer		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- PAGING ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- PAGING
--
-- **************************************************************

Paging ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PagingIEs} },
	...
}

PagingIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UEPagingIdentity				CRITICALITY ignore	TYPE UEPagingIdentity					PRESENCE mandatory	}|
	{ ID id-PagingDRX						CRITICALITY ignore	TYPE PagingDRX							PRESENCE optional		}|
	{ ID id-TAIListForPaging				CRITICALITY ignore	TYPE TAIListForPaging					PRESENCE mandatory	}|
	{ ID id-PagingPriority					CRITICALITY ignore	TYPE PagingPriority						PRESENCE optional		}|
	{ ID id-UERadioCapabilityForPaging		CRITICALITY ignore	TYPE UERadioCapabilityForPaging			PRESENCE optional		}|
	{ ID id-PagingOrigin					CRITICALITY ignore	TYPE PagingOrigin						PRESENCE optional		}|
	{ ID id-AssistanceDataForPaging			CRITICALITY ignore	TYPE AssistanceDataForPaging			PRESENCE optional		}|
	{ ID id-NB-IoT-Paging-eDRXInfo			CRITICALITY ignore	TYPE NB-IoT-Paging-eDRXInfo				PRESENCE optional		}|
	{ ID id-NB-IoT-PagingDRX				CRITICALITY ignore	TYPE NB-IoT-PagingDRX					PRESENCE optional		}|
	{ ID id-Enhanced-CoverageRestriction	CRITICALITY ignore	TYPE Enhanced-CoverageRestriction		PRESENCE optional		}|
	{ ID id-WUS-Assistance-Information		CRITICALITY ignore	TYPE WUS-Assistance-Information			PRESENCE optional		}|
	{ ID id-EUTRA-PagingeDRXInformation		CRITICALITY ignore	TYPE EUTRA-PagingeDRXInformation		PRESENCE optional		}|
	{ ID id-CEmodeBrestricted				CRITICALITY ignore	TYPE CEmodeBrestricted					PRESENCE optional		}|
	{ ID id-NR-PagingeDRXInformation		CRITICALITY ignore	TYPE NR-PagingeDRXInformation			PRESENCE optional		}|
	{ ID id-PagingCause						CRITICALITY ignore	TYPE PagingCause						PRESENCE optional		}|
	{ ID id-PEIPSassistanceInformation		CRITICALITY ignore	TYPE PEIPSassistanceInformation			PRESENCE optional		}|
	{ ID id-LPWUSPSAssistanceInformation	CRITICALITY ignore	TYPE LPWUSPSAssistanceInformation		PRESENCE optional		}|
	{ ID id-LPWUSDisableIndication      	CRITICALITY ignore	TYPE LPWUSDisableIndication  		   PRESENCE optional		},
	...
}

-- **************************************************************
--
-- NAS TRANSPORT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- INITIAL UE MESSAGE
--
-- **************************************************************

InitialUEMessage ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InitialUEMessage-IEs} },
	...
}

InitialUEMessage-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-NAS-PDU									CRITICALITY reject	TYPE NAS-PDU										PRESENCE mandatory	}|
	{ ID id-UserLocationInformation					CRITICALITY reject	TYPE UserLocationInformation						PRESENCE mandatory	}|
	{ ID id-RRCEstablishmentCause					CRITICALITY ignore	TYPE RRCEstablishmentCause						PRESENCE mandatory	}|
	{ ID id-FiveG-S-TMSI							CRITICALITY reject	TYPE FiveG-S-TMSI									PRESENCE optional		}|
	{ ID id-AMFSetID								CRITICALITY ignore	TYPE AMFSetID										PRESENCE optional		}|
	{ ID id-UEContextRequest						CRITICALITY ignore	TYPE UEContextRequest								PRESENCE optional		}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI									PRESENCE optional		}|
	{ ID id-SourceToTarget-AMFInformationReroute	CRITICALITY ignore	TYPE SourceToTarget-AMFInformationReroute	PRESENCE optional		}|
	{ ID id-SelectedPLMNIdentity					CRITICALITY ignore	TYPE PLMNIdentity									PRESENCE optional		}|
	{ ID id-IABNodeIndication						CRITICALITY reject	TYPE IABNodeIndication								PRESENCE optional		}|
	{ ID id-CEmodeBSupport-Indicator				CRITICALITY reject	TYPE CEmodeBSupport-Indicator					PRESENCE optional		}|
	{ ID id-LTEM-Indication							CRITICALITY ignore	TYPE LTEM-Indication								PRESENCE optional		}|
	{ ID id-EDT-Session								CRITICALITY ignore	TYPE EDT-Session									PRESENCE optional		}|
	{ ID id-AuthenticatedIndication					CRITICALITY ignore	TYPE AuthenticatedIndication						PRESENCE optional		}|
	{ ID id-NPN-AccessInformation					CRITICALITY reject	TYPE NPN-AccessInformation						PRESENCE optional		}|
	{ ID id-RedCapIndication						CRITICALITY ignore	TYPE RedCapIndication								PRESENCE optional		}|
	{ ID id-SelectedNID								CRITICALITY ignore	TYPE NID											PRESENCE optional		}|
	{ ID id-MobileIABNodeIndication					CRITICALITY reject	TYPE MobileIABNodeIndication						PRESENCE optional		}|
	{ ID id-Partially-Allowed-NSSAI					CRITICALITY ignore	TYPE Partially-Allowed-NSSAI	   				PRESENCE optional		}|
	{ ID id-ERedCapIndication						CRITICALITY ignore	TYPE ERedCapIndication								PRESENCE optional		}|
	{ ID id-AUN3DeviceAccessInfo					CRITICALITY ignore	TYPE AUN3DeviceAccessInfo							PRESENCE optional		}|
	{ ID id-GUAMI									CRITICALITY ignore	TYPE GUAMI											PRESENCE optional		}|
	{ ID id-GUAMIType								CRITICALITY ignore	TYPE GUAMIType										PRESENCE optional		}|
	{ ID id-RequestedNSSAI							CRITICALITY ignore	TYPE RequestedNSSAI								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- DOWNLINK NAS TRANSPORT
--
-- **************************************************************

DownlinkNASTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkNASTransport-IEs} },
	...
}

DownlinkNASTransport-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-OldAMF							CRITICALITY reject	TYPE AMFName						PRESENCE optional		}|
	{ ID id-RANPagingPriority				CRITICALITY ignore	TYPE RANPagingPriority				PRESENCE optional		}|
	{ ID id-NAS-PDU							CRITICALITY reject	TYPE NAS-PDU						PRESENCE mandatory	}|
	{ ID id-MobilityRestrictionList			CRITICALITY ignore	TYPE MobilityRestrictionList		PRESENCE optional		}|
	{ ID id-IndexToRFSP						CRITICALITY ignore	TYPE IndexToRFSP					PRESENCE optional		}|
	{ ID id-UEAggregateMaximumBitRate		CRITICALITY ignore	TYPE UEAggregateMaximumBitRate		PRESENCE optional		}|
	{ ID id-AllowedNSSAI					CRITICALITY reject	TYPE AllowedNSSAI					PRESENCE optional		}|
	{ ID id-SRVCCOperationPossible			CRITICALITY ignore	TYPE SRVCCOperationPossible			PRESENCE optional		}|
	{ ID id-Enhanced-CoverageRestriction	CRITICALITY ignore	TYPE Enhanced-CoverageRestriction	PRESENCE optional		}|
	{ ID id-Extended-ConnectedTime			CRITICALITY ignore	TYPE Extended-ConnectedTime			PRESENCE optional		}|
	{ ID id-UE-DifferentiationInfo			CRITICALITY ignore	TYPE UE-DifferentiationInfo			PRESENCE optional		}|
	{ ID id-CEmodeBrestricted				CRITICALITY ignore	TYPE CEmodeBrestricted				PRESENCE optional		}|
	{ ID id-UERadioCapability				CRITICALITY ignore	TYPE UERadioCapability				PRESENCE optional		}|
	{ ID id-UECapabilityInfoRequest			CRITICALITY ignore	TYPE UECapabilityInfoRequest		PRESENCE optional		}|
	{ ID id-EndIndication					CRITICALITY ignore	TYPE EndIndication					PRESENCE optional		}|
	{ ID id-UERadioCapabilityID				CRITICALITY reject	TYPE UERadioCapabilityID			PRESENCE optional		}|
	{ ID id-TargetNSSAIInformation			CRITICALITY ignore	TYPE TargetNSSAIInformation			PRESENCE optional		}|
	{ ID id-MaskedIMEISV					CRITICALITY ignore	TYPE MaskedIMEISV					PRESENCE optional		}|
	{ ID id-Partially-Allowed-NSSAI			CRITICALITY ignore	TYPE Partially-Allowed-NSSAI		PRESENCE optional		}|
	{ ID id-MobileIAB-Authorized			CRITICALITY ignore	TYPE MobileIAB-Authorized			PRESENCE optional		}|
	{ ID id-ExtendedOldAMF					CRITICALITY ignore	TYPE Extended-AMFName				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UPLINK NAS TRANSPORT
--
-- **************************************************************

UplinkNASTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container	{ {UplinkNASTransport-IEs} },
	...
}

-- WS modification, add a definition for messages
W-AGFIdentityInformation ::= OCTET STRING
TNGFIdentityInformation ::= OCTET STRING
TWIFIdentityInformation ::= OCTET STRING

UplinkNASTransport-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-NAS-PDU						CRITICALITY reject	TYPE NAS-PDU						PRESENCE mandatory	}|
	{ ID id-UserLocationInformation		CRITICALITY ignore	TYPE UserLocationInformation		PRESENCE mandatory	}|
-- WS modification, add a definition for messages
--	{ ID id-W-AGFIdentityInformation	CRITICALITY reject	TYPE OCTET STRING					PRESENCE optional	}|
	{ ID id-W-AGFIdentityInformation	CRITICALITY reject	TYPE W-AGFIdentityInformation					PRESENCE optional	}|
--	{ ID id-TNGFIdentityInformation		CRITICALITY reject	TYPE OCTET STRING					PRESENCE optional	}|
	{ ID id-TNGFIdentityInformation		CRITICALITY reject	TYPE TNGFIdentityInformation					PRESENCE optional	}|
--	{ ID id-TWIFIdentityInformation		CRITICALITY reject	TYPE OCTET STRING					PRESENCE optional	},
	{ ID id-TWIFIdentityInformation		CRITICALITY reject	TYPE TWIFIdentityInformation					PRESENCE optional	},
	...
}

-- **************************************************************
--
-- NAS NON DELIVERY INDICATION
--
-- **************************************************************

NASNonDeliveryIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NASNonDeliveryIndication-IEs} },
	...
}

NASNonDeliveryIndication-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID		CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID		CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-NAS-PDU				CRITICALITY ignore	TYPE NAS-PDU			PRESENCE mandatory	}|
	{ ID id-Cause				CRITICALITY ignore	TYPE Cause				PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- REROUTE NAS REQUEST
--
-- **************************************************************

RerouteNASRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RerouteNASRequest-IEs} },
	...
}

-- WS modification, add a definition for NGAP Message
NGAP-Message ::= OCTET STRING

RerouteNASRequest-IEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID									PRESENCE mandatory	}|
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY ignore	TYPE AMF-UE-NGAP-ID									PRESENCE optional		}|
-- WS modification, add a definition for NGAP Message
--	{ ID id-NGAP-Message							CRITICALITY reject	TYPE OCTET STRING									PRESENCE mandatory	}|
	{ ID id-NGAP-Message							CRITICALITY reject	TYPE NGAP-Message									PRESENCE mandatory	}|
	{ ID id-AMFSetID								CRITICALITY reject	TYPE AMFSetID										PRESENCE mandatory	}|
	{ ID id-AllowedNSSAI							CRITICALITY reject	TYPE AllowedNSSAI									PRESENCE optional		}|
	{ ID id-SourceToTarget-AMFInformationReroute	CRITICALITY ignore	TYPE SourceToTarget-AMFInformationReroute	PRESENCE optional 	}|
	{ ID id-Partially-Allowed-NSSAI					CRITICALITY ignore	TYPE Partially-Allowed-NSSAI	               PRESENCE optional		},
	...
}

-- **************************************************************
--
-- INTERFACE MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- NG Removal Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- NG REMOVAL REQUEST
--
-- **************************************************************

NGRemovalRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGRemovalRequestIEs} },
	...
}

NGRemovalRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-GlobalRANNodeID				CRITICALITY reject	TYPE GlobalRANNodeID				PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NG REMOVAL RESPONSE
--
-- **************************************************************

NGRemovalResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGRemovalResponseIEs} },
	...
}

NGRemovalResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMFName 					CRITICALITY reject	TYPE AMFName					PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		}|
	{ ID id-Extended-AMFName			CRITICALITY ignore	TYPE Extended-AMFName			PRESENCE optional		},
	...
}

-- **************************************************************
--
-- NG REMOVAL FAILURE
--
-- **************************************************************

NGRemovalFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGRemovalFailureIEs} },
	...
}

NGRemovalFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- NG Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- NG SETUP REQUEST
--
-- **************************************************************

NGSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGSetupRequestIEs} },
	...
}

NGSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-GlobalRANNodeID				CRITICALITY reject	TYPE GlobalRANNodeID				PRESENCE mandatory	}|
	{ ID id-RANNodeName					CRITICALITY ignore	TYPE RANNodeName					PRESENCE optional	}|
	{ ID id-SupportedTAList				CRITICALITY reject	TYPE SupportedTAList				PRESENCE mandatory	}|
	{ ID id-DefaultPagingDRX			CRITICALITY ignore	TYPE PagingDRX						PRESENCE mandatory	}|
	{ ID id-UERetentionInformation		CRITICALITY ignore	TYPE UERetentionInformation			PRESENCE optional	}|
	{ ID id-NB-IoT-DefaultPagingDRX		CRITICALITY ignore	TYPE NB-IoT-DefaultPagingDRX		PRESENCE optional	}|
	{ ID id-Extended-RANNodeName		CRITICALITY ignore	TYPE Extended-RANNodeName			PRESENCE optional	}|
	{ ID id-AIoT-Support				CRITICALITY reject	TYPE AIoT-Support					PRESENCE optional	}|
	{ ID id-AdditionalULI				CRITICALITY ignore	TYPE AdditionalULI 					PRESENCE optional	},
	...
}

-- **************************************************************
--
-- NG SETUP RESPONSE
--
-- **************************************************************

NGSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGSetupResponseIEs} },
	...
}

NGSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMFName						CRITICALITY reject	TYPE AMFName					PRESENCE mandatory	}|
	{ ID id-ServedGUAMIList				CRITICALITY reject	TYPE ServedGUAMIList			PRESENCE mandatory	}|
	{ ID id-RelativeAMFCapacity			CRITICALITY ignore	TYPE RelativeAMFCapacity		PRESENCE mandatory	}|
	{ ID id-PLMNSupportList				CRITICALITY reject	TYPE PLMNSupportList			PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		}|
	{ ID id-UERetentionInformation		CRITICALITY ignore	TYPE UERetentionInformation		PRESENCE optional		}|
	{ ID id-IAB-Supported				CRITICALITY ignore	TYPE IAB-Supported				PRESENCE optional		}|
	{ ID id-Extended-AMFName			CRITICALITY ignore	TYPE Extended-AMFName			PRESENCE optional		}|
	{ ID id-MobileIAB-Supported			CRITICALITY ignore	TYPE MobileIAB-Supported    	PRESENCE optional		}|
	{ ID id-AIOTFIdentifier				CRITICALITY reject	TYPE AIOTFIdentifier			PRESENCE optional		}|
	{ ID id-AIOTFName					CRITICALITY reject	TYPE AIOTFName					PRESENCE optional		},
	...
}

-- **************************************************************
--
-- NG SETUP FAILURE
--
-- **************************************************************

NGSetupFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGSetupFailureIEs} },
	...
}

NGSetupFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-TimeToWait					CRITICALITY ignore	TYPE TimeToWait					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- RAN Configuration Update Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- RAN CONFIGURATION UPDATE
--
-- **************************************************************

RANConfigurationUpdate ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RANConfigurationUpdateIEs} },
	...
}

RANConfigurationUpdateIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RANNodeName								CRITICALITY ignore	TYPE RANNodeName									PRESENCE optional	}|
	{ ID id-SupportedTAList							CRITICALITY reject	TYPE SupportedTAList								PRESENCE optional	}|
	{ ID id-DefaultPagingDRX						CRITICALITY ignore	TYPE PagingDRX										PRESENCE optional	}|
	{ ID id-GlobalRANNodeID							CRITICALITY ignore	TYPE GlobalRANNodeID								PRESENCE optional	}|
	{ ID id-NGRAN-TNLAssociationToRemoveList		CRITICALITY reject	TYPE NGRAN-TNLAssociationToRemoveList			PRESENCE optional	}|
	{ ID id-NB-IoT-DefaultPagingDRX					CRITICALITY ignore	TYPE NB-IoT-DefaultPagingDRX						PRESENCE optional	}|
	{ ID id-Extended-RANNodeName					CRITICALITY ignore	TYPE Extended-RANNodeName							PRESENCE optional	}|
	{ ID id-AdditionalULI							CRITICALITY ignore	TYPE AdditionalULI 									PRESENCE optional	}|
	{ ID id-AIoT-Support							CRITICALITY reject	TYPE AIoT-Support									PRESENCE optional	},
	...
}

-- **************************************************************
--
-- RAN CONFIGURATION UPDATE ACKNOWLEDGE
--
-- **************************************************************

RANConfigurationUpdateAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RANConfigurationUpdateAcknowledgeIEs} },
	...
}

RANConfigurationUpdateAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- RAN CONFIGURATION UPDATE FAILURE
--
-- **************************************************************

RANConfigurationUpdateFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {RANConfigurationUpdateFailureIEs} },
	...
}

RANConfigurationUpdateFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-TimeToWait					CRITICALITY ignore	TYPE TimeToWait					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
...
}

-- **************************************************************
--
-- AMF Configuration Update Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- AMF CONFIGURATION UPDATE
--
-- **************************************************************

AMFConfigurationUpdate ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFConfigurationUpdateIEs} },
	...
}

AMFConfigurationUpdateIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMFName								CRITICALITY reject	TYPE AMFName								PRESENCE optional		}|
	{ ID id-ServedGUAMIList						CRITICALITY reject	TYPE ServedGUAMIList						PRESENCE optional		}|
	{ ID id-RelativeAMFCapacity					CRITICALITY ignore	TYPE RelativeAMFCapacity					PRESENCE optional		}|
	{ ID id-PLMNSupportList						CRITICALITY reject	TYPE PLMNSupportList						PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationToAddList			CRITICALITY ignore	TYPE AMF-TNLAssociationToAddList			PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationToRemoveList		CRITICALITY ignore	TYPE AMF-TNLAssociationToRemoveList		PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationToUpdateList		CRITICALITY ignore	TYPE AMF-TNLAssociationToUpdateList		PRESENCE optional		}|
	{ ID id-Extended-AMFName					CRITICALITY ignore	TYPE Extended-AMFName						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- AMF CONFIGURATION UPDATE ACKNOWLEDGE
--
-- **************************************************************

AMFConfigurationUpdateAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFConfigurationUpdateAcknowledgeIEs} },
	...
}

AMFConfigurationUpdateAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-TNLAssociationSetupList				CRITICALITY ignore	TYPE AMF-TNLAssociationSetupList			PRESENCE optional		}|
	{ ID id-AMF-TNLAssociationFailedToSetupList		CRITICALITY ignore	TYPE TNLAssociationList							PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics					PRESENCE optional		},
	...
}

-- **************************************************************
--
-- AMF CONFIGURATION UPDATE FAILURE
--
-- **************************************************************

AMFConfigurationUpdateFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFConfigurationUpdateFailureIEs} },
	...
}

AMFConfigurationUpdateFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-TimeToWait					CRITICALITY ignore	TYPE TimeToWait					PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- AMF Status Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- AMF STATUS INDICATION
--
-- **************************************************************

AMFStatusIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AMFStatusIndicationIEs} },
	...
}

AMFStatusIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UnavailableGUAMIList		CRITICALITY reject	TYPE UnavailableGUAMIList		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NG Reset Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- NG RESET
--
-- **************************************************************

NGReset ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGResetIEs} },
	...
}

NGResetIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-ResetType					CRITICALITY reject	TYPE ResetType					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NG RESET ACKNOWLEDGE
--
-- **************************************************************

NGResetAcknowledge ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {NGResetAcknowledgeIEs} },
	...
}

NGResetAcknowledgeIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UE-associatedLogicalNG-connectionList			CRITICALITY ignore	TYPE UE-associatedLogicalNG-connectionList			PRESENCE optional	}|
	{ ID id-CriticalityDiagnostics							CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional	},
	...
}

-- **************************************************************
--
-- Error Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- ERROR INDICATION
--
-- **************************************************************

ErrorIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {ErrorIndicationIEs} },
	...
}

ErrorIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY ignore	TYPE AMF-UE-NGAP-ID				PRESENCE optional		}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY ignore	TYPE RAN-UE-NGAP-ID				PRESENCE optional		}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		}|
	{ ID id-FiveG-S-TMSI				CRITICALITY ignore	TYPE FiveG-S-TMSI				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- OVERLOAD START
--
-- **************************************************************

OverloadStart ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {OverloadStartIEs} },
	...
}

OverloadStartIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMFOverloadResponse						CRITICALITY reject	TYPE OverloadResponse							PRESENCE optional 	}|
	{ ID id-AMFTrafficLoadReductionIndication		CRITICALITY ignore	TYPE TrafficLoadReductionIndication		PRESENCE optional		}|
	{ ID id-OverloadStartNSSAIList					CRITICALITY ignore	TYPE OverloadStartNSSAIList					PRESENCE optional		}|
	{ ID id-GUAMIList						CRITICALITY ignore	TYPE GUAMIList									PRESENCE optional		},
	...
}

-- **************************************************************
--
-- OVERLOAD STOP
--
-- **************************************************************

OverloadStop ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {OverloadStopIEs} },
	...
}

OverloadStopIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-GUAMIList			CRITICALITY ignore	TYPE GUAMIList		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- CONFIGURATION TRANSFER ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UPLINK RAN CONFIGURATION TRANSFER
--
-- **************************************************************

UplinkRANConfigurationTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkRANConfigurationTransferIEs} },
	...
}

UplinkRANConfigurationTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-SONConfigurationTransferUL					CRITICALITY ignore	TYPE SONConfigurationTransfer						PRESENCE optional		}|
	{ ID id-ENDC-SONConfigurationTransferUL				CRITICALITY ignore	TYPE EN-DCSONConfigurationTransfer				PRESENCE optional		}|
	{ ID id-IntersystemSONConfigurationTransferUL		CRITICALITY ignore	TYPE IntersystemSONConfigurationTransfer		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- DOWNLINK RAN CONFIGURATION TRANSFER
--
-- **************************************************************

DownlinkRANConfigurationTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkRANConfigurationTransferIEs} },
	...
}

DownlinkRANConfigurationTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-SONConfigurationTransferDL					CRITICALITY ignore	TYPE SONConfigurationTransfer						PRESENCE optional		}|
	{ ID id-ENDC-SONConfigurationTransferDL				CRITICALITY ignore	TYPE EN-DCSONConfigurationTransfer				PRESENCE optional		}|
	{ ID id-IntersystemSONConfigurationTransferDL		CRITICALITY ignore	TYPE IntersystemSONConfigurationTransfer		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- WARNING MESSAGE TRANSMISSION ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Write-Replace Warning Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- WRITE-REPLACE WARNING REQUEST
--
-- **************************************************************

WriteReplaceWarningRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {WriteReplaceWarningRequestIEs} },
	...
}

WriteReplaceWarningRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MessageIdentifier				CRITICALITY reject	TYPE MessageIdentifier					PRESENCE mandatory	}|
	{ ID id-SerialNumber					CRITICALITY reject	TYPE SerialNumber						PRESENCE mandatory	}|
	{ ID id-WarningAreaList					CRITICALITY ignore	TYPE WarningAreaList					PRESENCE optional		}|
	{ ID id-RepetitionPeriod				CRITICALITY reject	TYPE RepetitionPeriod					PRESENCE mandatory	}|
	{ ID id-NumberOfBroadcastsRequested		CRITICALITY reject	TYPE NumberOfBroadcastsRequested		PRESENCE mandatory	}|
	{ ID id-WarningType						CRITICALITY ignore	TYPE WarningType						PRESENCE optional		}|
	{ ID id-WarningSecurityInfo				CRITICALITY ignore	TYPE WarningSecurityInfo				PRESENCE optional		}|
	{ ID id-DataCodingScheme				CRITICALITY ignore	TYPE DataCodingScheme					PRESENCE optional		}|
	{ ID id-WarningMessageContents			CRITICALITY ignore	TYPE WarningMessageContents				PRESENCE optional		}|
	{ ID id-ConcurrentWarningMessageInd		CRITICALITY reject	TYPE ConcurrentWarningMessageInd		PRESENCE optional		}|
	{ ID id-WarningAreaCoordinates			CRITICALITY ignore	TYPE WarningAreaCoordinates				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- WRITE-REPLACE WARNING RESPONSE
--
-- **************************************************************

WriteReplaceWarningResponse ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {WriteReplaceWarningResponseIEs} },
	...
}

WriteReplaceWarningResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MessageIdentifier				CRITICALITY reject	TYPE MessageIdentifier					PRESENCE mandatory	}|
	{ ID id-SerialNumber					CRITICALITY reject	TYPE SerialNumber						PRESENCE mandatory	}|
	{ ID id-BroadcastCompletedAreaList		CRITICALITY ignore	TYPE BroadcastCompletedAreaList			PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics			CRITICALITY ignore	TYPE CriticalityDiagnostics				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PWS Cancel Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PWS CANCEL REQUEST
--
-- **************************************************************

PWSCancelRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSCancelRequestIEs} },
	...
}

PWSCancelRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MessageIdentifier			CRITICALITY reject	TYPE MessageIdentifier				PRESENCE mandatory	}|
	{ ID id-SerialNumber				CRITICALITY reject	TYPE SerialNumber					PRESENCE mandatory	}|
	{ ID id-WarningAreaList				CRITICALITY ignore	TYPE WarningAreaList				PRESENCE optional	}|
	{ ID id-CancelAllWarningMessages	CRITICALITY reject	TYPE CancelAllWarningMessages		PRESENCE optional	},
	...
}

-- **************************************************************
--
-- PWS CANCEL RESPONSE
--
-- **************************************************************

PWSCancelResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSCancelResponseIEs} },
	...
}

PWSCancelResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MessageIdentifier			CRITICALITY reject	TYPE MessageIdentifier				PRESENCE mandatory	}|
	{ ID id-SerialNumber				CRITICALITY reject	TYPE SerialNumber					PRESENCE mandatory	}|
	{ ID id-BroadcastCancelledAreaList	CRITICALITY ignore	TYPE BroadcastCancelledAreaList		PRESENCE optional	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics			PRESENCE optional	},
	...
}

-- **************************************************************
--
-- PWS Restart Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PWS RESTART INDICATION
--
-- **************************************************************

PWSRestartIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSRestartIndicationIEs} },
	...
}

PWSRestartIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-CellIDListForRestart			CRITICALITY reject	TYPE CellIDListForRestart				PRESENCE mandatory	}|
	{ ID id-GlobalRANNodeID					CRITICALITY reject	TYPE GlobalRANNodeID					PRESENCE mandatory	}|
	{ ID id-TAIListForRestart				CRITICALITY reject	TYPE TAIListForRestart					PRESENCE mandatory	}|
	{ ID id-EmergencyAreaIDListForRestart	CRITICALITY reject	TYPE EmergencyAreaIDListForRestart	PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PWS Failure Indication Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- PWS FAILURE INDICATION
--
-- **************************************************************

PWSFailureIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {PWSFailureIndicationIEs} },
	...
}

PWSFailureIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-PWSFailedCellIDList			CRITICALITY reject	TYPE PWSFailedCellIDList	PRESENCE mandatory	}|
	{ ID id-GlobalRANNodeID				CRITICALITY reject	TYPE GlobalRANNodeID		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- NRPPA TRANSPORT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- DOWNLINK UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

DownlinkUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkUEAssociatedNRPPaTransportIEs} },
	...
}

DownlinkUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UPLINK UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

UplinkUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkUEAssociatedNRPPaTransportIEs} },
	...
}

UplinkUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- DOWNLINK NON UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

DownlinkNonUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkNonUEAssociatedNRPPaTransportIEs} },
	...
}

DownlinkNonUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UPLINK NON UE ASSOCIATED NRPPA TRANSPORT
--
-- **************************************************************

UplinkNonUEAssociatedNRPPaTransport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkNonUEAssociatedNRPPaTransportIEs} },
	...
}

UplinkNonUEAssociatedNRPPaTransportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-NRPPa-PDU				CRITICALITY reject	TYPE NRPPa-PDU					PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- TRACE ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- TRACE START
--
-- **************************************************************

TraceStart ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {TraceStartIEs} },
	...
}

TraceStartIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-TraceActivation				CRITICALITY ignore	TYPE TraceActivation			PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- TRACE FAILURE INDICATION
--
-- **************************************************************

TraceFailureIndication ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {TraceFailureIndicationIEs} },
	...
}

TraceFailureIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-NGRANTraceID				CRITICALITY ignore	TYPE NGRANTraceID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- DEACTIVATE TRACE
--
-- **************************************************************

DeactivateTrace ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DeactivateTraceIEs} },
	...
}

DeactivateTraceIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-NGRANTraceID				CRITICALITY ignore	TYPE NGRANTraceID				PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- CELL TRAFFIC TRACE
--
-- **************************************************************

CellTrafficTrace ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {CellTrafficTraceIEs} },
	...
}

CellTrafficTraceIEs NGAP-PROTOCOL-IES ::= {
	{ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ID id-NGRANTraceID						CRITICALITY ignore	TYPE NGRANTraceID				PRESENCE mandatory	}|
	{ID id-NGRAN-CGI						CRITICALITY ignore	TYPE NGRAN-CGI					PRESENCE mandatory	}|
	{ID id-TraceCollectionEntityIPAddress	CRITICALITY ignore	TYPE TransportLayerAddress		PRESENCE mandatory	}|
	{ID id-PrivacyIndicator					CRITICALITY ignore	TYPE PrivacyIndicator			PRESENCE optional	}|
	{ID id-TraceCollectionEntityURI			CRITICALITY ignore	TYPE URI-address				PRESENCE optional	},
	...
}

-- **************************************************************
--
-- LOCATION REPORTING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- LOCATION REPORTING CONTROL
--
-- **************************************************************

LocationReportingControl ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {LocationReportingControlIEs} },
	...
}

LocationReportingControlIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID						PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID						PRESENCE mandatory	}|
	{ ID id-LocationReportingRequestType	CRITICALITY ignore	TYPE LocationReportingRequestType		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- LOCATION REPORTING FAILURE INDICATION
--
-- **************************************************************

LocationReportingFailureIndication ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {LocationReportingFailureIndicationIEs} },
	...
}

LocationReportingFailureIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause					CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-Aerial-UE-FlightInformationOngoingReporting-failed			CRITICALITY ignore	TYPE Aerial-UE-FlightInformationOngoingReporting-failed					PRESENCE optional},
	...
}


Aerial-UE-FlightInformationOngoingReporting-failed::= ENUMERATED {
	true,
	...
}

-- **************************************************************
--
-- LOCATION REPORT
--
-- **************************************************************

LocationReport ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {LocationReportIEs} },
	...
}

LocationReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID						CRITICALITY reject	TYPE AMF-UE-NGAP-ID							PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID						CRITICALITY reject	TYPE RAN-UE-NGAP-ID							PRESENCE mandatory	}|
	{ ID id-UserLocationInformation				CRITICALITY ignore	TYPE UserLocationInformation				PRESENCE mandatory	}|
	{ ID id-UEPresenceInAreaOfInterestList		CRITICALITY ignore	TYPE UEPresenceInAreaOfInterestList		PRESENCE optional		}|
	{ ID id-LocationReportingRequestType		CRITICALITY ignore	TYPE LocationReportingRequestType		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE TNLA BINDING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UE TNLA BINDING RELEASE REQUEST
--
-- **************************************************************

UETNLABindingReleaseRequest ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {UETNLABindingReleaseRequestIEs} },
	...
}

UETNLABindingReleaseRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID		CRITICALITY reject	TYPE AMF-UE-NGAP-ID		PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID		CRITICALITY reject	TYPE RAN-UE-NGAP-ID		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE RADIO CAPABILITY MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UE RADIO CAPABILITY INFO INDICATION
--
-- **************************************************************

UERadioCapabilityInfoIndication ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {UERadioCapabilityInfoIndicationIEs} },
	...
}

UERadioCapabilityInfoIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-UERadioCapability				CRITICALITY ignore	TYPE UERadioCapability				PRESENCE mandatory	}|
	{ ID id-UERadioCapabilityForPaging		CRITICALITY ignore	TYPE UERadioCapabilityForPaging		PRESENCE optional		}|
	{ ID id-UERadioCapability-EUTRA-Format	CRITICALITY ignore	TYPE UERadioCapability				PRESENCE optional		}|
	{ ID id-XrDeviceWith2Rx					CRITICALITY ignore	TYPE XrDeviceWith2Rx				PRESENCE optional		},
	...
}

-- **************************************************************
--
-- UE Radio Capability Check Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- UE RADIO CAPABILITY CHECK REQUEST
--
-- **************************************************************

UERadioCapabilityCheckRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UERadioCapabilityCheckRequestIEs} },
	...
}

UERadioCapabilityCheckRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID			CRITICALITY reject	TYPE AMF-UE-NGAP-ID			PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID			CRITICALITY reject	TYPE RAN-UE-NGAP-ID			PRESENCE mandatory	}|
	{ ID id-UERadioCapability		CRITICALITY ignore	TYPE UERadioCapability		PRESENCE optional	}|
	{ ID id-UERadioCapabilityID		CRITICALITY reject	TYPE UERadioCapabilityID	PRESENCE optional	},
	...
}

-- **************************************************************
--
-- UE RADIO CAPABILITY CHECK RESPONSE
--
-- **************************************************************

UERadioCapabilityCheckResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UERadioCapabilityCheckResponseIEs} },
	...
}

UERadioCapabilityCheckResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY ignore	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY ignore	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-IMSVoiceSupportIndicator		CRITICALITY reject	TYPE IMSVoiceSupportIndicator		PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics			CRITICALITY ignore	TYPE CriticalityDiagnostics			PRESENCE optional		},
	...
}

-- **************************************************************
--
-- PRIVATE MESSAGE ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- PRIVATE MESSAGE
--
-- **************************************************************

PrivateMessage ::= SEQUENCE {
	privateIEs		PrivateIE-Container		{ { PrivateMessageIEs } },
	...
}

PrivateMessageIEs NGAP-PRIVATE-IES ::= {
	...
}


-- **************************************************************
--
-- DATA USAGE REPORTING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- SECONDARY RAT DATA USAGE REPORT
--
-- **************************************************************

SecondaryRATDataUsageReport ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {SecondaryRATDataUsageReportIEs} },
	...
}

SecondaryRATDataUsageReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID								CRITICALITY ignore	TYPE AMF-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID								CRITICALITY ignore	TYPE RAN-UE-NGAP-ID												PRESENCE mandatory	}|
	{ ID id-PDUSessionResourceSecondaryRATUsageList		CRITICALITY ignore	TYPE PDUSessionResourceSecondaryRATUsageList			PRESENCE mandatory	}|
	{ ID id-HandoverFlag								CRITICALITY ignore	TYPE HandoverFlag												PRESENCE optional		}|
	{ ID id-UserLocationInformation						CRITICALITY ignore	TYPE UserLocationInformation								PRESENCE optional 	},
	...
}

-- **************************************************************
--
-- RIM INFORMATION TRANSFER ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UPLINK RIM INFORMATION TRANSFER
--
-- **************************************************************

UplinkRIMInformationTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UplinkRIMInformationTransferIEs} },
	...
}

UplinkRIMInformationTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RIMInformationTransfer	CRITICALITY ignore	TYPE RIMInformationTransfer	PRESENCE optional	},
	...
}

-- **************************************************************
--
-- DOWNLINK RIM INFORMATION TRANSFER
--
-- **************************************************************

DownlinkRIMInformationTransfer ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DownlinkRIMInformationTransferIEs} },
	...
}

DownlinkRIMInformationTransferIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RIMInformationTransfer	CRITICALITY ignore	TYPE RIMInformationTransfer	PRESENCE optional	},
	...
}

-- **************************************************************
--
-- Connection Establishment Indication
--
-- **************************************************************

ConnectionEstablishmentIndication::= SEQUENCE {
	protocolIEs			ProtocolIE-Container { {ConnectionEstablishmentIndicationIEs} },
	...
}

ConnectionEstablishmentIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-UERadioCapability				CRITICALITY ignore	TYPE UERadioCapability				PRESENCE optional 	}|
	{ ID id-EndIndication					CRITICALITY ignore	TYPE EndIndication					PRESENCE optional		}|
	{ ID id-S-NSSAI							CRITICALITY ignore	TYPE S-NSSAI						PRESENCE optional		}|
	{ ID id-AllowedNSSAI					CRITICALITY ignore	TYPE AllowedNSSAI					PRESENCE optional		}|
	{ ID id-UE-DifferentiationInfo			CRITICALITY ignore	TYPE UE-DifferentiationInfo			PRESENCE optional		}|
	{ ID id-DL-CP-SecurityInformation		CRITICALITY ignore	TYPE DL-CP-SecurityInformation		PRESENCE optional		}|
	{ ID id-NB-IoT-UEPriority				CRITICALITY ignore	TYPE NB-IoT-UEPriority				PRESENCE optional		}|
	{ ID id-Enhanced-CoverageRestriction	CRITICALITY ignore	TYPE Enhanced-CoverageRestriction	PRESENCE optional		}|
	{ ID id-CEmodeBrestricted				CRITICALITY ignore	TYPE CEmodeBrestricted				PRESENCE optional		}|
	{ ID id-UERadioCapabilityID				CRITICALITY reject	TYPE UERadioCapabilityID			PRESENCE optional		}|
	{ ID id-MaskedIMEISV					CRITICALITY ignore	TYPE MaskedIMEISV					PRESENCE optional		}|
	{ ID id-OldAMF							CRITICALITY reject	TYPE AMFName						PRESENCE optional		}|
	{ ID id-Partially-Allowed-NSSAI			CRITICALITY ignore	TYPE Partially-Allowed-NSSAI		PRESENCE optional		}|
	{ ID id-ExtendedOldAMF					CRITICALITY ignore	TYPE Extended-AMFName				PRESENCE optional		},
	...
}


-- **************************************************************
--
-- UE RADIO CAPABILITY ID MAPPING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- UE RADIO CAPABILITY ID MAPPING REQUEST
--
-- **************************************************************

UERadioCapabilityIDMappingRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UERadioCapabilityIDMappingRequestIEs} },
	...
}

UERadioCapabilityIDMappingRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UERadioCapabilityID		CRITICALITY reject	TYPE UERadioCapabilityID	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- UE RADIO CAPABILITY ID MAPPING RESPONSE
--
-- **************************************************************

UERadioCapabilityIDMappingResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {UERadioCapabilityIDMappingResponseIEs} },
	...
}

UERadioCapabilityIDMappingResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-UERadioCapabilityID			CRITICALITY reject	TYPE UERadioCapabilityID		PRESENCE mandatory	}|
	{ ID id-UERadioCapability			CRITICALITY ignore	TYPE UERadioCapability			PRESENCE mandatory 	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- AMF CP Relocation Indication
--
-- **************************************************************

AMFCPRelocationIndication ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container { { AMFCPRelocationIndicationIEs} },
	...
}

AMFCPRelocationIndicationIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-S-NSSAI						CRITICALITY ignore	TYPE S-NSSAI					PRESENCE optional		}| --this IE is not used and ignored
	{ ID id-AllowedNSSAI				CRITICALITY ignore	TYPE AllowedNSSAI				PRESENCE optional		}| --this IE is not used and ignored
	{ ID id-Partially-Allowed-NSSAI		CRITICALITY ignore	TYPE Partially-Allowed-NSSAI	PRESENCE optional		}, --this IE is not used and ignored
	...
}

-- **************************************************************
--
-- MBS SESSION MANAGEMENT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Broadcast Session Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- BROADCAST SESSION SETUP REQUEST
--
-- **************************************************************

BroadcastSessionSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionSetupRequestIEs} },
	...
}
-- WS modification: define a dedicated type
MBSSessionSetupOrModRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBSSessionSetupOrModRequestTransfer)

BroadcastSessionSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID						CRITICALITY reject	TYPE MBS-SessionID										PRESENCE mandatory	}|
	{ ID id-S-NSSAI								CRITICALITY reject	TYPE S-NSSAI											PRESENCE mandatory	}|
	{ ID id-MBS-ServiceArea						CRITICALITY reject	TYPE MBS-ServiceArea									PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MBSSessionSetupRequestTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING MBSSessionSetupOrModRequestTransfer)		PRESENCE mandatory	}|
	{ ID id-MBSSessionSetupRequestTransfer		CRITICALITY reject	TYPE MBSSessionSetupOrModRequestTransfer-OCTET-STRING		PRESENCE mandatory	}|
	{ ID id-AssociatedSessionID					CRITICALITY ignore	TYPE AssociatedSessionID							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- BROADCAST SESSION SETUP RESPONSE
--
-- **************************************************************

BroadcastSessionSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionSetupResponseIEs} },
	...
}

-- WS modification: define a dedicated type
MBSSessionSetupOrModResponseTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBSSessionSetupOrModResponseTransfer)

BroadcastSessionSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID						CRITICALITY reject	TYPE MBS-SessionID										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MBSSessionSetupResponseTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING MBSSessionSetupOrModResponseTransfer)	PRESENCE optional		}|
	{ ID id-MBSSessionSetupResponseTransfer		CRITICALITY reject	TYPE MBSSessionSetupOrModResponseTransfer-OCTET-STRING	PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics				CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- BROADCAST SESSION SETUP FAILURE
--
-- **************************************************************

BroadcastSessionSetupFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionSetupFailureIEs} },
	...
}

-- WS modification: define a dedicated type
MBSSessionSetupOrModFailureTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBSSessionSetupOrModFailureTransfer)

BroadcastSessionSetupFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID						CRITICALITY reject	TYPE MBS-SessionID										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MBSSessionSetupFailureTransfer		CRITICALITY ignore	TYPE OCTET STRING (CONTAINING MBSSessionSetupOrModFailureTransfer	)	PRESENCE optional 	}|
	{ ID id-MBSSessionSetupFailureTransfer		CRITICALITY ignore	TYPE MBSSessionSetupOrModFailureTransfer-OCTET-STRING	PRESENCE optional 	}|
	{ ID id-Cause								CRITICALITY ignore	TYPE Cause												PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics				CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Broadcast Session Modification Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- BROADCAST SESSION MODIFICATION REQUEST
--
-- **************************************************************

BroadcastSessionModificationRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionModificationRequestIEs} },
	...
}

BroadcastSessionModificationRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID							CRITICALITY reject	TYPE MBS-SessionID									PRESENCE mandatory	}|
	{ ID id-MBS-ServiceArea							CRITICALITY reject	TYPE MBS-ServiceArea								PRESENCE optional		}|
-- WS modification: define a dedicated type
--	{ ID id-MBSSessionModificationRequestTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING MBSSessionSetupOrModRequestTransfer)		PRESENCE optional		},
	{ ID id-MBSSessionModificationRequestTransfer	CRITICALITY reject	TYPE MBSSessionSetupOrModRequestTransfer-OCTET-STRING		PRESENCE optional		},	...
}

-- **************************************************************
--
-- BROADCAST SESSION MODIFICATION RESPONSE
--
-- **************************************************************

BroadcastSessionModificationResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionModificationResponseIEs} },
	...
}

BroadcastSessionModificationResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID							CRITICALITY reject	TYPE MBS-SessionID									PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MBSSessionModificationResponseTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING MBSSessionSetupOrModResponseTransfer)	PRESENCE optional 	}|
	{ ID id-MBSSessionModificationResponseTransfer	CRITICALITY reject	TYPE MBSSessionSetupOrModResponseTransfer-OCTET-STRING	PRESENCE optional 	}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- BROADCAST SESSION MODIFICATION  FAILURE
--
-- **************************************************************

BroadcastSessionModificationFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionModificationFailureIEs} },
	...
}

BroadcastSessionModificationFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID							CRITICALITY reject	TYPE MBS-SessionID									PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MBSSessionModificationFailureTransfer	CRITICALITY ignore	TYPE OCTET STRING (CONTAINING MBSSessionSetupOrModFailureTransfer)	PRESENCE optional	}|
	{ ID id-MBSSessionModificationFailureTransfer	CRITICALITY ignore	TYPE MBSSessionSetupOrModFailureTransfer-OCTET-STRING	PRESENCE optional	}|
	{ ID id-Cause									CRITICALITY ignore	TYPE Cause											PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Broadcast Session Release Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- BROADCAST SESSION RELEASE REQUEST
--
-- **************************************************************

BroadcastSessionReleaseRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionReleaseRequestIEs} },
	...
}

BroadcastSessionReleaseRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID							CRITICALITY reject	TYPE MBS-SessionID									PRESENCE mandatory	}|
	{ ID id-Cause									CRITICALITY ignore	TYPE Cause											PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- Broadcast Session Release Required Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- BROADCAST SESSION RELEASE REQUIRED
--
-- **************************************************************

BroadcastSessionReleaseRequired ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionReleaseRequiredIEs} },
	...
}

BroadcastSessionReleaseRequiredIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID							CRITICALITY reject	TYPE MBS-SessionID									PRESENCE mandatory	}|
	{ ID id-Cause									CRITICALITY ignore	TYPE Cause											PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- BROADCAST SESSION RELEASE RESPONSE
--
-- **************************************************************

BroadcastSessionReleaseResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionReleaseResponseIEs} },
	...
}

-- WS modification: define a dedicated type
MBSSessionReleaseResponseTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBSSessionReleaseResponseTransfer)

BroadcastSessionReleaseResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID							CRITICALITY reject	TYPE MBS-SessionID								PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MBSSessionReleaseResponseTransfer		CRITICALITY ignore	TYPE OCTET STRING (CONTAINING MBSSessionReleaseResponseTransfer)		PRESENCE optional		}|
	{ ID id-MBSSessionReleaseResponseTransfer		CRITICALITY ignore	TYPE MBSSessionReleaseResponseTransfer-OCTET-STRING		PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics					PRESENCE optional		},
	...
}


-- **************************************************************
--
-- Broadcast Session Transport Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- BROADCAST SESSION TRANSPORT REQUEST
--
-- **************************************************************

BroadcastSessionTransportRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionTransportRequestIEs} },
	...
}

-- WS modification: define a dedicated type
BroadcastTransportRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING BroadcastTransportRequestTransfer)

BroadcastSessionTransportRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID						CRITICALITY reject	TYPE MBS-SessionID				PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-BroadcastTransportRequestTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING BroadcastTransportRequestTransfer)		PRESENCE mandatory	},
	{ ID id-BroadcastTransportRequestTransfer	CRITICALITY reject	TYPE BroadcastTransportRequestTransfer-OCTET-STRING		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- BROADCAST SESSION TRANSPORT RESPONSE
--
-- **************************************************************

BroadcastSessionTransportResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionTransportResponseIEs} },
	...
}

-- WS modification: define a dedicated type
BroadcastTransportResponseTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING BroadcastTransportResponseTransfer)

BroadcastSessionTransportResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID						CRITICALITY reject	TYPE MBS-SessionID				PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-BroadcastTransportResponseTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING BroadcastTransportResponseTransfer)	PRESENCE mandatory	}|
	{ ID id-BroadcastTransportResponseTransfer	CRITICALITY reject	TYPE BroadcastTransportResponseTransfer-OCTET-STRING	PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics				CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- BROADCAST SESSION TRANSPORT FAILURE
--
-- **************************************************************

BroadcastSessionTransportFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {BroadcastSessionTransportFailureIEs} },
	...
}

-- WS modification: define a dedicated type
BroadcastTransportFailureTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING BroadcastTransportFailureTransfer)

BroadcastSessionTransportFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID						CRITICALITY reject	TYPE MBS-SessionID				PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-BroadcastTransportFailureTransfer	CRITICALITY ignore	TYPE OCTET STRING (CONTAINING BroadcastTransportFailureTransfer)	PRESENCE 	mandatory	}|
	{ ID id-BroadcastTransportFailureTransfer	CRITICALITY ignore	TYPE BroadcastTransportFailureTransfer-OCTET-STRING	PRESENCE 	mandatory	}|
	{ ID id-Cause								CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics				CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}



-- **************************************************************
--
-- Distribution Setup Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- DISTRIBUTION SETUP REQUEST
--
-- **************************************************************

DistributionSetupRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DistributionSetupRequestIEs} },
	...
}

-- WS modification: define a dedicated type
MBS-DistributionSetupRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBS-DistributionSetupRequestTransfer)

DistributionSetupRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID							CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
-- WS modification: define a dedicated type
--	{ ID id-MBS-DistributionSetupRequestTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING MBS-DistributionSetupRequestTransfer)			PRESENCE mandatory	},
	{ ID id-MBS-DistributionSetupRequestTransfer		CRITICALITY reject	TYPE MBS-DistributionSetupRequestTransfer-OCTET-STRING			PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- DISTRIBUTION SETUP RESPONSE
--
-- **************************************************************

DistributionSetupResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DistributionSetupResponseIEs} },
	...
}

-- WS modification: define a dedicated type
MBS-DistributionSetupResponseTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBS-DistributionSetupResponseTransfer)

DistributionSetupResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID							CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
-- WS modification: define a dedicated type
--	{ ID id-MBS-DistributionSetupResponseTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING MBS-DistributionSetupResponseTransfer)			PRESENCE mandatory	}|
	{ ID id-MBS-DistributionSetupResponseTransfer		CRITICALITY reject	TYPE MBS-DistributionSetupResponseTransfer-OCTET-STRING			PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- DISTRIBUTION SETUP FAILURE
--
-- **************************************************************

DistributionSetupFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DistributionSetupFailureIEs} },
	...
}

-- WS modification: define a dedicated type
MBS-DistributionSetupUnsuccessfulTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBS-DistributionSetupUnsuccessfulTransfer)

DistributionSetupFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID							CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
-- WS modification: define a dedicated type
--	{ ID id-MBS-DistributionSetupUnsuccessfulTransfer	CRITICALITY ignore	TYPE OCTET STRING (CONTAINING MBS-DistributionSetupUnsuccessfulTransfer)	PRESENCE mandatory	}|
	{ ID id-MBS-DistributionSetupUnsuccessfulTransfer	CRITICALITY ignore	TYPE MBS-DistributionSetupUnsuccessfulTransfer-OCTET-STRING	PRESENCE mandatory	}|
	{ ID id-Cause										CRITICALITY ignore	TYPE Cause													PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Distribution Release Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- DISTRIBUTION RELEASE REQUEST
--
-- **************************************************************

DistributionReleaseRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DistributionReleaseRequestIEs} },
	...
}

-- WS modification: define a dedicated type
MBS-DistributionReleaseRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MBS-DistributionReleaseRequestTransfer)

DistributionReleaseRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID							CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
-- WS modification: define a dedicated type
--	{ ID id-MBS-DistributionReleaseRequestTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING MBS-DistributionReleaseRequestTransfer)		PRESENCE mandatory	}|
	{ ID id-MBS-DistributionReleaseRequestTransfer		CRITICALITY reject	TYPE MBS-DistributionReleaseRequestTransfer-OCTET-STRING		PRESENCE mandatory	}|
	{ ID id-Cause										CRITICALITY ignore	TYPE Cause													PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- DISTRIBUTION RELEASE RESPONSE
--
-- **************************************************************

DistributionReleaseResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {DistributionReleaseResponseIEs} },
	...
}

DistributionReleaseResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID							CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Multicast Session Activation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- MULTICAST SESSION ACTIVATION REQUEST
--
-- **************************************************************

MulticastSessionActivationRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionActivationRequestIEs} },
	...
}

-- WS modification: define a dedicated type
MulticastSessionActivationRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MulticastSessionActivationRequestTransfer)

MulticastSessionActivationRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MulticastSessionActivationRequestTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING MulticastSessionActivationRequestTransfer)	PRESENCE mandatory	},
	{ ID id-MulticastSessionActivationRequestTransfer	CRITICALITY reject	TYPE MulticastSessionActivationRequestTransfer-OCTET-STRING	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- MULTICAST SESSION ACTIVATION RESPONSE
--
-- **************************************************************

MulticastSessionActivationResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionActivationResponseIEs} },
	...
}

MulticastSessionActivationResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- MULTICAST SESSION ACTIVATION FAILURE
--
-- **************************************************************

MulticastSessionActivationFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionActivationFailureIEs} },
	...
}

MulticastSessionActivationFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID									CRITICALITY reject	TYPE MBS-SessionID										PRESENCE mandatory	}|
	{ ID id-Cause											CRITICALITY ignore	TYPE Cause													PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics							CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Multicast Session Deactivation Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- MULTICAST SESSION DEACTIVATION REQUEST
--
-- **************************************************************

MulticastSessionDeactivationRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionDeactivationRequestIEs} },
	...
}

-- WS modification: define a dedicated type
MulticastSessionDeactivationRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MulticastSessionDeactivationRequestTransfer)

MulticastSessionDeactivationRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-MulticastSessionDeactivationRequestTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING MulticastSessionDeactivationRequestTransfer)	PRESENCE mandatory	},
	{ ID id-MulticastSessionDeactivationRequestTransfer	CRITICALITY reject	TYPE MulticastSessionDeactivationRequestTransfer-OCTET-STRING	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- MULTICAST SESSION DEACTIVATION RESPONSE
--
-- **************************************************************

MulticastSessionDeactivationResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionDeactivationResponseIEs} },
	...
}

MulticastSessionDeactivationResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID									CRITICALITY reject	TYPE MBS-SessionID										PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics							CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Multicast Session Update Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- MULTICAST SESSION UPDATE REQUEST
--
-- **************************************************************

MulticastSessionUpdateRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionUpdateRequestIEs} },
	...
}

-- WS modification: define a dedicated type
MulticastSessionUpdateRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING MulticastSessionUpdateRequestTransfer)

MulticastSessionUpdateRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID							CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
-- WS modification: define a dedicated type
--	{ ID id-MulticastSessionUpdateRequestTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING MulticastSessionUpdateRequestTransfer)			PRESENCE mandatory	},
	{ ID id-MulticastSessionUpdateRequestTransfer		CRITICALITY reject	TYPE MulticastSessionUpdateRequestTransfer-OCTET-STRING			PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- MULTICAST SESSION UPDATE RESPONSE
--
-- **************************************************************

MulticastSessionUpdateResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionUpdateResponseIEs} },
	...
}

MulticastSessionUpdateResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID								CRITICALITY reject	TYPE MBS-SessionID											PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID							CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
	{ ID id-CriticalityDiagnostics						CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- MULTICAST SESSION UPDATE FAILURE
--
-- **************************************************************

MulticastSessionUpdateFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastSessionUpdateFailureIEs} },
	...
}

MulticastSessionUpdateFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID									CRITICALITY reject	TYPE MBS-SessionID										PRESENCE mandatory	}|
	{ ID id-MBS-AreaSessionID								CRITICALITY reject	TYPE MBS-AreaSessionID									PRESENCE optional		}|
	{ ID id-Cause											CRITICALITY ignore	TYPE Cause													PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics							CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}

-- **************************************************************
--
-- MULTICAST GROUP PAGING ELEMENTARY PROCEDURE
--
-- **************************************************************

-- **************************************************************
--
-- MULTICAST GROUP PAGING
--
-- **************************************************************

MulticastGroupPaging ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MulticastGroupPagingIEs} },
	...
}

MulticastGroupPagingIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-MBS-SessionID							CRITICALITY ignore	TYPE MBS-SessionID						PRESENCE mandatory	}|
	{ ID id-MBS-ServiceArea							CRITICALITY ignore	TYPE MBS-ServiceArea					PRESENCE optional		}|
	{ ID id-MulticastGroupPagingAreaList			CRITICALITY ignore	TYPE MulticastGroupPagingAreaList	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- TIMING SYNCHRONISATION STATUS REPORTING ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Timing Synchronisation Status Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- TIMING SYNCHRONISATION STATUS REQUEST
--
-- **************************************************************

TimingSynchronisationStatusRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {TimingSynchronisationStatusRequestIEs} },
	...
}

TimingSynchronisationStatusRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID				CRITICALITY reject	TYPE RoutingID			PRESENCE mandatory	}|
	{ ID id-RAN-TSSRequestType		CRITICALITY reject	TYPE RAN-TSSRequestType	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- TIMING SYNCHRONISATION STATUS RESPONSE
--
-- **************************************************************

TimingSynchronisationStatusResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {TimingSynchronisationStatusResponseIEs} },
	...
}

TimingSynchronisationStatusResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID					CRITICALITY ignore	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- TIMING SYNCHRONISATION STATUS FAILURE
--
-- **************************************************************

TimingSynchronisationStatusFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { TimingSynchronisationStatusFailureIEs} },
	...
}

TimingSynchronisationStatusFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID							CRITICALITY ignore	TYPE RoutingID					PRESENCE mandatory	}|
	{ ID id-Cause								CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics				CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************
--
-- Timing Synchronisation Status Reporting Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- TIMING SYNCHRONISATION STATUS REPORT
--
-- **************************************************************

TimingSynchronisationStatusReport ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container		{ {TimingSynchronisationStatusReportIEs} },
	...
}

TimingSynchronisationStatusReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-RoutingID							CRITICALITY ignore	TYPE RoutingID												PRESENCE mandatory	}|
	{ ID id-RANTimingSynchronisationStatusInfo	CRITICALITY ignore	TYPE RANTimingSynchronisationStatusInfo				PRESENCE mandatory	}|
	{ ID id-RAN-TSSScope							CRITICALITY ignore	TYPE RAN-TSSScope											PRESENCE mandatory	},
	...
}


-- **************************************************************
--
-- MT Communication Handling Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- MT COMMUNICATION HANDLING REQUEST
--
-- **************************************************************

MTCommunicationHandlingRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { MTCommunicationHandlingRequestIEs} },
	...
}

MTCommunicationHandlingRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY reject	TYPE AMF-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY reject	TYPE RAN-UE-NGAP-ID					PRESENCE mandatory	}|
	{ ID id-FiveGCAction					CRITICALITY reject	TYPE FiveGCAction					PRESENCE mandatory	}|
	{ ID id-PDUSessionListMTCommHReq		CRITICALITY reject	TYPE PDUSessionListMTCommHReq		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- MT COMMUNICATION HANDLING RESPONSE
--
-- **************************************************************

MTCommunicationHandlingResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {MTCommunicationHandlingResponseIEs} },
	...
}

MTCommunicationHandlingResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID							CRITICALITY reject	TYPE AMF-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID							CRITICALITY reject	TYPE RAN-UE-NGAP-ID										PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics					CRITICALITY ignore	TYPE CriticalityDiagnostics							PRESENCE optional		},
	...
}


-- **************************************************************
--
-- MT COMMUNICATION HANDLING FAILURE
--
-- **************************************************************

MTCommunicationHandlingFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ { MTCommunicationHandlingFailureIEs} },
	...
}

MTCommunicationHandlingFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID				CRITICALITY reject	TYPE AMF-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID				CRITICALITY reject	TYPE RAN-UE-NGAP-ID				PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause						PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics		PRESENCE optional		},
	...
}

-- **************************************************************

-- RAN Paging Request procedure
--
-- **************************************************************

-- **************************************************************
--
-- RAN PAGING REQUEST
--
-- **************************************************************

RANPagingRequest ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container       { {  RANPagingRequestIEs} },
	...
}

RANPagingRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AMF-UE-NGAP-ID					CRITICALITY ignore	TYPE AMF-UE-NGAP-ID						PRESENCE mandatory	}|
	{ ID id-RAN-UE-NGAP-ID					CRITICALITY ignore	TYPE RAN-UE-NGAP-ID						PRESENCE mandatory	}|
	{ ID id-PagingPolicyDifferentiation		CRITICALITY ignore	TYPE PagingPolicyDifferentiation		PRESENCE optional		}|
	{ ID id-DL-Signalling					CRITICALITY ignore	TYPE DL-Signalling						PRESENCE optional		},
	...
}

-- **************************************************************
--
-- A-IoT ELEMENTARY PROCEDURES
--
-- **************************************************************

-- **************************************************************
--
-- Inventory Request Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- INVENTORY REQUEST
--
-- **************************************************************

InventoryRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InventoryRequestIEs} },
	...
}

-- WS modification: define a dedicated type
InventoryRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING InventoryRequestTransfer)

InventoryRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier				CRITICALITY reject	TYPE AIOTFIdentifier												PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier	CRITICALITY reject	TYPE AIoT-CorrelationIdentifier										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-InventoryRequestTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING InventoryRequestTransfer)		PRESENCE mandatory	},
	{ ID id-InventoryRequestTransfer	CRITICALITY reject	TYPE InventoryRequestTransfer-OCTET-STRING		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- INVENTORY RESPONSE
--
-- **************************************************************

InventoryResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InventoryResponseIEs} },
	...
}

-- WS modification: define a dedicated type
InventoryResponseTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING InventoryResponseTransfer)

InventoryResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier				CRITICALITY reject	TYPE AIOTFIdentifier												PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier	CRITICALITY reject	TYPE AIoT-CorrelationIdentifier										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-InventoryResponseTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING InventoryResponseTransfer)	PRESENCE mandatory	}|
	{ ID id-InventoryResponseTransfer	CRITICALITY reject	TYPE InventoryResponseTransfer-OCTET-STRING	PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics											PRESENCE optional		},
	...
}

-- **************************************************************
--
-- INVENTORY FAILURE
--
-- **************************************************************

InventoryFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {InventoryFailureIEs} },
	...
}

-- WS modification: define a dedicated type
InventoryFailureTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING InventoryFailureTransfer)

InventoryFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier				CRITICALITY ignore	TYPE AIOTFIdentifier												PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier	CRITICALITY ignore	TYPE AIoT-CorrelationIdentifier										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-InventoryFailureTransfer	CRITICALITY ignore	TYPE OCTET STRING (CONTAINING InventoryFailureTransfer	)	PRESENCE mandatory	}|
	{ ID id-InventoryFailureTransfer	CRITICALITY ignore	TYPE InventoryFailureTransfer-OCTET-STRING	PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause															PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics											PRESENCE optional		},
	...
}

-- **************************************************************

-- Inventory Report procedure
--
-- **************************************************************

-- **************************************************************
--
-- INVENTORY REPORT
--
-- **************************************************************

InventoryReport ::= SEQUENCE {
	protocolIEs			ProtocolIE-Container       { {  InventoryReportIEs} },
	...
}

-- WS modification: define a dedicated type
InventoryReportTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING InventoryReportTransfer)

InventoryReportIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier				CRITICALITY reject	TYPE AIOTFIdentifier												PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier	CRITICALITY reject	TYPE AIoT-CorrelationIdentifier										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-InventoryReportTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING InventoryReportTransfer	)	PRESENCE mandatory	},
	{ ID id-InventoryReportTransfer		CRITICALITY reject	TYPE InventoryReportTransfer-OCTET-STRING	PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- Command Request Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- COMMAND REQUEST
--
-- **************************************************************

CommandRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {CommandRequestIEs} },
	...
}

-- WS modification: define a dedicated type
CommandRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING CommandRequestTransfer)

CommandRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier				CRITICALITY reject	TYPE AIOTFIdentifier												PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier	CRITICALITY reject	TYPE AIoT-CorrelationIdentifier										PRESENCE mandatory	}|
	{ ID id-RAN-AIOT-Device-NGAP-ID		CRITICALITY reject	TYPE RAN-AIOT-Device-NGAP-ID										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-CommandRequestTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING CommandRequestTransfer)		PRESENCE mandatory	},
	{ ID id-CommandRequestTransfer		CRITICALITY reject	TYPE CommandRequestTransfer-OCTET-STRING		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- COMMAND RESPONSE
--
-- **************************************************************

CommandResponse ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {CommandResponseIEs} },
	...
}

-- WS modification: define a dedicated type
CommandResponseTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING CommandResponseTransfer)

CommandResponseIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier				CRITICALITY reject	TYPE AIOTFIdentifier												PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier	CRITICALITY reject	TYPE AIoT-CorrelationIdentifier										PRESENCE mandatory	}|
	{ ID id-RAN-AIOT-Device-NGAP-ID		CRITICALITY reject	TYPE RAN-AIOT-Device-NGAP-ID										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-CommandResponseTransfer		CRITICALITY reject	TYPE OCTET STRING (CONTAINING CommandResponseTransfer)		PRESENCE mandatory	}|
	{ ID id-CommandResponseTransfer		CRITICALITY reject	TYPE CommandResponseTransfer-OCTET-STRING		PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics											PRESENCE optional		},
	...
}

-- **************************************************************
--
-- COMMAND FAILURE
--
-- **************************************************************

CommandFailure ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {CommandFailureIEs} },
	...
}

-- WS modification: define a dedicated type
CommandFailureTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING CommandFailureTransfer)

CommandFailureIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier				CRITICALITY ignore	TYPE AIOTFIdentifier												PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier	CRITICALITY ignore	TYPE AIoT-CorrelationIdentifier										PRESENCE mandatory	}|
	{ ID id-RAN-AIOT-Device-NGAP-ID		CRITICALITY ignore	TYPE RAN-AIOT-Device-NGAP-ID										PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-CommandFailureTransfer		CRITICALITY ignore	TYPE OCTET STRING (CONTAINING CommandFailureTransfer	)		PRESENCE mandatory	}|
	{ ID id-CommandFailureTransfer		CRITICALITY ignore	TYPE CommandFailureTransfer-OCTET-STRING		PRESENCE mandatory	}|
	{ ID id-Cause						CRITICALITY ignore	TYPE Cause															PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics		CRITICALITY ignore	TYPE CriticalityDiagnostics											PRESENCE optional		},
	...
}

-- **************************************************************
--
-- A-IoT Session Release Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- AIOT SESSION RELEASE COMMAND
--
-- **************************************************************

AIOTSessionReleaseCommand ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AIOTSessionReleaseCommandIEs} },
	...
}

-- WS modification: define a dedicated type
AIOTSessionReleaseCommandTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING AIOTSessionReleaseCommandTransfer)

AIOTSessionReleaseCommandIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier						CRITICALITY reject	TYPE AIOTFIdentifier									PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier			CRITICALITY reject	TYPE AIoT-CorrelationIdentifier						PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-AIOTSessionReleaseCommandTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING AIOTSessionReleaseCommandTransfer)		PRESENCE mandatory	},
	{ ID id-AIOTSessionReleaseCommandTransfer	CRITICALITY reject	TYPE AIOTSessionReleaseCommandTransfer-OCTET-STRING		PRESENCE mandatory	},
	...
}

-- **************************************************************
--
-- AIOT SESSION RELEASE COMPLETE
--
-- **************************************************************

AIOTSessionReleaseComplete ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AIOTSessionReleaseCompleteIEs} },
	...
}

-- WS modification: define a dedicated type
AIOTSessionReleaseCompleteTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING AIOTSessionReleaseCompleteTransfer)

AIOTSessionReleaseCompleteIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier						CRITICALITY ignore	TYPE AIOTFIdentifier									PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier			CRITICALITY ignore	TYPE AIoT-CorrelationIdentifier						PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-AIOTSessionReleaseCompleteTransfer	CRITICALITY ignore	TYPE OCTET STRING (CONTAINING AIOTSessionReleaseCompleteTransfer)	PRESENCE mandatory	}|
	{ ID id-AIOTSessionReleaseCompleteTransfer	CRITICALITY ignore	TYPE AIOTSessionReleaseCompleteTransfer-OCTET-STRING	PRESENCE mandatory	}|
	{ ID id-CriticalityDiagnostics				CRITICALITY ignore	TYPE CriticalityDiagnostics								PRESENCE optional		},
	...
}

-- **************************************************************
--
-- A-IoT Session Release Request Elementary Procedure
--
-- **************************************************************

-- **************************************************************
--
-- AIOT SESSION RELEASE REQUEST
--
-- **************************************************************

AIOTSessionReleaseRequest ::= SEQUENCE {
	protocolIEs		ProtocolIE-Container		{ {AIOTSessionReleaseRequestIEs} },
	...
}

-- WS modification: define a dedicated type
AIOTSessionReleaseRequestTransfer-OCTET-STRING ::= OCTET STRING (CONTAINING AIOTSessionReleaseRequestTransfer)

AIOTSessionReleaseRequestIEs NGAP-PROTOCOL-IES ::= {
	{ ID id-AIOTFIdentifier						CRITICALITY reject	TYPE AIOTFIdentifier									PRESENCE mandatory	}|
	{ ID id-AIoT-CorrelationIdentifier			CRITICALITY reject	TYPE AIoT-CorrelationIdentifier						PRESENCE mandatory	}|
-- WS modification: define a dedicated type
--	{ ID id-AIOTSessionReleaseRequestTransfer	CRITICALITY reject	TYPE OCTET STRING (CONTAINING AIOTSessionReleaseRequestTransfer)		PRESENCE mandatory	},
	{ ID id-AIOTSessionReleaseRequestTransfer	CRITICALITY reject	TYPE AIOTSessionReleaseRequestTransfer-OCTET-STRING		PRESENCE mandatory	},
	...
}

END
