/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Timea Moder
******************************************************************************/
//
//  File:               GiSGiInterface_3GPP_TS29061_b90_QoS_Detailed.ddf
//  Description:        DDF for Gi/SGi according to 3GPP TS 29.061 V11.9.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: GI
// APPLICATION-REVISION: V11_9_0

// AVP implementations according to: 
// 3GPP TS 29.061 V11.9.0 - Interworking between the Public Land Mobile Network (PLMN) supporting packet based services and Packet Data Networks (PDN)
//
//
// Dependant applications
// -

// 3GPP TS 29.061 V11.9.0 16a.4
type enumerated Command_Code 
{
  Authorize_Authenticate (265),
  Session_Termination    (275),
  Abort_Session          (274),
  Accounting             (271)
}



// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-IMSI (1) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_IMSI;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-Charging-Id (2) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_Charging_Id;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-PDP-Type (3) 3GPP (10415)
// 16.4.7
type enumerated 3GPP_PDP_Type
{
  IPv4   (0),
  PPP    (1),
  IPv6   (2),
  IPv4v6 (3)
}


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-CG-Address (4) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_CG_Address;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-GPRS-Negotiated-QoS-Profile (5) 3GPP (10415)
// 16.4.7
type GPRS_Negotiated_QoS_Profile 3GPP_GPRS_Negotiated_QoS_Profile;

// EXT_CC: GiSGiInterface_3GPP_TS29061_930_QoS_Detailed.tpl

modulepar boolean Negotiated_QoS_Profile_decode_as_detailed:=false;

type union GPRS_Negotiated_QoS_Profile{
  AVP_UTF8String                       raw_QoS_Profile,
  GPRS_Negotiated_QoS_Profile_detailed QoS_Profile_detailed
}

type record GPRS_Negotiated_QoS_Profile_detailed{
  charstring        qos_profile_header length(3),
  AVP_qos_profile   qos_profile_data
} with {
  variant (qos_profile_data) "CROSSTAG(
                                rel98, qos_profile_header=\"98-\";
                                rel99, qos_profile_header=\"99-\";
                                rel05, qos_profile_header=\"05-\";
                                rel07, qos_profile_header=\"07-\";
                                
                              )"
}

type union AVP_qos_profile
{
  qos_rel98_t  rel98,
  qos_rel99_t  rel99,
  qos_rel05_t  rel05,
  qos_rel07_t  rel07
}

type bitstring BITSTR1 length(1) with { variant "FIELDLENGTH(1)" };
type bitstring BITSTR2 length(2) with { variant "FIELDLENGTH(2)" };
type bitstring BITSTR3 length(3) with { variant "FIELDLENGTH(3)" };
type bitstring BITSTR4 length(4) with { variant "FIELDLENGTH(4)" };
type bitstring BITSTR5 length(5) with { variant "FIELDLENGTH(5)" };
type bitstring BITSTR6 length(6) with { variant "FIELDLENGTH(6)" };
type octetstring OCTSTR1 length(1) with { variant "FIELDLENGTH(1)" };

type record qos_rel98_t // 3GPP 24.008 v3.0.0
{
  BITSTR3                reliabilityClass,
  BITSTR3                delayClass,
  BITSTR2                spare1,  // '00'B
  BITSTR3                precedenceClass,
  BITSTR1                spare2,
  BITSTR4                peakThroughput,
  BITSTR5                meanThroughput,
  BITSTR3                spare3
} with {variant ""}

type record qos_rel99_t // 3GPP 24.008 v4.16.0
{
  BITSTR3                reliabilityClass,
  BITSTR3                delayClass,
  BITSTR2                spare1,  // '00'B
  BITSTR3                precedenceClass,
  BITSTR1                spare2,
  BITSTR4                peakThroughput,
  BITSTR5                meanThroughput,
  BITSTR3                spare3,
  BITSTR3                deliverErroneusSDU,
  BITSTR2                deliveryOrder,
  BITSTR3                trafficClass,
  OCTSTR1                maxSDUSize,
  OCTSTR1                maxBitrateUplink,
  OCTSTR1                maxBitrateDownlink,
  BITSTR4                sduErrorRatio,
  BITSTR4                residualBER,
  BITSTR2                trafficHandlingPriority,
  BITSTR6                transferDelay,
  OCTSTR1                guaranteedBitRateUplink,
  OCTSTR1                guaranteedBitRateDownlink
} with {variant ""}

type record qos_rel05_t // 3GPP 24.008 v6.12.0
{
  BITSTR3                reliabilityClass,
  BITSTR3                delayClass,
  BITSTR2                spare1,  // '00'B
  BITSTR3                precedenceClass,
  BITSTR1                spare2,
  BITSTR4                peakThroughput,
  BITSTR5                meanThroughput,
  BITSTR3                spare3,
  BITSTR3                deliverErroneusSDU,
  BITSTR2                deliveryOrder,
  BITSTR3                trafficClass,
  OCTSTR1                maxSDUSize,
  OCTSTR1                maxBitrateUplink,
  OCTSTR1                maxBitrateDownlink,
  BITSTR4                sduErrorRatio,
  BITSTR4                residualBER,
  BITSTR2                trafficHandlingPriority,
  BITSTR6                transferDelay,
  OCTSTR1                guaranteedBitRateUplink,
  OCTSTR1                guaranteedBitRateDownlink,
  BITSTR4                sourceStatisticsDescriptor,
  BITSTR1                signallingIndication,
  BITSTR3                spare4,
  OCTSTR1                maxBitRateDownlinkExtended,
  OCTSTR1                guaranteedBitRateDownlinkExtended
} with {variant ""}

type record qos_rel07_t
{
  BITSTR3                reliabilityClass,
  BITSTR3                delayClass,
  BITSTR2                spare1,  // '00'B
  BITSTR3                precedenceClass,
  BITSTR1                spare2,
  BITSTR4                peakThroughput,
  BITSTR5                meanThroughput,
  BITSTR3                spare3,
  BITSTR3                deliverErroneusSDU optional,
  BITSTR2                deliveryOrder optional,
  BITSTR3                trafficClass optional,
  OCTSTR1                maxSDUSize optional,
  OCTSTR1                maxBitrateUplink optional,
  OCTSTR1                maxBitrateDownlink optional,
  BITSTR4                sduErrorRatio optional,
  BITSTR4                residualBER optional,
  BITSTR2                trafficHandlingPriority optional,
  BITSTR6                transferDelay optional,
  OCTSTR1                guaranteedBitRateUplink optional,
  OCTSTR1                guaranteedBitRateDownlink optional,
  BITSTR4                sourceStatisticsDescriptor optional,
  BITSTR1                signallingIndication optional,
  BITSTR3                spare4 optional,
  OCTSTR1                maxBitRateDownlinkExtended optional,
  OCTSTR1                guaranteedBitRateDownlinkExtended optional,
  OCTSTR1                maxBitRateUplinkExtended optional,
  OCTSTR1                guaranteedBitRateUplinkExtended  optional
} with {variant ""}

external function f_decode_qos_rel98(in octetstring stream, out qos_rel98_t pdu) return integer
with { extension "prototype(backtrack) decode(RAW)" };
external function f_decode_qos_rel99(in octetstring stream, out qos_rel99_t pdu) return integer
with { extension "prototype(backtrack) decode(RAW)" };
external function f_decode_qos_rel05(in octetstring stream, out qos_rel05_t pdu) return integer
with { extension "prototype(backtrack) decode(RAW)" };
external function f_decode_qos_rel07(in octetstring stream, out qos_rel07_t pdu) return integer
with { extension "prototype(backtrack) decode(RAW)" };
external function f_enc_AVP_qos_profile(in AVP_qos_profile pdu) return octetstring
with { extension "prototype(convert) encode(RAW)" };

external function f_handle_QoS_Profile(inout GPRS_Negotiated_QoS_Profile pl_pdu)

// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-SGSN-Address (6) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_SGSN_Address;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-GGSN-Address (7) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_GGSN_Address;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-IMSI-MCC-MNC (8) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_IMSI_MCC_MNC;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-GGSN-MCC-MNC (9) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_GGSN_MCC_MNC;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-NSAPI (10) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_NSAPI;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-Session-Stop-Indicator (11) 3GPP (10415)
type AVP_UTF8String 3GPP_Session_Stop_Indicator;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-Selection-Mode (12) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_Selection_Mode;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-Charging-Characteristics (13) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_Charging_Characteristics;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-CG-IPv6-Address (14) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_CG_IPv6_Address;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-SGSN-IPv6-Address (15) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_SGSN_IPv6_Address;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-GGSN-IPv6-Address (16) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_GGSN_IPv6_Address;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-IPv6-DNS-Servers (17) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_IPv6_DNS_Servers;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-SGSN-MCC-MNC (18) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_SGSN_MCC_MNC;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-IMEISV (20) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_IMEISV;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-RAT-Type (21) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_RAT_Type;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-User-Location-Info (22) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_User_Location_Info;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-MS-TimeZone (23) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_MS_TimeZone;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-CAMEL-Charging-Info (24) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_CAMEL_Charging_Info;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-Packet-Filter (25) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_Packet_Filter;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-Negotiated-DSCP (26) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_Negotiated_DSCP;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-Allocate-IP-Type (27) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_Allocate_IP_Type;

// 3GPP TS 29.061 V11.9.0
// AVP: External-Identifier (28) 3GPP (10415)
// 16.4.7
type AVP_UTF8String External_Identifier;

// 3GPP TS 29.061 V11.9.0
// AVP: TWAN-Identifier (29) 3GPP (10415)
// 16.4.7
type AVP_OctetString TWAN_Identifier;


// 3GPP TS 29.061 V11.9.0
// AVP: 3GPP-User-Location-Info-Time (30) 3GPP (10415)
// 16.4.7
type AVP_Unsigned32 3GPP_User_Location_Info_Time;
