/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               GiSGiInterface_3GPP_TS29061_810.ddf
//  Description:        DDF for Gi/SGi according to 3GPP TS 29.061 V8.1.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: GI
// APPLICATION-REVISION: V8_1_0

// AVP implementations according to: 
// 3GPP TS 29.061 V8.1.0 - Interworking between the Public Land Mobile Network (PLMN) supporting packet based services and Packet Data Networks (PDN)
//
//
// Dependant applications
// -

// 3GPP TS 29.061 V8.1.0 16a.4
type enumerated Command_Code 
{
  Authorize_Authenticate (265),
  Session_Termination    (275),
  Abort_Session          (274),
  Accounting             (271)
}



// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-IMSI (1) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_IMSI;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-Charging-Id (2) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_Charging_Id;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-PDP-Type (3) 3GPP (10415)
// 16.4.7
type enumerated 3GPP_PDP_Type
{
  IPv4   (0),
  PPP    (1),
  IPv6   (2),
  IPv4v6 (3)
}


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-CG-Address (4) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_CG_Address;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-GPRS-Negotiated-QoS-Profile (5) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_GPRS_Negotiated_QoS_Profile;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-SGSN-Address (6) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_SGSN_Address;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-GGSN-Address (7) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_GGSN_Address;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-IMSI-MCC-MNC (8) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_IMSI_MCC_MNC;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-GGSN-MCC-MNC (9) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_GGSN_MCC_MNC;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-NSAPI (10) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_NSAPI;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-Session-Stop-Indicator (11) 3GPP (10415)
type AVP_UTF8String 3GPP_Session_Stop_Indicator;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-Selection-Mode (12) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_Selection_Mode;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-Charging-Characteristics (13) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_Charging_Characteristics;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-CG-IPv6-Address (14) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_CG_IPv6_Address;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-SGSN-IPv6-Address (15) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_SGSN_IPv6_Address;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-GGSN-IPv6-Address (16) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_GGSN_IPv6_Address;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-IPv6-DNS-Servers (17) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_IPv6_DNS_Servers;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-SGSN-MCC-MNC (18) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_SGSN_MCC_MNC;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-IMEISV (20) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_IMEISV;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-RAT-Type (21) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_RAT_Type;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-User-Location-Info (22) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_User_Location_Info;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-MS-TimeZone (23) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_MS_TimeZone;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-CAMEL-Charging-Info (24) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_CAMEL_Charging_Info;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-Packet-Filter (25) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_Packet_Filter;


// 3GPP TS 29.061 V8.1.0
// AVP: 3GPP-Negotiated-DSCP (26) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_Negotiated_DSCP;

