[MODULE_PARAMETERS]
# This section shall contain the values of all parameters that are defined in your TTCN-3 modules.

NAS_Pics.PICS_NAS_GNB_IUT := true
NAS_Pics.PICS_NAS_AMF_IUT := false

[LOGGING]
# In this section you can specify the name of the log file and the classes of events
# you want to log into the file or display on console (standard error).

LogFile := "../logs/Ats_NG_NAS/%e.%h-%r.%s"
FileMask := LOG_ALL | USER | DEBUG | MATCHING
ConsoleMask := LOG_ALL | USER | DEBUG | MATCHING
#FileMask := ERROR | WARNING | USER | MATCHING | EXECUTOR_RUNTIME | VERDICTOP | PORTEVENT | TESTCASE
#ConsoleMask := ERROR | WARNING | USER | MATCHING | EXECUTOR_RUNTIME | VERDICTOP | PORTEVENT | TESTCASE
LogSourceInfo := Stack
LogEntityName:= Yes
LogEventTypes:= Yes
#TimeStampFormat := DateTime

[TESTPORT_PARAMETERS]
# In this section you can specify parameters that are passed to Test Ports.
system.NGAP_gNB_1.params := "NAS/NGAP/SCTP_FILE/IP_OFFLINE/PCAP_FILE(file=../captures/5g_reg.pcapng)"
system.N2_gNBaMF_P.params := "NAS/NGAP/SCTP_FILE/IP_OFFLINE/PCAP_FILE(file=../captures/5g_reg.pcapng)"
#aMFNASComponent.N2_gNBaMF_P.params := "NAS/SCTP_FILE/IP_FILE/ETH/PCAP_FILE(file=../captures/free5gc.pcap)"

[DEFINE]
# In this section you can create macro definitions,
# that can be used in other configuration file sections except [INCLUDE] and [ORDERED_INCLUDE].

[INCLUDE]
# To use configuration settings given in other configuration files,
# the configuration files just need to be listed in this section, with their full or relative pathnames.

[ORDERED_INCLUDE]
# To use configuration settings given in other configuration files,
# the configuration files just need to be listed in this section, with their full or relative pathnames.

[EXTERNAL_COMMANDS]
# This section can define external commands (shell scripts) to be executed by the ETS
# whenever a control part or test case is started or terminated.

#BeginTestCase := ""
#EndTestCase := ""
#BeginControlPart := ""
#EndControlPart := ""

[EXECUTE]
# In this section you can specify what parts of your test suite you want to execute.
#AtsImsIot_TestControl.control

[GROUPS]
# In this section you can specify groups of hosts. These groups can be used inside the
# [COMPONENTS] section to restrict the creation of certain PTCs to a given set of hosts.

[COMPONENTS]
# This section consists of rules restricting the location of created PTCs.

[MAIN_CONTROLLER]
# The options herein control the behavior of MC.
KillTimer := 10.0
LocalAddress := 127.0.0.1
TCPPort := 12000
NumHCs := 1
