===== test_call_mo
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000010650 LU-type=NORMAL
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 901-70-23
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: rev=R99 net=UTRAN Auth+Ciph
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DVLR VLR subscr IMSI-901700000010650 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000010650 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000010650) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:UTRAN-Iu:LU: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DVLR VLR subscr IMSI-901700000010650 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = e229c19e791f2e41)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650) AUTH on UTRAN received RES: e229c19e791f2e41 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=27497388b6cb044648f396aa155b95ef
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  security_mode_ctrl_sent == 1
  lu_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends GSUP LU Req to HLR
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: Received Event VLR_ULA_E_CIPH_RES
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000010650 has MSISDN:42342
DMSC msub(IMSI-901700000010650:MSISDN-42342) VLR: update for IMSI=901700000010650 (MSISDN=42342)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU, with TMSI 0x03020100
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
msc_a_is_accepted() == false
- MS sends TMSI Realloc Complete
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + attached: now used by 2 (active-conn,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,attached)
  iu_release_sent == 1
- LU was successful, and the conn has already been closed
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + lu_utran_tmsi: now used by 2 (attached,lu_utran_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, IMSI) == 0
  LAC == 23
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - lu_utran_tmsi: now used by 1 (attached)


- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=UTRAN Auth+Ciph
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...autn=1843a645b98d00005b2d666af46c45d9
- ...expecting res=7db47cf7f81e4dc7
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = 7db47cf7f81e4dc7)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH on UTRAN received RES: 7db47cf7f81e4dc7 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=1159ec926a50e98c034a6b7d7c9f418d
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_cc)
  security_mode_ctrl_sent == 1
  cm_service_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts; above Ciphering is an implicit CM Service Accept
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: Received Event PR_ARQ_E_CIPH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
  cm_service_result_sent == 0


- a call is initiated
- CC SETUP causes CRCX towards CN and RAN
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x80000001 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) codecs: :0{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) new state NULL -> INITIATED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) codecs: :0{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x1 codecs=AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x1 codecs=VND.3GPP.IUFP/16000#96
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to VND.3GPP.IUFP/16000#96
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x80000001: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000001: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx MNCC_RTP_CREATE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) Assignment Complete: RAN: VND.3GPP.IUFP/16000#96, CN: AMR:octet-align=1#112
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x80000001: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000001: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) new state INITIATED -> MO_CALL_PROC
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 1.000023 s
- The other call leg got established (not shown here), MNCC tells us so
  MSC <-- MNCC: callref 0x80000001: MNCC_ALERT_REQ

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx MNCC_ALERT_REQ
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <-- MNCC: callref 0x80000001: MNCC_SETUP_RSP

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx MNCC_SETUP_RSP
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) new state CALL_DELIVERED -> CONNECT_IND
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 2.000046 s
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x80000001: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)


- RTP stream goes ahead, not shown here.
- Total time passed: 125.000091 s


- Call ends
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x80000001: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x80000001: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000001 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000001: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-1:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) freeing VLR subscr (max total use count was 4)
===== test_call_mo: SUCCESS

===== test_call_mt
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000010650 LU-type=NORMAL
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 901-70-23
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: rev=R99 net=UTRAN Auth+Ciph
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DVLR VLR subscr IMSI-901700000010650 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000010650 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000010650) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:UTRAN-Iu:LU: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DVLR VLR subscr IMSI-901700000010650 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = e229c19e791f2e41)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650) AUTH on UTRAN received RES: e229c19e791f2e41 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=27497388b6cb044648f396aa155b95ef
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  security_mode_ctrl_sent == 1
  lu_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends GSUP LU Req to HLR
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: Received Event VLR_ULA_E_CIPH_RES
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000010650 has MSISDN:42342
DMSC msub(IMSI-901700000010650:MSISDN-42342) VLR: update for IMSI=901700000010650 (MSISDN=42342)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU, with TMSI 0x03020100
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
msc_a_is_accepted() == false
- MS sends TMSI Realloc Complete
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + attached: now used by 2 (active-conn,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,attached)
  iu_release_sent == 1
- LU was successful, and the conn has already been closed
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + lu_utran_tmsi: now used by 2 (attached,lu_utran_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, IMSI) == 0
  LAC == 23
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - lu_utran_tmsi: now used by 1 (attached)


- after a while, MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=10.23.23.1:23{AMR:octet-align=1#112})
DPAG Paging: IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 on UTRAN-Iu
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, and VLR sends Auth Request
  MSC <--UTRAN-Iu-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=UTRAN Auth+Ciph
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...autn=1843a645b98d00005b2d666af46c45d9
- ...expecting res=7db47cf7f81e4dc7
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (paging-response)
  auth_request_sent == 1
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (paging-response,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = 7db47cf7f81e4dc7)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH on UTRAN received RES: 7db47cf7f81e4dc7 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=1159ec926a50e98c034a6b7d7c9f418d
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (paging-response)
  security_mode_ctrl_sent == 1
- MS sends SecurityModeControl acceptance, VLR accepts, sends CC Setup
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: Received Event PR_ARQ_E_CIPH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 2 (paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - Paging: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x2 codecs=AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x2 codecs=VND.3GPP.IUFP/16000#96
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to VND.3GPP.IUFP/16000#96
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MGW acknowledges the CRCX to RAN, triggering Assignment
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Assignment completes, triggering CRCX to CN
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: VND.3GPP.IUFP/16000#96, CN: AMR:octet-align=1#112
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE with full SDP
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- Total time passed: 1.000023 s
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- Total time passed: 2.000046 s
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 125.000091 s


- Call ends
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-2:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) freeing VLR subscr (max total use count was 5)
===== test_call_mt: SUCCESS

===== test_call_mt2
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000010650 LU-type=NORMAL
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 901-70-23
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: rev=R99 net=UTRAN Auth+Ciph
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DVLR VLR subscr IMSI-901700000010650 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000010650 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000010650) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:UTRAN-Iu:LU: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DVLR VLR subscr IMSI-901700000010650 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = e229c19e791f2e41)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650) AUTH on UTRAN received RES: e229c19e791f2e41 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=27497388b6cb044648f396aa155b95ef
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  security_mode_ctrl_sent == 1
  lu_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends GSUP LU Req to HLR
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: Received Event VLR_ULA_E_CIPH_RES
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000010650 has MSISDN:42342
DMSC msub(IMSI-901700000010650:MSISDN-42342) VLR: update for IMSI=901700000010650 (MSISDN=42342)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU, with TMSI 0x03020100
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
msc_a_is_accepted() == false
- MS sends TMSI Realloc Complete
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + attached: now used by 2 (active-conn,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,attached)
  iu_release_sent == 1
- LU was successful, and the conn has already been closed
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + lu_utran_tmsi: now used by 2 (attached,lu_utran_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, IMSI) == 0
  LAC == 23
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - lu_utran_tmsi: now used by 1 (attached)


- after a while, MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=10.23.23.1:23{AMR:octet-align=1#112})
DPAG Paging: IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 on UTRAN-Iu
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, and VLR sends Auth Request
  MSC <--UTRAN-Iu-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=UTRAN Auth+Ciph
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...autn=1843a645b98d00005b2d666af46c45d9
- ...expecting res=7db47cf7f81e4dc7
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (paging-response)
  auth_request_sent == 1
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (paging-response,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = 7db47cf7f81e4dc7)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH on UTRAN received RES: 7db47cf7f81e4dc7 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=1159ec926a50e98c034a6b7d7c9f418d
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (paging-response)
  security_mode_ctrl_sent == 1
- MS sends SecurityModeControl acceptance, VLR accepts, sends CC Setup
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: Received Event PR_ARQ_E_CIPH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_WAIT_CIPH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 2 (paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - Paging: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x3 codecs=AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x3 codecs=VND.3GPP.IUFP/16000#96
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to VND.3GPP.IUFP/16000#96
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112})
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX to RAN, triggering Assignment
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Assignment completes, triggering CRCX to CN
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: VND.3GPP.IUFP/16000#96, CN: AMR:octet-align=1#112
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- When the CN side RTP address is known, ack MNCC_RTP_CREATE with full SDP
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- Total time passed: 1.000023 s
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 remote=10.23.23.1:23{AMR:octet-align=1#112} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- Total time passed: 16.000046 s
- The call failed, the BSC sends a BSSMAP Clear Request
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_CN_CLOSE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 1 (cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 4 (attached,CC,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 5 (attached,CC,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 4 (attached,CC,active-conn,msc_a_fsm_releasing_onenter)
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) Freeing transaction
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_IND
  MSC --> MNCC: callref 0x423: MNCC_REL_IND

DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> RELEASE_REQ
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_RELEASE: 032d0802e1af
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP callref-0x423 tid-0) new state RELEASE_REQ -> NULL
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - CC: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: - cc: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP:trans-0:call-3:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 2
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
- Total time passed: 31.000069 s
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) freeing VLR subscr (max total use count was 5)
===== test_call_mt2: SUCCESS

===== test_call_mo_to_unknown
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000010650 LU-type=NORMAL
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 901-70-23
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: rev=R99 net=UTRAN Auth+Ciph
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DVLR VLR subscr IMSI-901700000010650 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000010650 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000010650) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:UTRAN-Iu:LU: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DVLR VLR subscr IMSI-901700000010650 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = e229c19e791f2e41)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650) AUTH on UTRAN received RES: e229c19e791f2e41 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=27497388b6cb044648f396aa155b95ef
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  security_mode_ctrl_sent == 1
  lu_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends GSUP LU Req to HLR
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: Received Event VLR_ULA_E_CIPH_RES
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000010650 has MSISDN:42342
DMSC msub(IMSI-901700000010650:MSISDN-42342) VLR: update for IMSI=901700000010650 (MSISDN=42342)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU, with TMSI 0x03020100
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
msc_a_is_accepted() == false
- MS sends TMSI Realloc Complete
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + attached: now used by 2 (active-conn,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,attached)
  iu_release_sent == 1
- LU was successful, and the conn has already been closed
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + lu_utran_tmsi: now used by 2 (attached,lu_utran_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, IMSI) == 0
  LAC == 23
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - lu_utran_tmsi: now used by 1 (attached)


- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=UTRAN Auth+Ciph
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...autn=1843a645b98d00005b2d666af46c45d9
- ...expecting res=7db47cf7f81e4dc7
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = 7db47cf7f81e4dc7)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH on UTRAN received RES: 7db47cf7f81e4dc7 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=1159ec926a50e98c034a6b7d7c9f418d
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_cc)
  security_mode_ctrl_sent == 1
  cm_service_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts; above Ciphering is an implicit CM Service Accept
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: Received Event PR_ARQ_E_CIPH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
  cm_service_result_sent == 0


- a call is initiated
- CC SETUP causes CRCX towards CN and RAN
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x80000002 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) codecs: :0{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) new state NULL -> INITIATED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) codecs: :0{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x4 codecs=AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x4 codecs=VND.3GPP.IUFP/16000#96
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to VND.3GPP.IUFP/16000#96
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x80000002: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000002: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) rx MNCC_RTP_CREATE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) Assignment Complete: RAN: VND.3GPP.IUFP/16000#96, CN: AMR:octet-align=1#112
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x80000002: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000002: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) new state INITIATED -> MO_CALL_PROC
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- But the other side's MSISDN could not be resolved, MNCC tells us to cancel
  MSC <-- MNCC: callref 0x80000002: MNCC_REL_REQ

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) rx MNCC_REL_REQ
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) new state MO_CALL_PROC -> RELEASE_REQ
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 10.000023 s
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) Timeout of T308
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) starting timer T308 with 10 seconds
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000002 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000002: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-4:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) freeing VLR subscr (max total use count was 4)
===== test_call_mo_to_unknown: SUCCESS

===== test_call_mo_to_unknown_timeout
- Total time passed: 0.000000 s
- Location Update request causes a GSUP Send Auth Info request to HLR
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000010650 LU-type=NORMAL
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 901-70-23
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: rev=R99 net=UTRAN Auth+Ciph
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DVLR VLR subscr IMSI-901700000010650 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000010650 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST: 08010809710000000156f02801020a0101
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_NEEDS_AUTH_WAIT_AI
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- from HLR, rx _SEND_AUTH_INFO_RESULT; VLR sends Auth Req to MS
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: 0a010809710000000156f00362201039fa2f4e3d523d8619a73b4f65c3e14d21049b36efdf2208059a4f668f6fbe39231027497388b6cb044648f396aa155b95ef2410f64735036e5871319c679f4742a75ea125108704f5ba55f30000d2ee44b22c8ea9192708e229c19e791f2e4103622010c187a53a5e6b9d573cac7c74451fd46d210485aa31302208d3d50a000bf04f6e23101159ec926a50e98c034a6b7d7c9f418d2410df3a03d9ca5335641efc8e36d76cd20b25101843a645b98d00005b2d666af46c45d927087db47cf7f81e4dc703622010efa9c29a9742148d5c9070348716e1bb210469d5f9fb22083df176f0c29f1a3d2310eb50e770ddcc3060101d2f43b6c2b884241076542abce5ff9345b0e8947f4c6e019c2510f9375e6d41e1000096e7fe4ff1c27e392708706f996719ba609c03622010f023d5a3b24726e0631b64b3840f82532104d570c03f2208ec011be8919883d62310c4e58af4ba43f3bcd904e16984f086d724100593f65e752e5cb7f473862bda05aa0a2510541ff1f077270000c5ea00d658bc7e9a27083fd26072eaa2a04d036220102f8f90c780d6a9c0c53da7ac57b6707e2104b072446f220823f39f9f425ad6e6231065af0527fda95b0dc5ae4aa515cdf32f2410537c3b35a3b13b08d08eeb28098f45cc25104bf4e564f75300009bc796706bc6574427080edb0eadbea94ac20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: Received Event VLR_AUTH_E_HLR_SAI_ACK
DVLR SUBSCR(IMSI-901700000010650) Received 5 auth tuples
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_NEEDS_AUTH_WAIT_AI}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=0 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:UTRAN-Iu:LU: tuple use_count=1 key_seq=0 auth_types=0x3 and...
- ...rand=39fa2f4e3d523d8619a73b4f65c3e14d
- ...autn=8704f5ba55f30000d2ee44b22c8ea919
- ...expecting res=e229c19e791f2e41
DVLR VLR subscr IMSI-901700000010650 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT: vlr_gsupc_read_cb() returns 0
  auth_request_sent == 1
  lu_result_sent == 0
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = e229c19e791f2e41)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650) AUTH on UTRAN received RES: e229c19e791f2e41 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Received Event VLR_ULA_E_AUTH_SUCCESS
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=27497388b6cb044648f396aa155b95ef
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_AUTH}: state_chg to VLR_ULA_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:UTRAN-Iu:LU){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  security_mode_ctrl_sent == 1
  lu_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts and sends GSUP LU Req to HLR
DIUCS msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: Received Event VLR_ULA_E_CIPH_RES
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000010650:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU){VLR_ULA_S_WAIT_CIPH}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:UTRAN-Iu:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
  gsup_tx_confirmed == 1
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804032443f20a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000010650 has MSISDN:42342
DMSC msub(IMSI-901700000010650:MSISDN-42342) VLR: update for IMSI=901700000010650 (MSISDN=42342)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: lu_compl_vlr_new_tmsi()
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_WAIT_TMSI_CNF
- sending LU Accept for IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU, with TMSI 0x03020100
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:UTRAN-Iu:LU){UPD_HLR_VLR_S_DONE}: Deallocated
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 1
- a LU Accept with a new TMSI was sent, waiting for TMSI Realloc Compl
  llist_count(&msub_list) == 1
msc_a_is_accepted() == false
- MS sends TMSI Realloc Complete
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_TMSI_REALL_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (lu,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_TMSI_REALL_COMPL
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: TMSI Reallocation Completed
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSInew-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_NEW_TMSI_ACK
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: Received Event LU_COMPL_VLR_E_NEW_TMSI_ACK
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) VLR: update for IMSI=901700000010650 (MSISDN=42342)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + attached: now used by 2 (active-conn,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_WAIT_TMSI_CNF}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-42342:UTRAN-Iu:LU){LU_COMPL_VLR_S_DONE}: Deallocated
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 1 (rx_from_ms)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){VLR_ULA_S_DONE}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (active-conn,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (active-conn,attached)
  iu_release_sent == 1
- LU was successful, and the conn has already been closed
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + lu_utran_tmsi: now used by 2 (attached,lu_utran_tmsi)
  vsub != NULL == 1
  strcmp(vsub->imsi, IMSI) == 0
  LAC == 23
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - lu_utran_tmsi: now used by 1 (attached)


- after a while, a new conn sends a CM Service Request. VLR responds with Auth Req, 2nd auth vector
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DIUCS msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:UTRAN-Iu:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=UTRAN Auth+Ciph
DVLR Process_Access_Request_VLR(IMSI-901700000010650:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_WAIT_AUTH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Allocated
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: is child of Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: Received Event VLR_AUTH_E_START
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_NEEDS_AUTH}: state_chg to VLR_SUB_AS_WAIT_RESP
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: got auth tuple: use_count=1 key_seq=1 -- will use UMTS AKA (is_r99=yes, at->vec.auth_types=0x3)
- sending UMTS Auth Request for IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ: tuple use_count=1 key_seq=1 auth_types=0x3 and...
- ...rand=c187a53a5e6b9d573cac7c74451fd46d
- ...autn=1843a645b98d00005b2d666af46c45d9
- ...expecting res=7db47cf7f81e4dc7
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 0
  auth_request_sent == 1
- needs auth, not yet accepted
msc_a_is_accepted() == false
- MS sends Authen Response, VLR accepts and sends SecurityModeControl
  MSC <--UTRAN-Iu-- MS: GSM48_MT_MM_AUTH_RESP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Dispatching 04.08 message: MM GSM48_MT_MM_AUTH_RESP
DMM msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: MM UMTS AUTHENTICATION RESPONSE (res = 7db47cf7f81e4dc7)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Received Event VLR_AUTH_E_MS_AUTH_RESP
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH on UTRAN received RES: 7db47cf7f81e4dc7 (8 bytes)
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) AUTH established UMTS security context
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: Authentication terminating with result PASSED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_WAIT_RESP}: state_chg to VLR_SUB_AS_AUTHENTICATED
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Removing from parent Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Received Event PR_ARQ_E_AUTH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: Set Ciphering Mode
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: CIPHER_MODE_COMMAND on UTRAN-Iu
- sending SecurityModeControl: ik=1159ec926a50e98c034a6b7d7c9f418d
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_AUTH}: state_chg to PR_ARQ_S_WAIT_CIPH
DVLR VLR_Authenticate(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){VLR_SUB_AS_AUTHENTICATED}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (cm_service_cc)
  security_mode_ctrl_sent == 1
  cm_service_result_sent == 0
- MS sends SecurityModeControl acceptance, VLR accepts; above Ciphering is an implicit CM Service Accept
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN decode: CIPHER_MODE_COMPLETE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: Received Event PR_ARQ_E_CIPH_RES
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_WAIT_CIPH}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
  cm_service_result_sent == 0


- a call is initiated
- CC SETUP causes CRCX towards CN and RAN
  MSC <--UTRAN-Iu-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 callref-0x80000003 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) codecs: :0{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) new state NULL -> INITIATED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) codecs: :0{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x5 codecs=AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x5 codecs=VND.3GPP.IUFP/16000#96
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to VND.3GPP.IUFP/16000#96
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x80000003: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000003: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) rx MNCC_RTP_CREATE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) Assignment Complete: RAN: VND.3GPP.IUFP/16000#96, CN: AMR:octet-align=1#112
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={AMR:octet-align=1#112,AMR-WB/16000:octet-align=1#113})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112})
  MSC --> MNCC: callref 0x80000003: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=ptime:20

- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000003: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) new state INITIATED -> MO_CALL_PROC
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- But the other side's MSISDN could not be resolved, MNCC tells us to cancel
  MSC <-- MNCC: callref 0x80000003: MNCC_REL_REQ

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) rx MNCC_REL_REQ
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) new state MO_CALL_PROC -> RELEASE_REQ
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Despite our repeated CC Release Requests, the MS does not respond anymore
- Total time passed: 10.000023 s
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) Timeout of T308
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) starting timer T308 with 10 seconds
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on UTRAN-Iu
- DTAP --UTRAN-Iu--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- The CC Release times out and we still properly clear the conn
- Total time passed: 20.000046 s
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) Timeout of T308
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) Freeing transaction
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000003: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ callref-0x80000003 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ:trans-8:call-5:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on UTRAN-Iu
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DIUCS msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100:UTRAN-Iu:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0
DVLR SUBSCR(IMSI-901700000010650:MSISDN-42342:TMSI-0x03020100) freeing VLR subscr (max total use count was 4)
===== test_call_mo_to_unknown_timeout: SUCCESS

===== test_codecs
- Total time passed: 0.000000 s
- Location Update request causes a GSUP LU request to HLR
  MSC <--GERAN-A-- MS: GSM48_MT_MM_LOC_UPD_REQUEST
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_LOC_UPD_REQUEST
DMM msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: LOCATION UPDATING REQUEST: MI=IMSI-901700000010650 LU-type=NORMAL
DMM msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: USIM: old LAI: 901-70-23
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + mm_rx_loc_upd_req: now used by 2 (rx_from_ms,mm_rx_loc_upd_req)
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: + lu: now used by 3 (rx_from_ms,mm_rx_loc_upd_req,lu)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: Allocated
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: is child of msc_a(IMSI-901700000010650:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: rev=R99 net=GERAN (no Auth)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: Received Event VLR_ULA_E_UPDATE_LA
DVLR VLR subscr unknown + _lu_fsm_associate_vsub: now used by 1 (_lu_fsm_associate_vsub)
DVLR set IMSI on subscriber; IMSI=901700000010650 id=901700000010650
DVLR New subscr, IMSI: 901700000010650
DVLR VLR subscr IMSI-901700000010650 + active-conn: now used by 2 (_lu_fsm_associate_vsub,active-conn)
DMSC msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR VLR subscr IMSI-901700000010650 - _lu_fsm_associate_vsub: now used by 1 (active-conn)
DVLR set Last E-UTRAN PLMN ID on subscriber: (none)
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1_pre()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node1()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_post_auth()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_post_ciph()
DMSC msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: vlr_loc_upd_node_4()
DVLR vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU){VLR_ULA_S_IDLE}: state_chg to VLR_ULA_S_WAIT_HLR_UPD
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Allocated
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: Received Event UPD_HLR_VLR_E_START
GSUP --> HLR: OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST: 04010809710000000156f02801020a0101
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_INIT}: state_chg to UPD_HLR_VLR_S_WAIT_FOR_DATA
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - mm_rx_loc_upd_req: now used by 2 (rx_from_ms,lu)
DREF msc_a(IMSI-901700000010650:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: - rx_from_ms: now used by 1 (lu)
  lu_result_sent == 0
- HLR sends _INSERT_DATA_REQUEST, VLR responds with _INSERT_DATA_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: 10010809710000000156f00804036470f10a0101
DVLR VLR subscr IMSI-901700000010650 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR IMSI:901700000010650 has MSISDN:46071
DMSC msub(IMSI-901700000010650:MSISDN-46071) VLR: update for IMSI=901700000010650 (MSISDN=46071)
GSUP --> HLR: OSMO_GSUP_MSGT_INSERT_DATA_RESULT: 12010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_gsup_rx: now used by 1 (active-conn)
<-- GSUP rx OSMO_GSUP_MSGT_INSERT_DATA_REQUEST: vlr_gsupc_read_cb() returns 0
  lu_result_sent == 0
- HLR also sends GSUP _UPDATE_LOCATION_RESULT
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: 06010809710000000156f00a0101
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_gsup_rx: now used by 2 (active-conn,vlr_gsup_rx)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_HLR_LU_RES
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: Received Event UPD_HLR_VLR_E_UPD_LOC_ACK
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_WAIT_FOR_DATA}: state_chg to UPD_HLR_VLR_S_DONE
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: Received Event VLR_ULA_E_UPD_HLR_COMPL
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_HLR_UPD}: state_chg to VLR_ULA_S_WAIT_LU_COMPL
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Allocated
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: is child of vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: Received Event LU_COMPL_VLR_E_START
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_INIT}: state_chg to LU_COMPL_VLR_S_WAIT_SUB_PRES
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: Received Event LU_COMPL_VLR_E_SUB_PRES_COMPL
- sending LU Accept for IMSI-901700000010650:MSISDN-46071:GERAN-A:LU
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + attached: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_WAIT_SUB_PRES}: state_chg to LU_COMPL_VLR_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: Received Event VLR_ULA_E_LU_COMPL_SUCCESS
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU))
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Removing from parent vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU)
DVLR lu_compl_vlr_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){LU_COMPL_VLR_S_DONE}: Deferring: will deallocate with upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_WAIT_LU_COMPL}: state_chg to VLR_ULA_S_DONE
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU))
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: fsm_lu_cleanup called with cause OSMO_FSM_TERM_REGULAR
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: - lu: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 5 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 4 (active-conn,vlr_gsup_rx,attached,msc_a_fsm_releasing_onenter)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 3 (active-conn,vlr_gsup_rx,attached)
DVLR vlr_lu_fsm(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){VLR_ULA_S_DONE}: Deferring: will deallocate with upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU)
DVLR upd_hlr_vlr_fsm(IMSI-901700000010650:GERAN-A:LU){UPD_HLR_VLR_S_DONE}: Deallocated, including all deferred deallocations
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_gsup_rx: now used by 2 (active-conn,attached)
<-- GSUP rx OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT: vlr_gsupc_read_cb() returns 0
- LU was successful, and the conn has already been closed
  lu_result_sent == 1
  bssap_clear_sent == 1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:LU){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== MO call: AMR picked by both MO and MT
- CM Service Request with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 1
msc_a_is_accepted() == true
- MS sends CC SETUP with Bearer Capability =  AMR AMR AMR GSM-EFR GSM GSM-HR-08
  MSC <--GERAN-A-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x80000004 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) new state NULL -> INITIATED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x6 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x6 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000004: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_ind == AMR GSM-EFR GSM GSM-HR-08
- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000004: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000004: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_rtp_create == AMR GSM-EFR GSM GSM-HR-08
- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000004: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) new state INITIATED -> MO_CALL_PROC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 1.000023 s
- The other call leg got established (not shown here), MNCC tells us so, with codecs { AMR GSM-EFR GSM GSM-HR-08 }
  MSC <-- MNCC: callref 0x80000004: MNCC_ALERT_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx MNCC_ALERT_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI){UNINITIALIZED}: no change: codecs already set to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:56
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <-- MNCC: callref 0x80000004: MNCC_SETUP_RSP
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx MNCC_SETUP_RSP (RTP=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) new state CALL_DELIVERED -> CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: no change: codecs already set to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: remote addr already 1.2.3.4:56, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 2.000046 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x80000004: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_compl_ind ==


- RTP stream goes ahead, not shown here.
- Total time passed: 125.000091 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x80000004: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x80000004: MNCC_REL_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000004 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000004: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-6:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MO call: AMR picked by both MO and MT


- ======================== MT call: AMR picked by both MO and MT


- MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
- VLR accepts, MSC sends CC Setup with Bearer Capability = TS 24.008 § D.1.2
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 3 (rx_from_ms,paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - Paging: now used by 4 (attached,CC,proc_arq_vlr_fn_init,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 2 (rx_from_ms,cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x7 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x7 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_call_conf_ind ==
- MGW acknowledges the CRCX to RAN, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mt_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment completes, triggering CRCX to CN
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_rtp_create == AMR GSM-EFR GSM GSM-HR-08
- Total time passed: 126.000114 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_alert_ind == AMR GSM-EFR GSM GSM-HR-08
- Total time passed: 127.000137 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_setup_cnf == AMR GSM-EFR GSM GSM-HR-08
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 250.000182 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-7:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MT call: AMR picked by both MO and MT


- ======================== MO call: FR1 picked by MO from Codec List (BSS Supported), MT hence also picks FR1
- CM Service Request with Codec List (BSS Supported) = FR1
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 1
msc_a_is_accepted() == true
- MS sends CC SETUP with Bearer Capability =  AMR AMR AMR GSM-EFR GSM GSM-HR-08
  MSC <--GERAN-A-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x80000005 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) codecs: :0{GSM#3} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) new state NULL -> INITIATED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) codecs: :0{GSM#3} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x8 codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x8 codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x80000005: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_ind == GSM
- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000005: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment with FR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_assignment_perm_speech == FR1
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_RAN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x80000005: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_rtp_create == GSM
- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000005: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) new state INITIATED -> MO_CALL_PROC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 251.000205 s
- The other call leg got established (not shown here), MNCC tells us so, with codecs { GSM }
  MSC <-- MNCC: callref 0x80000005: MNCC_ALERT_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx MNCC_ALERT_REQ (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:56
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <-- MNCC: callref 0x80000005: MNCC_SETUP_RSP
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx MNCC_SETUP_RSP (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) new state CALL_DELIVERED -> CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: remote addr already 1.2.3.4:56, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 252.000228 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x80000005: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_compl_ind ==


- RTP stream goes ahead, not shown here.
- Total time passed: 375.000273 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x80000005: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x80000005: MNCC_REL_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000005 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000005: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-8:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MO call: FR1 picked by MO from Codec List (BSS Supported), MT hence also picks FR1


- ======================== MT call: FR1 picked by MO from Codec List (BSS Supported), MT hence also picks FR1


- MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=1.2.3.4:56{GSM#3} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=1.2.3.4:56{GSM#3})
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
- VLR accepts, MSC sends CC Setup with Bearer Capability = TS 24.008 § D.1.2
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 3 (rx_from_ms,paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - Paging: now used by 4 (attached,CC,proc_arq_vlr_fn_init,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 2 (rx_from_ms,cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x9 codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x9 codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_call_conf_ind ==
- MGW acknowledges the CRCX to RAN, triggering Assignment with FR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mt_tx_assignment_perm_speech == FR1
- Assignment completes, triggering CRCX to CN
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_RAN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_rtp_create == GSM
- Total time passed: 376.000296 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_alert_ind == GSM
- Total time passed: 377.000319 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_setup_cnf == GSM
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 500.000364 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-9:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MT call: FR1 picked by MO from Codec List (BSS Supported), MT hence also picks FR1


- ======================== MO call: FR1 picked by MO from Bearer Cap, MT hence also picks FR1
- CM Service Request with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 1
msc_a_is_accepted() == true
- MS sends CC SETUP with Bearer Capability =  GSM
  MSC <--GERAN-A-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x80000006 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) codecs: :0{GSM#3} (from: MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) new state NULL -> INITIATED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) codecs: :0{GSM#3} (from: MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0xa codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0xa codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x80000006: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_ind == GSM
- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000006: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment with FR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_assignment_perm_speech == FR1
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_RAN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x80000006: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_rtp_create == GSM
- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000006: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) new state INITIATED -> MO_CALL_PROC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 501.000387 s
- The other call leg got established (not shown here), MNCC tells us so, with codecs { GSM }
  MSC <-- MNCC: callref 0x80000006: MNCC_ALERT_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx MNCC_ALERT_REQ (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:56
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <-- MNCC: callref 0x80000006: MNCC_SETUP_RSP
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx MNCC_SETUP_RSP (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) new state CALL_DELIVERED -> CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: remote addr already 1.2.3.4:56, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 502.000410 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x80000006: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_compl_ind ==


- RTP stream goes ahead, not shown here.
- Total time passed: 625.000455 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x80000006: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x80000006: MNCC_REL_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000006 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000006: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-10:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MO call: FR1 picked by MO from Bearer Cap, MT hence also picks FR1


- ======================== MT call: FR1 picked by MO from Bearer Cap, MT hence also picks FR1


- MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=1.2.3.4:56{GSM#3} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=1.2.3.4:56{GSM#3})
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
- VLR accepts, MSC sends CC Setup with Bearer Capability = TS 24.008 § D.1.2
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 3 (rx_from_ms,paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - Paging: now used by 4 (attached,CC,proc_arq_vlr_fn_init,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 2 (rx_from_ms,cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0xb codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0xb codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_call_conf_ind ==
- MGW acknowledges the CRCX to RAN, triggering Assignment with FR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mt_tx_assignment_perm_speech == FR1
- Assignment completes, triggering CRCX to CN
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_RAN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_rtp_create == GSM
- Total time passed: 626.000478 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_alert_ind == GSM
- Total time passed: 627.000501 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_setup_cnf == GSM
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 750.000546 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-11:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MT call: FR1 picked by MO from Bearer Cap, MT hence also picks FR1


- ======================== MO call: FR1 picked by MT's Codec List (BSS Supported), hence MO re-assigns to FR1
- CM Service Request with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 1
msc_a_is_accepted() == true
- MS sends CC SETUP with Bearer Capability =  AMR AMR AMR GSM-EFR GSM GSM-HR-08
  MSC <--GERAN-A-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x80000007 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) new state NULL -> INITIATED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0xc codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0xc codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000007: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_ind == AMR GSM-EFR GSM GSM-HR-08
- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000007: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000007: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_rtp_create == AMR GSM-EFR GSM GSM-HR-08
- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000007: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) new state INITIATED -> MO_CALL_PROC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 751.000569 s
- The other call leg got established (not shown here), MNCC tells us so, with codecs { GSM }
- Expecting re-assignment
  MSC <-- MNCC: callref 0x80000007: MNCC_ALERT_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx MNCC_ALERT_REQ (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:56
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) Remote call leg mismatches assigned codec: 10.23.23.1:23{GSM#3} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Validating re-assignment
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_reassignment_perm_speech == FR1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: setting codecs to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: remote addr already 1.2.3.4:1234, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) Re-Assignment complete
  MSC <-- MNCC: callref 0x80000007: MNCC_SETUP_RSP
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx MNCC_SETUP_RSP (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) new state CALL_DELIVERED -> CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: remote addr already 1.2.3.4:56, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 752.000592 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x80000007: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_compl_ind ==


- RTP stream goes ahead, not shown here.
- Total time passed: 875.000637 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x80000007: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x80000007: MNCC_REL_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000007 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000007: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-12:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MO call: FR1 picked by MT's Codec List (BSS Supported), hence MO re-assigns to FR1


- ======================== MT call: FR1 picked by MT's Codec List (BSS Supported), hence MO re-assigns to FR1


- MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, with Codec List (BSS Supported) = FR1
- VLR accepts, MSC sends CC Setup with Bearer Capability = TS 24.008 § D.1.2
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 3 (rx_from_ms,paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - Paging: now used by 4 (attached,CC,proc_arq_vlr_fn_init,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 2 (rx_from_ms,cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0xd codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0xd codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_call_conf_ind ==
- MGW acknowledges the CRCX to RAN, triggering Assignment with FR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mt_tx_assignment_perm_speech == FR1
- Assignment completes, triggering CRCX to CN
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_RAN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_rtp_create == GSM
- Total time passed: 876.000660 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_alert_ind == GSM
- Total time passed: 877.000683 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_setup_cnf == GSM
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 1000.000728 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-13:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MT call: FR1 picked by MT's Codec List (BSS Supported), hence MO re-assigns to FR1


- ======================== MO call: FR1 picked by MT's MS Bearer Capability, hence MO re-assigns to FR1
- CM Service Request with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 1
msc_a_is_accepted() == true
- MS sends CC SETUP with Bearer Capability =  AMR AMR AMR GSM-EFR GSM GSM-HR-08
  MSC <--GERAN-A-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x80000008 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) new state NULL -> INITIATED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0xe codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0xe codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000008: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_ind == AMR GSM-EFR GSM GSM-HR-08
- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000008: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000008: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_rtp_create == AMR GSM-EFR GSM GSM-HR-08
- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000008: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) new state INITIATED -> MO_CALL_PROC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 1001.000751 s
- The other call leg got established (not shown here), MNCC tells us so, with codecs { GSM }
- Expecting re-assignment
  MSC <-- MNCC: callref 0x80000008: MNCC_ALERT_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx MNCC_ALERT_REQ (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:56
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) Remote call leg mismatches assigned codec: 10.23.23.1:23{GSM#3} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Validating re-assignment
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_reassignment_perm_speech == FR1
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: setting codecs to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: remote addr already 1.2.3.4:1234, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) Re-Assignment complete
  MSC <-- MNCC: callref 0x80000008: MNCC_SETUP_RSP
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx MNCC_SETUP_RSP (RTP=1.2.3.4:56{GSM#3})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) new state CALL_DELIVERED -> CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{GSM#3} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: remote addr already 1.2.3.4:56, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 1002.000774 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x80000008: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_compl_ind ==


- RTP stream goes ahead, not shown here.
- Total time passed: 1125.000819 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x80000008: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x80000008: MNCC_REL_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000008 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000008: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-14:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MO call: FR1 picked by MT's MS Bearer Capability, hence MO re-assigns to FR1


- ======================== MT call: FR1 picked by MT's MS Bearer Capability, hence MO re-assigns to FR1


- MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
- VLR accepts, MSC sends CC Setup with Bearer Capability = TS 24.008 § D.1.2
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 3 (rx_from_ms,paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - Paging: now used by 4 (attached,CC,proc_arq_vlr_fn_init,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 2 (rx_from_ms,cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0xf codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0xf codecs=GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to GSM#3
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_call_conf_ind ==
- MGW acknowledges the CRCX to RAN, triggering Assignment with FR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mt_tx_assignment_perm_speech == FR1
- Assignment completes, triggering CRCX to CN
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_RAN:no-CI){UNINITIALIZED}: no change: codecs already set to GSM#3
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: GSM#3, CN: GSM#3
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_rtp_create == GSM
- Total time passed: 1126.000842 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_alert_ind == GSM
- Total time passed: 1127.000865 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{GSM#3} (from: assigned=GSM#3 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={GSM#3} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{GSM#3})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 3
a=rtpmap:3 GSM/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_setup_cnf == GSM
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 1250.000910 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-15:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MT call: FR1 picked by MT's MS Bearer Capability, hence MO re-assigns to FR1


- ======================== MO call: AMR picked by both MO and MT, but MT assigns a different payload type number
- CM Service Request with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 1
msc_a_is_accepted() == true
- MS sends CC SETUP with Bearer Capability =  AMR AMR AMR GSM-EFR GSM GSM-HR-08
  MSC <--GERAN-A-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x80000009 tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) new state NULL -> INITIATED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x10 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x10 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000009: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_ind == AMR GSM-EFR GSM GSM-HR-08
- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x80000009: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x80000009: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_rtp_create == AMR GSM-EFR GSM GSM-HR-08
- MNCC says that's fine
  MSC <-- MNCC: callref 0x80000009: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) new state INITIATED -> MO_CALL_PROC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 1251.000933 s
- The other call leg got established (not shown here), MNCC tells us so, with codecs { AMR#96 GSM-EFR GSM GSM-HR-08 }
  MSC <-- MNCC: callref 0x80000009: MNCC_ALERT_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 96 110 3 111
a=rtpmap:96 AMR/8000
a=fmtp:96 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx MNCC_ALERT_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:56
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <-- MNCC: callref 0x80000009: MNCC_SETUP_RSP
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 96 110 3 111
a=rtpmap:96 AMR/8000
a=fmtp:96 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx MNCC_SETUP_RSP (RTP=1.2.3.4:56{AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) new state CALL_DELIVERED -> CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: no change: codecs already set to AMR:octet-align=1#96,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: remote addr already 1.2.3.4:56, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 1252.000956 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x80000009: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_compl_ind ==


- RTP stream goes ahead, not shown here.
- Total time passed: 1375.001001 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x80000009: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x80000009: MNCC_REL_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 96 110 3 111
a=rtpmap:96 AMR/8000
a=fmtp:96 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x80000009 tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x80000009: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-16:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MO call: AMR picked by both MO and MT, but MT assigns a different payload type number


- ======================== MT call: AMR picked by both MO and MT, but MT assigns a different payload type number


- MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
- VLR accepts, MSC sends CC Setup with Bearer Capability = TS 24.008 § D.1.2
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 3 (rx_from_ms,paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - Paging: now used by 4 (attached,CC,proc_arq_vlr_fn_init,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 2 (rx_from_ms,cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x11 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x11 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_call_conf_ind ==
- MGW acknowledges the CRCX to RAN, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mt_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment completes, triggering CRCX to CN
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_rtp_create == AMR#96 GSM-EFR GSM GSM-HR-08
- Total time passed: 1376.001024 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_alert_ind == AMR#96 GSM-EFR GSM GSM-HR-08
- Total time passed: 1377.001047 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_setup_cnf == AMR#96 GSM-EFR GSM GSM-HR-08
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 1500.001092 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-17:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MT call: AMR picked by both MO and MT, but MT assigns a different payload type number


- ======================== MO call: AMR picked by both MO and MT, but MO assigns a different payload type number
- CM Service Request with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
  MSC <--GERAN-A-- MS: GSM48_MT_MM_CM_SERV_REQ
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: MM GSM48_MT_MM_CM_SERV_REQ
DMM msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Rx CM SERVICE REQUEST cm_service_type=MO-Call
DREF msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: + cm_service_cc: now used by 2 (rx_from_ms,cm_service_cc)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 2 (attached,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 3 (attached,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Sending DTAP: MM GSM48_MT_MM_CM_SERV_ACC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_MM_CM_SERV_ACC: 0521
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: - rx_from_ms: now used by 1 (cm_service_cc)
  cm_service_result_sent == 1
msc_a_is_accepted() == true
- MS sends CC SETUP with Bearer Capability =  AMR AMR AMR GSM-EFR GSM GSM-HR-08
  MSC <--GERAN-A-- MS: GSM48_MT_CC_SETUP
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: + rx_from_ms: now used by 2 (cm_service_cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Dispatching 04.08 message: CC GSM48_MT_CC_SETUP
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,active-conn,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x8000000a tid-8) New transaction
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + cc: now used by 3 (cm_service_cc,rx_from_ms,cc)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cm_service_cc: now used by 2 (rx_from_ms,cc)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx SETUP in state NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) starting guard timer with 180 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) SETUP to 123
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) new state NULL -> INITIATED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) codecs: :0{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x12 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x12 codecs=AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- As soon as the MGW port towards CN is created, MNCC_SETUP_IND is triggered
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) tx MNCC_SETUP_IND (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x8000000a: MNCC_SETUP_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_ind == AMR GSM-EFR GSM GSM-HR-08
- MNCC replies with MNCC_RTP_CREATE
  MSC <-- MNCC: callref 0x8000000a: MNCC_RTP_CREATE

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- MGW acknowledges the CRCX, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mo_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment succeeds, triggering MNCC_RTP_CREATE ack to MNCC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x8000000a: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 112 110 3 111
a=rtpmap:112 AMR/8000
a=fmtp:112 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_rtp_create == AMR#98 GSM-EFR GSM GSM-HR-08
- MNCC says that's fine
  MSC <-- MNCC: callref 0x8000000a: MNCC_CALL_PROC_REQ

DMNCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx MNCC_CALL_PROC_REQ
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) stopping pending guard timer
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) starting guard timer with 180 seconds
DCC trans(CC:INITIATED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) new state INITIATED -> MO_CALL_PROC
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CALL_PROC
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CALL_PROC: 8302
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- Total time passed: 1501.001115 s
- The other call leg got established (not shown here), MNCC tells us so, with codecs { AMR#98 GSM-EFR GSM GSM-HR-08 }
  MSC <-- MNCC: callref 0x8000000a: MNCC_ALERT_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 98 110 3 111
a=rtpmap:98 AMR/8000
a=fmtp:98 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx MNCC_ALERT_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) stopping pending guard timer
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) starting guard timer with 180 seconds
DCC trans(CC:MO_CALL_PROC IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) new state MO_CALL_PROC -> CALL_DELIVERED
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:56
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_ALERTING
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_ALERTING: 8301
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <-- MNCC: callref 0x8000000a: MNCC_SETUP_RSP
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 98 110 3 111
a=rtpmap:98 AMR/8000
a=fmtp:98 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx MNCC_SETUP_RSP (RTP=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) stopping pending guard timer
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) starting guard timer with 180 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) starting timer T313 with 30 seconds
DCC trans(CC:CALL_DELIVERED IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) new state CALL_DELIVERED -> CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) codecs: 10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: no change: codecs already set to AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: remote addr already 1.2.3.4:56, no change
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT: 8307
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- Total time passed: 1502.001138 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT_ACK
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT_ACK
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx CONNECT_ACK in state CONNECT_IND
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) stopping pending timer T313
DCC trans(CC:CONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) new state CONNECT_IND -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) stopping pending guard timer
DMNCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) tx MNCC_SETUP_COMPL_IND
  MSC --> MNCC: callref 0x8000000a: MNCC_SETUP_COMPL_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mo_tx_sdp_mncc_setup_compl_ind ==


- RTP stream goes ahead, not shown here.
- Total time passed: 1625.001183 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x8000000a: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x8000000a: MNCC_REL_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 98 110 3 111
a=rtpmap:98 AMR/8000
a=fmtp:98 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 832d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x8000000a tid-8) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x8000000a: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ callref-0x0 tid-8) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ:trans-8:call-18:RTP_TO_CN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-56){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:CM_SERVICE_REQ){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MO call: AMR picked by both MO and MT, but MO assigns a different payload type number


- ======================== MT call: AMR picked by both MO and MT, but MO assigns a different payload type number


- MNCC asks us to setup a call, causing Paging
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_REQ
v=0
o=OsmoMSC 0 0 IN IP4 1.2.3.4
s=GSM Call
c=IN IP4 1.2.3.4
t=0 0
m=audio 56 RTP/AVP 98 110 3 111
a=rtpmap:98 AMR/8000
a=fmtp:98 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + mncc_tx_to_gsm_cc: now used by 2 (attached,mncc_tx_to_gsm_cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + CC: now used by 3 (attached,mncc_tx_to_gsm_cc,CC)
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) New transaction
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) codecs: :0{(no-codecs)} (from: remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} RAN={(no-codecs)})
DMNCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) rx MNCC_SETUP_REQ (RTP=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Starting paging
  paging request (CALL_CONVERSATIONAL) to IMSI-901700000010650:MSISDN-46071 on GERAN-A
  strcmp(paging_expecting_imsi, vsub->imsi) == 0
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + Paging: now used by 4 (attached,mncc_tx_to_gsm_cc,CC,Paging)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - mncc_tx_to_gsm_cc: now used by 3 (attached,CC,Paging)
  paging_sent == 1
- MS replies with Paging Response, with Codec List (BSS Supported) = FR1 FR2 FR3 HR1 HR3
- VLR accepts, MSC sends CC Setup with Bearer Capability = TS 24.008 § D.1.2
  MSC <--GERAN-A-- MS: GSM48_MT_RR_PAG_RESP
  new conn
DMSC msub_fsm{active}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: Allocated
DMSC msc_a{MSC_A_ST_VALIDATE_L3}: is child of msub_fsm
DMSC msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_VALIDATE_L3
DMSC dummy_msc_i{0}: Allocated
DMSC dummy_msc_i{0}: is child of msub_fsm
DREF msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: + rx_from_ms: now used by 1 (rx_from_ms)
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: RAN decode: COMPL_L3
DBSSAP msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Complete Layer 3: Codec List (BSS Supported): GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111
DRLL msc_a(unknown:GERAN-A:NONE){MSC_A_ST_VALIDATE_L3}: Dispatching 04.08 message: RR GSM48_MT_RR_PAG_RESP
DRR msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Rx PAGING RESPONSE IMSI-901700000010650
DREF msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: + paging-response: now used by 2 (rx_from_ms,paging-response)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Allocated
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: is child of msc_a(IMSI-901700000010650:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: rev=R99 net=GERAN (no Auth)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: Received Event PR_ARQ_E_START
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + proc_arq_vlr_fn_init: now used by 4 (attached,CC,Paging,proc_arq_vlr_fn_init)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + active-conn: now used by 5 (attached,CC,Paging,proc_arq_vlr_fn_init,active-conn)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: Received Event MSC_A_EV_COMPLETE_LAYER_3_OK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_VALIDATE_L3}: state_chg to MSC_A_ST_AUTH_CIPH
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_vlr_fn_post_imsi()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_ciph()
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: RAN encode: COMMON_ID on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_node2_post_vlr()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_pres()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_trace()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: _proc_arq_vlr_post_imei()
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: proc_arq_fsm_done(PASSED)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_INIT}: state_chg to PR_ARQ_S_DONE
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Process Access Request result: PASSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: Received Event MSC_A_EV_AUTHENTICATED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTH_CIPH}: state_chg to MSC_A_ST_AUTHENTICATED
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Paging Response action (success)
DPAG Paging: IMSI-901700000010650:MSISDN-46071 for MNCC: establish call: Removing Paging Request
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071 callref-0x423 tid-255) Paging succeeded
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: + cc: now used by 3 (rx_from_ms,paging-response,cc)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: Received Event MSC_A_EV_TRANSACTION_ACCEPTED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_AUTHENTICATED}: state_chg to MSC_A_ST_COMMUNICATING
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T303 with 30 seconds
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state NULL -> CALL_PRESENT
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_SETUP
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_SETUP: 03050401a0
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - Paging: now used by 4 (attached,CC,proc_arq_vlr_fn_init,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - paging-response: now used by 2 (rx_from_ms,cc)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - proc_arq_vlr_fn_init: now used by 3 (attached,CC,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- MS confirms call, we create a RAN-side RTP and forward MNCC_CALL_CONF_IND
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CALL_CONF
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CALL_CONF
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CALL_CONF in state CALL_PRESENT
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T303
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T310 with 30 seconds
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Starting call assignment
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Allocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: is child of msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MGW <--CRCX to RTP_TO_CN-- MSC: call_id=0x13 codecs=AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_CN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111
  MGW <--CRCX to RTP_TO_RAN-- MSC: call_id=0x13 codecs=AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: Allocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){UNINITIALIZED}: is child of call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:CALL_PRESENT IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_PRESENT -> MO_TERM_CALL_CONF
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_CALL_CONF_IND
  MSC --> MNCC: callref 0x423: MNCC_CALL_CONF_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_call_conf_ind ==
- MGW acknowledges the CRCX to RAN, triggering Assignment with FR3 HR3 FR2 FR1 HR1
  MGW --CRCX OK to RTP_TO_RAN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_RAN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Sending Assignment Command
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: ASSIGNMENT_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
- VALIDATE_PERM_SPEECH OK: &bssap_assignment_command_last_channel_type == t->mt_tx_assignment_perm_speech == FR3 HR3 FR2 FR1 HR1
- Assignment completes, triggering CRCX to CN
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: ASSIGNMENT_COMPLETE
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_RAN:no-CI){UNINITIALIZED}: setting codecs to AMR:octet-align=1#112
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_RAN:no-CI:local-10-23-23-1-23){UNINITIALIZED}: setting remote addr to 1.2.3.4:1234
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Not committing: no MGW endpoint CI set up
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: :0{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment Complete: RAN: AMR:octet-align=1#112, CN: AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) Assignment complete, but still waiting for the CRCX OK on the CN side RTP
- MNCC sends MNCC_RTP_CREATE, which first waits for the CN side RTP
  MSC <-- MNCC: callref 0x423: MNCC_RTP_CREATE

DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_RTP_CREATE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Assignment for this trans already started earlier
- When the CN side RTP address is known, ack MNCC_RTP_CREATE
  MGW --CRCX OK to RTP_TO_CN--> MSC
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: Received Event CALL_LEG_EV_RTP_STREAM_ADDR_AVAILABLE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_EV_CALL_LEG_RTP_LOCAL_ADDR_AVAILABLE
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: MGW endpoint's RTP address available for the CI RTP_TO_CN: 10.23.23.1:23 (osmux=no:-2)
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_RTP_CREATE (RTP=10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_RTP_CREATE
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 98 110 3 111
a=rtpmap:98 AMR/8000
a=fmtp:98 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_rtp_create == AMR#98 GSM-EFR GSM GSM-HR-08
- Total time passed: 1626.001206 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_ALERTING
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_ALERTING
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx ALERTING in state MO_TERM_CALL_CONF
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T310
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T301 with 180 seconds
DCC trans(CC:MO_TERM_CALL_CONF IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state MO_TERM_CALL_CONF -> CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_ALERT_IND (RTP=10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_ALERT_IND
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 98 110 3 111
a=rtpmap:98 AMR/8000
a=fmtp:98 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_alert_ind == AMR#98 GSM-EFR GSM GSM-HR-08
- Total time passed: 1627.001229 s
  MSC <--GERAN-A-- MS: GSM48_MT_CC_CONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_CONNECT
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx CONNECT in state CALL_RECEIVED
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T301
DCC trans(CC:CALL_RECEIVED IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CALL_RECEIVED -> CONNECT_REQUEST
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) codecs: 10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} (from: assigned=AMR:octet-align=1#112 remote=1.2.3.4:56{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111} MS={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111} bss={GSM#3,GSM-EFR#110,AMR:octet-align=1#112,GSM-HR-08#111} RAN={AMR:octet-align=1#112,GSM-EFR#110,GSM#3,GSM-HR-08#111})
DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_SETUP_CNF (RTP=10.23.23.1:23{AMR:octet-align=1#98,GSM-EFR#110,GSM#3,GSM-HR-08#111})
  MSC --> MNCC: callref 0x423: MNCC_SETUP_CNF
v=0
o=OsmoMSC 0 0 IN IP4 10.23.23.1
s=GSM Call
c=IN IP4 10.23.23.1
t=0 0
m=audio 23 RTP/AVP 98 110 3 111
a=rtpmap:98 AMR/8000
a=fmtp:98 octet-align=1
a=rtpmap:110 GSM-EFR/8000
a=rtpmap:3 GSM/8000
a=rtpmap:111 GSM-HR-08/8000
a=ptime:20

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
- VALIDATE_SDP OK: cc_to_mncc_tx_last_sdp == t->mt_tx_sdp_mncc_setup_cnf == AMR#98 GSM-EFR GSM GSM-HR-08
  MSC <-- MNCC: callref 0x423: MNCC_SETUP_COMPL_REQ

DMNCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_SETUP_COMPL_REQ
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:CONNECT_REQUEST IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state CONNECT_REQUEST -> ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending guard timer
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_CONNECT_ACK
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_CONNECT_ACK: 030f
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST


- RTP stream goes ahead, not shown here.
- Total time passed: 1750.001274 s


- Call ends
  MSC <--GERAN-A-- MS: GSM48_MT_CC_DISCONNECT
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_DISCONNECT
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx DISCONNECT in state ACTIVE
DCC trans(CC:ACTIVE IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state ACTIVE -> DISCONNECT_IND
DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_DISC_IND
  MSC --> MNCC: callref 0x423: MNCC_DISC_IND

DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 1 (cc)
  MSC <-- MNCC: callref 0x423: MNCC_REL_REQ

DMNCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx MNCC_REL_REQ
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting guard timer with 180 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) starting timer T308 with 10 seconds
DCC trans(CC:DISCONNECT_IND IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) new state DISCONNECT_IND -> RELEASE_REQ
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Sending DTAP: CC GSM48_MT_CC_RELEASE
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN encode: DTAP on GERAN-A
- DTAP --GERAN-A--> MS: GSM48_MT_CC_RELEASE: 032d
- DTAP matches expected message
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
  MSC <--GERAN-A-- MS: GSM48_MT_CC_RELEASE_COMPL
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: + rx_from_ms: now used by 2 (cc,rx_from_ms)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: RAN decode: DTAP
DRLL msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Dispatching 04.08 message: CC GSM48_MT_CC_RELEASE_COMPL
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) rx RELEASE_COMPL in state RELEASE_REQ
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) stopping pending timer T308
DMNCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x423 tid-0) tx MNCC_REL_CNF
  MSC --> MNCC: callref 0x423: MNCC_REL_CNF

DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) Freeing transaction
DCC trans(CC:RELEASE_REQ IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) new state RELEASE_REQ -> NULL
DCC trans(CC:NULL IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP callref-0x0 tid-0) stopping pending guard timer
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - CC: now used by 2 (attached,active-conn)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - cc: now used by 1 (rx_from_ms)
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: - rx_from_ms: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_COMMUNICATING}: state_chg to MSC_A_ST_RELEASING
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Releasing: msc_a use is 0 (-)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + msc_a_fsm_releasing_onenter: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 + vlr_subscr_cancel_attach_fsm: now used by 4 (attached,active-conn,msc_a_fsm_releasing_onenter,vlr_subscr_cancel_attach_fsm)
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - vlr_subscr_cancel_attach_fsm: now used by 3 (attached,active-conn,msc_a_fsm_releasing_onenter)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){ESTABLISHING}: state_chg to RELEASING
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_RAN:no-CI:local-10-23-23-1-23:remote-1-2-3-4-1234){UNINITIALIZED}: Deallocated
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_CN:no-CI){UNINITIALIZED}: Terminating (cause = OSMO_FSM_TERM_PARENT)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_CN:no-CI){UNINITIALIZED}: Removing from parent call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DCC rtp_stream(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP:trans-0:call-19:RTP_TO_CN:no-CI){UNINITIALIZED}: Deallocated
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_EV_CALL_LEG_TERM
DCC call_leg(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){RELEASING}: Deallocated
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: + wait-Clear-Complete: now used by 1 (wait-Clear-Complete)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN encode: CLEAR_COMMAND on GERAN-A
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Received Event MSC_I_EV_FROM_A_FORWARD_ACCESS_SIGNALLING_REQUEST
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - msc_a_fsm_releasing_onenter: now used by 2 (attached,active-conn)
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: RAN decode: CLEAR_COMPLETE
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: - wait-Clear-Complete: now used by 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: Received Event MSC_A_EV_UNUSED
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASING}: state_chg to MSC_A_ST_RELEASED
DBSSAP msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Released: msc_a use is 0 (-)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Terminating (cause = OSMO_FSM_TERM_REGULAR)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Removing from parent msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DVLR Process_Access_Request_VLR(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){PR_ARQ_S_DONE}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Removing from parent msub_fsm
DREF msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: max total use count was 3
DMSC msub_fsm{active}: Received Event MSUB_EV_ROLE_TERMINATED
DMSC msub(IMSI-901700000010650:MSISDN-46071) MSC-A terminated
DMSC msub(IMSI-901700000010650:MSISDN-46071) 1 MSC-I still active
DMSC msub_fsm{active}: state_chg to terminating
DMSC msub_fsm{terminating}: Terminating in cascade, depth 2 (cause = OSMO_FSM_TERM_REGULAR, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Terminating in cascade, depth 3 (cause = OSMO_FSM_TERM_PARENT, caused by: msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP))
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Removing from parent msub_fsm
DMSC dummy_msc_i(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){0}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msub(IMSI-901700000010650:MSISDN-46071) Free
DVLR VLR subscr IMSI-901700000010650:MSISDN-46071 - active-conn: now used by 1 (attached)
DMSC msub_fsm{terminating}: Deferring: will deallocate with msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP)
DMSC msc_a(IMSI-901700000010650:MSISDN-46071:GERAN-A:PAGING_RESP){MSC_A_ST_RELEASED}: Deallocated, including all deferred deallocations
- msub gone
  llist_count(&msub_list) == 0


- ======================== SUCCESS: MT call: AMR picked by both MO and MT, but MO assigns a different payload type number
  llist_count(&msub_list) == 0
DVLR SUBSCR(IMSI-901700000010650:MSISDN-46071) freeing VLR subscr (max total use count was 5)
===== test_codecs: SUCCESS

