Copyright (C) 2017-2019 by Vadim Yanitskiy <axilirator@gmail.com>
License GPLv2+: GNU GPL version 2 or later <http://gnu.org/licenses/gpl.html>
This is free software: you are free to change and redistribute it.
There is NO WARRANTY, to the extent permitted by law.

[INFO] transceiver.py:157 Init transceiver 'BTS@127.0.0.1:5700'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5702 <-> R:127.0.0.1:5802)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5701 <-> R:127.0.0.1:5801)
[INFO] transceiver.py:157 Init transceiver 'MS@127.0.0.1:6700'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:6702 <-> R:127.0.0.1:6802)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:6701 <-> R:127.0.0.1:6801)
[INFO] transceiver.py:157 Init transceiver 'TRX1@127.0.0.1:5700/1'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5704 <-> R:127.0.0.1:5804)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5703 <-> R:127.0.0.1:5803)
[INFO] transceiver.py:157 Init transceiver 'TRX2@127.0.0.1:5700/2'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5706 <-> R:127.0.0.1:5806)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5705 <-> R:127.0.0.1:5805)
[INFO] transceiver.py:157 Init transceiver 'TRX3@127.0.0.1:5700/3'
[DEBUG] data_if.py:31 Init TRXD interface (L:0.0.0.0:5708 <-> R:127.0.0.1:5808)
[DEBUG] ctrl_if.py:29 Init TRXC interface (L:0.0.0.0:5707 <-> R:127.0.0.1:5807)
[INFO] fake_trx.py:430 Init complete
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:124 (BTS@127.0.0.1:5700) Recv RXTUNE cmd
[DEBUG] ctrl_if_trx.py:229 (TRX1@127.0.0.1:5700/1) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX2@127.0.0.1:5700/2) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:229 (TRX3@127.0.0.1:5700/3) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:131 (BTS@127.0.0.1:5700) Recv TXTUNE cmd
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX1@127.0.0.1:5700/1) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX2@127.0.0.1:5700/2) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (TRX1@127.0.0.1:5700/1) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX1@127.0.0.1:5700/1) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (TRX3@127.0.0.1:5700/3) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:229 (BTS@127.0.0.1:5700) Ignore CMD SETTSC
[DEBUG] ctrl_if_trx.py:182 (TRX2@127.0.0.1:5700/2) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX2@127.0.0.1:5700/2) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:215 (BTS@127.0.0.1:5700) Recv NOMTXPOWER cmd
[DEBUG] ctrl_if_trx.py:182 (TRX3@127.0.0.1:5700/3) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (TRX3@127.0.0.1:5700/3) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 0 -> 1
[DEBUG] ctrl_if_trx.py:207 (BTS@127.0.0.1:5700) Recv SETPOWER cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[WARNING] ctrl_if_trx.py:196 (BTS@127.0.0.1:5700) Requested TRXD header version 2 is not supported, suggesting 1...
[DEBUG] ctrl_if_trx.py:182 (BTS@127.0.0.1:5700) Recv SETFORMAT cmd
[INFO] ctrl_if_trx.py:201 (BTS@127.0.0.1:5700) TRXD header version 1 -> 1
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:115 (BTS@127.0.0.1:5700) Recv POWEROFF cmd
[INFO] ctrl_if_trx.py:117 (BTS@127.0.0.1:5700) Stopping transceiver...
[DEBUG] ctrl_if_trx.py:220 (TRX1@127.0.0.1:5700/1) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX2@127.0.0.1:5700/2) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (TRX3@127.0.0.1:5700/3) Recv RFMUTE cmd
[DEBUG] ctrl_if_trx.py:220 (BTS@127.0.0.1:5700) Recv RFMUTE cmd
