/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Timea Moder - initial implementation
******************************************************************************/
//
//  File:               ChargingApplications_3GPP_TS32299_be0.ddf
//  Description:        DDF for Diameter Charging Application 3GPP TS 32.299 11.15.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////

// APPLICATION-NAME: DCA
// APPLICATION-REVISION: V11_15_0

// AVP implementations according to: 
// 3GPP TS 32.299 V11.15.0 - Telecommunication management; Charging management;
//
//
// Dependant applications
// 3GPP TS 29.229  - Cx and Dx interfaces based on the Diameter protocol
// IETF RFC 3588   - Diameter Base Protocol
// RFC 4006 - Diameter Credit Control Application
//
// Notes:
//


// 3GPP TS 32.299 V11.5.0 
type enumerated Command_Code 
{  
  Accounting     (271),
  Re_Auth        (258)
}


// 3GPP TS 32.299 V11.15.0
// AVP: Access-Network-Information (1263) 3GPP (10415)
// 7.2.1
type AVP_OctetString Access_Network_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Access-Transfer-Information (2709) 3GPP (10415)
// 7.2.1A
type AVP_Grouped Access_Transfer_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Access-Transfer-Type (2710) 3GPP (10415)
// 7.2.1.B
type enumerated Access_Transfer_Type
{
  PS_to_CS_Transfer (0),
  CS_to_PS_Transfer (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Account-Expiration  (2309) 3GPP (10415)
// 7.2.2
type AVP_Time Account_Expiration;

// 3GPP TS 32.299 V11.15.0
// AVP: Accumulated-Cost (2052) 3GPP (10415)
// 7.2.3
type AVP_Grouped Accumulated_Cost;

// 3GPP TS 32.299 V11.15.0
// AVP: Adaptations (1217) 3GPP (10415)
// 7.2.4
type enumerated Adaptations
{
  YES (0),
  NO  (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Additional-Content-Information (1207) 3GPP (10415)
// 7.2.5
type AVP_Grouped Additional_Content_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Additional-Type-Information (1205) 3GPP (10415)
// 7.2.6
type AVP_UTF8String Additional_Type_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Address-Data (897) 3GPP (10415)
// 7.2.7
type AVP_UTF8String Address_Data;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Address-Domain (898) 3GPP (10415)
// 7.2.8
type AVP_Grouped Address_Domain;

// 3GPP TS 32.299 V11.15.0
// AVP: Address-Type (899) 3GPP (10415)
// 7.2.9
type enumerated Address_Type
{
  E_MAIL_ADDRESS         (0),
  MSISDN                 (1),
  IPV4_ADDRESS           (2),
  IPV6_ADDRESS           (3),
  NUMERIC_SHORTCODE      (4),
  ALPHANUMERIC_SHORTCODE (5),
  OTHER                  (6),
  IMSI                   (7)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Addressee-Type (1208) 3GPP (10415)
// 7.2.10
type enumerated Addressee_Type
{
  TO  (0),
  CC  (1),
  BCC (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: AF-Correlation-Information (1276) 3GPP (10415)
// 7.2.11
type AVP_Grouped AF_Correlation_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Alternate-Charged-Party-Address (1280) 3GPP (10415)
// 7.2.12
type AVP_UTF8String Alternate_Charged_Party_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Cost-Information (2053) 3GPP (10415)
// 7.2.13
type AVP_Grouped AoC_Cost_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Format (2310) 3GPP (10415)
// 7.2.14
type enumerated AoC_Format
{
  MONETARY (0),
  NON_MONETARY  (1),
  CAI (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Information (2054) 3GPP (10415)
// 7.2.15
type AVP_Grouped AoC_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Request-Type (2055) 3GPP (10415)
// 7.2.16
type enumerated AoC_Request_Type
{
  AoC_NOT_REQUESTED     (0),
  AoC_FULL              (1),
  AoC_COST_ONLY         (2),
  AoC_TARIFF_ONLY       (3)
}

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Service (2311) 3GPP (10415)
// 7.2.17
type AVP_Grouped AoC_Service;

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Service-Obligatory-Type (2312) 3GPP (10415)
// 7.2.18
type enumerated AoC_Service_Obligatory_Type
{
  NON_BINDING   (0),
  BINDING       (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Service-Type (2313) 3GPP (10415)
// 7.2.19
type enumerated AoC_Service_Type
{
  NONE   (0),
  AOC_S  (1),
  AOC_D  (2),
  AOC_E  (3)
}

// 3GPP TS 32.299 V11.15.0
// AVP: AoC-Subscription-Information (2314) 3GPP (10415)
// 7.2.20
type AVP_Grouped AoC_Subscription_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Applic-ID (1218) 3GPP (10415)
// 7.2.21
type AVP_UTF8String Applic_ID;

// 3GPP TS 32.299 V11.15.0
// AVP: Application-provided-Called-Party-Address (837) 3GPP (10415)
// 7.2.22
type AVP_UTF8String Application_provided_Called_Party_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Application-Server (836) 3GPP (10415)
// 7.2.23
type AVP_UTF8String Application_Server;

// 3GPP TS 32.299 V11.15.0
// AVP: Application-Server-Information (850) 3GPP (10415)
// 7.2.24
type AVP_Grouped Application_Server_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Associated-Party-Address (2035) 3GPP (10415)
// 7.2.25
type AVP_UTF8String Associated_Party_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Associated-URI (856) 3GPP (10415)
// 7.2.26
type AVP_UTF8String Associated_URI;

// 3GPP TS 32.299 V11.15.0
// AVP: Authorised-QoS (849) 3GPP (10415)
// 7.2.27
type AVP_UTF8String Authorised_QoS;

// 3GPP TS 32.299 V11.15.0
// AVP: Aux-Applic-Info (1219) 3GPP (10415)
// 7.2.28
type AVP_UTF8String Aux_Applic_Info;

// 3GPP TS 32.299 V11.15.0
// AVP: Base-Time-Interval (1265) 3GPP (10415)
// 7.2.29
type AVP_Unsigned32 Base_Time_Interval;

// 3GPP TS 32.299 V11.15.0
// AVP: Bearer-Service (854) 3GPP (10415)
// 7.2.30
type AVP_OctetString Bearer_Service;

// 3GPP TS 32.299 V11.15.0
// AVP: BSSID (2716) 3GPP (10415)
// 7.2.30A
type AVP_UTF8String BSSID;

// 3GPP TS 32.299 V11.15.0
// AVP: Called-Asserted-Identity (1250) 3GPP (10415)
// 7.2.31
type AVP_UTF8String Called_Asserted_Identity;

// 3GPP TS 32.299 V11.15.0
// AVP: Called-Party-Address (832) 3GPP (10415)
// 7.2.32
type AVP_UTF8String Called_Party_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Calling-Party-Address (831) 3GPP (10415)
// 7.2.33
type AVP_UTF8String Calling_Party_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Carrier-Select-Routing-Information (2023) 3GPP (10415)
// 7.2.34
type AVP_UTF8String Carrier_Select_Routing_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Cause-Code (861) 3GPP (10415)
// 7.2.35
type AVP_Integer32 Cause_Code;
		
// 3GPP TS 32.299 V11.15.0
// AVP: CG-Address (846) 3GPP (10415)
// 7.2.36
type AVP_Address CG_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Change-Condition  (2037) 3GPP (10415)
// 7.2.37
type AVP_Integer32 Change_Condition;

// 3GPP TS 32.299 V11.15.0
// AVP: Change-Time  (2038) 3GPP (10415)
// 7.2.38
type AVP_Time Change_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Charge-Reason-Code (2118) 3GPP (10415)
// 7.2.38A
type enumerated Charge_Reason_Code
{
  UNKNOWN (0),
  USAGE (1),
  COMMUNICATION_ATTEMPT_CHARGE (2),
  SETUP_CHARGE (3),
  ADD_ON_CHARGE (4)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Charged-Party (857) 3GPP (10415)
// 7.2.39
type AVP_UTF8String Charged_Party;

// 3GPP TS 32.299 V11.15.0
// AVP: Charging-Characteristics-Selection-Mode (2066) 3GPP (10415)
// 7.2.39A
type enumerated Charging_Characteristics_Selection_Mode
{
  SERVING_NODE_SUPPLIED (0),
  SUBSCRIPTION_SPECIFIC (1),
  APN_SPECIFIC (2),
  HOME_DEFAULT (3),
  ROAMING_DEFAULT (4),
  VISITING_DEFAULT (5)
}
		
// 3GPP TS 32.299 V11.15.0
// AVP: Class-Identifier (1214) 3GPP (10415)
// 7.2.40
type enumerated Class_Identifier
{
  PERSONAL      (0),
  ADVERTISMENT  (1),
  INFORMATIONAL (2),
  AUTO          (3)
}
	
// 3GPP TS 32.299 V11.15.0
// AVP: Client-Address (2018) 3GPP (10415)
// 7.2.41
type AVP_Address Client_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Content-Class (1220) 3GPP (10415)
// 7.2.42
type enumerated Content_Class
{
  TEXT          (0),
  IMAGE_BASIC   (1),
  IMAGE_RICH    (2),
  VIDEO_BASIC   (3),
  VIDEO_RICH    (4),
  MEGAPIXEL     (5),
  CONTENT_BASIC (6),
  CONTENT_RICH  (7)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Content-Disposition (828) 3GPP (10415)
// 7.2.43
type AVP_UTF8String Content_Disposition;

// 3GPP TS 32.299 V11.15.0
// AVP: Content-Length (827) 3GPP (10415)
// 7.2.44
type AVP_Unsigned32 Content_Length;

// 3GPP TS 32.299 V11.15.0
// AVP: Content-Size (1206) 3GPP (10415)
// 7.2.45
type AVP_Unsigned32 Content_Size;

// 3GPP TS 32.299 V11.15.0
// AVP: Content-Type (826) 3GPP (10415)
// 7.2.46
type AVP_UTF8String Content_Type;
		
// 3GPP TS 32.299 V11.15.0
// AVP: CSG-Access-Mode (2317) 3GPP (10415)
// 7.2.46A
type enumerated CSG_Access_Mode
{
  CLOSED_MODE (0),
  HYBRID_MODE (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: CSG-Membership-Indication (2318) 3GPP (10415)
// 7.2.46B
type enumerated CSG_Membership_Indication
{
  NOT_CSG_MEMBER (0),
  CSG_MEMBER (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Current-Tariff (2056) 3GPP (10415)
// 7.2.47
type AVP_Grouped Current_Tariff;

// 3GPP TS 32.299 V11.15.0
// AVP: CUG-Information (2304) 3GPP (10415)
// 7.2.48
type AVP_OctetString CUG_Information;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Data-Coding-Scheme (2001) 3GPP (10415)
// 7.2.49
type AVP_Integer32 Data_Coding_Scheme;		

// 3GPP TS 32.299 V11.15.0
// AVP: DCD-Information (2115) 3GPP (10415)
// 7.2.50
type AVP_Grouped DCD_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Deferred-Location-Event-Type (1230) 3GPP (10415)
// 7.2.51
type AVP_UTF8String Deferred_Location_Event_Type;

// 3GPP TS 32.299 V11.15.0
// AVP: Delivery-Report-Requested (1216) 3GPP (10415)
// 7.2.52
type enumerated Delivery_Report_Requested
{
  NO  (0),
  YES (1)
}
		
// 3GPP TS 32.299 V11.15.0
// AVP: Destination-Interface (2002) 3GPP (10415)
// 7.2.53
type AVP_Grouped Destination_Interface;		

// 3GPP TS 32.299 V11.15.0
// AVP: Diagnostics (2039) 3GPP (10415)
// 7.2.54
type AVP_Integer32 Diagnostics;

// 3GPP TS 32.299 V11.15.0
// AVP: Domain-Name (1200) 3GPP (10415)
// 7.2.55
type AVP_UTF8String Domain_Name;

// 3GPP TS 32.299 V11.15.0
// AVP: DRM-Content (1221) 3GPP (10415)
// 7.2.56
type enumerated DRM_Content
{
  NO  (0),
  YES (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Dynamic-Address-Flag (2051) 3GPP (10415)
// 7.2.57
type enumerated Dynamic_Address_Flag
{
  STATIC    (0),
  DYNAMIC   (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Dynamic-Address-Flag-Extension (2068) 3GPP (10415)
// 7.2.57A
type enumerated Dynamic_Address_Flag_Extension
{
  STATIC    (0),
  DYNAMIC   (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Early-Media-Description (1272) 3GPP (10415)
// 7.2.58
type AVP_Grouped Early_Media_Description;

// 3GPP TS 32.299 V11.15.0
// AVP: Envelope (1266) 3GPP (10415)
// 7.2.59
type AVP_Grouped Envelope;

// 3GPP TS 32.299 V11.15.0
// AVP: Envelope-End-Time (1267) 3GPP (10415)
// 7.2.60
type AVP_Time Envelope_End_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Envelope-Reporting (1268) 3GPP (10415)
// 7.2.61
type enumerated Envelope_Reporting
{
  DO_NOT_REPORT_ENVELOPES                 (0),
  REPORT_ENVELOPES                        (1),
  REPORT_ENVELOPES_WITH_VOLUME            (2),
  REPORT_ENVELOPES_WITH_EVENTS            (3),
  REPORT_ENVELOPES_WITH_VOLUME_AND_EVENTS (4)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Envelope-Start-Time (1269) 3GPP (10415)
// 7.2.62
type AVP_Time Envelope_Start_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Event (825) 3GPP (10415)
// 7.2.63
type AVP_UTF8String Event;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Event-Charging-TimeStamp (1258) 3GPP (10415)
// 7.2.64
type AVP_Time Event_Charging_TimeStamp;

// 3GPP TS 32.299 V11.15.0
// AVP: Event-Type (823) 3GPP (10415)
// 7.2.65
type AVP_Grouped Event_Type;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Expires (888) 3GPP (10415)
// 7.2.66
type AVP_Unsigned32 Expires;

// 3GPP TS 32.299 V11.15.0
// AVP: File-Repair-Supported (1224) 3GPP (10415)
// 7.2.67
type enumerated File_Repair_Supported
{
  SUPPORTED     (1),
  NOT_SUPPORTED (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: From-Address (2708) 3GPP (10415)
// 7.2.67A
type AVP_UTF8String From_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: GGSN-Address (847) 3GPP (10415)
// 7.2.68
type AVP_Address GGSN_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: IM-Information (2110) 3GPP (10415)
// 7.2.69
type AVP_Grouped IM_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Incremental-Cost (2062) 3GPP (10415)
// 7.2.70
type AVP_Grouped Incremental_Cost;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Interface-Id (2003) 3GPP (10415)
// 7.2.71
type AVP_UTF8String Interface_Id;		
		
// 3GPP TS 32.299 V11.15.0
// AVP: Interface-Port (2004) 3GPP (10415)
// 7.2.72
type AVP_UTF8String Interface_Port;		
		
// 3GPP TS 32.299 V11.15.0
// AVP: Interface-Text (2005) 3GPP (10415)
// 7.2.73
type AVP_UTF8String Interface_Text;		
		
// 3GPP TS 32.299 V11.15.0
// AVP: Interface-Type (2006) 3GPP (10415)
// 7.2.74
type enumerated Interface_Type;	
{
  UNKNOWN                 (0),
  MOBILE_ORIGINATING      (1),
  MOBILE_TERMINATING      (2),
  APPLICATION_ORIGINATING (3),
  APPLICATION_TERMINATION (4)
}

// 3GPP TS 32.299 V11.15.0
// AVP: IMS-Application-Reference-Identifier (2601) 3GPP (10415)
// 7.2.74A
type AVP_UTF8String IMS_Application_Reference_Identifier;

// 3GPP TS 32.299 V11.15.0
// AVP: IMS-Charging-Identifier (841) 3GPP (10415)
// 7.2.75
type AVP_UTF8String IMS_Charging_Identifier;

// 3GPP TS 32.299 V11.15.0
// AVP: IMS-Communication-Service-Identifier (1281) 3GPP (10415)
// 7.2.76
type AVP_UTF8String IMS_Communication_Service_Identifier;		

// 3GPP TS 32.299 V11.15.0
// AVP: IMS-Emergency-Indicator (2322) 3GPP (10415)
// 7.2.76A
type enumerated IMS_Emergency_Indicator;
{
  Non_Emergency (0),
  Emergency (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: IMS-Information (876) 3GPP (10415)
// 7.2.77
type AVP_Grouped IMS_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: IMS-Visited-Network-Identifier (2713) 3GPP (10415)
// 7.2.77A
type AVP_UTF8String IMS_Visited_Network_Identifier;

// 3GPP TS 32.299 V11.15.0
// AVP: IMSI-Unauthenticated-Flag (2308) 3GPP (10415)
// 7.2.78
type enumerated IMSI_Unauthenticated_Flag;	
{
  AUTHENTICATED    (0),
  UNAUTHENTICATED  (1)
}
	
// 3GPP TS 32.299 V11.15.0
// AVP: Incoming-Trunk-Group-Id (852) 3GPP (10415)
// 7.2.79
type AVP_UTF8String Incoming_Trunk_Group_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: Initial-IMS-Charging-Identifier (2321) 3GPP (10415)
// 7.2.79A
type AVP_UTF8String Initial_IMS_Charging_Identifier;

// 3GPP TS 32.299 V11.15.0
// AVP: Inter-Operator-Identifier (838) 3GPP (10415)
// 7.2.80
type AVP_Grouped Inter_Operator_Identifier;

// 3GPP TS 32.299 V11.15.0
// AVP: IP-Realm-Default-Indication (2603) 3GPP (10415)
// 7.2.80A
type enumerated IP_Realm_Default_Indication;	
{
  DEFAULT_IP_REALM_NOT_USED    (0),
  DEFAULT_IP_REALM_USED        (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-APN (1231) 3GPP (10415)
// 7.2.81
type AVP_UTF8String LCS_APN;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Client-Dialed-By-MS (1233) 3GPP (10415)
// 7.2.82
type AVP_UTF8String LCS_Client_Dialed_By_MS;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Client-External-ID (1234) 3GPP (10415)
// 7.2.83
type AVP_UTF8String LCS_Client_External_ID;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Client-Id (1232) 3GPP (10415)
// 7.2.84
type AVP_Grouped LCS_Client_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Client-Name (1235) 3GPP (10415)
// 7.2.85
type AVP_Grouped LCS_Client_Name;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Client-Type (1241) 3GPP (10415)
// 7.2.86
type enumerated LCS_Client_Type
{
  EMERGENCY_SERVICES        (0),
  VALUE_ADDED_SERVICES      (1),
  PLMN_OPERATOR_SERVICES    (2),
  LAWFUL_INTERCEPT_SERVICES (3)
}

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Data-Coding-Scheme (1236) 3GPP (10415)
// 7.2.87
type AVP_UTF8String LCS_Data_Coding_Scheme;		
		
// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Format-Indicator (1237) 3GPP (10415)
// 7.2.88
type enumerated LCS_Format_Indicator
{
  LOGICAL_NAME   (0),
  EMAIL_ADDRESS  (1),
  MSISDN         (2),
  URL		 (3),
  SIP_URL        (4)
}

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Information (878) 3GPP (10415)
// 7.2.89
type AVP_Grouped LCS_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Name-String (1238) 3GPP (10415)
// 7.2.90
type AVP_UTF8String LCS_Name_String;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Requestor-Id (1239) 3GPP (10415)
// 7.2.91
type AVP_Grouped LCS_Requestor_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: LCS-Requestor-Id-String (1240) 3GPP (10415)
// 7.2.92
type AVP_UTF8String LCS_Requestor_Id_String;


// 3GPP TS 32.299 V11.15.0
// AVP: Local-GW-Inserted-Indication (2604) 3GPP (10415)
// 7.2.92A
type enumerated Local_GW_Inserted_Indication 
{
  LOCAL_GW_NOT_INSERTED            (0),
  LOCAL_GW_INSERTED                (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Local-Sequence-Number (2063) 3GPP (10415)
// 7.2.93
type AVP_Unsigned32 Local_Sequence_Number;


// 3GPP TS 32.299 V11.15.0
// AVP: Location-Estimate (1242) 3GPP (10415)
// 7.2.94
type AVP_OctetString Location_Estimate;

// 3GPP TS 32.299 V11.15.0
// AVP: Location-Estimate-Type (1243) 3GPP (10415)
// 7.2.95
type enumerated Location_Estimate_Type 
{
  CURRENT_LOCATION            (0),
  CURRENT_LAST_KNOWN_LOCATION (1),
  INITIAL_LOCATION            (2),
  ACTIVATE_DEFERRED_LOCATION  (3),
  CANCEL_DEFERRED_LOCATION    (4)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Location-Type (1244) 3GPP (10415)
// 7.2.96
type AVP_Grouped Location_Type;
	
// 3GPP TS 32.299 V11.15.0
// AVP: Low-Balance-Indication (2020) 3GPP (10415)
// 7.2.97
type enumerated Low_Balance_Indication
{
  NOT_APPLICABLE (0),
  YES            (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Low-Priority-Indicator (2602) 3GPP (10415)
// 7.2.97A
type enumerated Low_Priority_Indicator
{
  NOT_APPLICABLE (0),
  YES            (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: MBMS-GW-Address (2307) 3GPP (10415)
// 7.2.98
type AVP_Address MBMS_GW_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: MBMS-Information (880) 3GPP (10415)
// 7.2.99
type AVP_Grouped MBMS_Information;		

// 3GPP TS 32.299 V11.15.0
// AVP: MBMS-User-Service-Type (1225) 3GPP (10415)
// 7.2.100
type enumerated MBMS_User_Service_Type
{
  DOWNLOAD  (1),
  STREAMING (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Media-Initiator-Flag (882) 3GPP (10415)
// 7.2.101
type enumerated Media_Initiator_Flag
{
  CALLED_PARTY   (0),
  CALLING_PARTY  (1),
  UNKNOWN        (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Media-Initiator-Party (1288) 3GPP (10415)
// 7.2.102
type AVP_UTF8String Media_Initiator_Party;		

// 3GPP TS 32.299 V11.15.0
// AVP: Message-Body (889) 3GPP (10415)
// 7.2.103
type AVP_Grouped Message_Body;
	
// 3GPP TS 32.299 V11.15.0
// AVP: Message-Class (1213) 3GPP (10415)
// 7.2.104
type AVP_Grouped Message_Class;		

// 3GPP TS 32.299 V11.15.0
// AVP: Message-ID (1210) 3GPP (10415)
// 7.2.105
type AVP_UTF8String Message_ID;

// 3GPP TS 32.299 V11.15.0
// AVP: Message-Size (1212) 3GPP (10415)
// 7.2.106
type AVP_Unsigned32 Message_Size;	 	

// 3GPP TS 32.299 V11.15.0
// AVP: Message-Type (1211) 3GPP (10415)
// 7.2.107
type enumerated Message_Type
{
  M_SEMD_REQ          (1),
  M_SEMD_CONF         (2),
  M_NOTIFICATION_IND  (3),
  M_NOTIFYRESP_IND    (4),
  M_RETRIEVE_CONF     (5),
  M_ACKNOWLEDGE_IND   (6),
  M_DELIVERY_IND      (7),
  M_READ_REC_IND      (8),
  M_READ_ORIG_IND     (9),
  M_FORWARD_REQ      (10),
  M_FORWARD_CONF     (11),
  M_MBOX_STORE_CONF  (12),
  M_MBOX_VIEW_CONF   (13),
  M_MBOX_UPLOAD_CONF (14),
  M_MBOX_DELETE_CONF (15)
}

// 3GPP TS 32.299 V11.15.0
// AVP: MM-Content-Type (1203) 3GPP (10415)
// 7.2.108
type AVP_Grouped MM_Content_Type;


// 3GPP TS 32.299 V11.15.0
// AVP: MMBox-Storage-Requested (1248) 3GPP (10415)
// 7.2.109
type enumerated MMBox_Storage_Requested
{
  NO  (0),
  YES (1)
}
// 3GPP TS 32.299 V11.15.0
// AVP: MMS-Information (877) 3GPP (10415)
// 7.2.110
type AVP_Grouped MMS_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: MMTel-Information (2030) 3GPP (10415)
// 7.2.111
type AVP_Grouped MMTel_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: MMTel-SService-Type (2031) 3GPP (10415)
// 7.2.111aA
type AVP_Unsigned32 MMTel_SService_Type;

// 3GPP TS 32.299 V11.15.0
// AVP: Neighbour-Node-Address (2705) 3GPP (10415)
// 7.2.111A
type AVP_Address Neighbour_Node_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Next-Tariff (2057) 3GPP (10415)
// 7.2.112
type AVP_Grouped Next_Tariff;

// 3GPP TS 32.299 V11.15.0
// AVP: NNI-Information (2703) 3GPP (10415)
// 7.2.112A
type AVP_Grouped NNI_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: NNI-Type (2704) 3GPP (10415)
// 7.2.112B
type enumerated NNI_Type
{
  Non_Roaming (0),
  Roaming_Without_Loopback (1),
  Roaming_With_Loopback (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Node-Functionality (862) 3GPP (10415)
// 7.2.113
type enumerated Node_Functionality
{
  S_CSCF  (0),
  P_CSCF  (1),
  I_CSCF  (2),
  MRFC    (3),
  MGCF    (4),
  BGCF    (5),
  AS      (6),
  IBCF    (7),
  S_GW    (8),
  P_GW    (9),
  HSGW    (10),
  E_CSCF  (11),
  MME     (12),
  TRF     (13),
  TF      (14),
  ATCF    (15)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Node-Id (2064) 3GPP (10415)
// 7.2.114
type AVP_UTF8String Node_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: Number-Of-Diversions (2034) 3GPP (10415)
// 7.2.115
type AVP_Unsigned32 Number_Of_Diversions;
	
// 3GPP TS 32.299 V11.15.0
// AVP: Number-of-Messages-Sent (2019) 3GPP (10415)
// 7.2.116
type AVP_Unsigned32 Number_of_Messages_Sent;		

// 3GPP TS 32.299 V11.15.0
// AVP: Number-Of-Participants (885) 3GPP (10415)
// 7.2.117
type AVP_Unsigned32 Number_Of_Participants;
			
// 3GPP TS 32.299 V11.15.0
// AVP: Number-Of-Received-Talk-Bursts (1282) 3GPP (10415)
// 7.2.118
type AVP_Unsigned32 Number_Of_Received_Talk_Bursts;

// 3GPP TS 32.299 V11.15.0
// AVP: Number-Of-Talk-Bursts (1283) 3GPP (10415)
// 7.2.119
type AVP_Unsigned32 Number_Of_Talk_Bursts;

// 3GPP TS 32.299 V11.15.0
// AVP: Number-Portability-Routing-Information (2024) 3GPP (10415)
// 7.2.120
type AVP_UTF8String Number_Portability_Routing_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Offline-Charging (1278) 3GPP (10415)
// 7.2.121
type AVP_Grouped Offline_Charging;

// 3GPP TS 32.299 V11.15.0
// AVP: Online-Charging-Flag (2303) 3GPP (10415)
// 7.2.122
type enumerated Online_Charging_Flag
{
  ECF_ADDRESS_NOT_PROVIDED  (0),
  ECF_ADDRESS_PROVIDED  (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Originating-IOI (839) 3GPP (10415)
// 7.2.123
type AVP_UTF8String Originating_IOI;

// 3GPP TS 32.299 V11.15.0
// AVP: Originator (864) 3GPP (10415)
// 7.2.124
type enumerated Originator
{
  CALLING_PARTY	(0),
  CALLED_PARTY 	(1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Originator-Address (886) 3GPP (10415)
// 7.2.125
type AVP_Grouped Originator_Address;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Originator-Interface (2009) 3GPP (10415)
// 7.2.126
type AVP_Grouped Originator_Interface;		

// 3GPP TS 32.299 V11.15.0
// AVP: Originator-Received-Address (2027) 3GPP (10415)
// 7.2.127 
type AVP_Grouped Originator_Received_Address;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Originating-SCCP-Address (2008) 3GPP (10415)
// 7.2.128
type AVP_Address Originating_SCCP_Address;		

// 3GPP TS 32.299 V11.15.0
// AVP: Outgoing-Session-Id (2320) 3GPP (10415)
// 7.2.128A
type AVP_UTF8String Outgoing_Session_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: Outgoing-Trunk-Group-Id (853) 3GPP (10415)
// 7.2.129
type AVP_UTF8String Outgoing_Trunk_Group_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: Participants-Involved (887) 3GPP (10415)
// 7.2.130
type AVP_UTF8String Participants_Involved;	

// 3GPP TS 32.299 V11.15.0
// AVP: Participant-Group (1260) 3GPP (10415)
// 7.2.131
type AVP_Grouped Participant_Group;

// 3GPP TS 32.299 V11.15.0
// AVP: Participant-Access-Priority (1259) 3GPP (10415)
// 7.2.132
type enumerated Participant_Access_Priority
{
  PRE_EMPTIVE_PRIORITY (1),
  HIGH_PRIORITY        (2),
  NORMAL_PRIORITY      (3),
  LOW_PRIORITY         (4)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Participant-Action-Type (2049) 3GPP (10415)
// 7.2.133
type enumerated Participant_Action_Type
{
  CREATE_CONF       (0),
  JOIN_CONF         (1),
  INVITE_INTO_CONF  (2),
  QUIT_CONF         (3)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PDG-Address (895) 3GPP (10415)
// 7.2.134
type AVP_Address PDG_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: PDG-Charging-Id (896) 3GPP (10415)
// 7.2.135
type AVP_Unsigned32 PDG_Charging_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: PDN-Connection-Charging-ID (2050) 3GPP (10415)
// 7.2.136
type AVP_Unsigned32 PDN_Connection_Charging_ID;

// 3GPP TS 32.299 V11.15.0
// AVP: PDP-Address (1227) 3GPP (10415)
// 7.2.137
type AVP_Address PDP_Address;		

// 3GPP TS 32.299 V11.15.0
// AVP: PDP-Address-Prefix-Length (2606) 3GPP (10415)
// 7.2.137a
type AVP_Unsigned32 PDP_Address_Prefix_Length;

// 3GPP TS 32.299 V11.15.0
// AVP: PDP-Context-Type (1247) 3GPP (10415)
// 7.2.138
type enumerated PDP_Context_Type
{
  PRIMARY   (0),
  SECONDARY (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Change-Conditions (1261) 3GPP (10415)
// 7.2.139
type enumerated PoC_Change_Conditions
{
  SERVICE_CHANGE                 (0),
  VOLUME_LIMIT                   (1),
  TIME_LIMIT                     (2),
  NUMBER_OF_TALK_BURST_LIMIT     (3),
  NUMBER_OF_ACTIVE_PARTICIPANTS  (4),
  TARIFF_TIME                    (5)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Change-Time (1262) 3GPP (10415)
// 7.2.140
type AVP_Time PoC_Change_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Controlling-Address (858) 3GPP (10415)
// 7.2.141
type AVP_UTF8String PoC_Controlling_Address;		

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Event-Type (2025) 3GPP (10415)
// 7.2.142
type enumerated PoC_Event_Type
{
  NORMAL                         (0),
  INSTANT_PERSONAL_ALERT_EVENT   (1),
  POC_GROUP_ADVERTISEMENT_EVENT  (2),
  EARLY_SESSION_SETTING_UP_EVENT (3),
  POC_TALK_BURST                 (4)
}
		
// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Group-Name (859) 3GPP (10415)
// 7.2.143
type AVP_UTF8String PoC_Group_Name;	

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Information (879) 3GPP (10415)
// 7.2.144
type AVP_Grouped PoC_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Server-Role	 (883) 3GPP (10415)
// 7.2.145
type enumerated PoC_Server_Role	
{
  PARTICIPATING_POC_SERVER  (0),
  CONTROLLING_POC_SERVER    (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Session-Id (1229) 3GPP (10415)
// 7.2.146
type AVP_UTF8String PoC_Session_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Session-Initiation-Type (1277) 3GPP (10415)
// 7.2.147
type enumerated PoC_Session_Initiation_Type
{
  PRE_ESTABLISHED (0),
  ON_DEMAND       (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-Session-Type (884) 3GPP (10415)
// 7.2.148
type enumerated PoC_Session_Type
{
  ONE_TO_ONE_POC_SESSION         (0),
  CHAT_POC_GROUP_SESSION         (1),
  PRE_ARRANGED_POC_GROUP_SESSION (2),
  AD_HOC_POC_GROUP_SESSION       (3)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-User-Role (1252) 3GPP (10415)
// 7.2.149
type AVP_Grouped PoC_User_Role;

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-User-Role-IDs (1253) 3GPP (10415)
// 7.2.150
type AVP_UTF8String PoC_User_Role_IDs;

// 3GPP TS 32.299 V11.15.0
// AVP: PoC-User-Role-info-Units (1254) 3GPP (10415)
// 7.2.151
type enumerated PoC_User_Role_info_Units
{
  MODERATOR           (1),
  DISPATCHER          (2),
  SESSION_OWNER       (3),
  SESSION_PARTICIPANT (4)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Positioning-Data (1245) 3GPP (10415)
// 7.2.152
type AVP_UTF8String Positioning_Data;		 	


// 3GPP TS 32.299 V11.15.0
// AVP: Preferred-AoC-Currency (2315) 3GPP (10415)
// 7.2.153
type AVP_Unsigned32 Preferred_AoC_Currency;

// 3GPP TS 32.299 V11.15.0
// AVP: Priority (1209) 3GPP (10415)
// 7.2.154
type enumerated Priority
{
  LOW    (0),
  NORMAL (1),
  HIGH   (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PS-Append-Free-Format-Data (867) 3GPP (10415)
// 7.2.155
type enumerated PS_Append_Free_Format_Data
{
  APPEND    (0),
  OVERWRITE (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: PS-Free-Format-Data (866) 3GPP (10415)
// 7.2.156
type AVP_OctetString PS_Free_Format_Data;

// 3GPP TS 32.299 V11.15.0
// AVP: PS-Furnish-Charging-Information (865) 3GPP (10415)
// 7.2.157
type AVP_Grouped PS_Furnish_Charging_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: PS-Information (874) 3GPP (10415)
// 7.2.158
type AVP_Grouped PS_Information;
				
// 3GPP TS 32.299 V11.15.0
// AVP: Quota-Consumption-Time (881) 3GPP (10415)
// 7.2.159
type AVP_Unsigned32 Quota_Consumption_Time;		

// 3GPP TS 32.299 V11.15.0
// AVP: Quota-Holding-Time (871) 3GPP (10415)
// 7.2.160
type AVP_Unsigned32 Quota_Holding_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Rate-Element (2058) 3GPP (10415)
// 7.2.161
type AVP_Grouped Rate_Element;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Read-Reply-Report-Requested (1222) 3GPP (10415)
// 7.2.162
type enumerated Read_Reply_Report_Requested
{
  NO  (0),
  YES (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Real-Time-Tariff-Information (2305) 3GPP (10415)
// 7.2.164
type AVP_Grouped Real_Time_Tariff_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Received-Talk-Burst-Time (1284) 3GPP (10415)
// 7.2.165
type AVP_Unsigned32 Received_Talk_Burst_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Received-Talk-Burst-Volume (1285) 3GPP (10415)
// 7.2.166
type AVP_Unsigned32 Received_Talk_Burst_Volume;

// 3GPP TS 32.299 V11.15.0
// AVP: Recipient-Address (1201) 3GPP (10415)
// 7.2.167
type AVP_Grouped Recipient_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Recipient-Info (2026) 3GPP (10415)
// 7.2.168
type AVP_Grouped Recipient_Info;

// 3GPP TS 32.299 V11.15.0
// AVP: Recipient-Received-Address (2028) 3GPP (10415)
// 7.2.169
type AVP_Grouped Recipient_Received_Address;
	
// 3GPP TS 32.299 V11.15.0
// AVP: Recipient-SCCP-Address (2010) 3GPP (10415)
// 7.2.170
type AVP_Address Recipient_SCCP_Address;		

// 3GPP TS 32.299 V11.15.0
// AVP: Refund-Information (2022) 3GPP (10415)
// 7.2.171
type AVP_OctetString Refund_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Relationship-Mode (2706) 3GPP (10415)
// 7.2.171A
type enumerated Relationship_Mode
{
  Trusted (0),
  Non_Trusted (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Related-IMS-Charging-Identifier (2711) 3GPP (10415)
// 7.2.171B
type AVP_UTF8String Related_IMS_Charging_Identifier;

// 3GPP TS 32.299 V11.15.0
// AVP: Related-IMS-Charging-Identifier-Node (2712) 3GPP (10415)
// 7.2.171C
type AVP_Address Related_IMS_Charging_Identifier_Node;
	
// 3GPP TS 32.299 V11.15.0
// AVP: Remaining-Balance (2021) 3GPP (10415)
// 7.2.172
type AVP_Grouped Remaining_Balance;

// 3GPP TS 32.299 V8.5.0
// AVP: Reply-Applic-ID (1223) 3GPP (10415)
// 7.2.173
type AVP_UTF8String Reply_Applic_ID;
	
// 3GPP TS 32.299 V11.15.0
// AVP: Reply-Path-Requested (2011) 3GPP (10415)
// 7.2.174
type enumerated Reply_Path_Requested
{
  NO_REPLY_PATH_SET (0),
  REPLY_PATH_SET    (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Reporting-Reason (872) 3GPP (10415)
// 7.2.175
type enumerated Reporting_Reason
{
  THRESHOLD                (0),
  QHT                      (1),
  FINAL                    (2),
  QUOTA_EXHAUSTED          (3),
  VALIDITY_TIME            (4),
  OTHER_QUOTA_TYPE         (5),
  RATING_CONDITION_CHANGE  (6),
  FORCED_REAUTHORISATION   (7),
  POOL_EXHAUSTED           (8)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Requested-Party-Address (1251) 3GPP (10415)
// 7.2.176
type AVP_UTF8String Requested_Party_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Role-Of-Node (829) 3GPP (10415)
// Note: not compatible with V9.2.0 or before (see spec.)
// 7.2.177
type enumerated Role_Of_Node
{
  ORIGINATING_ROLE  (0),
  TERMINATING_ROLE  (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Route-Header-Received (3403) 3GPP (10415)
// 7.2.177A
type AVP_UTF8String Route_Header_Received;

// 3GPP TS 32.299 V11.15.0
// AVP: Route-Header-Transmitted (3404) 3GPP (10415)
// 7.2.177B
type AVP_UTF8String Route_Header_Transmitted;

// 3GPP TS 32.299 V11.15.0
// AVP: Scale-Factor (2059) 3GPP (10415)
// 7.2.178
type AVP_Grouped Scale_Factor;

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-Answer-Timestamp (1275) 3GPP (10415)
// 7.2.179
type AVP_Time SDP_Answer_Timestamp;

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-Media-Component (843) 3GPP (10415)
// 7.2.180
type AVP_Grouped SDP_Media_Component;

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-Media-Description (845) 3GPP (10415)
// 7.2.181
type AVP_UTF8String SDP_Media_Description;		

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-Media-Name (844) 3GPP (10415)
// 7.2.182
type AVP_UTF8String SDP_Media_Name;

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-Offer-Timestamp (1274) 3GPP (10415)
// 7.2.183
type AVP_Time SDP_Offer_Timestamp;

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-Session-Description (842) 3GPP (10415)
// 7.2.184
type AVP_UTF8String SDP_Session_Description;

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-TimeStamps (1273) 3GPP (10415)
// 7.2.185
type AVP_Grouped SDP_TimeStamps;

// 3GPP TS 32.299 V11.15.0
// AVP: SDP-Type (2036) 3GPP (10415)
// 7.2.186
type enumerated SDP_Type
{
  SDP_OFFER  (0),
  SDP_ANSWER (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Session-Direction	(2707) 3GPP (10415)
// 7.2.186A
type enumerated Session_Direction
{
  Inbound (0),
  Outbound (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Served-Party-IP-Address	(848) 3GPP (10415)
// 7.2.187
type AVP_Address Served_Party_IP_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: Service-Data-Container (2040) 3GPP (10415)
// 7.2.189
type AVP_Grouped Service_Data_Container;

// 3GPP TS 32.299 V11.15.0
// AVP: Service-Id (855) 3GPP (10415)
// 7.2.190
type AVP_UTF8String Service_Id;
	
// 3GPP TS 32.299 V11.15.0
// AVP: Service-Generic-Information (1256) 3GPP (10415)
// 7.2.191
type AVP_Grouped Service_Generic_Information;	 			

// 3GPP TS 32.299 V11.15.0
// AVP: Service-Information (873) 3GPP (10415)
// 7.2.192
type AVP_Grouped Service_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Service-Mode (2032) 3GPP (10415)
// 7.2.193
type AVP_Unsigned32 Service_Mode;

// 3GPP TS 32.299 V11.15.0
// AVP: Service-Specific-Data (863) 3GPP (10415)
// 7.2.194
type AVP_UTF8String Service_Specific_Data;

// 3GPP TS 32.299 V11.15.0
// AVP: Service-Specific-Info (1249) 3GPP (10415)
// 7.2.195
type AVP_Grouped Service_Specific_Info;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Service-Specific-Type (1257) 3GPP (10415)
// 7.2.196
type AVP_Unsigned32 Service_Specific_Type;

// 3GPP TS 32.299 V11.15.0
// AVP: Serving-Node-Type (2047) 3GPP (10415)
// 7.2.198
type enumerated Serving_Node_Type
{
  SGSN      (0),
  PMIPSGW   (1),
  GTPSGW    (2),
  ePDG      (3),
  hSGW      (4),
  MME       (5)
}
		
// 3GPP TS 32.299 V11.15.0
// AVP: SGSN-Address (1228) 3GPP (10415)
// 7.2.199
type AVP_Address SGSN_Address;


// 3GPP TS 32.299 V11.15.0
// AVP: SGW-Address (2067) 3GPP (10415)
// 7.2.199A
type AVP_Address SGW_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: SGW-Change (2065) 3GPP (10415)
// 7.2.200
type enumerated SGW_Change
{
  ACR_Start_NOT_due_to_SGW_Change      (0),
  ACR_Start_due_to_SGW_Change          (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: SIP-Method (824) 3GPP (10415)
// 7.2.201
type AVP_UTF8String SIP_Method;

// 3GPP TS 32.299 V11.15.0
// AVP: SIP-Request-Timestamp (834) 3GPP (10415)
// 7.2.202
type AVP_Time SIP_Request_Timestamp;

// 3GPP TS 32.299 V11.15.0
// AVP: SIP-Request-Timestamp-Fraction (2301) 3GPP (10415)
// 7.2.203
type AVP_Unsigned32 SIP_Request_Timestamp_Fraction;

// 3GPP TS 32.299 V11.15.0
// AVP: SIP-Response-Timestamp (835) 3GPP (10415)
// 7.2.204
type AVP_Time SIP_Response_Timestamp;

// 3GPP TS 32.299 V11.15.0
// AVP: SIP-Response-Timestamp-Fraction (2302) 3GPP (10415)
// 7.2.205
type AVP_Unsigned32 SIP_Response_Timestamp_Fraction;

// 3GPP TS 32.299 V11.15.0
// AVP: SM-Discharge-Time (2012) 3GPP (10415)
// 7.2.206
type AVP_Time SM_Discharge_Time;		
		
// 3GPP TS 32.299 V11.15.0
// AVP: SM-Message-Type (2007) 3GPP (10415)
// 7.2.207
type enumerated SM_Message_Type
{
  SUBMISSION         (0),
  DELIVERY_REPORT    (1),
  SM_SERVICE_REQUEST (2)
}		
	
// 3GPP TS 32.299 V11.15.0
// AVP: SM-Protocol-ID (2013) 3GPP (10415)
// 7.2.208
type AVP_OctetString SM_Protocol_ID;

// 3GPP TS 32.299 V11.15.0
// AVP: SM-Status (2014) 3GPP (10415)
// 7.2.209
type AVP_OctetString SM_Status;		
	
// 3GPP TS 32.299 V11.15.0
// AVP: SM-User-Data-Header (2015) 3GPP (10415)
// 7.2.210
type AVP_OctetString SM_User_Data_Header;		
	
// 3GPP TS 32.299 V11.15.0
// AVP: SMS-Information (2000) 3GPP (10415)
// 7.2.211
type AVP_Grouped SMS_Information;		
	
// 3GPP TS 32.299 V11.15.0
// AVP: SMS-Node (2016) 3GPP (10415)
// 7.2.212
type enumerated SMS_Node
{
  SMS_ROUTER              (0),
  IP_SM_GW                (1),
  SMS_ROUTER_AND_IP_SM_GW (2),
  SMS_SC                  (3)
}

// WARNING: Unsigned32 used instead of enumerated type
// 3GPP TS 32.299 V11.15.0
// AVP: SM-Service-Type (2029) 3GPP (10415)
// 7.2.213
type AVP_Unsigned32 SM_Service_Type;
	
// 3GPP TS 32.299 V11.15.0
// AVP: SMSC-Address (2017) 3GPP (10415)
// 7.2.214
type AVP_Address SMSC_Address;	

// 3GPP TS 32.299 V11.15.0
// AVP: Start-Time (2041) 3GPP (10415)
// 7.2.215
type AVP_Time Start_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Status-AS-Code (2702) 3GPP (10415)
// 7.2.215A
type enumerated Status_AS_Code
{
  code_4xx (0),
  code_5xx (1),
  Timeout (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Stop-Time (2042) 3GPP (10415)
// 7.2.216
type AVP_Time Stop_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Submission-Time (1202) 3GPP (10415)
// 7.2.217
type AVP_Time Submission_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Subscriber-Role (2033) 3GPP (10415)
// 7.2.218
type enumerated Subscriber_Role
{
  ORIGINATING (0),
  TERMINATING (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Supplementary-Service (2048) 3GPP (10415)
// 7.2.219
type AVP_Grouped Supplementary_Service;

// 3GPP TS 32.299 V11.15.0
// AVP: TAD-Identifier (2717) 3GPP (10415)
// 7.2.219A
type enumerated TAD_Identifier
{
  CS (0),
  PS (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Talk-Burst-Exchange (1255) 3GPP (10415)
// 7.2.220
type AVP_Grouped Talk_Burst_Exchange;	 	

// 3GPP TS 32.299 V11.15.0
// AVP: Talk-Burst-Time (1286) 3GPP (10415)
// 7.2.221
type AVP_Unsigned32 Talk_Burst_Time;

// 3GPP TS 32.299 V11.15.0
// AVP: Talk-Burst-Volume (1287) 3GPP (10415)
// 7.2.222
type AVP_Unsigned32 Talk_Burst_Volume;

// 3GPP TS 32.299 V11.15.0
// AVP: Tariff-Information (2060) 3GPP (10415)
// 7.2.223
type AVP_Grouped Tariff_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: Tariff-XML (2306) 3GPP (10415)
// 7.2.224
type AVP_UTF8String Tariff_XML;

// 3GPP TS 32.299 V11.15.0
// AVP: Terminating-IOI (840) 3GPP (10415)
// 7.2.225
type AVP_UTF8String Terminating_IOI;

// 3GPP TS 32.299 V11.15.0
// AVP: Time_First_Usage (2043) 3GPP (10415)
// 7.2.226
type AVP_Time Time_First_Usage;

// 3GPP TS 32.299 V11.15.0
// AVP: Time_Last_Usage (2044) 3GPP (10415)
// 7.2.227
type AVP_Time Time_Last_Usage;

// 3GPP TS 32.299 V11.15.0
// AVP: Time-Quota-Mechanism (1270) 3GPP (10415)
// 7.2.228
type AVP_Grouped Time_Quota_Mechanism;

// 3GPP TS 32.299 V11.15.0
// AVP: Time-Quota-Threshold (868) 3GPP (10415)
// 7.2.229
type AVP_Unsigned32 Time_Quota_Threshold;		

// 3GPP TS 32.299 V11.15.0
// AVP: Time-Quota-Type (1271) 3GPP (10415)
// 7.2.230
type enumerated Time_Quota_Type
{
  DISCRETE_TIME_PERIOD    (0),
  CONTINUOUS_TIME_PERIOD  (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Time-Stamps (833) 3GPP (10415)
// 7.2.231
type AVP_Grouped Time_Stamps;

// 3GPP TS 32.299 V11.15.0
// AVP: Time-Usage (2045) 3GPP (10415)
// 7.2.232
type AVP_Unsigned32 Time_Usage;

// 3GPP TS 32.299 V11.15.0
// AVP: Traffic-Data-Volumes (2046) 3GPP (10415)
// 7.2.233
type AVP_Grouped Traffic_Data_Volumes;

// 3GPP TS 32.299 V11.15.0
// AVP: Transcoder-Inserted-Indication (2605) 3GPP (10415)
// 7.2.233A
type enumerated Transcoder_Inserted_Indication
{
  TRANSCODER_NOT_INSERTED    (0),
  TRANSCODER_INSERTED        (1)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Transit-IOI-List (2701) 3GPP (10415)
// 7.2.233B
type AVP_UTF8String Transit_IOI_List;

// 3GPP TS 32.299 V11.15.0
// AVP: Token-Text (1215) 3GPP (10415)
// 7.2.234
type AVP_UTF8String Token_Text;

// 3GPP TS 32.299 V11.15.0
// AVP: Trigger (1264) 3GPP (10415)
// 7.2.235
type AVP_Grouped Trigger;

// 3GPP TS 32.299 V11.15.0
// AVP: Trigger-Type (870) 3GPP (10415)
// 7.2.236
type enumerated Trigger_Type 
{
  CHANGE_IN_SGSN_IP_ADDRESS                     (1),
  CHANGE_IN_QOS                                 (2),
  CHANGE_IN_LOCATION                            (3),
  CHANGE_IN_RAT                                 (4),
  CHANGE_IN_UE_TIMEZONE                         (5),
  CHANGEINQOS_TRAFFIC_CLASS                    (10),
  CHANGEINQOS_RELIABILITY_CLASS                (11),
  CHANGEINQOS_DELAY_CLASS                      (12),
  CHANGEINQOS_PEAK_THROUGHPUT                  (13),
  CHANGEINQOS_PRECEDENCE_CLASS                 (14),
  CHANGEINQOS_MEAN_THROUGHPUT                  (15),
  CHANGEINQOS_MAXIMUM_BIT_RATE_FOR_UPLINK      (16),
  CHANGEINQOS_MAXIMUM_BIT_RATE_FOR_DOWNLINK    (17),
  CHANGEINQOS_RESIDUAL_BER                     (18),
  CHANGEINQOS_SDU_ERROR_RATIO                  (19),
  CHANGEINQOS_TRANSFER_DELAY                   (20),
  CHANGEINQOS_TRAFFIC_HANDLING_PRIORITY        (21),
  CHANGEINQOS_GUARANTEED_BIT_RATE_FOR_UPLINK   (22),
  CHANGEINQOS_GUARANTEED_BIT_RATE_FOR_DOWNLINK (23),
  CHANGEINLOCATION_MCC                         (30),
  CHANGEINLOCATION_MNC                         (31),
  CHANGEINLOCATION_RAC                         (32),
  CHANGEINLOCATION_LAC                         (33),
  CHANGEINLOCATION_CellId                      (34),
  CHANGEINLOCATION_TAC                         (35),
  CHANGEINLOCATION_ECGI                        (36),
  CHANGE_IN_MEDIA_COMPOSITION                  (40),
  CHANGE_IN_PARTICIPANTS_NMB                   (50),
  CHANGE_IN_THRSHLD_OF_PARTICIPANTS_NMB        (51),
  CHANGE_IN_USER_PARTICIPATING_TYPE            (52),
  CHANGE_IN_SERVICE_CONDITION                  (60),
  CHANGE_IN_SERVING_NODE                       (61),
  CHANGE_IN_USER_CSG_INFORMATION               (70),
  CHANGE_IN_HYBRID_SUBSCRIBED_USER_CSG_INFORMATION (71),
  CHANGE_IN_HYBRID_UNSUBSCRIBED_USER_CSG_INFORMATION (72)
}

// 3GPP TS 32.299 V11.15.0
// AVP: Trunk-Group-Id (851) 3GPP (10415)
// 7.2.237
type AVP_Grouped Trunk_Group_Id;

// 3GPP TS 32.299 V11.15.0
// AVP: TWAN-User-Location-Info (2714) 3GPP (10415)
//
type AVP_Grouped TWAN_User_Location_Info;

// WARNING: Unsigned32 used instead of enumerated type
// 3GPP TS 32.299 V11.15.0
// AVP: Type-Number (1204) 3GPP (10415)
// 7.2.238
type AVP_Unsigned32 Type_Number;

// 3GPP TS 32.299 V11.15.0
// AVP: Unit-Cost (2061) 3GPP (10415)
// 7.2.239
type AVP_Grouped Unit_Cost;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Unit-Quota-Threshold (1226) 3GPP (10415)
// 7.2.240
type AVP_Unsigned32 Unit_Quota_Threshold;

// 3GPP TS 32.299 V11.15.0
// AVP: User-CSG-Information (2319) 3GPP (10415)
// 7.2.240A
type AVP_Grouped User_CSG_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: User-Participating-Type (1279) 3GPP (10415)
// 7.2.241
type enumerated User_Participating_Type
{
  NORMAL     (0),
  NW_POC_BOX (1),
  UE_POC_BOX (2)
}

// 3GPP TS 32.299 V11.15.0
// AVP: User-Session-Id (830) 3GPP (10415)
// 7.2.242
type AVP_UTF8String User_Session_Id;
		
// 3GPP TS 32.299 V11.15.0
// AVP: Volume-Quota-Threshold (869) 3GPP (10415)
// 7.2.243
type AVP_Unsigned32 Volume_Quota_Threshold;
		
// 3GPP TS 32.299 V11.15.0
// AVP: WAG-Address (890) 3GPP (10415)
// 7.2.244
type AVP_Address WAG_Address;

// 3GPP TS 32.299 V11.15.0
// AVP: WAG-PLMN-Id (891) 3GPP (10415)
// 7.2.245
type AVP_OctetString WAG_PLMN_Id;		

// 3GPP TS 32.299 V11.15.0
// AVP: WLAN-Information (875) 3GPP (10415)
// 7.2.246
type AVP_Grouped WLAN_Information;

// 3GPP TS 32.299 V11.15.0
// AVP: WLAN-Radio-Container (892) 3GPP (10415)
// 7.2.247
type AVP_Grouped WLAN_Radio_Container;
		
// 3GPP TS 32.299 V11.15.0
// AVP: WLAN-Session-Id (1246) 3GPP (10415)
// 7.2.248
type AVP_Unsigned32 WLAN_Session_Id;
		
// 3GPP TS 32.299 V11.15.0
// AVP: WLAN-Technology (893) 3GPP (10415)
// 7.2.249
type AVP_Unsigned32 WLAN_Technology;
		
// 3GPP TS 32.299 V11.15.0
// AVP: WLAN-UE-Local-IPAddress (894) 3GPP (10415)
// 7.2.250
type AVP_Address WLAN_UE_Local_IPAddress;
