/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               GmbInterface_3GPP_TS29061_980.ddf
//  Description:        DDF for Gmb according to 3GPP TS 29.061 V9.8.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: GMB
// APPLICATION-REVISION: V9_8_0

// AVP implementations according to: 
// 3GPP TS 29.061 V9.8.0 - Interworking between the Public Land Mobile Network 
// (PLMN) supporting packet based services and Packet Data Networks (PDN)
//
//
// Dependant applications
// IETF RFC 3588  - Diameter Base Protocol
// IETF RFC 4005  - Diameter Network Address Server
//
// Notes: 
// Present application has its own vendor specific Diameter application id: 16777223
//

// 3GPP TS 29.061 V9.8.0 17.6
type enumerated Command_Code 
{
  Authorize_Authenticate (265),
  Re_Auth                (258),
  Session_Termination    (275),
  Abort_Session          (274)
}


// 3GPP TS 29.061 V9.8.0
// AVP: TMGI (900) 3GPP (10415)
// 17.7.2
type AVP_OctetString TMGI;

// 3GPP TS 29.061 V9.8.0
// AVP: Required-MBMS-Bearer-Capabilities (901) 3GPP (10415)
// 17.7.3
type AVP_UTF8String Required_MBMS_Bearer_Capabilities;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-StartStop-Indication (902) 3GPP (10415)
// 17.7.5
type enumerated MBMS_StartStop_Indication
{
  START              (0),
  STOP               (1),
  UPDATE             (2)
}

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Service-Area (903) 3GPP (10415)
// 17.7.6
type AVP_OctetString MBMS_Service_Area;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Session-Duration (904) 3GPP (10415)
// 17.7.7
type AVP_OctetString MBMS_Session_Duration;

// 3GPP TS 29.061 V9.8.0
// AVP: 3GPP-IMSI (1) 3GPP (10415)
// 16.4.7
type AVP_UTF8String 3GPP_IMSI;

// 3GPP TS 29.061 V9.8.0
// AVP: Alternative-APN (905) 3GPP (10415)
// 17.7.8
type AVP_UTF8String Alternative_APN;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Service-Type (906) 3GPP (10415)
// 17.7.9
type enumerated MBMS_Service_Type
{
  MULTICAST              (0),
  BROADCAST              (1)
}

// 3GPP TS 29.061 V9.8.0
// AVP: 3GPP-SGSN-Address (6) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_SGSN_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: 3GPP-SGSN-IPv6-Address (15) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_SGSN_IPv6_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-2G-3G-Indicator (907) 3GPP (10415)
// 17.7.10
type enumerated MBMS_2G_3G_Indicator
{
  TwoG                    (0),
  ThreeG                  (1),
  TwoG_AND_ThreeG         (2)
}

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Session-Identity (908) 3GPP (10415)
// 17.7.11
type AVP_OctetString MBMS_Session_Identity;

// 3GPP TS 29.061 V9.8.0
// AVP: RAI (909) 3GPP (10415)
// 17.7.12
type AVP_UTF8String RAI;


// 3GPP TS 29.061 V9.8.0
// AVP: 3GPP-IMEISV (20) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_IMEISV;

// 3GPP TS 29.061 V9.8.0
// AVP: 3GPP-RAT-Type (21) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_RAT_Type;

// 3GPP TS 29.061 V9.8.0
// AVP: 3GPP-User-Location-Info (22) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_User_Location_Info;

// 3GPP TS 29.061 V9.8.0
// AVP: 3GPP-MS-TimeZone (23) 3GPP (10415)
// 16.4.7
type AVP_OctetString 3GPP_MS_TimeZone;

// 3GPP TS 29.061 V9.8.0
// AVP: Additional-MBMS-Trace-Info (910) 3GPP (10415)
// 17.7.13
type AVP_OctetString Additional_MBMS_Trace_Info;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Time-To-Data-Transfer (911) 3GPP (10415)
// 17.7.14
type AVP_OctetString MBMS_Time_To_Data_Transfer;


// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Session-Repetition-Number (912) 3GPP (10415)
// 17.7.15
type AVP_OctetString MBMS_Session_Repetition_Number;


// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Required-QoS (913) 3GPP (10415)
// 17.7.16
type AVP_UTF8String MBMS_Required_QoS;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Counting-Information (914) 3GPP (10415)
// 17.7.17
type enumerated MBMS_Counting_Information
{
  COUNTING_NOT_APPLICABLE              (0),
  COUNTING_APPLICABLE                  (1)
}

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-User-Data-Mode-Indication (915) 3GPP (10415)
// 17.7.18
type enumerated MBMS_User_Data_Mode_Indication
{
  Unicast                (0),
  Multicast_and_Unicast  (1)
}

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-GGSN-Address (916) 3GPP (10415)
// 17.7.19
type AVP_OctetString MBMS_GGSN_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-GGSN-IPv6-Address (917) 3GPP (10415)
// 17.7.20
type AVP_OctetString MBMS_GGSN_IPv6_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-BMSC-SSM-IP-Address (918) 3GPP (10415)
// 17.7.21
type AVP_OctetString MBMS_BMSC_SSM_IP_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-BMSC-SSM-IPv6-Address (919) 3GPP (10415)
// 17.7.22
type AVP_OctetString MBMS_BMSC_SSM_IPv6_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Flow-Identifier (920) 3GPP (10415)
// 17.7.23
type AVP_OctetString MBMS_Flow_Identifier;

// 3GPP TS 29.061 V9.8.0
// AVP: CN-IP-Multicast-Distribution (921) 3GPP (10415)
// 17.7.24
type enumerated CN_IP_Multicast_Distribution
{
  NO_IP_MULTICAST (0),
  IP_MULTICAST    (1)
}

// WARNING: Unsigned32 used instead of enumerated type
// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-HC-Indicator (922) 3GPP (10415)
// 17.7.25
type AVP_Unsigned32 MBMS_HC_Indicator;
