/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               ShInterface_3GPP_TS29329_620.ddf
//  Description:        DDF for Sh Interface according to 3GPP 29.329 v6.2.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////

// APPLICATION-NAME: Sh
// APPLICATION-REVISION: v6_2_0

// AVP implementations according to: 
// 3GPP 29.329 v6.2.0 - Sh Interface based on the Diameter PROTOCOL
//
//
// Dependant applications
// 3GPP TS 29.229  - Cx and Dx interfaces based on the Diameter protocol
// IETF RFC 3588   - Diameter Base Protocol
//
// Notes: 
// Present application has its own vendor specific Diameter application id: 16777217
//

// 3GPP 29.329 v6.2.0  6.1
type enumerated Command_Code 
{
  User_Data              (306),
  Profile_Update         (307),
  Subscribe_Notification (308),
  Push_Notification      (309)
}

// 3GPP 29.329 v6.2.0
// AVP: User-Identity (700) 3GPP (10415)
// 6.3.1
type AVP_Grouped User_Identity;

// 3GPP 29.329 v6.2.0
// AVP: MSISDN (701) 3GPP (10415)
// 6.3.2
type AVP_OctetString MSISDN;

// 3GPP 29.329 v6.2.0
// AVP: User-Data (702) 3GPP (10415)
// 6.3.3
type AVP_OctetString User_Data;

// 3GPP 29.329 v6.2.0
// AVP: Data-Reference (703) 3GPP (10415)
// 6.3.4
type enumerated Data_Reference
{
  REPOSITORY_DATA          (0),
  IMS_PUBLIC_IDENTITY     (10),
  IMS_USER_STATE          (11),
  S_CSCF_NAME             (12),
  INITIAL_FILTER_CRITERIA (13),
  LOCATION_INFORMATION    (14),
  USER_STATE              (15),
  CHARGING_INFORMATION    (16),
  MSISDN                  (17)
}

// 3GPP 29.329 v6.2.0
// AVP: Service-Indication (704) 3GPP (10415)
// 6.3.5
type AVP_OctetString Service_Indication;

// 3GPP 29.329 v6.2.0
// AVP: Subs-Req-Type (705) 3GPP (10415)
// 6.3.6
type enumerated Subs_Req_Type
{
  SUBSCRIBE               (0),
  UNSUBSCRIBE             (1)
}

// 3GPP 29.329 v6.2.0
// AVP: Requested-Domain (706) 3GPP (10415)
// 6.3.7
type enumerated Requested_Domain
{
  CS_DOMAIN               (0),
  PS_DOMAIN               (1)
}

// 3GPP 29.329 v6.2.0
// AVP: Current-Location (707) 3GPP (10415)
// 6.3.8
type enumerated Current_Location
{
  DO_NOT_NEED_INITIATE_ACTIVE_LOCATION_RETRIEVAL  (0),
  INITIATE_ACTIVE_LOCATION_RETRIEVAL              (1)
}

// 3GPP 29.329 v6.2.0
// AVP: Identity-Set (708) 3GPP (10415)
// 6.3.10
type enumerated Identity_Set
{
  ALL_IDENTITIES          (0),
  REGISTERED_IDENTITES    (1),
  IMPLICIT_IDENTITIES     (2)
}


