module STP_Tests_TCAP {

/* Osmocom STP test suite in in TTCN-3, TCAP routing (TCAP: ITU Q.771-774)
 * (C) 2025 by sysmocom - s.f.m.c. GmbH <info@sysmocom.de>
 * Author: Pau Espin Pedrol <pespin@sysmocom.de>
 * All rights reserved.
 *
 * Released under the terms of GNU General Public License, Version 2 or
 * (at your option) any later version.
 *
 * SPDX-License-Identifier: GPL-2.0-or-later
 */

import from General_Types all;
import from Osmocom_Types all;
import from IPL4asp_Types all;
import from Misc_Helpers all;

import from Osmocom_VTY_Functions all;

import from M3UA_Types all;
import from M3UA_Templates all;
import from M3UA_CodecPort all;
import from M3UA_CodecPort_CtrlFunct all;

import from M3UA_Emulation all;
import from MTP3asp_Types all;
import from MTP3asp_PortType all;

import from SCCP_Types all;
import from SCCP_Templates all;
import from SCCPasp_Types all;
import from SCCP_Emulation all;
import from SCCP_Adapter all;

import from IPA_Emulation all;
import from IPA_EXT_TCAP_ROUTING all;

import from STP_Tests_Common all;
import from STP_Tests_IPA all;
import from STP_Tests_M3UA all;

import from TCAPMessages language "ASN.1:1997" all;
import from TCAP_Types all;
import from TCAP_Templates all;
import from TCAP_CodecPort all;

const integer MAX_NUM_ASP := 4;
const OCT1 c_M3UA_SI_SCCP := '03'O;

type record TCAP_CT_Configuration {
	/* Name of the ASP in the STP, (eg. to access it over VTY) */
	charstring asp_name,
	/* Name of the AS in the STP, (eg. to access it over VTY) */
	charstring as_name,
	SCCP_Adapter_Config cfg
}
type record of TCAP_CT_Configuration TCAP_CT_Configurations;

modulepar {
	/* local ASPs. Set in .cfg file: */
	TCAP_CT_Configurations mp_tcap_configs := {}
}

type component TCAP_CT extends Test_CT {
	var SCCP_Adapter g_tcap[MAX_NUM_ASP];
	port TCAP_CODEC_PT SCCP_TCAP[MAX_NUM_ASP];
	/* Port for IPA Extension TCAP_ROUTING */
	port IPA_TCAP_ROUTING_PT IPA_TCAP_ROUTING[MAX_NUM_ASP];
};

private function tcap_build_configs(template (omit) Misc_Helpers.ro_charstring asps := omit)
runs on TCAP_CT return TCAP_CT_Configurations
{
	if (not isvalue(asps)) {
		return mp_tcap_configs;
	}

	var TCAP_CT_Configurations tcap_configs := {};
	for (var integer i := 0; i < lengthof(asps); i := i + 1) {
		var boolean found := false;
		for (var integer j := 0; j < lengthof(mp_tcap_configs); j := j + 1) {
			if (mp_tcap_configs[j].asp_name == valueof(asps[i])) {
				found := true;
				tcap_configs := tcap_configs & {mp_tcap_configs[j]};
				break;
			}
		}
		if (not found) {
			Misc_Helpers.f_shutdown(__BFILE__, __LINE__, fail,
						log2str("Could not find ASP ", asps[i], ", check your configuration"));
		}
	}
	return tcap_configs;
}


private function f_init_tcap(TCAP_CT_Configurations tcap_configs) runs on TCAP_CT {
	f_init_common();

	for (var integer i := 0; i < lengthof(tcap_configs); i := i + 1) {
		if (tcap_configs[i].cfg.transport == SCCP_TRANSPORT_SCCPlite) {
			tcap_configs[i].cfg.tpars.sccplite.ipa_ccm_pars := c_IPA_default_ccm_pars;
			tcap_configs[i].cfg.tpars.sccplite.ipa_ccm_pars.name := tcap_configs[i].as_name;
		}
		f_sccp_adapter_init(g_tcap[i], tcap_configs[i].cfg, "STP_TCAP_" & int2str(i));
		connect(self:SCCP_TCAP[i], g_tcap[i].vc_SCCP:SCCP_SP_PORT);
		if (tcap_configs[i].cfg.transport == SCCP_TRANSPORT_SCCPlite) {
			connect(self:IPA_TCAP_ROUTING[i], g_tcap[i].vc_IPA:IPA_TCAP_ROUTING_PORT);
		}
	}

	for (var integer i := 0; i < lengthof(tcap_configs); i := i + 1) {
		f_sccp_adapter_start(g_tcap[i]);
	}

	/* M3UA Emulation doesn't yet signal events up the stack, so it's
	impossible to know exactly when the ASP becomes active. Hence, wait for
	a while here to do ASPUP+ASPAC procedures: */
	f_sleep(3.0);
}

private function f_asp_tx_ipa_ext_tcap_routing(template (value) IPA_EXT_TCAP_ROUTING_Message send_msg,
					       integer asp_idx := 0, boolean exp_ack := true)
runs on TCAP_CT
{
	var IPA_EXT_TCAP_ROUTING_Message msg;
	timer T := 2.0;

	IPA_TCAP_ROUTING[asp_idx].send(send_msg);
	T.start;
	alt {
	[exp_ack] IPA_TCAP_ROUTING[asp_idx].receive(tr_IPA_EXT_TCAP_ROUTING_ACK);
	[not exp_ack] IPA_TCAP_ROUTING[asp_idx].receive(tr_IPA_EXT_TCAP_ROUTING_NACK);
	[] IPA_TCAP_ROUTING[asp_idx].receive(IPA_EXT_TCAP_ROUTING_Message:?) -> value msg {
		setverdict(fail, __SCOPE__, "(): Rx unexpected IPA: ", msg);
		Misc_Helpers.f_shutdown(__BFILE__, __LINE__);
		}
	[] T.timeout {
		setverdict(fail, __SCOPE__, "(): Timeout waiting for IPA EXT TCAP ROUTING ACK/NACK");
		Misc_Helpers.f_shutdown(__BFILE__, __LINE__);
		}
	}
}

private function f_asp_tx_tcap(template (value) TCMessage tcap_msg,
			       integer asp_idx := 0)
runs on TCAP_CT
{
	var template (value) TCAP_N_UNITDATA_req sccp_unitdata_req :=
		ts_TCAP_UNITDATA_req(g_tcap[asp_idx].sccp_addr_peer,
				     g_tcap[asp_idx].sccp_addr_own,
				     tcap_msg,
				     RETURN_OPTION_ON_ERROR)
	SCCP_TCAP[asp_idx].send(sccp_unitdata_req);
}


private altstep as_asp_rx_tcap_any(template (present) TCMessage tcap_msg := ?,
				   integer tx_asp_idx := 0)
runs on TCAP_CT
{
	var template (present) TCAP_N_UNITDATA_ind exp_sccp_unitdata_ind :=
		tr_TCAP_UNITDATA_ind(g_tcap[tx_asp_idx].sccp_addr_peer,
				     g_tcap[tx_asp_idx].sccp_addr_own,
				     tcap_msg);
	[] any from SCCP_TCAP.receive(exp_sccp_unitdata_ind) {
		setverdict(pass);
	}
}

private altstep as_asp_rx_tcap(template (present) TCMessage tcap_msg := ?,
			       integer tx_asp_idx := 0,
			       integer rx_asp_idx := 0, boolean fail_rx_others := true)
runs on TCAP_CT
{
	var template (present) TCAP_N_UNITDATA_ind exp_sccp_unitdata_ind :=
		tr_TCAP_UNITDATA_ind(g_tcap[tx_asp_idx].sccp_addr_peer,
				     g_tcap[tx_asp_idx].sccp_addr_own,
				     tcap_msg);

	[] SCCP_TCAP[rx_asp_idx].receive(exp_sccp_unitdata_ind) {
		setverdict(pass);
	}
	[fail_rx_others] any from SCCP_TCAP.receive(exp_sccp_unitdata_ind) {
		Misc_Helpers.f_shutdown(__BFILE__, __LINE__, fail,
					log2str("Rx TCAP at unexpected ASP with idx != ", rx_asp_idx));
	}
}

private function f_asp_tx_tcap_exp(template (value) TCMessage tcap_msg,
				   integer tx_asp_idx,
				   integer rx_asp_idx)
runs on TCAP_CT
{
	f_asp_tx_tcap(tcap_msg, tx_asp_idx);
	as_asp_rx_tcap(tcap_msg, tx_asp_idx, rx_asp_idx);
}

private function f_asp_tx_tcap_exp_any(template (value) TCMessage tcap_msg,
				       integer tx_asp_idx)
runs on TCAP_CT
{
	f_asp_tx_tcap(tcap_msg, tx_asp_idx);
	as_asp_rx_tcap_any(tcap_msg, tx_asp_idx);
}

private function f_asp_tx_tcap_m3ua_ipa_transaction(integer o_asp_idx,
						integer t_asp_idx,
						OCT4 o_tid,
						OCT4 t_tid)
runs on TCAP_CT
{
	var template (value) TCMessage tcap_msg;

	/* TCAP Being: O -> T */
	tcap_msg := ts_TCAP_Begin(o_tid);
	f_asp_tx_tcap_exp(tcap_msg, o_asp_idx, t_asp_idx);

	/* TCAP Continue: O <- T */
	tcap_msg := ts_TCAP_Continue(t_tid, o_tid);
	f_asp_tx_tcap_exp_any(tcap_msg, t_asp_idx);

	/* TCAP Continue: O -> T */
	tcap_msg := ts_TCAP_Continue(o_tid, t_tid);
	f_asp_tx_tcap_exp(tcap_msg, o_asp_idx, t_asp_idx);

	/* TCAP End O <- T */
	tcap_msg := ts_TCAP_End(o_tid);
	f_asp_tx_tcap_exp_any(tcap_msg, t_asp_idx);
}

private function f_tcap_loadshare_register(integer node_a, integer tid_a_start, integer tid_a_stop,
					   integer node_b, integer tid_b_start, integer tid_b_stop,
					   boolean exp_ack := true, integer seq_nr := 1)
runs on TCAP_CT
{
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;

	/* Node a */
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := seq_nr,
							 tid_start := tid_a_start,
							 tid_end := tid_a_stop,
							 pc := IPA_EXT_TCAP_ROUTING_PC_WILDCARD,
							 ssn := IPA_EXT_TCAP_ROUTING_SSN_WILDCARD);
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, node_a);

	/* Node b */
	tcap_rt_msg.u.add_range.tid_start := tid_b_start;
	tcap_rt_msg.u.add_range.tid_end := tid_b_stop;
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, node_b, exp_ack := exp_ack);
}

/* test routing TCAP traffic from IPA AS to IPA AS */
testcase TC_tcap_loadshare_ipa_to_ipa() runs on TCAP_CT {
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-ipa-loadshare-1-0",
						      "asp-ipa-loadshare-1-1",
						      "asp-ipa-loadshare-2-0",
						      "asp-ipa-loadshare-2-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);

	/* Configure TCAP routing on ASP "asp-ipa-loadshare-1-0": */
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := 1,
							  tid_start := 0,
							  tid_end := 99,
							  pc := IPA_EXT_TCAP_ROUTING_PC_WILDCARD,
							  ssn := IPA_EXT_TCAP_ROUTING_SSN_WILDCARD)
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 0);
	/* Configure TCAP routing on ASP "asp-ipa-loadshare-2-0": */
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 2);

	/* Configure TCAP routing on ASP "asp-ipa-loadshare-1-1": */
	tcap_rt_msg.u.add_range.tid_start := 100;
	tcap_rt_msg.u.add_range.tid_end := 199;
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 1);
	/* Configure TCAP routing on ASP "asp-ipa-loadshare-2-1": */
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 3);

	f_asp_tx_tcap_m3ua_ipa_transaction(0, 3, int2oct(177, 4), int2oct(78, 4));

	setverdict(pass);
}

/* test routing TCAP traffic from IPA AS to M3UA AS */
testcase TC_tcap_loadshare_m3ua_to_ipa() runs on TCAP_CT {
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);

	/* Configure TCAP routing on ASP "asp-ipa-loadshare-0-0": */
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := 0,
							 tid_start := 0,
							 tid_end := 99,
							 pc := tcap_configs[2].cfg.own_pc,
							 ssn := tcap_configs[2].cfg.own_ssn);
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 2);

	/* Configure TCAP routing on ASP "asp-ipa-loadshare-0-1": */
	tcap_rt_msg.u.add_range.tid_start := 100;
	tcap_rt_msg.u.add_range.tid_end := 199;
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 3);

	f_asp_tx_tcap_m3ua_ipa_transaction(0, 2, int2oct(77, 4), int2oct(42, 4));

	setverdict(pass);
}



/* Test m3ua routing towards IPA/TCAP and register for wildcards ssn/pc */
testcase TC_tcap_loadshare_m3ua_to_ipa_wildcard() runs on TCAP_CT {
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);

	/* Configure TCAP routing on IPA ASPs "asp-ipa-loadshare-0-0/1" */
	f_tcap_loadshare_register(2, 0, 99, 3, 100, 199);
	f_sleep(1.0);

	f_asp_tx_tcap_m3ua_ipa_transaction(0, 2, int2oct(77, 4), int2oct(75, 4));

	setverdict(pass);
}

/* test routing TCAP traffic - do 100 sessions towards the same ipa/tcap node */
testcase TC_tcap_loadshare_m3ua_to_ipa_50(integer loops := 50) runs on TCAP_CT {
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);

	/* Configure TCAP routing on IPA ASPs "asp-ipa-loadshare-0-0/1" */
	f_tcap_loadshare_register(2, 0, 299, 3, 300, 599);

	var integer rand_tid := f_rnd_int(298);
	for (var integer i := 0; i < loops; i := i + 1) {
		var integer otid := 1 + i;
		var integer dtid := 1 + ((rand_tid + i) mod 298);
		f_asp_tx_tcap_m3ua_ipa_transaction(0, 2, int2oct(otid, 4), int2oct(dtid, 4));
	}

	setverdict(pass);
}

/* test routing TCAP overlapping ranges */
private function f_tcap_loadshare_ipa_tcap_range_fail_overlap(integer tid_a_start, integer tid_a_stop,
					       integer tid_b_start, integer tid_b_stop) runs on TCAP_CT
{
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);

	/* Configure TCAP routing on IPA ASPs "asp-ipa-loadshare-0-0/1" */
	f_tcap_loadshare_register(2, tid_a_start, tid_a_stop, 3, tid_b_start, tid_b_stop, exp_ack := false);
	setverdict(pass);
}

testcase TC_tcap_loadshare_ipa_tcap_range_fail_overlap_same() runs on TCAP_CT
{
	f_tcap_loadshare_ipa_tcap_range_fail_overlap(0, 99, 0, 99);
}

testcase TC_tcap_loadshare_ipa_tcap_range_fail_overlap_last() runs on TCAP_CT
{
	f_tcap_loadshare_ipa_tcap_range_fail_overlap(0, 99, 99, 199);
}

testcase TC_tcap_loadshare_ipa_tcap_range_fail_overlap_within() runs on TCAP_CT
{
	f_tcap_loadshare_ipa_tcap_range_fail_overlap(0, 99, 60, 80);
}

testcase TC_tcap_loadshare_ipa_tcap_range_fail_overlap_switch() runs on TCAP_CT
{
	f_tcap_loadshare_ipa_tcap_range_fail_overlap(99, 199, 0, 99);
}

private function f_tcap_loadshare_ipa_tcap_range_success_pc(TCAP_CT_Configurations tcap_configs)
runs on TCAP_CT
{
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := 1,
							 tid_start := 0,
							 tid_end := 99,
							 pc := IPA_EXT_TCAP_ROUTING_PC_WILDCARD,
							 ssn := IPA_EXT_TCAP_ROUTING_SSN_WILDCARD);
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 2);

	tcap_rt_msg.u.add_range.tid_start := 60;
	tcap_rt_msg.u.add_range.tid_end := 80;
	tcap_rt_msg.u.add_range.pc := tcap_configs[2].cfg.own_pc;
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 3);
}

/* Test overlapping tid ranges, but with a more specific PC, within the same AS
 *
 * node a: 0..99
 * node b: 60..80/pc (own)
 */
testcase TC_tcap_loadshare_ipa_tcap_range_success_pc() runs on TCAP_CT {
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);
	f_tcap_loadshare_ipa_tcap_range_success_pc(tcap_configs);
	f_asp_tx_tcap_m3ua_ipa_transaction(0, 2, int2oct(23, 4), int2oct(98, 4));
	f_asp_tx_tcap_m3ua_ipa_transaction(0, 3, int2oct(60, 4), int2oct(79, 4));
	/* TODO: check traffic routing with the correct PC, but different SSN, otid := 60 */

	setverdict(pass);
}

/* Test overlapping tid ranges, but with a more specific PC and SSN, within the same AS
 *
 * node a: 0..99
 * node b: 60..80/pc (own)
 * node b: 60..80/pc; 60..80/pc/ssn (own)
 */
testcase TC_tcap_loadshare_ipa_tcap_range_success_pc_ssn() runs on TCAP_CT {
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);
	f_init_tcap(tcap_configs);

	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;

	f_tcap_loadshare_ipa_tcap_range_success_pc(tcap_configs);
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := 2,
							 tid_start := 60,
							 tid_end := 80,
							 pc := tcap_configs[2].cfg.own_pc,
							 ssn := tcap_configs[2].cfg.own_ssn);
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 3);
	f_asp_tx_tcap_m3ua_ipa_transaction(0, 3, int2oct(60, 4), int2oct(70, 4));

	setverdict(pass);
}

/* Test overlapping tid ranges, but with a more specific PC and SSN, within the same AS
 *
 * node a: 0..99
 * node b: 60..80/pc (own)
 * node b: 60..80/pc; 60..80/ssn (own)
 */
testcase TC_tcap_loadshare_ipa_tcap_range_success_pc_ssn2() runs on TCAP_CT {
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;

	f_init_tcap(tcap_configs);
	f_tcap_loadshare_ipa_tcap_range_success_pc(tcap_configs);
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := 2,
							 tid_start := 60,
							 tid_end := 80,
							 pc := IPA_EXT_TCAP_ROUTING_PC_WILDCARD,
							 ssn := tcap_configs[2].cfg.own_ssn);
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 3);
	f_asp_tx_tcap_m3ua_ipa_transaction(0, 3, int2oct(60, 4), int2oct(99, 4));

	setverdict(pass);
}

/* Test overlapping tid ranges, but with a more specific PC and SSN, within the same AS
 *
 * node a: 0..99
 * node b: 60..80/pc (own)
 * node b: 60..80/ssn (own)
 * node b: 65..70/ssn (own) (fails)
 */
testcase TC_tcap_loadshare_ipa_tcap_range_fail_pc_ssn_overlap() runs on TCAP_CT {
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);
	f_tcap_loadshare_ipa_tcap_range_success_pc(tcap_configs);
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := 2,
							 tid_start := 60,
							 tid_end := 80,
							 pc := IPA_EXT_TCAP_ROUTING_PC_WILDCARD,
							 ssn := tcap_configs[2].cfg.own_ssn);
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 3);
	tcap_rt_msg := ts_IPA_EXT_TCAP_ROUTING_ADD_RANGE(seq_nr := 3,
							 tid_start := 65,
							 tid_end := 70,
							 pc := IPA_EXT_TCAP_ROUTING_PC_WILDCARD,
							 ssn := tcap_configs[2].cfg.own_ssn);
	f_asp_tx_ipa_ext_tcap_routing(tcap_rt_msg, 3, exp_ack := false);
	setverdict(pass);
}

/* Simulate a Insert Subscriber Data from IPA towards M3UA */
// FIXME: rename it to allow IPA -> M3UA traffic
private function f_asp_tx_tcap_ipa_m3ua_gt_isd_transaction(
		integer o_asp_idx,
		integer t_asp_idx,
		OCT4 o_tid,
		OCT4 t_tid)
runs on TCAP_CT
{
	var template (value) TCMessage tcap_msg;

	/* TCAP Being: O -> T */
	tcap_msg := ts_TCAP_Begin(o_tid);
	f_asp_tx_tcap_exp_any(tcap_msg, o_asp_idx);

	/* TCAP Continue: O <- T */
	tcap_msg := ts_TCAP_Continue(t_tid, o_tid);
	f_asp_tx_tcap_exp(tcap_msg, o_asp_idx, t_asp_idx);

	/* TCAP Continue: O -> T */
	tcap_msg := ts_TCAP_Continue(o_tid, t_tid);
	f_asp_tx_tcap_exp_any(tcap_msg, o_asp_idx);

	/* TCAP End O <- T */
	tcap_msg := ts_TCAP_End(o_tid);
	f_asp_tx_tcap_exp(tcap_msg, o_asp_idx, t_asp_idx);
}

/* Test m3ua -> ipa/tcap doing a ISD with SCCP GT */
testcase TC_tcap_loadshare_m3ua_to_ip_gt_isd() runs on TCAP_CT {
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	/* FIXME: create m3ua and ipa endpoints which contain GTs, using the same endpoints
	 *        as for 0-0.
	 */
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-1-0",
						      "asp-m3ua-loadshare-1-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);

	f_init_tcap(tcap_configs);

	/* Configure TCAP routing on IPA ASPs "asp-ipa-loadshare-0-0/1" */
	f_tcap_loadshare_register(2, 0, 99, 3, 100, 199);
	f_sleep(1.0);

	f_asp_tx_tcap_ipa_m3ua_gt_isd_transaction(0, 2, int2oct(77, 4), int2oct(75, 4));
	setverdict(pass);
}

/* Test if UTDS is sent back when sending a TCAP messages with a OTID not valid
 *
 * node a: 0..99
 * node b: 100..199
 */
testcase TC_tcap_loadshare_ipa_tcap_utds() runs on TCAP_CT {
	var template (value) IPA_EXT_TCAP_ROUTING_Message tcap_rt_msg;
	var Misc_Helpers.ro_charstring tcap_asps := { "asp-m3ua-loadshare-0-0",
						      "asp-m3ua-loadshare-0-1",
						      "asp-ipa-loadshare-0-0",
						      "asp-ipa-loadshare-0-1" };
	var TCAP_CT_Configurations tcap_configs := tcap_build_configs(tcap_asps);
	var template (value) TCMessage tcap_msg;
	timer T := 5.0;

	f_init_tcap(tcap_configs);
	/* Configure TCAP routing on IPA ASPs "asp-ipa-loadshare-0-0/1" */
	f_tcap_loadshare_register(2, 0, 99, 3, 100, 199);


	/* send a TCAP message with oTID 250 (no range available) */

	/* TCAP Being: O -> T */
	tcap_msg := ts_TCAP_Begin(int2oct(250, 4));
	f_asp_tx_tcap(tcap_msg, 0);

	var template (present) TCAP_N_NOTICE_ind exp_sccp_notice_ind :=
		tr_TCAP_N_NOTICE_ind(g_tcap[0].sccp_addr_own,
				     g_tcap[0].sccp_addr_peer,
				     *,
				     tcap_msg);
	T.start;
	alt {
	[] any from SCCP_TCAP.receive(exp_sccp_notice_ind) {
		setverdict(pass);
		}
	[] T.timeout {
		setverdict(fail, __SCOPE__, "(): Timeout waiting for UTDS");
		Misc_Helpers.f_shutdown(__BFILE__, __LINE__);
		}
	}

	setverdict(pass);
}

/* TODO: test TCAP Abort message is used.
 * TODO: test TCAP Begin+End message is used.
 * TODO: test TCAP GlobalTitles ISD
 * TODO: test TCAP GlobalTitles ULA
 */

control {
	execute( TC_tcap_loadshare_ipa_to_ipa() );
	execute( TC_tcap_loadshare_m3ua_to_ipa() );
	execute( TC_tcap_loadshare_m3ua_to_ipa_50() );
	execute( TC_tcap_loadshare_m3ua_to_ipa_wildcard() );
	execute( TC_tcap_loadshare_ipa_tcap_range_fail_overlap_same() );
	execute( TC_tcap_loadshare_ipa_tcap_range_fail_overlap_last() );
	execute( TC_tcap_loadshare_ipa_tcap_range_fail_overlap_within() );
	execute( TC_tcap_loadshare_ipa_tcap_range_fail_overlap_switch() );
	execute( TC_tcap_loadshare_ipa_tcap_range_success_pc() );
	execute( TC_tcap_loadshare_ipa_tcap_range_success_pc_ssn() );
	execute( TC_tcap_loadshare_ipa_tcap_range_success_pc_ssn2() );
	execute( TC_tcap_loadshare_ipa_tcap_range_fail_pc_ssn_overlap() );
	execute( TC_tcap_loadshare_ipa_tcap_utds() );
}



}
