/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               RxInterface_PCC_3GPP_TS29214_830.ddf
//  Description:        DDF for Rx according to 3GPP TS 29.214 V8.10.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: RX
// APPLICATION-REVISION: V8_A_0

// AVP implementations according to: 
// 3GPP TS 29.214 V8.10.0 - Policy and Charging Control over Rx reference point
//
//
// Dependant applications
// 3GPP TS 29.229  - Cx and Dx interfaces based on the Diameter protocol
// TS 183.017      - DIAMETER protocol for session based policy set-up information exchange between
//                   the Application Function (AF) and the Service Policy Decision Function (SPDF)
// IETF RFC 3588   - Diameter Base Protocol
// IETF RFC 4005   - Diameter Network Address Server
// IETF RFC 4006   - Diameter Credit Control Application
//
// Notes: 
// Present application has its own vendor specific Diameter application id: 16777236
//
// Type of enumerated AVP Media-Type is changed to AVP_Unsigned32 to
// give the ability to contain OTHER (0xFFFFFFFF) value
//

// 3GPP TS 29.214 V8.10.0 5.6
type enumerated Command_Code
{
  Authorize_Authenticate (265),
  Re_Auth                (258),
  Session_Termination    (275),
  Abort_Session          (274)
}



// 3GPP TS 29.214 V8.10.0
// AVP: Abort-Cause (500) 3GPP (10415)
// 5.3.1
type enumerated Abort_Cause
{
  BEARER_RELEASED               (0),
  INSUFFICIENT_SERVER_RESOURCES (1),
  INSUFFICIENT_BEARER_RESOURCES (2)
}


// 3GPP TS 29.214 V8.10.0
// AVP: Access-Network-Charging-Address (501) 3GPP (10415)
// 5.3.2
type AVP_Address Access_Network_Charging_Address;


// 3GPP TS 29.214 V8.10.0
// AVP: Access-Network-Charging-Identifier (502) 3GPP (10415)
// 5.3.3
type AVP_Grouped Access_Network_Charging_Identifier;


// 3GPP TS 29.214 V8.10.0
// AVP: Access-Network-Charging-Identifier-Value (503) 3GPP (10415)
// 5.3.4
type AVP_OctetString Access_Network_Charging_Identifier_Value;


// 3GPP TS 29.214 V8.10.0
// AVP: Acceptable-Service-Info (526) 3GPP (10415)
// 5.3.24
type AVP_Grouped Acceptable_Service_Info;


// 3GPP TS 29.214 V8.10.0
// AVP: AF-Application-Identifier (504) 3GPP (10415)
// 5.3.5
type AVP_OctetString AF_Application_Identifier;


// 3GPP TS 29.214 V8.10.0
// AVP: AF-Charging-Identifier (505) 3GPP (10415)
// 5.3.6
type AVP_OctetString AF_Charging_Identifier;


// 3GPP TS 29.214 V8.10.0
// AVP: Codec-Data  (524) 3GPP (10415)
// 5.3.7
type AVP_OctetString Codec_Data;


// 3GPP TS 29.214 V8.10.0
// AVP: Flow-Description (507) 3GPP (10415)
// 5.3.8
type AVP_IPFilterRule Flow_Description;


// 3GPP TS 29.214 V8.10.0
// AVP: Flow-Number (509) 3GPP (10415)
// 5.3.9
type AVP_Unsigned32 Flow_Number;


// 3GPP TS 29.214 V8.10.0
// AVP: Flows (510) 3GPP (10415)
// 5.3.10
type AVP_Grouped Flows;


// 3GPP TS 29.214 V8.10.0
// AVP: Flow-Status (511) 3GPP (10415)
// 5.3.11
type enumerated Flow_Status
{
  ENABLED_UPLINK      (0),
  ENABLED_DOWNLINK    (1),
  ENABLED             (2),
  DISABLED            (3),
  REMOVED             (4)
}


// 3GPP TS 29.214 V8.10.0
// AVP: Flow-Usage (512) 3GPP (10415)
// 5.3.12
type enumerated Flow_Usage
{
  NO_INFORMATION      (0),
  RTCP                (1),
  AF_SIGNALLING       (2)
}

// 3GPP TS 29.214 V8.10.0
// AVP:  Service-URN (525) 3GPP (10415)
// 5.3.23
type AVP_OctetString Service_URN;


// 3GPP TS 29.214 V8.10.0
// AVP: Specific-Action (513) 3GPP (10415)
// 5.3.13
type enumerated Specific_Action
{
  CHARGING_CORRELATION_EXCHANGE         (1),
  INDICATION_OF_LOSS_OF_BEARER          (2),
  INDICATION_OF_RECOVERY_OF_BEARER      (3),
  INDICATION_OF_RELEASE_OF_BEARER       (4),
  INDICATION_OF_ESTABLISHMENT_OF_BEARER (5),
  IP_CAN_CHANGE                         (6),
  INDICATION_OF_OUT_OF_CREDIT           (7),
  INDICATION_OF_SUCCESSFUL_RESOURCES_ALLOCATION (8),
  INDICATION_OF_FAILED_RESOURCES_ALLOCATION (9),
  INDICATION_OF_LIMITED_PCC_DEPLOYMENT (10)
}


// 3GPP TS 29.214 V8.10.0
// AVP: Max-Requested-Bandwidth-DL (515) 3GPP (10415)
// 5.3.14
type AVP_Unsigned32 Max_Requested_Bandwidth_DL;


// 3GPP TS 29.214 V8.10.0
// AVP: Max-Requested-Bandwidth-UL (516) 3GPP (10415)
// 5.3.15
type AVP_Unsigned32 Max_Requested_Bandwidth_UL;


// 3GPP TS 29.214 V8.10.0
// AVP: Media-Component-Description (517) 3GPP (10415)
// 5.3.16
type AVP_Grouped Media_Component_Description;


// 3GPP TS 29.214 V8.10.0
// AVP: Media-Component-Number (518) 3GPP (10415)
// 5.3.17
type AVP_Unsigned32 Media_Component_Number;


// 3GPP TS 29.214 V8.10.0
// AVP: Media-Sub-Component (519) 3GPP (10415)
// 5.3.18
type AVP_Grouped Media_Sub_Component;


// 3GPP TS 29.214 V8.10.0
// AVP: Media-Type (520) 3GPP (10415)
// 5.3.19
type AVP_Unsigned32 Media_Type;


// 3GPP TS 29.214 V8.10.0
// AVP: RR-Bandwidth (521) 3GPP (10415)
// 5.3.20
type AVP_Unsigned32 RR_Bandwidth;


// 3GPP TS 29.214 V8.10.0
// AVP: RS-Bandwidth (522) 3GPP (10415)
// 5.3.21
type AVP_Unsigned32 RS_Bandwidth;


// 3GPP TS 29.214 V8.10.0
// AVP: Service-Info-Status (527) 3GPP (10415)
// 5.3.25
type enumerated Service_Info_Status 
{
  FINAL_SERVICE_INFORMATION       (0),	
  PRELIMINARY_SERVICE_INFORMATION (1)
}


// 3GPP TS 29.214 V8.10.0
// AVP: SIP-Forking-Indication (523) 3GPP (10415)
// 5.3.22
type enumerated SIP_Forking_Indication
{
   SINGLE_DIALOGUE   (0),
   SEVERAL_DIALOGUES (1) 
}
