libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Structures | Macros | Enumerations | Functions | Variables
gsm_12_21.h File Reference
A-bis OML
`#include <stdint.h>`
`#include <stdbool.h>`
`#include <osmocom/gsm/tlv.h>`

Go to the source code of this file.

## Data Structures
struct | abis_om_hdr
| generic header in front of every OML message according to TS 08.59 More...
struct | abis_om_obj_inst
| OML Object Instance. More...
struct | abis_om_fom_hdr
| OML FOM header. More...
struct | abis_nm_channel
| Abis OML Channel (Section 9.4.1) More...
struct | abis_nm_ipacc_att_ns_cfg
| ip.access NM_ATT_IPACC_NS_CFG value More...
struct | abis_nm_ipacc_att_bssgp_cfg
| ip.access NM_ATT_IPACC_BSSGP_CFG value More...
struct | abis_nm_ipacc_att_rlc_cfg
| ip.access NM_ATT_IPACC_RLC_CFG value More...
struct | abis_nm_ipacc_att_rlc_cfg_2
| ip.access NM_ATT_IPACC_RLC_CFG_2 value More...
struct | abis_nm_ipacc_att_rlc_cfg_3
| ip.access NM_ATT_IPACC_RLC_CFG_3 value More...
struct | abis_nm_sw_desc
| 3GPP TS 52.021 §9.4.62 SW Description More...

## Macros
#define | ABIS_NM_MSG_SIZE 1024
#define | ABIS_NM_MSG_HEADROOM 128
#define | ABIS_OM_MDISC_FOM 0x80
| Message Discriminator for Formatted Object Messages. More...
#define | ABIS_OM_MDISC_MMI 0x40
| Message Discriminator for Man Machine Interface. More...
#define | ABIS_OM_MDISC_TRAU 0x20
| Message Discriminator for TRAU management. More...
#define | ABIS_OM_MDISC_MANUF 0x10
| Message Discriminator for Manufacturer Specific Messages. More...
#define | ABIS_OM_PLACEMENT_ONLY 0x80
| Entire OML message is in the L2 frame. More...
#define | ABIS_OM_PLACEMENT_FIRST 0x40
| First fragment of OML message is in this L2 frame. More...
#define | ABIS_OM_PLACEMENT_MIDDLE 0x20
| Middle fragment of OML message is in this L2 frame. More...
#define | ABIS_OM_PLACEMENT_LAST 0x10
| Last fragment of OML message is in this L2 frame. More...
#define | ABIS_OM_FOM_HDR_SIZE (sizeof(struct abis_om_hdr) + sizeof(struct abis_om_fom_hdr))
| Size of the OML FOM header in octets. More...
#define | NM_ATT_BS11_FILE_DATA NM_ATT_EVENT_TYPE
#define | NM_CHANC_OSMO_TCHFull_TCHHalf_PDCH NM_CHANC_OSMO_DYN
#define | NM_IPAC_F_FREQ_BAND_PGSM (1 << 0)
| ip.access support flags for NM_IPAC_EIE_FREQ_BANDS More...
#define | NM_IPAC_F_FREQ_BAND_EGSM (1 << 1)
#define | NM_IPAC_F_FREQ_BAND_RGSM (1 << 2)
#define | NM_IPAC_F_FREQ_BAND_DCS (1 << 3)
#define | NM_IPAC_F_FREQ_BAND_PCS (1 << 4)
#define | NM_IPAC_F_FREQ_BAND_850 (1 << 5)
#define | NM_IPAC_F_FREQ_BAND_480 (1 << 6)
#define | NM_IPAC_F_FREQ_BAND_450 (1 << 7)
#define | NM_IPAC_F_CIPH_ALGO_A51 (1 << 0)
| ip.access support flags for NM_IPAC_EIE_CIPH_ALGOS More...
#define | NM_IPAC_F_CIPH_ALGO_A52 (1 << 1)
#define | NM_IPAC_F_CIPH_ALGO_A53 (1 << 2)
#define | NM_IPAC_F_CIPH_ALGO_A54 (1 << 3)
#define | NM_IPAC_F_CIPH_ALGO_A55 (1 << 4)
#define | NM_IPAC_F_CIPH_ALGO_A56 (1 << 5)
#define | NM_IPAC_F_CIPH_ALGO_A57 (1 << 6)
#define | NM_IPAC_F_CIPH_ALGO_A58 (1 << 7)
#define | NM_IPAC_F_CHANT_TCHF (1 << 0)
| ip.access support flags for NM_IPAC_EIE_CHAN_TYPES (1st octet) More...
#define | NM_IPAC_F_CHANT_TCHH (1 << 1)
#define | NM_IPAC_F_CHANT_SDCCH8 (1 << 2)
#define | NM_IPAC_F_CHANT_BCCH (1 << 3)
#define | NM_IPAC_F_CHANT_BCCH_SDCCH4 (1 << 4)
#define | NM_IPAC_F_CHANT_BCH (1 << 5)
#define | NM_IPAC_F_CHANT_BCCH_SDCCH4_CBCH (1 << 6)
#define | NM_IPAC_F_CHANT_SDCCH8_CBCH (1 << 7)
#define | NM_IPAC_F_CHANT_PDCHF (1 << 8)
| ip.access support flags for NM_IPAC_EIE_CHAN_TYPES (2nd octet) More...
#define | NM_IPAC_F_CHANT_TCHF_PDCHF (1 << 9)
#define | NM_IPAC_F_CHANT_TCHH_PDCHH (1 << 10)
#define | NM_IPAC_F_CHANT_TCHF_TCHH (1 << 11)
#define | NM_IPAC_F_CHANM_SPEECH_FS (1 << 0)
| ip.access support flags for NM_IPAC_EIE_CHAN_MODES (speech codecs) More...
#define | NM_IPAC_F_CHANM_SPEECH_EFS (1 << 1)
#define | NM_IPAC_F_CHANM_SPEECH_AFS (1 << 2)
#define | NM_IPAC_F_CHANM_SPEECH_HS (1 << 3)
#define | NM_IPAC_F_CHANM_SPEECH_AHS (1 << 4)
#define | NM_IPAC_F_CHANM_CSD_NT_4k8 (1 << 8)
| ip.access support flags for NM_IPAC_EIE_CHAN_MODES (CSD non-transparent) More...
#define | NM_IPAC_F_CHANM_CSD_NT_9k6 (1 << 9)
#define | NM_IPAC_F_CHANM_CSD_NT_14k4 (1 << 10)
#define | NM_IPAC_F_CHANM_CSD_T_1200_75 (1 << 16)
| ip.access support flags for NM_IPAC_EIE_CHAN_MODES (CSD transparent) More...
#define | NM_IPAC_F_CHANM_CSD_T_600 (1 << 17)
#define | NM_IPAC_F_CHANM_CSD_T_1k2 (1 << 18)
#define | NM_IPAC_F_CHANM_CSD_T_2k4 (1 << 19)
#define | NM_IPAC_F_CHANM_CSD_T_4k8 (1 << 20)
#define | NM_IPAC_F_CHANM_CSD_T_9k6 (1 << 21)
#define | NM_IPAC_F_CHANM_CSD_T_14k4 (1 << 22)
#define | NM_IPAC_F_GPRS_CODING_CS1 (1 << 0)
| ip.access support flags for NM_IPAC_EIE_GPRS_CODING (GPRS) More...
#define | NM_IPAC_F_GPRS_CODING_CS2 (1 << 1)
#define | NM_IPAC_F_GPRS_CODING_CS3 (1 << 2)
#define | NM_IPAC_F_GPRS_CODING_CS4 (1 << 3)
#define | NM_IPAC_F_GPRS_CODING_MCS1 (1 << 8)
| ip.access support flags for NM_IPAC_EIE_GPRS_CODING (EGPRS) More...
#define | NM_IPAC_F_GPRS_CODING_MCS2 (1 << 9)
#define | NM_IPAC_F_GPRS_CODING_MCS3 (1 << 10)
#define | NM_IPAC_F_GPRS_CODING_MCS4 (1 << 11)
#define | NM_IPAC_F_GPRS_CODING_MCS5 (1 << 12)
#define | NM_IPAC_F_GPRS_CODING_MCS6 (1 << 13)
#define | NM_IPAC_F_GPRS_CODING_MCS7 (1 << 14)
#define | NM_IPAC_F_GPRS_CODING_MCS8 (1 << 15)
#define | NM_IPAC_F_GPRS_CODING_MCS9 (1 << 7)
#define | NM_IPAC_F_RTP_FEAT_COMPR_CONTROL (1 << 0) /* RTP Compression Control */
| ip.access support flags for NM_IPAC_EIE_RTP_FEATURES More...
#define | NM_IPAC_F_RTP_FEAT_IR_8k (1 << 1) /* IR 8 kbit/s */
#define | NM_IPAC_F_RTP_FEAT_IR_16k (1 << 2) /* IR 16 kbit/s */
#define | NM_IPAC_F_RTP_FEAT_IR_32k (1 << 3) /* IR 32 kbit/s */
#define | NM_IPAC_F_RTP_FEAT_IR_64k (1 << 4) /* IR 64 kbit/s */
#define | NM_IPAC_F_RTP_FEAT_MULTIPLEX_RTP (1 << 6) /* RTP Multiplexing */
#define | NM_IPAC_F_RTP_FEAT_MULTIPLEX_SRTP (1 << 7) /* SRTP Multiplexing */
#define | NM_IPAC_F_RSL_FEAT_PHYSICAL_CONTEXT (1 << 0)
| ip.access support flags for NM_IPAC_EIE_RSL_FEATURES More...
#define | NM_IPAC_F_RSL_FEAT_DYN_PDCH_ACT (1 << 1)
#define | NM_IPAC_F_RSL_FEAT_RTP_PT2 (1 << 2)

## Enumerations
enum | abis_nm_msgtype { NM_MT_LOAD_INIT = 0x01 , NM_MT_LOAD_INIT_ACK , NM_MT_LOAD_INIT_NACK , NM_MT_LOAD_SEG , NM_MT_LOAD_SEG_ACK , NM_MT_LOAD_ABORT , NM_MT_LOAD_END , NM_MT_LOAD_END_ACK , NM_MT_LOAD_END_NACK , NM_MT_SW_ACT_REQ , NM_MT_SW_ACT_REQ_ACK , NM_MT_SW_ACT_REQ_NACK , NM_MT_ACTIVATE_SW , NM_MT_ACTIVATE_SW_ACK , NM_MT_ACTIVATE_SW_NACK , NM_MT_SW_ACTIVATED_REP , NM_MT_ESTABLISH_TEI = 0x21 , NM_MT_ESTABLISH_TEI_ACK , NM_MT_ESTABLISH_TEI_NACK , NM_MT_CONN_TERR_SIGN , NM_MT_CONN_TERR_SIGN_ACK , NM_MT_CONN_TERR_SIGN_NACK , NM_MT_DISC_TERR_SIGN , NM_MT_DISC_TERR_SIGN_ACK , NM_MT_DISC_TERR_SIGN_NACK , NM_MT_CONN_TERR_TRAF , NM_MT_CONN_TERR_TRAF_ACK , NM_MT_CONN_TERR_TRAF_NACK , NM_MT_DISC_TERR_TRAF , NM_MT_DISC_TERR_TRAF_ACK , NM_MT_DISC_TERR_TRAF_NACK , NM_MT_CONN_MDROP_LINK = 0x31 , NM_MT_CONN_MDROP_LINK_ACK , NM_MT_CONN_MDROP_LINK_NACK , NM_MT_DISC_MDROP_LINK , NM_MT_DISC_MDROP_LINK_ACK , NM_MT_DISC_MDROP_LINK_NACK , NM_MT_SET_BTS_ATTR = 0x41 , NM_MT_SET_BTS_ATTR_ACK , NM_MT_SET_BTS_ATTR_NACK , NM_MT_SET_RADIO_ATTR , NM_MT_SET_RADIO_ATTR_ACK , NM_MT_SET_RADIO_ATTR_NACK , NM_MT_SET_CHAN_ATTR , NM_MT_SET_CHAN_ATTR_ACK , NM_MT_SET_CHAN_ATTR_NACK , NM_MT_PERF_TEST = 0x51 , NM_MT_PERF_TEST_ACK , NM_MT_PERF_TEST_NACK , NM_MT_TEST_REP , NM_MT_SEND_TEST_REP , NM_MT_SEND_TEST_REP_ACK , NM_MT_SEND_TEST_REP_NACK , NM_MT_STOP_TEST , NM_MT_STOP_TEST_ACK , NM_MT_STOP_TEST_NACK , NM_MT_STATECHG_EVENT_REP = 0x61 , NM_MT_FAILURE_EVENT_REP , NM_MT_STOP_EVENT_REP , NM_MT_STOP_EVENT_REP_ACK , NM_MT_STOP_EVENT_REP_NACK , NM_MT_REST_EVENT_REP , NM_MT_REST_EVENT_REP_ACK , NM_MT_REST_EVENT_REP_NACK , NM_MT_CHG_ADM_STATE , NM_MT_CHG_ADM_STATE_ACK , NM_MT_CHG_ADM_STATE_NACK , NM_MT_CHG_ADM_STATE_REQ , NM_MT_CHG_ADM_STATE_REQ_ACK , NM_MT_CHG_ADM_STATE_REQ_NACK , NM_MT_REP_OUTST_ALARMS = 0x93 , NM_MT_REP_OUTST_ALARMS_ACK , NM_MT_REP_OUTST_ALARMS_NACK , NM_MT_CHANGEOVER = 0x71 , NM_MT_CHANGEOVER_ACK , NM_MT_CHANGEOVER_NACK , NM_MT_OPSTART , NM_MT_OPSTART_ACK , NM_MT_OPSTART_NACK , NM_MT_REINIT , NM_MT_REINIT_ACK , NM_MT_REINIT_NACK , NM_MT_SET_SITE_OUT , NM_MT_SET_SITE_OUT_ACK , NM_MT_SET_SITE_OUT_NACK , NM_MT_CHG_HW_CONF = 0x90 , NM_MT_CHG_HW_CONF_ACK , NM_MT_CHG_HW_CONF_NACK , NM_MT_MEAS_RES_REQ = 0x8a , NM_MT_MEAS_RES_RESP , NM_MT_STOP_MEAS , NM_MT_START_MEAS , NM_MT_GET_ATTR = 0x81 , NM_MT_GET_ATTR_RESP , NM_MT_GET_ATTR_NACK , NM_MT_SET_ALARM_THRES , NM_MT_SET_ALARM_THRES_ACK , NM_MT_SET_ALARM_THRES_NACK }
| OML Message Type (Section 9.1) More...
enum | abis_nm_msgtype_bs11 { NM_MT_BS11_RESET_RESOURCE = 0x74 , NM_MT_BS11_BEGIN_DB_TX = 0xa3 , NM_MT_BS11_BEGIN_DB_TX_ACK , NM_MT_BS11_BEGIN_DB_TX_NACK , NM_MT_BS11_END_DB_TX = 0xa6 , NM_MT_BS11_END_DB_TX_ACK , NM_MT_BS11_END_DB_TX_NACK , NM_MT_BS11_CREATE_OBJ = 0xa9 , NM_MT_BS11_CREATE_OBJ_ACK , NM_MT_BS11_CREATE_OBJ_NACK , NM_MT_BS11_DELETE_OBJ = 0xac , NM_MT_BS11_DELETE_OBJ_ACK , NM_MT_BS11_DELETE_OBJ_NACK , NM_MT_BS11_SET_ATTR = 0xd0 , NM_MT_BS11_SET_ATTR_ACK , NM_MT_BS11_SET_ATTR_NACK , NM_MT_BS11_LMT_SESSION = 0xdc , NM_MT_BS11_GET_STATE = 0xe3 , NM_MT_BS11_GET_STATE_ACK , NM_MT_BS11_LMT_LOGON = 0xe5 , NM_MT_BS11_LMT_LOGON_ACK , NM_MT_BS11_RESTART = 0xe7 , NM_MT_BS11_RESTART_ACK , NM_MT_BS11_DISCONNECT = 0xe9 , NM_MT_BS11_DISCONNECT_ACK , NM_MT_BS11_LMT_LOGOFF = 0xec , NM_MT_BS11_LMT_LOGOFF_ACK , NM_MT_BS11_RECONNECT = 0xf1 , NM_MT_BS11_RECONNECT_ACK }
| Siemens specific OML Message Types. More...
enum | abis_nm_msgtype_ipacc { NM_MT_IPACC_RESTART = 0x87 , NM_MT_IPACC_RESTART_ACK , NM_MT_IPACC_RESTART_NACK , NM_MT_IPACC_RSL_CONNECT = 0xe0 , NM_MT_IPACC_RSL_CONNECT_ACK , NM_MT_IPACC_RSL_CONNECT_NACK , NM_MT_IPACC_RSL_DISCONNECT = 0xe3 , NM_MT_IPACC_RSL_DISCONNECT_ACK , NM_MT_IPACC_RSL_DISCONNECT_NACK , NM_MT_IPACC_CONN_TRAF = 0xe6 , NM_MT_IPACC_CONN_TRAF_ACK , NM_MT_IPACC_CONN_TRAF_NACK , NM_MT_IPACC_DEF_BOOT_SW = 0xec , NM_MT_IPACC_DEF_BOOT_SW_ACK , MN_MT_IPACC_DEF_BOOT_SW_NACK , NM_MT_IPACC_SET_NVATTR = 0xef , NM_MT_IPACC_SET_NVATTR_ACK , NM_MT_IPACC_SET_NVATTR_NACK , NM_MT_IPACC_GET_NVATTR = 0xf2 , NM_MT_IPACC_GET_NVATTR_ACK , NM_MT_IPACC_GET_NVATTR_NACK , NM_MT_IPACC_SET_ATTR = 0xf5 , NM_MT_IPACC_SET_ATTR_ACK , NM_MT_IPACC_SET_ATTR_NACK }
| ip.access specific OML Message Types More...
enum | abis_mm_event_causes { OSMO_EVT_CRIT_SW_FATAL = 0x0000 , OSMO_EVT_CRIT_PROC_STOP = 0x0002 , OSMO_EVT_CRIT_RTP_TOUT = 0x032c , OSMO_EVT_CRIT_BOOT_FAIL = 0x0401 , OSMO_EVT_MAJ_UKWN_MSG = 0x0002 , OSMO_EVT_MAJ_RSL_FAIL = 0x0309 , OSMO_EVT_MAJ_UNSUP_ATTR = 0x0318 , OSMO_EVT_MAJ_NET_CONGEST = 0x032b , OSMO_EVT_MIN_PAG_TAB_FULL = 0x0401 , OSMO_EVT_WARN_SW_WARN = 0x0001 , OSMO_EVT_EXT_ALARM = 0xfeed , OSMO_EVT_PCU_VERS = 0xface }
| OML Probable Cause (Section 9.4.43) Manufacturer specific values. More...
enum | abis_nm_bs11_cell_alloc { NM_BS11_CANR_GSM = 0x00 , NM_BS11_CANR_DCS1800 = 0x01 }
enum | abis_nm_obj_class { NM_OC_SITE_MANAGER = 0x00 , NM_OC_BTS , NM_OC_RADIO_CARRIER , NM_OC_CHANNEL , NM_OC_BASEB_TRANSC , NM_OC_IPAC_E1_TRUNK = 0x0e , NM_OC_IPAC_E1_PORT = 0x0f , NM_OC_IPAC_E1_CHAN = 0x10 , NM_OC_IPAC_CLK_MODULE = 0x22 , NM_OC_BS11_ADJC = 0xa0 , NM_OC_BS11_HANDOVER = 0xa1 , NM_OC_BS11_PWR_CTRL = 0xa2 , NM_OC_BS11_BTSE = 0xa3 , NM_OC_BS11_RACK = 0xa4 , NM_OC_BS11 = 0xa5 , NM_OC_BS11_TEST = 0xa6 , NM_OC_BS11_ENVABTSE = 0xa8 , NM_OC_BS11_BPORT = 0xa9 , NM_OC_GPRS_NSE = 0xf0 , NM_OC_GPRS_CELL = 0xf1 , NM_OC_GPRS_NSVC = 0xf2 , NM_OC_NULL = 0xff }
| OML Object Class (Section 9.2) More...
enum | abis_nm_attr { NM_ATT_ABIS_CHANNEL = 0x01 , NM_ATT_ADD_INFO , NM_ATT_ADD_TEXT , NM_ATT_ADM_STATE , NM_ATT_ARFCN_LIST , NM_ATT_AUTON_REPORT , NM_ATT_AVAIL_STATUS , NM_ATT_BCCH_ARFCN , NM_ATT_BSIC , NM_ATT_BTS_AIR_TIMER , NM_ATT_CCCH_L_I_P , NM_ATT_CCCH_L_T , NM_ATT_CHAN_COMB , NM_ATT_CONN_FAIL_CRIT , NM_ATT_DEST , NM_ATT_EVENT_TYPE = 0x11 , NM_ATT_FILE_ID , NM_ATT_FILE_VERSION , NM_ATT_GSM_TIME , NM_ATT_HSN , NM_ATT_HW_CONFIG , NM_ATT_HW_DESC , NM_ATT_INTAVE_PARAM , NM_ATT_INTERF_BOUND , NM_ATT_LIST_REQ_ATTR , NM_ATT_MAIO , NM_ATT_MANUF_STATE , NM_ATT_MANUF_THRESH , NM_ATT_MANUF_ID , NM_ATT_MAX_TA , NM_ATT_MDROP_LINK , NM_ATT_MDROP_NEXT , NM_ATT_NACK_CAUSES , NM_ATT_NY1 , NM_ATT_OPER_STATE , NM_ATT_OVERL_PERIOD , NM_ATT_PHYS_CONF , NM_ATT_POWER_CLASS , NM_ATT_POWER_THRESH , NM_ATT_PROB_CAUSE , NM_ATT_RACH_B_THRESH , NM_ATT_LDAVG_SLOTS , NM_ATT_RAD_SUBC , NM_ATT_RF_MAXPOWR_R , NM_ATT_SITE_INPUTS , NM_ATT_SITE_OUTPUTS , NM_ATT_SOURCE , NM_ATT_SPEC_PROB , NM_ATT_START_TIME , NM_ATT_T200 , NM_ATT_TEI , NM_ATT_TEST_DUR , NM_ATT_TEST_NO , NM_ATT_TEST_REPORT , NM_ATT_VSWR_THRESH , NM_ATT_WINDOW_SIZE , NM_ATT_BS11_RSSI_OFFS = 0x3d , NM_ATT_BS11_TXPWR = 0x3e , NM_ATT_BS11_DIVERSITY = 0x3f , NM_ATT_TSC = 0x40 , NM_ATT_SW_CONFIG , NM_ATT_SW_DESCR , NM_ATT_SEVERITY , NM_ATT_GET_ARI , NM_ATT_HW_CONF_CHG , NM_ATT_OUTST_ALARM , NM_ATT_FILE_DATA , NM_ATT_MEAS_RES , NM_ATT_MEAS_TYPE , NM_ATT_BS11_ESN_FW_CODE_NO = 0x4c , NM_ATT_BS11_ESN_HW_CODE_NO = 0x4f , NM_ATT_BS11_ESN_PCB_SERIAL = 0x55 , NM_ATT_BS11_EXCESSIVE_DISTANCE = 0x58 , NM_ATT_BS11_ALL_TEST_CATG = 0x60 , NM_ATT_BS11_BTSLS_HOPPING , NM_ATT_BS11_CELL_ALLOC_NR , NM_ATT_BS11_CELL_GLOBAL_ID , NM_ATT_BS11_ENA_INTERF_CLASS = 0x66 , NM_ATT_BS11_ENA_INT_INTEC_HANDO = 0x67 , NM_ATT_BS11_ENA_INT_INTRC_HANDO = 0x68 , NM_ATT_BS11_ENA_MS_PWR_CTRL = 0x69 , NM_ATT_BS11_ENA_PWR_BDGT_HO = 0x6a , NM_ATT_BS11_ENA_PWR_CTRL_RLFW = 0x6b , NM_ATT_BS11_ENA_RXLEV_HO = 0x6c , NM_ATT_BS11_ENA_RXQUAL_HO = 0x6d , NM_ATT_BS11_FACCH_QUAL = 0x6e , NM_ATT_IPACC_DST_IP = 0x80 , NM_ATT_IPACC_DST_IP_PORT = 0x81 , NM_ATT_IPACC_SSRC = 0x82 , NM_ATT_IPACC_RTP_PAYLD_TYPE = 0x83 , NM_ATT_IPACC_BASEB_ID = 0x84 , NM_ATT_IPACC_STREAM_ID = 0x85 , NM_ATT_IPACC_NV_FLAGS = 0x86 , NM_ATT_IPACC_FREQ_CTRL = 0x87 , NM_ATT_IPACC_PRIM_OML_CFG = 0x88 , NM_ATT_IPACC_SEC_OML_CFG = 0x89 , NM_ATT_IPACC_IP_IF_CFG = 0x8a , NM_ATT_IPACC_IP_GW_CFG = 0x8b , NM_ATT_IPACC_IN_SERV_TIME = 0x8c , NM_ATT_IPACC_TRX_BTS_ASS = 0x8d , NM_ATT_IPACC_LOCATION = 0x8e , NM_ATT_IPACC_PAGING_CFG = 0x8f , NM_ATT_IPACC_FILE_DATA = 0x90 , NM_ATT_IPACC_UNIT_ID = 0x91 , NM_ATT_IPACC_PARENT_UNIT_ID = 0x92 , NM_ATT_IPACC_UNIT_NAME = 0x93 , NM_ATT_IPACC_SNMP_CFG = 0x94 , NM_ATT_IPACC_PRIM_OML_CFG_LIST = 0x95 , NM_ATT_IPACC_PRIM_OML_FB_TOUT = 0x96 , NM_ATT_IPACC_CUR_SW_CFG = 0x97 , NM_ATT_IPACC_TIMING_BUS = 0x98 , NM_ATT_IPACC_CGI = 0x99 , NM_ATT_IPACC_RAC = 0x9a , NM_ATT_IPACC_OBJ_VERSION = 0x9b , NM_ATT_IPACC_GPRS_PAGING_CFG = 0x9c , NM_ATT_IPACC_NSEI = 0x9d , NM_ATT_IPACC_BVCI = 0x9e , NM_ATT_IPACC_NSVCI = 0x9f , NM_ATT_IPACC_NS_CFG = 0xa0 , NM_ATT_IPACC_BSSGP_CFG = 0xa1 , NM_ATT_IPACC_NS_LINK_CFG = 0xa2 , NM_ATT_IPACC_RLC_CFG = 0xa3 , NM_ATT_IPACC_ALM_THRESH_LIST = 0xa4 , NM_ATT_IPACC_MONIT_VAL_LIST = 0xa5 , NM_ATT_IPACC_TIB_CONTROL = 0xa6 , NM_ATT_IPACC_SUPP_FEATURES = 0xa7 , NM_ATT_IPACC_CODING_SCHEMES = 0xa8 , NM_ATT_IPACC_RLC_CFG_2 = 0xa9 , NM_ATT_IPACC_HEARTB_TOUT = 0xaa , NM_ATT_IPACC_UPTIME = 0xab , NM_ATT_IPACC_RLC_CFG_3 = 0xac , NM_ATT_IPACC_SSL_CFG = 0xad , NM_ATT_IPACC_SEC_POSSIBLE = 0xae , NM_ATT_IPACC_IML_SSL_STATE = 0xaf , NM_ATT_IPACC_REVOC_DATE = 0xb0 , NM_ATT_BS11_RF_RES_IND_PER = 0x8f , NM_ATT_BS11_RX_LEV_MIN_CELL = 0x90 , NM_ATT_BS11_ABIS_EXT_TIME = 0x91 , NM_ATT_BS11_TIMER_HO_REQUEST = 0x92 , NM_ATT_BS11_TIMER_NCELL = 0x93 , NM_ATT_BS11_TSYNC = 0x94 , NM_ATT_BS11_TTRAU = 0x95 , NM_ATT_BS11_EMRG_CFG_MEMBER = 0x9b , NM_ATT_BS11_TRX_AREA = 0x9f , NM_ATT_BS11_BCCH_RECONF = 0xd7 , NM_ATT_BS11_BIT_ERR_THESH = 0xa0 , NM_ATT_BS11_BOOT_SW_VERS = 0xa1 , NM_ATT_BS11_CCLK_ACCURACY = 0xa3 , NM_ATT_BS11_CCLK_TYPE = 0xa4 , NM_ATT_BS11_INP_IMPEDANCE = 0xaa , NM_ATT_BS11_L1_PROT_TYPE = 0xab , NM_ATT_BS11_LINE_CFG = 0xac , NM_ATT_BS11_LI_PORT_1 = 0xad , NM_ATT_BS11_LI_PORT_2 = 0xae , NM_ATT_BS11_L1_REM_ALM_TYPE = 0xb0 , NM_ATT_BS11_SW_LOAD_INTENDED = 0xbb , NM_ATT_BS11_SW_LOAD_SAFETY = 0xbc , NM_ATT_BS11_SW_LOAD_STORED = 0xbd , NM_ATT_BS11_VENDOR_NAME = 0xc1 , NM_ATT_BS11_HOPPING_MODE = 0xc5 , NM_ATT_BS11_LMT_LOGON_SESSION = 0xc6 , NM_ATT_BS11_LMT_LOGIN_TIME = 0xc7 , NM_ATT_BS11_LMT_USER_ACC_LEV = 0xc8 , NM_ATT_BS11_LMT_USER_NAME = 0xc9 , NM_ATT_BS11_L1_CONTROL_TS = 0xd8 , NM_ATT_BS11_RADIO_MEAS_GRAN = 0xdc , NM_ATT_BS11_RADIO_MEAS_REP = 0xdd , NM_ATT_BS11_SH_LAPD_INT_TIMER = 0xe8 , NM_ATT_BS11_BTS_STATE = 0xf0 , NM_ATT_BS11_E1_STATE = 0xf1 , NM_ATT_BS11_PLL = 0xf2 , NM_ATT_BS11_RX_OFFSET = 0xf3 , NM_ATT_BS11_ANT_TYPE = 0xf4 , NM_ATT_BS11_PLL_MODE = 0xfc , NM_ATT_BS11_PASSWORD = 0xfd , NM_ATT_OSMO_NS_LINK_CFG = 0xfd , NM_ATT_OSMO_REDUCEPOWER = 0xfe }
| OML Attributes / IEs (Section 9.4) More...
enum | abis_nm_adm_state { NM_STATE_LOCKED = 0x01 , NM_STATE_UNLOCKED = 0x02 , NM_STATE_SHUTDOWN = 0x03 , NM_STATE_NULL = 0xff }
| OML Administrative State (Section 9.4.4) More...
enum | abis_nm_avail_state { NM_AVSTATE_IN_TEST = 0 , NM_AVSTATE_FAILED = 1 , NM_AVSTATE_POWER_OFF = 2 , NM_AVSTATE_OFF_LINE = 3 , NM_AVSTATE_DEPENDENCY = 5 , NM_AVSTATE_DEGRADED = 6 , NM_AVSTATE_NOT_INSTALLED = 7 , NM_AVSTATE_OK = 0xff }
| OML Availability State (Section 9.4.7) More...
enum | abis_nm_op_state { NM_OPSTATE_DISABLED = 1 , NM_OPSTATE_ENABLED = 2 , NM_OPSTATE_NULL = 0xff }
| OML Operational State. More...
enum | abis_nm_chan_comb { NM_CHANC_TCHFull = 0x00 , NM_CHANC_TCHHalf = 0x01 , NM_CHANC_TCHHalf2 = 0x02 , NM_CHANC_SDCCH = 0x03 , NM_CHANC_mainBCCH = 0x04 , NM_CHANC_BCCHComb = 0x05 , NM_CHANC_BCCH = 0x06 , NM_CHANC_BCCH_CBCH = 0x07 , NM_CHANC_SDCCH_CBCH = 0x08 , NM_CHANC_IPAC_bPDCH = 0x0b , NM_CHANC_IPAC_cPDCH = 0x0c , NM_CHANC_IPAC_PDCH = 0x0d , NM_CHANC_IPAC_TCHFull_PDCH = 0x80 , NM_CHANC_IPAC_TCHFull_TCHHalf = 0x81 , NM_CHANC_OSMO_DYN = 0x90 }
enum | abis_nm_event_type { NM_EVT_COMM_FAIL = 0x00 , NM_EVT_QOS_FAIL = 0x01 , NM_EVT_PROC_FAIL = 0x02 , NM_EVT_EQUIP_FAIL = 0x03 , NM_EVT_ENV_FAIL = 0x04 }
| Event Type (Section 9.4.16) More...
enum | abis_nm_severity { NM_SEVER_CEASED = 0x00 , NM_SEVER_CRITICAL = 0x01 , NM_SEVER_MAJOR = 0x02 , NM_SEVER_MINOR = 0x03 , NM_SEVER_WARNING = 0x04 , NM_SEVER_INDETERMINATE = 0x05 }
| Perceived Severity (Section: 9.4.63) More...
enum | abis_nm_pcause_type { NM_PCAUSE_T_X721 = 0x01 , NM_PCAUSE_T_GSM = 0x02 , NM_PCAUSE_T_MANUF = 0x03 }
| Probable Cause Type (Section 9.4.43) More...
enum | abis_nm_nack_cause { NM_NACK_INCORR_STRUCT = 0x01 , NM_NACK_MSGTYPE_INVAL = 0x02 , NM_NACK_OBJCLASS_INVAL = 0x05 , NM_NACK_OBJCLASS_NOTSUPP = 0x06 , NM_NACK_BTSNR_UNKN = 0x07 , NM_NACK_TRXNR_UNKN = 0x08 , NM_NACK_OBJINST_UNKN = 0x09 , NM_NACK_ATTRID_INVAL = 0x0c , NM_NACK_ATTRID_NOTSUPP = 0x0d , NM_NACK_PARAM_RANGE = 0x0e , NM_NACK_ATTRLIST_INCONSISTENT = 0x0f , NM_NACK_SPEC_IMPL_NOTSUPP = 0x10 , NM_NACK_CANT_PERFORM = 0x11 , NM_NACK_RES_NOTIMPL = 0x19 , NM_NACK_RES_NOTAVAIL = 0x1a , NM_NACK_FREQ_NOTAVAIL = 0x1b , NM_NACK_TEST_NOTSUPP = 0x1c , NM_NACK_CAPACITY_RESTR = 0x1d , NM_NACK_PHYSCFG_NOTPERFORM = 0x1e , NM_NACK_TEST_NOTINIT = 0x1f , NM_NACK_PHYSCFG_NOTRESTORE = 0x20 , NM_NACK_TEST_NOSUCH = 0x21 , NM_NACK_TEST_NOSTOP = 0x22 , NM_NACK_MSGINCONSIST_PHYSCFG = 0x23 , NM_NACK_FILE_INCOMPLETE = 0x25 , NM_NACK_FILE_NOTAVAIL = 0x26 , NM_NACK_FILE_NOTACTIVATE = 0x27 , NM_NACK_REQ_NOT_GRANT = 0x28 , NM_NACK_WAIT = 0x29 , NM_NACK_NOTH_REPORT_EXIST = 0x2a , NM_NACK_MEAS_NOTSUPP = 0x2b , NM_NACK_MEAS_NOTSTART = 0x2c }
| NACK causes (Section 9.4.36) More...
enum | abis_nm_t200_idx { T200_SDCCH = 0 , T200_FACCH_F = 1 , T200_FACCH_H = 2 , T200_SACCH_TCH_SAPI0 = 3 , T200_SACCH_SDCCH = 4 , T200_SDCCH_SAPI3 = 5 , T200_SACCH_TCH_SAPI3 = 6 }
| 3GPP TS 12.21 9.4.53 T200 index More...
enum | abis_bs11_objtype { BS11_OBJ_ALCO = 0x01 , BS11_OBJ_BBSIG = 0x02 , BS11_OBJ_TRX1 = 0x03 , BS11_OBJ_CCLK = 0x04 , BS11_OBJ_GPSU = 0x06 , BS11_OBJ_LI = 0x07 , BS11_OBJ_PA = 0x09 }
| Siemens BS-11 specific objects in the SienemsHW (0xA5) object class. More...
enum | abis_bs11_trx_power { BS11_TRX_POWER_GSM_2W = 0x06 , BS11_TRX_POWER_GSM_250mW = 0x07 , BS11_TRX_POWER_GSM_80mW = 0x08 , BS11_TRX_POWER_GSM_30mW = 0x09 , BS11_TRX_POWER_DCS_3W = 0x0a , BS11_TRX_POWER_DCS_1W6 = 0x0b , BS11_TRX_POWER_DCS_500mW = 0x0c , BS11_TRX_POWER_DCS_160mW = 0x0d }
| Siemens BS11 TRX power. More...
enum | abis_bs11_li_pll_mode { BS11_LI_PLL_LOCKED = 2 , BS11_LI_PLL_STANDALONE = 3 }
| Siemens BS11 PLL mode. More...
enum | abis_bs11_line_cfg { BS11_LINE_CFG_STAR = 0x00 , BS11_LINE_CFG_MULTIDROP = 0x01 , BS11_LINE_CFG_LOOP = 0x02 }
| Siemens BS11 E1 line configuration. More...
enum | abis_bs11_phase { BS11_STATE_SOFTWARE_RQD = 0x01 , BS11_STATE_LOAD_SMU_INTENDED = 0x11 , BS11_STATE_LOAD_SMU_SAFETY = 0x21 , BS11_STATE_LOAD_FAILED = 0x31 , BS11_STATE_LOAD_DIAGNOSTIC = 0x41 , BS11_STATE_WARM_UP = 0x51 , BS11_STATE_WARM_UP_2 = 0x52 , BS11_STATE_WAIT_MIN_CFG = 0x62 , BS11_STATE_MAINTENANCE = 0x72 , BS11_STATE_LOAD_MBCCU = 0x92 , BS11_STATE_WAIT_MIN_CFG_2 = 0xA2 , BS11_STATE_NORMAL = 0x03 , BS11_STATE_ABIS_LOAD = 0x13 }
| Siemens BS11 boot phase. More...
enum | abis_nm_ipacc_test_no { NM_IPACC_TESTNO_RLOOP_ANT = 0x01 , NM_IPACC_TESTNO_RLOOP_XCVR = 0x02 , NM_IPACC_TESTNO_FUNC_OBJ = 0x03 , NM_IPACC_TESTNO_CHAN_USAGE = 0x40 , NM_IPACC_TESTNO_BCCH_CHAN_USAGE = 0x41 , NM_IPACC_TESTNO_FREQ_SYNC = 0x42 , NM_IPACC_TESTNO_BCCH_INFO = 0x43 , NM_IPACC_TESTNO_TX_BEACON = 0x44 , NM_IPACC_TESTNO_SYSINFO_MONITOR = 0x45 , NM_IPACC_TESTNO_BCCCH_MONITOR = 0x46 }
| ip.access test number More...
enum | abis_nm_ipacc_test_res { NM_IPACC_TESTRES_SUCCESS = 0 , NM_IPACC_TESTRES_TIMEOUT = 1 , NM_IPACC_TESTRES_NO_CHANS = 2 , NM_IPACC_TESTRES_PARTIAL = 3 , NM_IPACC_TESTRES_STOPPED = 4 }
| first byte after length inside NM_ATT_TEST_REPORT More...
enum | abis_nm_ipacc_testres_ie { NM_IPACC_TR_IE_FREQ_ERR_LIST = 3 , NM_IPACC_TR_IE_CHAN_USAGE = 4 , NM_IPACC_TR_IE_BCCH_INFO = 6 , NM_IPACC_TR_IE_RESULT_DETAILS = 8 , NM_IPACC_TR_IE_FREQ_ERR = 18 }
| internal IE inside NM_ATT_TEST_REPORT More...
enum | ipac_eie { NM_IPAC_EIE_ARFCN_WHITE = 0x01 , NM_IPAC_EIE_ARFCH_BLACK = 0x02 , NM_IPAC_EIE_FREQ_ERR_LIST = 0x03 , NM_IPAC_EIE_CHAN_USE_LIST = 0x04 , NM_IPAC_EIE_BCCH_INFO_TYPE = 0x05 , NM_IPAC_EIE_BCCH_INFO = 0x06 , NM_IPAC_EIE_CONFIG = 0x07 , NM_IPAC_EIE_RES_DETAILS = 0x08 , NM_IPAC_EIE_RXLEV_THRESH = 0x09 , NM_IPAC_EIE_FREQ_SYNC_OPTS = 0x0a , NM_IPAC_EIE_MAC_ADDR = 0x0b , NM_IPAC_EIE_HW_SW_COMPAT_NR = 0x0c , NM_IPAC_EIE_MANUF_SER_NR = 0x0d , NM_IPAC_EIE_OEM_ID = 0x0e , NM_IPAC_EIE_DATE_TIME_MANUF = 0x0f , NM_IPAC_EIE_DATE_TIME_CALIB = 0x10 , NM_IPAC_EIE_BEACON_INFO = 0x11 , NM_IPAC_EIE_FREQ_ERR = 0x12 , NM_IPAC_EIE_FREQ_BANDS = 0x1c , NM_IPAC_EIE_MAX_TA = 0x1d , NM_IPAC_EIE_CIPH_ALGOS = 0x1e , NM_IPAC_EIE_CHAN_TYPES = 0x1f , NM_IPAC_EIE_CHAN_MODES = 0x20 , NM_IPAC_EIE_GPRS_CODING = 0x21 , NM_IPAC_EIE_RTP_FEATURES = 0x22 , NM_IPAC_EIE_RSL_FEATURES = 0x23 , NM_IPAC_EIE_BTS_HW_CLASS = 0x24 , NM_IPAC_EIE_BTS_ID = 0x25 }
| ip.access IEI More...
enum | ipac_bcch_info_type { IPAC_BINF_RXLEV = (1 << 8) , IPAC_BINF_RXQUAL = (1 << 9) , IPAC_BINF_FREQ_ERR_QUAL = (1 << 10) , IPAC_BINF_FRAME_OFFSET = (1 << 11) , IPAC_BINF_FRAME_NR_OFFSET = (1 << 12) , IPAC_BINF_BSIC = (1 << 13) , IPAC_BINF_CGI = (1 << 14) , IPAC_BINF_NEIGH_BA_SI2 = (1 << 15) , IPAC_BINF_NEIGH_BA_SI2bis = (1 << 0) , IPAC_BINF_NEIGH_BA_SI2ter = (1 << 1) , IPAC_BINF_CELL_ALLOC = (1 << 2) }
| ip.access NWL BCCH information type More...
enum | osmo_oml_nsvc_address_type { OSMO_NSVC_ADDR_UNSPEC = 0x00 , OSMO_NSVC_ADDR_IPV4 = 0x04 , OSMO_NSVC_ADDR_IPV6 = 0x29 }
| Osmocom NSVC address type for NM_ATT_OSMO_NS_LINK_CFG. More...

## Functions
struct abis_om_hdr | __attribute__ ((packed))
uint16_t | abis_nm_sw_desc_len (const struct abis_nm_sw_desc *sw, bool put_sw_desc)
| Compute length of given 3GPP TS 52.021 §9.4.62 SW Description. More...
uint16_t | abis_nm_put_sw_desc (struct msgb *msg, const struct abis_nm_sw_desc *sw, bool put_sw_desc)
| Put given 3GPP TS 52.021 §9.4.62 SW Description into msgb. More...
uint16_t | abis_nm_put_sw_file (struct msgb *msg, const char *id, const char *ver, bool put_sw_desc)
| Put given file ID/Version pair as 3GPP TS 52.021 §9.4.62 SW Description into msgb. More...
uint32_t | abis_nm_get_sw_desc_len (const uint8_t *buf, size_t len)
| Get length of first 3GPP TS 52.021 §9.4.62 SW Description from buffer. More...
int | abis_nm_get_sw_conf (const uint8_t *buf, size_t buf_len, struct abis_nm_sw_desc *sw, uint16_t sw_len)
| Parse 3GPP TS 52.021 §9.4.61 SW Configuration from buffer. More...
struct msgb * | abis_nm_fail_evt_rep (enum abis_nm_event_type t, enum abis_nm_severity s, enum abis_nm_pcause_type ct, uint16_t cause_value, const char *fmt,...)
| Pack 3GPP TS 12.21 § 8.8.2 Failure Event Report into msgb. More...
struct msgb * | abis_nm_fail_evt_vrep (enum abis_nm_event_type t, enum abis_nm_severity s, enum abis_nm_pcause_type ct, uint16_t cause_value, const char *fmt, va_list ap)
| Pack 3GPP TS 12.21 § 8.8.2 Failure Event Report into msgb. More...

## Variables
uint8_t | mdisc
| Message Discriminator abis_oml_mdisc. More...
uint8_t | placement
| Placement (like ABIS_OM_PLACEMENT_ONLY) More...
uint8_t | sequence
| Sequence Number (if ABIS_OM_PLACEMENT_MIDDLE) More...
uint8_t | length
| Length in octets. More...
uint8_t | data [0]
| actual payload data More...
uint8_t | bts_nr
| BTS Number. More...
uint8_t | trx_nr
| TRX Number. More...
uint8_t | ts_nr
| Timeslot Number. More...
uint8_t | msg_type
| Message Type (abis_nm_msgtype) More...
uint8_t | obj_class
| Object Class (abis_nm_obj_class) More...
struct abis_om_obj_inst | obj_inst
| Object Instance. More...
enum abis_nm_msgtype | __attribute__
const struct value_string | abis_mm_event_cause_names []
const struct value_string | abis_nm_pcause_type_names []
const struct value_string | abis_nm_msgtype_names []
| 3GPP TS 52.021 §9.1 Message Types More...
const struct value_string | abis_nm_att_names []
| 3GPP TS 52.021 §9.4 Attributes and Parameters More...
uint8_t | attrib
uint8_t | bts_port
| BTS port number. More...
uint8_t | timeslot
| E1 timeslot. More...
uint8_t | subslot
| E1 sub-slot. More...
const uint8_t | abis_nm_t200_ms []
| 3GPP TS 12.21 9.4.53 T200 values (in msec) More...
const struct value_string | abis_nm_ipacc_freq_band_desc []
const struct value_string | abis_nm_ipacc_ciph_algo_desc []
const struct value_string | abis_nm_ipacc_chant_desc []
const struct value_string | abis_nm_ipacc_chanm_desc []
const struct value_string | abis_nm_ipacc_gprs_coding_desc []
const struct value_string | abis_nm_ipacc_rtp_feat_desc []
const struct value_string | abis_nm_ipacc_rsl_feat_desc []
uint8_t | un_blocking_timer
uint8_t | un_blocking_retries
uint8_t | reset_timer
uint8_t | reset_retries
uint8_t | test_timer
uint8_t | alive_timer
uint8_t | alive_retries
uint8_t | t1_s
uint8_t | t1_blocking_retries
uint8_t | t1_unblocking_retries
uint8_t | t2_s
uint8_t | t2_retries
uint8_t | t3_100ms
uint8_t | t3_retries
uint8_t | t4_100ms
uint8_t | t4_retries
uint8_t | t5_s
uint8_t | t5_retries
uint8_t | t3142
uint8_t | t3169
uint8_t | t3191
uint8_t | t3193_10ms
uint8_t | t3195
uint8_t | n3101
uint8_t | n3103
uint8_t | n3105
uint8_t | rlc_cv_countdown
uint16_t | t_dl_tbf_ext_10ms
uint16_t | t_ul_tbf_ext_10ms
uint8_t | initial_cs
uint8_t | initial_mcs

## Variable Documentation

## ◆ alive_retries

uint8_t alive_retries

## ◆ alive_timer

uint8_t alive_timer

## ◆ attrib

uint8_t attrib

## ◆ bts_nr

uint8_t bts_nr

BTS Number.

## ◆ bts_port

uint8_t bts_port

BTS port number.

## ◆ data

uint8_t data[0]

actual payload data

Data.

## ◆ initial_cs

uint8_t initial_cs

## ◆ initial_mcs

uint8_t initial_mcs

## ◆ length

uint8_t length

Length in octets.

## ◆ mdisc

uint8_t mdisc

Message Discriminator abis_oml_mdisc.

## ◆ msg_type

uint8_t msg_type

Message Type (abis_nm_msgtype)

## ◆ n3101

uint8_t n3101

## ◆ n3103

uint8_t n3103

## ◆ n3105

uint8_t n3105

## ◆ obj_class

uint8_t obj_class

Object Class (abis_nm_obj_class)

## ◆ obj_inst

struct abis_om_obj_inst obj_inst

Object Instance.

## ◆ placement

uint8_t placement

Placement (like ABIS_OM_PLACEMENT_ONLY)

## ◆ reset_retries

uint8_t reset_retries

## ◆ reset_timer

uint8_t reset_timer

## ◆ rlc_cv_countdown

uint8_t rlc_cv_countdown

## ◆ sequence

uint8_t sequence

Sequence Number (if ABIS_OM_PLACEMENT_MIDDLE)

## ◆ subslot

uint8_t subslot

E1 sub-slot.

## ◆ t1_blocking_retries

uint8_t t1_blocking_retries

## ◆ t1_s

uint8_t t1_s

## ◆ t1_unblocking_retries

uint8_t t1_unblocking_retries

## ◆ t2_retries

uint8_t t2_retries

## ◆ t2_s

uint8_t t2_s

## ◆ t3142

uint8_t t3142

## ◆ t3169

uint8_t t3169

## ◆ t3191

uint8_t t3191

## ◆ t3193_10ms

uint8_t t3193_10ms

## ◆ t3195

uint8_t t3195

## ◆ t3_100ms

uint8_t t3_100ms

## ◆ t3_retries

uint8_t t3_retries

## ◆ t4_100ms

uint8_t t4_100ms

## ◆ t4_retries

uint8_t t4_retries

## ◆ t5_retries

uint8_t t5_retries

## ◆ t5_s

uint8_t t5_s

## ◆ t_dl_tbf_ext_10ms

uint16_t t_dl_tbf_ext_10ms

## ◆ t_ul_tbf_ext_10ms

uint16_t t_ul_tbf_ext_10ms

## ◆ test_timer

uint8_t test_timer

## ◆ timeslot

uint8_t timeslot

E1 timeslot.

Referenced by rsl_dec_chan_nr(), and rsl_enc_chan_nr().

## ◆ trx_nr

uint8_t trx_nr

TRX Number.

## ◆ ts_nr

uint8_t ts_nr

Timeslot Number.

## ◆ un_blocking_retries

uint8_t un_blocking_retries

## ◆ un_blocking_timer

uint8_t un_blocking_timer