libosmocoding 1.13.1.1-afb4 Osmocom GSM/GPRS/EGPRS L1 channel coding library

Functions
gsm0503_interleaving.h File Reference
Interleaving

GSM TS 05.03 interleaving. More...

`#include <osmocom/core/bits.h>`

Go to the source code of this file.

## Functions
void | gsm0503_xcch_deinterleave (sbit_t *cB, const sbit_t *iB)
| De-Interleave burst bits according to TS 05.03 4.1.4. More...
void | gsm0503_xcch_interleave (const ubit_t *cB, ubit_t *iB)
| Interleave burst bits according to TS 05.03 4.1.4. More...
void | gsm0503_tch_fr_deinterleave (sbit_t *cB, const sbit_t *iB)
| GSM TCH FR/EFR/AFS De-Interleaving and burst mapping. More...
void | gsm0503_tch_fr_interleave (const ubit_t *cB, ubit_t *iB)
| GSM TCH FR/EFR/AFS Interleaving and burst mapping. More...
void | gsm0503_tch_hr_deinterleave (sbit_t *cB, const sbit_t *iB)
| GSM TCH HR/AHS De-Interleaving and burst mapping. More...
void | gsm0503_tch_hr_interleave (const ubit_t *cB, ubit_t *iB)
| GSM TCH HR/AHS Interleaving and burst mapping. More...
void | gsm0503_mcs1_ul_deinterleave (sbit_t *hc, sbit_t *dc, const sbit_t *iB)
| Interleave MCS1 UL burst bits according to TS 05.03 5.1.5.2.4. More...
void | gsm0503_mcs1_ul_interleave (const ubit_t *hc, const ubit_t *dc, ubit_t *iB)
| Interleave MCS1 DL burst bits according to TS 05.03 5.1.5.2.4. More...
void | gsm0503_mcs1_dl_deinterleave (sbit_t *u, sbit_t *hc, sbit_t *dc, const sbit_t *iB)
| De-Interleave MCS1 DL burst bits according to TS 05.03 5.1.5.1.5. More...
void | gsm0503_mcs1_dl_interleave (const ubit_t *up, const ubit_t *hc, const ubit_t *dc, ubit_t *iB)
| Interleave MCS1 DL burst bits according to TS 05.03 5.1.5.1.5. More...
void | gsm0503_mcs5_ul_deinterleave (sbit_t *hc, sbit_t *dc, const sbit_t *hi, const sbit_t *di)
| De-Interleave MCS5 UL burst bits according to TS 05.03 5.1.9.2.4. More...
void | gsm0503_mcs5_ul_interleave (const ubit_t *hc, const ubit_t *dc, ubit_t *hi, ubit_t *di)
| Interleave MCS5 UL burst bits according to TS 05.03 5.1.9.2.4. More...
void | gsm0503_mcs5_dl_deinterleave (sbit_t *hc, sbit_t *dc, const sbit_t *hi, const sbit_t *di)
| De-Interleave MCS5 UL burst bits according to TS 05.03 5.1.9.1.5. More...
void | gsm0503_mcs5_dl_interleave (const ubit_t *hc, const ubit_t *dc, ubit_t *hi, ubit_t *di)
| Interleave MCS5 DL burst bits according to TS 05.03 5.1.9.1.5. More...
void | gsm0503_mcs7_ul_deinterleave (sbit_t *hc, sbit_t *c1, sbit_t *c2, const sbit_t *hi, const sbit_t *di)
| De-Interleave MCS7 UL burst bits according to TS 05.03 5.1.11.2.4. More...
void | gsm0503_mcs7_ul_interleave (const ubit_t *hc, const ubit_t *c1, const ubit_t *c2, ubit_t *hi, ubit_t *di)
| Interleave MCS7 UL burst bits according to TS 05.03 5.1.11.2.4. More...
void | gsm0503_mcs7_dl_deinterleave (sbit_t *hc, sbit_t *c1, sbit_t *c2, const sbit_t *hi, const sbit_t *di)
| De-Interleave MCS7 DL burst bits according to TS 05.03 5.1.11.1.5. More...
void | gsm0503_mcs7_dl_interleave (const ubit_t *hc, const ubit_t *c1, const ubit_t *c2, ubit_t *hi, ubit_t *di)
| Interleave MCS7 DL burst bits according to TS 05.03 5.1.11.1.5. More...
void | gsm0503_mcs8_ul_deinterleave (sbit_t *hc, sbit_t *c1, sbit_t *c2, const sbit_t *hi, const sbit_t *di)
| De-Interleave MCS8 UL burst bits according to TS 05.03 5.1.12.2.4. More...
void | gsm0503_mcs8_ul_interleave (const ubit_t *hc, const ubit_t *c1, const ubit_t *c2, ubit_t *hi, ubit_t *di)
| Interleave MCS8 UL burst bits according to TS 05.03 5.1.12.2.4. More...
void | gsm0503_mcs8_dl_deinterleave (sbit_t *hc, sbit_t *c1, sbit_t *c2, const sbit_t *hi, const sbit_t *di)
| De-Interleave MCS8 DL burst bits according to TS 05.03 5.1.12.1.5. More...
void | gsm0503_mcs8_dl_interleave (const ubit_t *hc, const ubit_t *c1, const ubit_t *c2, ubit_t *hi, ubit_t *di)
| Interleave MCS8 DL burst bits according to TS 05.03 5.1.12.1.5. More...
void | gsm0503_tch_f96_deinterleave (sbit_t *cB, const sbit_t *iB)
void | gsm0503_tch_f96_interleave (const ubit_t *cB, ubit_t *iB)

## Detailed Description

GSM TS 05.03 interleaving.