libosmocore 1.13.1.1-afb4 Osmocom core library

Functions | Variables
gsmtap_util.h File Reference
GSMTAP
`#include <stdint.h>`
`#include <stdbool.h>`
`#include <osmocom/core/write_queue.h>`
`#include <osmocom/core/select.h>`

Go to the source code of this file.

## Functions
uint8_t | chantype_rsl2gsmtap2 (uint8_t rsl_chantype, uint8_t link_id, bool user_plane)
| convert RSL channel number to GSMTAP channel type More...
uint8_t | chantype_rsl2gsmtap (uint8_t rsl_chantype, uint8_t link_id)
| convert RSL channel number to GSMTAP channel type More...
void | chantype_gsmtap2rsl (uint8_t gsmtap_chantype, uint8_t *rsl_chantype, uint8_t *link_id)
| convert GSMTAP channel type to RSL channel number + Link ID More...
struct msgb * | gsmtap_makemsg_ex (uint8_t type, uint16_t arfcn, uint8_t ts, uint8_t chan_type, uint8_t ss, uint32_t fn, int8_t signal_dbm, int8_t snr, const uint8_t *data, unsigned int len)
| create an arbitrary type GSMTAP message More...
struct msgb * | gsmtap_makemsg (uint16_t arfcn, uint8_t ts, uint8_t chan_type, uint8_t ss, uint32_t fn, int8_t signal_dbm, int8_t snr, const uint8_t *data, unsigned int len)
| create L1/L2 data and put it into GSMTAP More...
int | gsmtap_inst_fd (struct gsmtap_inst *gti)
| Deprecated, use gsmtap_inst_fd2() instead. More...
int | gsmtap_inst_fd2 (const struct gsmtap_inst *gti)
| obtain the file descriptor associated with a gsmtap instance More...
int | gsmtap_source_init_fd (const char *host, uint16_t port)
int | gsmtap_source_init_fd2 (const char *local_host, uint16_t local_port, const char *rem_host, uint16_t rem_port)
int | gsmtap_source_add_sink_fd (int gsmtap_fd)
struct gsmtap_inst * | gsmtap_source_init (const char *host, uint16_t port, int ofd_wq_mode)
struct gsmtap_inst * | gsmtap_source_init2 (const char *local_host, uint16_t local_port, const char *rem_host, uint16_t rem_port, int ofd_wq_mode)
void | gsmtap_source_free (struct gsmtap_inst *gti)
int | gsmtap_source_set_nonblock (struct gsmtap_inst *gti, int on)
int | gsmtap_source_add_sink (struct gsmtap_inst *gti)
bool | gsmtap_source_using_wq (const struct gsmtap_inst *gti)
int | gsmtap_sendmsg (struct gsmtap_inst *gti, struct msgb *msg)
int | gsmtap_sendmsg_free (struct gsmtap_inst *gti, struct msgb *msg)
int | gsmtap_send_ex (struct gsmtap_inst *gti, uint8_t type, uint16_t arfcn, uint8_t ts, uint8_t chan_type, uint8_t ss, uint32_t fn, int8_t signal_dbm, int8_t snr, const uint8_t *data, unsigned int len)
int | gsmtap_send (struct gsmtap_inst *gti, uint16_t arfcn, uint8_t ts, uint8_t chan_type, uint8_t ss, uint32_t fn, int8_t signal_dbm, int8_t snr, const uint8_t *data, unsigned int len)

## Variables
const struct value_string | gsmtap_gsm_channel_names []
const struct value_string | gsmtap_type_names []