libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - s -

- s_bits : osmo_rlp_frame_decoded
- s_ftype : osmo_rlp_frame_decoded
- sac : osmo_service_area_id
- sacch_only : info_act_req_param
- sai : gsm0808_cell_id_u
- scheduling : osmo_gsm48_si_ro_info
- screen : gsm_mncc_number
- sdu_err_ratio : gsm48_qos
- secret_k : osmo_oap_client_config, osmo_oap_client_state
- secret_k_present : osmo_oap_client_config
- secret_opc : osmo_oap_client_config, osmo_oap_client_state
- secret_opc_present : osmo_oap_client_config
- sel_ciph_dl_sacch : gsm48_classmark3
- selection_params : osmo_gsm48_si_ro_info
- seq_last : gsm0808_cell_id_list_segment
- seq_number : gsm0808_cell_id_list_segment
- sequence : abis_om_hdr
- serial : gsm341_etws_message, gsm341_ms_message
- serial_nr : gsm23041_etws_primary_gsm, gsm23041_msg_param_gsm, gsm23041_msg_param_umts
- serno : ipaccess_unit
- serv_ind : gsm29118_paging_req
- session_id : osmo_gsup_message
- session_state : osmo_gsup_message
- si13_position : osmo_gsm48_si3_gprs_ind
- si2quater_indicator : osmo_gsm48_si_ro_info
- si2ter_indicator : osmo_gsm48_si_ro_info
- si_change_field : osmo_gsm48_si13_info
- sig_access : gsm_mncc_bearer_cap
- sig_ind : gsm48_qos
- single_band_supp : gsm48_classmark3
- single_slot_dtm : gsm48_classmark3
- site_id : ipaccess_unit
- sm_alert_rsn : osmo_gsup_message
- sm_rp_cause : osmo_gsup_message
- sm_rp_da : osmo_gsup_message
- sm_rp_da_len : osmo_gsup_message
- sm_rp_da_type : osmo_gsup_message
- sm_rp_mms : osmo_gsup_message
- sm_rp_mr : osmo_gsup_message
- sm_rp_oa : osmo_gsup_message
- sm_rp_oa_len : osmo_gsup_message
- sm_rp_oa_type : osmo_gsup_message
- sm_rp_ui : osmo_gsup_message
- sm_rp_ui_len : osmo_gsup_message
- sm_value : gsm48_classmark3
- sms : gsm0808_sms_to_vgcs
- sms_len : gsm0808_sms_to_vgcs
- sms_value : gsm48_classmark3
- snac : osmo_shared_network_area_id
- something1 : sdp_header_entry
- source_name : osmo_gsup_message
- source_name_len : osmo_gsup_message
- spare : gsm48_qos
- spare1 : osmo_iuup_rfci
- spare2 : gsm48_qos, osmo_iuup_rfci
- spare3 : gsm48_qos
- spare5 : gsm48_qos
- spare_extension : iuup_ctrl_ack
- spd_ind : rsl_ie_chan_mode
- speech_codec_chosen : gsm0808_handover_complete, gsm0808_handover_performed, gsm0808_handover_request_ack
- speech_codec_chosen_present : gsm0808_handover_complete, gsm0808_handover_performed, gsm0808_handover_request_ack
- speech_ctm : gsm_mncc_bearer_cap
- speech_ver : gsm_mncc_bearer_cap
- speech_version_chosen : gsm0808_handover_performed
- speech_version_chosen_present : gsm0808_handover_performed
- speech_version_used : gsm0808_handover_request, gsm0808_handover_required
- speech_version_used_present : gsm0808_handover_required
- spgc_ccch_sup : osmo_gsm48_si13_info
- sqn : osmo_sub_auth_data2, osmo_sub_auth_data
- sqn_ms : osmo_sub_auth_data2, osmo_sub_auth_data
- src_stats_desc : gsm48_qos
- sres : gsm48_auth_resp, osmo_auth_vector
- ss_code : ss_request
- ss_info : osmo_gsup_message
- ss_info_len : osmo_gsup_message
- start : sdp_header_entry
- state : osmo_oap_client_state, SHA1Context, sha256_state
- states : smcdatastate, smcdownstate, smrdatastate, smrdownstate
- status : osmo_iuup_rnl_prim
- sub : gsm_meas_rep_unidir
- subflow_sizes : osmo_iuup_rfci
- subslot : abis_nm_channel
- supported_rat_types : osmo_gsup_message
- supported_rat_types_len : osmo_gsup_message
- supported_versions_mask : osmo_iuup_rnl_config
- supports_egprs_11bit_rach : osmo_gprs_cell_options
- sw_part : sdp_firmware
- swversion : ipaccess_unit