libosmogb 1.13.1.1-afb4 Osmocom Gb library

Data Structures | Macros | Enumerations | Functions | Variables
gsm_08_18.h File Reference
`#include <stdint.h>`
`#include <osmocom/core/endian.h>`

Go to the source code of this file.

## Data Structures
struct | bssgp_ud_hdr
| BSSGP User-Data header (Section 10.2.1 and 10.2.2) More...
struct | bssgp_normal_hdr
| BSSGP normal header. More...
struct | bssgp_rim_pdu_ind

## Macros
#define | BVCI_SIGNALLING 0x0000
| Fixed BVCI definitions (Section 5.4.1) More...
#define | BVCI_PTM 0x0001
#define | BSSGP_PDUT_RA_CAPA_UDPATE BSSGP_PDUT_RA_CAPA_UPDATE
#define | BSSGP_FEAT_PFC 0x01 /* Packet Flow Context */
#define | BSSGP_FEAT_CBL 0x02 /* Current Bucket Level */
#define | BSSGP_FEAT_INR 0x04 /* Inter-NSE re-routing */
#define | BSSGP_FEAT_LCS 0x08 /* Location Services */
#define | BSSGP_FEAT_RIM 0x10 /* RAN Inoformation Management */
#define | BSSGP_FEAT_PFC_FC 0x20 /* PFC Flow Control */
#define | BSSGP_FEAT_ERS 0x40 /* Enhanced Radio Status */
#define | BSSGP_FEAT_MBMS 0x80 /* Multimedia Broadcast */
#define | BSSGP_XFEAT_PSHO 0x01 /* PS Handover */
#define | BSSGP_XFEAT_GBIT 0x02 /* Gigabit Interface */
#define | BSSGP_XFEAT_MOCN 0x04 /* Multi-Operator CN */
#define | BSSGP_XFEAT_CSPS 0x08 /* CS/PS coordination enhancements */
#define | BSSGP_XFEAT_ECIoT 0x10 /* EC-GSM-IoT */
#define | BSSGP_XFEAT_DCN 0x20 /* Dedicated CN */
#define | BSSGP_XFEAT_eDRX 0x40 /* eDRX */
#define | BSSGP_XFEAT_MSAD 0x80 /* MS-assisted Dedicated CN selection */

## Enumerations
enum | bssgp_pdu_type { BSSGP_PDUT_DL_UNITDATA = 0x00 , BSSGP_PDUT_UL_UNITDATA = 0x01 , BSSGP_PDUT_RA_CAPABILITY = 0x02 , BSSGP_PDUT_PTM_UNITDATA = 0x03 , BSSGP_PDUT_DL_MMBS_UNITDATA = 0x04 , BSSGP_PDUT_UL_MMBS_UNITDATA = 0x05 , BSSGP_PDUT_PAGING_PS = 0x06 , BSSGP_PDUT_PAGING_CS = 0x07 , BSSGP_PDUT_RA_CAPA_UPDATE = 0x08 , BSSGP_PDUT_RA_CAPA_UPDATE_ACK = 0x09 , BSSGP_PDUT_RADIO_STATUS = 0x0a , BSSGP_PDUT_SUSPEND = 0x0b , BSSGP_PDUT_SUSPEND_ACK = 0x0c , BSSGP_PDUT_SUSPEND_NACK = 0x0d , BSSGP_PDUT_RESUME = 0x0e , BSSGP_PDUT_RESUME_ACK = 0x0f , BSSGP_PDUT_RESUME_NACK = 0x10 , BSSGP_PDUT_PAGING_PS_REJECT = 0x11 , BSSGP_PDUT_DUMMY_PAGING_PS = 0x12 , BSSGP_PDUT_DUMMY_PAGING_PS_RESP = 0x13 , BSSGP_PDUT_MS_REGISTR_ENQ = 0x14 , BSSGP_PDUT_MS_REGISTR_ENQ_RESP = 0x15 , BSSGP_PDUT_BVC_BLOCK = 0x20 , BSSGP_PDUT_BVC_BLOCK_ACK = 0x21 , BSSGP_PDUT_BVC_RESET = 0x22 , BSSGP_PDUT_BVC_RESET_ACK = 0x23 , BSSGP_PDUT_BVC_UNBLOCK = 0x24 , BSSGP_PDUT_BVC_UNBLOCK_ACK = 0x25 , BSSGP_PDUT_FLOW_CONTROL_BVC = 0x26 , BSSGP_PDUT_FLOW_CONTROL_BVC_ACK = 0x27 , BSSGP_PDUT_FLOW_CONTROL_MS = 0x28 , BSSGP_PDUT_FLOW_CONTROL_MS_ACK = 0x29 , BSSGP_PDUT_FLUSH_LL = 0x2a , BSSGP_PDUT_FLUSH_LL_ACK = 0x2b , BSSGP_PDUT_LLC_DISCARD = 0x2c , BSSGP_PDUT_FLOW_CONTROL_PFC = 0x2d , BSSGP_PDUT_FLOW_CONTROL_PFC_ACK = 0x2e , BSSGP_PDUT_SGSN_INVOKE_TRACE = 0x40 , BSSGP_PDUT_STATUS = 0x41 , BSSGP_PDUT_OVERLOAD = 0x42 , BSSGP_PDUT_DOWNLOAD_BSS_PFC = 0x50 , BSSGP_PDUT_CREATE_BSS_PFC = 0x51 , BSSGP_PDUT_CREATE_BSS_PFC_ACK = 0x52 , BSSGP_PDUT_CREATE_BSS_PFC_NACK = 0x53 , BSSGP_PDUT_MODIFY_BSS_PFC = 0x54 , BSSGP_PDUT_MODIFY_BSS_PFC_ACK = 0x55 , BSSGP_PDUT_DELETE_BSS_PFC = 0x56 , BSSGP_PDUT_DELETE_BSS_PFC_ACK = 0x57 , BSSGP_PDUT_DELETE_BSS_PFC_REQ = 0x58 , BSSGP_PDUT_PS_HO_REQUIRED = 0x59 , BSSGP_PDUT_PS_HO_REQUIRED_ACK = 0x5a , BSSGP_PDUT_PS_HO_REQUIRED_NACK = 0x5b , BSSGP_PDUT_PS_HO_REQUEST = 0x5c , BSSGP_PDUT_PS_HO_REQUEST_ACK = 0x5d , BSSGP_PDUT_PS_HO_REQUEST_NACK = 0x5e , BSSGP_PDUT_PS_HO_COMPLETE = 0x91 , BSSGP_PDUT_PS_HO_CANCEL = 0x92 , BSSGP_PDUT_PS_HO_COMPLETE_ACK = 0x93 , BSSGP_PDUT_PERFORM_LOC_REQ = 0x60 , BSSGP_PDUT_PERFORM_LOC_RESP = 0x61 , BSSGP_PDUT_PERFORM_LOC_ABORT = 0x62 , BSSGP_PDUT_POSITION_COMMAND = 0x63 , BSSGP_PDUT_POSITION_RESPONSE = 0x64 , BSSGP_PDUT_RAN_INFO = 0x70 , BSSGP_PDUT_RAN_INFO_REQ = 0x71 , BSSGP_PDUT_RAN_INFO_ACK = 0x72 , BSSGP_PDUT_RAN_INFO_ERROR = 0x73 , BSSGP_PDUT_RAN_INFO_APP_ERROR = 0x74 , BSSGP_PDUT_MBMS_START_REQ = 0x80 , BSSGP_PDUT_MBMS_START_RESP = 0x81 , BSSGP_PDUT_MBMS_STOP_REQ = 0x82 , BSSGP_PDUT_MBMS_STOP_RESP = 0x83 , BSSGP_PDUT_MBMS_UPDATE_REQ = 0x84 , BSSGP_PDUT_MBMS_UPDATE_RESP = 0x85 }
| BSSGP PDU types (Section 11.3.26 / Table 11.27) More...
enum | bssgp_iei_type { BSSGP_IE_ALIGNMENT = 0x00 , BSSGP_IE_BMAX_DEFAULT_MS = 0x01 , BSSGP_IE_BSS_AREA_ID = 0x02 , BSSGP_IE_BUCKET_LEAK_RATE = 0x03 , BSSGP_IE_BVCI = 0x04 , BSSGP_IE_BVC_BUCKET_SIZE = 0x05 , BSSGP_IE_BVC_MEASUREMENT = 0x06 , BSSGP_IE_CAUSE = 0x07 , BSSGP_IE_CELL_ID = 0x08 , BSSGP_IE_CHAN_NEEDED = 0x09 , BSSGP_IE_DRX_PARAMS = 0x0a , BSSGP_IE_EMLPP_PRIO = 0x0b , BSSGP_IE_FLUSH_ACTION = 0x0c , BSSGP_IE_IMSI = 0x0d , BSSGP_IE_LLC_PDU = 0x0e , BSSGP_IE_LLC_FRAMES_DISCARDED = 0x0f , BSSGP_IE_LOCATION_AREA = 0x10 , BSSGP_IE_MOBILE_ID = 0x11 , BSSGP_IE_MS_BUCKET_SIZE = 0x12 , BSSGP_IE_MS_RADIO_ACCESS_CAP = 0x13 , BSSGP_IE_OMC_ID = 0x14 , BSSGP_IE_PDU_IN_ERROR = 0x15 , BSSGP_IE_PDU_LIFETIME = 0x16 , BSSGP_IE_PRIORITY = 0x17 , BSSGP_IE_QOS_PROFILE = 0x18 , BSSGP_IE_RADIO_CAUSE = 0x19 , BSSGP_IE_RA_CAP_UPD_CAUSE = 0x1a , BSSGP_IE_ROUTEING_AREA = 0x1b , BSSGP_IE_R_DEFAULT_MS = 0x1c , BSSGP_IE_SUSPEND_REF_NR = 0x1d , BSSGP_IE_TAG = 0x1e , BSSGP_IE_TLLI = 0x1f , BSSGP_IE_TMSI = 0x20 , BSSGP_IE_TRACE_REFERENC = 0x21 , BSSGP_IE_TRACE_TYPE = 0x22 , BSSGP_IE_TRANSACTION_ID = 0x23 , BSSGP_IE_TRIGGER_ID = 0x24 , BSSGP_IE_NUM_OCT_AFF = 0x25 , BSSGP_IE_LSA_ID_LIST = 0x26 , BSSGP_IE_LSA_INFORMATION = 0x27 , BSSGP_IE_PACKET_FLOW_ID = 0x28 , BSSGP_IE_PACKET_FLOW_TIMER = 0x29 , BSSGP_IE_AGG_BSS_QOS_PROFILE = 0x3a , BSSGP_IE_FEATURE_BITMAP = 0x3b , BSSGP_IE_BUCKET_FULL_RATIO = 0x3c , BSSGP_IE_SERVICE_UTRAN_CCO = 0x3d , BSSGP_IE_NSEI = 0x3e , BSSGP_IE_RRLP_APDU = 0x3f , BSSGP_IE_LCS_QOS = 0x40 , BSSGP_IE_LCS_CLIENT_TYPE = 0x41 , BSSGP_IE_REQUESTED_GPS_AST_DATA = 0x42 , BSSGP_IE_LOCATION_TYPE = 0x43 , BSSGP_IE_LOCATION_ESTIMATE = 0x44 , BSSGP_IE_POSITIONING_DATA = 0x45 , BSSGP_IE_DECIPHERING_KEYS = 0x46 , BSSGP_IE_LCS_PRIORITY = 0x47 , BSSGP_IE_LCS_CAUSE = 0x48 , BSSGP_IE_LCS_CAPABILITY = 0x49 , BSSGP_IE_RRLP_FLAGS = 0x4a , BSSGP_IE_RIM_APP_IDENTITY = 0x4b , BSSGP_IE_RIM_SEQ_NR = 0x4c , BSSGP_IE_RIM_REQ_APP_CONTAINER = 0x4d , BSSGP_IE_RAN_INFO_APP_CONTAINER = 0x4e , BSSGP_IE_RIM_PDU_INDICATIONS = 0x4f , BSSGP_IE_PFC_FLOW_CTRL_PARAMS = 0x52 , BSSGP_IE_GLOBAL_CN_ID = 0x53 , BSSGP_IE_RIM_ROUTING_INFO = 0x54 , BSSGP_IE_RIM_PROTOCOL_VERSION = 0x55 , BSSGP_IE_APP_ERROR_CONTAINER = 0x56 , BSSGP_IE_RI_REQ_RIM_CONTAINER = 0x57 , BSSGP_IE_RI_RIM_CONTAINER = 0x58 , BSSGP_IE_RI_APP_ERROR_RIM_CONT = 0x59 , BSSGP_IE_RI_ACK_RIM_CONTAINER = 0x5a , BSSGP_IE_RI_ERROR_RIM_COINTAINER = 0x5b , BSSGP_IE_TMGI = 0x5c , BSSGP_IE_MBMS_SESSION_ID = 0x5d , BSSGP_IE_MBMS_SESSION_DURATION = 0x5e , BSSGP_IE_MBMS_SA_ID_LIST = 0x5f , BSSGP_IE_MBMS_RESPONSE = 0x60 , BSSGP_IE_MBMS_RA_LIST = 0x61 , BSSGP_IE_MBMS_SESSION_INFO = 0x62 , BSSGP_IE_MBMS_STOP_CAUSE = 0x63 , BSSGP_IE_SBSS_TO_TBSS_TR_CONT = 0x64 , BSSGP_IE_TBSS_TO_SBSS_TR_CONT = 0x65 , BSSGP_IE_NAS_CONT_FOR_PS_HO = 0x66 , BSSGP_IE_PFC_TO_BE_SETUP_LIST = 0x67 , BSSGP_IE_LIST_OF_SETUP_PFC = 0x68 , BSSGP_IE_EXT_FEATURE_BITMAP = 0x69 , BSSGP_IE_SRC_TO_TGT_TR_CONT = 0x6a , BSSGP_IE_TGT_TO_SRC_TR_CONT = 0x6b , BSSGP_IE_NC_ID = 0x6c , BSSGP_IE_PAGE_MODE = 0x6d , BSSGP_IE_CONTAINER_ID = 0x6e , BSSGP_IE_GLOBAL_TFI = 0x6f , BSSGP_IE_IMEI = 0x70 , BSSGP_IE_TIME_TO_MBMS_DATA_XFR = 0x71 , BSSGP_IE_MBMS_SESSION_REP_NR = 0x72 , BSSGP_IE_INTER_RAT_HO_INFO = 0x73 , BSSGP_IE_PS_HO_COMMAND = 0x74 , BSSGP_IE_PS_HO_INDICATIONS = 0x75 , BSSGP_IE_SI_PSI_CONTAINER = 0x76 , BSSGP_IE_ACTIVE_PFC_LIST = 0x77 , BSSGP_IE_VELOCITY_DATA = 0x78 , BSSGP_IE_DTM_HO_COMMAND = 0x79 , BSSGP_IE_CS_INDICATION = 0x7a , BSSGP_IE_RQD_GANNS_AST_DATA = 0x7b , BSSGP_IE_GANSS_LOCATION_TYPE = 0x7c , BSSGP_IE_GANSS_POSITIONING_DATA = 0x7d , BSSGP_IE_FLOW_CTRL_GRANULARITY = 0x7e , BSSGP_IE_ENB_ID = 0x7f , BSSGP_IE_EUTRAN_IRAT_HO_INFO = 0x80 , BSSGP_IE_SUB_PID4RAT_FREQ_PRIO = 0x81 , BSSGP_IE_REQ4IRAT_HO_INFO = 0x82 , BSSGP_IE_RELIABLE_IRAT_HO_INFO = 0x83 , BSSGP_IE_SON_TRANSFER_APP_ID = 0x84 , BSSGP_IE_CSG_ID = 0x85 , BSSGP_IE_TAC = 0x86 , BSSGP_IE_REDIRECT_ATTEMPT_FLAG = 0x87 , BSSGP_IE_REDIRECTION_INDICATION = 0x88 , BSSGP_IE_REDIRECTION_COMPLETED = 0x89 , BSSGP_IE_UNCONF_SEND_STATE_VAR = 0x8a , BSSGP_IE_IRAT_MEASUREMENT_CONF = 0x8b , BSSGP_IE_SCI = 0x8c , BSSGP_IE_GGSN_PGW_LOCATION = 0x8d , BSSGP_IE_SELECTED_PLMN_ID = 0x8e , BSSGP_IE_PRIO_CLASS_IND = 0x8f , BSSGP_IE_SOURCE_CELL_ID = 0x90 , BSSGP_IE_IRAT_MEAS_CFG_E_EARFCN = 0x91 , BSSGP_IE_EDRX_PARAMETERS = 0x92 , BSSGP_IE_T_UNTIL_NEXT_PAGING = 0x93 , BSSGP_IE_COVERAGE_CLASS = 0x98 , BSSGP_IE_PAGING_ATTEMPT_INFO = 0x99 , BSSGP_IE_EXCEPTION_REPORT_FLAG = 0x9a , BSSGP_IE_OLD_RA_ID = 0x9b , BSSGP_IE_ATTACH_IND = 0x9c , BSSGP_IE_PLMN_ID = 0x9d , BSSGP_IE_MME_QUERY = 0x9e , BSSGP_IE_SGSN_GROUP_ID = 0x9f , BSSGP_IE_ADDITIONAL_PTMSI = 0xa0 , BSSGP_IE_UE_USAGE_TYPE = 0xa1 , BSSGP_IE_MLAT_TIMER = 0xa2 , BSSGP_IE_MLAT_TA = 0xa3 , BSSGP_IE_MS_SYNC_ACCURACY = 0xa4 , BSSGP_IE_BTS_RX_ACCURACY_LVL = 0xa5 , BSSGP_IE_TA_REQ = 0xa6 }
| BSSGP Information Element Identifiers (Section 11.3 / Table 11.3) More...
enum | gprs_bssgp_cause { BSSGP_CAUSE_PROC_OVERLOAD = 0x00 , BSSGP_CAUSE_EQUIP_FAIL = 0x01 , BSSGP_CAUSE_TRASIT_NET_FAIL = 0x02 , BSSGP_CAUSE_CAPA_GREATER_0KPBS = 0x03 , BSSGP_CAUSE_UNKNOWN_MS = 0x04 , BSSGP_CAUSE_UNKNOWN_BVCI = 0x05 , BSSGP_CAUSE_CELL_TRAF_CONG = 0x06 , BSSGP_CAUSE_SGSN_CONG = 0x07 , BSSGP_CAUSE_OML_INTERV = 0x08 , BSSGP_CAUSE_BVCI_BLOCKED = 0x09 , BSSGP_CAUSE_PFC_CREATE_FAIL = 0x0a , BSSGP_CAUSE_PFC_PREEMPTED = 0x0b , BSSGP_CAUSE_ABQP_NOT_SUPP = 0x0c , BSSGP_CAUSE_SEM_INCORR_PDU = 0x20 , BSSGP_CAUSE_INV_MAND_INF = 0x21 , BSSGP_CAUSE_MISSING_MAND_IE = 0x22 , BSSGP_CAUSE_MISSING_COND_IE = 0x23 , BSSGP_CAUSE_UNEXP_COND_IE = 0x24 , BSSGP_CAUSE_COND_IE_ERR = 0x25 , BSSGP_CAUSE_PDU_INCOMP_STATE = 0x26 , BSSGP_CAUSE_PROTO_ERR_UNSPEC = 0x27 , BSSGP_CAUSE_PDU_INCOMP_FEAT = 0x28 , BSSGP_CAUSE_REQ_INFO_NOT_AVAIL = 0x29 , BSSGP_CAUSE_UNKN_DST = 0x2a , BSSGP_CAUSE_UNKN_RIM_AI = 0x2b , BSSGP_CAUSE_INVAL_CONT_UI = 0x2c , BSSGP_CAUSE_PFC_QUEUE = 0x2d , BSSGP_CAUSE_PFC_CREATED = 0x2e , BSSGP_CAUSE_T12_EXPIRY = 0x2f , BSSGP_CAUSE_MS_UNDER_PS_HO = 0x30 , BSSGP_CAUSE_UL_QUALITY = 0x31 , BSSGP_CAUSE_UL_STRENGTH = 0x32 , BSSGP_CAUSE_DL_QUALITY = 0x33 , BSSGP_CAUSE_DL_STRENGTH = 0x34 , BSSGP_CAUSE_DISTANCE = 0x35 , BSSGP_CAUSE_BETTER_CELL = 0x36 , BSSGP_CAUSE_TRAFFIC = 0x37 , BSSGP_CAUSE_MS_RADIO_LOSS = 0x38 , BSSGP_CAUSE_MS_BACK_OLD_CHAN = 0x39 , BSSGP_CAUSE_T13_EXPIRY = 0x3a , BSSGP_CAUSE_T14_EXPIRY = 0x3b , BSSGP_CAUSE_NOT_ALL_PFC = 0x3c , BSSGP_CAUSE_CS = 0x3d , BSSGP_CAUSE_REQ_ALG_NOT_SUPP = 0x3e , BSSGP_CAUSE_RELOC_FAIL = 0x3f , BSSGP_CAUSE_DIR_RETRY = 0x40 , BSSGP_CAUSE_TIME_CRIT_RELOC = 0x41 , BSSGP_CAUSE_PS_HO_TARG_NA = 0x42 , BSSGP_CAUSE_PS_HO_TARG_NOT_SUPP = 0x43 , BSSGP_CAUSE_PUESBINE = 0x44 , BSSGP_CAUSE_DTM_HO_NO_CS_RES = 0x45 , BSSGP_CAUSE_DTM_HO_PS_ALLOC_FAIL = 0x46 , BSSGP_CAUSE_DTM_HO_T24_EXPIRY = 0x47 , BSSGP_CAUSE_DTM_HO_INVAL_CS_IND = 0x48 , BSSGP_CAUSE_DTM_HO_T23_EXPIRY = 0x49 , BSSGP_CAUSE_DTM_HO_MSC_ERR = 0x4a , BSSGP_CAUSE_INVAL_CSG_CELL = 0x4b }
| Cause coding (Section 11.3.8 / Table 11.10) More...
enum | bssgp_fc_granularity { BSSGP_FC_GRAN_100 = 0 , BSSGP_FC_GRAN_1000 = 1 , BSSGP_FC_GRAN_10000 = 2 , BSSGP_FC_GRAN_100000 = 3 }
enum | bssgp_rim_pdu_type { RIM_PDU_TYPE_STOP = 0 , RIM_PDU_TYPE_SING_REP = 1 , RIM_PDU_TYPE_MULT_REP = 2 }

## Functions
struct bssgp_ud_hdr | __attribute__ ((packed))

## Variables
uint8_t | pdu_type
| BSSGP PDU type. More...
uint32_t | tlli
| Temporary Link-Local Identifier. More...
uint8_t | qos_profile [3]
| QoS profile. More...
uint8_t | data [0]
struct bssgp_normal_hdr | __attribute__

## Macro Definition Documentation

## ◆ BSSGP_FEAT_CBL

#define BSSGP_FEAT_CBL 0x02 /* Current Bucket Level */

## ◆ BSSGP_FEAT_ERS

#define BSSGP_FEAT_ERS 0x40 /* Enhanced Radio Status */

## ◆ BSSGP_FEAT_INR

#define BSSGP_FEAT_INR 0x04 /* Inter-NSE re-routing */

## ◆ BSSGP_FEAT_LCS

#define BSSGP_FEAT_LCS 0x08 /* Location Services */

## ◆ BSSGP_FEAT_MBMS

#define BSSGP_FEAT_MBMS 0x80 /* Multimedia Broadcast */

## ◆ BSSGP_FEAT_PFC

#define BSSGP_FEAT_PFC 0x01 /* Packet Flow Context */

## ◆ BSSGP_FEAT_PFC_FC

#define BSSGP_FEAT_PFC_FC 0x20 /* PFC Flow Control */

## ◆ BSSGP_FEAT_RIM

#define BSSGP_FEAT_RIM 0x10 /* RAN Inoformation Management */

## ◆ BSSGP_PDUT_RA_CAPA_UDPATE

#define BSSGP_PDUT_RA_CAPA_UDPATE BSSGP_PDUT_RA_CAPA_UPDATE

## ◆ BSSGP_XFEAT_CSPS

#define BSSGP_XFEAT_CSPS 0x08 /* CS/PS coordination enhancements */

## ◆ BSSGP_XFEAT_DCN

#define BSSGP_XFEAT_DCN 0x20 /* Dedicated CN */

## ◆ BSSGP_XFEAT_ECIoT

#define BSSGP_XFEAT_ECIoT 0x10 /* EC-GSM-IoT */

## ◆ BSSGP_XFEAT_eDRX

#define BSSGP_XFEAT_eDRX 0x40 /* eDRX */

## ◆ BSSGP_XFEAT_GBIT

#define BSSGP_XFEAT_GBIT 0x02 /* Gigabit Interface */

## ◆ BSSGP_XFEAT_MOCN

#define BSSGP_XFEAT_MOCN 0x04 /* Multi-Operator CN */

## ◆ BSSGP_XFEAT_MSAD

#define BSSGP_XFEAT_MSAD 0x80 /* MS-assisted Dedicated CN selection */

## ◆ BSSGP_XFEAT_PSHO

#define BSSGP_XFEAT_PSHO 0x01 /* PS Handover */

## ◆ BVCI_PTM

#define BVCI_PTM 0x0001

## ◆ BVCI_SIGNALLING

#define BVCI_SIGNALLING 0x0000

Fixed BVCI definitions (Section 5.4.1)

## Enumeration Type Documentation

## ◆ bssgp_fc_granularity

enum bssgp_fc_granularity

Enumerator
BSSGP_FC_GRAN_100 |
BSSGP_FC_GRAN_1000 |
BSSGP_FC_GRAN_10000 |
BSSGP_FC_GRAN_100000 |

## ◆ bssgp_iei_type

enum bssgp_iei_type

BSSGP Information Element Identifiers (Section 11.3 / Table 11.3)

Enumerator
BSSGP_IE_ALIGNMENT |
BSSGP_IE_BMAX_DEFAULT_MS |
BSSGP_IE_BSS_AREA_ID |
BSSGP_IE_BUCKET_LEAK_RATE |
BSSGP_IE_BVCI |
BSSGP_IE_BVC_BUCKET_SIZE |
BSSGP_IE_BVC_MEASUREMENT |
BSSGP_IE_CAUSE |
BSSGP_IE_CELL_ID |
BSSGP_IE_CHAN_NEEDED |
BSSGP_IE_DRX_PARAMS |
BSSGP_IE_EMLPP_PRIO |
BSSGP_IE_FLUSH_ACTION |
BSSGP_IE_IMSI |
BSSGP_IE_LLC_PDU |
BSSGP_IE_LLC_FRAMES_DISCARDED |
BSSGP_IE_LOCATION_AREA |
BSSGP_IE_MOBILE_ID |
BSSGP_IE_MS_BUCKET_SIZE |
BSSGP_IE_MS_RADIO_ACCESS_CAP |
BSSGP_IE_OMC_ID |
BSSGP_IE_PDU_IN_ERROR |
BSSGP_IE_PDU_LIFETIME |
BSSGP_IE_PRIORITY |
BSSGP_IE_QOS_PROFILE |
BSSGP_IE_RADIO_CAUSE |
BSSGP_IE_RA_CAP_UPD_CAUSE |
BSSGP_IE_ROUTEING_AREA |
BSSGP_IE_R_DEFAULT_MS |
BSSGP_IE_SUSPEND_REF_NR |
BSSGP_IE_TAG |
BSSGP_IE_TLLI |
BSSGP_IE_TMSI |
BSSGP_IE_TRACE_REFERENC |
BSSGP_IE_TRACE_TYPE |
BSSGP_IE_TRANSACTION_ID |
BSSGP_IE_TRIGGER_ID |
BSSGP_IE_NUM_OCT_AFF |
BSSGP_IE_LSA_ID_LIST |
BSSGP_IE_LSA_INFORMATION |
BSSGP_IE_PACKET_FLOW_ID |
BSSGP_IE_PACKET_FLOW_TIMER |
BSSGP_IE_AGG_BSS_QOS_PROFILE |
BSSGP_IE_FEATURE_BITMAP |
BSSGP_IE_BUCKET_FULL_RATIO |
BSSGP_IE_SERVICE_UTRAN_CCO |
BSSGP_IE_NSEI |
BSSGP_IE_RRLP_APDU |
BSSGP_IE_LCS_QOS |
BSSGP_IE_LCS_CLIENT_TYPE |
BSSGP_IE_REQUESTED_GPS_AST_DATA |
BSSGP_IE_LOCATION_TYPE |
BSSGP_IE_LOCATION_ESTIMATE |
BSSGP_IE_POSITIONING_DATA |
BSSGP_IE_DECIPHERING_KEYS |
BSSGP_IE_LCS_PRIORITY |
BSSGP_IE_LCS_CAUSE |
BSSGP_IE_LCS_CAPABILITY |
BSSGP_IE_RRLP_FLAGS |
BSSGP_IE_RIM_APP_IDENTITY |
BSSGP_IE_RIM_SEQ_NR |
BSSGP_IE_RIM_REQ_APP_CONTAINER |
BSSGP_IE_RAN_INFO_APP_CONTAINER |
BSSGP_IE_RIM_PDU_INDICATIONS |
BSSGP_IE_PFC_FLOW_CTRL_PARAMS |
BSSGP_IE_GLOBAL_CN_ID |
BSSGP_IE_RIM_ROUTING_INFO |
BSSGP_IE_RIM_PROTOCOL_VERSION |
BSSGP_IE_APP_ERROR_CONTAINER |
BSSGP_IE_RI_REQ_RIM_CONTAINER |
BSSGP_IE_RI_RIM_CONTAINER |
BSSGP_IE_RI_APP_ERROR_RIM_CONT |
BSSGP_IE_RI_ACK_RIM_CONTAINER |
BSSGP_IE_RI_ERROR_RIM_COINTAINER |
BSSGP_IE_TMGI |
BSSGP_IE_MBMS_SESSION_ID |
BSSGP_IE_MBMS_SESSION_DURATION |
BSSGP_IE_MBMS_SA_ID_LIST |
BSSGP_IE_MBMS_RESPONSE |
BSSGP_IE_MBMS_RA_LIST |
BSSGP_IE_MBMS_SESSION_INFO |
BSSGP_IE_MBMS_STOP_CAUSE |
BSSGP_IE_SBSS_TO_TBSS_TR_CONT |
BSSGP_IE_TBSS_TO_SBSS_TR_CONT |
BSSGP_IE_NAS_CONT_FOR_PS_HO |
BSSGP_IE_PFC_TO_BE_SETUP_LIST |
BSSGP_IE_LIST_OF_SETUP_PFC |
BSSGP_IE_EXT_FEATURE_BITMAP |
BSSGP_IE_SRC_TO_TGT_TR_CONT |
BSSGP_IE_TGT_TO_SRC_TR_CONT |
BSSGP_IE_NC_ID |
BSSGP_IE_PAGE_MODE |
BSSGP_IE_CONTAINER_ID |
BSSGP_IE_GLOBAL_TFI |
BSSGP_IE_IMEI |
BSSGP_IE_TIME_TO_MBMS_DATA_XFR |
BSSGP_IE_MBMS_SESSION_REP_NR |
BSSGP_IE_INTER_RAT_HO_INFO |
BSSGP_IE_PS_HO_COMMAND |
BSSGP_IE_PS_HO_INDICATIONS |
BSSGP_IE_SI_PSI_CONTAINER |
BSSGP_IE_ACTIVE_PFC_LIST |
BSSGP_IE_VELOCITY_DATA |
BSSGP_IE_DTM_HO_COMMAND |
BSSGP_IE_CS_INDICATION |
BSSGP_IE_RQD_GANNS_AST_DATA |
BSSGP_IE_GANSS_LOCATION_TYPE |
BSSGP_IE_GANSS_POSITIONING_DATA |
BSSGP_IE_FLOW_CTRL_GRANULARITY |
BSSGP_IE_ENB_ID |
BSSGP_IE_EUTRAN_IRAT_HO_INFO |
BSSGP_IE_SUB_PID4RAT_FREQ_PRIO |
BSSGP_IE_REQ4IRAT_HO_INFO |
BSSGP_IE_RELIABLE_IRAT_HO_INFO |
BSSGP_IE_SON_TRANSFER_APP_ID |
BSSGP_IE_CSG_ID |
BSSGP_IE_TAC |
BSSGP_IE_REDIRECT_ATTEMPT_FLAG |
BSSGP_IE_REDIRECTION_INDICATION |
BSSGP_IE_REDIRECTION_COMPLETED |
BSSGP_IE_UNCONF_SEND_STATE_VAR |
BSSGP_IE_IRAT_MEASUREMENT_CONF |
BSSGP_IE_SCI |
BSSGP_IE_GGSN_PGW_LOCATION |
BSSGP_IE_SELECTED_PLMN_ID |
BSSGP_IE_PRIO_CLASS_IND |
BSSGP_IE_SOURCE_CELL_ID |
BSSGP_IE_IRAT_MEAS_CFG_E_EARFCN |
BSSGP_IE_EDRX_PARAMETERS |
BSSGP_IE_T_UNTIL_NEXT_PAGING |
BSSGP_IE_COVERAGE_CLASS |
BSSGP_IE_PAGING_ATTEMPT_INFO |
BSSGP_IE_EXCEPTION_REPORT_FLAG |
BSSGP_IE_OLD_RA_ID |
BSSGP_IE_ATTACH_IND |
BSSGP_IE_PLMN_ID |
BSSGP_IE_MME_QUERY |
BSSGP_IE_SGSN_GROUP_ID |
BSSGP_IE_ADDITIONAL_PTMSI |
BSSGP_IE_UE_USAGE_TYPE |
BSSGP_IE_MLAT_TIMER |
BSSGP_IE_MLAT_TA |
BSSGP_IE_MS_SYNC_ACCURACY |
BSSGP_IE_BTS_RX_ACCURACY_LVL |
BSSGP_IE_TA_REQ |

## ◆ bssgp_pdu_type

enum bssgp_pdu_type

BSSGP PDU types (Section 11.3.26 / Table 11.27)

Enumerator
BSSGP_PDUT_DL_UNITDATA |
BSSGP_PDUT_UL_UNITDATA |
BSSGP_PDUT_RA_CAPABILITY |
BSSGP_PDUT_PTM_UNITDATA |
BSSGP_PDUT_DL_MMBS_UNITDATA |
BSSGP_PDUT_UL_MMBS_UNITDATA |
BSSGP_PDUT_PAGING_PS |
BSSGP_PDUT_PAGING_CS |
BSSGP_PDUT_RA_CAPA_UPDATE |
BSSGP_PDUT_RA_CAPA_UPDATE_ACK |
BSSGP_PDUT_RADIO_STATUS |
BSSGP_PDUT_SUSPEND |
BSSGP_PDUT_SUSPEND_ACK |
BSSGP_PDUT_SUSPEND_NACK |
BSSGP_PDUT_RESUME |
BSSGP_PDUT_RESUME_ACK |
BSSGP_PDUT_RESUME_NACK |
BSSGP_PDUT_PAGING_PS_REJECT |
BSSGP_PDUT_DUMMY_PAGING_PS |
BSSGP_PDUT_DUMMY_PAGING_PS_RESP |
BSSGP_PDUT_MS_REGISTR_ENQ |
BSSGP_PDUT_MS_REGISTR_ENQ_RESP |
BSSGP_PDUT_BVC_BLOCK |
BSSGP_PDUT_BVC_BLOCK_ACK |
BSSGP_PDUT_BVC_RESET |
BSSGP_PDUT_BVC_RESET_ACK |
BSSGP_PDUT_BVC_UNBLOCK |
BSSGP_PDUT_BVC_UNBLOCK_ACK |
BSSGP_PDUT_FLOW_CONTROL_BVC |
BSSGP_PDUT_FLOW_CONTROL_BVC_ACK |
BSSGP_PDUT_FLOW_CONTROL_MS |
BSSGP_PDUT_FLOW_CONTROL_MS_ACK |
BSSGP_PDUT_FLUSH_LL |
BSSGP_PDUT_FLUSH_LL_ACK |
BSSGP_PDUT_LLC_DISCARD |
BSSGP_PDUT_FLOW_CONTROL_PFC |
BSSGP_PDUT_FLOW_CONTROL_PFC_ACK |
BSSGP_PDUT_SGSN_INVOKE_TRACE |
BSSGP_PDUT_STATUS |
BSSGP_PDUT_OVERLOAD |
BSSGP_PDUT_DOWNLOAD_BSS_PFC |
BSSGP_PDUT_CREATE_BSS_PFC |
BSSGP_PDUT_CREATE_BSS_PFC_ACK |
BSSGP_PDUT_CREATE_BSS_PFC_NACK |
BSSGP_PDUT_MODIFY_BSS_PFC |
BSSGP_PDUT_MODIFY_BSS_PFC_ACK |
BSSGP_PDUT_DELETE_BSS_PFC |
BSSGP_PDUT_DELETE_BSS_PFC_ACK |
BSSGP_PDUT_DELETE_BSS_PFC_REQ |
BSSGP_PDUT_PS_HO_REQUIRED |
BSSGP_PDUT_PS_HO_REQUIRED_ACK |
BSSGP_PDUT_PS_HO_REQUIRED_NACK |
BSSGP_PDUT_PS_HO_REQUEST |
BSSGP_PDUT_PS_HO_REQUEST_ACK |
BSSGP_PDUT_PS_HO_REQUEST_NACK |
BSSGP_PDUT_PS_HO_COMPLETE |
BSSGP_PDUT_PS_HO_CANCEL |
BSSGP_PDUT_PS_HO_COMPLETE_ACK |
BSSGP_PDUT_PERFORM_LOC_REQ |
BSSGP_PDUT_PERFORM_LOC_RESP |
BSSGP_PDUT_PERFORM_LOC_ABORT |
BSSGP_PDUT_POSITION_COMMAND |
BSSGP_PDUT_POSITION_RESPONSE |
BSSGP_PDUT_RAN_INFO |
BSSGP_PDUT_RAN_INFO_REQ |
BSSGP_PDUT_RAN_INFO_ACK |
BSSGP_PDUT_RAN_INFO_ERROR |
BSSGP_PDUT_RAN_INFO_APP_ERROR |
BSSGP_PDUT_MBMS_START_REQ |
BSSGP_PDUT_MBMS_START_RESP |
BSSGP_PDUT_MBMS_STOP_REQ |
BSSGP_PDUT_MBMS_STOP_RESP |
BSSGP_PDUT_MBMS_UPDATE_REQ |
BSSGP_PDUT_MBMS_UPDATE_RESP |

## ◆ bssgp_rim_pdu_type

enum bssgp_rim_pdu_type

Enumerator
RIM_PDU_TYPE_STOP |
RIM_PDU_TYPE_SING_REP |
RIM_PDU_TYPE_MULT_REP |

## ◆ gprs_bssgp_cause

enum gprs_bssgp_cause

Cause coding (Section 11.3.8 / Table 11.10)

Enumerator
BSSGP_CAUSE_PROC_OVERLOAD |
BSSGP_CAUSE_EQUIP_FAIL |
BSSGP_CAUSE_TRASIT_NET_FAIL |
BSSGP_CAUSE_CAPA_GREATER_0KPBS |
BSSGP_CAUSE_UNKNOWN_MS |
BSSGP_CAUSE_UNKNOWN_BVCI |
BSSGP_CAUSE_CELL_TRAF_CONG |
BSSGP_CAUSE_SGSN_CONG |
BSSGP_CAUSE_OML_INTERV |
BSSGP_CAUSE_BVCI_BLOCKED |
BSSGP_CAUSE_PFC_CREATE_FAIL |
BSSGP_CAUSE_PFC_PREEMPTED |
BSSGP_CAUSE_ABQP_NOT_SUPP |
BSSGP_CAUSE_SEM_INCORR_PDU |
BSSGP_CAUSE_INV_MAND_INF |
BSSGP_CAUSE_MISSING_MAND_IE |
BSSGP_CAUSE_MISSING_COND_IE |
BSSGP_CAUSE_UNEXP_COND_IE |
BSSGP_CAUSE_COND_IE_ERR |
BSSGP_CAUSE_PDU_INCOMP_STATE |
BSSGP_CAUSE_PROTO_ERR_UNSPEC |
BSSGP_CAUSE_PDU_INCOMP_FEAT |
BSSGP_CAUSE_REQ_INFO_NOT_AVAIL |
BSSGP_CAUSE_UNKN_DST |
BSSGP_CAUSE_UNKN_RIM_AI |
BSSGP_CAUSE_INVAL_CONT_UI |
BSSGP_CAUSE_PFC_QUEUE |
BSSGP_CAUSE_PFC_CREATED |
BSSGP_CAUSE_T12_EXPIRY |
BSSGP_CAUSE_MS_UNDER_PS_HO |
BSSGP_CAUSE_UL_QUALITY |
BSSGP_CAUSE_UL_STRENGTH |
BSSGP_CAUSE_DL_QUALITY |
BSSGP_CAUSE_DL_STRENGTH |
BSSGP_CAUSE_DISTANCE |
BSSGP_CAUSE_BETTER_CELL |
BSSGP_CAUSE_TRAFFIC |
BSSGP_CAUSE_MS_RADIO_LOSS |
BSSGP_CAUSE_MS_BACK_OLD_CHAN |
BSSGP_CAUSE_T13_EXPIRY |
BSSGP_CAUSE_T14_EXPIRY |
BSSGP_CAUSE_NOT_ALL_PFC |
BSSGP_CAUSE_CS |
BSSGP_CAUSE_REQ_ALG_NOT_SUPP |
BSSGP_CAUSE_RELOC_FAIL |
BSSGP_CAUSE_DIR_RETRY |
BSSGP_CAUSE_TIME_CRIT_RELOC |
BSSGP_CAUSE_PS_HO_TARG_NA |
BSSGP_CAUSE_PS_HO_TARG_NOT_SUPP |
BSSGP_CAUSE_PUESBINE |
BSSGP_CAUSE_DTM_HO_NO_CS_RES |
BSSGP_CAUSE_DTM_HO_PS_ALLOC_FAIL |
BSSGP_CAUSE_DTM_HO_T24_EXPIRY |
BSSGP_CAUSE_DTM_HO_INVAL_CS_IND |
BSSGP_CAUSE_DTM_HO_T23_EXPIRY |
BSSGP_CAUSE_DTM_HO_MSC_ERR |
BSSGP_CAUSE_INVAL_CSG_CELL |

## Variable Documentation

## ◆ __attribute__

struct bssgp_normal_hdr __attribute__

## ◆ data

uint8_t data[0]

## ◆ pdu_type

uint8_t pdu_type

BSSGP PDU type.

## ◆ qos_profile

uint8_t qos_profile[3]

QoS profile.

Referenced by bssgp_tx_ul_ud().

## ◆ tlli

uint32_t tlli

Temporary Link-Local Identifier.