libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Structures | Macros | Enumerations | Functions | Variables
gsm_08_58.h File Reference
A-bis RSL

GSM Radio Signalling Link messages on the A-bis interface. More...

`#include <stdint.h>`
`#include <osmocom/core/endian.h>`

Go to the source code of this file.

## Data Structures
union | abis_rsl_chan_nr
union | abis_rsl_link_id
struct | abis_rsl_common_hdr
| RSL common header. More...
struct | abis_rsl_rll_hdr
struct | abis_rsl_dchan_hdr
struct | abis_rsl_cchan_hdr
struct | abis_rsl_osmo_rep_acch_cap
struct | abis_rsl_osmo_temp_ovp_acch_cap
struct | rsl_ie_chan_mode
| RSL Channel Mode IF (Chapter 9.3.6) More...
struct | rsl_ie_chan_ident
| RSL Channel Identification IE (Chapter 9.3.5) More...
struct | rsl_ie_cb_cmd_type
| RSL Cell Broadcast Command (Chapter 9.3.41) More...
struct | rsl_ie_nch_drx_info
| NCH DRX Information (Chapter 9.3.47) More...
struct | rsl_mrpci
struct | ipac_preproc_ave_cfg
struct | osmo_preproc_ave_cfg_field
struct | osmo_preproc_ave_cfg
struct | ipac_preproc_pc_thresh
| MS/BS Power Control Thresholds (RSL_IPAC_EIE_MS_PWR_CTL) More...
struct | osmo_preproc_pc_thresh
| Osmocom extension for: MS/BS Power Control Thresholds (RSL_IPAC_EIE_OSMO_MS_PWR_CTL) More...
struct | ipac_preproc_ho_thresh
| Handover Thresholds. More...
struct | ipac_preproc_pc_comp
| PC Threshold Comparators (RSL_IPAC_EIE_PC_THRESH_COMP) More...
struct | ipac_preproc_pc_comp_field
| Osmocom extension for: PC Threshold Comparators (RSL_IPAC_EIE_OSMO_PC_THRESH_COMP) More...
struct | osmo_preproc_pc_comp
struct | ipac_preproc_ho_comp
| HO Threshold Comparators. More...
struct | ipac_preproc_ho_candidates
struct | ipac_preproc_ncell_dflts
struct | ipac_preproc_ho_ctl_param
struct | ipac_preproc_cfg
struct | rsl_l1_info

## Macros
#define | ABIS_RSL_CHAN_NR_CBITS_Bm_ACCHs 0x01
#define | ABIS_RSL_CHAN_NR_CBITS_Lm_ACCHs(ss) (0x02 + (ss))
#define | ABIS_RSL_CHAN_NR_CBITS_SDCCH4_ACCH(ss) (0x04 + (ss))
#define | ABIS_RSL_CHAN_NR_CBITS_SDCCH8_ACCH(ss) (0x08 + (ss))
#define | ABIS_RSL_CHAN_NR_CBITS_BCCH 0x10
#define | ABIS_RSL_CHAN_NR_CBITS_RACH 0x11
#define | ABIS_RSL_CHAN_NR_CBITS_PCH_AGCH 0x12
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_PDCH 0x18 /*< non-standard, for dyn TS */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH4 0x19 /*< non-standard, for CBCH/SDCCH4 */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_CBCH8 0x1a /*< non-standard, for CBCH/SDCCH8 */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Bm_ACCHs 0x1d /*< VAMOS TCH/F */
#define | ABIS_RSL_CHAN_NR_CBITS_OSMO_VAMOS_Lm_ACCHs(ss) (0x1e + (ss)) /*< VAMOS TCH/H */
#define | ABIS_RSL_LINK_ID_CBITS_FACCH_SDCCH 0x00
#define | ABIS_RSL_LINK_ID_CBITS_SACCH 0x01
#define | ABIS_RSL_MDISC_RLL 0x02
#define | ABIS_RSL_MDISC_DED_CHAN 0x08
#define | ABIS_RSL_MDISC_COM_CHAN 0x0c
#define | ABIS_RSL_MDISC_TRX 0x10
#define | ABIS_RSL_MDISC_LOC 0x20
#define | ABIS_RSL_MDISC_IPACCESS 0x7e
#define | ABIS_RSL_MDISC_TRANSP 0x01
#define | ABIS_RSL_MDISC_IS_TRANSP(x) (x & 0x01)
#define | RSL_IE_ERIC_PAGING_GROUP 0x0e
#define | RSL_IE_ERIC_INST_NR 0x48
#define | RSL_IE_ERIC_PGSL_TIMERS 0x49
#define | RSL_IE_ERIC_REPEAT_DL_FACCH 0x4a
#define | RSL_IE_ERIC_POWER_INFO 0xf0
#define | RSL_IE_ERIC_MOBILE_ID 0xf1
#define | RSL_IE_ERIC_BCCH_MAPPING 0xf2
#define | RSL_IE_ERIC_PACKET_PAG_IND 0xf3
#define | RSL_IE_ERIC_CNTR_CTRL 0xf4
#define | RSL_IE_ERIC_CNTR_CTRL_ACK 0xf5
#define | RSL_IE_ERIC_CNTR_REPORT 0xf6
#define | RSL_IE_ERIC_ICP_CONN 0xf7
#define | RSL_IE_ERIC_EMR_SUPPORT 0xf8
#define | RSL_IE_ERIC_EGPRS_REQ_REF 0xf9
#define | RSL_IE_ERIC_VGCS_REL 0xfa
#define | RSL_IE_ERIC_REP_PER_NCH 0xfb
#define | RSL_IE_ERIC_NY2 0xfc
#define | RSL_IE_ERIC_T3115 0xfd
#define | RSL_IE_ERIC_ACTIVATE_FLAG 0xfe
#define | RSL_IE_ERIC_FULL_NCH_INFO 0xff
#define | RSL_CHAN_NR_MASK 0xf8
#define | RSL_CHAN_NR_1 0x08 /*< bit to add for 2nd,... lchan */
#define | RSL_CHAN_Bm_ACCHs 0x08
#define | RSL_CHAN_Lm_ACCHs 0x10 /* .. 0x18 */
#define | RSL_CHAN_SDCCH4_ACCH 0x20 /* .. 0x38 */
#define | RSL_CHAN_SDCCH8_ACCH 0x40 /* ...0x78 */
#define | RSL_CHAN_BCCH 0x80
#define | RSL_CHAN_RACH 0x88
#define | RSL_CHAN_PCH_AGCH 0x90
#define | RSL_CHAN_OSMO_PDCH 0xc0 /*< non-standard, for dyn TS */
#define | RSL_CHAN_OSMO_CBCH4 0xc8 /*< non-standard, for CBCH/SDCCH4 */
#define | RSL_CHAN_OSMO_CBCH8 0xd0 /*< non-standard, for CBCH/SDCCH8 */
#define | RSL_CHAN_OSMO_VAMOS_Bm_ACCHs 0xe8 /* VAMOS TCH/F */
#define | RSL_CHAN_OSMO_VAMOS_Lm_ACCHs 0xf0 /* VAMOS TCH/H */
#define | RSL_CHAN_OSMO_VAMOS_MASK 0xe0 /* VAMOS TCH/{F,H} */
#define | RSL_ACT_TYPE_INITIAL 0x00
#define | RSL_ACT_TYPE_REACT 0x80
#define | RSL_ACT_INTRA_IMM_ASS 0x00
#define | RSL_ACT_INTRA_NORM_ASS 0x01
#define | RSL_ACT_INTER_ASYNC 0x02
#define | RSL_ACT_INTER_SYNC 0x03
#define | RSL_ACT_SECOND_ADD 0x04
#define | RSL_ACT_SECOND_MULTI 0x05
#define | RSL_ACT_OSMO_PDCH 0x0f /*< non-standard, for dyn TS */
#define | RSL_CMOD_DTXu 0x01 /* uplink */
#define | RSL_CMOD_DTXd 0x02 /* downlink */
#define | RSL_CMOD_SP_NT_14k5 RSL_CMOD_CSD_NT_14k5
#define | RSL_CMOD_SP_NT_12k0 RSL_CMOD_CSD_NT_12k0
#define | RSL_CMOD_SP_NT_6k0 RSL_CMOD_CSD_NT_6k0
#define | RSL_CMOD_CSD_T_32000 RSL_CMOD_CSD_T_32k0
#define | RSL_CMOD_CSD_T_29000 RSL_CMOD_CSD_T_29k0
#define | RSL_CMOD_CSD_T_14400 RSL_CMOD_CSD_T_14k4
#define | RSL_CMOD_CSD_T_9600 RSL_CMOD_CSD_T_9k6
#define | RSL_CMOD_CSD_T_4800 RSL_CMOD_CSD_T_4k8
#define | RSL_CMOD_CSD_T_2400 RSL_CMOD_CSD_T_2k4
#define | RSL_CMOD_CSD_T_1200 RSL_CMOD_CSD_T_1k2
#define | RLL_CAUSE_T200_EXPIRED 0x01
#define | RLL_CAUSE_REEST_REQ 0x02
#define | RLL_CAUSE_UNSOL_UA_RESP 0x03
#define | RLL_CAUSE_UNSOL_DM_RESP 0x04
#define | RLL_CAUSE_UNSOL_DM_RESP_MF 0x05
#define | RLL_CAUSE_UNSOL_SPRV_RESP 0x06
#define | RLL_CAUSE_SEQ_ERR 0x07
#define | RLL_CAUSE_UFRM_INC_PARAM 0x08
#define | RLL_CAUSE_SFRM_INC_PARAM 0x09
#define | RLL_CAUSE_IFRM_INC_MBITS 0x0a
#define | RLL_CAUSE_IFRM_INC_LEN 0x0b
#define | RLL_CAUSE_FRM_UNIMPL 0x0c
#define | RLL_CAUSE_SABM_MF 0x0d
#define | RLL_CAUSE_SABM_INFO_NOTALL 0x0e
#define | RSL_ERRCLS_NORMAL 0x00
#define | RSL_ERRCLS_RESOURCE_UNAVAIL 0x20
#define | RSL_ERRCLS_SERVICE_UNAVAIL 0x30
#define | RSL_ERRCLS_SERVICE_UNIMPL 0x40
#define | RSL_ERRCLS_INVAL_MSG 0x50
#define | RSL_ERRCLS_PROTO_ERROR 0x60
#define | RSL_ERRCLS_INTERWORKING 0x70
#define | RSL_ERR_RADIO_IF_FAIL 0x00
#define | RSL_ERR_RADIO_LINK_FAIL 0x01
#define | RSL_ERR_HANDOVER_ACC_FAIL 0x02
#define | RSL_ERR_TALKER_ACC_FAIL 0x03
#define | RSL_ERR_OM_INTERVENTION 0x07
#define | RSL_ERR_NORMAL_UNSPEC 0x0f
#define | RSL_ERR_T_MSRFPCI_EXP 0x18
#define | RSL_ERR_EQUIPMENT_FAIL 0x20
#define | RSL_ERR_RR_UNAVAIL 0x21
#define | RSL_ERR_TERR_CH_FAIL 0x22
#define | RSL_ERR_CCCH_OVERLOAD 0x23
#define | RSL_ERR_ACCH_OVERLOAD 0x24
#define | RSL_ERR_PROCESSOR_OVERLOAD 0x25
#define | RSL_ERR_BTS_NOT_EQUIPPED 0x27
#define | RSL_ERR_REMOTE_TRANSC_FAIL 0x28
#define | RSL_ERR_NOTIFICATION_OVERFL 0x29
#define | RSL_ERR_RES_UNAVAIL 0x2f
#define | RSL_ERR_TRANSC_UNAVAIL 0x30
#define | RSL_ERR_SERV_OPT_UNAVAIL 0x3f
#define | RSL_ERR_ENCR_UNIMPL 0x40
#define | RSL_ERR_SERV_OPT_UNIMPL 0x4f
#define | RSL_ERR_RCH_ALR_ACTV_ALLOC 0x50
#define | RSL_ERR_INVALID_MESSAGE 0x5f
#define | RSL_ERR_MSG_DISCR 0x60
#define | RSL_ERR_MSG_TYPE 0x61
#define | RSL_ERR_MSG_SEQ 0x62
#define | RSL_ERR_IE_ERROR 0x63
#define | RSL_ERR_MAND_IE_ERROR 0x64
#define | RSL_ERR_OPT_IE_ERROR 0x65
#define | RSL_ERR_IE_NONEXIST 0x66
#define | RSL_ERR_IE_LENGTH 0x67
#define | RSL_ERR_IE_CONTENT 0x68
#define | RSL_ERR_PROTO 0x6f
#define | RSL_ERR_INTERWORKING 0x7f
#define | RSL_SYSTEM_INFO_8 0x00
#define | RSL_SYSTEM_INFO_1 0x01
#define | RSL_SYSTEM_INFO_2 0x02
#define | RSL_SYSTEM_INFO_3 0x03
#define | RSL_SYSTEM_INFO_4 0x04
#define | RSL_SYSTEM_INFO_5 0x05
#define | RSL_SYSTEM_INFO_6 0x06
#define | RSL_SYSTEM_INFO_7 0x07
#define | RSL_SYSTEM_INFO_16 0x08
#define | RSL_SYSTEM_INFO_17 0x09
#define | RSL_SYSTEM_INFO_2bis 0x0a
#define | RSL_SYSTEM_INFO_2ter 0x0b
#define | RSL_SYSTEM_INFO_5bis 0x0d
#define | RSL_SYSTEM_INFO_5ter 0x0e
#define | RSL_SYSTEM_INFO_10 0x0f
#define | RSL_EXT_MEAS_ORDER 0x47
#define | RSL_MEAS_INFO 0x48
#define | RSL_SYSTEM_INFO_13 0x28
#define | RSL_ERIC_SYSTEM_INFO_13 0x0C
#define | RSL_SYSTEM_INFO_2quater 0x29
#define | RSL_SYSTEM_INFO_9 0x2a
#define | RSL_SYSTEM_INFO_18 0x2b
#define | RSL_SYSTEM_INFO_19 0x2c
#define | RSL_SYSTEM_INFO_20 0x2d
#define | RSL_CHANNEED_ANY 0x00
#define | RSL_CHANNEED_SDCCH 0x01
#define | RSL_CHANNEED_TCH_F 0x02
#define | RSL_CHANNEED_TCH_ForH 0x03
#define | RSL_CB_CMD_TYPE_NORMAL 0x00
#define | RSL_CB_CMD_TYPE_SCHEDULE 0x08
#define | RSL_CB_CMD_TYPE_DEFAULT 0x0e
#define | RSL_CB_CMD_TYPE_NULL 0x0f
#define | RSL_CB_CMD_DEFBCAST_NORMAL 0
#define | RSL_CB_CMD_DEFBCAST_NULL 1
#define | RSL_CB_CMD_LASTBLOCK_4 0
#define | RSL_CB_CMD_LASTBLOCK_1 1
#define | RSL_CB_CMD_LASTBLOCK_2 2
#define | RSL_CB_CMD_LASTBLOCK_3 3
#define | RSL_CMD_INDICATOR_START 0x00
| Command Indicator (Chapter 9.3.48) More...
#define | RSL_CMD_INDICATOR_STOP 0x01
#define | RSL_BCCH_CCCH_CONF_1_NC 0x00
#define | RSL_BCCH_CCCH_CONF_1_C 0x01
#define | RSL_BCCH_CCCH_CONF_2_NC 0x02
#define | RSL_BCCH_CCCH_CONF_3_NC 0x04
#define | RSL_BCCH_CCCH_CONF_4_NC 0x06
#define | RSL_BS_PA_MFRMS_2 0x00
#define | RSL_BS_PA_MFRMS_3 0x01
#define | RSL_BS_PA_MFRMS_4 0x02
#define | RSL_BS_PA_MFRMS_5 0x03
#define | RSL_BS_PA_MFRMS_6 0x04
#define | RSL_BS_PA_MFRMS_7 0x05
#define | RSL_BS_PA_MFRMS_8 0x06
#define | RSL_BS_PA_MFRMS_9 0x07

## Enumerations
enum | abis_rsl_msgtype { RSL_MT_DATA_REQ = 0x01 , RSL_MT_DATA_IND , RSL_MT_ERROR_IND , RSL_MT_EST_REQ , RSL_MT_EST_CONF , RSL_MT_EST_IND , RSL_MT_REL_REQ , RSL_MT_REL_CONF , RSL_MT_REL_IND , RSL_MT_UNIT_DATA_REQ , RSL_MT_UNIT_DATA_IND , RSL_MT_SUSP_REQ , RSL_MT_SUSP_CONF , RSL_MT_RES_REQ , RSL_MT_RECON_REQ , RSL_MT_BCCH_INFO = 0x11 , RSL_MT_CCCH_LOAD_IND , RSL_MT_CHAN_RQD , RSL_MT_DELETE_IND , RSL_MT_PAGING_CMD , RSL_MT_IMMEDIATE_ASSIGN_CMD , RSL_MT_SMS_BC_REQ , RSL_MT_CHAN_CONF , RSL_MT_RF_RES_IND = 0x19 , RSL_MT_SACCH_FILL , RSL_MT_OVERLOAD , RSL_MT_ERROR_REPORT , RSL_MT_SMS_BC_CMD , RSL_MT_CBCH_LOAD_IND , RSL_MT_NOT_CMD , RSL_MT_CHAN_ACTIV = 0x21 , RSL_MT_CHAN_ACTIV_ACK , RSL_MT_CHAN_ACTIV_NACK , RSL_MT_CONN_FAIL , RSL_MT_DEACTIVATE_SACCH , RSL_MT_ENCR_CMD , RSL_MT_HANDO_DET , RSL_MT_MEAS_RES , RSL_MT_MODE_MODIFY_REQ , RSL_MT_MODE_MODIFY_ACK , RSL_MT_MODE_MODIFY_NACK , RSL_MT_PHY_CONTEXT_REQ , RSL_MT_PHY_CONTEXT_CONF , RSL_MT_RF_CHAN_REL , RSL_MT_MS_POWER_CONTROL , RSL_MT_BS_POWER_CONTROL , RSL_MT_PREPROC_CONFIG , RSL_MT_PREPROC_MEAS_RES , RSL_MT_RF_CHAN_REL_ACK , RSL_MT_SACCH_INFO_MODIFY , RSL_MT_TALKER_DET , RSL_MT_LISTENER_DET , RSL_MT_REMOTE_CODEC_CONF_REP , RSL_MT_RTD_REP , RSL_MT_PRE_HANDO_NOTIF , RSL_MT_MR_CODEC_MOD_REQ , RSL_MT_MR_CODEC_MOD_ACK , RSL_MT_MR_CODEC_MOD_NACK , RSL_MT_MR_CODEC_MOD_PER , RSL_MT_TFO_REP , RSL_MT_TFO_MOD_REQ , RSL_MT_LOCATION_INFO = 0x41 , RSL_MT_IPAC_DIR_RETR_ENQ = 0x40 , RSL_MT_IPAC_PDCH_ACT = 0x48 , RSL_MT_IPAC_PDCH_ACT_ACK , RSL_MT_IPAC_PDCH_ACT_NACK , RSL_MT_IPAC_PDCH_DEACT = 0x4b , RSL_MT_IPAC_PDCH_DEACT_ACK , RSL_MT_IPAC_PDCH_DEACT_NACK , RSL_MT_IPAC_CONNECT_MUX = 0x50 , RSL_MT_IPAC_CONNECT_MUX_ACK , RSL_MT_IPAC_CONNECT_MUX_NACK , RSL_MT_IPAC_BIND_MUX = 0x53 , RSL_MT_IPAC_BIND_MUX_ACK , RSL_MT_IPAC_BIND_MUX_NACK , RSL_MT_IPAC_DISC_MUX = 0x56 , RSL_MT_IPAC_DISC_MUX_ACK , RSL_MT_IPAC_DISC_MUX_NACK , RSL_MT_IPAC_MEAS_PREPROC_DFT = 0x60 , RSL_MT_IPAC_HO_CAN_ENQ = 0x61 , RSL_MT_IPAC_HO_CAN_RES = 0x62 , RSL_MT_IPAC_CRCX = 0x70 , RSL_MT_IPAC_CRCX_ACK , RSL_MT_IPAC_CRCX_NACK , RSL_MT_IPAC_MDCX = 0x73 , RSL_MT_IPAC_MDCX_ACK , RSL_MT_IPAC_MDCX_NACK , RSL_MT_IPAC_DLCX_IND = 0x76 , RSL_MT_IPAC_DLCX = 0x77 , RSL_MT_IPAC_DLCX_ACK , RSL_MT_IPAC_DLCX_NACK , RSL_MT_OSMO_ETWS_CMD = 0x7f }
enum | abis_rsl_msgtype_siemens { RSL_MT_SIEMENS_MRPCI = 0x41 , RSL_MT_SIEMENS_INTRAC_HO_COND_IND = 0x42 , RSL_MT_SIEMENS_INTERC_HO_COND_IND = 0x43 , RSL_MT_SIEMENS_FORCED_HO_REQ = 0x44 , RSL_MT_SIEMENS_PREF_AREA_REQ = 0x45 , RSL_MT_SIEMENS_PREF_AREA = 0x46 , RSL_MT_SIEMENS_START_TRACE = 0x47 , RSL_MT_SIEMENS_START_TRACE_ACK = 0x48 , RSL_MT_SIEMENS_STOP_TRACE = 0x49 , RSL_MT_SIEMENS_TRMR = 0x4a , RSL_MT_SIEMENS_HO_FAIL_IND = 0x4b , RSL_MT_SIEMENS_STOP_TRACE_ACK = 0x4c , RSL_MT_SIEMENS_UPLF = 0x4d , RSL_MT_SIEMENS_UPLB = 0x4e , RSL_MT_SIEMENS_SET_SYS_INFO_10 = 0x4f , RSL_MT_SIEMENS_MODIF_COND_IND = 0x50 }
| Siemens vendor-specific RSL message types. More...
enum | abis_rsl_msgtype_ericsson { RSL_MT_ERICSSON_IMM_ASS_SENT = 0x10 }
| Ericsson vendor-specific RSL message types. More...
enum | abis_rsl_ie { RSL_IE_CHAN_NR = 0x01 , RSL_IE_LINK_IDENT , RSL_IE_ACT_TYPE , RSL_IE_BS_POWER , RSL_IE_CHAN_IDENT , RSL_IE_CHAN_MODE , RSL_IE_ENCR_INFO , RSL_IE_FRAME_NUMBER , RSL_IE_HANDO_REF , RSL_IE_L1_INFO , RSL_IE_L3_INFO , RSL_IE_MS_IDENTITY , RSL_IE_MS_POWER , RSL_IE_PAGING_GROUP , RSL_IE_PAGING_LOAD , RSL_IE_PYHS_CONTEXT = 0x10 , RSL_IE_ACCESS_DELAY , RSL_IE_RACH_LOAD , RSL_IE_REQ_REFERENCE , RSL_IE_RELEASE_MODE , RSL_IE_RESOURCE_INFO , RSL_IE_RLM_CAUSE , RSL_IE_STARTNG_TIME , RSL_IE_TIMING_ADVANCE , RSL_IE_UPLINK_MEAS , RSL_IE_CAUSE , RSL_IE_MEAS_RES_NR , RSL_IE_MSG_ID , RSL_IE_SYSINFO_TYPE = 0x1e , RSL_IE_MS_POWER_PARAM , RSL_IE_BS_POWER_PARAM , RSL_IE_PREPROC_PARAM , RSL_IE_PREPROC_MEAS , RSL_IE_IMM_ASS_INFO , RSL_IE_SMSCB_INFO = 0x24 , RSL_IE_MS_TIMING_OFFSET , RSL_IE_ERR_MSG , RSL_IE_FULL_BCCH_INFO , RSL_IE_CHAN_NEEDED , RSL_IE_CB_CMD_TYPE , RSL_IE_SMSCB_MSG , RSL_IE_FULL_IMM_ASS_INFO , RSL_IE_SACCH_INFO , RSL_IE_CBCH_LOAD_INFO , RSL_IE_SMSCB_CHAN_INDICATOR , RSL_IE_GROUP_CALL_REF , RSL_IE_CHAN_DESC = 0x30 , RSL_IE_NCH_DRX_INFO , RSL_IE_CMD_INDICATOR , RSL_IE_EMLPP_PRIO , RSL_IE_UIC , RSL_IE_MAIN_CHAN_REF , RSL_IE_MR_CONFIG , RSL_IE_MR_CONTROL , RSL_IE_SUP_CODEC_TYPES , RSL_IE_CODEC_CONFIG , RSL_IE_RTD , RSL_IE_TFO_STATUS , RSL_IE_LLP_APDU , RSL_IE_TFO_XPAR_CONT , RSL_IE_SIEMENS_MRPCI = 0x40 , RSL_IE_SIEMENS_PREF_AREA_TYPE = 0x43 , RSL_IE_SIEMENS_ININ_CELL_HO_PAR = 0x45 , RSL_IE_SIEMENS_TRACE_REF_NR = 0x46 , RSL_IE_SIEMENS_INT_TRACE_IDX = 0x47 , RSL_IE_SIEMENS_L2_HDR_INFO = 0x48 , RSL_IE_SIEMENS_HIGHEST_RATE = 0x4e , RSL_IE_SIEMENS_SUGGESTED_RATE = 0x4f , RSL_IE_OSMO_REP_ACCH_CAP = 0x60 , RSL_IE_OSMO_TRAINING_SEQUENCE = 0x61 , RSL_IE_OSMO_TEMP_OVP_ACCH_CAP = 0x62 , RSL_IE_OSMO_OSMUX_CID = 0x63 , RSL_IE_OSMO_RTP_EXTENSIONS = 0x64 , RSL_IE_IPAC_SRTP_CONFIG = 0xe0 , RSL_IE_IPAC_PROXY_UDP = 0xe1 , RSL_IE_IPAC_BSCMPL_TOUT = 0xe2 , RSL_IE_IPAC_REMOTE_IP = 0xf0 , RSL_IE_IPAC_REMOTE_PORT = 0xf1 , RSL_IE_IPAC_RTP_PAYLOAD = 0xf2 , RSL_IE_IPAC_LOCAL_PORT = 0xf3 , RSL_IE_IPAC_SPEECH_MODE = 0xf4 , RSL_IE_IPAC_LOCAL_IP = 0xf5 , RSL_IE_IPAC_CONN_STAT = 0xf6 , RSL_IE_IPAC_HO_C_PARMS = 0xf7 , RSL_IE_IPAC_CONN_ID = 0xf8 , RSL_IE_IPAC_RTP_CSD_FMT = 0xf9 , RSL_IE_IPAC_RTP_JIT_BUF = 0xfa , RSL_IE_IPAC_RTP_COMPR = 0xfb , RSL_IE_IPAC_RTP_PAYLOAD2 = 0xfc , RSL_IE_IPAC_RTP_MPLEX = 0xfd , RSL_IE_IPAC_RTP_MPLEX_ID = 0xfe }
| RSL Information Element Identifiers (Chapter 9.3) More...
enum | { IPAC_UNWEIGHTED_AVE = 0 , IPAC_WEIGHTED_AVE , IPAC_MEDIAN_AVE , IPAC_OSMO_EWMA_AVE }
enum | { IPAC_RXLEV_AVE = 0 , IPAC_RXQUAL_AVE , IPAC_MS_BTS_DIS_AVE }
enum | { IPAC_HO_RQD_CAUSE_L_RXLEV_UL_H = 0x01 , IPAC_HO_RQD_CAUSE_L_RXLEV_DL_H , IPAC_HO_RQD_CAUSE_L_RXQUAL_UL_H , IPAC_HO_RQD_CAUSE_L_RXQUAL_DL_H , IPAC_HO_RQD_CAUSE_RXLEV_UL_IH , IPAC_HO_RQD_CAUSE_RXLEV_DL_IH , IPAC_HO_RQD_CAUSE_MAX_MS_RANGE , IPAC_HO_RQD_CAUSE_POWER_BUDGET , IPAC_HO_RQD_CAUSE_ENQUIRY , IPAC_HO_RQD_CAUSE_ENQUIRY_FAILED , IPAC_HO_RQD_CAUSE_NORMAL3G , IPAC_HO_RQD_CAUSE_EMERGENCY3G , IPAC_HO_RQD_CAUSE_SERVICE_PREFERRED3G , IPAC_HO_RQD_CAUSE_O_M_SHUTDOWN , IPAC_HO_RQD_CAUSE_QUALITY_PROMOTION , IPAC_HO_RQD_CAUSE_LOAD_PROMOTION , IPAC_HO_RQD_CAUSE_LOAD_DEMOTION , IPAC_HO_RQD_CAUSE_MAX }
enum | rsl_cmod_spd { RSL_CMOD_SPD_SPEECH = 0x01 , RSL_CMOD_SPD_DATA = 0x02 , RSL_CMOD_SPD_SIGN = 0x03 }
enum | rsl_cmod_crt { RSL_CMOD_CRT_SDCCH = 0x01 , RSL_CMOD_CRT_TCH_Bm = 0x08 , RSL_CMOD_CRT_TCH_Lm = 0x09 , RSL_CMOD_CRT_TCH_BI_Bm = 0x0a , RSL_CMOD_CRT_TCH_UNI_Bm = 0x1a , RSL_CMOD_CRT_TCH_GROUP_Bm = 0x18 , RSL_CMOD_CRT_TCH_GROUP_Lm = 0x19 , RSL_CMOD_CRT_TCH_BCAST_Bm = 0x28 , RSL_CMOD_CRT_TCH_BCAST_Lm = 0x29 , RSL_CMOD_CRT_OSMO_TCH_VAMOS_Bm = 0x88 , RSL_CMOD_CRT_OSMO_TCH_VAMOS_Lm = 0x89 }
| Channel rate and type. More...
enum | rsl_cmod_sp { RSL_CMOD_SP_GSM1 = 0x01 , RSL_CMOD_SP_GSM2 = 0x11 , RSL_CMOD_SP_GSM3 = 0x21 , RSL_CMOD_SP_GSM4 = 0x31 , RSL_CMOD_SP_GSM5 = 0x09 , RSL_CMOD_SP_GSM6 = 0x0d }
| Speech. More...
enum | rsl_cmod_csd_nt { RSL_CMOD_CSD_NTA_43k5_14k5 = 0x61 , RSL_CMOD_CSD_NTA_29k0_14k5 = 0x62 , RSL_CMOD_CSD_NTA_43k5_29k0 = 0x63 , RSL_CMOD_CSD_NTA_14k5_43k5 = 0x69 , RSL_CMOD_CSD_NTA_14k5_29k0 = 0x6a , RSL_CMOD_CSD_NTA_29k0_43k5 = 0x6b , RSL_CMOD_CSD_NT_43k5 = 0x74 , RSL_CMOD_CSD_NT_28k8 = 0x71 , RSL_CMOD_CSD_NT_14k5 = 0x58 , RSL_CMOD_CSD_NT_12k0 = 0x50 , RSL_CMOD_CSD_NT_6k0 = 0x51 }
| Non-transparent data. More...
enum | rsl_cmod_csd_t { RSL_CMOD_CSD_T_32k0 = 0x38 , RSL_CMOD_CSD_T_29k0 = 0x39 , RSL_CMOD_CSD_T_14k4 = 0x18 , RSL_CMOD_CSD_T_9k6 = 0x10 , RSL_CMOD_CSD_T_4k8 = 0x11 , RSL_CMOD_CSD_T_2k4 = 0x12 , RSL_CMOD_CSD_T_1k2 = 0x13 , RSL_CMOD_CSD_T_600 = 0x14 , RSL_CMOD_CSD_T_1200_75 = 0x15 }
| Transparent data. More...
enum | rsl_ipac_rtp_payload { RSL_IPAC_RTP_GSM = 1 , RSL_IPAC_RTP_EFR , RSL_IPAC_RTP_AMR , RSL_IPAC_RTP_CSD , RSL_IPAC_RTP_MUX }
enum | rsl_ipac_speech_mode_s { RSL_IPAC_SPEECH_GSM_FR = 0 , RSL_IPAC_SPEECH_GSM_EFR = 1 , RSL_IPAC_SPEECH_GSM_AMR_FR = 2 , RSL_IPAC_SPEECH_GSM_HR = 3 , RSL_IPAC_SPEECH_GSM_AMR_HR = 5 , RSL_IPAC_SPEECH_AS_RTP = 0xf }
enum | rsl_ipac_speech_mode_m { RSL_IPAC_SPEECH_M_RXTX = 0 , RSL_IPAC_SPEECH_M_RX = 1 , RSL_IPAC_SPEECH_M_TX = 2 }
enum | rsl_ipac_rtp_csd_format_d { RSL_IPAC_RTP_CSD_EXT_TRAU = 0 , RSL_IPAC_RTP_CSD_NON_TRAU = 1 , RSL_IPAC_RTP_CSD_TRAU_BTS = 2 , RSL_IPAC_RTP_CSD_IWF_FREE = 3 }
enum | rsl_ipac_rtp_csd_format_ir { RSL_IPAC_RTP_CSD_IR_8k = 0 , RSL_IPAC_RTP_CSD_IR_16k = 1 , RSL_IPAC_RTP_CSD_IR_32k = 2 , RSL_IPAC_RTP_CSD_IR_64k = 3 }
enum | rsl_mrpci_pwrclass { RSL_MRPCI_PWRC_1 = 0 , RSL_MRPCI_PWRC_2 = 1 , RSL_MRPCI_PWRC_3 = 2 , RSL_MRPCI_PWRC_4 = 3 , RSL_MRPCI_PWRC_5 = 4 }
enum | rsl_mrpci_phase { RSL_MRPCI_PHASE_1 = 0 , RSL_MRPCI_PHASE_2 = 2 , RSL_MRPCI_PHASE_2PLUS = 3 }
enum | rsl_rel_mode { RSL_REL_NORMAL = 0 , RSL_REL_LOCAL_END = 1 }
enum | rsl_ipac_embedded_ie { RSL_IPAC_EIE_RXLEV = 0x00 , RSL_IPAC_EIE_RXQUAL = 0x01 , RSL_IPAC_EIE_FREQ_ERR = 0x02 , RSL_IPAC_EIE_TIMING_ERR = 0x03 , RSL_IPAC_EIE_MEAS_AVG_CFG = 0x04 , RSL_IPAC_EIE_BS_PWR_CTL = 0x05 , RSL_IPAC_EIE_MS_PWR_CTL = 0x06 , RSL_IPAC_EIE_HANDO_THRESH = 0x07 , RSL_IPAC_EIE_NCELL_DEFAULTS = 0x08 , RSL_IPAC_EIE_NCELL_LIST = 0x09 , RSL_IPAC_EIE_PC_THRESH_COMP = 0x0a , RSL_IPAC_EIE_HO_THRESH_COMP = 0x0b , RSL_IPAC_EIE_HO_CAUSE = 0x0c , RSL_IPAC_EIE_HO_CANDIDATES = 0x0d , RSL_IPAC_EIE_NCELL_BA_CHG_LIST = 0x0e , RSL_IPAC_EIE_NUM_OF_MS = 0x10 , RSL_IPAC_EIE_HO_CAND_EXT = 0x11 , RSL_IPAC_EIE_NCELL_DEF_EXT = 0x12 , RSL_IPAC_EIE_NCELL_LIST_EXT = 0x13 , RSL_IPAC_EIE_MASTER_KEY = 0x14 , RSL_IPAC_EIE_MASTER_SALT = 0x15 , RSL_IPAC_EIE_MEAS_TRANS_RES = 0x16 , RSL_IPAC_EIE_3G_HO_PARAM = 0x17 , RSL_IPAC_EIE_3G_NCELL_LIST = 0x18 , RSL_IPAC_EIE_SDCCH_CTL_PARAM = 0x1a , RSL_IPAC_EIE_AMR_CONV_THRESH = 0x1b , RSL_IPAC_EIE_OSMO_MEAS_AVG_CFG = 0xf0 , RSL_IPAC_EIE_OSMO_MS_PWR_CTL = 0xf1 , RSL_IPAC_EIE_OSMO_PC_THRESH_COMP = 0xf2 }
| ip.access specific embedded information elements More...

## Functions
union abis_rsl_chan_nr | __attribute__ ((packed))

## Variables
uint8_t | chan_nr
uint8_t | link_id
uint8_t | msg_discr
| message discriminator (ABIS_RSL_MDISC_*) More...
uint8_t | msg_type
| message type (abis_rsl_msgtype) More...
uint8_t | data [0]
| actual payload data More...
struct abis_rsl_common_hdr | c
uint8_t | ie_chan
| RSL_IE_CHAN_NR (tag) More...
union {
uint8_t chan_nr
union abis_rsl_chan_nr chan_nr_fields
| RSL channel number (value) More...
}; |
uint8_t | ie_link_id
| RSL_IE_LINK_IDENT (tag) More...
union {
uint8_t link_id
union abis_rsl_link_id link_id_fields
| RSL link identifier (value) More...
}; |
union {
uint8_t chan_nr
union abis_rsl_chan_nr chan_nr_fields
| RSL channel number (value) More...
}; |
union {
uint8_t chan_nr
union abis_rsl_chan_nr chan_nr_fields
| RSL channel number (value) More...
}; |
enum abis_rsl_msgtype | __attribute__
uint8_t | dtx_dtu
uint8_t | spd_ind
uint8_t | chan_rt
uint8_t | chan_rate
struct {
uint8_t iei
uint8_t chan_nr
uint8_t oct3
uint8_t oct4
} | chan_desc
uint8_t | power_class
uint8_t | vgcs_capable
uint8_t | vbs_capable
uint8_t | gsm_phase
struct osmo_preproc_ave_cfg_field | ci_fr
struct osmo_preproc_ave_cfg_field | ci_hr
struct osmo_preproc_ave_cfg_field | ci_amr_fr
struct osmo_preproc_ave_cfg_field | ci_amr_hr
struct osmo_preproc_ave_cfg_field | ci_sdcch
struct osmo_preproc_ave_cfg_field | ci_gprs
uint8_t | params [0]
int8_t | l_ci_fr
int8_t | u_ci_fr
int8_t | l_ci_hr
int8_t | u_ci_hr
int8_t | l_ci_amr_fr
int8_t | u_ci_amr_fr
int8_t | l_ci_amr_hr
int8_t | u_ci_amr_hr
int8_t | l_ci_sdcch
int8_t | u_ci_sdcch
int8_t | l_ci_gprs
int8_t | u_ci_gprs

## Detailed Description

GSM Radio Signalling Link messages on the A-bis interface.

3GPP TS 08.58 version 8.6.0 Release 1999 / ETSI TS 100 596 V8.6.0

## Variable Documentation

## ◆

union { ... }

## ◆

union { ... }

## ◆

union { ... }

## ◆

union { ... }

## ◆ c

struct abis_rsl_common_hdr c

Referenced by SHA1Transform().

## ◆

struct { ... } chan_desc

## ◆ chan_nr

uint8_t chan_nr

## ◆ chan_nr_fields

union abis_rsl_chan_nr chan_nr_fields

RSL channel number (value)

## ◆ chan_rate

uint8_t chan_rate

## ◆ chan_rt

uint8_t chan_rt

## ◆ ci_amr_fr

struct ipac_preproc_pc_comp_field ci_amr_fr

## ◆ ci_amr_hr

struct ipac_preproc_pc_comp_field ci_amr_hr

## ◆ ci_fr

struct ipac_preproc_pc_comp_field ci_fr

## ◆ ci_gprs

struct ipac_preproc_pc_comp_field ci_gprs

## ◆ ci_hr

struct ipac_preproc_pc_comp_field ci_hr

## ◆ ci_sdcch

struct ipac_preproc_pc_comp_field ci_sdcch

## ◆ data

uint8_t data[0]

actual payload data

message payload data

## ◆ dtx_dtu

uint8_t dtx_dtu

## ◆ gsm_phase

uint8_t gsm_phase

## ◆ ie_chan

uint8_t ie_chan

RSL_IE_CHAN_NR (tag)

## ◆ ie_link_id

uint8_t ie_link_id

RSL_IE_LINK_IDENT (tag)

## ◆ iei

uint8_t iei

Referenced by decode_auth_info(), decode_pdp_info(), encode_auth_info(), encode_pdp_info(), msgb_sgsap_name_put(), osmo_bsslap_ie_dec_cause(), osmo_bsslap_ie_dec_cell_id(), osmo_bsslap_ie_dec_chan_desc(), osmo_bsslap_ie_dec_ta(), osmo_bssmap_le_ie_dec_apdu(), osmo_bssmap_le_ie_dec_cell_id(), osmo_bssmap_le_ie_dec_imei(), osmo_bssmap_le_ie_dec_imsi(), osmo_bssmap_le_ie_dec_lcs_client_type(), osmo_bssmap_le_ie_dec_lcs_priority(), osmo_bssmap_le_ie_dec_lcs_qos(), osmo_bssmap_le_ie_dec_location_type(), osmo_gsup_decode(), osmo_lcs_cause_dec(), osmo_oap_decode(), osmo_tlv_prot_ie_name(), osmo_tlv_prot_validate_tp(), parse_ss_info_elements(), and sgsap_iei_name().

## ◆ l_ci_amr_fr

int8_t l_ci_amr_fr

## ◆ l_ci_amr_hr

int8_t l_ci_amr_hr

## ◆ l_ci_fr

int8_t l_ci_fr

## ◆ l_ci_gprs

int8_t l_ci_gprs

## ◆ l_ci_hr

int8_t l_ci_hr

## ◆ l_ci_sdcch

int8_t l_ci_sdcch

## ◆ link_id

uint8_t link_id

## ◆ link_id_fields

union abis_rsl_link_id link_id_fields

RSL link identifier (value)

## ◆ msg_discr

uint8_t msg_discr

message discriminator (ABIS_RSL_MDISC_*)

## ◆ msg_type

uint8_t msg_type

message type (abis_rsl_msgtype)

## ◆ oct3

uint8_t oct3

## ◆ oct4

uint8_t oct4

## ◆ params

uint8_t params[0]

Referenced by gsm0808_create_handover_command(), gsm0808_create_handover_complete(), gsm0808_create_handover_failure(), gsm0808_create_handover_performed(), gsm0808_create_handover_request(), gsm0808_create_handover_request_ack(), gsm0808_create_handover_request_ack2(), gsm0808_create_handover_required(), gsm0808_create_handover_required_reject(), gsm0808_create_notification_data(), gsm0808_create_perform_location_request(), gsm0808_create_perform_location_response(), gsm0808_create_uplink_app_data(), gsm0808_create_uplink_reject_cmd(), gsm0808_create_uplink_release_ind(), gsm0808_create_uplink_request(), gsm0808_create_uplink_request_ack(), gsm0808_create_uplink_request_cnf(), gsm0808_create_uplink_seized_cmd(), gsm0808_create_vgcs_vbs_area_cell_info(), gsm0808_create_vgcs_vbs_assign_fail(), gsm0808_create_vgcs_vbs_assign_req(), gsm0808_create_vgcs_vbs_assign_res(), gsm0808_create_vgcs_vbs_assign_stat(), gsm0808_create_vgcs_vbs_setup(), gsm0808_create_vgcs_vbs_setup_ack(), gsm29118_create_paging_req(), gsm29118_create_reset_ack(), gsm29118_create_reset_ind(), osmo_bssmap_le_dec_conn_oriented_info(), osmo_bssmap_le_dec_perform_loc_abort(), osmo_bssmap_le_dec_perform_loc_req(), osmo_bssmap_le_dec_perform_loc_resp(), osmo_bssmap_le_enc_conn_oriented_info(), osmo_bssmap_le_enc_perform_loc_abort(), osmo_bssmap_le_enc_perform_loc_req(), and osmo_bssmap_le_enc_perform_loc_resp().

## ◆ power_class

uint8_t power_class

## ◆ spd_ind

uint8_t spd_ind

## ◆ u_ci_amr_fr

int8_t u_ci_amr_fr

## ◆ u_ci_amr_hr

int8_t u_ci_amr_hr

## ◆ u_ci_fr

int8_t u_ci_fr

## ◆ u_ci_gprs

int8_t u_ci_gprs

## ◆ u_ci_hr

int8_t u_ci_hr

## ◆ u_ci_sdcch

int8_t u_ci_sdcch

## ◆ vbs_capable

uint8_t vbs_capable

## ◆ vgcs_capable

uint8_t vgcs_capable