libosmocore 1.13.1.1-afb4 Osmocom core library

Macros | Enumerations | Functions
sercomm.c File Reference
Seriall Communications (HDLC)
`#include "config.h"`
`#include <stdint.h>`
`#include <stdio.h>`
`#include <errno.h>`
`#include <osmocom/core/msgb.h>`
`#include <osmocom/core/utils.h>`
`#include <osmocom/core/sercomm.h>`
`#include <osmocom/core/linuxlist.h>`

## Macros
#define | DEFAULT_RX_MSG_SIZE 2048
#define | HDLC_FLAG 0x7E
#define | HDLC_ESCAPE 0x7D
#define | HDLC_C_UI 0x03
#define | HDLC_C_P_BIT (1 << 4)
#define | HDLC_C_F_BIT (1 << 4)

## Enumerations
enum | rx_state { RX_ST_WAIT_START , RX_ST_ADDR , RX_ST_CTRL , RX_ST_DATA , RX_ST_ESCAPE }

## Functions
void | sercomm_drv_lock (unsigned long __attribute__((unused)) *flags)
| Protect against IRQ context. More...
void | sercomm_drv_unlock (unsigned long __attribute__((unused)) *flags)
| Release protection against IRQ context. More...
| __attribute__ ((weak))
void | osmo_sercomm_init (struct osmo_sercomm_inst *sercomm)
| Initialize an Osmocom sercomm instance. More...
int | osmo_sercomm_initialized (struct osmo_sercomm_inst *sercomm)
| Determine if a given Osmocom sercomm instance has been initialized. More...
void | osmo_sercomm_sendmsg (struct osmo_sercomm_inst *sercomm, uint8_t dlci, struct msgb *msg)
| User interface for transmitting messages for a given DLCI. More...
unsigned int | osmo_sercomm_tx_queue_depth (struct osmo_sercomm_inst *sercomm, uint8_t dlci)
| How deep is the Tx queue for a given DLCI? More...
int | osmo_sercomm_change_speed (struct osmo_sercomm_inst *sercomm, uint32_t bdrt)
| wait until everything has been transmitted, then grab the lock and change the baud rate as requested More...
int | osmo_sercomm_drv_pull (struct osmo_sercomm_inst *sercomm, uint8_t *ch)
| fetch one octet of to-be-transmitted serial data More...
int | osmo_sercomm_register_rx_cb (struct osmo_sercomm_inst *sercomm, uint8_t dlci, dlci_cb_t cb)
| Register a handler for a given DLCI. More...
static void | dispatch_rx_msg (struct osmo_sercomm_inst *sercomm, uint8_t dlci, struct msgb *msg)
int | osmo_sercomm_drv_rx_char (struct osmo_sercomm_inst *sercomm, uint8_t ch)
| the driver has received one byte, pass it into sercomm layer More...