\doxysection{gsm\+\_\+03\+\_\+40.\+h}
\label{gsm__03__40_8h_source}\index{include/osmocom/gsm/protocol/gsm\_03\_40.h@{include/osmocom/gsm/protocol/gsm\_03\_40.h}}
\textbf{ Go to the documentation of this file.}
\begin{DoxyCode}{0}
\DoxyCodeLine{1 }
\DoxyCodeLine{4 \textcolor{preprocessor}{\#pragma once}}
\DoxyCodeLine{5 }
\DoxyCodeLine{6 \textcolor{comment}{/* SM-\/TP-\/UD (User-\/Data) field may contain up to 140 octets}}
\DoxyCodeLine{7 \textcolor{comment}{ * (or 140 * 8 / 7 = 160 septets). See section 9.2.3.24. */}}
\DoxyCodeLine{8 \textcolor{preprocessor}{\#define GSM340\_UDL\_OCT\_MAX 140  }}
\DoxyCodeLine{9 \textcolor{preprocessor}{\#define GSM340\_UDL\_SPT\_MAX 160  }}
\DoxyCodeLine{14 \textcolor{keyword}{enum} \{}
\DoxyCodeLine{15         GSM340\_TYPE\_UNKNOWN          = 0,}
\DoxyCodeLine{16         GSM340\_TYPE\_INTERNATIONAL      = 1,}
\DoxyCodeLine{17         GSM340\_TYPE\_NATIONAL                = 2,}
\DoxyCodeLine{18         GSM340\_TYPE\_NETWORK          = 3,}
\DoxyCodeLine{19         GSM340\_TYPE\_SUBSCRIBER            = 4,}
\DoxyCodeLine{20         GSM340\_TYPE\_ALPHA\_NUMERIC      = 5,}
\DoxyCodeLine{21         GSM340\_TYPE\_ABBREVIATED          = 6,}
\DoxyCodeLine{22         GSM340\_TYPE\_RESERVED                = 7,}
\DoxyCodeLine{23 \};}
\DoxyCodeLine{24 }
\DoxyCodeLine{29 \textcolor{keyword}{enum} \{}
\DoxyCodeLine{30         GSM340\_PLAN\_UNKNOWN          = 0,}
\DoxyCodeLine{31         GSM340\_PLAN\_ISDN                = 1,}
\DoxyCodeLine{32         GSM340\_PLAN\_DATA                = 3,}
\DoxyCodeLine{33         GSM340\_PLAN\_TELEX              = 4,}
\DoxyCodeLine{34         GSM340\_PLAN\_NATIONAL                = 8,}
\DoxyCodeLine{35         GSM340\_PLAN\_PRIVATE          = 9,}
\DoxyCodeLine{36         GSM340\_PLAN\_ERMES              = 10,}
\DoxyCodeLine{37         GSM340\_PLAN\_RESERVED                = 15,}
\DoxyCodeLine{38 \};}

\end{DoxyCode}
