libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Macros | Functions | Variables
rsl.h File Reference
A-bis RSL
`#include <stdint.h>`
`#include <osmocom/core/utils.h>`
`#include <osmocom/core/msgb.h>`
`#include <osmocom/gsm/protocol/gsm_08_58.h>`

Go to the source code of this file.

## Macros
#define | rsl_tlv_parse(dec, buf, len) tlv_parse(dec, &rsl_att_tlvdef, buf, len, 0, 0)
| Parse RSL TLV structure using tlv_parse. More...
#define | rsl_ipac_eie_tlv_parse(dec, buf, len) tlv_parse(dec, &rsl_ipac_eie_tlvdef, buf, len, 0, 0)
| Parse RSL IPAC EIE TLV structure using tlv_parse. More...

## Functions
void | rsl_init_rll_hdr (struct abis_rsl_rll_hdr *dh, uint8_t msg_type)
| Initialize a RSL RLL header. More...
void | rsl_init_cchan_hdr (struct abis_rsl_cchan_hdr *ch, uint8_t msg_type)
| Initialize a RSL Common Channel header. More...
uint8_t | rsl_enc_chan_nr (uint8_t type, uint8_t subch, uint8_t timeslot)
| Encode channel number as per Section 9.3.1. More...
int | rsl_dec_chan_nr (uint8_t chan_nr, uint8_t *type, uint8_t *subch, uint8_t *timeslot)
| Decode RSL channel number. More...
char * | rsl_chan_nr_str_buf (char *buf, size_t buf_len, uint8_t chan_nr)
| Get human-readable string for RSL channel number, in caller-provided buffer. More...
const char * | rsl_chan_nr_str (uint8_t chan_nr)
| Get human-readable string for RSL channel number, in static buffer. More...
char * | rsl_chan_nr_str_c (const void *ctx, uint8_t chan_nr)
| Get human-readable string for RSL channel number, in dynamically-allocated buffer. More...
const char * | rsl_err_name (uint8_t err)
| Get human-readable name for RSL Error. More...
const char * | rsl_rlm_cause_name (uint8_t err)
| Get human-readable string for RLM cause. More...
const char * | rsl_msg_name (uint8_t msg_type)
| Get human-readable string for RSL Message Type. More...
const char * | rsl_ipac_msg_name (uint8_t msg_type)
| Get human-readable name of ip.access RSL msg type. More...
const char * | rsl_or_ipac_msg_name (uint8_t msg_type)
| Get human-readable name of standard or ip.access RSL msg type. More...
int | rsl_ccch_conf_to_bs_cc_chans (int ccch_conf)
void | rsl_rll_push_hdr (struct msgb *msg, uint8_t msg_type, uint8_t chan_nr, uint8_t link_id, int transparent)
| Push a RSL RLL header onto an existing msgb. More...
void | rsl_rll_push_l3 (struct msgb *msg, uint8_t msg_type, uint8_t chan_nr, uint8_t link_id, int transparent)
| Wrap msgb in L3 Info IE and push a RSL RLL header. More...
struct msgb * | rsl_rll_simple (uint8_t msg_type, uint8_t chan_nr, uint8_t link_id, int transparent)
| Create msgb with RSL RLL header. More...
static const char * | rsl_act_type_name (uint8_t act_type)
| Return a human readable name for GSM 08.58 RSL_ACT_* constants. More...

## Variables
const struct tlv_definition | rsl_att_tlvdef
const struct tlv_definition | rsl_ipac_eie_tlvdef
| TLV parser definitions for IPA embedded IEs. More...
const struct value_string | rsl_act_type_names []
| String names of RSL Channel Activation Types. More...