\doxysection{info\+\_\+meas\+\_\+ind\+\_\+param Struct Reference}
\label{structinfo__meas__ind__param}\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}}


for MEAS MPH-\/\+INFO.\+ind  




{\ttfamily \#include $<$l1sap.\+h$>$}

\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
uint8\+\_\+t \textbf{ chan\+\_\+nr}
\begin{DoxyCompactList}\small\item\em Channel Number (Like RSL) \end{DoxyCompactList}\item 
uint32\+\_\+t \textbf{ fn}
\begin{DoxyCompactList}\small\item\em GSM Frame Number. \end{DoxyCompactList}\item 
uint16\+\_\+t \textbf{ ber10k}
\begin{DoxyCompactList}\small\item\em BER in units of 0.\+01\%. \end{DoxyCompactList}\item 
\begin{tabbing}
xx\=xx\=xx\=xx\=xx\=xx\=xx\=xx\=xx\=\kill
union \{\\
\>int16\_t \textbf{ ta\_offs\_qbits}\\
\>\>{\em timing advance offset (in qbits) }\\
\>int16\_t \textbf{ ta\_offs\_256bits}\\
\>\>{\em timing advance offset (in 1/256th bits) }\\
\}; \\

\end{tabbing}\item 
int16\+\_\+t \textbf{ c\+\_\+i\+\_\+cb}
\begin{DoxyCompactList}\small\item\em C/I ratio in 0.\+1 dB. \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ is\+\_\+sub}\+:1
\begin{DoxyCompactList}\small\item\em flags \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ inv\+\_\+rssi}
\begin{DoxyCompactList}\small\item\em RSSI in d\+Bm $\ast$ -\/1. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
for MEAS MPH-\/\+INFO.\+ind 

\doxysubsection{Field Documentation}
\mbox{\label{structinfo__meas__ind__param_a13a587590a9e2127bcca12d61863d818}} 
\doxysubsubsection{}
{\footnotesize\ttfamily union  \{ ... \}  info\+\_\+meas\+\_\+ind\+\_\+param\+::@22}

\mbox{\label{structinfo__meas__ind__param_af8d2706dc2bae5598f085a72341b094d}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!ber10k@{ber10k}}
\index{ber10k@{ber10k}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{ber10k}
{\footnotesize\ttfamily uint16\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::ber10k}



BER in units of 0.\+01\%. 

\mbox{\label{structinfo__meas__ind__param_a7e37ad0e8e127b3ba20d88c18ae8a2d5}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!c\_i\_cb@{c\_i\_cb}}
\index{c\_i\_cb@{c\_i\_cb}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{c\_i\_cb}
{\footnotesize\ttfamily int16\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::c\+\_\+i\+\_\+cb}



C/I ratio in 0.\+1 dB. 

\mbox{\label{structinfo__meas__ind__param_a20de77f57cae76ccae1e4c5f9bf9fd03}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!chan\_nr@{chan\_nr}}
\index{chan\_nr@{chan\_nr}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{chan\_nr}
{\footnotesize\ttfamily uint8\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::chan\+\_\+nr}



Channel Number (Like RSL) 

\mbox{\label{structinfo__meas__ind__param_a8ba931c45bfbd44a4d5b13f3a9078b5b}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!fn@{fn}}
\index{fn@{fn}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{fn}
{\footnotesize\ttfamily uint32\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::fn}



GSM Frame Number. 

\mbox{\label{structinfo__meas__ind__param_af9911ec26e21597db31610c95459efa4}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!inv\_rssi@{inv\_rssi}}
\index{inv\_rssi@{inv\_rssi}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{inv\_rssi}
{\footnotesize\ttfamily uint8\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::inv\+\_\+rssi}



RSSI in d\+Bm $\ast$ -\/1. 

\mbox{\label{structinfo__meas__ind__param_a6835f57e595d610921a0b8aafdf8ef7a}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!is\_sub@{is\_sub}}
\index{is\_sub@{is\_sub}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{is\_sub}
{\footnotesize\ttfamily uint8\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::is\+\_\+sub}



flags 

\mbox{\label{structinfo__meas__ind__param_acc61a3065d520a7b23ac414d9ff428cb}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!ta\_offs\_256bits@{ta\_offs\_256bits}}
\index{ta\_offs\_256bits@{ta\_offs\_256bits}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{ta\_offs\_256bits}
{\footnotesize\ttfamily int16\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::ta\+\_\+offs\+\_\+256bits}



timing advance offset (in 1/256th bits) 

\mbox{\label{structinfo__meas__ind__param_ae3db1710f922f0ec482fe5c3c32e9be0}} 
\index{info\_meas\_ind\_param@{info\_meas\_ind\_param}!ta\_offs\_qbits@{ta\_offs\_qbits}}
\index{ta\_offs\_qbits@{ta\_offs\_qbits}!info\_meas\_ind\_param@{info\_meas\_ind\_param}}
\doxysubsubsection{ta\_offs\_qbits}
{\footnotesize\ttfamily int16\+\_\+t info\+\_\+meas\+\_\+ind\+\_\+param\+::ta\+\_\+offs\+\_\+qbits}



timing advance offset (in qbits) 



The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
include/osmocom/gsm/\textbf{ l1sap.\+h}\end{DoxyCompactItemize}
