libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - m -

- mac_addr : ipaccess_unit
- magic : sdp_firmware
- major_ori : osmo_gad_ell_point_alt_unc_ell, osmo_gad_ell_point_unc_ellipse, osmo_gad_ha_ell_point_alt_unc_ell
- mand_count : osmo_tlv_prot_msg_def
- mand_ies : osmo_tlv_prot_msg_def
- marker : ph_tch_param
- mask : gsm_sysinfo_freq
- max_bitrate_down : gsm48_qos
- max_bitrate_down_ext : gsm48_qos
- max_bitrate_up : gsm48_qos
- max_lapdm : osmo_gsm48_si_dtm_support
- max_sdu_size : gsm48_qos
- max_txpwr : osmo_gsm48_si_gprs_ms_txpwr_max_ccch
- mcc : gprs_ra_id, osmo_gsm48_lsa_params, osmo_plmn_id
- mcs : egprs_cps
- mctx : lapdm_datalink
- mdisc : abis_om_hdr
- mean_tput : gsm48_qos
- meas_bw : osmo_earfcn_si2q
- meas_ind : mph_info_param
- meas_mode_flags : ipac_preproc_cfg
- meas_rep_mode : ipac_preproc_cfg
- message_class : osmo_gsup_message
- message_id : gsm23041_etws_primary_gsm, gsm23041_msg_param_gsm, gsm23041_msg_param_umts
- message_type : osmo_gsup_message, osmo_oap_message
- method : gsm48_classmark3
- mi : gsm0808_uplink_request, gsm48_imsi_detach_ind
- mi_len : gsm48_imsi_detach_ind
- mi_present : gsm0808_uplink_request
- min_len : osmo_tlv_prot_ie_def
- mm_send : gsm411_smc_inst
- mme : osmo_gummei
- mme_name : gsm29118_reset_msg
- mme_name_present : gsm29118_reset_msg
- mn_recv : gsm411_smc_inst
- mn_send : gsm411_smr_inst
- mnc : gprs_ra_id, osmo_gsm48_lsa_params, osmo_plmn_id
- mnc_3_digits : gprs_ra_id, osmo_plmn_id
- mob_alloc : gsm48_frq_redef, gsm48_imm_ass, gsm48_imm_ass_ext
- mob_alloc_len : gsm48_frq_redef, gsm48_imm_ass, gsm48_imm_ass_ext
- mod_cap : gsm48_classmark3
- mode : gsm0808_old_bss_to_new_bss_info, gsm48_chan_mode_modify, gsm_mncc_bearer_cap, lapdm_entity
- mode_version : osmo_iuup_instance, osmo_iuup_rnl_status
- modem_type : gsm_mncc_bearer_cap
- more_items : bsslap_reset, bsslap_ta_layer3, bsslap_ta_response, bssmap_le_conn_oriented_info, bssmap_le_perform_loc_req, bssmap_le_perform_loc_resp, gsm0808_cipher_mode_command, gsm0808_handover_command, gsm0808_handover_complete, gsm0808_handover_failure, gsm0808_handover_performed, gsm0808_handover_request, gsm0808_handover_request_ack, gsm0808_handover_required, gsm0808_handover_required_reject, gsm0808_old_bss_to_new_bss_info, gsm0808_perform_location_request
- more_items2 : bssmap_le_perform_loc_req, gsm0808_handover_request, gsm0808_handover_request_ack
- more_magic : sdp_firmware
- more_more_magic : sdp_firmware
- ms_ave_cfg : ipac_preproc_cfg
- ms_meas_cap : gsm48_classmark3
- ms_pos_method_cap : gsm48_classmark3
- msg : gsm0808_diagnostics
- msg_content : osmo_cbsp_write_replace
- msg_def : osmo_tlv_prot_def
- msg_discr : abis_rsl_common_hdr
- msg_id : gsm341_etws_message, gsm341_ms_message, osmo_cbsp_error_ind, osmo_cbsp_kill, osmo_cbsp_kill_complete, osmo_cbsp_kill_failure, osmo_cbsp_msg_status_query, osmo_cbsp_msg_status_query_complete, osmo_cbsp_msg_status_query_failure, osmo_cbsp_write_replace, osmo_cbsp_write_replace_complete, osmo_cbsp_write_replace_failure
- msg_ref : gsm411_rp_hdr
- msg_status_query : osmo_cbsp_decoded
- msg_status_query_compl : osmo_cbsp_decoded
- msg_status_query_fail : osmo_cbsp_decoded
- msg_type : abis_om_fom_hdr, abis_rsl_common_hdr, bsslap_pdu, bssmap_le_pdu, cbsp_header, gsm23041_msg_param_umts, gsm411_rp_hdr, gsm48_hdr, gsm48_imm_ass, gsm48_imm_ass_ext, gsm48_imm_ass_rej, gsm48_notification_nch, osmo_bsslap_err, osmo_bssmap_le_err, osmo_cbsp_decoded
- msgt_names : osmo_tlv_prot_def
- msisdn : gsm0808_notification_data
- msisdn_enc : osmo_gsup_message
- msisdn_enc_len : osmo_gsup_message
- msisdn_present : gsm0808_notification_data
- mslot_class : gsm48_classmark3
- mtmsi : osmo_guti
- mult_band_supp : gsm48_classmark3