libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - l -

- l1_ctx : lapdm_entity
- l1_prim_cb : lapdm_entity
- l2_plen : gsm48_imm_ass, gsm48_imm_ass_ext, gsm48_imm_ass_rej, gsm48_notification_nch
- l3 : gsm0808_layer_3_information, gsm0808_uplink_app_data, gsm0808_uplink_request, gsm0808_uplink_request_cnf
- l3_cb : lapdm_entity
- l3_ctx : lapdm_entity
- l3_info : gsm0808_handover_command, gsm0808_handover_request_ack
- l3_info_len : gsm0808_handover_command, gsm0808_handover_request_ack
- l3_len : gsm0808_layer_3_information
- l3_present : gsm0808_uplink_request
- l_ci_amr_fr : osmo_preproc_pc_thresh
- l_ci_amr_hr : osmo_preproc_pc_thresh
- l_ci_fr : osmo_preproc_pc_thresh
- l_ci_gprs : osmo_preproc_pc_thresh
- l_ci_hr : osmo_preproc_pc_thresh
- l_ci_sdcch : osmo_preproc_pc_thresh
- lac : gprs_ra_id, gsm0808_cell_id_u, gsm48_loc_area_id, gsm48_ra_id, osmo_lac_and_ci_id, osmo_location_area_id, osmo_routing_area_id
- lac_and_ci : gsm0808_cell_id_u
- lai : gsm29118_paging_req, gsm48_system_information_type_3, gsm48_system_information_type_4, osmo_cell_global_id, osmo_service_area_id
- lai_and_lac : gsm0808_cell_id_u
- lai_present : gsm29118_paging_req
- lapdm_acch : lapdm_channel
- lapdm_ch : lapdm_entity
- lapdm_dcch : lapdm_channel
- lapdm_fmt : lapdm_msg_ctx
- last : osmo_nri_range
- last_eutran_plmn_id : gsm0808_old_bss_to_new_bss_info
- last_eutran_plmn_id_present : gsm0808_old_bss_to_new_bss_info
- last_tx_dequeue : lapdm_entity
- lat : gad_raw_ell_point, gad_raw_ell_point_alt, gad_raw_polygon, osmo_gad_ell_arc, osmo_gad_ell_point, osmo_gad_ell_point_alt, osmo_gad_ell_point_alt_unc_ell, osmo_gad_ell_point_unc_circle, osmo_gad_ell_point_unc_ellipse, osmo_gad_ha_ell_point_alt_unc_ell
- lcls_bss_status : gsm0808_handover_complete, gsm0808_handover_performed
- lcls_bss_status_present : gsm0808_handover_complete, gsm0808_handover_performed
- lcs : gsm0808_old_bss_to_new_bss_info
- lcs_cause : bssmap_le_perform_loc_resp, gsm0808_perform_location_response
- lcs_client_type : bssmap_le_perform_loc_req
- lcs_client_type_present : bssmap_le_perform_loc_req
- lcs_priority : bssmap_le_perform_loc_req
- lcs_priority_present : bssmap_le_perform_loc_req
- lcs_qos : bssmap_le_perform_loc_req
- lcs_qos_present : bssmap_le_perform_loc_req
- len : cbsp_header, fn_remap_table, gsm0808_speech_codec_list, gsm411_rp_hdr, gsm_mncc_facility, gsm_mncc_ssversion, ipaccess_head, tlv_p_entry
- length : abis_om_hdr, bssmap_header, dtap_header, osmo_bssap_le_header, osmo_earfcn_si2q, osmo_gsn_address, sdp_header_entry, sha256_state
- link_id : abis_rsl_link_id, abis_rsl_rll_hdr, dtap_header, lapdm_msg_ctx, ph_data_param
- link_id_fields : abis_rsl_rll_hdr
- list : gprs_cipher_impl, lapdm_channel, osmo_auth_impl, osmo_cbsp_cell_ent, osmo_cbsp_cell_list, osmo_cbsp_content, osmo_cbsp_fail_ent, osmo_cbsp_loading_ent, osmo_cbsp_loading_list, osmo_cbsp_num_compl_ent, osmo_cbsp_num_compl_list
- list_len : gsm0808_circuit_pool_list
- load : osmo_cbsp_loading_ent
- load_query : osmo_cbsp_decoded
- load_query_compl : osmo_cbsp_decoded
- load_query_fail : osmo_cbsp_decoded
- loading_list : osmo_cbsp_load_query_complete, osmo_cbsp_load_query_failure
- location : gsm_mncc_cause, gsm_mncc_progress
- location1 : ipaccess_unit
- location2 : ipaccess_unit
- location_estimate : bssmap_le_perform_loc_resp, gsm0808_perform_location_response
- location_estimate_present : bssmap_le_perform_loc_resp, gsm0808_perform_location_response
- location_information : bssmap_le_location_type
- location_type : bssmap_le_perform_loc_req, gsm0808_perform_location_request
- logmsg : osmo_bssap_le_err, osmo_bsslap_err, osmo_bssmap_le_err, osmo_gad_err
- lon : gad_raw_ell_point, gad_raw_ell_point_alt, gad_raw_polygon, osmo_gad_ell_arc, osmo_gad_ell_point, osmo_gad_ell_point_alt, osmo_gad_ell_point_alt_unc_ell, osmo_gad_ell_point_unc_circle, osmo_gad_ell_point_unc_ellipse, osmo_gad_ha_ell_point_alt_unc_ell
- lqual_cb : ph_data_param, ph_rach_ind_param, ph_tch_param
- lsa_offset : osmo_gsm48_lsa_params
- lsa_params : osmo_gsm48_si_ro_info
- lv : tlv_parsed