libosmogsm 1.13.1.1-afb4 Osmocom GSM library

gsup.h
Go to the documentation of this file.
1
18/*
19 * (C) 2014 by sysmocom - s.f.m.c. GmbH, Author: Jacob Erlbeck
20 * (C) 2016 by Harald Welte <laforge@gnumonks.org>
21 * All Rights Reserved
22 *
23 * SPDX-License-Identifier: GPL-2.0+
24 *
25 * This program is free software; you can redistribute it and/or modify
26 * it under the terms of the GNU General Public License as published by
27 * the Free Software Foundation; either version 2 of the License, or
28 * (at your option) any later version.
29 *
30 * This program is distributed in the hope that it will be useful,
31 * but WITHOUT ANY WARRANTY; without even the implied warranty of
32 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the
33 * GNU General Public License for more details.
34 *
35 * You should have received a copy of the GNU General Public License
36 * along with this program. If not, see <http://www.gnu.org/licenses/>.
37 *
38 */
39#pragma once
40
41#include <stdint.h>
42#include <osmocom/core/msgb.h>
43#include <osmocom/core/defs.h>
44#include <osmocom/core/endian.h>
45#include <osmocom/core/socket.h>
46#include <osmocom/gsm/gsup_sms.h>
47#include <osmocom/gsm/protocol/gsm_23_003.h>
48#include <osmocom/gsm/protocol/gsm_03_40.h>
49#include <osmocom/gsm/protocol/gsm_04_08_gprs.h>
50#include <osmocom/gsm/protocol/gsm_08_08.h>
51#include <osmocom/gsm/gsm_utils.h>
52#include <osmocom/crypt/auth.h>
53
54#define OSMO_GSUP_PORT 4222
55
57#define OSMO_GSUP_MAX_NUM_PDP_INFO 10 /* GSM 09.02 limits this to 50 */
59#define OSMO_GSUP_MAX_NUM_AUTH_INFO 5
61#define OSMO_GSUP_MAX_MSISDN_LEN 9
62#define OSMO_GSUP_MAX_CALLED_PARTY_BCD_LEN 43 /* TS 24.008 10.5.4.7 */
63#define OSMO_GSUP_MAX_PCO_LEN 251
64
66 enum osmo_gsup_iei {
67 OSMO_GSUP_IMSI_IE = 0x01,
68 OSMO_GSUP_CAUSE_IE = 0x02,
69 OSMO_GSUP_AUTH_TUPLE_IE = 0x03,
70 OSMO_GSUP_PDP_INFO_COMPL_IE = 0x04,
71 OSMO_GSUP_PDP_INFO_IE = 0x05,
72 OSMO_GSUP_CANCEL_TYPE_IE = 0x06,
73 OSMO_GSUP_FREEZE_PTMSI_IE = 0x07,
74 OSMO_GSUP_MSISDN_IE = 0x08,
75 OSMO_GSUP_HLR_NUMBER_IE = 0x09,
76 OSMO_GSUP_MESSAGE_CLASS_IE = 0x0a,
77 OSMO_GSUP_PDP_CONTEXT_ID_IE = 0x10,
78 OSMO_GSUP_PDP_ADDRESS_IE = 0x11,
79#define OSMO_GSUP_PDP_TYPE_IE OSMO_GSUP_PDP_ADDRESS_IE /* Backward compat */
80 OSMO_GSUP_ACCESS_POINT_NAME_IE = 0x12,
81 OSMO_GSUP_PDP_QOS_IE = 0x13,
82 OSMO_GSUP_CHARG_CHAR_IE = 0x14,
83 OSMO_GSUP_PCO_IE = 0x15,
84 OSMO_GSUP_RAND_IE = 0x20,
85 OSMO_GSUP_SRES_IE = 0x21,
86 OSMO_GSUP_KC_IE = 0x22,
87 /* 3G support */
88 OSMO_GSUP_IK_IE = 0x23,
89 OSMO_GSUP_CK_IE = 0x24,
90 OSMO_GSUP_AUTN_IE = 0x25,
91 OSMO_GSUP_AUTS_IE = 0x26,
92 OSMO_GSUP_RES_IE = 0x27,
93 OSMO_GSUP_CN_DOMAIN_IE = 0x28,
94 OSMO_GSUP_SUPPORTED_RAT_TYPES_IE = 0x29, /* supported RAT types */
95 OSMO_GSUP_CURRENT_RAT_TYPE_IE = 0x2a, /* currently used RAT type */
96
97 OSMO_GSUP_SESSION_ID_IE = 0x30,
98 OSMO_GSUP_SESSION_STATE_IE = 0x31,
99
101 OSMO_GSUP_SS_INFO_IE = 0x35,
102
103 /* SM related IEs (see 3GPP TS 29.002, section 7.6.8) */
104 OSMO_GSUP_SM_RP_MR_IE = 0x40,
105 OSMO_GSUP_SM_RP_DA_IE = 0x41,
106 OSMO_GSUP_SM_RP_OA_IE = 0x42,
107 OSMO_GSUP_SM_RP_UI_IE = 0x43,
108 OSMO_GSUP_SM_RP_CAUSE_IE = 0x44,
109 OSMO_GSUP_SM_RP_MMS_IE = 0x45,
110 OSMO_GSUP_SM_ALERT_RSN_IE = 0x46,
111
112 OSMO_GSUP_IMEI_IE = 0x50,
113 OSMO_GSUP_IMEI_RESULT_IE = 0x51,
114 OSMO_GSUP_NUM_VECTORS_REQ_IE = 0x52,
115
116 /* Inter-MSC handover related */
117 OSMO_GSUP_SOURCE_NAME_IE = 0x60,
118 OSMO_GSUP_DESTINATION_NAME_IE = 0x61,
119 OSMO_GSUP_AN_APDU_IE = 0x62,
120 OSMO_GSUP_CAUSE_RR_IE = 0x63,
121 OSMO_GSUP_CAUSE_BSSAP_IE = 0x64,
122 OSMO_GSUP_CAUSE_SM_IE = 0x65,
123
124 _OSMO_GSUP_IEI_END_MARKER
125};
126
139 enum osmo_gsup_message_type {
140 OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST = 0b00000100,
141 OSMO_GSUP_MSGT_UPDATE_LOCATION_ERROR = 0b00000101,
142 OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT = 0b00000110,
143
144 OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST = 0b00001000,
145 OSMO_GSUP_MSGT_SEND_AUTH_INFO_ERROR = 0b00001001,
146 OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT = 0b00001010,
147
148 OSMO_GSUP_MSGT_AUTH_FAIL_REPORT = 0b00001011,
149
150 OSMO_GSUP_MSGT_PURGE_MS_REQUEST = 0b00001100,
151 OSMO_GSUP_MSGT_PURGE_MS_ERROR = 0b00001101,
152 OSMO_GSUP_MSGT_PURGE_MS_RESULT = 0b00001110,
153
154 OSMO_GSUP_MSGT_INSERT_DATA_REQUEST = 0b00010000,
155 OSMO_GSUP_MSGT_INSERT_DATA_ERROR = 0b00010001,
156 OSMO_GSUP_MSGT_INSERT_DATA_RESULT = 0b00010010,
157
158 OSMO_GSUP_MSGT_DELETE_DATA_REQUEST = 0b00010100,
159 OSMO_GSUP_MSGT_DELETE_DATA_ERROR = 0b00010101,
160 OSMO_GSUP_MSGT_DELETE_DATA_RESULT = 0b00010110,
161
162 OSMO_GSUP_MSGT_LOCATION_CANCEL_REQUEST = 0b00011100,
163 OSMO_GSUP_MSGT_LOCATION_CANCEL_ERROR = 0b00011101,
164 OSMO_GSUP_MSGT_LOCATION_CANCEL_RESULT = 0b00011110,
165
166 OSMO_GSUP_MSGT_PROC_SS_REQUEST = 0b00100000,
167 OSMO_GSUP_MSGT_PROC_SS_ERROR = 0b00100001,
168 OSMO_GSUP_MSGT_PROC_SS_RESULT = 0b00100010,
169
170 OSMO_GSUP_MSGT_MO_FORWARD_SM_REQUEST = 0b00100100,
171 OSMO_GSUP_MSGT_MO_FORWARD_SM_ERROR = 0b00100101,
172 OSMO_GSUP_MSGT_MO_FORWARD_SM_RESULT = 0b00100110,
173
174 OSMO_GSUP_MSGT_MT_FORWARD_SM_REQUEST = 0b00101000,
175 OSMO_GSUP_MSGT_MT_FORWARD_SM_ERROR = 0b00101001,
176 OSMO_GSUP_MSGT_MT_FORWARD_SM_RESULT = 0b00101010,
177
178 OSMO_GSUP_MSGT_READY_FOR_SM_REQUEST = 0b00101100,
179 OSMO_GSUP_MSGT_READY_FOR_SM_ERROR = 0b00101101,
180 OSMO_GSUP_MSGT_READY_FOR_SM_RESULT = 0b00101110,
181
182 OSMO_GSUP_MSGT_CHECK_IMEI_REQUEST = 0b00110000,
183 OSMO_GSUP_MSGT_CHECK_IMEI_ERROR = 0b00110001,
184 OSMO_GSUP_MSGT_CHECK_IMEI_RESULT = 0b00110010,
185
186 OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_REQUEST = 0b00110100,
187 OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_ERROR = 0b00110101,
188 OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_RESULT = 0b00110110,
189
190 OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_REQUEST = 0b00111000,
191 OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_ERROR = 0b00111001,
192 OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_RESULT = 0b00111010,
193
194 OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_REQUEST = 0b00111100,
195 OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_ERROR = 0b00111101,
196 OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_RESULT = 0b00111110,
197
198 OSMO_GSUP_MSGT_E_PROCESS_ACCESS_SIGNALLING_REQUEST = 0b01000000,
199 OSMO_GSUP_MSGT_E_FORWARD_ACCESS_SIGNALLING_REQUEST = 0b01000100,
200
201 OSMO_GSUP_MSGT_E_CLOSE = 0b01000111,
202 OSMO_GSUP_MSGT_E_ABORT = 0b01001011,
203
204 OSMO_GSUP_MSGT_ROUTING_ERROR = 0b01001110,
205
206 OSMO_GSUP_MSGT_EPDG_TUNNEL_REQUEST = 0b01010000,
207 OSMO_GSUP_MSGT_EPDG_TUNNEL_ERROR = 0b01010001,
208 OSMO_GSUP_MSGT_EPDG_TUNNEL_RESULT = 0b01010010,
209};
210
211#define OSMO_GSUP_MSGT_E_ROUTING_ERROR OSMO_GSUP_MSGT_ROUTING_ERROR
212
213#define OSMO_GSUP_IS_MSGT_REQUEST(msgt) (((msgt) & 0b00000011) == 0b00)
214#define OSMO_GSUP_IS_MSGT_ERROR(msgt) (((msgt) & 0b00000011) == 0b01)
215#define OSMO_GSUP_IS_MSGT_RESULT(msgt) (((msgt) & 0b00000011) == 0b10)
216#define OSMO_GSUP_TO_MSGT_REQUEST(msgt) (((msgt) & 0b11111100))
217#define OSMO_GSUP_TO_MSGT_ERROR(msgt) (((msgt) & 0b11111100) | 0b01)
218#define OSMO_GSUP_TO_MSGT_RESULT(msgt) (((msgt) & 0b11111100) | 0b10)
219
220 extern const struct value_string osmo_gsup_message_type_names[];
221 static inline const char *
222 osmo_gsup_message_type_name(enum osmo_gsup_message_type val)
223{ return get_value_string(osmo_gsup_message_type_names, val); }
224
225 enum osmo_gsup_cancel_type {
226 OSMO_GSUP_CANCEL_TYPE_UPDATE = 1, /* on wire: 0 */
227 OSMO_GSUP_CANCEL_TYPE_WITHDRAW = 2, /* on wire: 1 */
228};
229
230 enum osmo_gsup_cn_domain {
231 OSMO_GSUP_CN_DOMAIN_PS = 1,
232 OSMO_GSUP_CN_DOMAIN_CS = 2,
233};
234
235 enum osmo_gsup_imei_result {
236 OSMO_GSUP_IMEI_RESULT_ACK = 1, /* on wire: 0 */
237 OSMO_GSUP_IMEI_RESULT_NACK = 2, /* on wire: 1 */
238};
239
240/* 3GPP 29.002 AccessNetworkProtocolId */
241 enum osmo_gsup_access_network_protocol {
242 OSMO_GSUP_ACCESS_NETWORK_PROTOCOL_TS3G_48006 = 1,
243 OSMO_GSUP_ACCESS_NETWORK_PROTOCOL_TS3G_25413 = 2,
244};
245
247 enum osmo_gsup_session_state {
249 OSMO_GSUP_SESSION_STATE_NONE = 0x00,
251 OSMO_GSUP_SESSION_STATE_BEGIN = 0x01,
253 OSMO_GSUP_SESSION_STATE_CONTINUE = 0x02,
255 OSMO_GSUP_SESSION_STATE_END = 0x03,
256};
257
258 extern const struct value_string osmo_gsup_session_state_names[];
259 static inline const char *
260 osmo_gsup_session_state_name(enum osmo_gsup_session_state val)
261{ return get_value_string(osmo_gsup_session_state_names, val); }
262
264 struct osmo_gsup_pdp_info {
265 unsigned int context_id;
266 int have_info;
268 union {
269 uint16_t pdp_type OSMO_DEPRECATED("use pdp_type_org and pdp_type_nr instead");
270 struct {
271#if OSMO_IS_LITTLE_ENDIAN
272 uint8_t pdp_type_nr; /* enum gsm48_pdp_type_nr */
273 uint8_t pdp_type_org; /* enum gsm48_pdp_type_org */
274#elif OSMO_IS_BIG_ENDIAN
275 uint8_t pdp_type_org; /* enum gsm48_pdp_type_org */
276 uint8_t pdp_type_nr; /* enum gsm48_pdp_type_nr */
277#endif
278 };
279 };
280 struct osmo_sockaddr pdp_address[2];
283 const uint8_t *apn_enc;
285 size_t apn_enc_len;
288 const uint8_t *qos_enc;
290 size_t qos_enc_len;
293 const uint8_t *pdp_charg_enc;
295 size_t pdp_charg_enc_len;
296};
297
298 enum osmo_gsup_message_class {
299 OSMO_GSUP_MESSAGE_CLASS_UNSET = 0,
300 OSMO_GSUP_MESSAGE_CLASS_SUBSCRIBER_MANAGEMENT = 1,
301 OSMO_GSUP_MESSAGE_CLASS_SMS = 2,
302 OSMO_GSUP_MESSAGE_CLASS_USSD = 3,
303 OSMO_GSUP_MESSAGE_CLASS_INTER_MSC = 4,
304 OSMO_GSUP_MESSAGE_CLASS_IPSEC_EPDG = 5,
305 /* Keep this as last entry with a value of max(enum osmo_gsup_message_class) + 1.
306 * This value shall serve as the size for an array to aid de-muxing all known GSUP classes. */
307 OSMO_GSUP_MESSAGE_CLASS_ARRAYSIZE
308};
309
310 extern const struct value_string osmo_gsup_message_class_names[];
311 static inline const char *osmo_gsup_message_class_name(enum osmo_gsup_message_class val)
312{ return get_value_string(osmo_gsup_message_class_names, val); }
313
315 struct osmo_gsup_an_apdu {
316 /* AccessNetworkProtocolId as in 3GPP TS 29.002. */
317 enum osmo_gsup_access_network_protocol access_network_proto;
318 const uint8_t *data;
319 size_t data_len;
320};
321
323 struct osmo_gsup_message {
324 enum osmo_gsup_message_type message_type;
325 char imsi[OSMO_IMSI_BUF_SIZE];
326 enum gsm48_gmm_cause cause;
327 enum osmo_gsup_cancel_type cancel_type;
328 int pdp_info_compl;
329 int freeze_ptmsi;
330 struct osmo_auth_vector auth_vectors[OSMO_GSUP_MAX_NUM_AUTH_INFO];
331 size_t num_auth_vectors;
332 struct osmo_gsup_pdp_info pdp_infos[OSMO_GSUP_MAX_NUM_PDP_INFO];
333 size_t num_pdp_infos;
334 const uint8_t *msisdn_enc;
335 size_t msisdn_enc_len;
336 const uint8_t *hlr_enc;
337 size_t hlr_enc_len;
338 const uint8_t *auts;
339 const uint8_t *rand;
340 enum osmo_gsup_cn_domain cn_domain;
341 const uint8_t *pdp_charg_enc;
342 size_t pdp_charg_enc_len;
343
345 enum osmo_gsup_session_state session_state;
348 uint32_t session_id;
349
351 uint8_t *ss_info;
352 size_t ss_info_len;
353
357 const uint8_t *sm_rp_mr;
359 enum osmo_gsup_sms_sm_rp_oda_t sm_rp_da_type;
360 size_t sm_rp_da_len;
361 const uint8_t *sm_rp_da;
363 enum osmo_gsup_sms_sm_rp_oda_t sm_rp_oa_type;
364 size_t sm_rp_oa_len;
365 const uint8_t *sm_rp_oa;
367 const uint8_t *sm_rp_ui;
368 size_t sm_rp_ui_len;
370 const uint8_t *sm_rp_cause;
372 const uint8_t *sm_rp_mms;
374 enum osmo_gsup_sms_sm_alert_rsn_t sm_alert_rsn;
375
376 const uint8_t *imei_enc;
377 size_t imei_enc_len;
378 enum osmo_gsup_imei_result imei_result;
379
383 enum osmo_gsup_message_class message_class;
384
386 const uint8_t *source_name;
388 size_t source_name_len;
391 const uint8_t *destination_name;
393 size_t destination_name_len;
394
396 struct osmo_gsup_an_apdu an_apdu;
397
398 uint8_t cause_rr;
399 bool cause_rr_set;
401 enum gsm0808_cause cause_bssap;
402 bool cause_bssap_set;
405 enum gsm48_gsm_cause cause_sm;
406
407 enum osmo_rat_type current_rat_type;
408 enum osmo_rat_type supported_rat_types[8];
409 size_t supported_rat_types_len;
410
412 const uint8_t *pco;
414 size_t pco_len;
415
416};
417
418 int osmo_gsup_decode(const uint8_t *data, size_t data_len,
419 struct osmo_gsup_message *gsup_msg);
420 int osmo_gsup_encode(struct msgb *msg, const struct osmo_gsup_message *gsup_msg);
421 int osmo_gsup_get_err_msg_type(enum osmo_gsup_message_type type_in)
422 OSMO_DEPRECATED("Use OSMO_GSUP_TO_MSGT_ERROR() instead");
auth.h
defs.h
endian.h
osmo_gsup_message_class_name
static const char * osmo_gsup_message_class_name(enum osmo_gsup_message_class val)
Definition: gsup.h:311
osmo_gsup_session_state
osmo_gsup_session_state
TCAP-like session state.
Definition: gsup.h:247
osmo_gsup_access_network_protocol
osmo_gsup_access_network_protocol
Definition: gsup.h:241
osmo_gsup_get_err_msg_type
int osmo_gsup_get_err_msg_type(enum osmo_gsup_message_type type_in) OSMO_DEPRECATED("Use OSMO_GSUP_TO_MSGT_ERROR() instead")
return the error message type corresponding to type_in.
Definition: gsup.c:124
osmo_gsup_message_type_names
const struct value_string osmo_gsup_message_type_names[]
Definition: gsup.c:39
osmo_gsup_cancel_type
osmo_gsup_cancel_type
Definition: gsup.h:225
OSMO_GSUP_MAX_NUM_AUTH_INFO
#define OSMO_GSUP_MAX_NUM_AUTH_INFO
Maximum number of auth info inside osmo_gsup_message.
Definition: gsup.h:59
osmo_gsup_message_type_name
static const char * osmo_gsup_message_type_name(enum osmo_gsup_message_type val)
Definition: gsup.h:222
OSMO_GSUP_MAX_NUM_PDP_INFO
#define OSMO_GSUP_MAX_NUM_PDP_INFO
Maximum nubmer of PDP inside osmo_gsup_message.
Definition: gsup.h:57
osmo_gsup_sms_sm_alert_rsn_t
osmo_gsup_sms_sm_alert_rsn_t
Alert reason values, see 7.6.8.8.
Definition: gsup_sms.h:26
osmo_gsup_message_class
osmo_gsup_message_class
Definition: gsup.h:298
osmo_gsup_sms_sm_rp_oda_t
osmo_gsup_sms_sm_rp_oda_t
Possible identity types for SM-RP-{OA|DA}.
Definition: gsup_sms.h:16
osmo_gsup_iei
osmo_gsup_iei
Information Element Identifiers for GSUP IEs.
Definition: gsup.h:66
osmo_gsup_session_state_names
const struct value_string osmo_gsup_session_state_names[]
Definition: gsup.c:113
osmo_gsup_message_type
osmo_gsup_message_type
GSUP message type Make sure that new messages follow this scheme:
Definition: gsup.h:139
osmo_gsup_message_class_names
const struct value_string osmo_gsup_message_class_names[]
Definition: gsup.c:1012
osmo_gsup_session_state_name
static const char * osmo_gsup_session_state_name(enum osmo_gsup_session_state val)
Definition: gsup.h:260
osmo_gsup_encode
int osmo_gsup_encode(struct msgb *msg, const struct osmo_gsup_message *gsup_msg)
Encode a GSUP message.
Definition: gsup.c:797
osmo_gsup_decode
int osmo_gsup_decode(const uint8_t *data, size_t data_len, struct osmo_gsup_message *gsup_msg)
Decode (parse) a GSUP message.
Definition: gsup.c:356
osmo_gsup_cn_domain
osmo_gsup_cn_domain
Definition: gsup.h:230
osmo_gsup_imei_result
osmo_gsup_imei_result
Definition: gsup.h:235
OSMO_GSUP_SESSION_STATE_NONE
@ OSMO_GSUP_SESSION_STATE_NONE
Undefined session state.
Definition: gsup.h:249
OSMO_GSUP_SESSION_STATE_CONTINUE
@ OSMO_GSUP_SESSION_STATE_CONTINUE
Communication of an existing session.
Definition: gsup.h:253
OSMO_GSUP_SESSION_STATE_BEGIN
@ OSMO_GSUP_SESSION_STATE_BEGIN
Initiation of a new session.
Definition: gsup.h:251
OSMO_GSUP_SESSION_STATE_END
@ OSMO_GSUP_SESSION_STATE_END
Indication of the session end.
Definition: gsup.h:255
OSMO_GSUP_ACCESS_NETWORK_PROTOCOL_TS3G_48006
@ OSMO_GSUP_ACCESS_NETWORK_PROTOCOL_TS3G_48006
Definition: gsup.h:242
OSMO_GSUP_ACCESS_NETWORK_PROTOCOL_TS3G_25413
@ OSMO_GSUP_ACCESS_NETWORK_PROTOCOL_TS3G_25413
Definition: gsup.h:243
OSMO_GSUP_CANCEL_TYPE_UPDATE
@ OSMO_GSUP_CANCEL_TYPE_UPDATE
Definition: gsup.h:226
OSMO_GSUP_CANCEL_TYPE_WITHDRAW
@ OSMO_GSUP_CANCEL_TYPE_WITHDRAW
Definition: gsup.h:227
OSMO_GSUP_MESSAGE_CLASS_SMS
@ OSMO_GSUP_MESSAGE_CLASS_SMS
Definition: gsup.h:301
OSMO_GSUP_MESSAGE_CLASS_UNSET
@ OSMO_GSUP_MESSAGE_CLASS_UNSET
Definition: gsup.h:299
OSMO_GSUP_MESSAGE_CLASS_IPSEC_EPDG
@ OSMO_GSUP_MESSAGE_CLASS_IPSEC_EPDG
Definition: gsup.h:304
OSMO_GSUP_MESSAGE_CLASS_INTER_MSC
@ OSMO_GSUP_MESSAGE_CLASS_INTER_MSC
Definition: gsup.h:303
OSMO_GSUP_MESSAGE_CLASS_USSD
@ OSMO_GSUP_MESSAGE_CLASS_USSD
Definition: gsup.h:302
OSMO_GSUP_MESSAGE_CLASS_ARRAYSIZE
@ OSMO_GSUP_MESSAGE_CLASS_ARRAYSIZE
Definition: gsup.h:307
OSMO_GSUP_MESSAGE_CLASS_SUBSCRIBER_MANAGEMENT
@ OSMO_GSUP_MESSAGE_CLASS_SUBSCRIBER_MANAGEMENT
Definition: gsup.h:300
OSMO_GSUP_SM_RP_MR_IE
@ OSMO_GSUP_SM_RP_MR_IE
Definition: gsup.h:104
OSMO_GSUP_MSISDN_IE
@ OSMO_GSUP_MSISDN_IE
Definition: gsup.h:74
OSMO_GSUP_SOURCE_NAME_IE
@ OSMO_GSUP_SOURCE_NAME_IE
Definition: gsup.h:117
OSMO_GSUP_PDP_ADDRESS_IE
@ OSMO_GSUP_PDP_ADDRESS_IE
Definition: gsup.h:78
OSMO_GSUP_SESSION_ID_IE
@ OSMO_GSUP_SESSION_ID_IE
Definition: gsup.h:97
OSMO_GSUP_KC_IE
@ OSMO_GSUP_KC_IE
Definition: gsup.h:86
OSMO_GSUP_SESSION_STATE_IE
@ OSMO_GSUP_SESSION_STATE_IE
Definition: gsup.h:98
OSMO_GSUP_CK_IE
@ OSMO_GSUP_CK_IE
Definition: gsup.h:89
OSMO_GSUP_CAUSE_IE
@ OSMO_GSUP_CAUSE_IE
Definition: gsup.h:68
OSMO_GSUP_IK_IE
@ OSMO_GSUP_IK_IE
Definition: gsup.h:88
OSMO_GSUP_AUTH_TUPLE_IE
@ OSMO_GSUP_AUTH_TUPLE_IE
Definition: gsup.h:69
OSMO_GSUP_SM_RP_DA_IE
@ OSMO_GSUP_SM_RP_DA_IE
Definition: gsup.h:105
OSMO_GSUP_SS_INFO_IE
@ OSMO_GSUP_SS_INFO_IE
Supplementary Services payload.
Definition: gsup.h:101
OSMO_GSUP_PDP_CONTEXT_ID_IE
@ OSMO_GSUP_PDP_CONTEXT_ID_IE
Definition: gsup.h:77
OSMO_GSUP_CURRENT_RAT_TYPE_IE
@ OSMO_GSUP_CURRENT_RAT_TYPE_IE
Definition: gsup.h:95
OSMO_GSUP_FREEZE_PTMSI_IE
@ OSMO_GSUP_FREEZE_PTMSI_IE
Definition: gsup.h:73
OSMO_GSUP_SM_RP_UI_IE
@ OSMO_GSUP_SM_RP_UI_IE
Definition: gsup.h:107
OSMO_GSUP_IMEI_RESULT_IE
@ OSMO_GSUP_IMEI_RESULT_IE
Definition: gsup.h:113
OSMO_GSUP_NUM_VECTORS_REQ_IE
@ OSMO_GSUP_NUM_VECTORS_REQ_IE
Definition: gsup.h:114
OSMO_GSUP_AUTS_IE
@ OSMO_GSUP_AUTS_IE
Definition: gsup.h:91
_OSMO_GSUP_IEI_END_MARKER
@ _OSMO_GSUP_IEI_END_MARKER
Definition: gsup.h:124
OSMO_GSUP_CAUSE_RR_IE
@ OSMO_GSUP_CAUSE_RR_IE
Definition: gsup.h:120
OSMO_GSUP_SM_RP_MMS_IE
@ OSMO_GSUP_SM_RP_MMS_IE
Definition: gsup.h:109
OSMO_GSUP_CHARG_CHAR_IE
@ OSMO_GSUP_CHARG_CHAR_IE
Definition: gsup.h:82
OSMO_GSUP_PDP_INFO_IE
@ OSMO_GSUP_PDP_INFO_IE
Definition: gsup.h:71
OSMO_GSUP_ACCESS_POINT_NAME_IE
@ OSMO_GSUP_ACCESS_POINT_NAME_IE
Definition: gsup.h:80
OSMO_GSUP_CAUSE_BSSAP_IE
@ OSMO_GSUP_CAUSE_BSSAP_IE
Definition: gsup.h:121
OSMO_GSUP_CN_DOMAIN_IE
@ OSMO_GSUP_CN_DOMAIN_IE
Definition: gsup.h:93
OSMO_GSUP_RES_IE
@ OSMO_GSUP_RES_IE
Definition: gsup.h:92
OSMO_GSUP_SM_RP_OA_IE
@ OSMO_GSUP_SM_RP_OA_IE
Definition: gsup.h:106
OSMO_GSUP_MESSAGE_CLASS_IE
@ OSMO_GSUP_MESSAGE_CLASS_IE
Definition: gsup.h:76
OSMO_GSUP_IMSI_IE
@ OSMO_GSUP_IMSI_IE
Definition: gsup.h:67
OSMO_GSUP_AN_APDU_IE
@ OSMO_GSUP_AN_APDU_IE
Definition: gsup.h:119
OSMO_GSUP_SUPPORTED_RAT_TYPES_IE
@ OSMO_GSUP_SUPPORTED_RAT_TYPES_IE
Definition: gsup.h:94
OSMO_GSUP_IMEI_IE
@ OSMO_GSUP_IMEI_IE
Definition: gsup.h:112
OSMO_GSUP_SRES_IE
@ OSMO_GSUP_SRES_IE
Definition: gsup.h:85
OSMO_GSUP_RAND_IE
@ OSMO_GSUP_RAND_IE
Definition: gsup.h:84
OSMO_GSUP_PDP_INFO_COMPL_IE
@ OSMO_GSUP_PDP_INFO_COMPL_IE
Definition: gsup.h:70
OSMO_GSUP_PCO_IE
@ OSMO_GSUP_PCO_IE
Definition: gsup.h:83
OSMO_GSUP_PDP_QOS_IE
@ OSMO_GSUP_PDP_QOS_IE
Definition: gsup.h:81
OSMO_GSUP_DESTINATION_NAME_IE
@ OSMO_GSUP_DESTINATION_NAME_IE
Definition: gsup.h:118
OSMO_GSUP_CANCEL_TYPE_IE
@ OSMO_GSUP_CANCEL_TYPE_IE
Definition: gsup.h:72
OSMO_GSUP_SM_RP_CAUSE_IE
@ OSMO_GSUP_SM_RP_CAUSE_IE
Definition: gsup.h:108
OSMO_GSUP_AUTN_IE
@ OSMO_GSUP_AUTN_IE
Definition: gsup.h:90
OSMO_GSUP_SM_ALERT_RSN_IE
@ OSMO_GSUP_SM_ALERT_RSN_IE
Definition: gsup.h:110
OSMO_GSUP_CAUSE_SM_IE
@ OSMO_GSUP_CAUSE_SM_IE
Definition: gsup.h:122
OSMO_GSUP_HLR_NUMBER_IE
@ OSMO_GSUP_HLR_NUMBER_IE
Definition: gsup.h:75
OSMO_GSUP_MSGT_DELETE_DATA_ERROR
@ OSMO_GSUP_MSGT_DELETE_DATA_ERROR
Definition: gsup.h:159
OSMO_GSUP_MSGT_EPDG_TUNNEL_RESULT
@ OSMO_GSUP_MSGT_EPDG_TUNNEL_RESULT
Definition: gsup.h:208
OSMO_GSUP_MSGT_MO_FORWARD_SM_RESULT
@ OSMO_GSUP_MSGT_MO_FORWARD_SM_RESULT
Definition: gsup.h:172
OSMO_GSUP_MSGT_DELETE_DATA_REQUEST
@ OSMO_GSUP_MSGT_DELETE_DATA_REQUEST
Definition: gsup.h:158
OSMO_GSUP_MSGT_ROUTING_ERROR
@ OSMO_GSUP_MSGT_ROUTING_ERROR
Definition: gsup.h:204
OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_REQUEST
@ OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_REQUEST
Definition: gsup.h:186
OSMO_GSUP_MSGT_EPDG_TUNNEL_ERROR
@ OSMO_GSUP_MSGT_EPDG_TUNNEL_ERROR
Definition: gsup.h:207
OSMO_GSUP_MSGT_EPDG_TUNNEL_REQUEST
@ OSMO_GSUP_MSGT_EPDG_TUNNEL_REQUEST
Definition: gsup.h:206
OSMO_GSUP_MSGT_E_PROCESS_ACCESS_SIGNALLING_REQUEST
@ OSMO_GSUP_MSGT_E_PROCESS_ACCESS_SIGNALLING_REQUEST
Definition: gsup.h:198
OSMO_GSUP_MSGT_INSERT_DATA_RESULT
@ OSMO_GSUP_MSGT_INSERT_DATA_RESULT
Definition: gsup.h:156
OSMO_GSUP_MSGT_LOCATION_CANCEL_ERROR
@ OSMO_GSUP_MSGT_LOCATION_CANCEL_ERROR
Definition: gsup.h:163
OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_REQUEST
@ OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_REQUEST
Definition: gsup.h:190
OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_REQUEST
@ OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_REQUEST
Definition: gsup.h:194
OSMO_GSUP_MSGT_PURGE_MS_REQUEST
@ OSMO_GSUP_MSGT_PURGE_MS_REQUEST
Definition: gsup.h:150
OSMO_GSUP_MSGT_READY_FOR_SM_RESULT
@ OSMO_GSUP_MSGT_READY_FOR_SM_RESULT
Definition: gsup.h:180
OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT
@ OSMO_GSUP_MSGT_SEND_AUTH_INFO_RESULT
Definition: gsup.h:146
OSMO_GSUP_MSGT_DELETE_DATA_RESULT
@ OSMO_GSUP_MSGT_DELETE_DATA_RESULT
Definition: gsup.h:160
OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_ERROR
@ OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_ERROR
Definition: gsup.h:195
OSMO_GSUP_MSGT_INSERT_DATA_ERROR
@ OSMO_GSUP_MSGT_INSERT_DATA_ERROR
Definition: gsup.h:155
OSMO_GSUP_MSGT_MT_FORWARD_SM_RESULT
@ OSMO_GSUP_MSGT_MT_FORWARD_SM_RESULT
Definition: gsup.h:176
OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_RESULT
@ OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_RESULT
Definition: gsup.h:188
OSMO_GSUP_MSGT_PURGE_MS_ERROR
@ OSMO_GSUP_MSGT_PURGE_MS_ERROR
Definition: gsup.h:151
OSMO_GSUP_MSGT_PROC_SS_REQUEST
@ OSMO_GSUP_MSGT_PROC_SS_REQUEST
Definition: gsup.h:166
OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT
@ OSMO_GSUP_MSGT_UPDATE_LOCATION_RESULT
Definition: gsup.h:142
OSMO_GSUP_MSGT_LOCATION_CANCEL_RESULT
@ OSMO_GSUP_MSGT_LOCATION_CANCEL_RESULT
Definition: gsup.h:164
OSMO_GSUP_MSGT_CHECK_IMEI_ERROR
@ OSMO_GSUP_MSGT_CHECK_IMEI_ERROR
Definition: gsup.h:183
OSMO_GSUP_MSGT_SEND_AUTH_INFO_ERROR
@ OSMO_GSUP_MSGT_SEND_AUTH_INFO_ERROR
Definition: gsup.h:145
OSMO_GSUP_MSGT_PROC_SS_ERROR
@ OSMO_GSUP_MSGT_PROC_SS_ERROR
Definition: gsup.h:167
OSMO_GSUP_MSGT_MT_FORWARD_SM_REQUEST
@ OSMO_GSUP_MSGT_MT_FORWARD_SM_REQUEST
Definition: gsup.h:174
OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST
@ OSMO_GSUP_MSGT_SEND_AUTH_INFO_REQUEST
Definition: gsup.h:144
OSMO_GSUP_MSGT_UPDATE_LOCATION_ERROR
@ OSMO_GSUP_MSGT_UPDATE_LOCATION_ERROR
Definition: gsup.h:141
OSMO_GSUP_MSGT_MT_FORWARD_SM_ERROR
@ OSMO_GSUP_MSGT_MT_FORWARD_SM_ERROR
Definition: gsup.h:175
OSMO_GSUP_MSGT_E_FORWARD_ACCESS_SIGNALLING_REQUEST
@ OSMO_GSUP_MSGT_E_FORWARD_ACCESS_SIGNALLING_REQUEST
Definition: gsup.h:199
OSMO_GSUP_MSGT_PURGE_MS_RESULT
@ OSMO_GSUP_MSGT_PURGE_MS_RESULT
Definition: gsup.h:152
OSMO_GSUP_MSGT_READY_FOR_SM_REQUEST
@ OSMO_GSUP_MSGT_READY_FOR_SM_REQUEST
Definition: gsup.h:178
OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_ERROR
@ OSMO_GSUP_MSGT_E_PREPARE_HANDOVER_ERROR
Definition: gsup.h:187
OSMO_GSUP_MSGT_PROC_SS_RESULT
@ OSMO_GSUP_MSGT_PROC_SS_RESULT
Definition: gsup.h:168
OSMO_GSUP_MSGT_CHECK_IMEI_REQUEST
@ OSMO_GSUP_MSGT_CHECK_IMEI_REQUEST
Definition: gsup.h:182
OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST
@ OSMO_GSUP_MSGT_UPDATE_LOCATION_REQUEST
Definition: gsup.h:140
OSMO_GSUP_MSGT_MO_FORWARD_SM_ERROR
@ OSMO_GSUP_MSGT_MO_FORWARD_SM_ERROR
Definition: gsup.h:171
OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_RESULT
@ OSMO_GSUP_MSGT_E_SEND_END_SIGNAL_RESULT
Definition: gsup.h:196
OSMO_GSUP_MSGT_AUTH_FAIL_REPORT
@ OSMO_GSUP_MSGT_AUTH_FAIL_REPORT
Definition: gsup.h:148
OSMO_GSUP_MSGT_LOCATION_CANCEL_REQUEST
@ OSMO_GSUP_MSGT_LOCATION_CANCEL_REQUEST
Definition: gsup.h:162
OSMO_GSUP_MSGT_E_ABORT
@ OSMO_GSUP_MSGT_E_ABORT
Definition: gsup.h:202
OSMO_GSUP_MSGT_MO_FORWARD_SM_REQUEST
@ OSMO_GSUP_MSGT_MO_FORWARD_SM_REQUEST
Definition: gsup.h:170
OSMO_GSUP_MSGT_E_CLOSE
@ OSMO_GSUP_MSGT_E_CLOSE
Definition: gsup.h:201
OSMO_GSUP_MSGT_CHECK_IMEI_RESULT
@ OSMO_GSUP_MSGT_CHECK_IMEI_RESULT
Definition: gsup.h:184
OSMO_GSUP_MSGT_READY_FOR_SM_ERROR
@ OSMO_GSUP_MSGT_READY_FOR_SM_ERROR
Definition: gsup.h:179
OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_RESULT
@ OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_RESULT
Definition: gsup.h:192
OSMO_GSUP_MSGT_INSERT_DATA_REQUEST
@ OSMO_GSUP_MSGT_INSERT_DATA_REQUEST
Definition: gsup.h:154
OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_ERROR
@ OSMO_GSUP_MSGT_E_PREPARE_SUBSEQUENT_HANDOVER_ERROR
Definition: gsup.h:191
OSMO_GSUP_CN_DOMAIN_PS
@ OSMO_GSUP_CN_DOMAIN_PS
Definition: gsup.h:231
OSMO_GSUP_CN_DOMAIN_CS
@ OSMO_GSUP_CN_DOMAIN_CS
Definition: gsup.h:232
OSMO_GSUP_IMEI_RESULT_NACK
@ OSMO_GSUP_IMEI_RESULT_NACK
Definition: gsup.h:237
OSMO_GSUP_IMEI_RESULT_ACK
@ OSMO_GSUP_IMEI_RESULT_ACK
Definition: gsup.h:236
data
uint8_t data[0]
OSMO_DEPRECATED
#define OSMO_DEPRECATED(text)
get_value_string
const char * get_value_string(const struct value_string *vs, uint32_t val)
gsm_03_40.h
GSM TS 03.40.
gsm_04_08_gprs.h
gsm48_gmm_cause
gsm48_gmm_cause
Definition: gsm_04_08_gprs.h:235
gsm48_gsm_cause
gsm48_gsm_cause
Definition: gsm_04_08_gprs.h:271
gsm_08_08.h
gsm0808_cause
gsm0808_cause
Definition: gsm_08_08.h:367
msg
uint8_t msg[0]
Definition: gsm_08_08.h:8
gsm_23_003.h
OSMO_IMSI_BUF_SIZE
#define OSMO_IMSI_BUF_SIZE
The char[] buffer size to completely contain an IMSI including the optional checksum digit as well as...
Definition: gsm_23_003.h:10
gsm_utils.h
GSM utility functions, e.g.
osmo_rat_type
osmo_rat_type
Definition: gsm_utils.h:262
gsup_sms.h
SMS (Short Message Service) extensions for Osmocom GSUP.
msgb.h
socket.h
msgb
osmo_auth_vector
Definition: auth.h:89
osmo_gsup_an_apdu
AccessNetworkSignalInfo as in 3GPP TS 29.002.
Definition: gsup.h:315
osmo_gsup_an_apdu::data_len
size_t data_len
Definition: gsup.h:319
osmo_gsup_an_apdu::data
const uint8_t * data
Definition: gsup.h:318
osmo_gsup_an_apdu::access_network_proto
enum osmo_gsup_access_network_protocol access_network_proto
Definition: gsup.h:317
osmo_gsup_message
parsed/decoded GSUP protocol message
Definition: gsup.h:323
osmo_gsup_message::pdp_charg_enc_len
size_t pdp_charg_enc_len
Definition: gsup.h:342
osmo_gsup_message::msisdn_enc_len
size_t msisdn_enc_len
Definition: gsup.h:335
osmo_gsup_message::source_name_len
size_t source_name_len
Number of bytes in source_name.
Definition: gsup.h:388
osmo_gsup_message::cause_rr
uint8_t cause_rr
0 is a valid cause
Definition: gsup.h:398
osmo_gsup_message::cancel_type
enum osmo_gsup_cancel_type cancel_type
Definition: gsup.h:327
osmo_gsup_message::sm_rp_mr
const uint8_t * sm_rp_mr
SM-RP-MR (see 3GPP TS 29.002, 7.6.1.1), Message Reference.
Definition: gsup.h:357
osmo_gsup_message::imei_enc_len
size_t imei_enc_len
Definition: gsup.h:377
osmo_gsup_message::cause_bssap_set
bool cause_bssap_set
whether cause_bssap is set
Definition: gsup.h:402
osmo_gsup_message::cause_rr_set
bool cause_rr_set
whether cause_rr is set
Definition: gsup.h:399
osmo_gsup_message::sm_rp_ui_len
size_t sm_rp_ui_len
Definition: gsup.h:368
osmo_gsup_message::auts
const uint8_t * auts
Definition: gsup.h:338
osmo_gsup_message::hlr_enc
const uint8_t * hlr_enc
Definition: gsup.h:336
osmo_gsup_message::num_auth_vectors
size_t num_auth_vectors
Definition: gsup.h:331
osmo_gsup_message::message_type
enum osmo_gsup_message_type message_type
Definition: gsup.h:324
osmo_gsup_message::pdp_infos
struct osmo_gsup_pdp_info pdp_infos[OSMO_GSUP_MAX_NUM_PDP_INFO]
Definition: gsup.h:332
osmo_gsup_message::ss_info_len
size_t ss_info_len
Definition: gsup.h:352
osmo_gsup_message::supported_rat_types_len
size_t supported_rat_types_len
Definition: gsup.h:409
osmo_gsup_message::ss_info
uint8_t * ss_info
ASN.1 encoded MAP payload for Supplementary Services.
Definition: gsup.h:351
osmo_gsup_message::sm_rp_oa_type
enum osmo_gsup_sms_sm_rp_oda_t sm_rp_oa_type
SM-RP-OA (see 3GPP TS 29.002, 7.6.8.2), Originating Address.
Definition: gsup.h:363
osmo_gsup_message::pco_len
size_t pco_len
Number of bytes of the PCO.
Definition: gsup.h:414
osmo_gsup_message::sm_rp_da_len
size_t sm_rp_da_len
Definition: gsup.h:360
osmo_gsup_message::freeze_ptmsi
int freeze_ptmsi
Definition: gsup.h:329
osmo_gsup_message::destination_name
const uint8_t * destination_name
For messages routed via another GSUP entity (via HLR), the IPA name of the entity that should ultimat...
Definition: gsup.h:391
osmo_gsup_message::imei_enc
const uint8_t * imei_enc
Definition: gsup.h:376
osmo_gsup_message::sm_alert_rsn
enum osmo_gsup_sms_sm_alert_rsn_t sm_alert_rsn
Alert reason (see 3GPP TS 29.002, 7.6.8.8)
Definition: gsup.h:374
osmo_gsup_message::imsi
char imsi[OSMO_IMSI_BUF_SIZE]
Definition: gsup.h:325
osmo_gsup_message::cn_domain
enum osmo_gsup_cn_domain cn_domain
Definition: gsup.h:340
osmo_gsup_message::source_name
const uint8_t * source_name
For messages routed via another GSUP entity (via HLR), the IPA name of the entity that sent this mess...
Definition: gsup.h:386
osmo_gsup_message::sm_rp_ui
const uint8_t * sm_rp_ui
SM-RP-UI (see 3GPP TS 29.002, 7.6.8.4), SMS TPDU.
Definition: gsup.h:367
osmo_gsup_message::cause
enum gsm48_gmm_cause cause
Definition: gsup.h:326
osmo_gsup_message::sm_rp_cause
const uint8_t * sm_rp_cause
SM-RP-Cause value (1 oct.) as per GSM TS 04.11, section 8.2.5.4.
Definition: gsup.h:370
osmo_gsup_message::num_pdp_infos
size_t num_pdp_infos
Definition: gsup.h:333
osmo_gsup_message::sm_rp_da_type
enum osmo_gsup_sms_sm_rp_oda_t sm_rp_da_type
SM-RP-DA (see 3GPP TS 29.002, 7.6.8.1), Destination Address.
Definition: gsup.h:359
osmo_gsup_message::cause_bssap
enum gsm0808_cause cause_bssap
0 is a valid cause
Definition: gsup.h:401
osmo_gsup_message::imei_result
enum osmo_gsup_imei_result imei_result
Definition: gsup.h:378
osmo_gsup_message::sm_rp_oa_len
size_t sm_rp_oa_len
Definition: gsup.h:364
osmo_gsup_message::sm_rp_oa
const uint8_t * sm_rp_oa
Definition: gsup.h:365
osmo_gsup_message::an_apdu
struct osmo_gsup_an_apdu an_apdu
inter-MSC AN-APDU.
Definition: gsup.h:396
osmo_gsup_message::cause_sm
enum gsm48_gsm_cause cause_sm
Session Management cause as of 3GPP TS 24.008 10.5.6.6 / Table 10.5.157.
Definition: gsup.h:405
osmo_gsup_message::pco
const uint8_t * pco
PCO protocol option 3GPP TS 24.008 10.5.6.3 / Table 10.5.136.
Definition: gsup.h:412
osmo_gsup_message::msisdn_enc
const uint8_t * msisdn_enc
Definition: gsup.h:334
osmo_gsup_message::session_state
enum osmo_gsup_session_state session_state
Session state osmo_gsup_session_state.
Definition: gsup.h:345
osmo_gsup_message::destination_name_len
size_t destination_name_len
Number of bytes in destination_name.
Definition: gsup.h:393
osmo_gsup_message::auth_vectors
struct osmo_auth_vector auth_vectors[OSMO_GSUP_MAX_NUM_AUTH_INFO]
Definition: gsup.h:330
osmo_gsup_message::supported_rat_types
enum osmo_rat_type supported_rat_types[8]
arbitrary choice
Definition: gsup.h:408
osmo_gsup_message::current_rat_type
enum osmo_rat_type current_rat_type
Definition: gsup.h:407
osmo_gsup_message::rand
const uint8_t * rand
Definition: gsup.h:339
osmo_gsup_message::sm_rp_mms
const uint8_t * sm_rp_mms
SM-RP-MMS (More Messages to Send), section 7.6.8.7.
Definition: gsup.h:372
osmo_gsup_message::sm_rp_da
const uint8_t * sm_rp_da
Definition: gsup.h:361
osmo_gsup_message::pdp_info_compl
int pdp_info_compl
Definition: gsup.h:328
osmo_gsup_message::message_class
enum osmo_gsup_message_class message_class
Indicate the message class to trivially dispatch incoming GSUP messages to the right code paths.
Definition: gsup.h:383
osmo_gsup_message::pdp_charg_enc
const uint8_t * pdp_charg_enc
Definition: gsup.h:341
osmo_gsup_message::session_id
uint32_t session_id
Unique session identifier and origination flag.
Definition: gsup.h:348
osmo_gsup_message::hlr_enc_len
size_t hlr_enc_len
Definition: gsup.h:337
osmo_gsup_pdp_info
parsed/decoded PDP context information
Definition: gsup.h:264
osmo_gsup_pdp_info::pdp_charg_enc
const uint8_t * pdp_charg_enc
PDP Charging Characteristics, still in encoded form.
Definition: gsup.h:293
osmo_gsup_pdp_info::qos_enc_len
size_t qos_enc_len
length (in octets) of qos_enc
Definition: gsup.h:290
osmo_gsup_pdp_info::context_id
unsigned int context_id
Definition: gsup.h:265
osmo_gsup_pdp_info::apn_enc
const uint8_t * apn_enc
APN information, still in encoded form.
Definition: gsup.h:283
osmo_gsup_pdp_info::pdp_charg_enc_len
size_t pdp_charg_enc_len
length (in octets) of pdp_charg_enc
Definition: gsup.h:295
osmo_gsup_pdp_info::qos_enc
const uint8_t * qos_enc
QoS information, still in encoded form.
Definition: gsup.h:288
osmo_gsup_pdp_info::pdp_address
struct osmo_sockaddr pdp_address[2]
Definition: gsup.h:280
osmo_gsup_pdp_info::apn_enc_len
size_t apn_enc_len
length (in octets) of apn_enc
Definition: gsup.h:285
osmo_gsup_pdp_info::have_info
int have_info
Definition: gsup.h:266
osmo_sockaddr
value_string