libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Functions
gsm44021.h File Reference
`#include <osmocom/isdn/v110.h>`

Go to the source code of this file.

## Functions
int | osmo_csd_12k_6k_decode_frame (struct osmo_v110_decoded_frame *fr, const ubit_t *ra_bits, size_t n_bits)
| Decode a 60-bit GSM 12kbit/s CSD frame present as 60 ubits into a struct osmo_v110_decoded_frame. More...
int | osmo_csd_12k_6k_encode_frame (ubit_t *ra_bits, size_t ra_bits_size, const struct osmo_v110_decoded_frame *fr)
int | osmo_csd_3k6_decode_frame (struct osmo_v110_decoded_frame *fr, const ubit_t *ra_bits, size_t n_bits)
| Decode a 36-bit GSM 3k6kbit/s CSD frame present as 36 ubits into a struct osmo_v110_decoded_frame. More...
int | osmo_csd_3k6_encode_frame (ubit_t *ra_bits, size_t ra_bits_size, const struct osmo_v110_decoded_frame *fr)
void | osmo_csd_ubit_dump (FILE *outf, const ubit_t *fr, size_t in_len)
| Print a encoded "CSD modififed V.110" frame in the same table-like structure as the spec. More...

## Function Documentation

## ◆ osmo_csd_12k_6k_decode_frame()

int osmo_csd_12k_6k_decode_frame | ( | struct osmo_v110_decoded_frame * | fr,
|  | const ubit_t * | ra_bits,
|  | size_t | n_bits
| ) |  |

Decode a 60-bit GSM 12kbit/s CSD frame present as 60 ubits into a struct osmo_v110_decoded_frame.

Parameters

  [out] | caller-allocated | output data structure, filled by this function
  [in] | ra_bits | One V.110 frame as 60 unpacked bits.

References osmo_v110_decoded_frame::d_bits, osmo_v110_decoded_frame::e_bits, osmo_v110_decoded_frame::s_bits, and osmo_v110_decoded_frame::x_bits.

## ◆ osmo_csd_12k_6k_encode_frame()

int osmo_csd_12k_6k_encode_frame | ( | ubit_t * | ra_bits,
|  | size_t | ra_bits_size,
|  | const struct osmo_v110_decoded_frame * | fr
| ) |  |

References osmo_v110_decoded_frame::d_bits, osmo_v110_decoded_frame::e_bits, osmo_v110_decoded_frame::s_bits, and osmo_v110_decoded_frame::x_bits.

## ◆ osmo_csd_3k6_decode_frame()

int osmo_csd_3k6_decode_frame | ( | struct osmo_v110_decoded_frame * | fr,
|  | const ubit_t * | ra_bits,
|  | size_t | n_bits
| ) |  |

Decode a 36-bit GSM 3k6kbit/s CSD frame present as 36 ubits into a struct osmo_v110_decoded_frame.

Parameters

  [out] | caller-allocated | output data structure, filled by this function
  [in] | ra_bits | One V.110 frame as 36 unpacked bits.

References osmo_v110_decoded_frame::d_bits, osmo_v110_decoded_frame::e_bits, OSMO_ASSERT, osmo_v110_decoded_frame::s_bits, and osmo_v110_decoded_frame::x_bits.

## ◆ osmo_csd_3k6_encode_frame()

int osmo_csd_3k6_encode_frame | ( | ubit_t * | ra_bits,
|  | size_t | ra_bits_size,
|  | const struct osmo_v110_decoded_frame * | fr
| ) |  |

References osmo_v110_decoded_frame::d_bits, osmo_v110_decoded_frame::e_bits, OSMO_ASSERT, osmo_v110_decoded_frame::s_bits, and osmo_v110_decoded_frame::x_bits.

## ◆ osmo_csd_ubit_dump()

void osmo_csd_ubit_dump | ( | FILE * | outf,
|  | const ubit_t * | fr,
|  | size_t | in_len
| ) |  |

Print a encoded "CSD modififed V.110" frame in the same table-like structure as the spec.

Parameters

  | outf | output FILE stream to which to dump
  [in] | fr | unpacked bits to dump
  [in] | in_len | length of unpacked bits available at fr.