libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
osmo_iuup_rnl_status Struct Reference

`#include <iuup.h>`

## Data Fields
enum iuup_procedure | procedure
union {
struct {
enum iuup_error_cause cause
enum iuup_error_distance distance
} error_event
struct {
uint16_t mode_version
uint8_t data_pdu_type
uint8_t num_rfci
uint8_t num_subflows
bool IPTIs_present
struct osmo_iuup_rfci rfci [IUUP_MAX_RFCIS]
} initialization
struct {
} rate_control
struct {
} time_alignment
} | u

## Field Documentation

## ◆ cause

enum iuup_error_cause osmo_iuup_rnl_status::cause

Referenced by irp_error_event_alloc_c().

## ◆ data_pdu_type

uint8_t osmo_iuup_rnl_status::data_pdu_type

Referenced by irp_init_ind_alloc().

## ◆ distance

enum iuup_error_distance osmo_iuup_rnl_status::distance

Referenced by irp_error_event_alloc_c().

## ◆

struct { ... } osmo_iuup_rnl_status::error_event

Referenced by irp_error_event_alloc_c().

## ◆

struct { ... } osmo_iuup_rnl_status::initialization

Referenced by irp_init_ind_alloc().

## ◆ IPTIs_present

bool osmo_iuup_rnl_status::IPTIs_present

Referenced by irp_init_ind_alloc().

## ◆ mode_version

uint16_t osmo_iuup_rnl_status::mode_version

Referenced by irp_init_ind_alloc().

## ◆ num_rfci

uint8_t osmo_iuup_rnl_status::num_rfci

Referenced by irp_init_ind_alloc().

## ◆ num_subflows

uint8_t osmo_iuup_rnl_status::num_subflows

Referenced by irp_init_ind_alloc().

## ◆ procedure

enum iuup_procedure osmo_iuup_rnl_status::procedure

Referenced by irp_error_event_alloc_c(), and irp_init_ind_alloc().

## ◆

struct { ... } osmo_iuup_rnl_status::rate_control

## ◆ rfci

struct osmo_iuup_rfci osmo_iuup_rnl_status::rfci[IUUP_MAX_RFCIS]

Referenced by irp_init_ind_alloc().

## ◆

struct { ... } osmo_iuup_rnl_status::time_alignment

## ◆

union { ... } osmo_iuup_rnl_status::u

Referenced by irp_error_event_alloc_c(), and irp_init_ind_alloc().

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/iuup.h