libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - d -

- data : abis_om_fom_hdr, abis_om_hdr, abis_rsl_cchan_hdr, abis_rsl_common_hdr, abis_rsl_dchan_hdr, abis_rsl_rll_hdr, gsm0808_application_data, gsm341_etws_message, gsm341_ms_message, gsm411_rp_hdr, gsm48_act_pdp_ctx_req, gsm48_add_ass, gsm48_ass_cmd, gsm48_chan_rel, gsm48_cm_change, gsm48_hdr, gsm48_ho_cmd, gsm48_ho_cpl, gsm48_notification_nch, gsm48_system_information_type_4, gsm48_talker_indication, gsm_mncc_bearer_cap, ipaccess_head, ipaccess_head_ext, osmo_bssap_le_header, osmo_cbsp_content, osmo_gsup_an_apdu, osmo_iuup_rnl_prim, osmo_phsap_prim
- data_asym_pref : gsm0808_channel_type
- data_asym_pref_is_set : gsm0808_channel_type
- data_ident : gsm0808_notification_data
- data_len : gsm0808_application_data, osmo_gsup_an_apdu
- data_pdu_type : osmo_iuup_rnl_config, osmo_iuup_rnl_status
- data_rate : gsm0808_channel_type
- data_rate_allowed : gsm0808_channel_type
- data_rate_allowed_is_set : gsm0808_channel_type
- data_transparent : gsm0808_channel_type
- datalink : lapdm_entity
- date : sdp_firmware, sdp_header_entry
- dcs : gsm23041_msg_param_gsm, gsm23041_msg_param_umts, gsm341_ms_message, osmo_cbsp_write_replace
- def : tlv_definition
- delay_class : gsm48_qos
- deliv_err_sdu : gsm48_qos
- deliv_order : gsm48_qos
- descr : gsm_mncc_progress
- destination_name : osmo_gsup_message
- destination_name_len : osmo_gsup_message
- diag : gsm_mncc_cause
- diag_len : gsm_mncc_cause
- diag_val : lcs_cause_ie
- diag_val_present : lcs_cause_ie
- digits : gsm48_loc_area_id, gsm48_ra_id
- discr : bssap_le_pdu
- distance : fn_remap_table, osmo_iuup_rnl_status
- dl : lapdm_datalink, lapdm_msg_ctx
- dl_advanced_rx_perf : gsm48_classmark3
- downlink : gprs_cs_desc, info_ciph_req_param
- downlink_dtx_flag : gsm0808_vgcs_vbs_assign_req
- downlink_dtx_flag_present : gsm0808_vgcs_vbs_assign_req
- drx_timer_max : osmo_gprs_cell_options
- dtap_err : osmo_bssap_le_err
- dtm_egprs_high_multislot_cap : gsm48_classmark3
- dtm_egprs_multislot_cap : gsm48_classmark3
- dtm_enhancements_cap : gsm48_classmark3
- dtm_gprs_high_multislot_cap : gsm48_classmark3
- dtm_gprs_multislot_cap : gsm48_classmark3
- dtm_support : osmo_gsm48_si6_ro_info
- dtm_supported : osmo_gprs_cell_options
- dtmf : gsm_mncc_cccap
- dtx_dtu : rsl_ie_chan_mode