libosmogsm 1.13.1.1-afb4 Osmocom GSM library

Data Fields
gsm0808_uplink_seized_cmd Struct Reference
GSM 08.08 / 3GPP TS 48.008 A Interface

3GPP TS 48.008 §3.2.1.63 (VGCS) UPLINK SEIZED COMMAND More...

`#include <gsm0808.h>`

## Data Fields
enum gsm0808_cause | cause
bool | talker_priority_present
enum gsm0808_talker_priority | talker_priority
bool | emerg_set_ind_present
bool | talker_identity_present
struct gsm0808_talker_identity | talker_identity

## Detailed Description

3GPP TS 48.008 §3.2.1.63 (VGCS) UPLINK SEIZED COMMAND

## Field Documentation

## ◆ cause

enum gsm0808_cause gsm0808_uplink_seized_cmd::cause

## ◆ emerg_set_ind_present

bool gsm0808_uplink_seized_cmd::emerg_set_ind_present

## ◆ talker_identity

struct gsm0808_talker_identity gsm0808_uplink_seized_cmd::talker_identity

## ◆ talker_identity_present

bool gsm0808_uplink_seized_cmd::talker_identity_present

## ◆ talker_priority

enum gsm0808_talker_priority gsm0808_uplink_seized_cmd::talker_priority

## ◆ talker_priority_present

bool gsm0808_uplink_seized_cmd::talker_priority_present

The documentation for this struct was generated from the following file:

- include/osmocom/gsm/gsm0808.h