osmo-gmr 0.2.104-2b98 Osmocom GMR-1

Files | Functions
FACCH3 channel coding
GMR-1 Layer 1 library » Channel coder / decoders

## Files
file | facch3.h
| Osmocom GMR-1 FACCH3 channel coding header.
file | facch3.c
| Osmocom GMR-1 FACCH3 channel coding implementation.

## Functions
void | gmr1_facch3_encode (ubit_t *bits_e, const uint8_t *l2, const ubit_t *bits_s, const ubit_t *ciph)
| Stateless GMR-1 FACCH3 channel coder. More...
int | gmr1_facch3_decode (uint8_t *l2, ubit_t *bits_s, const sbit_t *bits_e, const ubit_t *ciph, int *conv_rv)
| Stateless GMR-1 FACCH3 channel decoder. More...

## Detailed Description

## Function Documentation

## ◆ gmr1_facch3_decode()

int gmr1_facch3_decode | ( | uint8_t * | l2,
|  | ubit_t * | bits_s,
|  | const sbit_t * | bits_e,
|  | const ubit_t * | ciph,
|  | int * | conv_rv
| ) |  |

Stateless GMR-1 FACCH3 channel decoder.

Parameters

  [out] | l2 | L2 packet data
  [out] | bits_s | 4*8 status bits de-multiplexed
  [in] | bits_e | 4*104 encoded bits of 4 bursts
  [in] | ciph | 4*96 bits of cipher stream (can be NULL)
  [out] | conv_rv | Return of the convolutional decode (can be NULL)

Returns
  0 if CRC check pass, any other value for fail.

L2 data is 10 byte long. bits_s is 32 bits, 8 bits for each of the 4 burts, organized as 4 s_n followed by 4 s_p, as shown in section 7.3.2.2. bits_e is a 424 soft bits array unmapped from 4 bursts. ciph is the A5 cipher stream to use, 96 bits for each of the 4 burts.

References gmr1_deinterleave_intra(), gmr1_scramble_sbit(), and osmo_conv_decode().

## ◆ gmr1_facch3_encode()

void gmr1_facch3_encode | ( | ubit_t * | bits_e,
|  | const uint8_t * | l2,
|  | const ubit_t * | bits_s,
|  | const ubit_t * | ciph
| ) |  |

Stateless GMR-1 FACCH3 channel coder.

Parameters

  [out] | bits_e | 4*104 encoded bits of 4 bursts
  [in] | l2 | L2 packet data
  [in] | bits_s | 4*8 status bits to be multiplexed
  [in] | ciph | 4*96 bits of cipher stream (can be NULL)

L2 data is 10 byte long. bits_s is 32 bits, 8 bits for each of the 4 burts, organized as 4 s_n followed by 4 s_p, as shown in section 7.3.2.2. bits_e is a 432 hard bit array to be mapped on 4 bursts. ciph is the A5 cipher stream to use, 96 bits for each of the 4 burts.

References gmr1_crc16, osmo_conv_encode(), osmo_crc16gen_set_bits(), and osmo_pbit2ubit_ext().