libosmogsm 1.13.1.1-afb4 Osmocom GSM library

gsm_08_08.h
Go to the documentation of this file.
1/* From GSM08.08 / 3GPP TS 48.008 version 11.7.0 Release 11 */
2
3#pragma once
4
5#include <stdlib.h>
6#include <stdbool.h>
7#include <stdint.h>
8#include <osmocom/core/linuxlist.h>
9#include <osmocom/core/utils.h>
10#include <osmocom/core/endian.h>
11
12/*
13 * this is from GSM 03.03 CGI but is copied in GSM 08.08
14 * in § 3.2.2.27 for Cell Identifier List.
15 * See gsm0808_cell_id_discr_name() for a human readable representation.
16 */
17 enum CELL_IDENT {
18 CELL_IDENT_WHOLE_GLOBAL = 0,
19 CELL_IDENT_LAC_AND_CI = 1,
20 CELL_IDENT_CI = 2,
21 CELL_IDENT_NO_CELL = 3,
22 CELL_IDENT_LAI = 4,
23 CELL_IDENT_LAC = 5,
24 CELL_IDENT_BSS = 6,
25 CELL_IDENT_UTRAN_PLMN_LAC_RNC = 8,
26 CELL_IDENT_UTRAN_RNC = 9,
27 CELL_IDENT_UTRAN_LAC_RNC = 10,
28 CELL_IDENT_SAI = 11,
29
30 /* Not in 03.03 nor 08.08. Place them > 0x0f (discr_id is 4 bits) */
31 CELL_IDENT_WHOLE_GLOBAL_PS = 128, /* CGI + RAC, TS 48.018 8c.1.4.1.1 */
32};
33/* Keep this misnamed CELL_IDENT for API backwards compatibility (see OS#3124). */
34#define CELL_IDENT_LAI_AND_LAC CELL_IDENT_LAI
35
36/* GSM 08.06 § 6.3 */
37 enum BSSAP_MSG_TYPE {
38 BSSAP_MSG_BSS_MANAGEMENT = 0x0,
39 BSSAP_MSG_DTAP = 0x1,
40};
41
42 struct bssmap_header {
43 uint8_t type;
44 uint8_t length;
45} __attribute__((packed));
46
47 struct dtap_header {
48 uint8_t type;
49 union {
50 uint8_t link_id; /* Backward compatibility */
51 struct {
52#if OSMO_IS_LITTLE_ENDIAN
53 uint8_t dlci_sapi:3, /* enum gsm0406_dlci_sapi */
54 dlci_spare:3,
55 dlci_cc:2;
56#elif OSMO_IS_BIG_ENDIAN
57/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
58 uint8_t dlci_cc:2, dlci_spare:3, dlci_sapi:3;
59#endif
60 };
61 };
62 uint8_t length;
63} __attribute__((packed));
64
65/* Data Link Control SAPI, GSM 08.06 § 6.3.2, GSM 04.06 § 3.3.3 */
66 enum gsm0406_dlci_sapi {
67 DLCI_SAPI_RR_MM_CC = 0x0,
68 DLCI_SAPI_SMS = 0x3,
69};
70 extern const struct value_string gsm0406_dlci_sapi_names[];
71 static inline const char *gsm0406_dlci_sapi_name(enum gsm0406_dlci_sapi val)
72{ return get_value_string(gsm0406_dlci_sapi_names, val); }
73
74 enum BSS_MAP_MSG_TYPE {
75 BSS_MAP_MSG_RESERVED_0 = 0,
76
77 /* ASSIGNMENT MESSAGES */
78 BSS_MAP_MSG_ASSIGNMENT_RQST = 1,
79 BSS_MAP_MSG_ASSIGNMENT_COMPLETE = 2,
80 BSS_MAP_MSG_ASSIGNMENT_FAILURE = 3,
81 BSS_MAP_MSG_CHAN_MOD_RQST = 8,
82
83 /* HANDOVER MESSAGES */
84 BSS_MAP_MSG_HANDOVER_RQST = 16,
85 BSS_MAP_MSG_HANDOVER_REQUIRED = 17,
86 BSS_MAP_MSG_HANDOVER_RQST_ACKNOWLEDGE= 18,
87 BSS_MAP_MSG_HANDOVER_CMD = 19,
88 BSS_MAP_MSG_HANDOVER_COMPLETE = 20,
89 BSS_MAP_MSG_HANDOVER_SUCCEEDED = 21,
90 BSS_MAP_MSG_HANDOVER_FAILURE = 22,
91 BSS_MAP_MSG_HANDOVER_PERFORMED = 23,
92 BSS_MAP_MSG_HANDOVER_CANDIDATE_ENQUIRE = 24,
93 BSS_MAP_MSG_HANDOVER_CANDIDATE_RESPONSE = 25,
94 BSS_MAP_MSG_HANDOVER_REQUIRED_REJECT = 26,
95 BSS_MAP_MSG_HANDOVER_DETECT = 27,
96 BSS_MAP_MSG_INT_HANDOVER_REQUIRED = 0x70,
97 BSS_MAP_MSG_INT_HANDOVER_REQUIRED_REJ = 0x71,
98 BSS_MAP_MSG_INT_HANDOVER_CMD = 0x72,
99 BSS_MAP_MSG_INT_HANDOVER_ENQUIRY = 0x73,
100
101 /* RELEASE MESSAGES */
102 BSS_MAP_MSG_CLEAR_CMD = 32,
103 BSS_MAP_MSG_CLEAR_COMPLETE = 33,
104 BSS_MAP_MSG_CLEAR_RQST = 34,
105 BSS_MAP_MSG_RESERVED_1 = 35,
106 BSS_MAP_MSG_RESERVED_2 = 36,
107 BSS_MAP_MSG_SAPI_N_REJECT = 37,
108 BSS_MAP_MSG_CONFUSION = 38,
109
110 /* OTHER CONNECTION RELATED MESSAGES */
111 BSS_MAP_MSG_SUSPEND = 40,
112 BSS_MAP_MSG_RESUME = 41,
113 BSS_MAP_MSG_CONNECTION_ORIENTED_INFORMATION = 42,
114 BSS_MAP_MSG_PERFORM_LOCATION_RQST = 43,
115 BSS_MAP_MSG_LSA_INFORMATION = 44,
116 BSS_MAP_MSG_PERFORM_LOCATION_RESPONSE = 45,
117 BSS_MAP_MSG_PERFORM_LOCATION_ABORT = 46,
118 BSS_MAP_MSG_COMMON_ID = 47,
119 BSS_MAP_MSG_REROUTE_CMD = 0x78,
120 BSS_MAP_MSG_REROUTE_COMPLETE = 0x79,
121
122 /* GENERAL MESSAGES */
123 BSS_MAP_MSG_RESET = 48,
124 BSS_MAP_MSG_RESET_ACKNOWLEDGE = 49,
125 BSS_MAP_MSG_OVERLOAD = 50,
126 BSS_MAP_MSG_RESERVED_3 = 51,
127 BSS_MAP_MSG_RESET_CIRCUIT = 52,
128 BSS_MAP_MSG_RESET_CIRCUIT_ACKNOWLEDGE = 53,
129 BSS_MAP_MSG_MSC_INVOKE_TRACE = 54,
130 BSS_MAP_MSG_BSS_INVOKE_TRACE = 55,
131 BSS_MAP_MSG_CONNECTIONLESS_INFORMATION = 58,
132 BSS_MAP_MSG_RESET_IP_RSRC = 0x3d,
133 BSS_MAP_MSG_RESET_IP_RSRC_ACK = 0x3e,
134
135 /* TERRESTRIAL RESOURCE MESSAGES */
136 BSS_MAP_MSG_BLOCK = 64,
137 BSS_MAP_MSG_BLOCKING_ACKNOWLEDGE = 65,
138 BSS_MAP_MSG_UNBLOCK = 66,
139 BSS_MAP_MSG_UNBLOCKING_ACKNOWLEDGE = 67,
140 BSS_MAP_MSG_CIRCUIT_GROUP_BLOCK = 68,
141 BSS_MAP_MSG_CIRCUIT_GROUP_BLOCKING_ACKNOWLEDGE = 69,
142 BSS_MAP_MSG_CIRCUIT_GROUP_UNBLOCK = 70,
143 BSS_MAP_MSG_CIRCUIT_GROUP_UNBLOCKING_ACKNOWLEDGE = 71,
144 BSS_MAP_MSG_UNEQUIPPED_CIRCUIT = 72,
145 BSS_MAP_MSG_CHANGE_CIRCUIT = 78,
146 BSS_MAP_MSG_CHANGE_CIRCUIT_ACKNOWLEDGE = 79,
147
148 /* RADIO RESOURCE MESSAGES */
149 BSS_MAP_MSG_RESOURCE_RQST = 80,
150 BSS_MAP_MSG_RESOURCE_INDICATION = 81,
151 BSS_MAP_MSG_PAGING = 82,
152 BSS_MAP_MSG_CIPHER_MODE_CMD = 83,
153 BSS_MAP_MSG_CLASSMARK_UPDATE = 84,
154 BSS_MAP_MSG_CIPHER_MODE_COMPLETE = 85,
155 BSS_MAP_MSG_QUEUING_INDICATION = 86,
156 BSS_MAP_MSG_COMPLETE_LAYER_3 = 87,
157 BSS_MAP_MSG_CLASSMARK_RQST = 88,
158 BSS_MAP_MSG_CIPHER_MODE_REJECT = 89,
159 BSS_MAP_MSG_LOAD_INDICATION = 90,
160
161 /* VGCS/VBS */
162 BSS_MAP_MSG_VGCS_VBS_SETUP = 4,
163 BSS_MAP_MSG_VGCS_VBS_SETUP_ACK = 5,
164 BSS_MAP_MSG_VGCS_VBS_SETUP_REFUSE = 6,
165 BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_RQST = 7,
166 BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_RESULT = 28,
167 BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_FAILURE = 29,
168 BSS_MAP_MSG_VGCS_VBS_QUEUING_INDICATION = 30,
169 BSS_MAP_MSG_UPLINK_RQST = 31,
170 BSS_MAP_MSG_UPLINK_RQST_ACKNOWLEDGE = 39,
171 BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_STATUS = 59,
172 BSS_MAP_MSG_VGCS_VBS_AREA_CELL_INFO = 60,
173 BSS_MAP_MSG_UPLINK_RQST_CONFIRMATION = 73,
174 BSS_MAP_MSG_UPLINK_RELEASE_INDICATION = 74,
175 BSS_MAP_MSG_UPLINK_REJECT_CMD = 75,
176 BSS_MAP_MSG_UPLINK_RELEASE_CMD = 76,
177 BSS_MAP_MSG_UPLINK_SEIZED_CMD = 77,
178 BSS_MAP_MSG_VGCS_ADDL_INFO = 0x60,
179 BSS_MAP_MSG_VGCS_SMS = 0x61,
180 BSS_MAP_MSG_NOTIFICATION_DATA = 0x62,
181 BSS_MAP_MSG_UPLINK_APP_DATA = 0x63,
182
183 /* LOCAL SWITCHING */
184 BSS_MAP_MSG_LCLS_CONNECT_CTRL = 0x74,
185 BSS_MAP_MSG_LCLS_CONNECT_CTRL_ACK = 0x75,
186 BSS_MAP_MSG_LCLS_NOTIFICATION = 0x76,
187};
188
189#define BSS_MAP_MSG_ASSIGMENT_RQST BSS_MAP_MSG_ASSIGNMENT_RQST
190#define BSS_MAP_MSG_ASSIGMENT_COMPLETE BSS_MAP_MSG_ASSIGNMENT_COMPLETE
191#define BSS_MAP_MSG_ASSIGMENT_FAILURE BSS_MAP_MSG_ASSIGNMENT_FAILURE
192
193 enum GSM0808_IE_CODING {
194 GSM0808_IE_CIRCUIT_IDENTITY_CODE = 1,
195 GSM0808_IE_RESERVED_0 = 2,
196 GSM0808_IE_RESOURCE_AVAILABLE = 3,
197 GSM0808_IE_CAUSE = 4,
198 GSM0808_IE_CELL_IDENTIFIER = 5,
199 GSM0808_IE_PRIORITY = 6,
200 GSM0808_IE_LAYER_3_HEADER_INFORMATION = 7,
201 GSM0808_IE_IMSI = 8,
202 GSM0808_IE_TMSI = 9,
203 GSM0808_IE_ENCRYPTION_INFORMATION = 10,
204 GSM0808_IE_CHANNEL_TYPE = 11,
205 GSM0808_IE_PERIODICITY = 12,
206 GSM0808_IE_EXTENDED_RESOURCE_INDICATOR = 13,
207 GSM0808_IE_NUMBER_OF_MSS = 14,
208 GSM0808_IE_RESERVED_1 = 15,
209 GSM0808_IE_RESERVED_2 = 16,
210 GSM0808_IE_RESERVED_3 = 17,
211 GSM0808_IE_CLASSMARK_INFORMATION_T2 = 18,
212 GSM0808_IE_CLASSMARK_INFORMATION_T3 = 19,
213 GSM0808_IE_INTERFERENCE_BAND_TO_USE = 20,
214 GSM0808_IE_RR_CAUSE = 21,
215 GSM0808_IE_RESERVED_4 = 22,
216 GSM0808_IE_LAYER_3_INFORMATION = 23,
217 GSM0808_IE_DLCI = 24,
218 GSM0808_IE_DOWNLINK_DTX_FLAG = 25,
219 GSM0808_IE_CELL_IDENTIFIER_LIST = 26,
220 GSM0808_IE_RESPONSE_RQST = 27,
221 GSM0808_IE_RESOURCE_INDICATION_METHOD = 28,
222 GSM0808_IE_CLASSMARK_INFORMATION_TYPE_1 = 29,
223 GSM0808_IE_CIRCUIT_IDENTITY_CODE_LIST = 30,
224 GSM0808_IE_DIAGNOSTIC = 31,
225 GSM0808_IE_LAYER_3_MESSAGE_CONTENTS = 32,
226 GSM0808_IE_CHOSEN_CHANNEL = 33,
227 GSM0808_IE_TOTAL_RESOURCE_ACCESSIBLE = 34,
228 GSM0808_IE_CIPHER_RESPONSE_MODE = 35,
229 GSM0808_IE_CHANNEL_NEEDED = 36,
230 GSM0808_IE_TRACE_TYPE = 37,
231 GSM0808_IE_TRIGGERID = 38,
232 GSM0808_IE_TRACE_REFERENCE = 39,
233 GSM0808_IE_TRANSACTIONID = 40,
234 GSM0808_IE_MOBILE_IDENTITY = 41,
235 GSM0808_IE_OMCID = 42,
236 GSM0808_IE_FORWARD_INDICATOR = 43,
237 GSM0808_IE_CHOSEN_ENCR_ALG = 44,
238 GSM0808_IE_CIRCUIT_POOL = 45,
239 GSM0808_IE_CIRCUIT_POOL_LIST = 46,
240 GSM0808_IE_TIME_INDICATION = 47,
241 GSM0808_IE_RESOURCE_SITUATION = 48,
242 GSM0808_IE_CURRENT_CHANNEL_TYPE_1 = 49,
243 GSM0808_IE_QUEUEING_INDICATOR = 50,
244 GSM0808_IE_SPEECH_VERSION = 64,
245 GSM0808_IE_ASSIGNMENT_REQUIREMENT = 51,
246 GSM0808_IE_TALKER_FLAG = 53,
247 GSM0808_IE_CONNECTION_RELEASE_RQSTED = 54,
248 GSM0808_IE_GROUP_CALL_REFERENCE = 55,
249 GSM0808_IE_EMLPP_PRIORITY = 56,
250 GSM0808_IE_CONFIG_EVO_INDI = 57,
251 GSM0808_IE_OLD_BSS_TO_NEW_BSS_INFORMATION = 58,
252 GSM0808_IE_LSA_IDENTIFIER = 59,
253 GSM0808_IE_LSA_IDENTIFIER_LIST = 60,
254 GSM0808_IE_LSA_INFORMATION = 61,
255 GSM0808_IE_LCS_QOS = 62,
256 GSM0808_IE_LSA_ACCESS_CTRL_SUPPR = 63,
257 GSM0808_IE_LCS_PRIORITY = 67,
258 GSM0808_IE_LOCATION_TYPE = 68,
259 GSM0808_IE_LOCATION_ESTIMATE = 69,
260 GSM0808_IE_POSITIONING_DATA = 70,
261 GSM0808_IE_LCS_CAUSE = 71,
262 GSM0808_IE_LCS_CLIENT_TYPE = 72,
263 GSM0808_IE_APDU = 73,
264 GSM0808_IE_NETWORK_ELEMENT_IDENTITY = 74,
265 GSM0808_IE_GPS_ASSISTANCE_DATA = 75,
266 GSM0808_IE_DECIPHERING_KEYS = 76,
267 GSM0808_IE_RETURN_ERROR_RQST = 77,
268 GSM0808_IE_RETURN_ERROR_CAUSE = 78,
269 GSM0808_IE_SEGMENTATION = 79,
270 GSM0808_IE_SERVICE_HANDOVER = 80,
271 GSM0808_IE_SOURCE_RNC_TO_TARGET_RNC_TRANSPARENT_UMTS = 81,
272 GSM0808_IE_SOURCE_RNC_TO_TARGET_RNC_TRANSPARENT_CDMA2000 = 82,
273 GSM0808_IE_RESERVED_5 = 65,
274 GSM0808_IE_RESERVED_6 = 66,
275 GSM0808_IE_GERAN_CLASSMARK = 0x53,
276 GSM0808_IE_GERAN_BSC_CONTAINER = 0x54,
277 GSM0808_IE_NEW_BSS_TO_OLD_BSS_INFO = 0x61,
278 GSM0800_IE_INTER_SYSTEM_INFO = 0x63,
279 GSM0808_IE_SNA_ACCESS_INFO = 0x64,
280 GSM0808_IE_VSTK_RAND_INFO = 0x65,
281 GSM0808_IE_VSTK_INFO = 0x66,
282 GSM0808_IE_PAGING_INFO = 0x67,
283 GSM0808_IE_IMEI = 0x68,
284 GSM0808_IE_VELOCITY_ESTIMATE = 0x55,
285 GSM0808_IE_VGCS_FEATURE_FLAGS = 0x69,
286 GSM0808_IE_TALKER_PRIORITY = 0x6a,
287 GSM0808_IE_EMERGENCY_SET_INDICATION = 0x6b,
288 GSM0808_IE_TALKER_IDENTITY = 0x6c,
289 GSM0808_IE_CELL_ID_LIST_SEGMENT = 0x6d,
290 GSM0808_IE_SMS_TO_VGCS = 0x6e,
291 GSM0808_IE_VGCS_TALKER_MODE = 0x6f,
292 GSM0808_IE_VGCS_VBS_CELL_STATUS = 0x70,
293 GSM0808_IE_CELL_ID_LIST_SEG_EST_CELLS = 0x71,
294 GSM0808_IE_CELL_ID_LIST_SEG_CELLS_TBE = 0x72,
295 GSM0808_IE_CELL_ID_LIST_SEG_REL_CELLS = 0x73,
296 GSM0808_IE_CELL_ID_LIST_SEG_NE_CELLS = 0x74,
297 GSM0808_IE_GANSS_ASSISTANCE_DATA = 0x75,
298 GSM0808_IE_GANSS_POSITIONING_DATA = 0x76,
299 GSM0808_IE_GANSS_LOCATION_TYPE = 0x77,
300 GSM0808_IE_APP_DATA = 0x78,
301 GSM0808_IE_DATA_IDENTITY = 0x79,
302 GSM0808_IE_APP_DATA_INFO = 0x7a,
303 GSM0808_IE_MSISDN = 0x7b,
304 GSM0808_IE_AOIP_TRASP_ADDR = 0x7c,
305 GSM0808_IE_SPEECH_CODEC_LIST = 0x7d,
306 GSM0808_IE_SPEECH_CODEC = 0x7e,
307 GSM0808_IE_CALL_ID = 0x7f,
308 GSM0808_IE_CALL_ID_LIST = 0x80,
309 GSM0808_IE_A_IF_SEL_FOR_RESET = 0x81,
310 GSM0808_IE_KC_128 = 0x83,
311 GSM0808_IE_CSG_IDENTIFIER = 0x84,
312 GSM0808_IE_REDIR_ATTEMPT_FLAG = 0x85,
313 GSM0808_IE_REROUTE_REJ_CAUSE = 0x86,
314 GSM0808_IE_SEND_SEQ_NUM = 0x87,
315 GSM0808_IE_REROUTE_COMPL_OUTCOME = 0x88,
316 GSM0808_IE_GLOBAL_CALL_REF = 0x89,
317 GSM0808_IE_LCLS_CONFIG = 0x8a,
318 GSM0808_IE_LCLS_CONN_STATUS_CTRL = 0x8b,
319 GSM0808_IE_LCLS_CORR_NOT_NEEDED = 0x8c,
320 GSM0808_IE_LCLS_BSS_STATUS = 0x8d,
321 GSM0808_IE_LCLS_BREAK_REQ = 0x8e,
322 GSM0808_IE_CSFB_INDICATION = 0x8f,
323 GSM0808_IE_CS_TO_PS_SRVCC = 0x90,
324 GSM0808_IE_SRC_ENB_TO_TGT_ENB_TRANSP = 0x91,
325 GSM0808_IE_CS_TO_PS_SRVCC_IND = 0x92,
326 GSM0808_IE_CN_TO_MS_TRANSP_INFO = 0x93,
327 GSM0808_IE_SELECTED_PLMN_ID = 0x94,
328 GSM0808_IE_LAST_USED_EUTRAN_PLMN_ID = 0x95,
329 GSM0808_IE_OLD_LAI = 0x96,
330 GSM0808_IE_ATTACH_INDICATOR = 0x97,
331 GSM0808_IE_SELECTED_OPERATOR = 0x98,
332 GSM0808_IE_PS_REGISTERED_OPERATOR = 0x99,
333 GSM0808_IE_CS_REGISTERED_OPERATOR = 0x9a,
334
335 /* Osmocom and Themyscira extensions: */
336 GSM0808_IE_OSMO_OSMUX_SUPPORT = 0xf0,
337 GSM0808_IE_OSMO_OSMUX_CID = 0xf1,
338 GSM0808_IE_THEMWI_RTP_EXTENSIONS = 0xf2,
339};
340
341/* 3GPP TS 48.008 3.2.3 Signalling Field Element Coding.
342 See also extra fields in 3.2.2.58 and 3.2.2.80 */
343 enum GSM0808_SIGNALLING_FIELD_ELEMENT_CODING {
344 GSM0808_FE_IE_EXTRA_INFORMATION = 0x01, /*< 3.2.3.1 */
345 GSM0808_FE_IE_CURRENT_CHANNEL_TYPE_2 = 0x02, /*< 3.2.3.2 */
346 GSM0808_FE_IE_TARGET_CELL_RADIO_INFORMATION = 0x03, /*< 3.2.3.3 */
347 GSM0808_FE_IE_GPRS_SUSPEND_INFORMATION = 0x04, /*< 3.2.3.4 */
348 GSM0808_FE_IE_MULTIRATE_CONFIGURATION_INFORMATION = 0x05, /*< 3.2.3.5 */
349 GSM0808_FE_IE_DUAL_TRANSFER_MODE_INFORMATION = 0x06, /*< 3.2.3.6 */
350 GSM0808_FE_IE_INTER_RAT_HANDOVER_INFO = 0x07, /*< 3.2.3.7 */
351 GSM0808_FE_IE_CDMA2000_CAPABILITY_INFORMATION = 0x08, /*< 3.2.3.8 */
352 GSM0808_FE_IE_DOWNLINK_CELL_LOAD_INFORMATION = 0x09, /*< 3.2.3.9 */
353 GSM0808_FE_IE_UPLINK_CELL_LOAD_INFORMATION = 0x0a, /*< 3.2.3.10 */
354 GSM0808_FE_IE_CELL_LOAD_INFORMATION_GROUP = 0x0b, /*< 3.2.3.11 */
355 GSM0808_FE_IE_CELL_LOAD_INFORMATION = 0x0c, /*< 3.2.3.12 */
356 GSM0808_FE_IE_PS_INDICATION = 0x0d, /*< 3.2.3.13 */
357 GSM0808_FE_IE_DTM_HANDOVER_COMMAND_INDICATION = 0x0e, /*< 3.2.3.14 */
358 GSM0808_FE_IE_D_RNTI = 0xfe, /*< 3.2.3.15 */
359 GSM0808_FE_IE_IRAT_MEASUREMENT_CONFIGURATION = 0x0f, /*< 3.2.3.16 */
360 GSM0808_FE_IE_SOURCE_CELL_ID = 0x10, /*< 3.2.3.17 */
361 GSM0808_FE_IE_IRAT_MEASUREMENT_CONFIGURATION_EXTENDED_E_ARFCNS = 0x11, /*< 3.2.3.18 */
362 GSM0808_FE_IE_VGCS_TALKER_MODE = 0x6f, /*< 3.2.2.93 */
363 GSM0808_FE_IE_LAST_USED_EUTRAN_PLMN_ID = 0x95, /*< 3.2.2.127 */
364};
365
366/* 3GPP TS 48.008 3.2.2.5 Cause */
367 enum gsm0808_cause {
368 GSM0808_CAUSE_RADIO_INTERFACE_MESSAGE_FAILURE = 0,
369 GSM0808_CAUSE_RADIO_INTERFACE_FAILURE = 1,
370 GSM0808_CAUSE_UPLINK_QUALITY = 2,
371 GSM0808_CAUSE_UPLINK_STRENGTH = 3,
372 GSM0808_CAUSE_DOWNLINK_QUALITY = 4,
373 GSM0808_CAUSE_DOWNLINK_STRENGTH = 5,
374 GSM0808_CAUSE_DISTANCE = 6,
375 GSM0808_CAUSE_O_AND_M_INTERVENTION = 7,
376 GSM0808_CAUSE_RESPONSE_TO_MSC_INVOCATION = 8,
377 GSM0808_CAUSE_CALL_CONTROL = 9,
378 GSM0808_CAUSE_RADIO_INTERFACE_FAILURE_REVERSION = 10,
379 GSM0808_CAUSE_HANDOVER_SUCCESSFUL = 11,
380 GSM0808_CAUSE_BETTER_CELL = 12,
381 GSM0808_CAUSE_DIRECTED_RETRY = 13,
382 GSM0808_CAUSE_JOINED_GROUP_CALL_CHANNEL = 14,
383 GSM0808_CAUSE_TRAFFIC = 15,
384 GSM0808_CAUSE_REDUCE_LOAD_IN_SERVING_CELL = 0x10,
385 GSM0808_CAUSE_TRAFFIC_LOAD_IN_TGT_HIGHER_THAN_IN_SRC_CELL = 0x11,
386 GSM0808_CAUSE_RELOCATION_TRIGGERED = 0x12,
387 GSM0808_CAUSE_REQUESTED_OPT_NOT_AUTHORISED = 0x14,
388 GSM0808_CAUSE_ALT_CHAN_CONFIG_REQUESTED = 0x15,
389 GSM0808_CAUSE_RESP_TO_INT_HO_ENQ_MSG = 0x16,
390 GSM0808_CAUSE_INT_HO_ENQUIRY_REJECT = 0x17,
391 GSM0808_CAUSE_REDUNDANCY_LEVEL_NOT_ADEQUATE = 0x18,
392 GSM0808_CAUSE_EQUIPMENT_FAILURE = 32,
393 GSM0808_CAUSE_NO_RADIO_RESOURCE_AVAILABLE = 33,
394 GSM0808_CAUSE_RQSTED_TERRESTRIAL_RESOURCE_UNAVAILABLE = 34,
395 GSM0808_CAUSE_CCCH_OVERLOAD = 35,
396 GSM0808_CAUSE_PROCESSOR_OVERLOAD = 36,
397 GSM0808_CAUSE_BSS_NOT_EQUIPPED = 37,
398 GSM0808_CAUSE_MS_NOT_EQUIPPED = 38,
399 GSM0808_CAUSE_INVALID_CELL = 39,
400 GSM0808_CAUSE_TRAFFIC_LOAD = 40,
401 GSM0808_CAUSE_PREEMPTION = 41,
402 GSM0808_CAUSE_DTM_HO_SGSN_FAILURE = 0x2a,
403 GSM0808_CAUSE_DTM_HO_PS_ALLOC_FAILURE = 0x2b,
404 GSM0808_CAUSE_RQSTED_TRANSCODING_RATE_ADAPTION_UNAVAILABLE = 48,
405 GSM0808_CAUSE_CIRCUIT_POOL_MISMATCH = 49,
406 GSM0808_CAUSE_SWITCH_CIRCUIT_POOL = 50,
407 GSM0808_CAUSE_RQSTED_SPEECH_VERSION_UNAVAILABLE = 51,
408 GSM0808_CAUSE_LSA_NOT_ALLOWED = 52,
409 GSM0808_CAUSE_REQ_CODEC_TYPE_OR_CONFIG_UNAVAIL = 0x35,
410 GSM0808_CAUSE_REQ_A_IF_TYPE_UNAVAIL = 0x36,
411 GSM0808_CAUSE_INVALID_CSG_CELL = 0x37,
412 GSM0808_CAUSE_REQ_REDUND_LEVEL_NOT_AVAIL = 0x3f,
413 GSM0808_CAUSE_CIPHERING_ALGORITHM_NOT_SUPPORTED = 64,
414 GSM0808_CAUSE_GERAN_IU_MODE_FAILURE = 0x41,
415 GSM0808_CAUSE_INC_RELOC_NOT_SUPP_DT_PUESBINE_FEATURE = 0x42,
416 GSM0808_CAUSE_ACCESS_RESTRICTED_DUE_TO_SHARED_NETWORKS = 0x43,
417 GSM0808_CAUSE_REQ_CODEC_TYPE_OR_CONFIG_NOT_SUPP = 0x44,
418 GSM0808_CAUSE_REQ_A_IF_TYPE_NOT_SUPP = 0x45,
419 GSM0808_CAUSE_REQ_REDUND_LVL_NOT_SUPP = 0x46,
420 GSM0808_CAUSE_TERRESTRIAL_CIRCUIT_ALREADY_ALLOCATED = 80,
421 GSM0808_CAUSE_INVALID_MESSAGE_CONTENTS = 81,
422 GSM0808_CAUSE_INFORMATION_ELEMENT_OR_FIELD_MISSING = 82,
423 GSM0808_CAUSE_INCORRECT_VALUE = 83,
424 GSM0808_CAUSE_UNKNOWN_MESSAGE_TYPE = 84,
425 GSM0808_CAUSE_UNKNOWN_INFORMATION_ELEMENT = 85,
426 GSM0808_CAUSE_DTM_HO_INVALID_PS_IND = 0x56,
427 GSM0808_CAUSE_CALL_ID_ALREADY_ALLOC = 0x57,
428 GSM0808_CAUSE_PROTOCOL_ERROR_BETWEEN_BSS_AND_MSC = 96,
429 GSM0808_CAUSE_VGCS_VBS_CALL_NON_EXISTENT = 0x61,
430 GSM0808_CAUSE_DTM_HO_TIMER_EXPIRY = 0x62,
431};
432
433/* 3GPP TS 08.08 §3.2.2.5 Cause Class */
434 enum gsm0808_cause_class {
435 GSM0808_CAUSE_CLASS_NORM0 = 0,
436 GSM0808_CAUSE_CLASS_NORM1 = 1,
437 GSM0808_CAUSE_CLASS_RES_UNAVAIL = 2,
438 GSM0808_CAUSE_CLASS_SRV_OPT_NA = 3,
439 GSM0808_CAUSE_CLASS_SRV_OPT_NIMPL = 4,
440 GSM0808_CAUSE_CLASS_INVAL = 5,
441 GSM0808_CAUSE_CLASS_PERR = 6,
442 GSM0808_CAUSE_CLASS_INTW = 7,
443};
444
445/* GSM 08.08 3.2.2.11 Channel Type */
446 enum gsm0808_chan_indicator {
447 GSM0808_CHAN_SPEECH = 1,
448 GSM0808_CHAN_DATA = 2,
449 GSM0808_CHAN_SIGN = 3,
450 GSM0808_CHAN_SPEECH_CTM_TEXT_TELEPHONY = 4,
451};
452
453/* GSM 08.08 3.2.2.11 Channel Type */
454#define GSM0808_DATA_FULL_RPREF GSM0808_DATA_FULL_PREF
455 enum gsm0808_chan_rate_type_data {
456 GSM0808_DATA_FULL_BM = 0x8,
457 GSM0808_DATA_HALF_LM = 0x9,
458 GSM0808_DATA_FULL_PREF = 0xa,
459 GSM0808_DATA_HALF_PREF = 0xb,
460 GSM0808_DATA_FULL_PREF_NO_CHANGE = 0x1a,
461 GSM0808_DATA_HALF_PREF_NO_CHANGE = 0x1b,
462 GSM0808_DATA_MULTI_MASK = 0x20,
463 GSM0808_DATA_MULTI_MASK_NO_CHANGE = 0x30,
464};
465
466/* GSM 08.08 3.2.2.11 Channel Type */
467 enum gsm0808_chan_rate_type_speech {
468 GSM0808_SPEECH_FULL_BM = 0x8,
469 GSM0808_SPEECH_HALF_LM = 0x9,
470 GSM0808_SPEECH_FULL_PREF= 0xa,
471 GSM0808_SPEECH_HALF_PREF= 0xb,
472 GSM0808_SPEECH_FULL_PREF_NO_CHANGE = 0x1a,
473 GSM0808_SPEECH_HALF_PREF_NO_CHANGE = 0x1b,
474 GSM0808_SPEECH_PERM = 0xf,
475 GSM0808_SPEECH_PERM_NO_CHANGE = 0x1f,
476};
477
478/* GSM 08.08 3.2.2.11 Channel Type */
479 enum gsm0808_chan_rate_type_sign {
480 GSM0808_SIGN_ANY = 0x00,
481 GSM0808_SIGN_SDCCH = 0x01,
482 GSM0808_SIGN_SDCCH_FULL_BM = 0x02,
483 GSM0808_SIGN_SDCCH_HALF_LM = 0x03,
484 GSM0808_SIGN_FULL_BM = 0x08,
485 GSM0808_SIGN_HALF_LM = 0x09,
486 GSM0808_SIGN_FULL_PREF = 0x0a,
487 GSM0808_SIGN_HALF_PREF = 0x0b,
488 GSM0808_SIGN_FULL_PREF_NO_CHANGE = 0x1a,
489 GSM0808_SIGN_HALF_PREF_NO_CHANGE = 0x1b,
490};
491
494 enum gsm0808_permitted_speech {
495 GSM0808_PERM_FR1 = 0x01,
496 GSM0808_PERM_FR2 = 0x11,
497 GSM0808_PERM_FR3 = 0x21,
498 GSM0808_PERM_FR4 = 0x41,
499 GSM0808_PERM_FR5 = 0x42,
500 GSM0808_PERM_HR1 = GSM0808_PERM_FR1 | 0x4,
501 GSM0808_PERM_HR2 = GSM0808_PERM_FR2 | 0x4,
502 GSM0808_PERM_HR3 = GSM0808_PERM_FR3 | 0x4,
503 GSM0808_PERM_HR4 = 0x46,
504 GSM0808_PERM_HR6 = 0x45,
505};
506
507/* 3GPP TS 48.008 3.2.2.11 Channel Type
508 * Transparent: Data Rate */
509 enum gsm0808_data_rate_transp {
510 GSM0808_DATA_RATE_TRANSP_32k0 = 0x3a,
511 GSM0808_DATA_RATE_TRANSP_28k8 = 0x39,
512 GSM0808_DATA_RATE_TRANSP_14k4 = 0x18,
513 GSM0808_DATA_RATE_TRANSP_9k6 = 0x10,
514 GSM0808_DATA_RATE_TRANSP_4k8 = 0x11,
515 GSM0808_DATA_RATE_TRANSP_2k4 = 0x12,
516 GSM0808_DATA_RATE_TRANSP_1k2 = 0x13,
517 GSM0808_DATA_RATE_TRANSP_600 = 0x14,
518 GSM0808_DATA_RATE_TRANSP_1200_75 = 0x15,
519};
520
521/* 3GPP TS 48.008 3.2.2.11 Channel Type
522 * Non-Transparent: Radio Interface Data Rate (preferred) */
523 enum gsm0808_data_rate_non_transp {
524 GSM0808_DATA_RATE_NON_TRANSP_12000_6000 = 0x00,
525 GSM0808_DATA_RATE_NON_TRANSP_43k5 = 0x34,
526 GSM0808_DATA_RATE_NON_TRANSP_29k0 = 0x31,
527 GSM0808_DATA_RATE_NON_TRANSP_14k5 = 0x14,
528 GSM0808_DATA_RATE_NON_TRANSP_12k0 = 0x10,
529 GSM0808_DATA_RATE_NON_TRANSP_6k0 = 0x11,
530};
531
532/* 3GPP TS 48.008 3.2.2.11 Channel Type
533 * Non-Transparent: Allowed Radio Interface Data Rate (all possible allowed) */
534 enum gsm0808_data_rate_allowed_r_if {
535 GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_43k5 = 0x40,
536 GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_32k0 = 0x20,
537 GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_29k0 = 0x10,
538 GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_14k5 = 0x08,
539 GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_12k0 = 0x02,
540 GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_6k0 = 0x01,
541};
542
543 extern const struct value_string gsm0808_permitted_speech_names[];
544 static inline const char *gsm0808_permitted_speech_name(enum gsm0808_permitted_speech val)
545{ return get_value_string(gsm0808_permitted_speech_names, val); }
546
548 enum gsm0808_speech_codec_type {
549 GSM0808_SCT_FR1 = 0x0,
550 GSM0808_SCT_FR2 = 0x2,
551 GSM0808_SCT_FR3 = 0x3,
552 GSM0808_SCT_FR4 = 0xc,
553 GSM0808_SCT_FR5 = 0x9,
554 GSM0808_SCT_HR1 = 0x1,
555 GSM0808_SCT_HR3 = 0x4,
556 GSM0808_SCT_HR4 = 0xd,
557 GSM0808_SCT_HR6 = 0xb,
558 GSM0808_SCT_CSD = 0xfd,
559};
560
561/* Codec Extension (the real Codec Type follows in the next octet).
562 * This value is intentionally not included in gsm0808_speech_codec_type,
563 * because {enc,dec}_speech_codec() functions take care of the extended
564 * encoding internally. It shall not be used in struct gsm0808_speech_codec. */
565#define GSM0808_SCT_EXT 0x0f
566
567 extern const struct value_string gsm0808_speech_codec_type_names[];
568 static inline const char *gsm0808_speech_codec_type_name(enum gsm0808_speech_codec_type val)
569{ return get_value_string(gsm0808_speech_codec_type_names, val); }
570
571/* GSM 08.08 3.2.2.44 Chosen Encryption Algorithm */
572 enum gsm0808_chosen_enc_alg {
573 GSM0808_ALG_ID_A5_0 = 0x01,
574 GSM0808_ALG_ID_A5_1 = 0x02,
575 GSM0808_ALG_ID_A5_2 = 0x03,
576 GSM0808_ALG_ID_A5_3 = 0x04,
577 GSM0808_ALG_ID_A5_4 = 0x05,
578 GSM0808_ALG_ID_A5_5 = 0x06,
579 GSM0808_ALG_ID_A5_6 = 0x07,
580 GSM0808_ALG_ID_A5_7 = 0x08,
581};
582 extern const struct value_string gsm0808_chosen_enc_alg_names[];
583
584/* GSM 08.08 3.2.2.85 Paging Information */
585 enum gsm0808_paging_info {
586 GSM0808_PAGINF_FOR_MT_CALL = 0x00,
587 GSM0808_PAGINF_FOR_SMS = 0x01,
588 GSM0808_PAGINF_FOR_USSD = 0x02,
589};
590
593 struct gsm0808_speech_codec {
595 bool fi;
597 bool pi;
599 bool pt;
601 bool tf;
603 uint8_t type;
605 uint16_t cfg;
606};
607
657 enum gsm0808_speech_codec_defaults {
658 GSM0808_SC_CFG_DEFAULT_FR_AMR = 0x57ff,
659 GSM0808_SC_CFG_DEFAULT_HR_AMR = 0x073f,
660 GSM0808_SC_CFG_DEFAULT_OHR_AMR = 0x57ff,
661 GSM0808_SC_CFG_DEFAULT_FR_AMR_WB = 0x01,
662 GSM0808_SC_CFG_DEFAULT_OFR_AMR_WB = 0x15,
663 GSM0808_SC_CFG_DEFAULT_OHR_AMR_WB = 0x01,
664};
665
672 enum gsm0808_speech_codec_rate_defaults {
673 GSM0808_SC_CFG_DEFAULT_AMR_4_75 = 0xff03,
674 GSM0808_SC_CFG_DEFAULT_AMR_5_15 = 0x0000,
675 GSM0808_SC_CFG_DEFAULT_AMR_5_90 = 0xff06,
676 GSM0808_SC_CFG_DEFAULT_AMR_6_70 = 0x3e08,
677 GSM0808_SC_CFG_DEFAULT_AMR_7_40 = 0x0c12,
678 GSM0808_SC_CFG_DEFAULT_AMR_7_95 = 0xc020,
679 GSM0808_SC_CFG_DEFAULT_AMR_10_2 = 0x3040,
680 GSM0808_SC_CFG_DEFAULT_AMR_12_2 = 0xc082
681};
682
689 enum gsm0808_speech_codec_rate {
690 GSM0808_SC_CFG_AMR_4_75 = 0x0001,
691 GSM0808_SC_CFG_AMR_4_75_5_90_7_40_12_20 = 0x0002,
692 GSM0808_SC_CFG_AMR_5_90 = 0x0004,
693 GSM0808_SC_CFG_AMR_6_70 = 0x0008,
694 GSM0808_SC_CFG_AMR_7_40 = 0x0010,
695 GSM0808_SC_CFG_AMR_7_95 = 0x0020,
696 GSM0808_SC_CFG_AMR_10_2 = 0x0040,
697 GSM0808_SC_CFG_AMR_12_2 = 0x0080,
698};
699
700/* Bit index of a mode as returned by gsm0808_amr_modes_from_cfg[].
701 * Example:
702 * if (gsm0808_amr_modes_from_cfg[full_rate ? 1 : 0][9] & GSM0808_AMR_MODE_4_75)
703 * printf("S9 supports 4k75");
704 */
705 enum gsm0808_amr_mode {
706 GSM0808_AMR_MODE_4_75 = 0,
707 GSM0808_AMR_MODE_5_15,
708 GSM0808_AMR_MODE_5_90,
709 GSM0808_AMR_MODE_6_70,
710 GSM0808_AMR_MODE_7_40,
711 GSM0808_AMR_MODE_7_95,
712 GSM0808_AMR_MODE_10_2,
713 GSM0808_AMR_MODE_12_2,
714};
715 extern const struct value_string gsm0808_amr_mode_names[];
716 static inline const char *gsm0808_amr_mode_name(enum gsm0808_amr_mode val)
717{
718 return get_value_string(gsm0808_amr_mode_names, val);
719}
720
721 extern const uint8_t gsm0808_amr_modes_from_cfg[2][16];
722
723/* 3GPP TS 48.008 3.2.2.103 Speech Codec List */
724#define SPEECH_CODEC_MAXLEN 255
725 struct gsm0808_speech_codec_list {
726 struct gsm0808_speech_codec codec[SPEECH_CODEC_MAXLEN];
727 uint8_t len;
728};
729
730/* 3GPP TS 48.008 3.2.2.11 Channel Type
731 * Asymmetry Preference (used for data, non-transparent service) */
732 enum gsm0808_channel_type_asym_pref {
733 GSM0808_CT_ASYM_PREF_NOT_APPLICABLE = 0,
734 GSM0808_CT_ASYM_PREF_UL = 1,
735 GSM0808_CT_ASYM_PREF_DL = 2,
736 GSM0808_CT_ASYM_PREF_SPARE = 3,
737};
738
739/* 3GPP TS 48.008 3.2.2.11 Channel Type */
740#define CH_TYPE_PERM_SPCH_MAXLEN 9
741 struct gsm0808_channel_type {
742 uint8_t ch_indctr;
743 uint8_t ch_rate_type;
744
745 /* Speech only */
746 uint8_t perm_spch[CH_TYPE_PERM_SPCH_MAXLEN];
747 unsigned int perm_spch_len;
748
749 /* Data only */
750 bool data_transparent;
751 uint8_t data_rate;
752 bool data_rate_allowed_is_set;
753 uint8_t data_rate_allowed;
754 bool data_asym_pref_is_set;
755 enum gsm0808_channel_type_asym_pref data_asym_pref;
756};
757
758/* 3GPP TS 48.008 3.2.2.10 Encryption Information */
759#define ENCRY_INFO_KEY_MAXLEN 252
760#define ENCRY_INFO_PERM_ALGO_MAXLEN 8
761 struct gsm0808_encrypt_info {
762 uint8_t perm_algo[ENCRY_INFO_PERM_ALGO_MAXLEN];
763 unsigned int perm_algo_len;
764 uint8_t key[ENCRY_INFO_KEY_MAXLEN];
765 unsigned int key_len;
766};
767
768#define CELL_ID_LIST_LAC_MAXLEN 127
775 struct gsm0808_cell_id_list {
776 uint8_t id_discr;
777 uint16_t id_list_lac[CELL_ID_LIST_LAC_MAXLEN];
778 unsigned int id_list_len;
779};
780
781/* TS 48.008 3.2.2.116 */
782 enum gsm0808_lcls_config {
783 GSM0808_LCLS_CFG_BOTH_WAY = 0x00,
784 GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL = 0x01,
785 GSM0808_LCLS_CFG_BOTH_WAY_AND_SEND_DL = 0x02,
786 GSM0808_LCLS_CFG_BOTH_WAY_AND_SEND_DL_BLOCK_LOCAL_DL = 0x03,
787 GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL_SEND_DL = 0x04,
788 GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL_SEND_DL_BLOCK_LOCAL_DL = 0x05,
789 GSM0808_LCLS_CFG_NA = 0xFF
790};
791
792/* TS 48.008 3.2.2.117 */
793 enum gsm0808_lcls_control {
794 GSM0808_LCLS_CSC_CONNECT = 0x00,
795 GSM0808_LCLS_CSC_DO_NOT_CONNECT = 0x01,
796 GSM0808_LCLS_CSC_RELEASE_LCLS = 0x02,
797 GSM0808_LCLS_CSC_BICAST_UL_AT_HANDOVER = 0x03,
798 GSM0808_LCLS_CSC_BICAST_UL_AND_RECV_DL_AT_HANDOVER = 0x04,
799 GSM0808_LCLS_CSC_NA = 0xFF
800};
801
802/* TS 48.008 3.2.2.119 */
803 enum gsm0808_lcls_status {
804 GSM0808_LCLS_STS_NOT_YET_LS = 0x00,
805 GSM0808_LCLS_STS_NOT_POSSIBLE_LS = 0x01,
806 GSM0808_LCLS_STS_NO_LONGER_LS = 0x02,
807 GSM0808_LCLS_STS_REQ_LCLS_NOT_SUPP = 0x03,
808 GSM0808_LCLS_STS_LOCALLY_SWITCHED = 0x04,
809 GSM0808_LCLS_STS_NA = 0xFF
810};
811
812/* 3GPP TS 48.008 3.2.2.32 Diagnostics */
813 struct gsm0808_diagnostics {
814 uint8_t error_pointer_octet;
815#if OSMO_IS_LITTLE_ENDIAN
816 uint8_t error_pointer_bit_spare:4,
817 error_pointer_bit:4;
818#elif OSMO_IS_BIG_ENDIAN
819/* auto-generated from the little endian part above (libosmocore/contrib/struct_endianness.py) */
820 uint8_t error_pointer_bit:4, error_pointer_bit_spare:4;
821#endif
822 uint8_t msg[0];
823} __attribute__((packed));
endian.h
gsm0808_speech_codec_type_names
const struct value_string gsm0808_speech_codec_type_names[]
Definition: gsm0808.c:2478
gsm0808_permitted_speech_names
const struct value_string gsm0808_permitted_speech_names[]
Definition: gsm0808.c:2493
gsm0808_chosen_enc_alg_names
const struct value_string gsm0808_chosen_enc_alg_names[]
Definition: gsm0808.c:2507
gsm0808_amr_mode_names
const struct value_string gsm0808_amr_mode_names[]
Definition: gsm0808.c:2780
gsm0406_dlci_sapi_names
const struct value_string gsm0406_dlci_sapi_names[]
Definition: gsm0808.c:2351
gsm0808_amr_modes_from_cfg
const uint8_t gsm0808_amr_modes_from_cfg[2][16]
Definition: gsm0808.c:2725
get_value_string
const char * get_value_string(const struct value_string *vs, uint32_t val)
gsm0808_speech_codec_type_name
static const char * gsm0808_speech_codec_type_name(enum gsm0808_speech_codec_type val)
Definition: gsm_08_08.h:568
gsm0808_data_rate_allowed_r_if
gsm0808_data_rate_allowed_r_if
Definition: gsm_08_08.h:534
GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_12k0
@ GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_12k0
Definition: gsm_08_08.h:539
GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_32k0
@ GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_32k0
Definition: gsm_08_08.h:536
GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_14k5
@ GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_14k5
Definition: gsm_08_08.h:538
GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_29k0
@ GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_29k0
Definition: gsm_08_08.h:537
GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_43k5
@ GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_43k5
Definition: gsm_08_08.h:535
GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_6k0
@ GSM0808_DATA_RATE_NON_TRANSP_ALLOWED_6k0
Definition: gsm_08_08.h:540
gsm0808_chan_indicator
gsm0808_chan_indicator
Definition: gsm_08_08.h:446
GSM0808_CHAN_SPEECH
@ GSM0808_CHAN_SPEECH
Definition: gsm_08_08.h:447
GSM0808_CHAN_DATA
@ GSM0808_CHAN_DATA
Definition: gsm_08_08.h:448
GSM0808_CHAN_SIGN
@ GSM0808_CHAN_SIGN
Definition: gsm_08_08.h:449
GSM0808_CHAN_SPEECH_CTM_TEXT_TELEPHONY
@ GSM0808_CHAN_SPEECH_CTM_TEXT_TELEPHONY
Definition: gsm_08_08.h:450
gsm0808_channel_type_asym_pref
gsm0808_channel_type_asym_pref
Definition: gsm_08_08.h:732
GSM0808_CT_ASYM_PREF_NOT_APPLICABLE
@ GSM0808_CT_ASYM_PREF_NOT_APPLICABLE
Definition: gsm_08_08.h:733
GSM0808_CT_ASYM_PREF_SPARE
@ GSM0808_CT_ASYM_PREF_SPARE
Definition: gsm_08_08.h:736
GSM0808_CT_ASYM_PREF_UL
@ GSM0808_CT_ASYM_PREF_UL
Definition: gsm_08_08.h:734
GSM0808_CT_ASYM_PREF_DL
@ GSM0808_CT_ASYM_PREF_DL
Definition: gsm_08_08.h:735
gsm0808_cause
gsm0808_cause
Definition: gsm_08_08.h:367
GSM0808_CAUSE_RELOCATION_TRIGGERED
@ GSM0808_CAUSE_RELOCATION_TRIGGERED
Definition: gsm_08_08.h:386
GSM0808_CAUSE_REQ_A_IF_TYPE_UNAVAIL
@ GSM0808_CAUSE_REQ_A_IF_TYPE_UNAVAIL
Definition: gsm_08_08.h:410
GSM0808_CAUSE_DTM_HO_INVALID_PS_IND
@ GSM0808_CAUSE_DTM_HO_INVALID_PS_IND
Definition: gsm_08_08.h:426
GSM0808_CAUSE_NO_RADIO_RESOURCE_AVAILABLE
@ GSM0808_CAUSE_NO_RADIO_RESOURCE_AVAILABLE
Definition: gsm_08_08.h:393
GSM0808_CAUSE_PROCESSOR_OVERLOAD
@ GSM0808_CAUSE_PROCESSOR_OVERLOAD
Definition: gsm_08_08.h:396
GSM0808_CAUSE_RESPONSE_TO_MSC_INVOCATION
@ GSM0808_CAUSE_RESPONSE_TO_MSC_INVOCATION
Definition: gsm_08_08.h:376
GSM0808_CAUSE_TERRESTRIAL_CIRCUIT_ALREADY_ALLOCATED
@ GSM0808_CAUSE_TERRESTRIAL_CIRCUIT_ALREADY_ALLOCATED
Definition: gsm_08_08.h:420
GSM0808_CAUSE_UNKNOWN_INFORMATION_ELEMENT
@ GSM0808_CAUSE_UNKNOWN_INFORMATION_ELEMENT
Definition: gsm_08_08.h:425
GSM0808_CAUSE_DIRECTED_RETRY
@ GSM0808_CAUSE_DIRECTED_RETRY
Definition: gsm_08_08.h:381
GSM0808_CAUSE_REDUNDANCY_LEVEL_NOT_ADEQUATE
@ GSM0808_CAUSE_REDUNDANCY_LEVEL_NOT_ADEQUATE
Definition: gsm_08_08.h:391
GSM0808_CAUSE_RADIO_INTERFACE_MESSAGE_FAILURE
@ GSM0808_CAUSE_RADIO_INTERFACE_MESSAGE_FAILURE
Definition: gsm_08_08.h:368
GSM0808_CAUSE_RQSTED_SPEECH_VERSION_UNAVAILABLE
@ GSM0808_CAUSE_RQSTED_SPEECH_VERSION_UNAVAILABLE
Definition: gsm_08_08.h:407
GSM0808_CAUSE_INVALID_CSG_CELL
@ GSM0808_CAUSE_INVALID_CSG_CELL
Definition: gsm_08_08.h:411
GSM0808_CAUSE_REQ_REDUND_LVL_NOT_SUPP
@ GSM0808_CAUSE_REQ_REDUND_LVL_NOT_SUPP
Definition: gsm_08_08.h:419
GSM0808_CAUSE_DOWNLINK_QUALITY
@ GSM0808_CAUSE_DOWNLINK_QUALITY
Definition: gsm_08_08.h:372
GSM0808_CAUSE_TRAFFIC_LOAD_IN_TGT_HIGHER_THAN_IN_SRC_CELL
@ GSM0808_CAUSE_TRAFFIC_LOAD_IN_TGT_HIGHER_THAN_IN_SRC_CELL
Definition: gsm_08_08.h:385
GSM0808_CAUSE_RADIO_INTERFACE_FAILURE
@ GSM0808_CAUSE_RADIO_INTERFACE_FAILURE
Definition: gsm_08_08.h:369
GSM0808_CAUSE_DOWNLINK_STRENGTH
@ GSM0808_CAUSE_DOWNLINK_STRENGTH
Definition: gsm_08_08.h:373
GSM0808_CAUSE_PROTOCOL_ERROR_BETWEEN_BSS_AND_MSC
@ GSM0808_CAUSE_PROTOCOL_ERROR_BETWEEN_BSS_AND_MSC
Definition: gsm_08_08.h:428
GSM0808_CAUSE_INC_RELOC_NOT_SUPP_DT_PUESBINE_FEATURE
@ GSM0808_CAUSE_INC_RELOC_NOT_SUPP_DT_PUESBINE_FEATURE
Definition: gsm_08_08.h:415
GSM0808_CAUSE_BSS_NOT_EQUIPPED
@ GSM0808_CAUSE_BSS_NOT_EQUIPPED
Definition: gsm_08_08.h:397
GSM0808_CAUSE_RADIO_INTERFACE_FAILURE_REVERSION
@ GSM0808_CAUSE_RADIO_INTERFACE_FAILURE_REVERSION
Definition: gsm_08_08.h:378
GSM0808_CAUSE_ACCESS_RESTRICTED_DUE_TO_SHARED_NETWORKS
@ GSM0808_CAUSE_ACCESS_RESTRICTED_DUE_TO_SHARED_NETWORKS
Definition: gsm_08_08.h:416
GSM0808_CAUSE_DISTANCE
@ GSM0808_CAUSE_DISTANCE
Definition: gsm_08_08.h:374
GSM0808_CAUSE_O_AND_M_INTERVENTION
@ GSM0808_CAUSE_O_AND_M_INTERVENTION
Definition: gsm_08_08.h:375
GSM0808_CAUSE_EQUIPMENT_FAILURE
@ GSM0808_CAUSE_EQUIPMENT_FAILURE
Definition: gsm_08_08.h:392
GSM0808_CAUSE_VGCS_VBS_CALL_NON_EXISTENT
@ GSM0808_CAUSE_VGCS_VBS_CALL_NON_EXISTENT
Definition: gsm_08_08.h:429
GSM0808_CAUSE_BETTER_CELL
@ GSM0808_CAUSE_BETTER_CELL
Definition: gsm_08_08.h:380
GSM0808_CAUSE_GERAN_IU_MODE_FAILURE
@ GSM0808_CAUSE_GERAN_IU_MODE_FAILURE
Definition: gsm_08_08.h:414
GSM0808_CAUSE_INT_HO_ENQUIRY_REJECT
@ GSM0808_CAUSE_INT_HO_ENQUIRY_REJECT
Definition: gsm_08_08.h:390
GSM0808_CAUSE_SWITCH_CIRCUIT_POOL
@ GSM0808_CAUSE_SWITCH_CIRCUIT_POOL
Definition: gsm_08_08.h:406
GSM0808_CAUSE_TRAFFIC
@ GSM0808_CAUSE_TRAFFIC
Definition: gsm_08_08.h:383
GSM0808_CAUSE_RQSTED_TERRESTRIAL_RESOURCE_UNAVAILABLE
@ GSM0808_CAUSE_RQSTED_TERRESTRIAL_RESOURCE_UNAVAILABLE
Definition: gsm_08_08.h:394
GSM0808_CAUSE_RESP_TO_INT_HO_ENQ_MSG
@ GSM0808_CAUSE_RESP_TO_INT_HO_ENQ_MSG
Definition: gsm_08_08.h:389
GSM0808_CAUSE_RQSTED_TRANSCODING_RATE_ADAPTION_UNAVAILABLE
@ GSM0808_CAUSE_RQSTED_TRANSCODING_RATE_ADAPTION_UNAVAILABLE
Definition: gsm_08_08.h:404
GSM0808_CAUSE_CIRCUIT_POOL_MISMATCH
@ GSM0808_CAUSE_CIRCUIT_POOL_MISMATCH
Definition: gsm_08_08.h:405
GSM0808_CAUSE_CALL_ID_ALREADY_ALLOC
@ GSM0808_CAUSE_CALL_ID_ALREADY_ALLOC
Definition: gsm_08_08.h:427
GSM0808_CAUSE_REDUCE_LOAD_IN_SERVING_CELL
@ GSM0808_CAUSE_REDUCE_LOAD_IN_SERVING_CELL
Definition: gsm_08_08.h:384
GSM0808_CAUSE_INFORMATION_ELEMENT_OR_FIELD_MISSING
@ GSM0808_CAUSE_INFORMATION_ELEMENT_OR_FIELD_MISSING
Definition: gsm_08_08.h:422
GSM0808_CAUSE_CCCH_OVERLOAD
@ GSM0808_CAUSE_CCCH_OVERLOAD
Definition: gsm_08_08.h:395
GSM0808_CAUSE_DTM_HO_TIMER_EXPIRY
@ GSM0808_CAUSE_DTM_HO_TIMER_EXPIRY
Definition: gsm_08_08.h:430
GSM0808_CAUSE_REQ_REDUND_LEVEL_NOT_AVAIL
@ GSM0808_CAUSE_REQ_REDUND_LEVEL_NOT_AVAIL
Definition: gsm_08_08.h:412
GSM0808_CAUSE_INVALID_MESSAGE_CONTENTS
@ GSM0808_CAUSE_INVALID_MESSAGE_CONTENTS
Definition: gsm_08_08.h:421
GSM0808_CAUSE_INVALID_CELL
@ GSM0808_CAUSE_INVALID_CELL
Definition: gsm_08_08.h:399
GSM0808_CAUSE_DTM_HO_SGSN_FAILURE
@ GSM0808_CAUSE_DTM_HO_SGSN_FAILURE
Definition: gsm_08_08.h:402
GSM0808_CAUSE_HANDOVER_SUCCESSFUL
@ GSM0808_CAUSE_HANDOVER_SUCCESSFUL
Definition: gsm_08_08.h:379
GSM0808_CAUSE_TRAFFIC_LOAD
@ GSM0808_CAUSE_TRAFFIC_LOAD
Definition: gsm_08_08.h:400
GSM0808_CAUSE_CALL_CONTROL
@ GSM0808_CAUSE_CALL_CONTROL
Definition: gsm_08_08.h:377
GSM0808_CAUSE_DTM_HO_PS_ALLOC_FAILURE
@ GSM0808_CAUSE_DTM_HO_PS_ALLOC_FAILURE
Definition: gsm_08_08.h:403
GSM0808_CAUSE_MS_NOT_EQUIPPED
@ GSM0808_CAUSE_MS_NOT_EQUIPPED
Definition: gsm_08_08.h:398
GSM0808_CAUSE_JOINED_GROUP_CALL_CHANNEL
@ GSM0808_CAUSE_JOINED_GROUP_CALL_CHANNEL
Definition: gsm_08_08.h:382
GSM0808_CAUSE_UPLINK_STRENGTH
@ GSM0808_CAUSE_UPLINK_STRENGTH
Definition: gsm_08_08.h:371
GSM0808_CAUSE_LSA_NOT_ALLOWED
@ GSM0808_CAUSE_LSA_NOT_ALLOWED
Definition: gsm_08_08.h:408
GSM0808_CAUSE_UNKNOWN_MESSAGE_TYPE
@ GSM0808_CAUSE_UNKNOWN_MESSAGE_TYPE
Definition: gsm_08_08.h:424
GSM0808_CAUSE_CIPHERING_ALGORITHM_NOT_SUPPORTED
@ GSM0808_CAUSE_CIPHERING_ALGORITHM_NOT_SUPPORTED
Definition: gsm_08_08.h:413
GSM0808_CAUSE_UPLINK_QUALITY
@ GSM0808_CAUSE_UPLINK_QUALITY
Definition: gsm_08_08.h:370
GSM0808_CAUSE_REQ_CODEC_TYPE_OR_CONFIG_UNAVAIL
@ GSM0808_CAUSE_REQ_CODEC_TYPE_OR_CONFIG_UNAVAIL
Definition: gsm_08_08.h:409
GSM0808_CAUSE_REQ_CODEC_TYPE_OR_CONFIG_NOT_SUPP
@ GSM0808_CAUSE_REQ_CODEC_TYPE_OR_CONFIG_NOT_SUPP
Definition: gsm_08_08.h:417
GSM0808_CAUSE_REQ_A_IF_TYPE_NOT_SUPP
@ GSM0808_CAUSE_REQ_A_IF_TYPE_NOT_SUPP
Definition: gsm_08_08.h:418
GSM0808_CAUSE_PREEMPTION
@ GSM0808_CAUSE_PREEMPTION
Definition: gsm_08_08.h:401
GSM0808_CAUSE_ALT_CHAN_CONFIG_REQUESTED
@ GSM0808_CAUSE_ALT_CHAN_CONFIG_REQUESTED
Definition: gsm_08_08.h:388
GSM0808_CAUSE_INCORRECT_VALUE
@ GSM0808_CAUSE_INCORRECT_VALUE
Definition: gsm_08_08.h:423
GSM0808_CAUSE_REQUESTED_OPT_NOT_AUTHORISED
@ GSM0808_CAUSE_REQUESTED_OPT_NOT_AUTHORISED
Definition: gsm_08_08.h:387
gsm0808_lcls_status
gsm0808_lcls_status
Definition: gsm_08_08.h:803
GSM0808_LCLS_STS_NA
@ GSM0808_LCLS_STS_NA
Definition: gsm_08_08.h:809
GSM0808_LCLS_STS_LOCALLY_SWITCHED
@ GSM0808_LCLS_STS_LOCALLY_SWITCHED
Definition: gsm_08_08.h:808
GSM0808_LCLS_STS_NOT_YET_LS
@ GSM0808_LCLS_STS_NOT_YET_LS
Definition: gsm_08_08.h:804
GSM0808_LCLS_STS_NO_LONGER_LS
@ GSM0808_LCLS_STS_NO_LONGER_LS
Definition: gsm_08_08.h:806
GSM0808_LCLS_STS_NOT_POSSIBLE_LS
@ GSM0808_LCLS_STS_NOT_POSSIBLE_LS
Definition: gsm_08_08.h:805
GSM0808_LCLS_STS_REQ_LCLS_NOT_SUPP
@ GSM0808_LCLS_STS_REQ_LCLS_NOT_SUPP
Definition: gsm_08_08.h:807
gsm0808_paging_info
gsm0808_paging_info
Definition: gsm_08_08.h:585
GSM0808_PAGINF_FOR_USSD
@ GSM0808_PAGINF_FOR_USSD
Definition: gsm_08_08.h:588
GSM0808_PAGINF_FOR_SMS
@ GSM0808_PAGINF_FOR_SMS
Definition: gsm_08_08.h:587
GSM0808_PAGINF_FOR_MT_CALL
@ GSM0808_PAGINF_FOR_MT_CALL
Definition: gsm_08_08.h:586
gsm0808_cause_class
gsm0808_cause_class
Definition: gsm_08_08.h:434
GSM0808_CAUSE_CLASS_NORM1
@ GSM0808_CAUSE_CLASS_NORM1
Definition: gsm_08_08.h:436
GSM0808_CAUSE_CLASS_INVAL
@ GSM0808_CAUSE_CLASS_INVAL
Definition: gsm_08_08.h:440
GSM0808_CAUSE_CLASS_SRV_OPT_NIMPL
@ GSM0808_CAUSE_CLASS_SRV_OPT_NIMPL
Definition: gsm_08_08.h:439
GSM0808_CAUSE_CLASS_RES_UNAVAIL
@ GSM0808_CAUSE_CLASS_RES_UNAVAIL
Definition: gsm_08_08.h:437
GSM0808_CAUSE_CLASS_SRV_OPT_NA
@ GSM0808_CAUSE_CLASS_SRV_OPT_NA
Definition: gsm_08_08.h:438
GSM0808_CAUSE_CLASS_PERR
@ GSM0808_CAUSE_CLASS_PERR
Definition: gsm_08_08.h:441
GSM0808_CAUSE_CLASS_INTW
@ GSM0808_CAUSE_CLASS_INTW
Definition: gsm_08_08.h:442
GSM0808_CAUSE_CLASS_NORM0
@ GSM0808_CAUSE_CLASS_NORM0
Definition: gsm_08_08.h:435
gsm0808_lcls_control
gsm0808_lcls_control
Definition: gsm_08_08.h:793
GSM0808_LCLS_CSC_RELEASE_LCLS
@ GSM0808_LCLS_CSC_RELEASE_LCLS
Definition: gsm_08_08.h:796
GSM0808_LCLS_CSC_BICAST_UL_AT_HANDOVER
@ GSM0808_LCLS_CSC_BICAST_UL_AT_HANDOVER
Definition: gsm_08_08.h:797
GSM0808_LCLS_CSC_DO_NOT_CONNECT
@ GSM0808_LCLS_CSC_DO_NOT_CONNECT
Definition: gsm_08_08.h:795
GSM0808_LCLS_CSC_BICAST_UL_AND_RECV_DL_AT_HANDOVER
@ GSM0808_LCLS_CSC_BICAST_UL_AND_RECV_DL_AT_HANDOVER
Definition: gsm_08_08.h:798
GSM0808_LCLS_CSC_CONNECT
@ GSM0808_LCLS_CSC_CONNECT
Definition: gsm_08_08.h:794
GSM0808_LCLS_CSC_NA
@ GSM0808_LCLS_CSC_NA
Definition: gsm_08_08.h:799
__attribute__
enum gsm0406_dlci_sapi __attribute__
gsm0808_speech_codec_defaults
gsm0808_speech_codec_defaults
Default speech codec configurations: Some codecs specified with struct gsm0808_speech_codec,...
Definition: gsm_08_08.h:657
GSM0808_SC_CFG_DEFAULT_HR_AMR
@ GSM0808_SC_CFG_DEFAULT_HR_AMR
Definition: gsm_08_08.h:659
GSM0808_SC_CFG_DEFAULT_FR_AMR_WB
@ GSM0808_SC_CFG_DEFAULT_FR_AMR_WB
Definition: gsm_08_08.h:661
GSM0808_SC_CFG_DEFAULT_OHR_AMR_WB
@ GSM0808_SC_CFG_DEFAULT_OHR_AMR_WB
Definition: gsm_08_08.h:663
GSM0808_SC_CFG_DEFAULT_OHR_AMR
@ GSM0808_SC_CFG_DEFAULT_OHR_AMR
Definition: gsm_08_08.h:660
GSM0808_SC_CFG_DEFAULT_OFR_AMR_WB
@ GSM0808_SC_CFG_DEFAULT_OFR_AMR_WB
Definition: gsm_08_08.h:662
GSM0808_SC_CFG_DEFAULT_FR_AMR
@ GSM0808_SC_CFG_DEFAULT_FR_AMR
Definition: gsm_08_08.h:658
gsm0808_data_rate_transp
gsm0808_data_rate_transp
Definition: gsm_08_08.h:509
GSM0808_DATA_RATE_TRANSP_2k4
@ GSM0808_DATA_RATE_TRANSP_2k4
Definition: gsm_08_08.h:515
GSM0808_DATA_RATE_TRANSP_600
@ GSM0808_DATA_RATE_TRANSP_600
Definition: gsm_08_08.h:517
GSM0808_DATA_RATE_TRANSP_1200_75
@ GSM0808_DATA_RATE_TRANSP_1200_75
Definition: gsm_08_08.h:518
GSM0808_DATA_RATE_TRANSP_9k6
@ GSM0808_DATA_RATE_TRANSP_9k6
Definition: gsm_08_08.h:513
GSM0808_DATA_RATE_TRANSP_4k8
@ GSM0808_DATA_RATE_TRANSP_4k8
Definition: gsm_08_08.h:514
GSM0808_DATA_RATE_TRANSP_14k4
@ GSM0808_DATA_RATE_TRANSP_14k4
Definition: gsm_08_08.h:512
GSM0808_DATA_RATE_TRANSP_1k2
@ GSM0808_DATA_RATE_TRANSP_1k2
Definition: gsm_08_08.h:516
GSM0808_DATA_RATE_TRANSP_32k0
@ GSM0808_DATA_RATE_TRANSP_32k0
Definition: gsm_08_08.h:510
GSM0808_DATA_RATE_TRANSP_28k8
@ GSM0808_DATA_RATE_TRANSP_28k8
Definition: gsm_08_08.h:511
GSM0808_IE_CODING
GSM0808_IE_CODING
Definition: gsm_08_08.h:193
GSM0808_IE_LCS_CAUSE
@ GSM0808_IE_LCS_CAUSE
Definition: gsm_08_08.h:261
GSM0808_IE_KC_128
@ GSM0808_IE_KC_128
Definition: gsm_08_08.h:310
GSM0808_IE_LAYER_3_MESSAGE_CONTENTS
@ GSM0808_IE_LAYER_3_MESSAGE_CONTENTS
Definition: gsm_08_08.h:225
GSM0808_IE_CS_TO_PS_SRVCC_IND
@ GSM0808_IE_CS_TO_PS_SRVCC_IND
Definition: gsm_08_08.h:325
GSM0808_IE_NEW_BSS_TO_OLD_BSS_INFO
@ GSM0808_IE_NEW_BSS_TO_OLD_BSS_INFO
Definition: gsm_08_08.h:277
GSM0808_IE_CONNECTION_RELEASE_RQSTED
@ GSM0808_IE_CONNECTION_RELEASE_RQSTED
Definition: gsm_08_08.h:247
GSM0808_IE_EMERGENCY_SET_INDICATION
@ GSM0808_IE_EMERGENCY_SET_INDICATION
Definition: gsm_08_08.h:287
GSM0808_IE_CS_TO_PS_SRVCC
@ GSM0808_IE_CS_TO_PS_SRVCC
Definition: gsm_08_08.h:323
GSM0808_IE_SMS_TO_VGCS
@ GSM0808_IE_SMS_TO_VGCS
Definition: gsm_08_08.h:290
GSM0808_IE_DIAGNOSTIC
@ GSM0808_IE_DIAGNOSTIC
Definition: gsm_08_08.h:224
GSM0808_IE_REROUTE_COMPL_OUTCOME
@ GSM0808_IE_REROUTE_COMPL_OUTCOME
Definition: gsm_08_08.h:315
GSM0808_IE_CURRENT_CHANNEL_TYPE_1
@ GSM0808_IE_CURRENT_CHANNEL_TYPE_1
Definition: gsm_08_08.h:242
GSM0808_IE_OMCID
@ GSM0808_IE_OMCID
Definition: gsm_08_08.h:235
GSM0808_IE_CIRCUIT_POOL_LIST
@ GSM0808_IE_CIRCUIT_POOL_LIST
Definition: gsm_08_08.h:239
GSM0808_IE_CELL_ID_LIST_SEG_CELLS_TBE
@ GSM0808_IE_CELL_ID_LIST_SEG_CELLS_TBE
Definition: gsm_08_08.h:294
GSM0808_IE_SPEECH_VERSION
@ GSM0808_IE_SPEECH_VERSION
Definition: gsm_08_08.h:244
GSM0808_IE_CHOSEN_CHANNEL
@ GSM0808_IE_CHOSEN_CHANNEL
Definition: gsm_08_08.h:226
GSM0808_IE_REROUTE_REJ_CAUSE
@ GSM0808_IE_REROUTE_REJ_CAUSE
Definition: gsm_08_08.h:313
GSM0808_IE_DOWNLINK_DTX_FLAG
@ GSM0808_IE_DOWNLINK_DTX_FLAG
Definition: gsm_08_08.h:218
GSM0808_IE_VGCS_VBS_CELL_STATUS
@ GSM0808_IE_VGCS_VBS_CELL_STATUS
Definition: gsm_08_08.h:292
GSM0808_IE_RESERVED_2
@ GSM0808_IE_RESERVED_2
Definition: gsm_08_08.h:209
GSM0808_IE_FORWARD_INDICATOR
@ GSM0808_IE_FORWARD_INDICATOR
Definition: gsm_08_08.h:236
GSM0808_IE_CSG_IDENTIFIER
@ GSM0808_IE_CSG_IDENTIFIER
Definition: gsm_08_08.h:311
GSM0808_IE_GANSS_ASSISTANCE_DATA
@ GSM0808_IE_GANSS_ASSISTANCE_DATA
Definition: gsm_08_08.h:297
GSM0808_IE_RESERVED_3
@ GSM0808_IE_RESERVED_3
Definition: gsm_08_08.h:210
GSM0808_IE_LCLS_BSS_STATUS
@ GSM0808_IE_LCLS_BSS_STATUS
Definition: gsm_08_08.h:320
GSM0808_IE_NETWORK_ELEMENT_IDENTITY
@ GSM0808_IE_NETWORK_ELEMENT_IDENTITY
Definition: gsm_08_08.h:264
GSM0808_IE_CHANNEL_NEEDED
@ GSM0808_IE_CHANNEL_NEEDED
Definition: gsm_08_08.h:229
GSM0808_IE_AOIP_TRASP_ADDR
@ GSM0808_IE_AOIP_TRASP_ADDR
Definition: gsm_08_08.h:304
GSM0808_IE_TIME_INDICATION
@ GSM0808_IE_TIME_INDICATION
Definition: gsm_08_08.h:240
GSM0808_IE_SRC_ENB_TO_TGT_ENB_TRANSP
@ GSM0808_IE_SRC_ENB_TO_TGT_ENB_TRANSP
Definition: gsm_08_08.h:324
GSM0808_IE_RESOURCE_INDICATION_METHOD
@ GSM0808_IE_RESOURCE_INDICATION_METHOD
Definition: gsm_08_08.h:221
GSM0808_IE_DECIPHERING_KEYS
@ GSM0808_IE_DECIPHERING_KEYS
Definition: gsm_08_08.h:266
GSM0808_IE_CELL_ID_LIST_SEG_EST_CELLS
@ GSM0808_IE_CELL_ID_LIST_SEG_EST_CELLS
Definition: gsm_08_08.h:293
GSM0808_IE_LCS_CLIENT_TYPE
@ GSM0808_IE_LCS_CLIENT_TYPE
Definition: gsm_08_08.h:262
GSM0808_IE_ATTACH_INDICATOR
@ GSM0808_IE_ATTACH_INDICATOR
Definition: gsm_08_08.h:330
GSM0808_IE_CELL_ID_LIST_SEG_REL_CELLS
@ GSM0808_IE_CELL_ID_LIST_SEG_REL_CELLS
Definition: gsm_08_08.h:295
GSM0808_IE_LCLS_CONFIG
@ GSM0808_IE_LCLS_CONFIG
Definition: gsm_08_08.h:317
GSM0808_IE_LSA_IDENTIFIER_LIST
@ GSM0808_IE_LSA_IDENTIFIER_LIST
Definition: gsm_08_08.h:253
GSM0808_IE_EMLPP_PRIORITY
@ GSM0808_IE_EMLPP_PRIORITY
Definition: gsm_08_08.h:249
GSM0808_IE_LCLS_BREAK_REQ
@ GSM0808_IE_LCLS_BREAK_REQ
Definition: gsm_08_08.h:321
GSM0808_IE_PS_REGISTERED_OPERATOR
@ GSM0808_IE_PS_REGISTERED_OPERATOR
Definition: gsm_08_08.h:332
GSM0808_IE_THEMWI_RTP_EXTENSIONS
@ GSM0808_IE_THEMWI_RTP_EXTENSIONS
Definition: gsm_08_08.h:338
GSM0808_IE_GANSS_LOCATION_TYPE
@ GSM0808_IE_GANSS_LOCATION_TYPE
Definition: gsm_08_08.h:299
GSM0808_IE_SOURCE_RNC_TO_TARGET_RNC_TRANSPARENT_CDMA2000
@ GSM0808_IE_SOURCE_RNC_TO_TARGET_RNC_TRANSPARENT_CDMA2000
Definition: gsm_08_08.h:272
GSM0808_IE_RESOURCE_AVAILABLE
@ GSM0808_IE_RESOURCE_AVAILABLE
Definition: gsm_08_08.h:196
GSM0808_IE_PAGING_INFO
@ GSM0808_IE_PAGING_INFO
Definition: gsm_08_08.h:282
GSM0808_IE_PERIODICITY
@ GSM0808_IE_PERIODICITY
Definition: gsm_08_08.h:205
GSM0808_IE_TRANSACTIONID
@ GSM0808_IE_TRANSACTIONID
Definition: gsm_08_08.h:233
GSM0808_IE_CIRCUIT_IDENTITY_CODE_LIST
@ GSM0808_IE_CIRCUIT_IDENTITY_CODE_LIST
Definition: gsm_08_08.h:223
GSM0808_IE_RESERVED_1
@ GSM0808_IE_RESERVED_1
Definition: gsm_08_08.h:208
GSM0808_IE_TRIGGERID
@ GSM0808_IE_TRIGGERID
Definition: gsm_08_08.h:231
GSM0808_IE_TALKER_FLAG
@ GSM0808_IE_TALKER_FLAG
Definition: gsm_08_08.h:246
GSM0808_IE_SEGMENTATION
@ GSM0808_IE_SEGMENTATION
Definition: gsm_08_08.h:269
GSM0808_IE_OLD_LAI
@ GSM0808_IE_OLD_LAI
Definition: gsm_08_08.h:329
GSM0808_IE_LAYER_3_INFORMATION
@ GSM0808_IE_LAYER_3_INFORMATION
Definition: gsm_08_08.h:216
GSM0808_IE_LSA_ACCESS_CTRL_SUPPR
@ GSM0808_IE_LSA_ACCESS_CTRL_SUPPR
Definition: gsm_08_08.h:256
GSM0808_IE_GANSS_POSITIONING_DATA
@ GSM0808_IE_GANSS_POSITIONING_DATA
Definition: gsm_08_08.h:298
GSM0808_IE_DATA_IDENTITY
@ GSM0808_IE_DATA_IDENTITY
Definition: gsm_08_08.h:301
GSM0808_IE_RESERVED_0
@ GSM0808_IE_RESERVED_0
Definition: gsm_08_08.h:195
GSM0808_IE_SEND_SEQ_NUM
@ GSM0808_IE_SEND_SEQ_NUM
Definition: gsm_08_08.h:314
GSM0808_IE_CELL_ID_LIST_SEG_NE_CELLS
@ GSM0808_IE_CELL_ID_LIST_SEG_NE_CELLS
Definition: gsm_08_08.h:296
GSM0808_IE_CONFIG_EVO_INDI
@ GSM0808_IE_CONFIG_EVO_INDI
Definition: gsm_08_08.h:250
GSM0808_IE_APP_DATA
@ GSM0808_IE_APP_DATA
Definition: gsm_08_08.h:300
GSM0808_IE_CALL_ID_LIST
@ GSM0808_IE_CALL_ID_LIST
Definition: gsm_08_08.h:308
GSM0808_IE_CHANNEL_TYPE
@ GSM0808_IE_CHANNEL_TYPE
Definition: gsm_08_08.h:204
GSM0808_IE_TMSI
@ GSM0808_IE_TMSI
Definition: gsm_08_08.h:202
GSM0808_IE_RESPONSE_RQST
@ GSM0808_IE_RESPONSE_RQST
Definition: gsm_08_08.h:220
GSM0808_IE_TALKER_IDENTITY
@ GSM0808_IE_TALKER_IDENTITY
Definition: gsm_08_08.h:288
GSM0808_IE_LCS_PRIORITY
@ GSM0808_IE_LCS_PRIORITY
Definition: gsm_08_08.h:257
GSM0808_IE_PRIORITY
@ GSM0808_IE_PRIORITY
Definition: gsm_08_08.h:199
GSM0808_IE_RESERVED_4
@ GSM0808_IE_RESERVED_4
Definition: gsm_08_08.h:215
GSM0808_IE_OLD_BSS_TO_NEW_BSS_INFORMATION
@ GSM0808_IE_OLD_BSS_TO_NEW_BSS_INFORMATION
Definition: gsm_08_08.h:251
GSM0800_IE_INTER_SYSTEM_INFO
@ GSM0800_IE_INTER_SYSTEM_INFO
Definition: gsm_08_08.h:278
GSM0808_IE_CELL_ID_LIST_SEGMENT
@ GSM0808_IE_CELL_ID_LIST_SEGMENT
Definition: gsm_08_08.h:289
GSM0808_IE_CALL_ID
@ GSM0808_IE_CALL_ID
Definition: gsm_08_08.h:307
GSM0808_IE_GERAN_BSC_CONTAINER
@ GSM0808_IE_GERAN_BSC_CONTAINER
Definition: gsm_08_08.h:276
GSM0808_IE_NUMBER_OF_MSS
@ GSM0808_IE_NUMBER_OF_MSS
Definition: gsm_08_08.h:207
GSM0808_IE_LCS_QOS
@ GSM0808_IE_LCS_QOS
Definition: gsm_08_08.h:255
GSM0808_IE_RESERVED_5
@ GSM0808_IE_RESERVED_5
Definition: gsm_08_08.h:273
GSM0808_IE_GPS_ASSISTANCE_DATA
@ GSM0808_IE_GPS_ASSISTANCE_DATA
Definition: gsm_08_08.h:265
GSM0808_IE_GERAN_CLASSMARK
@ GSM0808_IE_GERAN_CLASSMARK
Definition: gsm_08_08.h:275
GSM0808_IE_LSA_IDENTIFIER
@ GSM0808_IE_LSA_IDENTIFIER
Definition: gsm_08_08.h:252
GSM0808_IE_CLASSMARK_INFORMATION_TYPE_1
@ GSM0808_IE_CLASSMARK_INFORMATION_TYPE_1
Definition: gsm_08_08.h:222
GSM0808_IE_LOCATION_TYPE
@ GSM0808_IE_LOCATION_TYPE
Definition: gsm_08_08.h:258
GSM0808_IE_VSTK_RAND_INFO
@ GSM0808_IE_VSTK_RAND_INFO
Definition: gsm_08_08.h:280
GSM0808_IE_RETURN_ERROR_CAUSE
@ GSM0808_IE_RETURN_ERROR_CAUSE
Definition: gsm_08_08.h:268
GSM0808_IE_CLASSMARK_INFORMATION_T2
@ GSM0808_IE_CLASSMARK_INFORMATION_T2
Definition: gsm_08_08.h:211
GSM0808_IE_RESERVED_6
@ GSM0808_IE_RESERVED_6
Definition: gsm_08_08.h:274
GSM0808_IE_LAST_USED_EUTRAN_PLMN_ID
@ GSM0808_IE_LAST_USED_EUTRAN_PLMN_ID
Definition: gsm_08_08.h:328
GSM0808_IE_SOURCE_RNC_TO_TARGET_RNC_TRANSPARENT_UMTS
@ GSM0808_IE_SOURCE_RNC_TO_TARGET_RNC_TRANSPARENT_UMTS
Definition: gsm_08_08.h:271
GSM0808_IE_VSTK_INFO
@ GSM0808_IE_VSTK_INFO
Definition: gsm_08_08.h:281
GSM0808_IE_DLCI
@ GSM0808_IE_DLCI
Definition: gsm_08_08.h:217
GSM0808_IE_REDIR_ATTEMPT_FLAG
@ GSM0808_IE_REDIR_ATTEMPT_FLAG
Definition: gsm_08_08.h:312
GSM0808_IE_OSMO_OSMUX_CID
@ GSM0808_IE_OSMO_OSMUX_CID
Definition: gsm_08_08.h:337
GSM0808_IE_CIPHER_RESPONSE_MODE
@ GSM0808_IE_CIPHER_RESPONSE_MODE
Definition: gsm_08_08.h:228
GSM0808_IE_POSITIONING_DATA
@ GSM0808_IE_POSITIONING_DATA
Definition: gsm_08_08.h:260
GSM0808_IE_LCLS_CORR_NOT_NEEDED
@ GSM0808_IE_LCLS_CORR_NOT_NEEDED
Definition: gsm_08_08.h:319
GSM0808_IE_MOBILE_IDENTITY
@ GSM0808_IE_MOBILE_IDENTITY
Definition: gsm_08_08.h:234
GSM0808_IE_CLASSMARK_INFORMATION_T3
@ GSM0808_IE_CLASSMARK_INFORMATION_T3
Definition: gsm_08_08.h:212
GSM0808_IE_OSMO_OSMUX_SUPPORT
@ GSM0808_IE_OSMO_OSMUX_SUPPORT
Definition: gsm_08_08.h:336
GSM0808_IE_GROUP_CALL_REFERENCE
@ GSM0808_IE_GROUP_CALL_REFERENCE
Definition: gsm_08_08.h:248
GSM0808_IE_RETURN_ERROR_RQST
@ GSM0808_IE_RETURN_ERROR_RQST
Definition: gsm_08_08.h:267
GSM0808_IE_VGCS_TALKER_MODE
@ GSM0808_IE_VGCS_TALKER_MODE
Definition: gsm_08_08.h:291
GSM0808_IE_A_IF_SEL_FOR_RESET
@ GSM0808_IE_A_IF_SEL_FOR_RESET
Definition: gsm_08_08.h:309
GSM0808_IE_IMSI
@ GSM0808_IE_IMSI
Definition: gsm_08_08.h:201
GSM0808_IE_CELL_IDENTIFIER
@ GSM0808_IE_CELL_IDENTIFIER
Definition: gsm_08_08.h:198
GSM0808_IE_RESOURCE_SITUATION
@ GSM0808_IE_RESOURCE_SITUATION
Definition: gsm_08_08.h:241
GSM0808_IE_CS_REGISTERED_OPERATOR
@ GSM0808_IE_CS_REGISTERED_OPERATOR
Definition: gsm_08_08.h:333
GSM0808_IE_TRACE_TYPE
@ GSM0808_IE_TRACE_TYPE
Definition: gsm_08_08.h:230
GSM0808_IE_LAYER_3_HEADER_INFORMATION
@ GSM0808_IE_LAYER_3_HEADER_INFORMATION
Definition: gsm_08_08.h:200
GSM0808_IE_EXTENDED_RESOURCE_INDICATOR
@ GSM0808_IE_EXTENDED_RESOURCE_INDICATOR
Definition: gsm_08_08.h:206
GSM0808_IE_APDU
@ GSM0808_IE_APDU
Definition: gsm_08_08.h:263
GSM0808_IE_INTERFERENCE_BAND_TO_USE
@ GSM0808_IE_INTERFERENCE_BAND_TO_USE
Definition: gsm_08_08.h:213
GSM0808_IE_MSISDN
@ GSM0808_IE_MSISDN
Definition: gsm_08_08.h:303
GSM0808_IE_CIRCUIT_POOL
@ GSM0808_IE_CIRCUIT_POOL
Definition: gsm_08_08.h:238
GSM0808_IE_VELOCITY_ESTIMATE
@ GSM0808_IE_VELOCITY_ESTIMATE
Definition: gsm_08_08.h:284
GSM0808_IE_CSFB_INDICATION
@ GSM0808_IE_CSFB_INDICATION
Definition: gsm_08_08.h:322
GSM0808_IE_LCLS_CONN_STATUS_CTRL
@ GSM0808_IE_LCLS_CONN_STATUS_CTRL
Definition: gsm_08_08.h:318
GSM0808_IE_ENCRYPTION_INFORMATION
@ GSM0808_IE_ENCRYPTION_INFORMATION
Definition: gsm_08_08.h:203
GSM0808_IE_GLOBAL_CALL_REF
@ GSM0808_IE_GLOBAL_CALL_REF
Definition: gsm_08_08.h:316
GSM0808_IE_QUEUEING_INDICATOR
@ GSM0808_IE_QUEUEING_INDICATOR
Definition: gsm_08_08.h:243
GSM0808_IE_LOCATION_ESTIMATE
@ GSM0808_IE_LOCATION_ESTIMATE
Definition: gsm_08_08.h:259
GSM0808_IE_SNA_ACCESS_INFO
@ GSM0808_IE_SNA_ACCESS_INFO
Definition: gsm_08_08.h:279
GSM0808_IE_TRACE_REFERENCE
@ GSM0808_IE_TRACE_REFERENCE
Definition: gsm_08_08.h:232
GSM0808_IE_RR_CAUSE
@ GSM0808_IE_RR_CAUSE
Definition: gsm_08_08.h:214
GSM0808_IE_CN_TO_MS_TRANSP_INFO
@ GSM0808_IE_CN_TO_MS_TRANSP_INFO
Definition: gsm_08_08.h:326
GSM0808_IE_IMEI
@ GSM0808_IE_IMEI
Definition: gsm_08_08.h:283
GSM0808_IE_LSA_INFORMATION
@ GSM0808_IE_LSA_INFORMATION
Definition: gsm_08_08.h:254
GSM0808_IE_APP_DATA_INFO
@ GSM0808_IE_APP_DATA_INFO
Definition: gsm_08_08.h:302
GSM0808_IE_TOTAL_RESOURCE_ACCESSIBLE
@ GSM0808_IE_TOTAL_RESOURCE_ACCESSIBLE
Definition: gsm_08_08.h:227
GSM0808_IE_CHOSEN_ENCR_ALG
@ GSM0808_IE_CHOSEN_ENCR_ALG
Definition: gsm_08_08.h:237
GSM0808_IE_ASSIGNMENT_REQUIREMENT
@ GSM0808_IE_ASSIGNMENT_REQUIREMENT
Definition: gsm_08_08.h:245
GSM0808_IE_SERVICE_HANDOVER
@ GSM0808_IE_SERVICE_HANDOVER
Definition: gsm_08_08.h:270
GSM0808_IE_SPEECH_CODEC_LIST
@ GSM0808_IE_SPEECH_CODEC_LIST
Definition: gsm_08_08.h:305
GSM0808_IE_SELECTED_PLMN_ID
@ GSM0808_IE_SELECTED_PLMN_ID
Definition: gsm_08_08.h:327
GSM0808_IE_CELL_IDENTIFIER_LIST
@ GSM0808_IE_CELL_IDENTIFIER_LIST
Definition: gsm_08_08.h:219
GSM0808_IE_SELECTED_OPERATOR
@ GSM0808_IE_SELECTED_OPERATOR
Definition: gsm_08_08.h:331
GSM0808_IE_VGCS_FEATURE_FLAGS
@ GSM0808_IE_VGCS_FEATURE_FLAGS
Definition: gsm_08_08.h:285
GSM0808_IE_SPEECH_CODEC
@ GSM0808_IE_SPEECH_CODEC
Definition: gsm_08_08.h:306
GSM0808_IE_CAUSE
@ GSM0808_IE_CAUSE
Definition: gsm_08_08.h:197
GSM0808_IE_CIRCUIT_IDENTITY_CODE
@ GSM0808_IE_CIRCUIT_IDENTITY_CODE
Definition: gsm_08_08.h:194
GSM0808_IE_TALKER_PRIORITY
@ GSM0808_IE_TALKER_PRIORITY
Definition: gsm_08_08.h:286
gsm0808_chan_rate_type_data
gsm0808_chan_rate_type_data
Definition: gsm_08_08.h:455
GSM0808_DATA_FULL_PREF_NO_CHANGE
@ GSM0808_DATA_FULL_PREF_NO_CHANGE
Definition: gsm_08_08.h:460
GSM0808_DATA_FULL_BM
@ GSM0808_DATA_FULL_BM
Definition: gsm_08_08.h:456
GSM0808_DATA_HALF_LM
@ GSM0808_DATA_HALF_LM
Definition: gsm_08_08.h:457
GSM0808_DATA_HALF_PREF_NO_CHANGE
@ GSM0808_DATA_HALF_PREF_NO_CHANGE
Definition: gsm_08_08.h:461
GSM0808_DATA_HALF_PREF
@ GSM0808_DATA_HALF_PREF
Definition: gsm_08_08.h:459
GSM0808_DATA_MULTI_MASK
@ GSM0808_DATA_MULTI_MASK
Definition: gsm_08_08.h:462
GSM0808_DATA_FULL_PREF
@ GSM0808_DATA_FULL_PREF
Definition: gsm_08_08.h:458
GSM0808_DATA_MULTI_MASK_NO_CHANGE
@ GSM0808_DATA_MULTI_MASK_NO_CHANGE
Definition: gsm_08_08.h:463
gsm0808_speech_codec_rate_defaults
gsm0808_speech_codec_rate_defaults
Default speech codec configurations broken down by rate.
Definition: gsm_08_08.h:672
GSM0808_SC_CFG_DEFAULT_AMR_5_15
@ GSM0808_SC_CFG_DEFAULT_AMR_5_15
Definition: gsm_08_08.h:674
GSM0808_SC_CFG_DEFAULT_AMR_10_2
@ GSM0808_SC_CFG_DEFAULT_AMR_10_2
Definition: gsm_08_08.h:679
GSM0808_SC_CFG_DEFAULT_AMR_4_75
@ GSM0808_SC_CFG_DEFAULT_AMR_4_75
Definition: gsm_08_08.h:673
GSM0808_SC_CFG_DEFAULT_AMR_7_95
@ GSM0808_SC_CFG_DEFAULT_AMR_7_95
Definition: gsm_08_08.h:678
GSM0808_SC_CFG_DEFAULT_AMR_7_40
@ GSM0808_SC_CFG_DEFAULT_AMR_7_40
Definition: gsm_08_08.h:677
GSM0808_SC_CFG_DEFAULT_AMR_12_2
@ GSM0808_SC_CFG_DEFAULT_AMR_12_2
Definition: gsm_08_08.h:680
GSM0808_SC_CFG_DEFAULT_AMR_6_70
@ GSM0808_SC_CFG_DEFAULT_AMR_6_70
Definition: gsm_08_08.h:676
GSM0808_SC_CFG_DEFAULT_AMR_5_90
@ GSM0808_SC_CFG_DEFAULT_AMR_5_90
Definition: gsm_08_08.h:675
CELL_ID_LIST_LAC_MAXLEN
#define CELL_ID_LIST_LAC_MAXLEN
Definition: gsm_08_08.h:768
gsm0808_speech_codec_type
gsm0808_speech_codec_type
3GPP TS 48.008, 3.2.2.103 Speech Codec Type
Definition: gsm_08_08.h:548
GSM0808_SCT_HR4
@ GSM0808_SCT_HR4
OHR AMR-WB.
Definition: gsm_08_08.h:556
GSM0808_SCT_FR3
@ GSM0808_SCT_FR3
FR AMR.
Definition: gsm_08_08.h:551
GSM0808_SCT_HR6
@ GSM0808_SCT_HR6
OHR AMR.
Definition: gsm_08_08.h:557
GSM0808_SCT_FR5
@ GSM0808_SCT_FR5
FR AMR-WB.
Definition: gsm_08_08.h:553
GSM0808_SCT_HR3
@ GSM0808_SCT_HR3
HR_AMR.
Definition: gsm_08_08.h:555
GSM0808_SCT_CSD
@ GSM0808_SCT_CSD
CSData (see also TS 26.103)
Definition: gsm_08_08.h:558
GSM0808_SCT_FR4
@ GSM0808_SCT_FR4
OFR AMR-WB.
Definition: gsm_08_08.h:552
GSM0808_SCT_FR1
@ GSM0808_SCT_FR1
GSM FR.
Definition: gsm_08_08.h:549
GSM0808_SCT_HR1
@ GSM0808_SCT_HR1
GSM_HR.
Definition: gsm_08_08.h:554
GSM0808_SCT_FR2
@ GSM0808_SCT_FR2
GSM EFR.
Definition: gsm_08_08.h:550
gsm0808_lcls_config
gsm0808_lcls_config
Definition: gsm_08_08.h:782
GSM0808_LCLS_CFG_NA
@ GSM0808_LCLS_CFG_NA
Definition: gsm_08_08.h:789
GSM0808_LCLS_CFG_BOTH_WAY_AND_SEND_DL_BLOCK_LOCAL_DL
@ GSM0808_LCLS_CFG_BOTH_WAY_AND_SEND_DL_BLOCK_LOCAL_DL
Definition: gsm_08_08.h:786
GSM0808_LCLS_CFG_BOTH_WAY
@ GSM0808_LCLS_CFG_BOTH_WAY
Definition: gsm_08_08.h:783
GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL
@ GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL
Definition: gsm_08_08.h:784
GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL_SEND_DL
@ GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL_SEND_DL
Definition: gsm_08_08.h:787
GSM0808_LCLS_CFG_BOTH_WAY_AND_SEND_DL
@ GSM0808_LCLS_CFG_BOTH_WAY_AND_SEND_DL
Definition: gsm_08_08.h:785
GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL_SEND_DL_BLOCK_LOCAL_DL
@ GSM0808_LCLS_CFG_BOTH_WAY_AND_BICAST_UL_SEND_DL_BLOCK_LOCAL_DL
Definition: gsm_08_08.h:788
ENCRY_INFO_PERM_ALGO_MAXLEN
#define ENCRY_INFO_PERM_ALGO_MAXLEN
Definition: gsm_08_08.h:760
gsm0808_amr_mode
gsm0808_amr_mode
Definition: gsm_08_08.h:705
GSM0808_AMR_MODE_10_2
@ GSM0808_AMR_MODE_10_2
Definition: gsm_08_08.h:712
GSM0808_AMR_MODE_6_70
@ GSM0808_AMR_MODE_6_70
Definition: gsm_08_08.h:709
GSM0808_AMR_MODE_12_2
@ GSM0808_AMR_MODE_12_2
Definition: gsm_08_08.h:713
GSM0808_AMR_MODE_7_95
@ GSM0808_AMR_MODE_7_95
Definition: gsm_08_08.h:711
GSM0808_AMR_MODE_5_90
@ GSM0808_AMR_MODE_5_90
Definition: gsm_08_08.h:708
GSM0808_AMR_MODE_4_75
@ GSM0808_AMR_MODE_4_75
Definition: gsm_08_08.h:706
GSM0808_AMR_MODE_5_15
@ GSM0808_AMR_MODE_5_15
Definition: gsm_08_08.h:707
GSM0808_AMR_MODE_7_40
@ GSM0808_AMR_MODE_7_40
Definition: gsm_08_08.h:710
gsm0808_amr_mode_name
static const char * gsm0808_amr_mode_name(enum gsm0808_amr_mode val)
Definition: gsm_08_08.h:716
gsm0808_permitted_speech
gsm0808_permitted_speech
GSM 08.08 3.2.2.11 Channel Type (see also 3GPP TS 48.008, section 3.2.2.11)
Definition: gsm_08_08.h:494
GSM0808_PERM_FR2
@ GSM0808_PERM_FR2
GSM EFR.
Definition: gsm_08_08.h:496
GSM0808_PERM_HR6
@ GSM0808_PERM_HR6
OHR AMR.
Definition: gsm_08_08.h:504
GSM0808_PERM_FR1
@ GSM0808_PERM_FR1
GSM FR.
Definition: gsm_08_08.h:495
GSM0808_PERM_HR1
@ GSM0808_PERM_HR1
GSM HR.
Definition: gsm_08_08.h:500
GSM0808_PERM_HR4
@ GSM0808_PERM_HR4
OHR AMR-WB.
Definition: gsm_08_08.h:503
GSM0808_PERM_HR3
@ GSM0808_PERM_HR3
HR AMR.
Definition: gsm_08_08.h:502
GSM0808_PERM_HR2
@ GSM0808_PERM_HR2
(deprecated)
Definition: gsm_08_08.h:501
GSM0808_PERM_FR3
@ GSM0808_PERM_FR3
FR AMR.
Definition: gsm_08_08.h:497
GSM0808_PERM_FR4
@ GSM0808_PERM_FR4
OFR AMR-WB.
Definition: gsm_08_08.h:498
GSM0808_PERM_FR5
@ GSM0808_PERM_FR5
FR AMR-WB.
Definition: gsm_08_08.h:499
CELL_IDENT
CELL_IDENT
Definition: gsm_08_08.h:17
CELL_IDENT_SAI
@ CELL_IDENT_SAI
Definition: gsm_08_08.h:28
CELL_IDENT_UTRAN_PLMN_LAC_RNC
@ CELL_IDENT_UTRAN_PLMN_LAC_RNC
Definition: gsm_08_08.h:25
CELL_IDENT_LAC
@ CELL_IDENT_LAC
Definition: gsm_08_08.h:23
CELL_IDENT_UTRAN_RNC
@ CELL_IDENT_UTRAN_RNC
Definition: gsm_08_08.h:26
CELL_IDENT_WHOLE_GLOBAL
@ CELL_IDENT_WHOLE_GLOBAL
Definition: gsm_08_08.h:18
CELL_IDENT_UTRAN_LAC_RNC
@ CELL_IDENT_UTRAN_LAC_RNC
Definition: gsm_08_08.h:27
CELL_IDENT_WHOLE_GLOBAL_PS
@ CELL_IDENT_WHOLE_GLOBAL_PS
Definition: gsm_08_08.h:31
CELL_IDENT_BSS
@ CELL_IDENT_BSS
Definition: gsm_08_08.h:24
CELL_IDENT_NO_CELL
@ CELL_IDENT_NO_CELL
Definition: gsm_08_08.h:21
CELL_IDENT_LAC_AND_CI
@ CELL_IDENT_LAC_AND_CI
Definition: gsm_08_08.h:19
CELL_IDENT_CI
@ CELL_IDENT_CI
Definition: gsm_08_08.h:20
CELL_IDENT_LAI
@ CELL_IDENT_LAI
Definition: gsm_08_08.h:22
gsm0808_chosen_enc_alg
gsm0808_chosen_enc_alg
Definition: gsm_08_08.h:572
GSM0808_ALG_ID_A5_0
@ GSM0808_ALG_ID_A5_0
Definition: gsm_08_08.h:573
GSM0808_ALG_ID_A5_7
@ GSM0808_ALG_ID_A5_7
Definition: gsm_08_08.h:580
GSM0808_ALG_ID_A5_4
@ GSM0808_ALG_ID_A5_4
Definition: gsm_08_08.h:577
GSM0808_ALG_ID_A5_5
@ GSM0808_ALG_ID_A5_5
Definition: gsm_08_08.h:578
GSM0808_ALG_ID_A5_6
@ GSM0808_ALG_ID_A5_6
Definition: gsm_08_08.h:579
GSM0808_ALG_ID_A5_2
@ GSM0808_ALG_ID_A5_2
Definition: gsm_08_08.h:575
GSM0808_ALG_ID_A5_1
@ GSM0808_ALG_ID_A5_1
Definition: gsm_08_08.h:574
GSM0808_ALG_ID_A5_3
@ GSM0808_ALG_ID_A5_3
Definition: gsm_08_08.h:576
BSSAP_MSG_TYPE
BSSAP_MSG_TYPE
Definition: gsm_08_08.h:37
BSSAP_MSG_BSS_MANAGEMENT
@ BSSAP_MSG_BSS_MANAGEMENT
Definition: gsm_08_08.h:38
BSSAP_MSG_DTAP
@ BSSAP_MSG_DTAP
Definition: gsm_08_08.h:39
gsm0808_speech_codec_rate
gsm0808_speech_codec_rate
Single speech codec configurations broken down by rate.
Definition: gsm_08_08.h:689
GSM0808_SC_CFG_AMR_4_75
@ GSM0808_SC_CFG_AMR_4_75
Definition: gsm_08_08.h:690
GSM0808_SC_CFG_AMR_7_40
@ GSM0808_SC_CFG_AMR_7_40
Definition: gsm_08_08.h:694
GSM0808_SC_CFG_AMR_10_2
@ GSM0808_SC_CFG_AMR_10_2
Definition: gsm_08_08.h:696
GSM0808_SC_CFG_AMR_4_75_5_90_7_40_12_20
@ GSM0808_SC_CFG_AMR_4_75_5_90_7_40_12_20
Definition: gsm_08_08.h:691
GSM0808_SC_CFG_AMR_6_70
@ GSM0808_SC_CFG_AMR_6_70
Definition: gsm_08_08.h:693
GSM0808_SC_CFG_AMR_12_2
@ GSM0808_SC_CFG_AMR_12_2
Definition: gsm_08_08.h:697
GSM0808_SC_CFG_AMR_7_95
@ GSM0808_SC_CFG_AMR_7_95
Definition: gsm_08_08.h:695
GSM0808_SC_CFG_AMR_5_90
@ GSM0808_SC_CFG_AMR_5_90
Definition: gsm_08_08.h:692
GSM0808_SIGNALLING_FIELD_ELEMENT_CODING
GSM0808_SIGNALLING_FIELD_ELEMENT_CODING
Definition: gsm_08_08.h:343
GSM0808_FE_IE_GPRS_SUSPEND_INFORMATION
@ GSM0808_FE_IE_GPRS_SUSPEND_INFORMATION
Definition: gsm_08_08.h:347
GSM0808_FE_IE_DUAL_TRANSFER_MODE_INFORMATION
@ GSM0808_FE_IE_DUAL_TRANSFER_MODE_INFORMATION
Definition: gsm_08_08.h:349
GSM0808_FE_IE_DTM_HANDOVER_COMMAND_INDICATION
@ GSM0808_FE_IE_DTM_HANDOVER_COMMAND_INDICATION
Definition: gsm_08_08.h:357
GSM0808_FE_IE_UPLINK_CELL_LOAD_INFORMATION
@ GSM0808_FE_IE_UPLINK_CELL_LOAD_INFORMATION
Definition: gsm_08_08.h:353
GSM0808_FE_IE_SOURCE_CELL_ID
@ GSM0808_FE_IE_SOURCE_CELL_ID
Definition: gsm_08_08.h:360
GSM0808_FE_IE_INTER_RAT_HANDOVER_INFO
@ GSM0808_FE_IE_INTER_RAT_HANDOVER_INFO
Definition: gsm_08_08.h:350
GSM0808_FE_IE_LAST_USED_EUTRAN_PLMN_ID
@ GSM0808_FE_IE_LAST_USED_EUTRAN_PLMN_ID
Definition: gsm_08_08.h:363
GSM0808_FE_IE_CELL_LOAD_INFORMATION
@ GSM0808_FE_IE_CELL_LOAD_INFORMATION
Definition: gsm_08_08.h:355
GSM0808_FE_IE_CELL_LOAD_INFORMATION_GROUP
@ GSM0808_FE_IE_CELL_LOAD_INFORMATION_GROUP
Definition: gsm_08_08.h:354
GSM0808_FE_IE_D_RNTI
@ GSM0808_FE_IE_D_RNTI
Definition: gsm_08_08.h:358
GSM0808_FE_IE_EXTRA_INFORMATION
@ GSM0808_FE_IE_EXTRA_INFORMATION
Definition: gsm_08_08.h:344
GSM0808_FE_IE_PS_INDICATION
@ GSM0808_FE_IE_PS_INDICATION
Definition: gsm_08_08.h:356
GSM0808_FE_IE_CDMA2000_CAPABILITY_INFORMATION
@ GSM0808_FE_IE_CDMA2000_CAPABILITY_INFORMATION
Definition: gsm_08_08.h:351
GSM0808_FE_IE_IRAT_MEASUREMENT_CONFIGURATION
@ GSM0808_FE_IE_IRAT_MEASUREMENT_CONFIGURATION
Definition: gsm_08_08.h:359
GSM0808_FE_IE_TARGET_CELL_RADIO_INFORMATION
@ GSM0808_FE_IE_TARGET_CELL_RADIO_INFORMATION
Definition: gsm_08_08.h:346
GSM0808_FE_IE_CURRENT_CHANNEL_TYPE_2
@ GSM0808_FE_IE_CURRENT_CHANNEL_TYPE_2
Definition: gsm_08_08.h:345
GSM0808_FE_IE_DOWNLINK_CELL_LOAD_INFORMATION
@ GSM0808_FE_IE_DOWNLINK_CELL_LOAD_INFORMATION
Definition: gsm_08_08.h:352
GSM0808_FE_IE_VGCS_TALKER_MODE
@ GSM0808_FE_IE_VGCS_TALKER_MODE
Definition: gsm_08_08.h:362
GSM0808_FE_IE_IRAT_MEASUREMENT_CONFIGURATION_EXTENDED_E_ARFCNS
@ GSM0808_FE_IE_IRAT_MEASUREMENT_CONFIGURATION_EXTENDED_E_ARFCNS
Definition: gsm_08_08.h:361
GSM0808_FE_IE_MULTIRATE_CONFIGURATION_INFORMATION
@ GSM0808_FE_IE_MULTIRATE_CONFIGURATION_INFORMATION
Definition: gsm_08_08.h:348
gsm0808_chan_rate_type_sign
gsm0808_chan_rate_type_sign
Definition: gsm_08_08.h:479
GSM0808_SIGN_ANY
@ GSM0808_SIGN_ANY
Definition: gsm_08_08.h:480
GSM0808_SIGN_HALF_LM
@ GSM0808_SIGN_HALF_LM
Definition: gsm_08_08.h:485
GSM0808_SIGN_SDCCH_FULL_BM
@ GSM0808_SIGN_SDCCH_FULL_BM
Definition: gsm_08_08.h:482
GSM0808_SIGN_FULL_PREF_NO_CHANGE
@ GSM0808_SIGN_FULL_PREF_NO_CHANGE
Definition: gsm_08_08.h:488
GSM0808_SIGN_SDCCH_HALF_LM
@ GSM0808_SIGN_SDCCH_HALF_LM
Definition: gsm_08_08.h:483
GSM0808_SIGN_FULL_PREF
@ GSM0808_SIGN_FULL_PREF
Definition: gsm_08_08.h:486
GSM0808_SIGN_HALF_PREF
@ GSM0808_SIGN_HALF_PREF
Definition: gsm_08_08.h:487
GSM0808_SIGN_FULL_BM
@ GSM0808_SIGN_FULL_BM
Definition: gsm_08_08.h:484
GSM0808_SIGN_SDCCH
@ GSM0808_SIGN_SDCCH
Definition: gsm_08_08.h:481
GSM0808_SIGN_HALF_PREF_NO_CHANGE
@ GSM0808_SIGN_HALF_PREF_NO_CHANGE
Definition: gsm_08_08.h:489
BSS_MAP_MSG_TYPE
BSS_MAP_MSG_TYPE
Definition: gsm_08_08.h:74
BSS_MAP_MSG_CHANGE_CIRCUIT
@ BSS_MAP_MSG_CHANGE_CIRCUIT
Definition: gsm_08_08.h:145
BSS_MAP_MSG_VGCS_VBS_SETUP_REFUSE
@ BSS_MAP_MSG_VGCS_VBS_SETUP_REFUSE
Definition: gsm_08_08.h:164
BSS_MAP_MSG_INT_HANDOVER_CMD
@ BSS_MAP_MSG_INT_HANDOVER_CMD
Definition: gsm_08_08.h:98
BSS_MAP_MSG_VGCS_VBS_SETUP_ACK
@ BSS_MAP_MSG_VGCS_VBS_SETUP_ACK
Definition: gsm_08_08.h:163
BSS_MAP_MSG_NOTIFICATION_DATA
@ BSS_MAP_MSG_NOTIFICATION_DATA
Definition: gsm_08_08.h:180
BSS_MAP_MSG_BSS_INVOKE_TRACE
@ BSS_MAP_MSG_BSS_INVOKE_TRACE
Definition: gsm_08_08.h:130
BSS_MAP_MSG_UPLINK_RQST_ACKNOWLEDGE
@ BSS_MAP_MSG_UPLINK_RQST_ACKNOWLEDGE
Definition: gsm_08_08.h:170
BSS_MAP_MSG_ASSIGNMENT_FAILURE
@ BSS_MAP_MSG_ASSIGNMENT_FAILURE
Definition: gsm_08_08.h:80
BSS_MAP_MSG_VGCS_VBS_QUEUING_INDICATION
@ BSS_MAP_MSG_VGCS_VBS_QUEUING_INDICATION
Definition: gsm_08_08.h:168
BSS_MAP_MSG_ASSIGNMENT_RQST
@ BSS_MAP_MSG_ASSIGNMENT_RQST
Definition: gsm_08_08.h:78
BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_FAILURE
@ BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_FAILURE
Definition: gsm_08_08.h:167
BSS_MAP_MSG_CLASSMARK_UPDATE
@ BSS_MAP_MSG_CLASSMARK_UPDATE
Definition: gsm_08_08.h:153
BSS_MAP_MSG_HANDOVER_REQUIRED
@ BSS_MAP_MSG_HANDOVER_REQUIRED
Definition: gsm_08_08.h:85
BSS_MAP_MSG_RESOURCE_RQST
@ BSS_MAP_MSG_RESOURCE_RQST
Definition: gsm_08_08.h:149
BSS_MAP_MSG_INT_HANDOVER_REQUIRED_REJ
@ BSS_MAP_MSG_INT_HANDOVER_REQUIRED_REJ
Definition: gsm_08_08.h:97
BSS_MAP_MSG_MSC_INVOKE_TRACE
@ BSS_MAP_MSG_MSC_INVOKE_TRACE
Definition: gsm_08_08.h:129
BSS_MAP_MSG_VGCS_VBS_AREA_CELL_INFO
@ BSS_MAP_MSG_VGCS_VBS_AREA_CELL_INFO
Definition: gsm_08_08.h:172
BSS_MAP_MSG_RESET_ACKNOWLEDGE
@ BSS_MAP_MSG_RESET_ACKNOWLEDGE
Definition: gsm_08_08.h:124
BSS_MAP_MSG_RESET_CIRCUIT_ACKNOWLEDGE
@ BSS_MAP_MSG_RESET_CIRCUIT_ACKNOWLEDGE
Definition: gsm_08_08.h:128
BSS_MAP_MSG_RESET
@ BSS_MAP_MSG_RESET
Definition: gsm_08_08.h:123
BSS_MAP_MSG_HANDOVER_CMD
@ BSS_MAP_MSG_HANDOVER_CMD
Definition: gsm_08_08.h:87
BSS_MAP_MSG_RESET_IP_RSRC
@ BSS_MAP_MSG_RESET_IP_RSRC
Definition: gsm_08_08.h:132
BSS_MAP_MSG_HANDOVER_REQUIRED_REJECT
@ BSS_MAP_MSG_HANDOVER_REQUIRED_REJECT
Definition: gsm_08_08.h:94
BSS_MAP_MSG_CONNECTION_ORIENTED_INFORMATION
@ BSS_MAP_MSG_CONNECTION_ORIENTED_INFORMATION
Definition: gsm_08_08.h:113
BSS_MAP_MSG_COMMON_ID
@ BSS_MAP_MSG_COMMON_ID
Definition: gsm_08_08.h:118
BSS_MAP_MSG_CONFUSION
@ BSS_MAP_MSG_CONFUSION
Definition: gsm_08_08.h:108
BSS_MAP_MSG_INT_HANDOVER_REQUIRED
@ BSS_MAP_MSG_INT_HANDOVER_REQUIRED
Definition: gsm_08_08.h:96
BSS_MAP_MSG_UNBLOCK
@ BSS_MAP_MSG_UNBLOCK
Definition: gsm_08_08.h:138
BSS_MAP_MSG_VGCS_ADDL_INFO
@ BSS_MAP_MSG_VGCS_ADDL_INFO
Definition: gsm_08_08.h:178
BSS_MAP_MSG_RESERVED_1
@ BSS_MAP_MSG_RESERVED_1
Definition: gsm_08_08.h:105
BSS_MAP_MSG_QUEUING_INDICATION
@ BSS_MAP_MSG_QUEUING_INDICATION
Definition: gsm_08_08.h:155
BSS_MAP_MSG_CIPHER_MODE_CMD
@ BSS_MAP_MSG_CIPHER_MODE_CMD
Definition: gsm_08_08.h:152
BSS_MAP_MSG_RESERVED_2
@ BSS_MAP_MSG_RESERVED_2
Definition: gsm_08_08.h:106
BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_STATUS
@ BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_STATUS
Definition: gsm_08_08.h:171
BSS_MAP_MSG_CIRCUIT_GROUP_UNBLOCK
@ BSS_MAP_MSG_CIRCUIT_GROUP_UNBLOCK
Definition: gsm_08_08.h:142
BSS_MAP_MSG_HANDOVER_CANDIDATE_RESPONSE
@ BSS_MAP_MSG_HANDOVER_CANDIDATE_RESPONSE
Definition: gsm_08_08.h:93
BSS_MAP_MSG_RESET_IP_RSRC_ACK
@ BSS_MAP_MSG_RESET_IP_RSRC_ACK
Definition: gsm_08_08.h:133
BSS_MAP_MSG_CLEAR_CMD
@ BSS_MAP_MSG_CLEAR_CMD
Definition: gsm_08_08.h:102
BSS_MAP_MSG_RESERVED_0
@ BSS_MAP_MSG_RESERVED_0
Definition: gsm_08_08.h:75
BSS_MAP_MSG_UPLINK_RQST_CONFIRMATION
@ BSS_MAP_MSG_UPLINK_RQST_CONFIRMATION
Definition: gsm_08_08.h:173
BSS_MAP_MSG_HANDOVER_RQST
@ BSS_MAP_MSG_HANDOVER_RQST
Definition: gsm_08_08.h:84
BSS_MAP_MSG_LSA_INFORMATION
@ BSS_MAP_MSG_LSA_INFORMATION
Definition: gsm_08_08.h:115
BSS_MAP_MSG_PERFORM_LOCATION_ABORT
@ BSS_MAP_MSG_PERFORM_LOCATION_ABORT
Definition: gsm_08_08.h:117
BSS_MAP_MSG_INT_HANDOVER_ENQUIRY
@ BSS_MAP_MSG_INT_HANDOVER_ENQUIRY
Definition: gsm_08_08.h:99
BSS_MAP_MSG_COMPLETE_LAYER_3
@ BSS_MAP_MSG_COMPLETE_LAYER_3
Definition: gsm_08_08.h:156
BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_RESULT
@ BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_RESULT
Definition: gsm_08_08.h:166
BSS_MAP_MSG_RESUME
@ BSS_MAP_MSG_RESUME
Definition: gsm_08_08.h:112
BSS_MAP_MSG_OVERLOAD
@ BSS_MAP_MSG_OVERLOAD
Definition: gsm_08_08.h:125
BSS_MAP_MSG_LCLS_CONNECT_CTRL_ACK
@ BSS_MAP_MSG_LCLS_CONNECT_CTRL_ACK
Definition: gsm_08_08.h:185
BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_RQST
@ BSS_MAP_MSG_VGCS_VBS_ASSIGNMENT_RQST
Definition: gsm_08_08.h:165
BSS_MAP_MSG_HANDOVER_FAILURE
@ BSS_MAP_MSG_HANDOVER_FAILURE
Definition: gsm_08_08.h:90
BSS_MAP_MSG_PERFORM_LOCATION_RESPONSE
@ BSS_MAP_MSG_PERFORM_LOCATION_RESPONSE
Definition: gsm_08_08.h:116
BSS_MAP_MSG_CHANGE_CIRCUIT_ACKNOWLEDGE
@ BSS_MAP_MSG_CHANGE_CIRCUIT_ACKNOWLEDGE
Definition: gsm_08_08.h:146
BSS_MAP_MSG_HANDOVER_COMPLETE
@ BSS_MAP_MSG_HANDOVER_COMPLETE
Definition: gsm_08_08.h:88
BSS_MAP_MSG_PERFORM_LOCATION_RQST
@ BSS_MAP_MSG_PERFORM_LOCATION_RQST
Definition: gsm_08_08.h:114
BSS_MAP_MSG_UPLINK_RELEASE_CMD
@ BSS_MAP_MSG_UPLINK_RELEASE_CMD
Definition: gsm_08_08.h:176
BSS_MAP_MSG_UPLINK_APP_DATA
@ BSS_MAP_MSG_UPLINK_APP_DATA
Definition: gsm_08_08.h:181
BSS_MAP_MSG_HANDOVER_DETECT
@ BSS_MAP_MSG_HANDOVER_DETECT
Definition: gsm_08_08.h:95
BSS_MAP_MSG_CLASSMARK_RQST
@ BSS_MAP_MSG_CLASSMARK_RQST
Definition: gsm_08_08.h:157
BSS_MAP_MSG_RESOURCE_INDICATION
@ BSS_MAP_MSG_RESOURCE_INDICATION
Definition: gsm_08_08.h:150
BSS_MAP_MSG_RESET_CIRCUIT
@ BSS_MAP_MSG_RESET_CIRCUIT
Definition: gsm_08_08.h:127
BSS_MAP_MSG_HANDOVER_PERFORMED
@ BSS_MAP_MSG_HANDOVER_PERFORMED
Definition: gsm_08_08.h:91
BSS_MAP_MSG_PAGING
@ BSS_MAP_MSG_PAGING
Definition: gsm_08_08.h:151
BSS_MAP_MSG_UPLINK_RELEASE_INDICATION
@ BSS_MAP_MSG_UPLINK_RELEASE_INDICATION
Definition: gsm_08_08.h:174
BSS_MAP_MSG_CIRCUIT_GROUP_UNBLOCKING_ACKNOWLEDGE
@ BSS_MAP_MSG_CIRCUIT_GROUP_UNBLOCKING_ACKNOWLEDGE
Definition: gsm_08_08.h:143
BSS_MAP_MSG_UNBLOCKING_ACKNOWLEDGE
@ BSS_MAP_MSG_UNBLOCKING_ACKNOWLEDGE
Definition: gsm_08_08.h:139
BSS_MAP_MSG_CIPHER_MODE_COMPLETE
@ BSS_MAP_MSG_CIPHER_MODE_COMPLETE
Definition: gsm_08_08.h:154
BSS_MAP_MSG_CHAN_MOD_RQST
@ BSS_MAP_MSG_CHAN_MOD_RQST
Definition: gsm_08_08.h:81
BSS_MAP_MSG_LOAD_INDICATION
@ BSS_MAP_MSG_LOAD_INDICATION
Definition: gsm_08_08.h:159
BSS_MAP_MSG_UPLINK_SEIZED_CMD
@ BSS_MAP_MSG_UPLINK_SEIZED_CMD
Definition: gsm_08_08.h:177
BSS_MAP_MSG_HANDOVER_CANDIDATE_ENQUIRE
@ BSS_MAP_MSG_HANDOVER_CANDIDATE_ENQUIRE
Definition: gsm_08_08.h:92
BSS_MAP_MSG_VGCS_SMS
@ BSS_MAP_MSG_VGCS_SMS
Definition: gsm_08_08.h:179
BSS_MAP_MSG_SUSPEND
@ BSS_MAP_MSG_SUSPEND
Definition: gsm_08_08.h:111
BSS_MAP_MSG_UNEQUIPPED_CIRCUIT
@ BSS_MAP_MSG_UNEQUIPPED_CIRCUIT
Definition: gsm_08_08.h:144
BSS_MAP_MSG_BLOCKING_ACKNOWLEDGE
@ BSS_MAP_MSG_BLOCKING_ACKNOWLEDGE
Definition: gsm_08_08.h:137
BSS_MAP_MSG_UPLINK_REJECT_CMD
@ BSS_MAP_MSG_UPLINK_REJECT_CMD
Definition: gsm_08_08.h:175
BSS_MAP_MSG_ASSIGNMENT_COMPLETE
@ BSS_MAP_MSG_ASSIGNMENT_COMPLETE
Definition: gsm_08_08.h:79
BSS_MAP_MSG_REROUTE_CMD
@ BSS_MAP_MSG_REROUTE_CMD
Definition: gsm_08_08.h:119
BSS_MAP_MSG_CLEAR_RQST
@ BSS_MAP_MSG_CLEAR_RQST
Definition: gsm_08_08.h:104
BSS_MAP_MSG_CLEAR_COMPLETE
@ BSS_MAP_MSG_CLEAR_COMPLETE
Definition: gsm_08_08.h:103
BSS_MAP_MSG_BLOCK
@ BSS_MAP_MSG_BLOCK
Definition: gsm_08_08.h:136
BSS_MAP_MSG_HANDOVER_RQST_ACKNOWLEDGE
@ BSS_MAP_MSG_HANDOVER_RQST_ACKNOWLEDGE
Definition: gsm_08_08.h:86
BSS_MAP_MSG_RESERVED_3
@ BSS_MAP_MSG_RESERVED_3
Definition: gsm_08_08.h:126
BSS_MAP_MSG_CIPHER_MODE_REJECT
@ BSS_MAP_MSG_CIPHER_MODE_REJECT
Definition: gsm_08_08.h:158
BSS_MAP_MSG_UPLINK_RQST
@ BSS_MAP_MSG_UPLINK_RQST
Definition: gsm_08_08.h:169
BSS_MAP_MSG_LCLS_NOTIFICATION
@ BSS_MAP_MSG_LCLS_NOTIFICATION
Definition: gsm_08_08.h:186
BSS_MAP_MSG_REROUTE_COMPLETE
@ BSS_MAP_MSG_REROUTE_COMPLETE
Definition: gsm_08_08.h:120
BSS_MAP_MSG_VGCS_VBS_SETUP
@ BSS_MAP_MSG_VGCS_VBS_SETUP
Definition: gsm_08_08.h:162
BSS_MAP_MSG_LCLS_CONNECT_CTRL
@ BSS_MAP_MSG_LCLS_CONNECT_CTRL
Definition: gsm_08_08.h:184
BSS_MAP_MSG_HANDOVER_SUCCEEDED
@ BSS_MAP_MSG_HANDOVER_SUCCEEDED
Definition: gsm_08_08.h:89
BSS_MAP_MSG_CIRCUIT_GROUP_BLOCK
@ BSS_MAP_MSG_CIRCUIT_GROUP_BLOCK
Definition: gsm_08_08.h:140
BSS_MAP_MSG_SAPI_N_REJECT
@ BSS_MAP_MSG_SAPI_N_REJECT
Definition: gsm_08_08.h:107
BSS_MAP_MSG_CIRCUIT_GROUP_BLOCKING_ACKNOWLEDGE
@ BSS_MAP_MSG_CIRCUIT_GROUP_BLOCKING_ACKNOWLEDGE
Definition: gsm_08_08.h:141
BSS_MAP_MSG_CONNECTIONLESS_INFORMATION
@ BSS_MAP_MSG_CONNECTIONLESS_INFORMATION
Definition: gsm_08_08.h:131
gsm0808_chan_rate_type_speech
gsm0808_chan_rate_type_speech
Definition: gsm_08_08.h:467
GSM0808_SPEECH_PERM_NO_CHANGE
@ GSM0808_SPEECH_PERM_NO_CHANGE
Definition: gsm_08_08.h:475
GSM0808_SPEECH_HALF_PREF
@ GSM0808_SPEECH_HALF_PREF
Definition: gsm_08_08.h:471
GSM0808_SPEECH_FULL_BM
@ GSM0808_SPEECH_FULL_BM
Definition: gsm_08_08.h:468
GSM0808_SPEECH_HALF_PREF_NO_CHANGE
@ GSM0808_SPEECH_HALF_PREF_NO_CHANGE
Definition: gsm_08_08.h:473
GSM0808_SPEECH_PERM
@ GSM0808_SPEECH_PERM
Definition: gsm_08_08.h:474
GSM0808_SPEECH_FULL_PREF_NO_CHANGE
@ GSM0808_SPEECH_FULL_PREF_NO_CHANGE
Definition: gsm_08_08.h:472
GSM0808_SPEECH_HALF_LM
@ GSM0808_SPEECH_HALF_LM
Definition: gsm_08_08.h:469
GSM0808_SPEECH_FULL_PREF
@ GSM0808_SPEECH_FULL_PREF
Definition: gsm_08_08.h:470
SPEECH_CODEC_MAXLEN
#define SPEECH_CODEC_MAXLEN
Definition: gsm_08_08.h:724
gsm0808_data_rate_non_transp
gsm0808_data_rate_non_transp
Definition: gsm_08_08.h:523
GSM0808_DATA_RATE_NON_TRANSP_12000_6000
@ GSM0808_DATA_RATE_NON_TRANSP_12000_6000
Definition: gsm_08_08.h:524
GSM0808_DATA_RATE_NON_TRANSP_29k0
@ GSM0808_DATA_RATE_NON_TRANSP_29k0
Definition: gsm_08_08.h:526
GSM0808_DATA_RATE_NON_TRANSP_6k0
@ GSM0808_DATA_RATE_NON_TRANSP_6k0
Definition: gsm_08_08.h:529
GSM0808_DATA_RATE_NON_TRANSP_43k5
@ GSM0808_DATA_RATE_NON_TRANSP_43k5
Definition: gsm_08_08.h:525
GSM0808_DATA_RATE_NON_TRANSP_14k5
@ GSM0808_DATA_RATE_NON_TRANSP_14k5
Definition: gsm_08_08.h:527
GSM0808_DATA_RATE_NON_TRANSP_12k0
@ GSM0808_DATA_RATE_NON_TRANSP_12k0
Definition: gsm_08_08.h:528
CH_TYPE_PERM_SPCH_MAXLEN
#define CH_TYPE_PERM_SPCH_MAXLEN
Definition: gsm_08_08.h:740
gsm0406_dlci_sapi_name
static const char * gsm0406_dlci_sapi_name(enum gsm0406_dlci_sapi val)
Definition: gsm_08_08.h:71
ENCRY_INFO_KEY_MAXLEN
#define ENCRY_INFO_KEY_MAXLEN
Definition: gsm_08_08.h:759
gsm0406_dlci_sapi
gsm0406_dlci_sapi
Definition: gsm_08_08.h:66
DLCI_SAPI_RR_MM_CC
@ DLCI_SAPI_RR_MM_CC
Definition: gsm_08_08.h:67
DLCI_SAPI_SMS
@ DLCI_SAPI_SMS
Definition: gsm_08_08.h:68
gsm0808_permitted_speech_name
static const char * gsm0808_permitted_speech_name(enum gsm0808_permitted_speech val)
Definition: gsm_08_08.h:544
linuxlist.h
bssmap_header
Definition: gsm_08_08.h:42
bssmap_header::length
uint8_t length
Definition: gsm_08_08.h:44
bssmap_header::type
uint8_t type
Definition: gsm_08_08.h:43
dtap_header
Definition: gsm_08_08.h:47
dtap_header::length
uint8_t length
Definition: gsm_08_08.h:62
dtap_header::type
uint8_t type
Definition: gsm_08_08.h:48
dtap_header::link_id
uint8_t link_id
Definition: gsm_08_08.h:50
gsm0808_cell_id_list
DEPRECATED: This definition of the cell identifier list is insufficient.
Definition: gsm_08_08.h:775
gsm0808_cell_id_list::id_list_len
unsigned int id_list_len
Definition: gsm_08_08.h:778
gsm0808_cell_id_list::id_list_lac
uint16_t id_list_lac[CELL_ID_LIST_LAC_MAXLEN]
Definition: gsm_08_08.h:777
gsm0808_cell_id_list::id_discr
uint8_t id_discr
Definition: gsm_08_08.h:776
gsm0808_channel_type
Definition: gsm_08_08.h:741
gsm0808_channel_type::data_asym_pref
enum gsm0808_channel_type_asym_pref data_asym_pref
Definition: gsm_08_08.h:755
gsm0808_channel_type::perm_spch_len
unsigned int perm_spch_len
Definition: gsm_08_08.h:747
gsm0808_channel_type::ch_rate_type
uint8_t ch_rate_type
Definition: gsm_08_08.h:743
gsm0808_channel_type::data_transparent
bool data_transparent
Definition: gsm_08_08.h:750
gsm0808_channel_type::data_rate
uint8_t data_rate
Definition: gsm_08_08.h:751
gsm0808_channel_type::ch_indctr
uint8_t ch_indctr
Definition: gsm_08_08.h:742
gsm0808_channel_type::data_rate_allowed
uint8_t data_rate_allowed
Definition: gsm_08_08.h:753
gsm0808_channel_type::data_rate_allowed_is_set
bool data_rate_allowed_is_set
Definition: gsm_08_08.h:752
gsm0808_channel_type::data_asym_pref_is_set
bool data_asym_pref_is_set
Definition: gsm_08_08.h:754
gsm0808_channel_type::perm_spch
uint8_t perm_spch[CH_TYPE_PERM_SPCH_MAXLEN]
Definition: gsm_08_08.h:746
gsm0808_diagnostics
Definition: gsm_08_08.h:813
gsm0808_diagnostics::error_pointer_octet
uint8_t error_pointer_octet
Definition: gsm_08_08.h:814
gsm0808_diagnostics::msg
uint8_t msg[0]
Definition: gsm_08_08.h:822
gsm0808_encrypt_info
Definition: gsm_08_08.h:761
gsm0808_encrypt_info::key
uint8_t key[ENCRY_INFO_KEY_MAXLEN]
Definition: gsm_08_08.h:764
gsm0808_encrypt_info::perm_algo
uint8_t perm_algo[ENCRY_INFO_PERM_ALGO_MAXLEN]
Definition: gsm_08_08.h:762
gsm0808_encrypt_info::key_len
unsigned int key_len
Definition: gsm_08_08.h:765
gsm0808_encrypt_info::perm_algo_len
unsigned int perm_algo_len
Definition: gsm_08_08.h:763
gsm0808_speech_codec_list
Definition: gsm_08_08.h:725
gsm0808_speech_codec_list::codec
struct gsm0808_speech_codec codec[SPEECH_CODEC_MAXLEN]
Definition: gsm_08_08.h:726
gsm0808_speech_codec_list::len
uint8_t len
Definition: gsm_08_08.h:727
gsm0808_speech_codec
3GPP TS 48.008 3.2.2.104 Speech Codec.
Definition: gsm_08_08.h:593
gsm0808_speech_codec::fi
bool fi
Full IP: AoIP with compressed speech via RTP/UDP/IP.
Definition: gsm_08_08.h:595
gsm0808_speech_codec::cfg
uint16_t cfg
For examples, see enum gsm0808_speech_codec_defaults.
Definition: gsm_08_08.h:605
gsm0808_speech_codec::pi
bool pi
PCMoIP: PCM over A-Interface via RTP/UPD/IP.
Definition: gsm_08_08.h:597
gsm0808_speech_codec::type
uint8_t type
See enum gsm0808_speech_codec_type.
Definition: gsm_08_08.h:603
gsm0808_speech_codec::tf
bool tf
TFO (Inband Tandem Free Operation).
Definition: gsm_08_08.h:601
gsm0808_speech_codec::pt
bool pt
PCMoTDM: PCM over A-Interface with TDM as transport.
Definition: gsm_08_08.h:599
value_string
utils.h